SECTION 10 31 07

MANUFACTURED GAS FIREPLACES

Display hidden notes to specifier. (Don't know how? [Click Here](https://www.arcat.com/sd/display_hidden_notes.shtml))

*Copyright 2014 - 2016 ARCAT, Inc. - All rights reserved*

\*\* NOTE TO SPECIFIER \*\* Heatilator®; gas, wood and electric sourced fireplaces.  
This section is based on the products of Heatilator®, which is located at:  
7571 215th St. W.  
Lakeville, MN 55044   
Toll Free Tel: 800-927-6841   
Email: [request info (swansonm@hearthnhome.com)](https://admin.arcat.com/users.pl?action=UserEmail&company=Heatilator)  
Web: <http://pro.heatilator.com>   
 [ [Click Here](https://www.arcat.com/arcatcos/cos49/arc49248.html) ] for additional information.  
Heatilator is known as "the first name in fireplaces," and has been a leader in fireplace dependability and value for more than 85 years. The brand owns a rich history and is the most widely recognized, preferred and installed brand by builders. Heatilator offers a full lineup of gas fireplaces, stoves and fireplace inserts, and also hearth accessories. The company is headquartered in Mount Pleasant, Iowa and is a member of Hearth & Home Technologies, Inc. (HHT).

1. GENERAL
   1. SECTION INCLUDES

\*\* NOTE TO SPECIFIER \*\* Delete items below not required for project.

* + 1. Gas fireplaces and accessories including the following:
       1. Manufactured indoor gas fireplaces.
       2. Manufactured outdoor gas fireplaces.
       3. Indoor gas fireplace inserts.
       4. Indoor gas log sets.
       5. Outdoor gas log sets.
       6. Gas fireplace mantels and fireplace surrounds.
       7. Gas fireplace accessories.
  1. RELATED SECTIONS

\*\* NOTE TO SPECIFIER \*\* Delete any sections below not relevant to this project; add others as required.

* + 1. Section 06 10 00 - Rough Carpentry.
    2. Section 09 26 00 - Gypsum Board Assemblies.
    3. Section 22 05 00 - Common Work Results for Plumbing.
    4. Section 26 05 00 - Common Work Results for Electrical.
  1. REFERENCES

\*\* NOTE TO SPECIFIER \*\* Delete references from the list below that are not actually required by the text of the edited section.

* + 1. ANSI Z21.44 - Gas-Fired Gravity and Fan Type Direct Vent Wall Furnaces.
    2. ANSI Z21.88 - Vented Gas Fireplace Heaters.
    3. Z21.50b - Vented Gas Fireplaces.
    4. ANSI Z223.1 - National Fuel Gas Code.
    5. CSA 2.22b - Vented Gas Fireplaces.
    6. CSA 2.33 - Vented Gas Fireplace Heaters.
    7. CAN/ULC S610 - Factory-Built Fireplaces.
    8. UL 127 - Standard for Factory-Built Fireplaces.
    9. UL 907 - Standard for Fireplace Accessories
    10. UL 1482 - Standard for Safety for Solid-Fuel Type Room Heaters.
  1. SUBMITTALS
     1. Submit under provisions of Section 01 30 00 - Administrative Requirements.
     2. Product Data: Manufacturer's data sheets on each product to be used, including:
        1. Preparation instructions and recommendations.
        2. Storage and handling requirements and recommendations.
        3. Installation methods.
     3. Shop Drawings: Provide drawing of required clearances, rough-in of enclosure and utilities.

\*\* NOTE TO SPECIFIER \*\* Delete selection samples if colors have already been selected.

* + 1. Selection Samples: For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and finishes.
    2. Verification Samples: For each finish product specified, two samples, minimum size 6 inches (150 mm) square representing actual product.
  1. QUALITY ASSURANCE
     1. Manufacturer Qualifications: Minimum 5 year experience manufacturing similar products.
     2. Installer Qualifications: Minimum 2 year experience installing similar products.

\*\* NOTE TO SPECIFIER \*\* Include a mock-up if the project size and/or quality warrant taking such a precaution. The following is one example of how a mock-up on a large project might be specified. When deciding on the extent of the mock-up, consider all the major different types of work on the project.

* + 1. Multiple Installation Mock-Up: Provide a mock-up for evaluation of site and framing preparation techniques and installation workmanship.
       1. Provide representative fireplace in area designated by Architect.
       2. Do not proceed with remaining units until workmanship, installation and operation are approved by Architect.
       3. Remake mock-up unit as required to produce acceptable work.
  1. PRE-INSTALLATION MEETINGS
     1. Convene minimum two weeks prior to starting work of this section.
  2. DELIVERY, STORAGE, AND HANDLING
     1. Deliver and store products in manufacturer's unopened packaging bearing the brand name and manufacturer's identification until ready for installation.
     2. Handling: Handle materials to avoid damage.
  3. PROJECT CONDITIONS
     1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
  4. SEQUENCING
     1. Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
  5. WARRANTY
     1. Warranty: Provide manufacturer's standard warranty against defects in materials and workmanship.

1. PRODUCTS
   1. MANUFACTURERS
      1. Acceptable Manufacturer: Heatilator®, which is located at: 7571 215th St. W.; Lakeville, MN 55044 ; Toll Free Tel: 800-927-6841 ; Email: [request info (swansonm@hearthnhome.com)](https://admin.arcat.com/users.pl?action=UserEmail&company=Heatilator); Web: <http://pro.heatilator.com>

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions.

* + 1. Substitutions: Not permitted.
    2. Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* 1. MANUFACTURED INDOOR GAS FIREPLACES
     1. Compliance - General:
        1. Comply with applicable building codes.
        2. Comply with ANSI Z21.88/CSA 2.33 or Z21.50b/CSA 2.22b.

\*\* NOTE TO SPECIFIER \*\* The Heirloom provides authentic masonry style without the costs of a site-built masonry fireplace. The largest viewing areas in their class showcase intense fires and textured brick interiors. Powerful heat and high-efficiency performance help make the Heirloom a valuable addition to any home. Delete if not required.

* + 1. Heirloom Series:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Delete control not required.

* + - 1. Control: IntelliFire Plus RC200.
      2. Control: IntelliFire Plus RC100.
      3. Control: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete fronts and doors not required.

* + - 1. Fronts-Doors: Black Firescreen.
      2. Fronts-Doors: Black Cabinet Style Firescreen.
      3. Fronts-Doors: Black Arched Firescreen.
      4. Fronts-Doors: Bronze Firescreen.
      5. Fronts-Doors: Bronze Cabinet Style Firescreen.
      6. Fronts-Doors: Bronze Arched Firescreen.

\*\* NOTE TO SPECIFIER \*\* Delete refractory not required.

* + - 1. Refractory: Traditional.
      2. Refractory: Herringbone.
      3. Refractory: Castlewood.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model: HEIR36 as manufactured by Heatilator.
         1. Unit Front Width: 61 inches (1549 mm).
         2. Framing Front Width: 59-1/2 inches (1511 mm).
         3. Unit Back Width: 59-1/4 inches (1505 mm).
         4. Framing Back Width: 59-1/2 inches (1511 mm).
         5. Unit Height: 57-5/8 inches (1463 mm).
         6. Framing Height: 56 inches (1422 mm).
         7. Unit Depth: 24 inches (610 mm).
         8. Framing Depth: 24 inches (610 mm).
         9. Glass Size: 35-7/8 inches x 31-1/16 inches (904 mm x 789 mm).
         10. BTU/Hour Input: 45,000 (13.2 kW).
      2. Model: HEIR42 as manufactured by Heatilator.
         1. Unit Front Width: 67 inches (1702 mm).
         2. Framing Front Width: 65-9/16 inches (1665 mm).
         3. Unit Back Width: 65-5/16 inches (1659 mm).
         4. Framing Back Width: 65-9/16 inches (1665 mm).
         5. Unit Height: 62-5/8 inches (1591 mm).
         6. Framing Height: 61 inches (1549 mm).
         7. Unit Depth: 24 inches (610 mm).
         8. Framing Depth: 24 inches (610 mm).
         9. Glass Size: 41-7/8 inches x 36-1/16 inches (1064 mm x 916 mm).
         10. BTU/Hour Input: 54,000 (15.8 kW).
      3. Model: HEIR50 as manufactured by Heatilator.
         1. Unit Front Width: 75 inches (1905 mm).
         2. Framing Front Width: 73-9/16 inches (1868 mm).
         3. Unit Back Width: 73-5/16 inches (1862 mm).
         4. Framing Back Width: 73-9/16 inches (1868 mm).
         5. Unit Height: 66-5/8 inches (1682 mm).
         6. Framing Height: 65 inches (1651 mm).
         7. Unit Depth: 24 inches (610 mm).
         8. Framing Depth: 24 inches (610 mm).
         9. Glass Size: 49-7/8 inches x 40-1/16 inches (1267 mm x 1018 mm).
         10. BTU/Hour Input: 65,000 (19 kW).

\*\* NOTE TO SPECIFIER \*\* This attractive fireplace minimizes visible steel and maximizes viewing areas for the ultimate fireside experience. A top direct vent system offers a wide range of installation possibilities. Control the warmth and ambiance with a sophisticated remote. Delete if not required.

* + 1. Corner Series:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Delete control not required.

* + - 1. Control: WSK200.
      2. Control: Smart-Stat.
      3. Control: Smart-Batt.
      4. Control: WSK-MLT Wall Switch.

\*\* NOTE TO SPECIFIER \*\* Delete fronts and doors not required.

* + - 1. Fronts-Doors: Black Phoenix.
      2. Fronts-Doors: Black Simon.
      3. Fronts-Doors: Black Craftsman.
      4. Fronts-Doors: Bronze Phoenix.
      5. Fronts-Doors: Bronze Simon.
      6. Fronts-Doors: Bronze Craftsman.
      7. Model CDCLCR as manufactured by Heatilator.
         1. Unit Front Width: 42-1/2 inches (1080 mm).
         2. Framing Front Width: 40 inches (1016 mm).
         3. Unit Height: 38 inches (965 mm).
         4. Framing Height: 38-1/8 inches (968 mm).
         5. Unit Depth: 24-1/2 inches (622 mm).
         6. Framing Depth: 24 inches (610 mm).
         7. Glass Size: 36 inches (914 mm).
         8. BTU/Hour Input: 34,000 (9.7 kW).

\*\* NOTE TO SPECIFIER \*\* The Caliber nXt delivers high-efficiency heating and traditional ambiance. Realistic logs and bold flames fill the large viewing area with a beautiful, roaring fire. This unit includes a standard fan, allowing for even heat distribution. Delete if not required.

* + 1. Caliber nXt Series:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.
       2. Control: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete fronts and doors not required.

* + - 1. Fronts-Doors: Black Arts & Crafts.
      2. Fronts-Doors: Black Contour.
      3. Fronts-Doors: Bronze Contour.
      4. Fronts-Doors: Black Jamestown.
      5. Fronts-Doors: Bronze Phoenix.
      6. Fronts-Doors: Black Simon.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article. Bella cabinet not available for the Caliber nXt Series.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article. Atlas, Echo and Luna models not available for Caliber nXt Series.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelve Article. St. Cloud model not available for Caliber nXt Series.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model CNXT4236 as manufactured by Heatilator.
         1. Unit Front Width: 41 inches (1041 mm).
         2. Framing Front Width: 42 inches (1067 mm).
         3. Unit Back Width: 28-1/2 inches (724 mm).
         4. Framing Back Width: 42 inches (1067 mm).
         5. Unit Height: 39-7/8 inches (1013 mm).
         6. Framing Height: 40-1/8 inches (1019 mm).
         7. Unit Depth: 21 inches (533 mm).
         8. Framing Depth: 22 inches (559 mm).
         9. Glass Size: 35 inches x 24-1/8 inches (889 mm x 613 mm).
         10. BTU/Hour Input: 40,000 (11.7 kW).
      2. Model CNXT4842 as manufactured by Heatilator.
         1. Unit Front Width: 48 inches (1219 mm).
         2. Framing Front Width: 49 inches (1245 mm).
         3. Unit Back Width: 35-1/2 inches (902 mm).
         4. Framing Back Width: 49 inches (1245 mm).
         5. Unit Height: 41-7/8 inches (1064 mm).
         6. Framing Height: 42-1/8 inches (1070 mm).
         7. Unit Depth: 21 inches (533 mm).
         8. Framing Depth: 22 inches (559 mm).
         9. Glass Size: 42 inches (1067 mm) x 26-1/8 inches (664 mm).
         10. BTU/Hour Input: 45,000 (13.2 kW).

\*\* NOTE TO SPECIFIER \*\* A unique design enables the Peninsula gas fireplace to elegantly divide a space. A three-sided viewing area lets the flames reach out into different rooms. User-friendly controls let you match flame height and heat output to your mood. Delete if not required.

* + 1. Peninsula Series:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Designed exclusively for fireplaces with IntelliFire™, our state-of-the-art intermittent pilot ignition system. Includes: on/off, auto battery backup, battery strength indicator, fan speed, flame control, pilot activation. Delete control not required.

* + - 1. Controls: WSK200.

\*\* NOTE TO SPECIFIER \*\* An added level of function and convenience in a remote control fire fireplaces, stoves, inserts and gas logs with or without line power. Battery-powered or hardwired receiver. Includes: on/off, temperature readout, thermostat mode, timer mode. Delete control not required.

* + - 1. Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete control not required.

* + - 1. Controls: Smart-Batt.

\*\* NOTE TO SPECIFIER \*\* Command of both comfort and ambiance. Includes: on/off, fan speed, flame control, pilot activation, auxiliary function, temperature readout, thermostat mode. Delete control not required.

* + - 1. Controls: WSK-MLT Wall Switch.

\*\* NOTE TO SPECIFIER \*\* This remote control effortlessly manages heat output and comfort level. Includes: hardwired receiver, on/off, fan speed, flame control, temperature readout, thermostat mode, timer mode. Delete control not required.

* + - 1. Controls: RCT-MLT.

\*\* NOTE TO SPECIFIER \*\* Delete control not required.

* + - 1. Controls: WSK21.

\*\* NOTE TO SPECIFIER \*\* Delete fronts and doors not required.

* + - 1. Fronts-Doors: Black Phoenix.
      2. Fronts-Doors: Black Simon.
      3. Fronts-Doors: Black Craftsman.
      4. Fronts-Doors: Bronze Phoenix.
      5. Fronts-Doors: Bronze Simon.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model GBFL4136 as manufactured by Heatilator.
         1. Unit Front Width: 40-1/2 inches (1029 mm).
         2. Framing Front Width: 41 inches (1041 mm).
         3. Unit Height: 38 inches (965 mm).
         4. Framing Height: 38-1/2 inches (978 mm).
         5. Unit Depth: 24 inches (610 mm).
         6. Framing Depth: 23 inches (584 mm).
         7. Glass Size: 36 inches (914 mm).
         8. BTU/Hour Input: 37,000 (10.8 kW).
      2. Model GDFL4136 as manufactured by Heatilator.
         1. Unit Front Width: 40-1/2 inches (1029 mm).
         2. Framing Front Width: 41 inches (1041 mm).
         3. Unit Height: 38 inches (965 mm).
         4. Framing Height: 38-3/4 inches (984 mm).
         5. Unit Depth: 24 inches (610 mm).
         6. Framing Depth: 23 inches (584 mm).
         7. Glass Size: 36 inches (914 mm).
         8. BTU/Hour Input: 37,000 (10.8 kW).

\*\* NOTE TO SPECIFIER \*\* Link two separate spaces and enjoy double the ambiance with these attractive options. Advanced technology helps bold flames shine. And, the Heatilator name means these fireplaces will perform season after season, year after year. Delete if not required.

* + 1. See-Through Series:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Designed exclusively for fireplaces with IntelliFire™, our state-of-the-art intermittent pilot ignition system. Includes: on/off, auto battery backup, battery strength indicator, fan speed, flame control, pilot activation. Delete control not required.

* + - 1. Controls: WSK200.

\*\* NOTE TO SPECIFIER \*\* An added level of function and convenience in a remote control fire fireplaces, stoves, inserts and gas logs with or without line power. Battery-powered or hardwired receiver. Includes: on/off, temperature readout, thermostat mode, timer mode. Delete control not required.

* + - 1. Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete control not required.

* + - 1. Controls: Smart-Batt.

\*\* NOTE TO SPECIFIER \*\* Command of both comfort and ambiance. Includes: on/off, fan speed, flame control, pilot activation, auxiliary function, temperature readout, thermostat mode. Delete control not required.

* + - 1. Controls: WSK-MLT Wall Switch.

\*\* NOTE TO SPECIFIER \*\* This remote control effortlessly manages heat output and comfort level. Includes: hardwired receiver, on/off, fan speed, flame control, temperature readout, thermostat mode, timer mode.

* + - 1. Controls: RCT-MLT.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: WSK21.

\*\* NOTE TO SPECIFIER \*\* Delete front and door style and finish not required.

* + - 1. Fronts-Doors: Black Portfolio.
      2. Fronts-Doors: Bronze Portfolio.
      3. Fronts-Doors: Black Phoenix.
      4. Fronts-Doors: Bronze Phoenix.
      5. Fronts-Doors: Black Simon.
      6. Fronts-Doors: Black Craftsman.
      7. Fronts-Doors: Bronze Craftsman.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelves Article. St. Cloud not available for this model.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model GBST4336 as manufactured by Heatilator.
         1. Unit Front Width: 42-1/2 inches (1080 mm).
         2. Framing Front Width: 43 inches (1092 mm).
         3. Unit Height: 38 inches (965 mm).
         4. Framing Height: 38-1/2 inches (978 mm).
         5. Unit Depth: 24 inches (610 mm).
         6. Framing Depth: 23 inches (584 mm).
         7. Glass Size: 36 inches (914 mm) x 24-1/2 inches (622 mm).
         8. BTU/Hour Input: 37,000 (10.8 kW).
      2. Model GDST3831I as manufactured by Heatilator.
         1. Unit Front Width: 37-5/8 inches (956 mm).
         2. Framing Front Width: 38-1/8 inches (968 mm).
         3. Unit Height: 34-1/2 inches (876 mm).
         4. Framing Height: 34-3/4 inches (883 mm).
         5. Unit Depth: 16 inches (406 mm).
         6. Framing Depth: 15 inches (381 mm).
         7. Glass Size: 31 x 21 inches (533 mm).
         8. BTU/Hour Input: 21,000 (6.2 kW).
      3. Model GDST4336 as manufactured by Heatilator.
         1. Unit Front Width: 42-1/2 inches (1080 mm).
         2. Framing Front Width: 43 inches (1092 mm).
         3. Unit Height: 38 inches (965 mm).
         4. Framing Height: 38-3/4 inches (984 mm).
         5. Unit Depth: 24 inches (610 mm).
         6. Framing Depth: 23 inches (584 mm).
         7. Glass Size: 36 inches (914 mm) x 24-1/2 inches (622 mm).
         8. BTU/Hour Input: 37,000 (10.8 kW).

\*\* NOTE TO SPECIFIER \*\* Caliber Gas Fireplaces feature a deep steel interior and impressive heating power. Engineering innovations deliver high efficiency levels and easy operation. Create your unique look by pairing designer front and finish options to define any room. Delete if not required.

* + 1. Caliber Series:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: IntelliFire Plus RC100.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: IntelliFire Plus RC200.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: WSK21.

\*\* NOTE TO SPECIFIER \*\* Delete front and door style and finish not required.

* + - 1. Fronts-Doors: Black Arts & Crafts.
      2. Fronts-Doors: Bronze Contour.
      3. Fronts-Doors: Black Contour.
      4. Fronts-Doors: Black Jamestown.
      5. Fronts-Doors: Bronze Phoenix.
      6. Fronts-Doors: Black Simon.

\*\* NOTE TO SPECIFIER \*\* Refractory required.

* + - 1. Refractory: Caliber-WTBC-Weathered.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article. Bella cabinet and Kenwood corner not available for this model.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelves Article. St. Cloud not available for this model.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model CD4236 as manufactured by Heatilator.
         1. Unit Front Width: 41 inches (1041 mm).
         2. Framing Front Width: 42 inches (1067 mm).
         3. Unit Back Width: 28-1/2 inches (724 mm).
         4. Framing Back Width: 42 inches (1067 mm).
         5. Unit Height: 39-7/8 inches (1013 mm).
         6. Framing Height: 40-1/8 inches (1019 mm).
         7. Unit Depth: 21 inches (533 mm).
         8. Framing Depth: 22 inches (559 mm).
         9. Glass Size: 35 inches x 24-1/8 inches (889 mm x 613 mm).
         10. BTU/Hour Input: 30,000 (8.8 kW).
         11. Efficiency: Steady State - 75%, AFUE - 46%, Canada EnerGuide - 44%.
      2. Model CD4842 as manufactured by Heatilator.
         1. Unit Front Width: 48 inches (1219 mm).
         2. Framing Front Width: 49 inches (1245 mm).
         3. Unit Back Width: 35-1/2 inches (902 mm).
         4. Framing Back Width: 49 inches (1245 mm).
         5. Unit Height: 41-7/8 inches (1064 mm).
         6. Framing Height: 42-1/8 inches (1070 mm).
         7. Unit Depth: 21 inches (533 mm).
         8. Framing Depth: 22 inches (559 mm).
         9. Glass Size: 42 inches (1067 mm) x 26-1/8 inches (664 mm).
         10. BTU/Hour Input: 35,000 (10.3 kW).
         11. Efficiency: Steady State - 79%, AFUE - 50%, Canada EnerGuide - 48%.

\*\* NOTE TO SPECIFIER \*\* The Rave brings unmatched style to your home or office. Contemporary design elements are highlighted by a long, mesmerizing ribbon flame rising through attractive modern media. Define your room or office with class; let the Rave provide the panache. Delete if not required.

* + 1. Rave Series
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: WSK21.

\*\* NOTE TO SPECIFIER \*\* An added level of function and convenience in a remote control fire fireplaces, stoves, inserts and gas logs with or without line power. Battery-powered or hardwired receiver. Includes: on/off, temperature readout, thermostat mode, timer mode. Delete if not required.

* + - 1. Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Black Deco.
      2. Fronts-Doors: Bronze Deco.
      3. Fronts-Doors: Black Illusion.
      4. Fronts-Doors: Bronze Illusion.

\*\* NOTE TO SPECIFIER \*\* Delete media not required.

* + - 1. Media: Glass Media, Crystal.
      2. Media: Glass Media, Black.
      3. Media: Ceramic Fiber Stones.

\*\* NOTE TO SPECIFIER \*\* Complement your flame with the optional reflective ceramic glass liner that displays exceptional angles of the contemporary ribbon of flames spreading across the length of the firebox. Delete reflective liner if not required.

* + - 1. Reflective Refractory Liner: Reflective Ceramic Glass Liner.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model RAVE3012i as manufactured by Heatilator.
         1. Unit Front Width: 36-3/4 inches (933 mm).
         2. Framing Front Width: 37-3/4 inches (959 mm).
         3. Unit Back Width: 25-3/4 inches (654 mm).
         4. Framing Back Width: 37-3/4 inches (959 mm).
         5. Unit Height: 37 inches (940 mm).
         6. Framing Height: 36-1/2 inches (927 mm).
         7. Unit Depth: 18-5/8 inches (473 mm).
         8. Framing Depth: 18-1/4 inches (464 mm).
         9. Glass Size: 27-1/4 inches x 13-1/4 inches (692 mm x 337 mm).
         10. BTU/Hour Input: 20,000 (5.9 kW).
         11. Efficiency: Steady State - 60.5%, AFUE - 57.37%, Canada EnerGuide - 57.41%.
      2. Model RAVE4013i as manufactured by Heatilator.
         1. Unit Front Width: 48 inches (1219 mm).
         2. Framing Front Width: 50 inches (1270 mm).
         3. Unit Back Width: 37-3/4 inches (959 mm).
         4. Framing Back Width: 50 inches (1270 mm).
         5. Unit Height: 41-3/4 inches (1060 mm).
         6. Framing Height: 42-1/4 inches (1073 mm).
         7. Unit Depth: 18-1/4 inches (464 mm).
         8. Framing Depth: 18-1/4 inches (464 mm).
         9. Glass Size: 39-1/16 inches x 13-1/4 inches (992 mm x 337 mm).
         10. BTU/Hour Input: 26,000 (7.6 kW).
         11. Efficiency: Steady State - 75.3%, AFUE - 59.5%, Canada EnerGuide - 60.6%.

\*\* NOTE TO SPECIFIER \*\* Novus Evolution gas fireplaces blend fashionable style with advanced technology. A minimalist design lets the Evolution's clean lines and contemporary elements shine. Delete if not required.

* + 1. Novus Evolution Series:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: IntelliFire Plus RC100.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: IntelliFire Plus RC200.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: WSK21.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Cinema.
      2. Fronts-Doors: Black FFDEMI Non-operable.
      3. Fronts-Doors: Bronze FFDEMI Non-operable.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article. Kenwood corner not available for this model.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelves Article.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model NEVO3630I as manufactured by Heatilator.
         1. Unit Front Width: 35 inches (889 mm).
         2. Framing Front Width: 36 inches (914 mm).
         3. Unit Back Width: 8-5/8 inches (219 mm).
         4. Framing Back Width: 36 inches (914 mm).
         5. Unit Height: 39-1/8 inches (994 mm).
         6. Framing Height: 39-7/8 inches (1013 mm).
         7. Unit Depth: 19-1/8 inches (486 mm).
         8. Framing Depth: 19-5/8 inches (498 mm).
         9. Glass Size: 30 inches (762 mm) x 22-5/8 inches (575 mm).
         10. BTU/Hour Input: 20,000 (5.9 kW).
         11. Efficiency: Steady State - 82%, AFUE - 70%, Canada EnerGuide - 72%.
      2. Model NEVO4236I as manufactured by Heatilator.
         1. Unit Front Width: 41 inches (1041 mm).
         2. Framing Front Width: 42 inches (1067 mm).
         3. Unit Back Width: 14-5/8 inches (371 mm).
         4. Framing Back Width: 42 inches (1067 mm).
         5. Unit Height: 39-1/8 inches (994 mm).
         6. Framing Height: 39-7/8 inches (1013 mm).
         7. Unit Depth: 19-1/8 inches (486 mm).
         8. Framing Depth: 19-5/8 inches (498 mm).
         9. Glass Size: 36 inches (914 mm) x 22-5/8 inches (575 mm).
         10. BTU/Hour Input: 25,000 (7.3 kW).
         11. Efficiency: Steady State - 81%, AFUE - 69%, Canada EnerGuide - 72%.

\*\* NOTE TO SPECIFIER \*\* Heatilator has expanded the Novus platform, integrating contemporary styling and advanced technology into the Novus nXt gas fireplace. A 69% AFUE rating, 5-step flame height adjustment and smart technology deliver ultimate convenience for this stunning fireplace. Delete if not required.

* + 1. Novus nXt Series:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: IntelliFire Plus RC100.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: IntelliFire Plus RC200.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: IntelliFire Plus RC300.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: WSK21.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Black FFDEMI Non-operable.
      2. Fronts-Doors: Bronze FFDEMI Non-operable.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article. Kenwood corner not available for this model.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelves Article. St. Cloud not available for this model. Delete if not required.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model NNXT3933I as manufactured by Heatilator.
         1. Unit Front Width: 38 inches (965 mm).
         2. Framing Front Width: 39 inches (991 mm).
         3. Unit Back Width: 11-5/8 inches (295 mm).
         4. Framing Back Width: 39 inches (991 mm).
         5. Unit Height: 34 inches (864 mm).
         6. Framing Height: 34-7/8 inches (886 mm).
         7. Unit Depth: 19-1/8 inches (486 mm).
         8. Framing Depth: 19-5/8 inches (498 mm).
         9. Glass Size: 33 inches (838 mm) x 22-5/8 inches (575 mm).
         10. BTU/Hour Input: 29,000 (8.5 kW).
         11. Efficiency: Steady State - 71%, AFUE - 41%, Canada EnerGuide - 48%.
      2. Model NNXT4236I as manufactured by Heatilator.
         1. Unit Front Width: 41 inches (1041 mm).
         2. Framing Front Width: 42 inches (1067 mm).
         3. Unit Back Width: 14-5/8 inches (371 mm).
         4. Framing Back Width: 42 inches (1067 mm).
         5. Unit Height: 34 inches (864mm).
         6. Framing Height: 34-7/8 inches (886 mm).
         7. Unit Depth: 19-1/8 inches (486 mm).
         8. Framing Depth: 19-5/8 inches (498 mm).
         9. Glass Size: 36 inches (914 mm) x 22-5/8 inches (575 mm).
         10. BTU/Hour Input: 31,000 (9.0 kW).
         11. Efficiency: Steady State - 71%, AFUE - 41%, Canada EnerGuide - 48%.

\*\* NOTE TO SPECIFIER \*\* Recreate the timelessness of a wood-burning fire with the open-hearth Reveal. Match your mood and enjoy full, generous flames with the optional doors open or closed. Delete if not required.

* + 1. Reveal Series:
       1. B-Vent Flue Termination.

\*\* NOTE TO SPECIFIER \*\* An added level of function and convenience in a remote control fire fireplaces, stoves, inserts and gas logs with or without line power. Battery-powered or hardwired receiver. Includes: on/off, temperature readout, thermostat mode, timer mode. Control required.

* + - 1. Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: DF421.
      2. Fronts-Doors: Black DM1036.
      3. Fronts-Doors: Stainless steel DM1036.

\*\* NOTE TO SPECIFIER \*\* Delete refractory not required.

* + - 1. Refractory: Herringbone.
      2. Refractory: Traditional.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article. Bella cabinet and Kenwood corner not available for this model.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelves Article. St. Cloud not available for this model.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model RBV4236 as manufactured by Heatilator.
         1. Unit Front Width: 41 inches (1041 mm).
         2. Framing Front Width: 42 inches (1067 mm).
         3. Unit Back Width: 23-3/4 inches (603 mm).
         4. Framing Back Width: 42 inches (1067 mm).
         5. Unit Height: 39-1/2 inches (1003 mm).
         6. Framing Height: 39-3/4 inches (1010 mm).
         7. Unit Depth: 21-1/2 inches (546 mm).
         8. Framing Depth: 22 inches (559 mm).
         9. Glass Size: 36 inches (914 mm).
         10. BTU/Hour Input: 40,000 (11.7 kW).

\*\* NOTE TO SPECIFIER \*\* Contact manufacturer.

* + - * 1. Efficiency:
      1. Model RBV4842 as manufactured by Heatilator.
         1. Unit Front Width: 47 inches (1194 mm).
         2. Framing Front Width: 48 inches (1219 mm).
         3. Unit Back Width: 29-3/4 inches (756 mm).
         4. Framing Back Width: 48 inches (1219 mm).
         5. Unit Height: 39-1/2 inches (1003 mm).
         6. Framing Height: 39-3/4 inches (1010 mm).
         7. Unit Depth: 21-1/2 inches (546 mm).
         8. Framing Depth: 22 inches (559 mm).
         9. Glass Size: 42 inches (1067 mm).
         10. BTU/Hour Input: 43,000 (12.6 kW).

\*\* NOTE TO SPECIFIER \*\* Contact manufacturer.

* + - * 1. Efficiency:

\*\* NOTE TO SPECIFIER \*\* A slim, elegant profile makes the Aveo a perfect fit for condos, bedrooms, studies and other small spaces. It's compact design delivers solid heat, ambiance and fashionable style. Delete if not required.

* + 1. Aveo Series:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: Smart-Batt.

\*\* NOTE TO SPECIFIER \*\* An added level of function and convenience in a remote control fire fireplaces, stoves, inserts and gas logs with or without line power. Battery-powered or hardwired receiver. Includes: on/off, temperature readout, thermostat mode, timer mode. Delete if not required.

* + - 1. Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: WSK21.

\*\* NOTE TO SPECIFIER \*\* This remote control effortlessly manages heat output and comfort level. Includes: hardwired receiver, on/off, fan speed, flame control, temperature readout, thermostat mode, timer mode. Delete if not required.

* + - 1. Controls: RCT-MLT.

\*\* NOTE TO SPECIFIER \*\* Command of both comfort and ambiance. Includes: on/off, fan speed, flame control, pilot activation, auxiliary function, temperature readout, thermostat mode. Delete if not required.

* + - 1. Controls: WSK-MLT Wall Switch.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Black FF-DEMI.
      2. Fronts-Doors: Bronze FF-DEMI.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article. Bella cabinet and Kenwood corner not available for this model.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelves Article. St. Cloud not available for this model. Delete if not required.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model ADVR3428 as manufactured by Heatilator.
         1. Unit Front Width: 28 inches (711 mm).
         2. Framing Front Width: 34 inches (864mm).
         3. Unit Height: 30-1/2 inches (775 mm).
         4. Framing Height: 31-1/4 inches (794 mm).
         5. Unit Depth: 11-1/2 inches (292 mm).
         6. Framing Depth: 12 inches (305 mm).
         7. BTU/Hour Input: 18,000 (5.3 kW).
         8. Efficiency: Steady State - 73%, AFUE - 56%, Canada EnerGuide - 56%.
      2. Model ADVT3428 as manufactured by Heatilator.
         1. Unit Front Width: 28 inches (711 mm).
         2. Framing Front Width: 34 inches (864mm).
         3. Unit Height: 30-1/2 inches (775 mm).
         4. Framing Height: 31-1/4 inches (794 mm).
         5. Unit Depth: 11-1/2 inches (292 mm).
         6. Framing Depth: 12 inches (305 mm).
         7. BTU/Hour Input: 18,000 (5.3 kW).
         8. Efficiency: Steady State - 79%, AFUE - 59%, Canada EnerGuide - 61%.

\*\* NOTE TO SPECIFIER \*\* The Novus is the best-selling gas fireplace of all time. Why? Stylish design elements and robust flamescoupled with the long-lasting performance of Heatilator. Glowing embers, realistic logs and attractive finishing options add character to any space. Delete if not required.

* + 1. Novus Series:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: Smart-Batt.

\*\* NOTE TO SPECIFIER \*\* An added level of function and convenience in a remote control fire fireplaces, stoves, inserts and gas logs with or without line power. Battery-powered or hardwired receiver. Includes: on/off, temperature readout, thermostat mode, timer mode. Delete if not required.

* + - 1. Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: WSK21.

\*\* NOTE TO SPECIFIER \*\* Designed exclusively for fireplaces with IntelliFire™, our state-of-the-art intermittent pilot ignition system. Includes: on/off, auto battery backup, battery strength indicator, fan speed, flame control, pilot activation. Delete if not required.

* + - 1. Controls: WSK200.

\*\* NOTE TO SPECIFIER \*\* This remote control effortlessly manages heat output and comfort level. Includes: hardwired receiver, on/off, fan speed, flame control, temperature readout, thermostat mode, timer mode. Delete if not required.

* + - 1. Controls: RCT-MLT.

\*\* NOTE TO SPECIFIER \*\* Command of both comfort and ambiance. Includes: on/off, fan speed, flame control, pilot activation, auxiliary function, temperature readout, thermostat mode. Delete if not required.

* + - 1. Controls: WSK-MLT Wall Switch.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Demi Front, Non-operable, Black.
      2. Fronts-Doors: Demi Front, Non-operable, Bronze.
      3. Fronts-Doors: Tres Front, Non-operable, Black.
      4. Fronts-Doors: Tres Front, Non-operable, Bronze.
      5. Fronts-Doors: Simon Front, Black.

\*\* NOTE TO SPECIFIER \*\* Refractory required.

* + - 1. Refractory: Traditional.

\*\* NOTE TO SPECIFIER \*\* Select mantel from available in mantels Article. Bella cabinet and Kenwood corner not available for this model.

* + - 1. Wood Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select stone surrounds from available in stone surrounds Article.

* + - 1. Stone Surrounds: As specified.

\*\* NOTE TO SPECIFIER \*\* Select cast mantels from available in cast mantels Article.

* + - 1. Cast Mantels: As specified.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelves Article. Delete if not required.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model NBV3630 as manufactured by Heatilator.
         1. Unit Front Width: 35 inches (889 mm).
         2. Framing Front Width: 36 inches (914 mm).
         3. Unit Back Width: 8-5/8 inches (219 mm).
         4. Framing Back Width: 36 inches (914 mm).
         5. Unit Height: 34-1/2 inches (876 mm).
         6. Framing Height: 34-7/8 inches (886 mm).
         7. Unit Depth: 19-1/8 inches (486 mm).
         8. Framing Depth: 19-5/8 inches (498 mm).
         9. Glass Size: 30 inches (762 mm) x 22-5/8 inches (575 mm).
         10. BTU/Hour Input: 20,000 (5.9 kW).
         11. Efficiency: Steady State - 75%, AFUE - 52%, Canada EnerGuide - 55%.
      2. Model NBV3933 as manufactured by Heatilator.
         1. Unit Front Width: 38 inches (965 mm).
         2. Framing Front Width: 39 inches (991 mm).
         3. Unit Back Width: 11-5/8 inches (295 mm).
         4. Framing Back Width: 39 inches (991 mm).
         5. Unit Height: 34-1/2 inches (876 mm).
         6. Framing Height: 34-7/8 inches (886 mm).
         7. Unit Depth: 19-1/8 inches (486 mm).
         8. Framing Depth: 19-5/8 inches (498 mm).
         9. Glass Size: 33 inches (838 mm) x 22-5/8 inches (575 mm).
         10. BTU/Hour Input: 22,000 (6.4 kW).
         11. Efficiency: Steady State - 78%, AFUE - 48%, Canada EnerGuide - 51%.
      3. Model NBV4236 as manufactured by Heatilator.
         1. Unit Front Width: 41 inches (1041 mm).
         2. Framing Front Width: 42 inches (1067 mm).
         3. Unit Back Width: 14-5/8 inches (371 mm).
         4. Framing Back Width: 42 inches (1067 mm).
         5. Unit Height: 34-1/2 inches (876 mm).
         6. Framing Height: 34-7/8 inches (886 mm).
         7. Unit Depth: 19-1/8 inches (486 mm).
         8. Framing Depth: 19-5/8 inches (498 mm).
         9. Glass Size: 36 inches (914 mm) x 22-5/8 inches (575 mm).
         10. BTU/Hour Input: 25,000 (7.3 kW).
         11. Efficiency: Steady State - 73%, AFUE - 42%, Canada EnerGuide - 54%.
      4. Model NBV4842 as manufactured by Heatilator.
         1. Unit Front Width: 47 inches (1194 mm).
         2. Framing Front Width: 48 inches (1219 mm).
         3. Unit Back Width: 20-5/8 inches (524 mm).
         4. Framing Back Width: 48 inches (1219 mm).
         5. Unit Height: 34-1/2 inches (876 mm).
         6. Framing Height: 34-7/8 inches (886 mm).
         7. Unit Depth: 19-1/8 inches (486 mm).
         8. Framing Depth: 19-5/8 inches (498 mm).
         9. Glass Size: 42 inches (1067 mm) x 22-5/8 inches (575 mm).
         10. BTU/Hour Input: 30,000 (8.8 kW).
         11. Efficiency: Steady State - 77%, AFUE - 56%, Canada EnerGuide - 58%.
      5. Model NDV3630 as manufactured by Heatilator.
         1. Unit Front Width: 35 inches (889 mm).
         2. Framing Front Width: 36 inches (914 mm).
         3. Unit Back Width: 8-5/8 inches (219 mm).
         4. Framing Back Width: 36 inches (914 mm).
         5. Unit Height: 34-1/2 inches (876 mm).
         6. Framing Height: 34-7/8 inches (886 mm).
         7. Unit Depth: 19-1/8 inches (486 mm).
         8. Framing Depth: 19-5/8 inches (498 mm).
         9. Glass Size: 30 inches (762 mm) x 22-5/8 inches (575 mm).
         10. BTU/Hour Input: 20,000 (5.9 kW).
         11. Efficiency: Steady State - 75%, AFUE - 52%, Canada EnerGuide - 55%.
      6. Model NDV3933 as manufactured by Heatilator.
         1. Unit Front Width: 38 inches (965 mm).
         2. Framing Front Width: 39 inches (991 mm).
         3. Unit Back Width: 11-5/8 inches (295 mm).
         4. Framing Back Width: 39 inches (991 mm).
         5. Unit Height: 34-1/2 inches (876 mm).
         6. Framing Height: 34-7/8 inches (886 mm).
         7. Unit Depth: 19-1/8 inches (486 mm).
         8. Framing Depth: 19-5/8 inches (498 mm).
         9. Glass Size: 33 inches (838 mm) x 22-5/8 inches (575 mm).
         10. BTU/Hour Input: 22,000 (6.4 kW).
         11. Efficiency: Steady State - 78%, AFUE - 48%, Canada EnerGuide - 51%.
      7. Model NDV4236 as manufactured by Heatilator.
         1. Unit Front Width: 41 inches (1041 mm).
         2. Framing Front Width: 42 inches (1067 mm).
         3. Unit Back Width: 14-5/8 inches (371 mm).
         4. Framing Back Width: 42 inches (1067 mm).
         5. Unit Height: 34-1/2 inches (876 mm).
         6. Framing Height: 34-7/8 inches (886 mm).
         7. Unit Depth: 19-1/8 inches (486 mm).
         8. Framing Depth: 19-5/8 inches (498 mm).
         9. Glass Size: 36 inches (914 mm) x 22-5/8 inches (575 mm).
         10. BTU/Hour Input: 25,000 (7.3 kW).
         11. Efficiency: Steady State - 73%, AFUE - 42%, Canada EnerGuide - 54%.
      8. Model NDV4842 as manufactured by Heatilator.
         1. Unit Front Width: 47
         2. Framing Front Width: 48 inches (1219 mm).
         3. Unit Back Width: 20-5/8 inches (524 mm).
         4. Framing Back Width: 48 inches (1219 mm).
         5. Unit Height: 34-1/2 inches (876 mm).
         6. Framing Height: 34-7/8 inches (886 mm).
         7. Unit Depth: 19-1/8 inches (486 mm).
         8. Framing Depth: 19-5/8 inches (498 mm).
         9. Glass Size: 42 inches (1067 mm) x 22-5/8 inches (575 mm).
         10. BTU/Hour Input: 30,000 (8.8 kW).
         11. Efficiency: Steady State - 77%, AFUE - 56%, Canada EnerGuide - 58%.

\*\* NOTE TO SPECIFIER \*\* new series to be introduced.

* + 1. Crave Single Sided (SS) Series:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Delete control options not required.

* + - 1. Controls: IntelliFire Plus RC300 (Standard).
      2. Controls: IntelliFire RC200.
      3. Controls: IntelliFire Plus RC100.
      4. Safety Screen.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts - Clean Face Trim, Black.
      2. Fronts - Clean Face Trim, Bronze.
      3. Fronts - Four Square Front, Black.
      4. Fronts - Four Square Front, Bronze.
      5. Fronts - Illusion Front, Black.
      6. Fronts - Illusion Front, Bronze.

\*\* NOTE TO SPECIFIER \*\* Delete media options not required.

* + - 1. Media: Glass Media, Clear.
      2. Media: Glass Media, Ebony.
      3. Media: Glass Media, Amber.
      4. Media: Glass Media, Cobalt.
      5. Media Glass Media, Red.
      6. Media: Natural Log Set (Requires Glass Media).

\*\* NOTE TO SPECIFIER \*\* Delete models not required.

* + - 1. Model Crave4836 as manufactured by Heatilator.
         1. Unit Front Width: 46-3/16 inches (1173 mm).
         2. Framing Front Width: 48-1/4 inches (1226 mm).
         3. Unit Back Width: 46-3/16 inches (1173 mm).
         4. Framing Back Width: 48-1/4 inches (1226 mm).
         5. Unit Height: 41-3/4 inches (1060 mm).
         6. Framing Height: 42 inches (1067 mm).
         7. Unit Depth: 17-1/8 inches (435 mm).
         8. Framing Depth: 18-1/4 inches (464 mm).
         9. Glass Size: 35-1/2 inches (902 mm) x 12-1/2 inches (318 mm).
         10. BTU/Hour Input: 30,000 (8.8 kW).
      2. Model Crave6048 as manufactured by Heatilator.
         1. Unit Front Width: 58 inches (1473 mm).
         2. Framing Front Width: 60-1/4 inches (1530 mm).
         3. Unit Back Width: 58 inches (1473 mm).
         4. Framing Back Width: 60-1/4 inches (1530 mm).
         5. Unit Height: 41-3/4 inches (1060 mm).
         6. Framing Height: 42 inches (1067 mm).
         7. Unit Depth: 17-1/8 inches (435 mm).
         8. Framing Depth: 18-1/4 inches (464 mm).
         9. Glass Size: 47-1/2 inches (1206 mm) x 12-1/2 inches (318 mm).
         10. BTU/Hour Input: 40,000 (11.7 kW).
      3. Model Crave7260 as manufactured by Heatilator.
         1. Unit Front Width: 70 inches (1778 mm).
         2. Framing Front Width: 72-1/4 inches (1835 mm).
         3. Unit Back Width: 70 inches (1778 mm).
         4. Framing Back Width: 72-1/4 inches (1835 mm).
         5. Unit Height: 47-3/4 inches (1213 mm).
         6. Framing Height: 48 inches (1219 mm).
         7. Unit Depth: 17-1/8 inches (435 mm).
         8. Framing Depth: 18-1/4 inches (464 mm).
         9. Glass Size: 59-1/2 inches (1511 mm) x 12-1/2 inches (318 mm).
         10. BTU/Hour Input: 50,000 (14.7 kW).
      4. Model Crave8472 as manufactured by Heatilator.
         1. Unit Front Width: 82 inches (2083 mm).
         2. Framing Front Width: 84-1/4 inches (2140 mm).
         3. Unit Back Width: 82 inches (2083 mm).
         4. Framing Back Width: 84-1/4 inches (2140 mm).
         5. Unit Height: 47-3/4 inches (1213 mm).
         6. Framing Height: 48 inches (1219 mm).
         7. Unit Depth: 17-1/8 inches (435 mm).
         8. Framing Depth: 18-1/4 inches (464 mm).
         9. Glass Size: 71-1/2 inches (1816 mm) x 12-1/2 inches (318 mm).
         10. BTU/Hour Input: 58,000 (17.0 kW).

\*\* NOTE TO SPECIFIER \*\* new series to be introduced.

* + 1. Crave See Through (ST) Series:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Delete control options not required.

* + - 1. Controls: IntelliFire Plus RC300 (Standard).
      2. Controls: IntelliFire RC200.
      3. Controls: IntelliFire Plus RC100.
      4. Safety Screen.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts: Clean Face Trim, Black.
      2. Fronts: Clean Face Trim, Bronze.
      3. Fronts: Four Square Front, Black.
      4. Fronts: Four Square Front, Bronze.
      5. Fronts: Illusion Front, Black.
      6. Fronts: Illusion Front, Bronze.

\*\* NOTE TO SPECIFIER \*\* Delete media options not required.

* + - 1. Media: Glass Media, Clear.
      2. Media: Glass Media, Ebony.
      3. Media: Glass Media, Amber.
      4. Media: Glass Media, Cobalt.
      5. Media Glass Media, Red.
      6. Media: Natural Log Set (Requires Glass Media).

\*\* NOTE TO SPECIFIER \*\* Delete models not required.

* + - 1. Model Crave4836ST as manufactured by Heatilator.
         1. Unit Front Width: 46-3/16 inches (1173 mm).
         2. Framing Front Width: 48-1/4 inches (1226 mm).
         3. Unit Back Width: 46-3/16 inches (1173 mm).
         4. Framing Back Width: 48-1/4 inches (1226 mm).
         5. Unit Height: 41-3/4 inches (1060 mm).
         6. Framing Height: 42 inches (1067 mm).
         7. Unit Depth: 17-1/8 inches (435 mm).
         8. Framing Depth: 17 inches (432 mm).
         9. Glass Size: 35-1/2 inches (902 mm) x 12-1/2 inches (318 mm).
         10. BTU/Hour Input: 30,000 (8.8 kW).
      2. Model Crave6048ST as manufactured by Heatilator.
         1. Unit Front Width: 58 inches (1473 mm).
         2. Framing Front Width: 60-1/4 inches (1530 mm).
         3. Unit Back Width: 58 inches (1473 mm).
         4. Framing Back Width: 60-1/4 inches (1530 mm).
         5. Unit Height: 41-3/4 inches (1060 mm).
         6. Framing Height: 42 inches (1067 mm).
         7. Unit Depth: 17-1/8 inches (435 mm).
         8. Framing Depth: 17 inches (432 mm).
         9. Glass Size: 47-1/2 inches (1206 mm) x 12-1/2 inches (318 mm).
         10. BTU/Hour Input: 40,000 (11.7 kW).
      3. Model Crave7260ST as manufactured by Heatilator.
         1. Unit Front Width: 70 inches (1778 mm).
         2. Framing Front Width: 72-1/4 inches (1835 mm).
         3. Unit Back Width: 70 inches (1778 mm).
         4. Framing Back Width: 72-1/4 inches (1835 mm).
         5. Unit Height: 47-3/4 inches (1213 mm).
         6. Framing Height: 48 inches (1219 mm).
         7. Unit Depth: 17-1/8 inches (435 mm).
         8. Framing Depth: 17 inches (432 mm).
         9. Glass Size: 59-1/2 inches (1511 mm) x 12-1/2 inches (318 mm).
         10. BTU/Hour Input: 50,000 (14.7 kW).
      4. Model Crave8472ST as manufactured by Heatilator.
         1. Unit Front Width: 82 inches (2083 mm).
         2. Framing Front Width: 84-1/4 inches (2140 mm).
         3. Unit Back Width: 82 inches (2083 mm).
         4. Framing Back Width: 84-1/4 inches (2140 mm).
         5. Unit Height: 47-3/4 inches (1213 mm).
         6. Framing Height: 48 inches (1219 mm).
         7. Unit Depth: 17-1/8 inches (435 mm).
         8. Framing Depth: 17 inches (432 mm).
         9. Glass Size: 71-1/2 inches (1816 mm) x 12-1/2 inches (318 mm).
         10. BTU/Hour Input: 58,000 (17.0 kW).

\*\* NOTE TO SPECIFIER \*\* The Eclipse brings functional modern design into smaller spaces. These compact gas burning fireplaces fit in a much wider variety of spaces, and combined with a large selection of finishing options, provide unmatched versatility. A ribbon burner elevates the flames through finely crafted ceramic stones. Delete if not required.

* + 1. Eclipse Series Gas Fireplace:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Delete control options not required.

* + - 1. Controls:WSK21.
      2. Controls: Smart Stat.

\*\* NOTE TO SPECIFIER \*\* Delete front door style and finish not required.

* + - 1. Fronts-Doors: Clean Face Front.
      2. Fronts-Doors: Simon Front.

\*\* NOTE TO SPECIFIER \*\* Delete refractory if not required.

* + - 1. Refractory: Black Glass Liner.

\*\* NOTE TO SPECIFIER \*\* Delete media options not required.

* + - 1. Media: Crushed Glass, Ebony.
      2. Media: Crushed Glass, Amber.
      3. Media: Crushed Glass, Cobalt.
      4. Media: Glass Beads, Black.
      5. Media: Glass Beads, White.
      6. Media: Glass Beads, Clear.
      7. Media: Ceramic Fiber Stones.

\*\* NOTE TO SPECIFIER \*\* Delete models not required.

* + - 1. Model Eclipse 32 as manufactured by Heatilator.
         1. Unit Front Width: 36 inches (914 mm).
         2. Framing Front Width: 37 inches (940 mm).
         3. Unit Back Width: 25-3/4 inches (654 mm).
         4. Framing Back Width: 37 inches (940 mm).
         5. Unit Height: 34-3/8 inches (873 mm).
         6. Framing Height: 34-3/4 inches (883 mm).
         7. Unit Depth: 15-7/8 inches (403 mm).
         8. Framing Depth: 16-1/4 inches (413mm).
         9. Glass Size: 27-3/16 inches (691 mm) x 18-1/16 inches (459 mm).
         10. BTU/Hour Input: 17,500 (5.1 kW).
      2. Model Eclipse 36 as manufactured by Heatilator.
         1. Unit Front Width: 41 inches (1041 mm).
         2. Framing Front Width: 42 inches (1067 mm).
         3. Unit Back Width: 30-3/4 inches (781 mm).
         4. Framing Back Width: 42 inches (1067 mm).
         5. Unit Height: 37-7/8 inches (962 mm).
         6. Framing Height: 38-1/4 inches (972 mm).
         7. Unit Depth: 15-7/8 inches (403 mm).
         8. Framing Depth: 16-1/4 inches (413mm).
         9. Glass Size: 32-1/16 inches (814 mm) x 21-1/2 inches (546 mm).
         10. BTU/Hour Input: 23,500 (6.9 kW).

\*\* NOTE TO SPECIFIER \*\* Take modern style to new places with the Ion gas fireplace series. At only 7-inches deep, these square, vertical and horizontal models can install in nearly any roomquicker and easier than other fireplaces. The Ion series of shallow gas fireplaces offer two front choices and an ambient backlighting option create a truly unique look in any environment. Delete if not required.

* + 1. Ion Series Gas Fireplace:
       1. Direct Vent: 100% of combustion exhaust and fumes are removed.

\*\* NOTE TO SPECIFIER \*\* Delete control options not required.

* + - 1. Controls: RC200 IntelliFire Touch.
      2. Controls: RC100 IntelliFire Touch
      3. Controls: RC300 IntelliFire Touch.

\*\* NOTE TO SPECIFIER \*\* Delete front door style if not required.

* + - 1. Fronts-Doors: Four Square Front.

\*\* NOTE TO SPECIFIER \*\* Delete refractory if not required.

* + - 1. Refractory: Black Glass Liner.
      2. LED Backlighting.

\*\* NOTE TO SPECIFIER \*\* Delete models not required.

* + - 1. Model Ion V7 as manufactured by Heatilator.
         1. Unit Front Width: 19-1/4 inches (489 mm).
         2. Framing Front Width: 20-1/8 inches (511 mm).
         3. Unit Back Width: 19-1/4 inches (489 mm).
         4. Framing Back Width: 20-1/8 inches (511 mm).
         5. Unit Height: 36-1/8 inches (918 mm).
         6. Framing Height: 43-1/8 inches (1095 mm).
         7. Unit Depth: 6-3/8 inches (162 mm).
         8. Framing Depth: 2-5/8 inches (67 mm).
         9. Glass Size: 12 inches (305 mm) x 24 inches (610 mm).
         10. BTU/Hour Input: 14,250 (4.2 kW).
      2. Model Ion S7 as manufactured by Heatilator.
         1. Unit Front Width: 28-1/2 inches (724 mm).
         2. Framing Front Width: 29-3/8 inches (746 mm).
         3. Unit Back Width: 28-1/2 inches (724 mm).
         4. Framing Back Width: 29-3/8 inches (746 mm).
         5. Unit Height: 33-5/8 inches (854 mm).
         6. Framing Height: 40-1/2 inches (1029 mm).
         7. Unit Depth: 6-3/8 inches (162 mm).
         8. Framing Depth: 2-5/8 inches (67 mm).
         9. Glass Size: 21-1/8 inches (537 mm) x 21-3/8 inches (543 mm).
         10. BTU/Hour Input: 18,800 (5.5 kW).
      3. Model Ion H7 as manufactured by Heatilator.
         1. Unit Front Width: 38-1/4 inches (972 mm).
         2. Framing Front Width: 39-3/8 inches (1000 mm).
         3. Unit Back Width: 38-1/4 inches (972 mm).
         4. Framing Back Width: 39-3/8 inches (1000 mm).
         5. Unit Height: 29-1/8 inches (740 mm).
         6. Framing Height: 9 inches (229 mm).
         7. Unit Depth: 6-3/8 inches (162 mm).
         8. Framing Depth: 2-5/8 inches (67 mm).
         9. Glass Size: 31 inches (787 mm) x 17 inches (432 mm).
         10. BTU/Hour Input: 24,000 (7.0 kW).

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* 1. MANUFACTURED OUTDOOR GAS FIREPLACES

\*\* NOTE TO SPECIFIER \*\* Bolster your favorite room and upgrade your outdoor living space. The Twilight Modern is an evolution of the industry's first indoor/outdoor see-through fireplace, and delivers impressive fireside views whether relaxing inside or socializing outside. No chimney or venting required. Delete if not required.

* + 1. Twilight Modern Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Controls: WSK21

\*\* NOTE TO SPECIFIER \*\* An added level of function and convenience in a remote control fire fireplaces, stoves, inserts and gas logs with or without line power. Battery-powered or hardwired receiver. Includes: on/off, temperature readout, thermostat mode, timer mode. Delete if not required.

* + - 1. Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete front-door style and finish not required.

* + - 1. Fronts-Doors: Black Basic Front.
      2. Fronts-Doors: Black Contemporary front with built-in, overlapping surround.
      3. Fronts-Doors: Fog Contemporary front with built-in, overlapping surround.

\*\* NOTE TO SPECIFIER \*\* Delete media not required.

* + - 1. Media: Glass Media, Crystal.
      2. Media: Glass Media, Black.
      3. Media: Glass Media, Amber.
      4. Model TWILIGHT-II-MOD as manufactured by Heatilator.
         1. Unit Front Width: 43 inches (1092 mm).
         2. Framing Front Width: 44 inches (1118 mm).
         3. Unit Back Width: 43 inches (1092 mm).
         4. Framing Back Width: 44 inches (1118 mm).
         5. Unit Height - In: 40-3/4 inches (1035 mm).
         6. Unit Height - Out: 46-7/8 inches (1191 mm).
         7. Framing Height - In: 41-1/4 inches (1048 mm).
         8. Framing Height - Out: 47-5/8 inches (1210 mm).
         9. Unit Depth: 24 inches (610 mm).
         10. Framing Depth: 23 inches (584 mm).
         11. Glass Size: 35-5/8 inches (905 mm) x 21-1/2 inches (546 mm).
         12. BTU/Hour Input: 38,000 NG (11.1 kW).

\*\* NOTE TO SPECIFIER \*\* Add warmth and beauty to two spaceswith one fireplace. The Twilight II is the world's first see-thru indoor/outdoor gas fireplace. Enjoy the fire all year long, and from either side. An advanced design exceeds both window and gas fireplace standards, and rugged construction ensures impressive, consistent performance. Delete if not required.

* + 1. Twilight II Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Designed exclusively for fireplaces with IntelliFire™, our state-of-the-art intermittent pilot ignition system. Includes: on/off, auto battery backup, battery strength indicator, fan speed, flame control, pilot activation. Delete if not required.

* + - 1. Controls: WSK200.

\*\* NOTE TO SPECIFIER \*\* An added level of function and convenience in a remote control fire fireplaces, stoves, inserts and gas logs with or without line power. Battery-powered or hardwired receiver. Includes: on/off, temperature readout, thermostat mode, timer mode. Delete if not required.

* + - 1. Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete front-door style and finish not required.

* + - 1. Fronts-Doors: Black Basic Front.
      2. Fronts-Doors: Black Contemporary front with built-in, overlapping surround.
      3. Fronts-Doors: Fog Contemporary front with built-in, overlapping surround.
      4. Model TWILIGHTII as manufactured by Heatilator.
         1. Unit Front Width: 43 inches (1092 mm).
         2. Framing Front Width: 44 inches (1118 mm).
         3. Unit Back Width: 43 inches (1092 mm).
         4. Framing Back Width: 44 inches (1118 mm).
         5. Unit Height - In: 40-3/4 inches (1035 mm).
         6. Unit Height - Out: 46-7/8 inches (1191 mm).
         7. Framing Height - In: 41-1/4 inches (1048 mm).
         8. Framing Height - Out: 47-5/8 inches (1210 mm).
         9. Unit Depth: 24 inches (610 mm).
         10. Framing Depth: 23 inches (584 mm).
         11. Glass Size: 35-5/8 inches (905 mm) x 21-1/2 inches (546 mm).
         12. BTU/Hour Input: 38,000 NG (11.1 kW).

\*\* NOTE TO SPECIFIER \*\* The Dakota artfully blends style, function and utility with outdoor living. A rugged design loaded with advanced technology make the Dakota an enticing outdoor fireplace for years to come. Delete if not required.

* + 1. Dakota Gas Fireplace:
       1. Stainless steel construction.

\*\* NOTE TO SPECIFIER \*\* Delete Refractory design not required.

* + - 1. Refractory: Traditional Refractory.
      2. Refractory: Herringbone Refractory.
      3. Model Dakota as manufactured by Heatilator.
         1. Unit Front Width: 48 inches (1219 mm).
         2. Framing Front Width: 49 inches (1245 mm).
         3. Unit Back Width: 31 inches (787 mm).
         4. Framing Back Width: 49 inches (1245 mm).
         5. Unit Height: 40 inches (1016 mm).
         6. Framing Height: 43-7/8 inches (1114 mm).
         7. Unit Depth: 23-1/4 inches (591 mm).
         8. Framing Depth: 24-1/8 inches (613 mm).
         9. Glass Size: 26-13/16 inches (681 mm) x 42-1/2 inches (1080 mm).
         10. BTU/Hour Input: 60,000 (17.6 kW).

\*\* NOTE TO SPECIFIER \*\* The Carolina's compact footprint offers versatile installation opportunities. And, this attractive unit is packed with advanced technology, like the IntelliFire™ Plus auto-ignition system and Fire Brick technology for up to 25% more radiant heat. Extend your summer season with style. Bring the Carolina home. Delete if not required.

* + 1. Carolina:

\*\* NOTE TO SPECIFIER \*\* Designed exclusively for fireplaces with IntelliFire™, our state-of-the-art intermittent pilot ignition system. Features a simple, single mode function and is specifically designed for wall placement ensuring a great fire is just a tap of the switch away. Delete if not required.

* + - 1. Controls: IntelliFire Plus RC100.

\*\* NOTE TO SPECIFIER \*\* Combines an easy-to-use and intuitive control panel with a stylish and ergonomic design. Since it utilizes wireless control, it has the flexibility for wall placement anywhere in the room, or use as a remote only. Auto Battery Backup, Pilot Activation, On/Off, 5 Step Flame Height, Fan Speed, Child Lock, Wall Docking Station. Delete if not required.

* + - 1. Controls: IntelliFire Plus RC200.

\*\* NOTE TO SPECIFIER \*\* Delete front-door style if not required.

* + - 1. Fronts-Doors: DSCAR3642 Front.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model CAROLINA-36 as manufactured by Heatilator.
         1. Unit Front Width: 44 inches (1118 mm).
         2. Framing Front Width: 48 inches (1219 mm).
         3. Unit Back Width: 44 inches (1118 mm).
         4. Framing Back Width: 48 inches (1219 mm).
         5. Unit Height: 42-1/2 inches (1080 mm).
         6. Framing Height: 42-1/2 inches (1080 mm).
         7. Unit Depth: 17 inches (432 mm).
         8. Framing Depth: 17 inches (432 mm).
         9. Glass Size: 33-3/8 inches (848 mm) x 28-7/8 inches (733 mm).
         10. BTU/Hour Input: 55,000 (16.1 kW).
      2. Model CAROLINA-42 as manufactured by Heatilator.
         1. Unit Front Width: 50 inches (1270 mm).
         2. Framing Front Width: 54 inches (1372 mm).
         3. Unit Back Width: 50 inches (1270 mm).
         4. Framing Back Width: 54 inches (1372 mm).
         5. Unit Height: 50-1/2 inches (1283 mm).
         6. Framing Height: 50-1/2 inches (1283 mm).
         7. Unit Depth: 17 inches (432 mm).
         8. Framing Depth: 17 inches (432 mm).
         9. Glass Size: 39-1/8 inches (994 mm) x 33-3/4 inches (857 mm).
         10. BTU/Hour Input: 65,000 (19 kW).

\*\* NOTE TO SPECIFIER \*\* The Villa Gas is a versatile outdoor gas fireplace at a value price. This compact unit can easily be installed on decks or patios. A stainless steel surround withstands the elements, and complements an outdoor kitchen or contemporary living space. Delete if not required.

* + 1. Outdoor Lifestyles Villa Gas Fireplace:

\*\* NOTE TO SPECIFIER \*\* Delete Fronts-doors if not required.

* + - 1. Front-Door: Stainless Steel Operable Doors.

\*\* NOTE TO SPECIFIER \*\* Delete Refractory design not required.

* + - 1. Refractory: Traditional Refractory.
      2. Refractory: Herringbone Refractory.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model VILLA Gas-36 as manufactured by Heatilator.
         1. Unit Front Width: 41 inches (1041 mm).
         2. Framing Front Width: 42 inches (1067 mm).
         3. Unit Back Width: 23-3/4 inches (603 mm).
         4. Framing Back Width: 42 inches (1067 mm).
         5. Unit Height: 39-1/2 inches (1003 mm).
         6. Framing Height: 39-3/4 inches (1010 mm).
         7. Unit Depth: 21-3/8 inches (543 mm).
         8. Framing Depth: 21-1/2 inches (546 mm).
         9. Viewing Area: 36 inches (914 mm) x 20-7/8 inches (530 mm).
         10. BTU/Hour Input: 40,000 (11.7 kW).
      2. Model VILLA Gas-42 as manufactured by Heatilator.
         1. Unit Front Width: 47 inches (1194 mm).
         2. Framing Front Width: 48 inches (1219 mm).
         3. Unit Back Width: 29-3/4 inches (756 mm).
         4. Framing Back Width: 48 inches (1219 mm).
         5. Unit Height: 39-1/2 inches (1003 mm).
         6. Framing Height: 39-3/4 inches (1010 mm).
         7. Unit Depth: 21-3/8 inches (543 mm).
         8. Framing Depth: 21-1/2 inches (546 mm).
         9. Glass Size: 42 inches (1067 mm) x 20-7/8 inches (530 mm).
         10. BTU/Hour Input: 42,000 (12.3 kW).

\*\* NOTE TO SPECIFIER \*\* The Palazzo See-through is a new kind of outdoor fireplacea linear design with a clean look that provides a contemporary focal point in an outdoor setting. This eye-catching fireplace is tough, built with marine-grade stainless steel that is rust-resistant even in the harshest conditions. A tempered glass wind guard keeps the flames full and lively, while an industry-first Power Screen provides safety.   
The contemporary Palazzo outdoor linear model in a single sided configuration. Perfect for residential and commercial projects calling for a unique focal point for an outdoor living space or meeting area.  
Delete if not required.

* + 1. Outdoor Lifestyles Palazzo Series Modern Fireplace:
       1. Power Screen (Comes Standard).
       2. LED Lighting.

\*\* NOTE TO SPECIFIER \*\* Delete media options not required.

* + - 1. Media: Glass Media, Crystal.
      2. Media: Glass Media, Cobalt.
      3. Media: Glass Media, Ebony.
      4. Media: Glass Media, Scarlet.
      5. Media: Glass Media, Amber.

\*\* NOTE TO SPECIFIER \*\* Delete models not required.

* + - 1. Model Palazzo Single Sided as manufactured by Heatilator.
         1. Unit Front Width: 59-7/8 inches (1521 mm).
         2. Framing Front Width: 60 inches (1524 mm).
         3. Unit Back Width: 59-7/8 inches (1521 mm).
         4. Framing Back Width: 60 inches (1524 mm).
         5. Unit Height: 45-1/2 inches (1156 mm).
         6. Framing Height: 62-3/8 inches (1584 mm).
         7. Unit Depth: 18-5/8 inches (473 mm).
         8. Framing Depth: 18-1/8 inches (460 mm).
         9. Glass Size: 48 inches (1219 mm) x 13-7/8 inches (352 mm).
         10. BTU/Hour Input: 43,000 (12.6 kW).
      2. Model Palazzo See-Through as manufactured by Heatilator.
         1. Unit Front Width: 59-7/8 inches (1521 mm).
         2. Framing Front Width: 60 inches (1524 mm).
         3. Unit Back Width: 59-7/8 inches (1521 mm).
         4. Framing Back Width: 60 inches (1524 mm).
         5. Unit Height: 45-1/2 inches (1156 mm).
         6. Framing Height: 62-3/8 inches (1584 mm).
         7. Unit Depth: 18-1/4 inches (464 mm).
         8. Framing Depth: 17 inches (432 mm).
         9. Glass Size: 48 inches (1219 mm) x 13-7/8 inches (352 mm).
         10. BTU/Hour Input: 43,000 (12.6 kW).

\*\* NOTE TO SPECIFIER \*\* Gas fireplace inserts provide convenience and consistency when it comes to indoor air quality. Add an insert to your existing fireplace to achieve a more efficient, cleaner burn. Delete if not required.

* 1. INDOOR GAS LOG SETS

\*\* NOTE TO SPECIFIER \*\* Specifically designed to fill larger fireplaces, this winner of the 2005 Vesta Award for Best Gas Log Set easily fills generous hearths. 11 authentic looking logs, molded from real oak timber (12 logs on three-tiered 30 inches (762 mm)), state-of-the-art, tiered burner system creates a multi-level fire. Hidden controls are easily accessible, won't detract from the fire's authenticity, and allow the log set to fit perfectly centered. Offers three types of burners: Matchlight (NG only), Safety Pilot, and IntelliFire. Includes burner and hearth kit. Delete if not required.

* + 1. Fireside Grand Oak:
       1. Designed to fill larger fireplaces. 11 authentic looking logs, molded from real oak timber (12 logs on three-tiered 30 inches (762 mm)), state-of-the-art, tiered burner system creates a multi-level fire. Hidden controls are easily accessible, won't detract from the fire's authenticity, and allow the log set to fit perfectly centered.

\*\* NOTE TO SPECIFIER \*\* Delete burner not required.

* + - 1. Burner: Matchlight (NG only).
      2. Burner: Safety Pilot.
      3. Burner: IntelliFire.
      4. Include burner and hearth kit.

\*\* NOTE TO SPECIFIER \*\* An added level of function and convenience in a remote control fire fireplaces, stoves, inserts and gas logs with or without line power. Battery-powered or hardwired receiver. Includes: on/off, temperature readout, thermostat mode, timer mode. Delete remote control if not required.

* + - 1. Remote Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Recreates the natural look of a traditional campfire. Front log conceals and insulates the controls so that the log set can burn with fireplace doors closed. 18" and 24 inches (610 mm)." sets have 10 fiber logs, 30 inches (762 mm) set has 11 fiber logs. 24 inches (610 mm)." see-through version has 13 fiber logs to accommodate multi-sided fireplaces. Offers one type of burner: Remote Ready. Includes burner and hearth kit. Delete if not required.

* + 1. Campfire:
       1. Recreates the natural look of a traditional campfire. Front log conceals and insulates the controls so that the log set can burn with fireplace doors closed.

\*\* NOTE TO SPECIFIER \*\* Delete log set not required.

* + - 1. Log Set: 18 inches (457 mm) sets have 10 fiber logs.
      2. Log Set: 24 inches (610 mm) sets have 10 fiber logs.
      3. Log Set: 30 inches (762 mm) set has 11 fiber logs.
      4. Log Set: 24 inches (610 mm) "see-through" version has 13 fiber logs to accommodate multi-sided fireplaces.
      5. Remote Ready.
      6. Includes burner and hearth kit.

\*\* NOTE TO SPECIFIER \*\* Realistically detailed logs with the appeal of a fully charred, mature fire. 12 authentic-looking logs, molded from real oak timber and works with two types of burners: Matchlight (NG only) and Remote-Ready Standing Pilot. Hearth kit/burner sold separately. Delete if not required.

* + 1. Fireside Supreme Oak:
       1. Realistically detailed logs with the appeal of a fully charred, mature fire. 12 authentic-looking logs, molded from real oak timber.

\*\* NOTE TO SPECIFIER \*\* Hearth kit sold separately. Refer to manufacturer's literature for hearth designs available for the model. Delete if not required.

* + - 1. Hearth Kit:

\*\* NOTE TO SPECIFIER \*\* Burner sold separately. Delete burner not required.

* + - 1. Burner: Matchlight (NG only).
      2. Burner: Remote-Ready Standing Pilot.

\*\* NOTE TO SPECIFIER \*\* Ingenious design provides two different looks: split log or full bark - just turn the front logs around. The split log side gives you another option and a new flame experience. 11 authentic-looking logs, molded from real oak timber and works with two types of burners: Matchlight (NG only) and Remote-Ready Standing Pilot. Delete if not required.

* + 1. Fireside Versawood:
       1. Ingenious design provides two different looks: split log or full bark - just turn the front logs around. The split log side gives you another option and a new flame experience. 11 authentic-looking logs, molded from real oak timber.

\*\* NOTE TO SPECIFIER \*\* Delete burner not required.

* + - 1. Burner: Matchlight (NG only).
      2. Burner: Remote-Ready Standing Pilot.

\*\* NOTE TO SPECIFIER \*\* A good look at a great value! Eight richly-detailed logs and works with two types of burners: Matchlight (NG only) and Remote-Ready Standing Pilot. Hearth kit/burner sold separately. Delete if not required.

* + 1. Fireside Realwood:
       1. Eight richly-detailed logs.

\*\* NOTE TO SPECIFIER \*\* Delete burner not required.

* + - 1. Burner: Matchlight (NG only).
      2. Burner: Remote-Ready Standing Pilot.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* 1. INDOOR GAS FIREPLACE INSERTS
     1. NDI:
        1. Bold flames rise through hand-detailed log set.

\*\* NOTE TO SPECIFIER \*\* This remote control effortlessly manages heat output and comfort level. Includes: hardwired receiver, on/off, fan speed, flame control, temperature readout, thermostat mode, timer mode. Delete control not required.

* + - 1. Controls: RCT-MLT.

\*\* NOTE TO SPECIFIER \*\* An added level of function and convenience in a remote control fire fireplaces, stoves, inserts and gas logs with or without line power. Battery-powered or hardwired receiver. Includes: on/off, temperature readout, thermostat mode, timer mode. Delete control not required.

* + - 1. Controls: Smart-Stat.

\*\* NOTE TO SPECIFIER \*\* Delete control not required.

* + - 1. Controls: Smart-Batt.

\*\* NOTE TO SPECIFIER \*\* Delete fronts-doors if not required.

* + - 1. Front-Door: Black Cabinet.
      2. Front-Door: Bronze Cabinet.
      3. Front-Door: Black Firescreen.
      4. Front-Door: Bronze Firescreen.

\*\* NOTE TO SPECIFIER \*\* An optional steel refractory kit is available to change the look of the firebox. Delete steel refractory if not required.

* + - 1. Refractory: Steel refractory.

\*\* NOTE TO SPECIFIER \*\* A surround, available in various sizes, is required to fill the gap between the insert and the firebox opening. Delete surround if not required.

* + - 1. Front-Door: Black Gas Insert Surrounds.
      2. Front-Door: Bronze Gas Insert Surrounds.

\*\* NOTE TO SPECIFIER \*\* A termination cap finishes your gas insert with a clean, upscale look. And, these durable caps also protect venting components and ensure safe exhaust flow. Delete if not required.

* + - 1. Termination: Copper Square Termination Cap.
      2. Termination: Black Square Termination Cap.
      3. Termination: Stainless Steel Round Termination Cap.

\*\* NOTE TO SPECIFIER \*\* Select mantel shelves from available in mantel shelves Article.

* + - 1. Mantel Shelf: As specified.

\*\* NOTE TO SPECIFIER \*\* Delete model not required.

* + - 1. Model NDI30 as manufactured by Heatilator.
         1. Unit Front Width: 30-1/2 inches (775 mm).
         2. Front Width Min. Firebox Opening: 29-1/4 inches (743 mm).
         3. Unit Back Width: 20-1/4 inches (514 mm).
         4. Back Width Min. Firebox Opening: 20-1/2 inches (521 mm).
         5. Unit Height: 20-1/2 inches (521 mm).
         6. Height Min. Firebox Opening: 19-1/8 inches (486 mm).
         7. Unit Depth: 13-7/8 inches (352 mm).
         8. Depth Min. Firebox Opening: 13-7/8 inches (352 mm).
         9. Glass Size: 27-1/2 inches (699 mm) x 12-7/8 inches (327 mm).
         10. BTU/Hour Input: 32,000 (NG) (9.4 kW).
         11. Efficiency: Steady State - 84.1%, AFUE - 73.2%, Canada EnerGuide - 72.7%.
      2. Model NDI35 as manufactured by Heatilator.
         1. Unit Front Width: 34-5/8 inches (879 mm).
         2. Front Width Min. Firebox Opening: 33-1/4 inches 9845 mm).
         3. Unit Back Width: 23-1/2 inches (597 mm).
         4. Back Width Min. Firebox Opening: 24 inches (610 mm).
         5. Unit Height: 24 inches (610 mm).
         6. Height Min. Firebox Opening: 22-3/4 inches (578 mm).
         7. Unit Depth: 15-1/8 inches (384 mm).
         8. Depth Min. Firebox Opening: 15-1/8 inches (384 mm).
         9. Glass Size: 31-5/8 inches (803 mm) x 15-3/4 inches (400 mm).
         10. BTU/Hour Input: 35,000 (NG) (10.3 kW).
         11. Efficiency: Steady State - 78.5%, AFUE - 73.5%, Canada EnerGuide - 72.2%.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* 1. OUTDOOR GAS LOG SETS

\*\* NOTE TO SPECIFIER \*\* Specifically designed for the Castlewood Outdoor Wood Fireplace. Eleven authentic-looking logs, molded from real oak timber, state-of-the-art, tiered burner system creates a multi-level fire. Hidden controls are easily accessible, won't detract from the fire's authenticity, and allow the log set to fit perfectly centered. Offers two types of burners: Matchlight (NG only) and IntelliFire™. Includes outdoor burner and hearth kit. Delete if not required.

* + 1. Fireside Grand Oak:
       1. Design: Eleven authentic-looking logs, molded from real oak timber, state-of-the-art, tiered burner system shall create a multi-level fire. Hidden controls are easily accessible and shall not detract from the fire's authenticity, and allow the log set to fit centered in hearth.

\*\* NOTE TO SPECIFIER \*\* Delete burner not required.

* + - 1. Burner: Matchlight (NG only).
      2. Burner: IntelliFire.
      3. Hearth kit provided.

\*\* NOTE TO SPECIFIER \*\* Delete remote control if not required.

* + - 1. Control: Smart-Batt (On/off, temperature readout, thermostat mode, timer mode).

\*\* NOTE TO SPECIFIER \*\* A realistic log set that withstands the worst of Mother Nature. Stainless steel burner tube, grate and sand pan burner, eight richly-detailed logs and offers two types of burner: Matchlight (NG only) and Remote-Ready Standing Pilot. Burner and hearth kit sold separately. Delete if not required.

* + 1. Outdoor Fireside Realwood:
       1. Eight richly-detailed realistic log set. Stainless steel burner tube, grate and sand pan burner, ,

\*\* NOTE TO SPECIFIER \*\* Hearth kit sold separately. Refer to manufacturer's literature for hearth designs available for the model. Delete if not required.

* + - 1. Hearth Kit:

\*\* NOTE TO SPECIFIER \*\* Burner sold separately. Delete burner not required.

* + - 1. Burner: Matchlight (NG only).
      2. Burner: Remote-Ready Standing Pilot.
  1. GAS FIREPLACE MANTELS AND FIREPLACE SURROUNDS

\*\* NOTE TO SPECIFIER \*\* Dress up your fireplace with mantels and surrounds that complement any style. Heatilator's collection of wood mantels display simple elegance and classic beauty.

* + 1. Wood Mantels and Surrounds as manufactured by Heatilator.

\*\* NOTE TO SPECIFIER \*\* Delete style and finish not required.

* + - 1. Belair.
         1. Finish: Maple Auburn.
         2. Finish: Maple Chocolate.
         3. Finish: Maple Ginger.
         4. Finish: Maple Honey.
         5. Finish: Maple Natural.
         6. Finish: Oak Chocolate.
         7. Finish: Oak Ginger.
         8. Finish: Oak Honey.
         9. Finish: Oak Natural.
         10. Finish: Primed wood fiber.
      2. Bella Corner.
         1. Finish: Maple Auburn.
         2. Finish: Maple Chocolate.
         3. Finish: Maple Ginger.
         4. Finish: Maple Honey.
         5. Finish: Maple Natural.
         6. Finish: Oak Auburn.
         7. Finish: Oak Chocolate.
         8. Finish: Oak Ginger.
         9. Finish: Oak Honey.
         10. Finish: Oak Natural.
         11. Finish: Primed wood fiber.
      3. Bridgeport.
         1. Finish: Oak Chocolate.
         2. Finish: Oak Ginger.
         3. Finish: Oak Honey.
         4. Finish: Oak Natural.
         5. Finish: Primed wood fiber.
      4. Fairfield.
         1. Finish: Maple Auburn.
         2. Finish: Maple Chocolate.
         3. Finish: Maple Ginger.
         4. Finish: Maple Honey.
         5. Finish: Maple Natural.
         6. Finish: Oak Chocolate.
         7. Finish: Oak Ginger.
         8. Finish: Oak Honey.
         9. Finish: Oak Natural.
         10. Finish: Primed wood fiber.
      5. Hastings.
         1. Finish: Oak Chocolate.
         2. Finish: Oak Ginger.
         3. Finish: Oak Honey.
         4. Finish: Oak Natural.
         5. Finish: Primed wood fiber.
      6. Kenwood Corner.
         1. Finish: Maple Auburn.
         2. Finish: Maple Chocolate.
         3. Finish: Maple Ginger.
         4. Finish: Maple Honey.
         5. Finish: Maple Natural.
         6. Finish: Oak Chocolate.
         7. Finish: Oak Ginger.
         8. Finish: Oak Honey.
         9. Finish: Oak Natural.
         10. Finish: Primed wood fiber.
      7. Kenwood Corner with Base.
         1. Finish: Maple Auburn.
         2. Finish: Maple Chocolate.
         3. Finish: Maple Ginger.
         4. Finish: Maple Honey.
         5. Finish: Maple Natural.
         6. Finish: Oak Chocolate.
         7. Finish: Oak Ginger.
         8. Finish: Oak Honey.
         9. Finish: Oak Natural.
         10. Finish: Primed wood fiber.
      8. Kenwood Wall Cabinet.
         1. Finish: Maple Auburn.
         2. Finish: Maple Chocolate.
         3. Finish: Maple Ginger.
         4. Finish: Maple Honey.
         5. Finish: Maple Natural.
         6. Finish: Oak Chocolate.
         7. Finish: Oak Ginger.
         8. Finish: Oak Honey.
         9. Finish: Oak Natural.
         10. Finish: Primed wood fiber.
      9. Kenwood Wall Cabinet with Base.
         1. Finish: Maple Auburn.
         2. Finish: Maple Chocolate.
         3. Finish: Maple Ginger.
         4. Finish: Maple Honey.
         5. Finish: Maple Natural.
         6. Finish: Oak Chocolate.
         7. Finish: Oak Ginger.
         8. Finish: Oak Honey.
         9. Finish: Oak Natural.
         10. Finish: Primed wood fiber.
      10. Mount Vernon.
          1. Finish: Maple Auburn.
          2. Finish: Maple Chocolate.
          3. Finish: Maple Ginger.
          4. Finish: Maple Honey.
          5. Finish: Maple Natural.
          6. Finish: Oak Chocolate.
          7. Finish: Oak Ginger.
          8. Finish: Oak Honey.
          9. Finish: Oak Natural.
          10. Finish: Primed wood fiber.
      11. Newport.
          1. Finish: Oak Chocolate.
          2. Finish: Oak Ginger.
          3. Finish: Oak Honey.
          4. Finish: Oak Natural.
          5. Finish: Primed wood fiber.
      12. Philips Hall.
          1. Finish: Alder Auburn.
          2. Finish: Alder Chocolate.
          3. Finish: Alder Ginger.
          4. Finish: Alder Honey.
          5. Finish: Alder Natural.
          6. Finish: Maple Auburn.
          7. Finish: Maple Chocolate.
          8. Finish: Maple Ginger.
          9. Finish: Maple Honey.
          10. Finish: Maple Natural.
          11. Finish: Oak Chocolate.
          12. Finish: Oak Ginger.
          13. Finish: Oak Honey.
          14. Finish: Oak Natural.
          15. Finish: Primed wood fiber.
      13. Plymouth.
          1. Finish: Maple Auburn.
          2. Finish: Maple Chocolate.
          3. Finish: Maple Ginger.
          4. Finish: Maple Honey.
          5. Finish: Maple Natural.
          6. Finish: Oak Chocolate.
          7. Finish: Oak Ginger.
          8. Finish: Oak Honey.
          9. Finish: Oak Natural.
          10. Finish: Primed wood fiber.
      14. Portico with Filler.
          1. Finish: Alder Auburn.
          2. Finish: Alder Chocolate.
          3. Finish: Alder Ginger.
          4. Finish: Alder Honey.
          5. Finish: Alder Natural.
          6. Finish: Maple Auburn.
          7. Finish: Maple Chocolate.
          8. Finish: Maple Ginger.
          9. Finish: Maple Honey.
          10. Finish: Maple Natural.
          11. Finish: Oak Chocolate.
          12. Finish: Oak Ginger.
          13. Finish: Oak Honey.
          14. Finish: Oak Natural.
          15. Finish: Primed wood fiber.
      15. Portico without Filler.
          1. Finish: Alder Auburn.
          2. Finish: Alder Chocolate.
          3. Finish: Alder Ginger.
          4. Finish: Alder Honey.
          5. Finish: Alder Natural.
          6. Finish: Maple Auburn.
          7. Finish: Maple Chocolate.
          8. Finish: Maple Ginger.
          9. Finish: Maple Honey.
          10. Finish: Maple Natural.
          11. Finish: Oak Chocolate.
          12. Finish: Oak Ginger.
          13. Finish: Oak Honey.
          14. Finish: Oak Natural.
          15. Finish: Primed wood fiber.
      16. Portico with Filler Painted.
          1. Finish: Alder Auburn.
          2. Finish: Alder Chocolate.
          3. Finish: Alder Ginger.
          4. Finish: Alder Honey.
          5. Finish: Alder Natural.
          6. Finish: Maple Auburn.
          7. Finish: Maple Chocolate.
          8. Finish: Maple Ginger.
          9. Finish: Maple Honey.
          10. Finish: Maple Natural.
          11. Finish: Oak Chocolate.
          12. Finish: Oak Ginger.
          13. Finish: Oak Honey.
          14. Finish: Oak Natural.
          15. Finish: Primed wood fiber.
      17. Roseville.
          1. Finish: Maple Auburn.
          2. Finish: Maple Chocolate.
          3. Finish: Maple Ginger.
          4. Finish: Maple Honey.
          5. Finish: Maple Natural.
          6. Finish: Oak Chocolate.
          7. Finish: Oak Ginger.
          8. Finish: Oak Honey.
          9. Finish: Oak Natural.
          10. Finish: Primed wood fiber.
      18. Sonoma.
          1. Finish: Alder Auburn.
          2. Finish: Alder Chocolate.
          3. Finish: Alder Ginger.
          4. Finish: Alder Honey.
          5. Finish: Alder Natural.
          6. Finish: Maple Auburn.
          7. Finish: Maple Chocolate.
          8. Finish: Maple Ginger.
          9. Finish: Maple Honey.
          10. Finish: Maple Natural.
          11. Finish: Oak Chocolate.
          12. Finish: Oak Ginger.
          13. Finish: Oak Honey.
          14. Finish: Oak Natural.
          15. Finish: Primed wood fiber.
      19. Winchester.
          1. Finish: Oak Chocolate.
          2. Finish: Oak Ginger.
          3. Finish: Oak Honey.
          4. Finish: Oak Natural.
          5. Finish: Primed wood fiber.
      20. Yorktown.
          1. Finish: Oak Chocolate.
          2. Finish: Oak Ginger.
          3. Finish: Oak Honey.
          4. Finish: Oak Natural.
          5. Finish: Primed wood fiber.
      21. Parsons.
          1. Finish: Alder Auburn.
          2. Finish: Alder Chocolate.
          3. Finish: Alder Ginger.
          4. Finish: Alder Honey.
          5. Finish: Alder Natural.
          6. Finish: Maple Auburn.
          7. Finish: Maple Chocolate.
          8. Finish: Maple Ginger.
          9. Finish: Maple Honey.
          10. Finish: Maple Natural.
          11. Finish: Oak Chocolate.
          12. Finish: Oak Ginger.
          13. Finish: Oak Honey.
          14. Finish: Oak Natural.
          15. Finish: Primed wood fiber.

\*\* NOTE TO SPECIFIER \*\* Heatilator stone surround sets are the perfect design element to complement your fireplace. Available in granite, marble and slate, these fireplace surround sets feature elegance and quality. Delete if not required.

* + 1. Stone Surround Sets
       1. Absolute Black Granite.
       2. Beige Marble.
       3. Caledonia Granite.
       4. Green Granite.
       5. Marron Brown Marble.
       6. New Venetian Granite.
       7. Slate.
       8. Tan Brown Granite.
       9. Wheatfield Granite.

\*\* NOTE TO SPECIFIER \*\* Stylize your living space with a cast stone fireplace mantel and cast surround from Heatilator.

* + 1. Cast Mantels and Surrounds:
       1. Atlas.
       2. Avalon.
          1. Finish: Beige.
          2. Finish: Macchiato.
       3. Avalon with Overmantel.
          1. Finish: Beige.
          2. Finish: Macchiato.
       4. Biltmore.
          1. Finish: Beige.
          2. Finish: Macchiato.
       5. Biltmore with Overmantel.
          1. Finish: Beige.
          2. Finish: Macchiato.
       6. Hearst.
          1. Finish: Beige.
          2. Finish: Macchiato.
       7. Hearst with Overmantel.
          1. Finish: Beige.
          2. Finish: Macchiato.

\*\* NOTE TO SPECIFIER \*\* Accent the look of your Heatilator fireplace with a cast or wood mantel shelf. Whether it's for usability or for decor, a mantel shelf dresses up your fireplace perfectly.

* + 1. Mantel Shelves:

\*\* NOTE TO SPECIFIER \*\* Delete length not required.

* + - 1. Length: 48 inches (1219 mm)."
      2. Length: 59 inches (1499 mm).
      3. Length: 72 inches (1829 mm).

\*\* NOTE TO SPECIFIER \*\* Delete style and finish not required.

* + - 1. Bennington.
         1. Finish: Maple Auburn.
         2. Finish: Maple Chocolate.
         3. Finish: Maple Ginger.
         4. Finish: Maple Honey.
         5. Finish: Maple Natural.
         6. Finish: Oak Chocolate.
         7. Finish: Oak Ginger.
         8. Finish: Oak Honey.
         9. Finish: Oak Natural.
         10. Finish: Primed wood fiber.
      2. Covington.
         1. Finish: Oak Chocolate.
         2. Finish: Oak Ginger.
         3. Finish: Oak Honey.
         4. Finish: Oak Natural.
         5. Finish: Primed wood fiber.
      3. St Cloud.
         1. Finish: Oak Chocolate.
         2. Finish: Oak Ginger.
         3. Finish: Oak Honey.
         4. Finish: Oak Natural.
         5. Finish: Alder Auburn.
         6. Finish: Alder Chocolate.
         7. Finish: Alder Ginger.
         8. Finish: Alder Honey.
         9. Finish: Alder Natural.
         10. Finish: Maple Auburn.
         11. Finish: Maple Chocolate.
         12. Finish: Maple Ginger.
         13. Finish: Maple Honey.
         14. Finish: Maple Natural.
         15. Finish: Primed wood fiber.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* 1. GAS FIREPLACE ACCESSORIES

\*\* NOTE TO SPECIFIER \*\* Take convenience to a new level with fireplace remote controls. Simply point and click to start enjoying the comfort of a fire in your home. Take a look at our catalog to find a remote product that will work best for you. Delete if not required.

* + 1. Controls:
       1. Wall Switches.
       2. Wall Mounted Controls.

\*\* NOTE TO SPECIFIER \*\* Offering both decorative and traditional gas termination caps, Heatilator can help you polish your fireplace system with the perfect finishing touch. Delete if not required.

* + 1. Termination Caps: Gas.

\*\* NOTE TO SPECIFIER \*\* Delete termination cap not required.

* + - 1. Horizontal Termination.
      2. Firebrick Termination.
      3. HP Termination.
      4. High-Rise Termination.
      5. Basement Termination.
      6. High Wind Termination.
      7. Decorative Radius Termination.
      8. Safety Shield Termination.
      9. Octagon Shroud Termination.
      10. Square Shroud Termination.
      11. Terracotta Termination.
      12. Decorative Shroud Termination.
      13. Round Termination.
      14. Square Termination.
      15. Decorative Square Termination.

\*\* NOTE TO SPECIFIER \*\* Circulating fans not available for all models. Refer to manufacturer's literature for model fan ready for add-on of electric fan.

* + 1. Circulating Fans: Manufacturer's standard circulating fan compatible with specified fireplace.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

1. EXECUTION
   1. EXAMINATION
      1. Do not begin installation until substrates have been properly prepared.
      2. If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
   2. PREPARATION
      1. Clean surfaces thoroughly prior to installation.
      2. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
   3. INSTALLATION
      1. Install in accordance with manufacturer's instructions, ANSI Z21.44 and the requirements of authorities having jurisdiction.
      2. Use manufacturer's guidelines for minimum clearances to combustibles, walls, and finishes.
      3. Anchor all components firmly in position for long life under hard use.
   4. FIELD QUALITY CONTROL
      1. Upon completion of installation, visually inspect all exposed surfaces. Touch up scratches and abrasions with touch-up paint recommended by the manufacturer, make imperfections invisible to the unaided eye from a distance of 5 feet (1.5m).
      2. Test for proper operation, control and safety devices.
      3. Complete Installer's Warranty Validation Card.
   5. PROTECTION
      1. Protect installed products until completion of project.

END OF SECTION