IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2023-01-18T15:10:45"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Ladder_Caged-Access_ALACO_564-CP:as Specified" | object type "Ladder_Caged-Access_ALACO_564-CP:as Specified" | names: "Ladder_Caged-Access_ALACO_564-CP:as Specified:163879" | material: materials ("Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Analytical Model, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "Ladder_Caged-Access_ALACO_564-CP:as Specified" | 1 occurrence | material: materials ("Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill", "Metal - Aluminum - ALACO - Standard Mill") | property sets: Analytical Model, Constraints, Dimensions, Identity Data, Other, Phasing

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Ladder_Caged-Access_ALACO_564-CP" (IFCLABEL)
    Family and Type = "Ladder_Caged-Access_ALACO_564-CP: as Specified" (IFCLABEL)
    Type = "as Specified" (IFCLABEL)
    Type Id = "163845" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Ladder_Caged-Access_ALACO_564-CP" (IFCTEXT)
    Manufacturer Address = "5167 G St. Chino, CA 91710-5143" (IFCTEXT)
    Manufacturer Fax = "909-591-7565" (IFCTEXT)
    Manufacturer Phone - Toll Free = "888-310-7040" (IFCTEXT)
    Manufacturer Phone = "909-591-7561" (IFCTEXT)
    Manufacturer Website = "http://alacoladder.com/" (IFCTEXT)
    Send Message = "" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "as Specified" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "ALACO Ladder Co" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "as Specified" (IFCIDENTIFIER)
  Analytical Model | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Available Options = "as Specified" (IFCTEXT)
  Analytical Model | properties | on 1 type object
    Capacity = "1500 lbs per Rung" (IFCTEXT)
    Standards Conformance = "OSHA ANSI A14.3" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "Basic Wall : Wall 1" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Base Cage Starting Height = 7. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Ladder Base Offset = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Platform Cage Starting Height = 7. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Platform Height = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 157.36475067027905 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    FF to Top of Parapet = 30. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Parapet Height = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Parapet Thickness = 0.66666666666684471 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Projection from Host = 0.58333333333333337 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Projection from Parapet = 0.58333333333333315 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Height = 29.75 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Width_Outside Frame = 1.6875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 6.2581227759967488 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Unit Width = 1.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    firstladderheight = 16.541666666666668 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    secondladderheight = 18. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Include Security Door = FALSE (IFCBOOLEAN)
    Ladder_Floor Mounted = TRUE (IFCBOOLEAN)
    Ladder_Off Floor Mounted = FALSE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Frame Finish = "Metal - Aluminum - ALACO - Standard Mill" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Expected Lifespan (Years) = 0 (IFCINTEGER)
    Installation Phase = "" (IFCTEXT)
    Maintenance Schedule (Months) = 0 (IFCINTEGER)
    Warranty Duration (Years) = 0 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B1010700" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©Arcat Inc." (IFCTEXT)
    Description = "ALACO Exterior Roof with Parapet Caged Access and Crossover Platform Ladder with Resting Platform - Model 564-CP as Specified" (IFCTEXT)
    Drawn By = "Sumex Design, Inc. / Robert S. Weygant, CSI, CDT, SCIP" (IFCTEXT)
    Keynote = "05515" (IFCTEXT)
    Manufacturer = "ALACO Ladder Co" (IFCTEXT)
    Model = "564-CP" (IFCTEXT)
    OmniClass Number = "23.30.70.17.14" (IFCTEXT)
    OmniClass Title = "Vertical Ladders" (IFCTEXT)
    Revision = "R1_2016-12" (IFCTEXT)
    Type Name = "as Specified" (IFCTEXT)
    URL = "http://alacoladder.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Text | properties | on 1 type object
    Building Codes = "" (IFCTEXT)
    Construction Details = "" (IFCTEXT)
    Green Building-LEED = "" (IFCTEXT)
    Installation-Fabrication = "" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos30/arc30245.html" (IFCTEXT)
    Product Properties = "" (IFCTEXT)
    Sales Information = "" (IFCTEXT)
    SpecWizard = "" (IFCTEXT)
    Specification = "" (IFCTEXT)
    Test Data = "" (IFCTEXT)