IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-04-21T12:41:51"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "AGSGSV-Gas-Solenoid-Valve-REVIT:AGS-GSV2" | object type "AGSGSV-Gas-Solenoid-Valve-REVIT:AGS-GSV2" | names: "AGSGSV-Gas-Solenoid-Valve-REVIT:AGS-GSV2:1010291" | material: materials ("steel", "Glass", "BLACK BODY", "BLUE") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions

Types
  IFCVALVETYPE "AGSGSV-Gas-Solenoid-Valve-REVIT:AGS-GSV2" | 1 occurrence | material: "steel" | property sets: Constraints, Dimensions, Electrical, General, Identity Data, Other

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCFLOWCONTROLLER) | on 1 type object
    Category = "Pipe Accessories" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Category = "Pipe Accessories" (IFCLABEL)
    Family = "AGSGSV-Gas-Solenoid-Valve-REVIT" (IFCLABEL)
    Family and Type = "AGSGSV-Gas-Solenoid-Valve-REVIT: AGS-GSV2" (IFCLABEL)
    Type = "AGS-GSV2" (IFCLABEL)
    Type Id = "1010276" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Pipe Accessories" (IFCLABEL)
    Family Name = "AGSGSV-Gas-Solenoid-Valve-REVIT" (IFCTEXT)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "AGS-GSV2" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER) | on 1 type object
    Manufacturer = "American Gas Safety LLC" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "AGS-GSV2" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 5.7140933941367846 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Maximum Size = 0.16666666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Minimum Size = 0.16666666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Size = "" (IFCTEXT)
    Volume = 0.3044891815663448 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    A = 0.16666666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    B = 0.55750000000000011 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "The AGS range of normally closed, electrically operated gas valves provide safetyshut down over combustible gas such as natural (Methane) and LP (Liquefiedpetroleum). Closed when de-energized, open when energized." (IFCTEXT)
    Email = "info@americangassafety.com" (IFCTEXT)
    Head Office address = "6304 Benjamin Road, Suite 502, Tampa, FL 33634" (IFCTEXT)
    Manufacturer = "American Gas Safety LLC" (IFCTEXT)
    Model = "AGS-GSV2" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Tel = "(727) 608-4375" (IFCTEXT)
    Type Name = "AGS-GSV2" (IFCTEXT)
    URL = "https://americangassafety.com/wp-content/uploads/2022/09/AGSGSV-Spec-Sheet.pdf" (IFCTEXT)
  Insulation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overall Size = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Hydronic Supply" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Electrical | properties | on 1 type object
    Temp = "5F-140F" (IFCTEXT)
    Volt = "110V AC" (IFCTEXT)
  General | properties | on 1 type object
    Body color = "Die Cast Aluminum" (IFCTEXT)
    Indication = "Visual Power Indication" (IFCTEXT)
    Ports = "1/4" Inlet & Outlet Ports" (IFCTEXT)
    Pressure = "0-5 PSI Max Working Pressure" (IFCTEXT)
  Visibility | properties | on 1 type object
    AGS-GSV1 = FALSE (IFCBOOLEAN)
    AGS-GSV112 = FALSE (IFCBOOLEAN)
    AGS-GSV114 = FALSE (IFCBOOLEAN)
    AGS-GSV12 = FALSE (IFCBOOLEAN)
    AGS-GSV2 = TRUE (IFCBOOLEAN)
    AGS-GSV34 = FALSE (IFCBOOLEAN)