IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-04-21T13:09:53"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "LAB-CONTROL-PANELS:Merlin 1000SW+i" | object type "LAB-CONTROL-PANELS:Merlin 1000SW+i" | names: "LAB-CONTROL-PANELS:Merlin 1000SW+i:2368664" | material: materials ("flush body", "OPTION", "BIN", "ASH", "UL", "HEADING(1)", "HEADING", "ELE", "GREEN", "RED", "AGS", "QR CODE", "Default(4)", "BRASS(1)", "Default(3)", "Default(2)", "Default(1)", "BLUE", "YELLOW", "PANNEL BODY") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions

Types
  IFCBUILDINGELEMENTPROXYTYPE "LAB-CONTROL-PANELS:Merlin 1000SW+i" | 1 occurrence | material: materials ("PANNEL BODY", "flush body") | property sets: Constraints, Dimensions, Electrical, General, Identity Data, Materials and Finishes

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Electrical Fixtures" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Electrical Fixtures" (IFCLABEL)
    Family = "LAB-CONTROL-PANELS" (IFCLABEL)
    Family and Type = "LAB-CONTROL-PANELS: Merlin 1000SW+i" (IFCLABEL)
    Type = "Merlin 1000SW+i" (IFCLABEL)
    Type Id = "2368649" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Electrical Fixtures" (IFCLABEL)
    Family Name = "LAB-CONTROL-PANELS" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Merlin 1000SW+i" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "American Gas Safety LLC" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Merlin 1000SW+i" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 12.027207295449665 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 0.75210368996418808 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    O/All Dimensions (H x W x D) inch = "7.08 x 10 x 3.03"" (IFCTEXT)
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "14" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "The UL 61010 listed Merlin 1000S Laboratory Utility Controller has been designed specifically for use in School andUniversity Laboratories. This controller is to be used to carry out a gas proving test on the pipe work in order to highlight ifthere is a gas appliance open or a gas leak in the laboratory. The Merlin 1000S is designed to give the teacher full controlover the incoming gas supply with the lockable key-switch operation. In built connectivity allows for connection to existing firealarm and building management systems and with its easy to use system status panel and labeled PCB the Merlin 1000S iseasy to install and to operate.The Merlin 1000S can work in conjunction with carbon dioxide, natural gas, carbon monoxide and LPG sensors. The Merlin1000S also has a built in “timeout” facility which will automatically shut off the gas solenoid valve at the end of a specific timeperiod, this time period can be adjusted to 2, 4, 8 hours or can be overridden if required." (IFCTEXT)
    Email = "info@americangassafety.com" (IFCTEXT)
    Head Office address = "6304 Benjamin Road, Suite 502, Tampa, FL 33634" (IFCTEXT)
    Manufacturer = "American Gas Safety LLC" (IFCTEXT)
    Model = "Merlin 1000SW+i" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Tel = "(727) 608-4375" (IFCTEXT)
    Type Name = "Merlin 1000SW+i" (IFCTEXT)
    URL = "https://americangassafety.com/wp-content/uploads/2023/02/AGS-1000SWi-User-Installation-Guide.pdf" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    FLUSH MOUNT = TRUE (IFCBOOLEAN)
  Visibility | properties | on 1 type object
    Melrin 1000S+i = FALSE (IFCBOOLEAN)
    Merlin 1000S = FALSE (IFCBOOLEAN)
    Merlin 1000S+ = FALSE (IFCBOOLEAN)
    Merlin 1000SW+ = FALSE (IFCBOOLEAN)
    Merlin 1000SW+i = TRUE (IFCBOOLEAN)
    Merlin 1000Si = FALSE (IFCBOOLEAN)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Electrical | properties | on 1 type object
    Audible Alarm Buzzer dB = "65 dB (300mm distance in quiet conditions)" (IFCTEXT)
    Current Consumption = "12W max (50mA) @ 120VAC" (IFCTEXT)
    Flame Rating = "UL 94" (IFCTEXT)
    Gas Valve Output = "3.15A" (IFCTEXT)
    Housing Material = "Polylac PA-765 Flame Retardant" (IFCTEXT)
    Internal Fuse = "3.15A" (IFCTEXT)
    Mains Electrical Power Input = "110-120VAC" (IFCTEXT)
    Operating Temperature = "32 - 104°F 0-95%RH Non-Condensing" (IFCTEXT)
    Power Rating = "" (IFCTEXT)
    Pressure Sensor Operating Pressure = "0-1.45psi" (IFCTEXT)
    UL Approval Reference = "UL 61010-1 E464760" (IFCTEXT)
    Utility Output = "110-120VAC" (IFCTEXT)
    Voltage Rating = "" (IFCTEXT)
  General | properties | on 1 type object
    Visual Indication = "LED" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    PANNEL BODY = "PANNEL BODY" (IFCLABEL)