IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-01-09T12:55:00"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ArmaGirt_Z-Girt:101.6mm" | object type "ArmaGirt_Z-Girt:101.6mm" | names: "ArmaGirt_Z-Girt:101.6mm:103864" | material: "Armadillo_StructuralThermalBreak_Armatherm_Z-Girt" | property sets: Pset_BuildingElementProxyCommon, Pset_ElementShading, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_PrecastConcreteElementGeneral, Pset_ProductRequirements

Types
  IFCBUILDINGELEMENTPROXYTYPE "ArmaGirt_Z-Girt:101.6mm" | USERDEFINED | 1 occurrence | material: "Armadillo_StructuralThermalBreak_Armatherm_Z-Girt" | property sets: Constraints, Data, Dimensions, Identity Data, Materials and Finishes, Model Properties

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AssetIdentifier = "Please record on commissioning" (IFCTEXT)
    BarCode = "Please record on commissioning" (IFCTEXT)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "ArmaGirt_Z-Girt" (IFCLABEL)
    Family and Type = "ArmaGirt_Z-Girt: 101.6mm" (IFCLABEL)
    InstallationDate = "Please record on commissioning" (IFCTEXT)
    SerialNumber = "Please record on commissioning" (IFCTEXT)
    Type = "101.6mm" (IFCLABEL)
    Type Id = "103840" (IFCLABEL)
    WarrantyStartDate = "Please record on commissioning" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Specialty Equipment" (IFCLABEL)
    ClassificationName = "Uniclass2015" (IFCTEXT)
    ClassificationValue = "Pr_35_90_15_89" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    CreatedBy = "info@armatherm.com" (IFCTEXT)
    CreatedOn = "2020-01-01 T09:00:00" (IFCTEXT)
    DocumentationCertificates = "https://www.armatherm.co.uk/" (IFCTEXT)
    DocumentationInstallationGuide = "https://www.armatherm.co.uk/" (IFCTEXT)
    DocumentationLiterature = "https://www.bimstore.co/products/armatherm-z-girt-structural-thermal-break/document/product-literature" (IFCTEXT)
    DocumentationMaintenance = "https://www.armatherm.co.uk/" (IFCTEXT)
    DocumentationTechnical = "https://www.bimstore.co/products/armatherm-z-girt-structural-thermal-break/document/technical-data-sheet" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = 0 (IFCINTEGER)
    Family Name = "ArmaGirt_Z-Girt" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    ManufacturerName = "Armadillo" (IFCTEXT)
    Material = "Thermoset resin" (IFCTEXT)
    ModelNumber = "Z-Girt" (IFCTEXT)
    ModelReference = "Structural thermal break" (IFCTEXT)
    ProductionYear = "2020" (IFCTEXT)
    ReferencedStandard = "n/a" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    TypeName = "Structural thermal break" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "0" (IFCTEXT)
    WarrantyDurationParts = "0" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "info@armatherm.com" (IFCTEXT)
    WarrantyGuarantorParts = "info@armatherm.com" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "101.6mm" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Color = "n/a" (IFCLABEL)
  Pset_ManufacturerOccurrence | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    BarCode = "Please record on commissioning" (IFCIDENTIFIER)
    SerialNumber = "Please record on commissioning" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Armadillo" (IFCLABEL)
    ModelReference = "Structural thermal break" (IFCLABEL)
    ProductionYear = "2020" (IFCLABEL)
  Pset_PrecastConcreteElementGeneral | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    SerialNumber = "Please record on commissioning" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "101.6mm" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Depth = 0.33333333333333331 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Height = 0.31824146981627299 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Shape = "n/a" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "None" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 3.9370078740157481 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Length = 9. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.092509823273440567 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    C = 0.1673228346456693 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Depth = 0.33333333333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 0.31824146981627299 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    InnerRadius = 0.005905511811023622 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    OuterRadius = 0.015091863517060366 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Thickness = 0.016404199475065617 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Armatherm thermally broken cladding support connection solutions prevent excessive heat flow and potential condensation problems otherwise associated with thermal bridging." (IFCTEXT)
    Keynote = "G" (IFCTEXT)
    Manufacturer = "Armadillo" (IFCTEXT)
    Model = "Z-Girt" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Product data url = "https://www.bimobject.com/armatherm/product/z-girt-structural-thermal-break-cladding-attachment" (IFCTEXT)
    Type Comments = "Structural thermal break" (IFCTEXT)
    Type Name = "101.6mm" (IFCTEXT)
    URL = "https://www.armatherm.co.uk/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Data | properties | on 1 type object
    Density = "1.8-2.0 gr/cm³" (IFCTEXT)
    FlammabilityClassification = "V0" (IFCTEXT)
    FlexuralModulus = "not less than 11035 MPa" (IFCTEXT)
    FlexuralStrength = "230 MPa" (IFCTEXT)
    WaterAbsorption = "0.6% max" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    StructuralThermalBreakMaterial = "Armadillo_StructuralThermalBreak_Armatherm_Z-Girt" (IFCLABEL)
  Model Properties | properties | on 1 type object
    BIMObjectName = "Armadillo_StructuralThermalBreak_Armatherm_Z-Girt" (IFCTEXT)
    NBSDescription = "Thermal break connection plates" (IFCTEXT)
    NBSNote = "" (IFCTEXT)
    NBSObjectName = "Armadillo Thermal break connection plates" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-75-42/399" (IFCTEXT)
    _Author = "AM" (IFCTEXT)
    _AuthorizedBy = "bimstore" (IFCTEXT)
    _BSBibleVersion = 16 (IFCINTEGER)
    _BimSpecGuid = 0 (IFCINTEGER)
    _CreatedBy = "www.bimstore.co" (IFCTEXT)
    _CurrentRevision = 1 (IFCINTEGER)
    _DistributedBy = "www.bimstore.co" (IFCTEXT)
    _ObjectUserGuide = "" (IFCTEXT)