IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-01-09T12:55:09"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Armatherm500_US:500-280" | object type "Armatherm500_US:500-280" | INSULATION | names: "Armatherm500_US:500-280:104736" | material: "Armadillo_ThermalBreakMaterial_Armatherm500-280" | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_PrecastConcreteElementGeneral, Pset_ProductRequirements

Types
  IFCCOVERINGTYPE "Armatherm500_US:500-280" | INSULATION | 1 occurrence | property sets: Constraints, Data, Dimensions, Identity Data, Materials and Finishes, Model Properties

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCCOVERING)
    AssetIdentifier = "Please record on commissioning" (IFCTEXT)
    BarCode = "Please record on commissioning" (IFCTEXT)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Armatherm500_US" (IFCLABEL)
    Family and Type = "Armatherm500_US: 500-280" (IFCLABEL)
    InstallationDate = "Please record on commissioning" (IFCTEXT)
    SerialNumber = "Please record on commissioning" (IFCTEXT)
    Type = "500-280" (IFCLABEL)
    Type Id = "104712" (IFCLABEL)
    WarrantyStartDate = "Please record on commissioning" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Specialty Equipment" (IFCLABEL)
    ClassificationName = "Uniclass2015" (IFCTEXT)
    ClassificationValue = "Pr_35_90_15_89" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    CreatedBy = "sales@armatherm.com" (IFCTEXT)
    CreatedOn = "2020-01-01 T09:00:00" (IFCTEXT)
    DocumentationCertificates = "https://www.armatherm.com/" (IFCTEXT)
    DocumentationInstallationGuide = "https://www.armatherm.com/" (IFCTEXT)
    DocumentationLiterature = "https://www.bimstore.co/products/armatherm-500-thermal-break/document/product-literature" (IFCTEXT)
    DocumentationMaintenance = "https://www.armatherm.com/" (IFCTEXT)
    DocumentationTechnical = "https://www.bimstore.co/products/armatherm-500-thermal-break/document/technical-data-sheet" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = 0 (IFCINTEGER)
    Family Name = "Armatherm500_US" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    ManufacturerName = "Armadillo" (IFCTEXT)
    Material = "High strength polyurethane" (IFCTEXT)
    ModelNumber = "Armatherm 500" (IFCTEXT)
    ModelReference = "Thermal break" (IFCTEXT)
    ProductionYear = "2020" (IFCTEXT)
    ReferencedStandard = "n/a" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    TypeName = "Thermal break" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "0" (IFCTEXT)
    WarrantyDurationParts = "0" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "sales@armatherm.com" (IFCTEXT)
    WarrantyGuarantorParts = "sales@armatherm.com" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "n/a" (IFCTEXT)
    Material = "High strength polyurethane" (IFCLABEL)
    Reference = "500-280" (IFCIDENTIFIER)
    TotalThickness = 0.16666666666666666 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_CoveringCommon | properties | on 1 type object
    Finish = "n/a" (IFCTEXT)
    Material = "High strength polyurethane" (IFCLABEL)
    TotalThickness = 0.16666666666666666 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ElementShading | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Color = "n/a" (IFCLABEL)
  Pset_ManufacturerOccurrence | properties | on 1 object (1 IFCCOVERING)
    BarCode = "Please record on commissioning" (IFCIDENTIFIER)
    SerialNumber = "Please record on commissioning" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Manufacturer = "Armadillo" (IFCLABEL)
    ModelReference = "Thermal break" (IFCLABEL)
    ProductionYear = "2020" (IFCLABEL)
  Pset_PrecastConcreteElementGeneral | properties | on 1 object (1 IFCCOVERING)
    SerialNumber = "Please record on commissioning" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCCOVERING)
    Reference = "500-280" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCCOVERING)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "None" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 3.9370078740157481 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCCOVERING)
    Area = 34.00000000000135 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Depth = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 8. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 5.3333333333366131 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Thickness = 0.16666666666666666 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCCOVERING)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCCOVERING)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Armatherm™ 500 is a high strength, polyurethane material made in several densities to support a wide range of loading conditions. Due to it’s closed cell structure, it does not absorb water or moisture and has limited creep under continuous load. The material is thermoset, does not melt and is flame resistant making it an ideal material for use in structural thermal break connections." (IFCTEXT)
    Keynote = "G" (IFCTEXT)
    Manufacturer = "Armadillo" (IFCTEXT)
    Model = "Armatherm 500" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Product data url = "https://www.bimobject.com/armatherm/product/armatherm-500-series" (IFCTEXT)
    Type Comments = "Thermal break" (IFCTEXT)
    Type Name = "500-280" (IFCTEXT)
    URL = "https://www.armatherm.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Data | properties | on 1 type object
    CompressiveModulus = "PSI 49,300" (IFCTEXT)
    CompressiveStress = "PSI 2150" (IFCTEXT)
    MaximumOperatingTemperature = "+175°F" (IFCTEXT)
    MinimumOperatingTemperature = "-300°F" (IFCTEXT)
    RValuePerInch = "1.9" (IFCTEXT)
    ThermalConductivity = "0.53 BTU in/hr ft2 F" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    ThermalBreakMaterial = "Armadillo_ThermalBreakMaterial_Armatherm500-280" (IFCLABEL)
  Model Properties | properties | on 1 type object
    BIMObjectName = "Armadillo_ThermalBreakMaterial_Armatherm500_490" (IFCTEXT)
    NBSDescription = "Thermal break connection plates" (IFCTEXT)
    NBSNote = "" (IFCTEXT)
    NBSObjectName = "Armadillo Thermal break connection plates" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-75-42/399" (IFCTEXT)
    _Author = "AM" (IFCTEXT)
    _AuthorizedBy = "bimstore" (IFCTEXT)
    _BSBibleVersion = 16 (IFCINTEGER)
    _BimSpecGuid = 0 (IFCINTEGER)
    _CreatedBy = "www.bimstore.co" (IFCTEXT)
    _CurrentRevision = 1 (IFCINTEGER)
    _DistributedBy = "www.bimstore.co" (IFCTEXT)
    _ObjectUserGuide = "" (IFCTEXT)