IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2023-01-18T16:45:14"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Atlas_Sound_FAPSUB-1:Two Way, Full Range, Coaxial Ceiling Loudspeaker" | object type "Atlas_Sound_FAPSUB-1:Two Way, Full Range, Coaxial Ceiling Loudspeaker" | names: "Atlas_Sound_FAPSUB-1:Two Way, Full Range, Coaxial Ceiling Loudspeaker:196504" | material: materials ("QF_Plastic-White-Smooth", "QF_Plastic - White - Smooth", "QF_Plastic - Black - Fine Textured") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "Atlas_Sound_FAPSUB-1:Two Way, Full Range, Coaxial Ceiling Loudspeaker" | 1 occurrence | material: materials ("<Unnamed>", "QF_Plastic - White - Smooth", "QF_Plastic - Black - Fine Textured", "QF_Plastic-White-Smooth") | property sets: Constraints, Data, Dimensions, Electrical, Identity Data, Materials and Finishes

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Communication Devices" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Communication Devices" (IFCLABEL)
    Family = "Atlas_Sound_FAPSUB-1" (IFCLABEL)
    Family and Type = "Atlas_Sound_FAPSUB-1: Two Way, Full Range, Coaxial Ceiling Loudspeaker" (IFCLABEL)
    Speaker Cone Visible = FALSE (IFCBOOLEAN)
    Type = "Two Way, Full Range, Coaxial Ceiling Loudspeaker" (IFCLABEL)
    Type Id = "196470" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    100V Taps = "1.9, 3.8, 7.5, 15, 30, 60 Watts & 8Ω" (IFCTEXT)
    70V Taps = "1.9, 3.8, 7.5, 15, 30, 60 Watts & 8Ω" (IFCTEXT)
    Category = "Communication Devices" (IFCLABEL)
    Coverage Horizontal = 110. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Coverage Vertical = 110. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Dispersion Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Family Name = "Atlas_Sound_FAPSUB-1" (IFCTEXT)
    Regulatory Compliance = "UL Listed to Comply with UL1480" (IFCTEXT)
    SPL Max = 107. (IFCREAL)
    ScheduleType |RF| = "AtlasIED Master" (IFCTEXT)
    Transformer Option = TRUE (IFCBOOLEAN)
    Vertical Symmetry = TRUE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Two Way, Full Range, Coaxial Ceiling Loudspeaker" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "ATLAS SOUND" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Two Way, Full Range, Coaxial Ceiling Loudspeaker" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Height = 1.0625000000000002 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 1.3125000000000004 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Offset from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Radius of Speaker Cone = 12.990381056766552 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Speaker Cone Height = 7.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Work Plane = "???" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 1147.5498747635245 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Speaker Height = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Speaker Listening Height = 2.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.88844952091174578 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Height = 1.0625000000000002 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Speaker Dispersion = 120. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Width = 1.3125000000000004 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Family Version = "2017-01" (IFCTEXT)
    Mark = "44" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Cost = 267.99000000000001 (IFCREAL)
    Cost MSRP = 267.99000000000001 (IFCREAL)
    Description = "8" TUNED PORTED IN-CEILING SUBWOOFER WITH 60-WATT 70V/100V TRANSFORMER" (IFCTEXT)
    Family Code (default) = "LOUD SPEAKERS" (IFCTEXT)
    IQ Category = "SPEAKERS" (IFCTEXT)
    Manufacturer = "ATLAS SOUND" (IFCTEXT)
    Manufacturer Address = "4545 E. Baseline Rd., Phoenix, AZ 85042" (IFCTEXT)
    Manufacturer Email = "support@atlasied.com" (IFCTEXT)
    Manufacturer Phone = "(800) 876 - 3333" (IFCTEXT)
    Manufacturer URL = "https://www.atlasied.com/" (IFCTEXT)
    MasterFormat = "27 41 13" (IFCTEXT)
    MaterFormat Title = "SPEAKERS" (IFCTEXT)
    Model = "FABSUB-1" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Product Documentation Link = "https://www.atlasied.com/f/1868/FAPSUB_RevBData.pdf" (IFCTEXT)
    Product Page URL = "https://www.atlasied.com/fapsub-1" (IFCTEXT)
    Specification by User (default) = "TBD" (IFCTEXT)
    Type Name = "Two Way, Full Range, Coaxial Ceiling Loudspeaker" (IFCTEXT)
    URL = "www.atlassound.com" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Data | properties | on 1 type object
    Ingress Protection = "IP-21" (IFCTEXT)
    Safety Agency Ratings = "UL Listed to Comply with UL1480" (IFCTEXT)
    Warranty = "5 Year" (IFCTEXT)
  Electrical | properties | on 1 type object
    Impedance = 8. (IFCREAL)
    Power Handling = 100. (IFCREAL)
    Power Rating (RMS) = "100 Watts" (IFCTEXT)
    Sensitivity = 89. (IFCREAL)
  Materials and Finishes | properties | on 1 type object
    Body Material = "QF_Plastic - White - Smooth" (IFCLABEL)
    Grill Material = "QF_Plastic - Black - Fine Textured" (IFCLABEL)
    Mount Material = "QF_Plastic - White - Smooth" (IFCLABEL)
  Mechanical | properties | on 1 type object
    Controls = "Front Mounted Tap Selector Switch." (IFCTEXT)
    Frequency Response = "45Hz – 120Hz (±10dB),55Hz – 100Hz (±6dB)" (IFCTEXT)
    Input Connectors = "4 Pole Detachable Phoenix / Euro Style Connector Allows Easy Pre-Wiring" (IFCTEXT)
  Text | properties | on 1 type object
    Speaker Type = "S1" (IFCTEXT)