IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2024-08-26T20:06:56"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCDOOR | type IFCDOORSTYLE "assa_abloy_versamax_11:ICU-TE-3FBO-12" | object type "assa_abloy_versamax_11:ICU-TE-3FBO-12" | names: "assa_abloy_versamax_11:ICU-TE-3FBO-12:270074" | material: materials ("Clear Anodized", "Clear Anodized", "Clear Anodized", "Glass", "Clear Anodized", "<Unnamed>", "<Unnamed>", "Clear Anodized", "Clear Anodized", "Clear Anodized", "Clear Anodized", "Clear Anodized", "<Unnamed>", "<Unnamed>", "Clear Anodized", "Clear Anodized", "Clear Anodized", "Clear Anodized", "Clear Anodized", "Clear Anodized") | property sets: Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction

Types
  IFCDOORSTYLE "assa_abloy_versamax_11:ICU-TE-3FBO-12" | 1 occurrence | material: materials ("Clear Anodized", "Clear Anodized", "Clear Anodized", "Glass", "Clear Anodized", "<Unnamed>", "<Unnamed>", "Clear Anodized", "Clear Anodized", "Clear Anodized", "Clear Anodized", "Clear Anodized", "<Unnamed>", "<Unnamed>", "Clear Anodized", "Clear Anodized", "Clear Anodized", "Clear Anodized", "Clear Anodized", "Clear Anodized") | property sets: assa_abloy_versamax_11:ICU-TE-3FBO-12:270074, assa_abloy_versamax_11:ICU-TE-3FBO-12:270074:1, Analytical Properties, Construction, Data, Dimensions

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "assa_abloy_versamax_11" (IFCLABEL)
    Family and Type = "assa_abloy_versamax_11: ICU-TE-3FBO-12" (IFCLABEL)
    Head Height = 7.4791666666666661 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "270064" (IFCLABEL)
    Type = "ICU-TE-3FBO-12" (IFCLABEL)
    Type Id = "270028" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Bottom Profile Option 01 = "Fix Leaf1 : 0'4''" (IFCLABEL)
    Bottom Profile Option 02 = "Fix Leaf1 : 0'7''" (IFCLABEL)
    Bottom Profile Option 03 = "Fix Leaf1 : 0'10''" (IFCLABEL)
    Category = "Doors" (IFCLABEL)
    Family Name = "assa_abloy_versamax_11" (IFCTEXT)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ICU-TE-3FBO-12" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Manufacturer = "ASSA ABLOY Entrance Systems-North America" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDOOR)
    Reference = "ICU-TE-3FBO-12" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCDOOR)
    Sill Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCDOOR)
    Glass Type = "Glass Type : 5/8''" (IFCLABEL)
  Construction | properties | on 1 type object
    Bottom Profile Height = "Fix Leaf1 : 0'4''" (IFCLABEL)
    Function = "Interior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCDOOR)
    Area = 230.54036288435731 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Door Opening = 8.859375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Inset = 0.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Jumb Thickness = 0.14583333333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Leaf Bottom Profile Height = 0.33333333333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Leaf Width = 4.046875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Mid Leaf Position = 7.864583333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Mid Leaf Position If Opened = 7.864583333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Distance = 0.010416666666666666 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Profile = 7.625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 4.2925663034843327 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Gap = 0.020833333333333481 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 7.4791666666666661 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Leaf Height = 7.0625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 7.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 12.041666666666666 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Thickness = 0.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Top Profile Height = 0.33333333333333331 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCDOOR)
    Mark = "11" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    EAN code = "" (IFCTEXT)
    Installation instructions = "" (IFCTEXT)
    Manufacturer = "ASSA ABLOY Entrance Systems-North America" (IFCTEXT)
    OmniClass Number = "23.30.10.00" (IFCTEXT)
    OmniClass Title = "Doors" (IFCTEXT)
    Product certification = "" (IFCTEXT)
    Product data url = "http://besam-na.bimobject.com/VersaMax_Tele_OHC" (IFCTEXT)
    Technical description = "" (IFCTEXT)
    Type Mark = "39" (IFCTEXT)
    Type Name = "ICU-TE-3FBO-12" (IFCTEXT)
    Youtube clip = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCDOOR)
    Phase Created = "New Construction" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCDOOR)
    Closed = TRUE (IFCBOOLEAN)
    Horizontal Sash = TRUE (IFCBOOLEAN)
    Opened = FALSE (IFCBOOLEAN)
    Optional 1" Jambs = FALSE (IFCBOOLEAN)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  assa_abloy_versamax_11:ICU-TE-3FBO-12:270074 | predefined | on 1 type object
  assa_abloy_versamax_11:ICU-TE-3FBO-12:270074:1 | predefined | on 1 type object
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Data | properties | on 1 type object
    Brass Polished Finish = "Brass, Polished" (IFCLABEL)
    Brass Satin Finish = "Brass, Satin" (IFCLABEL)
    Clear Anodized = "Clear Anodized" (IFCLABEL)
    Dark Bronze Anodized = "Dark Bronze Anodized" (IFCLABEL)
    Stainless Steel Polished Finish = "Stainless Steel, Polished" (IFCLABEL)
    Stainless Steel Satin Finish = "Stainless Steel, Satin" (IFCLABEL)
  General | properties | on 1 type object
    Date of publishing = "2015-02-23" (IFCTEXT)
    Depth = "0.00" (IFCTEXT)
    Design country = "" (IFCTEXT)
    Edition number = "1" (IFCTEXT)
    Manufacturer country = "" (IFCTEXT)
    Manufacturer name = "ASSA ABLOY Entrance Systems-North America" (IFCTEXT)
    Nominal height = "0.00" (IFCTEXT)
    Nominal width = "0.00" (IFCTEXT)
    Product SKU = "VersaMax_Tele_OHC" (IFCTEXT)
    Product family = "ICU" (IFCTEXT)
    Product group = "Telescopic" (IFCTEXT)
    QR code = "http://besam-na.bimobject.com/VersaMax_Tele_OHC" (IFCTEXT)
    Region Africa = "None" (IFCTEXT)
    Region Antarctica = "None" (IFCTEXT)
    Region Asia = "None" (IFCTEXT)
    Region Europe = "None" (IFCTEXT)
    Region Middle East = "None" (IFCTEXT)
    Region North America = "AG, AI, AN, AW, BB, BL, BM, BQ, BS, BZ, CA, CR, CU, CW, DM, DO, GD, GL, GP, GT, HN, HT, JM, KN, KY, LC, MF, MQ, MS, MX, NI, PA, PM, PR, SV, SX, TC, TT, US, VC, VG, VI" (IFCTEXT)
    Region Oceania = "None" (IFCTEXT)
    Region South America = "None" (IFCTEXT)
    Weight Net (Kg) = "0" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Frame Material = "Clear Anodized" (IFCLABEL)
    Glass = "Glass" (IFCLABEL)
    Material main = "Aluminium" (IFCTEXT)
    Material secondary = "" (IFCTEXT)