IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-07-23T10:09:27"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 2 elements
          1 x IFCDOOR | type IFCDOORSTYLE "DO_WPB_Dynadry_BMP:Dynadry" | object type "DO_WPB_Dynadry_BMP:Dynadry" | names: "DO_WPB_Dynadry_BMP:Dynadry:118500" | material: materials ("Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Glass, transparent", "PVC", "Plastic, black", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304") | property sets: Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Data
          1 x IFCELECTRICDISTRIBUTIONPOINT | type IFCDISTRIBUTIONELEMENTTYPE "EE_WPB_control panel_BMP_SH:Control panel PVC" | object type "EE_WPB_control panel_BMP_SH:Control panel PVC" | SWITCHBOARD | names: "EE_WPB_control panel_BMP_SH:Control panel PVC:118501" | material: "PVC" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions

Types
  IFCDOORSTYLE "DO_WPB_Dynadry_BMP:Dynadry" | 1 occurrence | material: materials ("Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Glass, transparent", "PVC", "Plastic, black", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304", "Steel, stainless 304") | property sets: DO_WPB_Dynadry_BMP:Dynadry:118500, DO_WPB_Dynadry_BMP:Dynadry:118500:1, Analytical Properties, Constraints, General, Identity Data | description "High Speed Door"
  IFCDISTRIBUTIONELEMENTTYPE "EE_WPB_control panel_BMP_SH:Control panel PVC" | 1 occurrence | material: "PVC" | property sets: Constraints, General, Identity Data, Materials and Finishes, Other, Pset_ManufacturerTypeInformation | description "Control panel"

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCELECTRICDISTRIBUTIONPOINT) | on 1 type object
    Category = "Electrical Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "DO_WPB_Dynadry_BMP" (IFCLABEL)
    Family and Type = "DO_WPB_Dynadry_BMP: Dynadry" (IFCLABEL)
    H_calc = 6.5616797900262469 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    T_exit_height = 7.1522309711286089 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    T_exit_width = 5.9055118110236222 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Type = "Dynadry" (IFCLABEL)
    Type Id = "118464" (IFCLABEL)
    W_calc = 6.5616797900262469 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    additional_power_supply_check = FALSE (IFCBOOLEAN)
    bottom_window_check = 2 (IFCINTEGER)
    clearance_zone_control_panel = FALSE (IFCBOOLEAN)
    clearance_zone_length = 0.49212598425196852 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    clearance_zone_motor = FALSE (IFCBOOLEAN)
    clearance_zone_motor_bottom = 0.49212598425196852 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    control_panel_height = 1.3123359580052494 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    control_panel_length = 0.50853018372703407 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    control_panel_offset = 1.3123359580052494 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    control_panel_position_FB = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    control_panel_position_LR = 10.006561679790027 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    control_panel_position_height = 4.9212598425196852 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    control_panel_type_check = "EE_WPB_control panel_BMP_SH : Control panel PVC" (IFCLABEL)
    control_panel_width = 0.98425196850393704 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    curtain_bottom_thickness = 0.036089238845144353 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    curtain_position_FB = 0.25098425196850394 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    curtain_thickness = 0.022965879265091863 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    curtain_window_type = "curtain : rectangle window" (IFCLABEL)
    emergency_left = FALSE (IFCBOOLEAN)
    emergency_pictogram_height = 3.2808398950131235 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    emergency_pictogram_offset = 0.27395013123359579 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    emergency_pictogram_position_left = 2.7066929133858268 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    emergency_pictogram_position_right = 3.8549868766404201 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    emergency_right = FALSE (IFCBOOLEAN)
    error = FALSE (IFCBOOLEAN)
    field_height = 2.4606299212598426 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    fixed_cover = FALSE (IFCBOOLEAN)
    frame_length = 7.2178477690288716 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    free_top_space = 1.7224409448818898 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    front_motor_check = FALSE (IFCBOOLEAN)
    height_error = FALSE (IFCBOOLEAN)
    installation_zone_mounting_bracket = 0.16404199475065617 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    installation_zone_side = 0.065616797900262466 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    installation_zone_top = 0.065616797900262466 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    maintenance_zone_control_panel_front = 1.7224409448818898 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    maintenance_zone_motor_side = 0.6889763779527559 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    micro_switch_position = 0.20505249343832022 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    motor_clearance_zone_height = 6.3812335958005244 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    motor_cover = TRUE (IFCBOOLEAN)
    motor_cover_height_check = 1.9028871391076114 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    motor_cover_offset = 0.72178477690288712 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    motor_cover_position_FB = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    motor_cover_position_H = 8.2841207349081358 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    motor_cover_position_LR = 8.4645669291338574 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    motor_position = "side" (IFCTEXT)
    motor_side = "right" (IFCTEXT)
    mounting_bracket_height = 0.32808398950131235 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    mounting_offset = 0.30675853018372701 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    mounting_plate_angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    mounting_plate_flipped = TRUE (IFCBOOLEAN)
    mounting_plate_offset_x = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    mounting_plate_offset_y = -0.16076115485564305 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    nr_fields_height = 2 (IFCINTEGER)
    nr_fields_width = 1 (IFCINTEGER)
    nr_window_fields_height = 1 (IFCINTEGER)
    nr_window_fields_width = 1 (IFCINTEGER)
    one = FALSE (IFCBOOLEAN)
    power_supply_offset = 1.3123359580052494 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    power_supply_position_FB = 0.21325459317585299 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    power_supply_position_LR = 10.006561679790027 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    profile_counterweight = FALSE (IFCBOOLEAN)
    roll_cover_position_L = 0.41010498687664043 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    roll_cover_position_R = 0.41010498687664043 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    roll_cover_start_left = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    roll_length_left = 7.3818897637795278 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    roll_length_right = 0.016404199475065617 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    slanted_cover = TRUE (IFCBOOLEAN)
    total_height = 8.2841207349081358 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    total_width = 7.3818897637795278 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    voltage_check = 400.00000000000006 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    wall_void_position_FB = 0.42650918635170604 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    width_error = FALSE (IFCBOOLEAN)
    window_bottom_start = 4.5931758530183728 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    window_error = FALSE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCELECTRICDISTRIBUTIONPOINT)
    Category = "Electrical Equipment" (IFCLABEL)
    Family = "EE_WPB_control panel_BMP_SH" (IFCLABEL)
    Family and Type = "EE_WPB_control panel_BMP_SH: Control panel PVC" (IFCLABEL)
    H2 = 1.3123359580052494 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    H_calc = 1.3123359580052494 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Type = "Control panel PVC" (IFCLABEL)
    Type Id = "117986" (IFCLABEL)
    W_calc = 0.98425196850393704 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Doors" (IFCLABEL)
    Family Name = "DO_WPB_Dynadry_BMP" (IFCTEXT)
    csv = "Dynadry" (IFCTEXT)
    csv_metadata = "Dynadry_data" (IFCTEXT)
    curtain_bottom_height = 0.39370078740157477 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Other | properties | on 1 type object
    Category = "Electrical Equipment" (IFCLABEL)
    Family Name = "EE_WPB_control panel_BMP_SH" (IFCTEXT)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Dynadry" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (1 IFCDOOR, 1 IFCELECTRICDISTRIBUTIONPOINT) | on 2 type objects
    Manufacturer = "BMP High Speed Doors" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDOOR)
    Reference = "Dynadry" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCELECTRICDISTRIBUTIONPOINT)
    Reference = "Control panel PVC" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCDOOR)
    Offset from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Work Plane = "???" (IFCTEXT)
    control_panel_height_position = 4.9212598425196852 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    control_panel_width_position = 1.3123359580052494 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    front_motor = FALSE (IFCBOOLEAN)
    motor_left = FALSE (IFCBOOLEAN)
    motor_right = TRUE (IFCBOOLEAN)
    opening_height = 6.5616797900262469 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    opening_width = 6.5616797900262469 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    switch_control_panel_side = FALSE (IFCBOOLEAN)
    warning = "-" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCELECTRICDISTRIBUTIONPOINT)
    Elevation from Level = 4.921259842519671 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "None" (IFCTEXT)
    Offset from Host = 4.921259842519671 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Data | properties | on 1 object (1 IFCDOOR)
    1-channel_transmitter = FALSE (IFCBOOLEAN)
    2-channel_transmitter = FALSE (IFCBOOLEAN)
    4-channel_transmitter = FALSE (IFCBOOLEAN)
    CEE_plug = TRUE (IFCBOOLEAN)
    INOX_support_bracket = FALSE (IFCBOOLEAN)
    IP65motor_SS404_brake = FALSE (IFCBOOLEAN)
    LED_flashing_push_button = FALSE (IFCBOOLEAN)
    LED_strip_lights = FALSE (IFCBOOLEAN)
    LED_warning_light = FALSE (IFCBOOLEAN)
    Push_button_IP65_mushroom = FALSE (IFCBOOLEAN)
    SS304_brake = FALSE (IFCBOOLEAN)
    SS304_drum = FALSE (IFCBOOLEAN)
    UPS_battery_pack = FALSE (IFCBOOLEAN)
    additional_push-button = FALSE (IFCBOOLEAN)
    anti_drip_system = TRUE (IFCBOOLEAN)
    counterweight = FALSE (IFCBOOLEAN)
    crash_forgiving = TRUE (IFCBOOLEAN)
    extra_cable_extension = 0 (IFCINTEGER)
    extra_cord = FALSE (IFCBOOLEAN)
    flash_light = FALSE (IFCBOOLEAN)
    floor_loop = FALSE (IFCBOOLEAN)
    frame_base_in_RAL_color = FALSE (IFCBOOLEAN)
    galvanised_extension_bracket = FALSE (IFCBOOLEAN)
    galvanised_support_bracket = FALSE (IFCBOOLEAN)
    hand_crank = TRUE (IFCBOOLEAN)
    heated_side_guides = FALSE (IFCBOOLEAN)
    high_speed_motor = FALSE (IFCBOOLEAN)
    key_selector_with_pvc_box = FALSE (IFCBOOLEAN)
    keyswitch_selector_control_panel = FALSE (IFCBOOLEAN)
    light_curtain = FALSE (IFCBOOLEAN)
    light_curtain_with_sensor = FALSE (IFCBOOLEAN)
    motion_sensor_BEA_Condor = FALSE (IFCBOOLEAN)
    motion_sensor_BEA_Falcon = FALSE (IFCBOOLEAN)
    motor_heating = FALSE (IFCBOOLEAN)
    opening_speed = 4.4738725841088032 (IFCREAL)
    output_expansion = FALSE (IFCBOOLEAN)
    photocell_anti-roll_sensor = TRUE (IFCBOOLEAN)
    photocell_set_built-in = FALSE (IFCBOOLEAN)
    photocell_set_surface_mounted = FALSE (IFCBOOLEAN)
    pull_cord_switch = FALSE (IFCBOOLEAN)
    push-buttons_emergency_stop = FALSE (IFCBOOLEAN)
    reinforcement_kit = FALSE (IFCBOOLEAN)
    remote_control_receiver = FALSE (IFCBOOLEAN)
    rodent_barrier = FALSE (IFCBOOLEAN)
    selector_on_control_panel = FALSE (IFCBOOLEAN)
    selector_on_pvc_box = FALSE (IFCBOOLEAN)
    self-reinserting_break_away = TRUE (IFCBOOLEAN)
    sirene = FALSE (IFCBOOLEAN)
    stainless_steel_extension_bracket = FALSE (IFCBOOLEAN)
    standard_push_button = TRUE (IFCBOOLEAN)
    tof-spot_radar = FALSE (IFCBOOLEAN)
    weighted_bottom = TRUE (IFCBOOLEAN)
    wireless_safety_edge = FALSE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCDOOR)
    Area = 31.67901873424638 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    RSen_C_height = 6.5616797900262469 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    RSen_C_width = 6.5616797900262469 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 10.469231971122575 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
    max_opening_height = 19.685039370078741 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    max_opening_width = 14.763779527559056 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    motor_cover_height = 1.9028871391076114 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    motor_cover_length = 1.1482939632545932 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    motor_cover_width = 0.72178477690288712 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    profile_height_left = 0.42650918635170604 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    profile_height_right = 0.49212598425196852 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    profile_width = 0.41010498687664043 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    roll_cover_height = 1.0662729658792651 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    roll_cover_width = 0.82020997375328086 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    window_height = 1.6404199475065617 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    window_width = 6.1023622047244093 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCELECTRICDISTRIBUTIONPOINT)
    H = 1.3123359580052494 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    L = 0.50853018372703407 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    RSen_C_height = 1.3123359580052494 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    RSen_C_width = 0.98425196850393704 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.65685280101968657 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
    W = 0.98425196850393704 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical | properties | on 1 object (1 IFCDOOR)
    RSen_E_c01_apparent_power = 4000. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_current = 10. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    RSen_E_c01_load_classification = "Motor" (IFCLABEL)
    RSen_E_c01_number_of_poles = 3 (IFCINTEGER)
    RSen_E_c01_voltage = 400.00000000000006 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    RSen_E_c02_apparent_power = 0. (IFCPOWERMEASURE) [WATT]
    RSen_E_c02_current = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    RSen_E_c02_voltage = 0. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    additional_power_supply_24V = FALSE (IFCBOOLEAN)
    nr_plug_poles = 5 (IFCINTEGER)
  Electrical | properties | on 1 object (1 IFCELECTRICDISTRIBUTIONPOINT)
    RSen_E_c01_apparent_power = 4000.0000000000005 (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_current = 10. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    RSen_E_c01_load_classification = "Motor" (IFCLABEL)
    RSen_E_c01_number_of_poles = 3 (IFCINTEGER)
    RSen_E_c01_voltage = 400.00000000000006 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    UPS_battery_pack = FALSE (IFCBOOLEAN)
    nr_plug_poles = 5 (IFCINTEGER)
  General | properties | on 1 object (1 IFCDOOR)
    RSen_C_product_description = "Dynadry SRM325_ENG" (IFCTEXT)
  General | properties | on 1 object (1 IFCELECTRICDISTRIBUTIONPOINT)
    Location = "" (IFCTEXT)
    RSen_C_product_description = "Control panel" (IFCTEXT)
  General | properties | on 1 type object
    Classification.OmniClass.23.Description = "Rapid Opening Doors" (IFCTEXT)
    Classification.OmniClass.23.Number = "23.17.11.45.17" (IFCTEXT)
    Classification.Uniclass.EF.Description = "Doors" (IFCTEXT)
    Classification.Uniclass.EF.Number = "EF_25_30_25" (IFCTEXT)
    Classification.Uniclass.Pr.Description = "High-speed doorsets" (IFCTEXT)
    Classification.Uniclass.Pr.Number = "Pr_30_59_24_38" (IFCTEXT)
    Classification.Uniclass.Ss.Description = "High-speed doorset systems" (IFCTEXT)
    Classification.Uniclass.Ss.Number = "Ss_25_30_20_38" (IFCTEXT)
    RSen_C_code_ETIM = "EC003229" (IFCTEXT)
    RSen_C_code_ETIM_url = "https://prod.etim-international.com/Class/Details?classId=EC003229" (IFCTEXT)
    RSen_C_content_modification_date = "2025.01.22" (IFCTEXT)
    RSen_C_content_provider = "BMP High Speed Doors" (IFCTEXT)
    RSen_C_content_version = "V2" (IFCTEXT)
    RSen_C_model = "Dynadry" (IFCTEXT)
  General | properties | on 1 type object
    Classification.OmniClass.23.Description = "Rapid Opening Doors" (IFCTEXT)
    Classification.OmniClass.23.Number = "23.17.11.45.17" (IFCTEXT)
    Classification.Uniclass.EF.Description = "Doors" (IFCTEXT)
    Classification.Uniclass.EF.Number = "EF_25_30_25" (IFCTEXT)
    Classification.Uniclass.Pr.Description = "Door and gate-operating hardware" (IFCTEXT)
    Classification.Uniclass.Pr.Number = "Pr_75_30_23" (IFCTEXT)
    Classification.Uniclass.Ss.Description = "High-speed doorset systems" (IFCTEXT)
    Classification.Uniclass.Ss.Number = "Ss_25_30_20_38" (IFCTEXT)
    RSen_C_code_ETIM = "EC003836" (IFCTEXT)
    RSen_C_code_ETIM_url = "https://prod.etim-international.com/Class/Details?classId=EC003836" (IFCTEXT)
    RSen_C_content_modification_date = "2025.01.22" (IFCTEXT)
    RSen_C_content_provider = "BMP High Speed Doors" (IFCTEXT)
    RSen_C_content_version = "V1" (IFCTEXT)
    RSen_C_model = "Control panel" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCDOOR)
    T_exit = FALSE (IFCBOOLEAN)
    bottom_window = 2 (IFCINTEGER)
    control_panel_type = "EE_WPB_control panel_BMP_SH : Control panel PVC" (IFCLABEL)
    curtain_type = "curtain type : Standard curtain" (IFCLABEL)
    emergency_pictogram_left = FALSE (IFCBOOLEAN)
    emergency_pictogram_right = FALSE (IFCBOOLEAN)
    nr_window_fields = 1 (IFCINTEGER)
    side_emergency_exit = FALSE (IFCBOOLEAN)
    slanted_drum_motor_cover = TRUE (IFCBOOLEAN)
    switch_emergency_curtain_side = FALSE (IFCBOOLEAN)
    wall_thickness = 0.65616797900262469 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    window_type = "window type : Rectangle window" (IFCLABEL)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCELECTRICDISTRIBUTIONPOINT)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "High Speed Door" (IFCTEXT)
    LOD300 = FALSE (IFCBOOLEAN)
    LOD400 = TRUE (IFCBOOLEAN)
    Manufacturer = "BMP High Speed Doors" (IFCTEXT)
    Model = "Dynadry" (IFCTEXT)
    OmniClass Number = "23.17.11.45.17" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Mark = "1" (IFCTEXT)
    Type Name = "Dynadry" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Control panel" (IFCTEXT)
    LOD300 = FALSE (IFCBOOLEAN)
    LOD400 = TRUE (IFCBOOLEAN)
    Manufacturer = "BMP High Speed Doors" (IFCTEXT)
    Model = "Control panel" (IFCTEXT)
    OmniClass Number = "23.17.19.11.31" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "Control panel PVC" (IFCTEXT)
  Phasing | properties | on 2 objects (1 IFCDOOR, 1 IFCELECTRICDISTRIBUTIONPOINT)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCELECTRICDISTRIBUTIONPOINT)
    Reference = "Control panel PVC" (IFCIDENTIFIER)
  Electrical - Circuiting | properties | on 1 object (1 IFCELECTRICDISTRIBUTIONPOINT)
    Electrical Data = "400 V/3-4000 VA" (IFCTEXT)
    Supply From = "" (IFCTEXT)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  DO_WPB_Dynadry_BMP:Dynadry:118500 | predefined | on 1 type object
  DO_WPB_Dynadry_BMP:Dynadry:118500:1 | predefined | on 1 type object
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Materials and Finishes | properties | on 1 type object
    curtain_bottom_material = "Plastic, black" (IFCLABEL)
    curtain_material = "PVC" (IFCLABEL)
    frame_material = "Steel, stainless 304" (IFCLABEL)
    motor_cover_material = "Steel, stainless 304" (IFCLABEL)
    window_material = "Glass, transparent" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "PVC" (IFCLABEL)
  Visibility | properties | on 1 type object
    RSen_C_clashvolume = FALSE (IFCBOOLEAN)