IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2023-12-18T09:24:36"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.70.21 - Exporter 21.1.70.21 - Default UI"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1686682715 (2023-06-13T18:58:35Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "CEMCO-CST250:800CST250-68(50)" | object type "CEMCO-CST250:800CST250-68(50)" | names: "CEMCO-CST250:800CST250-68(50):107004" | material: "Steel, Galvanized" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "CEMCO-CST250:800CST250-68(50)" | 1 occurrence | material: "Steel, Galvanized" | property sets: Dimensions, Identity Data, Other, Structural, Structural Analysis, Pset_BuildingElementProxyCommon

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Structural Framing" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Structural Framing" (IFCLABEL)
    Family = "CEMCO-CST250: 800CST250-68(50)" (IFCLABEL)
    Family and Type = "CEMCO-CST250: 800CST250-68(50)" (IFCLABEL)
    Type = "CEMCO-CST250: 800CST250-68(50)" (IFCLABEL)
    Type Id = "CEMCO-CST250: 800CST250-68(50)" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Structural Framing" (IFCLABEL)
    Family Name = "CEMCO-CST250" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "800CST250-68(50)" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "CEMCO" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "800CST250-68(50)" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 5. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 5. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reported Length = 5. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 0.0321840277777774 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    bf = 0.208333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    d = 0.666666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    temp_t = 0.00594166666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    tf = 0.00594166666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Structural Material = "Steel, Galvanized" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B10" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "CEMCO CST Brand Slotted Tracks" (IFCTEXT)
    Keynote = "092216" (IFCTEXT)
    Manufacturer = "CEMCO" (IFCTEXT)
    Model = "V2" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Product Info = "CEMCO CST Slotted Tracks-Standard 2-1/2" Leg" (IFCTEXT)
    Product Submittal Info = "https://cemcosteel.com/product-category/cemco-cst-slotted-tracks-standard-2-1-2-leg/" (IFCTEXT)
    Type Name = "800CST250-68(50)" (IFCTEXT)
    URL = "https://cemcosteel.com/product-category/cemco-cst-slotted-tracks-standard-2-1-2-leg/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Structural | properties | on 1 type object
    A = 0.00173611111111111 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Section Shape = 20 (IFCINTEGER)
    W = 0.85 (IFCREAL)
  Structural Analysis | properties | on 1 type object
    Area = 0. (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Fy = 344737864.658418 (IFCPRESSUREMEASURE) [PASCAL]
    Ix = 0. (IFCMOMENTOFINERTIAMEASURE) [derived]
    Iy = 0. (IFCMOMENTOFINERTIAMEASURE) [derived]
    Mx = 0. (IFCREAL)
    Sx = 0. (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
    Vy = 0. (IFCFORCEMEASURE) [NEWTON]
    Weight = 3.1164 (IFCREAL)