IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2023-01-19T12:44:11"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCDOOR | type IFCDOORSTYLE "Door_Overhead-Coiling_CHI_6000-Insulated-Series:E Guide for Steel Structure with Urethane infill 115V" | object type "Door_Overhead-Coiling_CHI_6000-Insulated-Series:E Guide for Steel Structure with Urethane infill 115V" | names: "Door_Overhead-Coiling_CHI_6000-Insulated-Series:E Guide for Steel Structure with Urethane infill 115V:164365" | material: materials ("Metal - CHI - Black Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Silver Powdercoat Coarse Curtain") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints

Types
  IFCDOORSTYLE "Door_Overhead-Coiling_CHI_6000-Insulated-Series:E Guide for Steel Structure with Urethane infill 115V" | 1 occurrence | material: materials ("Metal - CHI - Black Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Black Powdercoat", "Metal - CHI - Silver Powdercoat", "Metal - CHI - Silver Powdercoat Coarse Curtain") | property sets: Door_Overhead-Coiling_CHI_6000-Insulated-Series:E Guide for Steel Structure with Urethane infill 115V:164365, Door_Overhead-Coiling_CHI_6000-Insulated-Series:E Guide for Steel Structure with Urethane infill 115V:164365:1, Analytical Model, Analytical Properties, Constraints, Construction

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "Door_Overhead-Coiling_CHI_6000-Insulated-Series" (IFCLABEL)
    Family and Type = "Door_Overhead-Coiling_CHI_6000-Insulated-Series: E Guide for Steel Structure with Urethane infill 115V" (IFCLABEL)
    Head Height = 9.2083333333333321 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "164355" (IFCLABEL)
    Type = "E Guide for Steel Structure with Urethane infill 115V" (IFCLABEL)
    Type Id = "164337" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Doors" (IFCLABEL)
    Family Name = "Door_Overhead-Coiling_CHI_6000-Insulated-Series" (IFCTEXT)
  Pset_ConcreteElementGeneral | properties | on 1 object (1 IFCDOOR) | on 1 type object
    FireRating = "As Specified in 08330" (IFCLABEL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireRating = "As Specified in 08330" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "E Guide for Steel Structure with Urethane infill 115V" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 type object
    FireRating = "As Specified in 08330" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Manufacturer = "CHI Overhead Doors" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDOOR)
    Reference = "E Guide for Steel Structure with Urethane infill 115V" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCDOOR)
    Sill Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Max Height = 25. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Max Width = 30. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    RO Offset = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCDOOR)
    Coil Control Station T = "[24V Keyed Switch][24V Keyed Switch with Stop Button][24V Two Button][24V Three Button]" (IFCTEXT)
    Lock Access Location = "[Coil Side][Fascia Side][Both Sides]" (IFCTEXT)
    Lock Mounting Point = "[Interior Mounted][Exterior Mounted][Keyed Both Sides]" (IFCTEXT)
    Operation_Chain Hoist = TRUE (IFCBOOLEAN)
    Operation_Manual Pushup = TRUE (IFCBOOLEAN)
    Operation_Motor_GH Motor = TRUE (IFCBOOLEAN)
    Operation_Motor_H Motor = TRUE (IFCBOOLEAN)
    Safety Option = "[Photoelectric Sensor][Electric Edge Two Wire][Electric Edge Four Wire][Pneumatic Reversing Edge][No Safety Device]" (IFCTEXT)
  Construction | properties | on 1 type object
    Function = "Interior" (IFCIDENTIFIER)
    Guide_Btwn Jamb = TRUE (IFCBOOLEAN)
    Guide_E Guide = TRUE (IFCBOOLEAN)
    Guide_Z Guide = FALSE (IFCBOOLEAN)
    Has Windlocks = FALSE (IFCBOOLEAN)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCDOOR)
    Area = 207.8569423577373 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Inset from Interior Face = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 44.66244533667367 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Height = 9.2083333333333321 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 9.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 9.0833333333333339 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Thickness = 0.020833333333333332 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 9. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Identity Data | properties | on 1 object (1 IFCDOOR)
    Mark = "18" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B2030420" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©Arcat Inc." (IFCTEXT)
    Description = "CHI Service Overhead Coiling Door - Model 6000 Insulated Service" (IFCTEXT)
    Drawn By = "Sumex Design, Inc. / Robert S. Weygant, CSI, CDT, SCIP" (IFCTEXT)
    Fire Rating = "As Specified in 08330" (IFCTEXT)
    Keynote = "08330" (IFCTEXT)
    Manufacturer = "CHI Overhead Doors" (IFCTEXT)
    Model = "6000 Insulated" (IFCTEXT)
    OmniClass Number = "23.30.10.17.27.11" (IFCTEXT)
    OmniClass Title = "Overhead Coiling" (IFCTEXT)
    Revision = "R1_02-2013" (IFCTEXT)
    Type Mark = "61" (IFCTEXT)
    Type Name = "E Guide for Steel Structure with Urethane infill 115V" (IFCTEXT)
    URL = "http://www.chiohd.com/garage-doors/" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCDOOR)
    Curtain Material for Coarse and Medium Views = "Metal - CHI - Silver Powdercoat Coarse Curtain" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Body Material = "Metal - CHI - Silver Powdercoat" (IFCLABEL)
    Frame Finish = "Metal - CHI - Black Powdercoat" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCDOOR)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Expected Lifespan (Years) = 0 (IFCINTEGER)
    Installation Phase = "" (IFCTEXT)
    Maintenance Schedule (Months) = 0 (IFCINTEGER)
    Warranty Duration (Years) = 0 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Door_Overhead-Coiling_CHI_6000-Insulated-Series:E Guide for Steel Structure with Urethane infill 115V:164365 | predefined | on 1 type object
  Door_Overhead-Coiling_CHI_6000-Insulated-Series:E Guide for Steel Structure with Urethane infill 115V:164365:1 | predefined | on 1 type object
  Analytical Model | properties | on 1 type object
    ASTM Conformance = "" (IFCTEXT)
    Air Infiltration = "" (IFCTEXT)
    R_Value = 6.7000000000000002 (IFCREAL)
    Sound Transmission Class (STC) = 0 (IFCINTEGER)
    Standards Conformance = "" (IFCTEXT)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Electrical Engineering | properties | on 1 type object
    Voltage_MEP = 115. (IFCELECTRICVOLTAGEMEASURE) [VOLT]