IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-01-03T10:37:48"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Overhead_Door-CHI_Overhead_Doors-MaxSpeed:MaxSpeed - 1200 - Safety Yellow - 1/4" Reinforced Rubber Curtain" | object type "Overhead_Door-CHI_Overhead_Doors-MaxSpeed:MaxSpeed - 1200 - Safety Yellow - 1/4" Reinforced Rubber Curtain" | names: "Overhead_Door-CHI_Overhead_Doors-MaxSpeed:MaxSpeed - 1200 - Safety Yellow - 1/4" Reinforced Rubber Curtain:264578" | material: materials ("Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Metal - C.H.I Overhead Doors - Safety Yellow", "Metal - C.H.I Overhead Doors - Safety Yellow", "Metal - C.H.I Overhead Doors - Safety Yellow", "Steel - C.H.I Overhead Doors - Gray", "Steel - C.H.I Overhead Doors - Gray", "Steel - C.H.I Overhead Doors - Gray", "Steel - C.H.I Overhead Doors - Gray", "Steel - C.H.I Overhead Doors - Gray", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction

Types
  IFCBUILDINGELEMENTPROXYTYPE "Overhead_Door-CHI_Overhead_Doors-MaxSpeed:MaxSpeed - 1200 - Safety Yellow - 1/4" Reinforced Rubber Curtain" | 1 occurrence | material: materials ("Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Metal - C.H.I Overhead Doors - Safety Yellow", "Metal - C.H.I Overhead Doors - Safety Yellow", "Metal - C.H.I Overhead Doors - Safety Yellow", "Steel - C.H.I Overhead Doors - Gray", "Steel - C.H.I Overhead Doors - Gray", "Steel - C.H.I Overhead Doors - Gray", "Steel - C.H.I Overhead Doors - Gray", "Steel - C.H.I Overhead Doors - Gray", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber", "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber") | property sets: Constraints, Dimensions, Electrical, Identity Data, Materials and Finishes, Model Properties

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    C Max Height = 30. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Max Width = 40. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Min Height = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Min Width = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Chain Length = 4.9140625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Family = "Overhead_Door-CHI_Overhead_Doors-MaxSpeed" (IFCLABEL)
    Family and Type = "Overhead_Door-CHI_Overhead_Doors-MaxSpeed: MaxSpeed - 1200 - Safety Yellow - 1/4" Reinforced Rubber Curtain" (IFCLABEL)
    H Array Number = 4 (IFCINTEGER)
    Host Id = "264568" (IFCLABEL)
    Motor Top Height = 0.96875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    No Hood = TRUE (IFCBOOLEAN)
    Shutterbox Length = 6.833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Type = "MaxSpeed - 1200 - Safety Yellow - 1/4" Reinforced Rubber Curtain" (IFCLABEL)
    Type Id = "264454" (IFCLABEL)
    V Array Number = 5 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Axis Offset from Top = 0.83333333333333337 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C Model = 4 (IFCINTEGER)
    Category = "Specialty Equipment" (IFCLABEL)
    Door Rail Depth = 0.5 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Rail Width = 0.41666666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Family Name = "Overhead_Door-CHI_Overhead_Doors-MaxSpeed" (IFCTEXT)
    H Motor = FALSE (IFCBOOLEAN)
    Motor Distance from Wall = 1.9687499999999998 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Motor Distance to Shutterbox = 0.65625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Motor Length = 1.9791666666666665 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Motor Side Offset = 1.1041666666666665 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Motor Vertical Offset from Top = 2.8125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Shutter Box Depth = 2. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Shutter Box Height = 2. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    V Motor = TRUE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "MaxSpeed - 1200 - Safety Yellow - 1/4" Reinforced Rubber Curtain" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "C.H.I. Overhead Doors" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "MaxSpeed - 1200 - Safety Yellow - 1/4" Reinforced Rubber Curtain" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Control Panel Offset from Door = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Control Panel Offset from Floor = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Hood Cover = FALSE (IFCBOOLEAN)
    Motor Cover = FALSE (IFCBOOLEAN)
    Vision Windows = FALSE (IFCBOOLEAN)
    Windows Size = "14" x 14" │ Contact Manufacturer for Sizing and Placements" (IFCTEXT)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 186.18287792784614 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Desired Opening Height = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Desired Opening Width = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Size Limits = "Min Size 6' x 6' │ Max Size 40'W x 30'H" (IFCTEXT)
    Opening Height = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Width = 6. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 19.894950197761023 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Motor Cover Distance from Wall = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Thickness = 0.020833333333333332 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B2030410" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©2024 C.H.I. Overhead Doors - a NUCOR® company All information presented is based on the specifications and features available at the time of printing and is subject to change without notice." (IFCTEXT)
    Description = "Hight Speed Springless Impactable Rubber Door" (IFCTEXT)
    Keynote = "08 30 00" (IFCTEXT)
    Manufacturer = "C.H.I. Overhead Doors" (IFCTEXT)
    Manufacturer Address = "1485 Sunrise Drive, Arthur, IL 61911" (IFCTEXT)
    Manufacturer Email = "mailto:aia@chiohd.com" (IFCTEXT)
    Manufacturer Fax Number = "800-677-2650" (IFCTEXT)
    Manufacturer Phone Number = "800-738-5006" (IFCTEXT)
    Model = "1200" (IFCTEXT)
    OmniClass Number = "23.30.10.21" (IFCTEXT)
    OmniClass Title = "Special Function Doors" (IFCTEXT)
    Product Documentation Link = "https://www.chiohd.com/hubfs/MaxSpeed.pdf" (IFCTEXT)
    Product Page URL = "https://www.chiohd.com/commercial-doors/high-performance/maxspeed" (IFCTEXT)
    Support Email = "mailito: support@bimsmith.com" (IFCTEXT)
    Support Phone = "(224) 699-9545" (IFCTEXT)
    Type Name = "MaxSpeed - 1200 - Safety Yellow - 1/4" Reinforced Rubber Curtain" (IFCTEXT)
    URL = "https://www.chiohd.com/" (IFCTEXT)
    Version = "2021-v1.a" (IFCTEXT)
    Warranty URL = "https://www.chiohd.com/support/warranty" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Electrical | properties | on 1 type object
    Apparent Load Phase 1 = 0. (IFCPOWERMEASURE) [WATT]
    Apparent Load Phase 2 = 0. (IFCPOWERMEASURE) [WATT]
    Apparent Load Phase 3 = 0. (IFCPOWERMEASURE) [WATT]
    Load Classification = "Motor" (IFCLABEL)
    Number of Poles = 3 (IFCINTEGER)
    Power Factor = 1. (IFCREAL)
    Voltage = 0. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materials and Finishes | properties | on 1 type object
    Curtain Material = "Rubber - C.H.I Overhead Doors - Reinforced Black Rubber" (IFCLABEL)
    Material = "Metal - C.H.I Overhead Doors - Safety Yellow" (IFCLABEL)
  Model Properties | properties | on 1 type object
    Closing Speed = "Up to 24 inches / second" (IFCTEXT)
    Opening Speed = "Up to 48 inches / second" (IFCTEXT)
    Steel Gauge = "1/4"" (IFCTEXT)