IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2024-04-08T10:05:55"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.70.21 - Exporter 21.1.70.21 - Default UI"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1686682715 (2023-06-13T18:58:35Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Electrical_Controls_Conspec_Primus-V-Ventilation-Controller:PRIMUS V - 120V AC" | object type "Electrical_Controls_Conspec_Primus-V-Ventilation-Controller:PRIMUS V - 120V AC" | names: "Electrical_Controls_Conspec_Primus-V-Ventilation-Controller:PRIMUS V - 120V AC:137004" | material: materials ("Conspec - Plastic - PC - Light Blue", "Conspec - Plastic - FR ABS - Grey", "Conspec - Plastic - PC - Black", "Conspec - Plastic - Green Transparent - Screen") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "Electrical_Controls_Conspec_Primus-V-Ventilation-Controller:PRIMUS V - 120V AC" | 1 occurrence | material: materials ("Conspec - Plastic - FR ABS - Grey", "Conspec - Plastic - PC - Light Blue") | property sets: Constraints, Data, Dimensions, Electrical, Electrical - Loads, Identity Data

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Electrical Fixtures" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Electrical Fixtures" (IFCLABEL)
    Family = "Electrical_Controls_Conspec_Primus-V-Ventilation-Controller: PRIMUS V - 120V AC" (IFCLABEL)
    Family and Type = "Electrical_Controls_Conspec_Primus-V-Ventilation-Controller: PRIMUS V - 120V AC" (IFCLABEL)
    Type = "Electrical_Controls_Conspec_Primus-V-Ventilation-Controller: PRIMUS V - 120V AC" (IFCLABEL)
    Type Id = "Electrical_Controls_Conspec_Primus-V-Ventilation-Controller: PRIMUS V - 120V AC" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Electrical Fixtures" (IFCLABEL)
    Family Name = "Electrical_Controls_Conspec_Primus-V-Ventilation-Controller" (IFCTEXT)
    z_120 = TRUE (IFCBOOLEAN)
    z_DC = FALSE (IFCBOOLEAN)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "PRIMUS V - 120V AC" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "CONSPEC Controls" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "PRIMUS V - 120V AC" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Depth = 0.440833333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Height = 0.753333333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.753333333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "None" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 1.27799454362572 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 0.253184731025509 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Depth = 0.440833333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Height = 0.753333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.753333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Circuiting | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Electrical Data = "Power Connector 120 V/3-0 VA" (IFCTEXT)
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Electrical - Loads | properties | on 1 type object
    Apparent Load = 0. (IFCPOWERMEASURE) [WATT]
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "23" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "D5030" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Date Created = "2023/10/17" (IFCTEXT)
    Date Updated = "2023/10/17" (IFCTEXT)
    Description = "PRIMUS V - CO and NO2 Detector for ventilation control in enclosed parking garages and other spaces subjected to toxic gases" (IFCTEXT)
    Keynote = "16000" (IFCTEXT)
    Manufacturer = "CONSPEC Controls" (IFCTEXT)
    Model = "PRIMUS V - 120V AC" (IFCTEXT)
    OmniClass Number = "23.85.30.21" (IFCTEXT)
    OmniClass Title = "Environmental Detection/Registration" (IFCTEXT)
    Product data url = "https://bimobject.com/conspec-controls/product/primus-v-ventilation-controller" (IFCTEXT)
    Type Name = "PRIMUS V - 120V AC" (IFCTEXT)
    URL = "https://www.conspec-controls.com/" (IFCTEXT)
    Version = 1 (IFCINTEGER)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Data | properties | on 1 type object
    Alarm = "4 custom alarm levels with off-delay timer, sensor Fail-High and Fail-Low alarms" (IFCTEXT)
    Input/Output = "3 RS485 scan ports, 6 Relay outputs (5A@ 30VDC), 2 channels 4-20mA outputs" (IFCTEXT)
    Operating Humidity = "0% to 95% RH Non-Condesing" (IFCTEXT)
    Operating Temperature = "-4°F to +122°F" (IFCTEXT)
    Software = "Conspec Subcon Windows Software" (IFCTEXT)
    User Interface = "IR remote control, 4 local tactile buttons, 1 local horn silence button, Built-in RS232 Port for PC connection" (IFCTEXT)
    Zoning = "Up to 12 programmable zones" (IFCTEXT)
  Electrical | properties | on 1 type object
    Frequency = 0. (IFCFREQUENCYMEASURE) [HERTZ]
    Maximum Current Consumption = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Number of Poles = 3 (IFCINTEGER)
    Power Factor = 0.8 (IFCREAL)
    Voltage = 120. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Voltage Range = "120V AC" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Product Material = "Conspec - Plastic - FR ABS - Grey" (IFCLABEL)
  Structural | properties | on 1 type object
    Weight = 0. (IFCREAL)