IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2025-12-03T10:29:08-05:00"
Preprocessor: "ODA SDAI 22.12"
Originating system: "23.0.11.19 - Exporter 23.0.11.19 - Default UI"
Application: "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)" | change NOCHANGE | created 1673537642 (2023-01-12T15:34:02Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Partition_Corflex_5600_Series_Inside_Pocket:Inside Pocket With Door Type 4" | object type "Partition_Corflex_5600_Series_Inside_Pocket:Inside Pocket With Door Type 4" | names: "Partition_Corflex_5600_Series_Inside_Pocket:Inside Pocket With Door Type 4:105540" | material: materials ("Corflex - Vinyl - Blizzard", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Vinyl - Blizzard", "<Unnamed>", "Corflex - Clearance beam and track", "<Unnamed>", "<Unnamed>", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Vinyl - Blizzard", "<Unnamed>", "<Unnamed>", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Vinyl - Blizzard") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Electrical - Loads

Types
  IFCBUILDINGELEMENTPROXYTYPE "Partition_Corflex_5600_Series_Inside_Pocket:Inside Pocket With Door Type 4" | 1 occurrence | material: materials ("Corflex - Vinyl - Blizzard", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Vinyl - Blizzard", "<Unnamed>", "Corflex - Clearance beam and track", "<Unnamed>", "<Unnamed>", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Vinyl - Blizzard", "<Unnamed>", "<Unnamed>", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Trim - Beige", "Corflex - Vinyl - Blizzard") | property sets: Constraints, Dimensions, Identity Data, Materials and Finishes, Other, Text

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Array Start Width = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Clg Hgt Control = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Family = "Partition_Corflex_5600_Series_Inside_Pocket" (IFCLABEL)
    Family and Type = "Partition_Corflex_5600_Series_Inside_Pocket: Inside Pocket With Door Type 4" (IFCLABEL)
    Field Decoration Allowance = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Finished Floor Thickness = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Flush Ceiling Track = FALSE (IFCBOOLEAN)
    Opening Back = 2.4524278215223099 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Front = 2.4524278215223099 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Height Auxiliary = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Finish Carpet = FALSE (IFCBOOLEAN)
    Panel Finish Vinyl = TRUE (IFCBOOLEAN)
    Panel Quantity Auxiliary = 9 (IFCINTEGER)
    Pocket Location = 3.5039370078740157 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Stack Depth Allowance = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Stack Spacing Plan = 0.30183727034120733 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Stack Spacing Plan Control = 0.15091863517060367 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Track Additional Perpendicular = FALSE (IFCBOOLEAN)
    Track Location Control = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Type = "Inside Pocket With Door Type 4" (IFCLABEL)
    Type Id = "105469" (IFCLABEL)
    Unit Height = 9.9166666666666661 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Bottom Seal Height = 0.125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Enter Pocket Door Type = 4 (IFCINTEGER)
    Family Name = "Partition_Corflex_5600_Series_Inside_Pocket" (IFCTEXT)
    Panel Width Max = 3.9993438320209975 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Width Min = 1.7486876640419948 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pocket With Door = TRUE (IFCBOOLEAN)
    Track Width Above = 0.29166666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Inside Pocket With Door Type 4" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Inside Pocket With Door Type 4" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Additional Panel Quantity = 0 (IFCINTEGER)
    Closure Width Lead 102 mm Only Available if Panel Quantity Exceeds 15 Panels = FALSE (IFCBOOLEAN)
    Closure Width Lead 114 mm Only Available if Panel Quantity Exceeds 15 Panels = FALSE (IFCBOOLEAN)
    Closure Width Lead 152 mm Only Available if Panel Quantity Exceeds 15 Panels = FALSE (IFCBOOLEAN)
    Closure Width Lead Calculated = 0.12467191601049868 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Contact Corflex for Opening Heights Above 4572mm = "" (IFCTEXT)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Height = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Width = 32.808398950131235 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Show Pocket Walls = TRUE (IFCBOOLEAN)
    Show Stacked = FALSE (IFCBOOLEAN)
    Total Panel Quantity = 9 (IFCINTEGER)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 1461.2617763100529 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Clearance Depth = 3.5039370078740157 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Clearance Width = 4.9048556430446197 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Thickness = 0.30183727034120733 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Width = 3.5761154855643045 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Width Stacked = 2.9101049868766404 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Partition Width = 32.808398950131235 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pocket Wall Thickness = 0.49868766404199472 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pocket Width Half = 2.4524278215223099 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Stack Depth = 2.841207349081365 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Track Distance = 2.9101049868766404 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Track Offset = 0.66601049868766404 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Track back offset = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Track center offset = 3.9370078740157473 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Track front offset = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 615.97695918678357 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Closure Width Lead Standard = 0.12467191601049868 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Closure Width Trail = 0.49868766404199472 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pocket Offset From Main Track = 0.99737532808398943 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pocket Offset From Transfer Track = 0.99737532808398943 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Track Height = 0.29166666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Track Width = 0.41666666666666669 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Pocket Door Type = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "C1010300" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    CAD Details = "https://www.arcat.com/company/corflex-partitions-inc-39436/cad" (IFCTEXT)
    CSI MasterFormat 2004 = "10 22 26" (IFCTEXT)
    CSI MasterFormat = "10 22 39" (IFCTEXT)
    Closure Type Lead = "Bulb Seal" (IFCTEXT)
    Closure Type Trail = "Lever" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "ARCAT" (IFCTEXT)
    Description = "Operable Partition" (IFCTEXT)
    Keynote = "10 22 26" (IFCTEXT)
    Manufacturer = "Corflex, Inc." (IFCTEXT)
    Manufacturer Telephone = "1 877 410-2422 or (1) 450 444-2441" (IFCTEXT)
    Model = "5600" (IFCTEXT)
    OmniClass Number = "23.25.40.17.11" (IFCTEXT)
    OmniClass Title = "Horizontally Sliding Partitions" (IFCTEXT)
    Product Page URL = "https://www.arcat.com/company/corflex-partitions-inc-39436" (IFCTEXT)
    Specification = "https://www.arcat.com/company/corflex-partitions-inc-39436/spec" (IFCTEXT)
    Type Name = "Inside Pocket With Door Type 4" (IFCTEXT)
    URL = "http://www.corflex.ca/" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Acoustic Seal = TRUE (IFCBOOLEAN)
    Show Extended = TRUE (IFCBOOLEAN)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Finish Material Metal = "Corflex - Trim - Beige" (IFCLABEL)
    Finish Material Panel = "Corflex - Vinyl - Blizzard" (IFCLABEL)
    Finish Material Pocket Door = "Corflex - Vinyl - Blizzard" (IFCLABEL)
    Finish Material Track = "Corflex - Track - Clear anodized" (IFCLABEL)
  Text | properties | on 1 type object
    Specification sheet = "https://corflex.ca/produits/cloisons-mobiles/" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "Corflex, Inc." (IFCLABEL)