IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2023-01-24T16:33:39"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20220517_1515(x64) - Exporter 20.2.90.12 - Default UI"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1671211015 (2022-12-16T17:16:55Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCDOOR | type IFCDOORSTYLE "Model 5210 Flush 2in" | object type "Overhead-Sect_HAAS_Res_Alum_5000:Model 5210 Flush 2in" | names: "Overhead-Sect_HAAS_Res_Alum_5000:Model 5210 Flush 2in:319372" | material: materials ("Metal - Steel - HAAS - Polar White", "Glass", "Finish - Trim - HAAS - Black", "Finish - Weather Seal - HAAS - Black", "Steel") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints

Types
  IFCDOORSTYLE "Model 5210 Flush 2in" | 1 occurrence | material: materials ("Metal - Steel - HAAS - Polar White", "Glass", "Finish - Trim - HAAS - Black", "Finish - Weather Seal - HAAS - Black", "Steel") | property sets: Overhead-Sect_HAAS_Res_Alum_5000:Model 5210 Flush 2in:319372, Analytical Model, Analytical Properties, Constraints, Construction, Dimensions

Property sets
  Pset_ConcreteElementGeneral | properties | on 1 object (1 IFCDOOR)
    ConstructionType (no value)
    FireRating (no value)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireRating (no value)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Model 5210 Flush 2in" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDOOR)
    Manufacturer = "Haas Door Co." (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDOOR)
    Reference = "Model 5210 Flush 2in" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCDOOR)
    Sill Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    End Stile Type = "Extruded End Cap" (IFCTEXT)
    Exterior Skin = "Flush Woodgrain Aluminum" (IFCTEXT)
    Interior Skin = "Aluminum Woodgrain" (IFCTEXT)
    Max Height = 12. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Max Width = 16. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCDOOR)
    Steel Jamb = FALSE (IFCBOOLEAN)
    Track Type = "Tracks_Standard-Lift" (IFCLABEL)
    Wood Jamb = TRUE (IFCBOOLEAN)
  Construction | properties | on 1 type object
    Construction Type = "" (IFCTEXT)
    Function = "Exterior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCDOOR)
    Area = 282.384675463773 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Opening Height = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Width = 14. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Height = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Width = 14. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Track_High Lift_CHECK WITH HAAS FOR VALUE = 0.583333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Unit Width = 14. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 39.424428695448 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Thickness = 0.166666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Thickness = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Width = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Graphics | properties | on 1 object (1 IFCDOOR)
    2in Track = TRUE (IFCBOOLEAN)
    3in Track = FALSE (IFCBOOLEAN)
    Overhead Sectional Style = "Design B" (IFCLABEL)
  Green Building Properties | properties | on 1 object (1 IFCDOOR)
    Recycled Content = "as Specified" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCDOOR)
    Mark = "31" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "B2030410" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "©Arcat Inc." (IFCTEXT)
    Cost = 0. (IFCREAL)
    Description = "Haas 5200 Series Residential Insulated Overhead Sectional Door - 5210 as Specified" (IFCTEXT)
    Drawn By = "Sumex Design, Inc." (IFCTEXT)
    Fire Rating = "" (IFCTEXT)
    Keynote = "08360" (IFCTEXT)
    Manufacturer = "Haas Door Co." (IFCTEXT)
    Model = "5210" (IFCTEXT)
    OmniClass Number = "23.30.10.17.37.14" (IFCTEXT)
    OmniClass Title = "Sectional Overhead Doors" (IFCTEXT)
    Revision = "R1_2015-11" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Mark = "86" (IFCTEXT)
    Type Name = "Model 5210 Flush 2in" (IFCTEXT)
    URL = "http://www.haasdoor.com/about/index.html" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCDOOR)
    Bottom Seal Color = "Finish - Weather Seal - HAAS - Black" (IFCLABEL)
    Panel Material_Exterior = "Metal - Steel - HAAS - Polar White" (IFCLABEL)
    Panel Material_Inset Panel = "Metal - Steel - HAAS - Polar White" (IFCLABEL)
    Panel Material_Interior = "Metal - Steel - HAAS - Polar White V-Groove" (IFCLABEL)
    Track = "Steel" (IFCLABEL)
    Viewport Frame Finish = "Finish - Trim - HAAS - Black" (IFCLABEL)
    Viewport Glazing = "Glass" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "Overhead-Sect_HAAS_Res_Alum_5000: Model 5210 Flush 2in" (IFCLABEL)
    Family and Type = "Overhead-Sect_HAAS_Res_Alum_5000: Model 5210 Flush 2in" (IFCLABEL)
    Head Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "Basic Wall: Wall 1" (IFCLABEL)
    Type = "Overhead-Sect_HAAS_Res_Alum_5000: Model 5210 Flush 2in" (IFCLABEL)
    Type Id = "Overhead-Sect_HAAS_Res_Alum_5000: Model 5210 Flush 2in" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Doors" (IFCLABEL)
    Family Name = "Overhead-Sect_HAAS_Res_Alum_5000" (IFCTEXT)
    Manufacturer Address = "320 Sycamore Rd. Wauseon, OH 43567" (IFCTEXT)
    Manufacturer Fax = "800-874-4227" (IFCTEXT)
    Manufacturer Phone - Toll Free = "" (IFCTEXT)
    Manufacturer Phone = "419-337-9900" (IFCTEXT)
    Manufacturer Website = "http://www.haasdoor.com/about/index.html" (IFCTEXT)
    Send Message = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCDOOR)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Expected Lifespan (Years) = 0 (IFCINTEGER)
    Installation Phase = "" (IFCTEXT)
    Maintenance Schedule (Months) = 0 (IFCINTEGER)
    Warranty Duration (Years) = 0 (IFCINTEGER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Overhead-Sect_HAAS_Res_Alum_5000:Model 5210 Flush 2in:319372 | predefined | on 2 type objects
  Analytical Model | properties | on 1 type object
    AAMA Designation = "as Specified" (IFCTEXT)
    Standards Conformance = "as Specified" (IFCTEXT)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Energy Analysis | properties | on 1 type object
    R-Value = 17.66 (IFCREAL)
    U Value = 0. (IFCREAL)
  General | properties | on 1 type object
    Roof Incline Default = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    rearspring = FALSE (IFCBOOLEAN)
  Text | properties | on 1 type object
    Building Codes = "" (IFCTEXT)
    Construction Details = "" (IFCTEXT)
    Green Building-LEED = "" (IFCTEXT)
    Installation-Fabrication = "" (IFCTEXT)
    Product Data = "http://www.arcat.com/arcatcos/cos32/arc32915.html" (IFCTEXT)
    Product Properties = "" (IFCTEXT)
    Sales Information = "http://www.haasdoor.com/locator/index.php" (IFCTEXT)
    SpecWizard = "" (IFCTEXT)
    Specification = "" (IFCTEXT)
    Test Data = "" (IFCTEXT)

Other addresses and roles
  2 x postal address (none given)