IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
Time stamp: "2023-01-25T13:47:40"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.30.34 - Exporter 22.5.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1674049610 (2023-01-18T13:46:50Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH:Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH" | object type "Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH:Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH" | names: "Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH:Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH:431573" | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH:Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH" | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Constraints, Construction, Dimensions, Green Building Properties, Identity Data, Other

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH" (IFCLABEL)
    Family and Type = "Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH: Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH" (IFCLABEL)
    Type = "Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH" (IFCLABEL)
    Type Id = "431539" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1582" (IFCLABEL)
  Other | properties | on 1 type object
    Annually = "Periodic inspections by a competent person are recommended by the manufacturer. InUK/Europe these are required under Regulation 5 of the Workplace (Health, Safety &Welfare) Regulations, the Work at Height Regulations and BS EN 365. The frequency willdepend upon the environment, location and usage but should be at least every 12 months.Walk and visually inspect the complete installed system in relation to the clients’ generalneeds. Establish if any modifications and/or additional products are required to reflectany refurbishment requirements or additional plant & equipment which have been installedand require access.Check installation configuration is complete as per the original installation drawing/plan.Ensure the system has not been modified or tampered with by unauthorised persons.Check all Kee Walk are in place as per the original drawing. This is essential for longevity ofthe roof.Check all fixings are in place and correctly torqued.Any galvanised components showing signs of corrosion should be wire brushed thoroughlyand galvanised spray/paint applied as appropriate. If rusted significantly, take digitalphotographs and include these in the inspection report. All component and assembledparts should be kept clean, using detergent if necessary, by wiping down with a wet clothor hosing with clean water, after which they should be wiped down with a dry cloth.Where toe-boards are fitted check the brackets that support the toe-board are in place andsufficiently torqued.Where applicable check fixings to walls/structures including cat ladder clamps are in placeand sufficiently torqued.If the Kee Walk becomes damaged in any, please arrange for inspection and any necessaryrepair or component replacement.." (IFCTEXT)
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Kee Safety" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 4.9015748031496074 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Height = 1.5097435926770928 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 5.2165354330708658 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 1 type object
    Width = 5.2165354330708658 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host = "Basic Wall : Wall 1" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 4. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Area = 30.044118868206226 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 9.5003484543827366 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Coverage Area = 16145.865625064584 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Gross Weight kg = "74" (IFCTEXT)
    Overall Height = 0.54790026246719159 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overall Length = 4.9015748031496065 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overall Width = 2.0341207349081363 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Shipping Weight kg = "74" (IFCTEXT)
    Width = 5.2165354330708658 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "KWM21" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    CE Approval = TRUE (IFCBOOLEAN)
    Code Name = "" (IFCTEXT)
    Description = "Kee Walk® System provides a safe, anti-slip, level walking surface for means of access to and across roofs. It provides ademarcation route which protects the roof membrane from unnecessary foot traffic and potential damage. Pre-assembledin 1,5m unit." (IFCTEXT)
    Design Country = "United Kingdom" (IFCTEXT)
    Features = "Modular Rooftop walkway to EN 516" (IFCTEXT)
    Manufacturer = "Kee Safety" (IFCTEXT)
    Manufacturer Country = "United Kingdom" (IFCTEXT)
    Manufacturer Website = "www.keesafety.co.uk" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Product Literature = "https://keesafety.co.uk/images/uploads/uk/documents/Kee_Walk_Brochure_1.pdf" (IFCTEXT)
    Product Model Number = "WW721ASSY" (IFCTEXT)
    Product Range = "KeeWalk" (IFCTEXT)
    Type Name = "Kee_Safety_KWM21_1_5M_FREE_STANDING_MODULE_75MPH" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Construction | properties | on 1 type object
    Colour = "Tread Black" (IFCTEXT)
    Finish = "Annodized Aluminium" (IFCTEXT)
    Material = "Aluminum" (IFCLABEL)
    Product Family = "KeeWalk" (IFCTEXT)
    Product Group = "KeeWalk" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    Location of Manufacturer = "Cradley Heath" (IFCTEXT)