IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2024-06-06T07:05:45"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.70.21 - Exporter 21.1.70.21 - Default UI"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1686682715 (2023-06-13T18:58:35Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Doors_Industrial_Overhead-Door-Corporation_Counter-Doors-651:Manual crank" | object type "Doors_Industrial_Overhead-Door-Corporation_Counter-Doors-651:Manual crank" | names: "Doors_Industrial_Overhead-Door-Corporation_Counter-Doors-651:Manual crank:120735" | material: materials ("Stainless Steel - Overhead Door - #4 Finish", "Metal - White", "Finish - Overhead Door - Black") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction

Types
  IFCBUILDINGELEMENTPROXYTYPE "Doors_Industrial_Overhead-Door-Corporation_Counter-Doors-651:Manual crank" | 1 occurrence | material: materials ("Finish - Overhead Door - Black", "Stainless Steel - Overhead Door - #4 Finish") | property sets: Constraints, Construction, Electrical, Identity Data, Materials and Finishes, Other

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Array = 11 (IFCINTEGER)
    Array Length = 9.46028645833333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Array Real = 11 (IFCINTEGER)
    Array Vis = TRUE (IFCBOOLEAN)
    BJ Opening Cut = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Bar = TRUE (IFCBOOLEAN)
    Category = "Specialty Equipment" (IFCLABEL)
    Countertop Thickness Real = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Height (Real) = 9.16666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Height True = 11.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Width (Real) = 10.0625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Width True = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Face of Wall Offset = 0.416666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Family = "Doors_Industrial_Overhead-Door-Corporation_Counter-Doors-651: Manual crank" (IFCLABEL)
    Family and Type = "Doors_Industrial_Overhead-Door-Corporation_Counter-Doors-651: Manual crank" (IFCLABEL)
    Floor To CL shaft = 9.64583333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Guide Depth = 0.177083333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Guide Width 1 = 0.229166666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Guide Width 2 = 0.229166666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Headplate Offset = 0.135416666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Headroom Height Real = 1.125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Hood Height = 0.958333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Hood Offset = 0.166666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Hood Option = 2 (IFCINTEGER)
    Host Id = "Basic Wall: Wall 1" (IFCLABEL)
    Installation Limits = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Installation Real = 0.666666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Jamb Offset 1 = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Jambs Offset 2 = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Lookup BD = 0.958333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Lookup HH = 0.958333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Motor Option Real = 1 (IFCINTEGER)
    Motor Position = 0.135416666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    One Array element = FALSE (IFCBOOLEAN)
    Opening Height Real = 9. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Width Real = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Setback = 0.0729166666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Slat = 1 (IFCINTEGER)
    Slat Center Offset = 0.0885416666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Slat Height = 0.860026041666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Slat Length = 10.0729166666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Type = "Doors_Industrial_Overhead-Door-Corporation_Counter-Doors-651: Manual crank" (IFCLABEL)
    Type Id = "Doors_Industrial_Overhead-Door-Corporation_Counter-Doors-651: Manual crank" (IFCLABEL)
    Wall Thickness = 0.666666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Warning Sign = FALSE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
    Connector Array = 3 (IFCINTEGER)
    Connector Array Distance = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Crank = TRUE (IFCBOOLEAN)
    Electric Operator = FALSE (IFCBOOLEAN)
    Family Name = "Doors_Industrial_Overhead-Door-Corporation_Counter-Doors-651" (IFCTEXT)
    Lookup Table = "Hood Dimensions" (IFCTEXT)
    Manual = FALSE (IFCBOOLEAN)
    Operator Visibility = TRUE (IFCBOOLEAN)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Manual crank" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Overhead Door Corporation" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Manual crank" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Max Opening Height = 9. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Max Opening Width = 20. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Min Opening Height = 3.33333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Min Opening Width = 3.33333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Aluminum Guide = TRUE (IFCBOOLEAN)
    Between Jambs Mounting = FALSE (IFCBOOLEAN)
    Face Of Wall Mounting = TRUE (IFCBOOLEAN)
    Guide Option = 1 (IFCINTEGER)
    Guide Type = "Face of Wall Extruded Aluminum" (IFCTEXT)
    Hood Type = "Square Hood" (IFCTEXT)
    Motor Option = 1 (IFCINTEGER)
    Motor Selection (Note) = "Generic operator shown. Contact Overhead Door when dimensions are critical." (IFCTEXT)
    Motor Type = "CDX Electric Operator" (IFCTEXT)
    Operation (Note) = "Standard door operation is manual push-up. Door could also operate by crank, electrical operator or chain hoist. Manual push up and crank could be used up to 80 sf." (IFCTEXT)
    Slat Type = "F-158" (IFCTEXT)
    Steel \ Stainless Steel Guide = FALSE (IFCBOOLEAN)
  Construction | properties | on 1 type object
    Wall Closure = "By host" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 287.898574963401 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Backroom Depth = 0.958333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Calculated Area = 92.2395833333334 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Clear Height = 9. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Clear Width = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Countertop Thickness = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Default Elevation Height = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Floor To (CL) of Shaft = 12.6458333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Headroom Height = 1.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Installation Offset = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Height = 9. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Width = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    True Opening Height = 9. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    True Opening Width = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 11.6029140537932 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
    Warning (Note) = "" (IFCTEXT)
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Hood Material = "Stainless Steel - Overhead Door - #4 Finish" (IFCLABEL)
    Material Finish = "Standard - Stainless #4" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Finish Material = "Finish - Overhead Door - Black" (IFCLABEL)
    Powder Coat (Note) = "PowderGuard® Premium powder coat finish options are available in approximately 200 colors as well as custom matching to specification. PowderGuard® Textured finish, a thicker, more scratch resistant coat, is available in 11 colors providing enhanced scratch resistance as well as aiding in hiding the dirt and blemishes that often occur in commercial environments.​" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Model 651 Rolling Counter Door" (IFCTEXT)
    Manufacturer = "Overhead Door Corporation" (IFCTEXT)
    Model = "651" (IFCTEXT)
    OmniClass Number = "23.30.10.21.34" (IFCTEXT)
    OmniClass Title = "Industrial Doors" (IFCTEXT)
    Product Guid = "fdcc4cb0-6b7c-4503-b5ba-f17c1e96cb91" (IFCTEXT)
    Product Page URL = "https://www.overheaddoor.com/counter-doors-651" (IFCTEXT)
    Product data url = "https://www.bimobject.com/overhead-door/product/counter-doors-651" (IFCTEXT)
    Type Name = "Manual crank" (IFCTEXT)
    URL = "https://www.overheaddoor.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Electrical | properties | on 1 type object
    Apparent Load Phase 1 = 0. (IFCPOWERMEASURE) [WATT]
    Apparent Load Phase 2 = 0. (IFCPOWERMEASURE) [WATT]
    Apparent Load Phase 3 = 0. (IFCPOWERMEASURE) [WATT]
    Current = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Frequency = 0. (IFCFREQUENCYMEASURE) [HERTZ]
    Number of Poles = 1 (IFCINTEGER)
    Power Factor = 1. (IFCREAL)
    Voltage = 0. (IFCELECTRICVOLTAGEMEASURE) [VOLT]