IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2024-05-24T12:44:18"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.70.21 - Exporter 21.1.70.21 - Default UI"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1686682715 (2023-06-13T18:58:35Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Doors_Industrial_Overhead-Door-Corporation_Insulated-Wind-Load-Sectional-Door-429:Chain Hoist" | object type "Doors_Industrial_Overhead-Door-Corporation_Insulated-Wind-Load-Sectional-Door-429:Chain Hoist" | names: "Doors_Industrial_Overhead-Door-Corporation_Insulated-Wind-Load-Sectional-Door-429:Chain Hoist:122479" | material: materials ("Metal - Overhead Door - Clear", "Clearance - Overhead Door - Red", "Finish - Overhead Door - White (Microgroove Panel)", "Glass - Overhead Door - DSB", "Plastic - Overhead Door - Nylon") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction

Types
  IFCBUILDINGELEMENTPROXYTYPE "Doors_Industrial_Overhead-Door-Corporation_Insulated-Wind-Load-Sectional-Door-429:Chain Hoist" | 1 occurrence | material: materials ("Glass - Overhead Door - DSB", "Finish - Overhead Door - White (Microgroove Panel)", "Metal - Overhead Door - Clear") | property sets: Constraints, Construction, Dimensions, Electrical, Identity Data, Other

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Array of Panels Up and Down = 5 (IFCINTEGER)
    Bottom Rail (Width) = 0.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "Doors_Industrial_Overhead-Door-Corporation_Insulated-Wind-Load-Sectional-Door-429: Chain Hoist" (IFCLABEL)
    Family and Type = "Doors_Industrial_Overhead-Door-Corporation_Insulated-Wind-Load-Sectional-Door-429: Chain Hoist" (IFCLABEL)
    High = TRUE (IFCBOOLEAN)
    Host Id = "Basic Wall: Wall 1" (IFCLABEL)
    Lift Option Real = 2 (IFCINTEGER)
    Low Headroom (Springs to Front) = FALSE (IFCBOOLEAN)
    Low Headroom (Springs to Rear) = FALSE (IFCBOOLEAN)
    Opening Height = 9.91666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Opening Width = 9.83333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overlapping Horizontal = 0.166666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overlapping Vertical = 0.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pitch (Real) = 1.19347033367446 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Real Height = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Real Width = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Section 4 Windows Real = FALSE (IFCBOOLEAN)
    Section 5 = TRUE (IFCBOOLEAN)
    Section 5 Windows Real = FALSE (IFCBOOLEAN)
    Section 6 = FALSE (IFCBOOLEAN)
    Section Height = 1.98333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Sections Array = 2 (IFCINTEGER)
    Sections Array Visibility = FALSE (IFCBOOLEAN)
    Standard = FALSE (IFCBOOLEAN)
    Top Rail (Width) = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Type = "Doors_Industrial_Overhead-Door-Corporation_Insulated-Wind-Load-Sectional-Door-429: Chain Hoist" (IFCLABEL)
    Type Id = "Doors_Industrial_Overhead-Door-Corporation_Insulated-Wind-Load-Sectional-Door-429: Chain Hoist" (IFCLABEL)
    Vertical = FALSE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Array Count = 2 (IFCINTEGER)
    Array Offset = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Specialty Equipment" (IFCLABEL)
    Chain Hoist = TRUE (IFCBOOLEAN)
    Family Name = "Doors_Industrial_Overhead-Door-Corporation_Insulated-Wind-Load-Sectional-Door-429" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Chain Hoist" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Overhead Door Corporation" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Chain Hoist" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Max Door Height = 24.0833333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Max Door Width = 14.1666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Max Headroom (High Lift Option) = 9.375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Max Pitch = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Min Door Height = 8.08333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Min Door Width = 8.16666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Min Headroom (High Lift Option) = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Min Pitch = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    2 Inch Track = TRUE (IFCBOOLEAN)
    3 Inch Track = FALSE (IFCBOOLEAN)
    Lift Option = 1 (IFCINTEGER)
    Lift Type = "High Lift" (IFCTEXT)
    Overlapping Door = TRUE (IFCBOOLEAN)
    Section 3 Windows = TRUE (IFCBOOLEAN)
    Section 4 Windows = FALSE (IFCBOOLEAN)
    Section 5 Windows = FALSE (IFCBOOLEAN)
    Section Windows (Note) = "More than one section windows unavailable, due to the high wind load" (IFCTEXT)
    Side Mount Operator = TRUE (IFCBOOLEAN)
    Trolley Operator = FALSE (IFCBOOLEAN)
    Wind Load (Note) = "Many windload options available. Contact Overhead Door distributor for details" (IFCTEXT)
  Construction | properties | on 1 type object
    Wall Closure = "By host" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 1230.51047103781 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Backroom Depth = 10.0416666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Depth into Room = 10.0416666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Height = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Door Width = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Floor To (CL) of Shaft = 12.4270833333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Headroom Height = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Headroom Note (High Lift Option) = "Headroom Height cannot exceed Opening Height - 6.5 inch" (IFCTEXT)
    High Lift Amount = 2.04166666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    High Lift Headroom Available = 3. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pitch = 1.19347033367446 (IFCREAL)
    Pitch Angle = 1.19347033367446 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Rough Height = 9.91666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Rough Width = 9.83333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Thickness = 0.166666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    True Height = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    True Width = 10. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Volume = 184.657721865904 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    End Stile (Width) = 0.276041666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Clearance = TRUE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Glass Material = "Glass - Overhead Door - DSB" (IFCLABEL)
    Panel Material = "Finish - Overhead Door - White (Microgroove Panel)" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Model 429 insulated ribbed face 24GA steel windload door R-value 7.6, U-factor .13" (IFCTEXT)
    Manufacturer = "Overhead Door Corporation" (IFCTEXT)
    Model = "429" (IFCTEXT)
    OmniClass Number = "23.30.10.21.34" (IFCTEXT)
    OmniClass Title = "Industrial Doors" (IFCTEXT)
    Product Guid = "5505b900-7bfd-453b-9caf-b0dbec117f44" (IFCTEXT)
    Product Page URL = "https://www.overheaddoor.com/insulated-wind-load-door-429" (IFCTEXT)
    Product data url = "https://www.bimobject.com/overhead-door/product/insulated-wind-load-sectional-doors-429" (IFCTEXT)
    Type Name = "Chain Hoist" (IFCTEXT)
    URL = "https://www.overheaddoor.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Electrical | properties | on 1 type object
    Apparent Load Phase 1 = 0. (IFCPOWERMEASURE) [WATT]
    Apparent Load Phase 2 = 0. (IFCPOWERMEASURE) [WATT]
    Apparent Load Phase 3 = 0. (IFCPOWERMEASURE) [WATT]
    Current = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Frequency = 0. (IFCFREQUENCYMEASURE) [HERTZ]
    Number of Poles = 1 (IFCINTEGER)
    Power Factor = 1. (IFCREAL)
    Voltage = 0. (IFCELECTRICVOLTAGEMEASURE) [VOLT]