IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2023-01-26T15:37:58"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20220517_1515(x64) - Exporter 20.2.90.12 - Default UI"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "billatarcat9MS5L" of Organization (no name given)
  Owner history of Person "billatarcat9MS5L" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1671211015 (2022-12-16T17:16:55Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "32' - 3"" | object type "Partition-17_Panels_High-Skyfold_Classic_Compact-32-3_to_34-2_FC_9830_to_10415:32' - 3"" | names: "Partition-17_Panels_High-Skyfold_Classic_Compact-32-3_to_34-2_FC_9830_to_10415:32' - 3":199247" | material: materials ("Cut mat", "Default", "Plastic_Seal") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction

Types
  IFCBUILDINGELEMENTPROXYTYPE "32' - 3"" | 1 occurrence | material: materials ("Cut mat", "Default", "Plastic_Seal") | property sets: Constraints, Dimensions, Identity Data, Other, Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "32' - 3"" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Skyfold" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "32' - 3"" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Offset From Ceiling = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Top Of Acoustic Barrier = 42. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Total Wall Length = 32. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 4337.53055030912 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Volume = 650.358182486321 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    Acoustic Barrier"C" = 36.8125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Beam Height"B" = 38.4583333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Finished Ceiling"A" = 32.25 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Panel Height"F" = 2.10416666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pocket Depth"D" = 4.64583333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Pocket Width"E" = 5.1875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Fold = FALSE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Panel 1 Material = "Default" (IFCLABEL)
    Panel 10 Material = "Default" (IFCLABEL)
    Panel 11 Material = "Default" (IFCLABEL)
    Panel 12 Material = "Default" (IFCLABEL)
    Panel 13 Material = "Default" (IFCLABEL)
    Panel 14 Material = "Default" (IFCLABEL)
    Panel 15 Material = "Default" (IFCLABEL)
    Panel 16 Material = "Default" (IFCLABEL)
    Panel 17 Material = "Default" (IFCLABEL)
    Panel 2 Material = "Default" (IFCLABEL)
    Panel 3 Material = "Default" (IFCLABEL)
    Panel 4 Material = "Default" (IFCLABEL)
    Panel 5 Material = "Default" (IFCLABEL)
    Panel 6 Material = "Default" (IFCLABEL)
    Panel 7 Material = "Default" (IFCLABEL)
    Panel 8 Material = "Default" (IFCLABEL)
    Panel 9 Material = "Default" (IFCLABEL)
    Pocket Material = "Default" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Center Pantograph Visibility = TRUE (IFCBOOLEAN)
    Center Pantographs = 3 (IFCINTEGER)
    Distance Between Panels = 7.96875 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Family = "Partition-17_Panels_High-Skyfold_Classic_Compact-32-3_to_34-2_FC_9830_to_10415: 32' - 3"" (IFCLABEL)
    Family and Type = "Partition-17_Panels_High-Skyfold_Classic_Compact-32-3_to_34-2_FC_9830_to_10415: 32' - 3"" (IFCLABEL)
    Height Between Panels = 2.14583333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Host Id = "Basic Wall: Wall 1" (IFCLABEL)
    Max Panel Length = 8. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Max Wall Length = 100. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Motor Positioning = 12.0364583333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Number Of Panels = 4 (IFCINTEGER)
    Panel Array = 4 (IFCINTEGER)
    Panel Length = 7.92708333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Type = "Partition-17_Panels_High-Skyfold_Classic_Compact-32-3_to_34-2_FC_9830_to_10415: 32' - 3"" (IFCLABEL)
    Type Id = "Partition-17_Panels_High-Skyfold_Classic_Compact-32-3_to_34-2_FC_9830_to_10415: 32' - 3"" (IFCLABEL)
    Unfold = TRUE (IFCBOOLEAN)
    Visibility Of Fold Panels = FALSE (IFCBOOLEAN)
    Visibility Of Fold Single Panel = FALSE (IFCBOOLEAN)
    Visibility Of Single Pantograph = FALSE (IFCBOOLEAN)
    Visibility Of Unfold Single Panel = FALSE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Generic Models" (IFCLABEL)
    Distance From Acoustic Barrier = 0.166666666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Family Name = "Partition-17_Panels_High-Skyfold_Classic_Compact-32-3_to_34-2_FC_9830_to_10415" (IFCTEXT)
    Total Panel Height = 36.4375 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Wall Thickness = 0.979166666666667 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Custom Powerlift Partitions" (IFCTEXT)
    Manufacturer = "Skyfold" (IFCTEXT)
    Model = "Compact Drive System" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "32' - 3"" (IFCTEXT)
    URL = "http://www.skyfold.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)

Other addresses and roles
  2 x postal address (none given)