SECTION 10 21 16

SHOWER DOORS AND ENCLOSURES

Display hidden notes to specifier. (Don't know how? [Click Here](https://www.arcat.com/sd/display_hidden_notes.shtml))

*Copyright 2009 - 2023 ARCAT, Inc. - All rights reserved*

\*\* NOTE TO SPECIFIER \*\* American Shower Door, Inc.; shower doors, sliding enclosures, and doors with panels.  
This section is based on the products ofAmerican Shower Door, Inc., which is located at:  
4019 Medford St.  
Los Angeles, CA 90063  
Phone: 323.726.2478  
Fax: 323.726.7469  
Email: inquiry@americanshowerdoor.com  
Web: [www.americanshowerdoor.com](http://www.americanshowerdoor.com)   
[Click Here] for additional information.  
American Shower Door Corporation is the premier manufacturer of shower enclosure systems. Since 1935, we have supplied products worldwide to customers who share in our commitment to maintain the highest levels of quality, design, and service.  
You may choose from an unlimited selection of creative products. Select solid brass (plated to your specification), anodized aluminum, or stainless steel metal to combine with hundreds of glass options from 3/16 inches (5 mm) to 3/4 inches (19 mm) thick. Framed or frameless, standard or a creative new design, remember to call American Shower Door to produce the exact product to fit your construction.

1. GENERAL
   1. SECTION INCLUDES

\*\* NOTE TO SPECIFIER\*\* Delete work not included.

* + 1. Shower doors.
    2. Sliding enclosures.
    3. Shower doors and panels.
  1. RELATED SECTIONS

\*\* NOTE TO SPECIFIER \*\* Delete any sections below not relevant to this project; add others as required.

* + 1. Section 06 10 00 - Rough Carpentry.
    2. Section 22 40 00 - Plumbing Fixtures; coordination with plumbing fixtures.
  1. REFERENCES

\*\* NOTE TO SPECIFIER \*\* Delete references from the list below that are not actually required by the text of the edited section.

* + 1. ADA and ABA Accessibility Guidelines for Buildings and Facilities.
  1. SUBMITTALS
     1. Submit under provisions of Section 01 30 00 - Administrative Requirements.
     2. Product Data: Manufacturer's data sheets on each product to be used, including:
        1. Preparation instructions and recommendations.
        2. Storage and handling requirements and recommendations.
        3. Installation and maintenance methods.
     3. Shop Drawings: Show plans, elevations and installation details including attachment to adjacent construction.
     4. Verification Samples: For each finish product specified, two samples, minimum size 2 inches (52 mm) square, representing frame finish and glass type.
  2. QUALITY ASSURANCE
     1. Manufacturer Qualifications: Firm specializing in manufacture of shower door assemblies since 1935. More than a minimum 10 years' experience.

\*\* NOTE TO SPECIFIER \*\* Include a mock-up if the project size and/or quality warrant taking such a precaution. The following is one example of how a mock-up on a large project might be specified. When deciding on the extent of the mock-up, consider all the major different types of work on the project.

* + 1. Mock-Up: Provide a mock-up for evaluation of materials and application workmanship.
       1. Install in areas designated by Architect.
       2. Do not proceed with remaining work until workmanship is approved by Architect.
       3. Remodel mock-up installation as required to produce acceptable work.

\*\* NOTE TO SPECIFIER \*\* Delete if not applicable.

* + 1. Accessibility Requirements: Shower door assemblies shall comply with ADA-ABA Accessibility Guidelines.
  1. DELIVERY, STORAGE, AND HANDLING
     1. Deliver and store packaged materials in original containers. Prevent damage or contamination to materials by construction activities.
  2. PROJECT CONDITIONS
     1. Verify field dimensions prior to fabrication to the greatest extent practical.

1. PRODUCTS
   1. MANUFACTURERS
      1. Acceptable Manufacturer: American Shower Door, Inc., which is located at: 4019 Medford St.; Los Angeles, CA 90063; Tel: 323-726-2478; Fax: 323-726-7469; Email: [request info (inquiry@americanshowerdoor.com)](https://admin.arcat.com/users.pl?action=UserEmail&company=American+Shower+Door,+Inc.&coid=30443&rep=&fax=323-726-7469&message=RE:%20Spec%20Question%20(10185asd):%20%20&mf=); Web: <http://www.americanshowerdoor.com>

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions.

* + 1. Substitutions: Not permitted.
    2. Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
    3. Obtain products from a single manufacturer.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required.

* 1. SHOWER DOORS

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Maximum stability in frameless shower, 0 to 1 inch adjustment available.

* + 1. Semi-Frameless Aluminum Shower Doors:
       1. Model: Elite 502 by American Shower Door.
       2. Hinge: Piano hinge.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimension options not applicable.

* + - 1. Glass Dimensions: 70 inches (1778 mm) high by width indicated.
      2. Glass Dimensions: 84 inches (2438 mm) high by width indicated.
      3. Glass Dimensions: Size indicated on the Drawings.
      4. Glass Thickness: 1/4 inch (6 mm) tempered glass.

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Slim profile with framed pivot, 0 to 1 inch adjustment available.

* + 1. Framed Aluminum Shower Doors:
       1. Model: Limited 202 by American Shower Door.
       2. Hinge: Pivot.
       3. Rail Framing: 200 Rail.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimension options not applicable.

* + - 1. Glass Dimensions: 70 inches (1778 mm) high by width indicated.
      2. Glass Dimensions: 74 inches (1880 mm) high by width indicated.
      3. Glass Dimensions: Size indicated on the Drawings.
      4. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Maximum 2 inches adjustment for heavy duty.

* + 1. Framed Aluminum Shower Doors:
       1. Model: Magnum 212 by American Shower Door.
       2. Hinge: Pivot.
       3. Rail Framing: 200 Rail.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimensions options not applicable.

* + - 1. Glass Dimensions: 63-5/16 inches (1608 mm) high by width indicated.
      2. Glass Dimensions: 69-5/16 inches (1761 mm) high by width indicated.
      3. Glass Dimensions: Size indicated on the Drawings.
      4. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Commercial modular design meets 36 barrier free requirements, maximum 2 inch adjustment available for heavy duty application.

* + 1. Framed Aluminum Heavy Duty Shower Doors:
       1. Model: Atlas 353 by American Shower Door.
       2. Hinge: Pivot.
       3. Rail Framing: 355 Rail.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimensions options not applicable.

* + - 1. Glass Dimensions: 63-5/16 inches (1608 mm) high by width indicated.
      2. Glass Dimensions: 69-5/16 inches (1761 mm) high by width indicated.
      3. Glass Dimensions: Size indicated on the Drawings.
      4. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + 1. Framed Aluminum Shower Doors:
       1. Model: Classic 220 by American Shower Door.
       2. Rail Framing: 200 Rail.

\*\* NOTE TO SPECIFIER \*\* Delete hinge option not applicable.

* + - 1. Hinge: Piano Hinge. Regular.
      2. Hinge: Piano Hinge. Steam.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimensions options not applicable.

* + - 1. Glass Dimensions: 70 inches (1778 mm) high by width indicated.
      2. Glass Dimensions: 84 inches (2134 mm) high by width indicated.
      3. Glass Dimensions: Size indicated on the Drawings.
      4. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + 1. Framed Aluminum Heavy Duty Shower Doors:
       1. Model: Max 355 by American Shower Door.
       2. Rail Framing: 355 Rail.

\*\* NOTE TO SPECIFIER \*\* Delete hinge option not applicable.

* + - 1. Hinge: Piano Hinge. Regular.
      2. Hinge: Piano Hinge. Steam.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimensions options not applicable.

* + - 1. Glass Dimensions: 70 inches (1778 mm) high by width indicated.
      2. Glass Dimensions: 96 inches (2438 mm) high by width indicated.
      3. Glass Dimensions: Size indicated on the Drawings.
      4. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + 1. Crystal Collection Heavy Glass Shower Doors; Fframeless:
       1. Model: Crystal 802 by American Shower Door.
       2. Hardware: Brass.
       3. Extrusions: Aluminum.

\*\* NOTE TO SPECIFIER \*\* Delete hinge options not applicable.

* + - 1. Hinge: Pivots.
      2. Hinge: Wall to glass.
      3. Hinge: Glass to glass.
      4. Hinge: Custom. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete fixed panel options not required.

* + - 1. Fixed Panel: Channel.
      2. Fixed Panel: Clips.
      3. Door Pulls: At 2 inch (52 mm) increments from 6 to 30 inches (152 to 762 mm)

\*\* NOTE TO SPECIFIER \*\* Delete transom option not required.

* + - 1. Transoms: Operable.
      2. Transoms: Fixed.

\*\* NOTE TO SPECIFIER \*\* 40 lb capacity per hinge.

* + - 1. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness and glass appearance options not applicable.

* + - 1. Glass Thickness: 3/8 inch (9.5 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Rain.
         4. Glass Appearance: Bubbles.
         5. Glass Appearance: Acid Etch.
         6. Glass Appearance: Low Iron Acid Etch.
         7. Glass Appearance: Clear Showergaurd.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: Antique.
         10. Glass Appearance: As selected by Architect.
      2. Glass Thickness: 1/2 inch (12.7 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Acid Etch.
         4. Glass Appearance: Low Iron Acid Etch.
         5. Glass Appearance: Clear Showergaurd.
         6. Glass Appearance: Low Iron Showergaurd.
         7. Glass Appearance: Antique.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: As selected by Architect.
      3. Glass Thickness: 3/4 inch (19 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Antique.
         4. Glass Appearance: As selected by Architect.

\*\* NOTE TO SPECIFIER \*\* Delete option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Frameless heavy glass-leakproof jambs or wall mount option.

* + 1. All Brass Crystal Collection Heavy Glass Shower Doors; Frameless:
       1. Model: Crystal 902 by American Shower Door.
       2. Hardware: Brass.
       3. Extrusions: Brass.

\*\* NOTE TO SPECIFIER \*\* Delete hinge options not applicable.

* + - 1. Hinge: Pivots.
      2. Hinge: Wall to glass.
      3. Hinge: Glass to glass.
      4. Hinge: Custom. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete fixed panel options not required.

* + - 1. Fixed Panel: Channel.
      2. Fixed Panel: Clips.
      3. Door Pulls: At 2 inch (52 mm) increments from 6 to 30 inches (152 to 762 mm).

\*\* NOTE TO SPECIFIER \*\* Delete transoms option not required.

* + - 1. Transoms: Operable.
      2. Transoms: Fixed.

\*\* NOTE TO SPECIFIER \*\* 40 lb capacity per hinge.

* + - 1. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness and glass appearance options not applicable.

* + - 1. Glass Thickness: 3/8 inch (9.5 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Rain.
         4. Glass Appearance: Bubbles.
         5. Glass Appearance: Acid Etch.
         6. Glass Appearance: Low Iron Acid Etch.
         7. Glass Appearance: Clear Showergaurd.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: Antique.
         10. Glass Appearance: As selected by Architect.
      2. Glass Thickness: 1/2 inch (12.7 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Acid Etch.
         4. Glass Appearance: Low Iron Acid Etch.
         5. Glass Appearance: Clear Showergaurd.
         6. Glass Appearance: Low Iron Showergaurd.
         7. Glass Appearance: Antique.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: As selected by Architect.
      3. Glass Thickness: 3/4 inch (19 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Antique.
         4. Glass Appearance: As selected by Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Enduroshield on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete finishes not applicable.

* + - 1. Finish: Polished Nickel.
      2. Finish: Brushed Nickel.
      3. Finish: Plated. Polished Chrome.
      4. Finish: Plated.Brushed Chrome.
      5. Finish: Plated. Oil Rubbed Bronzed.
      6. Finish: Plated. Antique Brass.
      7. Finish: Plated. Polished Brass.
      8. Finish: Plated. Brushed Brass.
      9. Finish: Plated. Pewter.
      10. Finish: Plated. 24k Gold.
      11. Finish: Plated. Rose Gold.
      12. Finish: Plated. Plating color match; custom.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Solid brass piano hinge using frameless 1/4 inch glass. 0 to 1 inch adjustment available.

* + 1. Solid Brass Shower Doors:
       1. Model: Vintage 455 by American Shower Door.
       2. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete hinge type not applicable.

* + - 1. Hinge: Framed piano hinge. Regular.
      2. Hinge: Framed piano hinge. Steam.
      3. Hinge: Integrated self-centering pivots.
      4. Glass Thickness: 1/4 inch (6 mm).

\*\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Enduroshield on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete finish options not applicable.

* + - 1. Finish: Polished Nickel.
      2. Finish: Brushed Nickel.
      3. Finish: Plated. Polished Chrome.
      4. Finish: Plated.Brushed Chrome.
      5. Finish: Plated. Oil Rubbed Bronzed.
      6. Finish: Plated. Antique Brass.
      7. Finish: Plated. Polished Brass.
      8. Finish: Plated. Brushed Brass.
      9. Finish: Plated. Pewter.
      10. Finish: Plated. 24k Gold.
      11. Finish: Plated. Rose Gold.
      12. Finish: Plated. Plating color match; custom.
    1. Stainless Steel Shower Doors:
       1. Model: Stainless 304 by American Shower Door.

\*\* NOTE TO SPECIFIER \*\* Delete hinge type not applicable.

* + - 1. Hinge: Framed piano hinge. Regular.
      2. Hinge: Framed piano hinge. Steam.

\*\* NOTE TO SPECIFIER \*\* Delete glass size options not applicable.

* + - 1. Glass Dimensions: 84 inches (2134 mm) high by width indicated.
      2. Glass Dimensions: Size indicated on the Drawings.
      3. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete finishes not applicable.

* + - 1. Finish: Polished.
      2. Finish: Brushed.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required.

* 1. SHOWER ENCLOSURES

\*\* NOTE TO SPECIFIER \*\* Delete if not required. 15 percent more openings. Thru glass TB included.

* + 1. Frameless Aluminum Triple Sliding Shower Enclosures:
       1. Model: Elite-Plus 810 by American Shower Door.
       2. Operation: Tri-sliding door.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimension options not applicable.

* + - 1. Glass Dimensions: 60 inches (1524 mm) high by width indicated.
      2. Glass Dimensions: 72 inches (1829 mm) high by width indicated.
      3. Glass Dimensions: 76 inches (1930 mm) high by width indicated.
      4. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness option not applicable.

* + - 1. Glass Thickness: 3/16 inch (4.7 mm).
      2. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: BDS. Bright dip silver.
      2. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      3. Aluminum Finish: SN. Satin nickel anodized.
      4. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete finishes not applicable.

* + 1. Frameless Triple Sliding Aluminum Shower Enclosures with Panels:
       1. Model: Elite-Plus 2810 by American Shower Door.
       2. Description: Tri-slider with panels.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimensions options not applicable.

* + - 1. Glass Dimensions: 60 inches (1524 mm) high by width indicated.
      2. Glass Dimensions: 72 inches (1829 mm) high by width indicated.
      3. Glass Dimensions: 76 inches (1930 mm) high by width indicated.
      4. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness not applicable.

* + - 1. Glass Thickness: 3/16 inch (4.7 mm).
      2. Glass Thickness:1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: BDS. Bright dip silver.
      2. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      3. Aluminum Finish: SN. Satin nickel anodized.
      4. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Frameless with "S"- jambs.

* + 1. Frameless Sliding Aluminum Shower Enclosures:
       1. Model: Elite 806 by American Shower Door.

\*\* NOTE TO SPECIFIER \*\* Delete glass size options not applicable.

* + - 1. Glass Dimensions: 57 inches (1448 mm) high by width indicated.
      2. Glass Dimensions: 69 inches (1753 mm) high by width indicated.
      3. Glass Dimensions: 76 inches (1930 mm) high by width indicated.
      4. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness not applicable.

* + - 1. Glass Thickness: 3/16 inch (4.7 mm).
      2. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      4. Aluminum Finish: SN. Satin nickel anodized.
      5. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      6. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Add panels to the 806.

* + 1. Frameless Aluminum Sliding Shower Enclosures with Panels:
       1. Model: Elite-E 2806 by American Shower Door.

\*\* NOTE TO SPECIFIER \*\* Delete glass size options not applicable.

* + - 1. Glass Dimensions:57 inches (1448 mm) high by width indicated.
      2. Glass Dimensions: 69 inches (1753 mm) high by width indicated.
      3. Glass Dimensions: 76 inches (1930 mm) high by width indicated.
      4. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness not applicable.

* + - 1. Glass Thickness: 3/16 inch (4.7 mm).
      2. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      4. Aluminum Finish: SN. Satin nickel anodized.
      5. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      6. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Tradition master T extrusions.

* + 1. Framed Aluminum Sliding Shower Enclosures:
       1. Model: Classic 253 by American Shower Door.
       2. Rail Framing: 200 Rail.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimensions options not applicable.

* + - 1. Glass Dimensions: 58-1/2 inches (1486 mm) high by width indicated.
      2. Glass Dimensions: 70-1/2 inches (1791 mm) high by width indicated.
      3. Glass Dimensions: 76 inches (1930 mm) high by width indicated.
      4. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness not applicable.

* + - 1. Glass Thickness: 3/16 inch (4.7 mm).
      2. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. "Quick stall" panel system.

* + 1. Framed Aluminum Sliding Shower Enclosures with Panels:
       1. Model: Classic 2253 by American Shower Door.

\*\* NOTE TO SPECIFIER \*\* Delete glass size options not applicable.

* + - 1. Glass Dimensions: 58-1/2 inches (1486 mm) high by width indicated.
      2. Glass Dimensions: 70-1/2 inches (1791 mm) high by width indicated.
      3. Glass Dimensions: 76 inches (1930 mm) high by width indicated.
      4. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness not applicable.

* + - 1. Glass Thickness: 3/16 inch (4.7 mm).
      2. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Secondary, economical tub/shower for multi-unit applications.

* + 1. Framed Aluminum Sliding Shower Enclosures:
       1. Model: Starlite 703 by American Shower Door.
       2. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete size options not applicable.

* + - 1. Glass Dimensions: 57-3/4 inches (1467 mm) high by width indicated.
      2. Glass Dimensions: 69-3/4 inches (1772 mm) high by width indicated.
      3. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness not applicable.

* + - 1. Glass Thickness: 3/16 inch (4.7 mm).
      2. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      4. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Secondary, economical tub/shower for multi-unit applications.

* + 1. Framed Aluminum Steam Sliding Shower Enclosures:
       1. Model: Tropic 272 by American Shower Door.
       2. Operation: Slider.

\*\* NOTE TO SPECIFIER \*\* Delete size options not applicable.

* + - 1. Glass Dimensions: 76 inches (1930 mm) high to 96 inches (2438 mm) high (with transom) by width indicated.
      2. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness not applicable.

* + - 1. Glass Thickness: 3/16 inch (4.7 mm).
      2. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure.
      3. Glass Appearance: As selected.

\*\* NOTE TO SPECIFIER \*\* Delete option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: BDS. Bright dip silver.
      2. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      3. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      4. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Frameless aluminum "euro" slider compatible with 3/8 inch (9.5 mm) and 1/2 inch (12.7 mm) glass.

* + 1. Crystal Collection Frameless Aluminum Sliding Shower Enclosures:
       1. Model: Crystal 851 by American Shower Door.
       2. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness and glass appearance options not applicable.

* + - 1. Glass Thickness: 3/8 inch (9.5 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Rain.
         4. Glass Appearance: Bubbles.
         5. Glass Appearance: Acid Etch.
         6. Glass Appearance: Low Iron Acid Etch.
         7. Glass Appearance: Clear Showergaurd.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: Antique.
         10. Glass Appearance: As selected by the Architect.
      2. Glass Thickness: 1/2 inch (12.7 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Acid Etch.
         4. Glass Appearance: Low Iron Acid Etch.
         5. Glass Appearance: Clear Showergaurd.
         6. Glass Appearance: Low Iron Showergaurd.
         7. Glass Appearance: Antique.
         8. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Additional panels for Crystal 853.

* + 1. Crystal Collection Frameless Aluminum Sliding Shower Enclosures with Panels:
       1. Model: Crystal 2853 by American Shower Door.
       2. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness and glass appearance options not applicable.

* + - 1. Glass Thickness: 3/8 inch (9.5 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Rain.
         4. Glass Appearance: Bubbles.
         5. Glass Appearance: Acid Etch.
         6. Glass Appearance: Low Iron Acid Etch.
         7. Glass Appearance: Clear Showergaurd.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: Antique.
         10. Glass Appearance: As selected by the Architect.
      2. Glass Thickness: 1/2 inch (12.7 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Acid Etch.
         4. Glass Appearance: Low Iron Acid Etch.
         5. Glass Appearance: Clear Showergaurd.
         6. Glass Appearance: Low Iron Showergaurd.
         7. Glass Appearance: Antique.
         8. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      4. Aluminum Finish: SN. Satin nickel anodized.
      5. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      6. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Solid Brass, custom plated.

* + 1. Crystal Collection Heavy Glass Frameless Brass Shower Enclosures:
       1. Model: Crystal 953 by American Shower Door.
       2. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness and glass appearance options not applicable.

* + - 1. Glass Thickness: 3/8 inch (9.5 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Rain.
         4. Glass Appearance: Bubbles.
         5. Glass Appearance: Acid Etch.
         6. Glass Appearance: Low Iron Acid Etch.
         7. Glass Appearance: Clear Showergaurd.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: Antique.
         10. Glass Appearance: As selected by the Architect.
      2. Glass Thickness: 1/2 inch (12.7 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Acid Etch.
         4. Glass Appearance: Low Iron Acid Etch.
         5. Glass Appearance: Clear Showergaurd.
         6. Glass Appearance: Low Iron Showergaurd.
         7. Glass Appearance: Antique.
         8. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Enduroshield on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete finish options not applicable.

* + - 1. Finish: Polished Nickel.
      2. Finish: Brushed Nickel.
      3. Finish: Plated. Polished Chrome.
      4. Finish: Plated.Brushed Chrome.
      5. Finish: Plated. Oil Rubbed Bronzed.
      6. Finish: Plated. Antique Brass.
      7. Finish: Plated. Polished Brass.
      8. Finish: Plated. Brushed Brass.
      9. Finish: Plated. Pewter.
      10. Finish: Plated. 24k Gold.
      11. Finish: Plated. Rose Gold.
      12. Finish: Plated. Plating color match; custom.
    1. Crystal Collection Frameless Brass Sliding Shower Enclosures with Panels:
       1. Model: Crystal 2953 by American Shower Door.
       2. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness and glass appearance options not applicable.

* + - 1. Glass Thickness: 3/8 inch (9.5 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Rain.
         4. Glass Appearance: Bubbles.
         5. Glass Appearance: Acid Etch.
         6. Glass Appearance: Low Iron Acid Etch.
         7. Glass Appearance: Clear Showergaurd.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: Antique.
         10. Glass Appearance: As selected by the Architect.
      2. Glass Thickness: 1/2 inch (12.7 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Acid Etch.
         4. Glass Appearance: Low Iron Acid Etch.
         5. Glass Appearance: Clear Showergaurd.
         6. Glass Appearance: Low Iron Showergaurd.
         7. Glass Appearance: Antique.
         8. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian.

\*\* NOTE TO SPECIFIER \*\* Delete finish options not applicable.

* + - 1. Finish: Polished Nickel.
      2. Finish: Brushed Nickel.
      3. Finish: Plated. Polished Chrome.
      4. Finish: Plated.Brushed Chrome.
      5. Finish: Plated. Oil Rubbed Bronzed.
      6. Finish: Plated. Antique Brass.
      7. Finish: Plated. Polished Brass.
      8. Finish: Plated. Brushed Brass.
      9. Finish: Plated. Pewter.
      10. Finish: Plated. 24k Gold.
      11. Finish: Plated. Rose Gold.
      12. Finish: Plated. Plating color match; custom.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. 15 percent wider openings; may add panels.

* + 1. Crystal Collection Frameless Three Panel Aluminum Sliding Shower Enclosures:
       1. Model: Crystal 838 by American Shower Door.
       2. Glass Dimensions: Size indicated on the Drawings.
       3. Operation: Tri-slider.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness and glass appearance options not applicable.

* + - 1. Glass Thickness: 3/8 inch (9.5 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Rain.
         4. Glass Appearance: Bubbles.
         5. Glass Appearance: Acid Etch.
         6. Glass Appearance: Low Iron Acid Etch.
         7. Glass Appearance: Clear Showergaurd.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: Antique.
         10. Glass Appearance: As selected by the Architect.
      2. Glass Thickness: 1/2 inch (12.7 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Acid Etch.
         4. Glass Appearance: Low Iron Acid Etch.
         5. Glass Appearance: Clear Showergaurd.
         6. Glass Appearance: Low Iron Showergaurd.
         7. Glass Appearance: Antique.
         8. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: BDS. Bright dip silver.
      2. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      3. Aluminum Finish: SN. Satin nickel anodized.
      4. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.
  1. SHOWER DOORS AND PANELS

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Accommodates standard or large frameless doors and panels.

* + 1. Semi-Frameless Aluminum Doors with Panels:
       1. Model: Elite-D 5020 by American Shower Door.
       2. Door Hinge: Piano hinge.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimension options not applicable.

* + - 1. Glass Dimensions: 72 inches (1829 mm) high by width indicated.
      2. Glass Dimensions: 84 inches (2134 mm) high by width indicated.
      3. Glass Dimensions: Size indicated on the Drawings.
      4. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Pivot door with narrow rails for frameless panels.

* + 1. Framed Aluminum Daylites with Panels:
       1. Model: Limited-D 2100 by American Shower Door.
       2. Door Hinge: Pivot.
       3. Rail Framing: 200 Rail.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimension options not applicable.

* + - 1. Glass Dimensions: 72 inches (1829 mm) high by width indicated.
      2. Glass Dimensions: 74 inches (1880 mm) high by width indicated.
      3. Glass Dimensions: Size indicated on the Drawings.
      4. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      4. Aluminum Finish: SN. Satin nickel anodized.
      5. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      6. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Piano hinged door with frameless panels.

* + 1. Framed Aluminum Doors and Panels:
       1. Model: Classic-D 5100 by American Shower Door.
       2. Rail Framing: 200 Rail.

\*\* NOTE TO SPECIFIER \*\* Delete door hinge type not applicable.

* + - 1. Door Hinge: Pivot - regular.
      2. Door Hinge: Pivot - steam.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimensions options not applicable.

* + - 1. Glass Dimensions: 72 inches (1829 mm) high by width indicated.
      2. Glass Dimensions: 84 inches (2134 mm) high by width indicated.
      3. Glass Dimensions: Size indicated on the Drawings.
      4. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on others.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      4. Aluminum Finish: SN. Satin nickel anodized.
      5. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      6. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Maximum strength 335 rail door and frameless panels for larger spaces.

* + 1. Framed Aluminum Heavy Duty Doors with Panels:
       1. Model:Max-D 3100 by American Shower Door.
       2. Rail Framing: 355 Rail.

\*\* NOTE TO SPECIFIER \*\* Delete hinge type not applicable.

* + - 1. Door Hinge: Piano - heavy duty.
      2. Door Hinge: Piano - steam, heavy duty.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimensions options not applicable.

* + - 1. Glass Dimensions: 96 inches (2438 mm) high by width indicated.
      2. Glass Dimensions: Size indicated on the Drawings.
      3. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      4. Aluminum Finish: SN. Satin nickel anodized.
      5. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      6. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Accommodates standard or large framed doors and panels.

* + 1. Framed Aluminum Doors and Framed Panels:
       1. Model: Classic-D 100 by American Shower Door.
       2. Rail Framing: 200 Rail.

\*\* NOTE TO SPECIFIER \*\* Delete panel option not applicable.

* + - 1. Panels: Regular.
      2. Panels: Steam.
      3. Hinge: Piano.

\*\* NOTE TO SPECIFIER \*\* Delete transoms option not required.

* + - 1. Transoms: Operable.
      2. Transoms: Fixed.

\*\* NOTE TO SPECIFIER \*\* Delete glass dimensions options not applicable.

* + - 1. Glass Dimensions: 69-15/16 inches (1776 mm) high by width indicated.
      2. Glass Dimensions: 84 inches (2134 mm) high by width indicated.
      3. Glass Dimensions: Size indicated on the Drawings.
      4. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on others glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      4. Aluminum Finish: SN. Satin nickel anodized.
      5. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      6. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Heavy frameless glass with brass hardware and aluminum extrusions.

* + 1. Crystal Collection Doors and Panels:
       1. Model: Crystal 8000 by American Shower Door.
       2. Hardware: Brass.
       3. Extrusions: Aluminum.

\*\* NOTE TO SPECIFIER \*\* Delete hinge type options not applicable.

* + - 1. Hinge Type: Pivots.
      2. Hinge Type: Wall to glass.
      3. Hinge Type: Glass to glass.
      4. Hinge Type: Custom. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete fixed panel options not required.

* + - 1. Fixed Panel: Channel.
      2. Fixed Panel: Clips.
      3. Door Pulls: At 2 inch (52 mm) increments from 6 to 30 inches (152 to 762 mm).

\*\* NOTE TO SPECIFIER \*\* Delete transom option not required.

* + - 1. Transoms: Operable.
      2. Transoms: Fixed.

\*\* NOTE TO SPECIFIER \*\* 40 lb capacity per hinge.

* + - 1. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness and glass appearance options not applicable.

* + - 1. Glass Thickness: 3/8 inch (9.5 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Rain.
         4. Glass Appearance: Bubbles.
         5. Glass Appearance: Acid Etch.
         6. Glass Appearance: Low Iron Acid Etch.
         7. Glass Appearance: Clear Showergaurd.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: Antique.
         10. Glass Appearance: As selected by Architect.
      2. Glass Thickness: 1/2 inch (12.7 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Acid Etch.
         4. Glass Appearance: Low Iron Acid Etch.
         5. Glass Appearance: Clear Showergaurd.
         6. Glass Appearance: Low Iron Showergaurd.
         7. Glass Appearance: Antique.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: As selected by Architect.
      3. Glass Thickness: 3/4 inch (19 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Antique.
         4. Glass Appearance: As selected by Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.
    1. Crystal Collection Doors and Panels:
       1. Model: Crystal 9000 by American Shower Door.
       2. Hardware: Brass.
       3. Extrusions: Brass.

\*\* NOTE TO SPECIFIER \*\* Delete hinge type options not applicable.

* + - 1. Hinge Type: Pivots.
      2. Hinge Type: Wall to glass.
      3. Hinge Type: Glass to glass.
      4. Hinge Type: Custom. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete fixed panel options not required.

* + - 1. Fixed Panel: Channel.
      2. Fixed Panel: Clips.
      3. Door Pulls: At 2 inch (52 mm) increments from 6 to 30 inches (152 to 762 mm).

\*\* NOTE TO SPECIFIER \*\* Delete transom option not required.

* + - 1. Transoms: Operable.
      2. Transoms: Fixed.

\*\* NOTE TO SPECIFIER \*\* 40 lb capacity per hinge.

* + - 1. Glass Dimensions: Size indicated on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness and glass appearance options not applicable.

* + - 1. Glass Thickness: 3/8 inch (9.5 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Rain.
         4. Glass Appearance: Bubbles.
         5. Glass Appearance: Acid Etch.
         6. Glass Appearance: Low Iron Acid Etch.
         7. Glass Appearance: Clear Showergaurd.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: Antique.
         10. Glass Appearance: As selected by Architect.
      2. Glass Thickness: 1/2 inch (12.7 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Acid Etch.
         4. Glass Appearance: Low Iron Acid Etch.
         5. Glass Appearance: Clear Showergaurd.
         6. Glass Appearance: Low Iron Showergaurd.
         7. Glass Appearance: Antique.
         8. Glass Appearance: Low Iron Showergaurd.
         9. Glass Appearance: As selected by Architect.
      3. Glass Thickness: 3/4 inch (19 mm).
         1. Glass Appearance: Clear.
         2. Glass Appearance: Low Iron.
         3. Glass Appearance: Antique.
         4. Glass Appearance: As selected by Architect.

\*\* NOTE TO SPECIFIER \*\* Delete option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Endurosheild on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete finish options not applicable.

* + - 1. Finish: Polished Nickel.
      2. Finish: Brushed Nickel.
      3. Finish: Plated. Polished Chrome.
      4. Finish: Plated. Brushed Chrome.
      5. Finish: Plated. Oil Rubbed Bronzed.
      6. Finish: Plated. Antique Brass.
      7. Finish: Plated. Polished Brass.
      8. Finish: Plated. Brushed Brass.
      9. Finish: Plated. Pewter.
      10. Finish: Plated. 24k Gold.
      11. Finish: Plated. Rose Gold.
      12. Finish: Plated. Plating color match; custom.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Brass 1/4 inch frameless door with contemporary frameless panels.

* + 1. Solid Brass Framed Door and Framed Panels:
       1. Model: Vintage-D 4550 by American Shower Door.
       2. Glass Dimensions: Size indicated on the Drawings.
       3. Panels: Framed.

\*\* NOTE TO SPECIFIER \*\* Delete hinge options not required.

* + - 1. Hinge: Framed piano hinge. Regular.
      2. Hinge: Framed piano hinge. Steam.
      3. Hinge: Integrated self-centering pivots.

\*\* NOTE TO SPECIFIER \*\* Delete transoms options not required.

* + - 1. Transoms: Operable.
      2. Transoms: Fixed.
      3. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Enduroshield on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete finish options not applicable.

* + - 1. Finish: Polished Nickel.
      2. Finish: Brushed Nickel.
      3. Finish: Plated. Polished Chrome.
      4. Finish: Plated. Brushed Chrome.
      5. Finish: Plated. Oil Rubbed Bronzed.
      6. Finish: Plated. Antique Brass.
      7. Finish: Plated. Polished Brass.
      8. Finish: Plated. Brushed Brass.
      9. Finish: Plated. Pewter.
      10. Finish: Plated. 24k Gold.
      11. Finish: Plated. Rose Gold.
      12. Finish: Plated. Plating color match; custom.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Framed door with contemporary frameless panels.

* + 1. Solid Brass Framed Door with Frameless Panels:
       1. Model: Vintage-D 4551 by American Shower Door.
       2. Glass Dimensions: Size indicated on the Drawings.
       3. Panels: Frameless.

\*\* NOTE TO SPECIFIER \*\* Delete hinge type not applicable.

* + - 1. Hinge Type: Framed piano hinge - regular.
      2. Hinge Type: Framed piano hinge - steam.
      3. Hinge Type: Integrated self-centering pivots.

\*\* NOTE TO SPECIFIER \*\* Delete transoms options not required.

* + - 1. Transoms: Operable.
      2. Transoms: Fixed.
      3. Glass Thickness: 1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure (P516).
      3. Glass Appearance: Rain.
      4. Glass Appearance: Low Iron.
      5. Glass Appearance: Acid Etch.
      6. Glass Appearance: Low Iron Acid Etch.
      7. Glass Appearance: Reed.
      8. Glass Appearance: Ribbed.
      9. Glass Appearance: Antique.
      10. Glass Appearance: Clear Showergaurd.
      11. Glass Appearance: As selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Delete option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian or Enduroshield on other glass.

\*\* NOTE TO SPECIFIER \*\* Delete finish options not applicable.

* + - 1. Finish: Polished Nickel.
      2. Finish: Brushed Nickel.
      3. Finish: Plated. Polished Chrome.
      4. Finish: Plated. Brushed Chrome.
      5. Finish: Plated. Oil Rubbed Bronzed.
      6. Finish: Plated. Antique Brass.
      7. Finish: Plated. Polished Brass.
      8. Finish: Plated. Brushed Brass.
      9. Finish: Plated. Pewter.
      10. Finish: Plated. 24k Gold.
      11. Finish: Plated. Rose Gold.
      12. Finish: Plated. Plating color match; custom.
    1. Stainless Steel Framed Doors and Panels:
       1. Model: No. 304 by American Shower Door.
       2. Glass Dimensions: Size indicated on the Drawings.
       3. Panels: Frameless.

\*\* NOTE TO SPECIFIER \*\* Delete hinge option not applicable.

* + - 1. Hinge: Regular.
      2. Hinge: Steam.

\*\* NOTE TO SPECIFIER \*\* Delete glass thickness option not applicable.

* + - 1. Glass Thickness: 3/16 inch (4.7 mm).
      2. Glass Thickness:1/4 inch (6 mm).

\*\* NOTE TO SPECIFIER \*\* Delete glass appearance options not applicable.

* + - 1. Glass Appearance: Clear.
      2. Glass Appearance: Obscure.
      3. Glass Appearance: As selected.

\*\* NOTE TO SPECIFIER \*\* Delete glass coating option below if not applicable.

* + - 1. Glass Coating: Corrosion-resistant glass coating, ShowerGuard by Guardian.

\*\* NOTE TO SPECIFIER \*\* Delete stainless steel finishes not applicable.

* + - 1. Stainless Steel Finish: Polished.
      2. Stainless Steel Finish: Plated.
      3. Stainless Steel Finish: Powder coated. Color as selected by Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required.

* 1. SPECIALTY ITEMS

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Easy to install, snap-in for panels. Cut to size and custom plated to specifications.

* + 1. Snap-In Extrusions:

\*\* NOTE TO SPECIFIER \*\* Delete model option not applicable.

* + - 1. Model: FB 272 by American Shower Door.
      2. Model: FC 272 by American Shower Door.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      4. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Cut to size and custom plated to specifications.

* + 1. Solid Brass Extrusions:
       1. Model: Brass extrusions by American Shower Door.

\*\* NOTE TO SPECIFIER \*\* Delete finishes not applicable.

* + - 1. Finish: Polished.
      2. Finish: Plated.
      3. Finish: Powder coated. Color as selected by Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Cut to size and custom plated to specifications.

* + 1. Aluminum Extrusions:
       1. Model: Aluminum extrusions by American Shower Door.

\*\* NOTE TO SPECIFIER \*\* Delete aluminum finish options not applicable.

* + - 1. Aluminum Finish: SS. Satin silver.
      2. Aluminum Finish: BDS. Bright dip silver.
      3. Aluminum Finish: BBDS. Brushed bright dip silver.
      4. Aluminum Finish: PC. Powder coat. As selected by the Architect or as detailed on the Drawings.
      5. Aluminum Finish: SN. Satin nickel anodized.
      6. Aluminum Finish: Custom anodized. As selected by the Architect or as detailed on the Drawings.
      7. Aluminum Finish: Custom powder coat. As selected by the Architect or as detailed on the Drawings.

\*\* NOTE TO SPECIFIER \*\* Delete if not required. Hinges, handles and parts for all lines.

* + 1. Hardware:

\*\* NOTE TO SPECIFIER \*\* Delete product lines not applicable.

* + - 1. Product Line: Concerto hardware by American Shower Door.
      2. Product Line: Symphony hardware by American Shower Door.
      3. Product Line: Wood hardware by American Shower Door.
      4. Product Line: Counterpoint hardware by American Shower Door.
      5. Product Line: C-Pull Collection hardware by American Shower Door.

\*\* NOTE TO SPECIFIER \*\* Delete materials not applicable.

* + - 1. Material: Aluminum.
      2. Material: Brass.
      3. Material: Crystal.
      4. Material: Wood.
      5. Material: Stainless steel.

\*\* NOTE TO SPECIFIER \*\* Delete finishes not applicable.

* + - 1. Finish: SS - Satin silver.
      2. Finish: BDS - Bright dip silver.
      3. Finish: BBDS - Brushed bright dip silver.
      4. Finish: PC - Powder coat.
      5. Finish: SNA - Satin nickel anodized.
      6. Finish: Custom anodized finish.
      7. Finish: Custom powder coat finish.
      8. Finish: Polished Nickel.
      9. Finish: Brushed Nickel.
      10. Finish: Polished Chrome.
      11. Finish: Brushed Chrome.
      12. Finish: Plated. Oil Rubbed Bronzed.
      13. Finish: Plated. Antique Brass.
      14. Finish: Plated. Polished Brass.
      15. Finish: Plated. Brushed Brass.
      16. Finish: Plated. Pewter.
      17. Finish: Plated. 24k Gold.
      18. Finish: Plated. Rose Gold.
      19. Finish: Plated. Plating color match; custom.

1. EXECUTION
   1. EXAMINATION
      1. Do not proceed with Work until surfaces and conditions comply with requirements in manufacturer's printed instructions.
   2. INSTALLATION
      1. Installation: Comply with manufacturer's written installation instructions.
         1. Install securely and in proper relationship with adjacent construction.
         2. Install straight and plumb.
         3. Test and adjust for proper operation.
      2. Protection and Cleaning:
         1. Protect installed materials from damage from construction operations.
         2. Repair or replace damaged units.
         3. Clean just prior to Substantial Completion.

END OF SECTION