SECTION 10 31 00

MANUFACTURED FIREPLACES

Display hidden notes to specifier. (Don't know how? [Click Here](https://www.arcat.com/sd/display_hidden_notes.shtml))

*Copyright 2014 - 2021 ARCAT, Inc. - All rights reserved*

\*\* NOTE TO SPECIFIER \*\* Napoleon Fireplaces; Manufactured fireplace products.  
This section is based on the products of Napoleon Fireplaces, which is located at:  
Wolf Steel USA 103 Miller Dr.  
Crittenden, KY 41030  
Toll Free Tel: 800-461-5581   
Email: [request info (jspray@napoleonproducts.com)](https://admin.arcat.com/users.pl?action=UserEmail&company=Napoleon+Fireplaces&coid=45452&rep=&fax=&message=RE:%20Spec%20Question%20(10305nap):%20%20&mf=)  
Web: <https://www.napoleon.com/en/us/fireplaces>   
 [ [Click Here](https://www.arcat.com/arcatcos/cos45/arc45452.html) ] for additional information.  
Napoleon Fireplaces is proud to be committed to your total home comfort. Time after time, Napoleon has led the way with new and innovative, patented technology. We are proud to say that our products continuously surpass industry standards, and our inspiration is you! More than anything we want you to feel confident in choosing Napoleon® for your home. Our products are designed to provide that confidence and ensure that every Napoleon® Product is beyond compare.  
It all began in 1976 when a small steel fabrication business launched by Wolfgang Schroeter started manufacturing steel railings in Barrie, Ontario, Canada. By 1981, the name "Napoleon" was born and, with it, the first single glass door (a first in the industry) using Pyroceram high temperature ceramic glass and a cast iron frame. This was the first of many milestones for Wolf Steel and over the next few years, the demand for Napoleon's wood stoves grew beyond Ontario's borders to the rest of Canada and the United States. Napoleon works with its customers designing and implementing features sought after by discriminating consumers around the globe.  
Time after time Wolf Steel has led the way with new and innovative patented technology: exclusive PHAZER® logs, luxurious Napoleon Gas Grills and some of North America's most advanced state-of-the-art fireplace technology. Innovative engineering and design, advanced manufacturing techniques, dedicated customer service, outstanding product quality, and superior warranties distinguish Napoleon® from its competitors.  
Napoleon® is an ISO9001 - 2008 registered company and operates with 1,200,000+ square feet of manufacturing space and over 1000 employees. We are North America's largest privately owned manufacturer of quality wood and gas fireplaces (inserts and stoves), gourmet gas and charcoal grills, outdoor living products and heating & cooling products. The only gas furnaces made in Canada.  
Napoleon's commitment to producing quality products combined with honest, reliable service has proven to be a successful framework to ensuring the continued rapid growth of the company.

1. GENERAL
   1. SECTION INCLUDES

\*\* NOTE TO SPECIFIER \*\* Delete items below not required for project.

* + 1. Gas Burning Indoor Vent Free Fireplaces.
    2. Gas Burning Indoor Direct Vent Fireplaces.
    3. Gas burning linear indoor direct vent fireplaces.
    4. Electric indoor fireplaces.
    5. Wood burning indoor fireplaces.
    6. Gas burning stoves.
    7. Wood burning stoves.
    8. Gas burning fireplace inserts.
    9. Gas burning log sets.
    10. Wood burning fireplace inserts.
    11. Electric log sets.
    12. Wood burning fireplace inserts.
    13. Gas burning outdoor fireplaces.
  1. RELATED SECTIONS

\*\* NOTE TO SPECIFIER \*\* Delete any sections below not relevant to this project; add others as required.

* + 1. Section 04 27 23 - Cavity Wall Unit Masonry.
    2. Section 06 10 00 - Rough Carpentry.
    3. Section 09 28 13 - Cementitious Backing Boards.
    4. Section 22 11 13 - Facility Water Distribution Piping.
    5. Section 26 05 00 - Common Work Results for Electrical
  1. REFERENCES

\*\* NOTE TO SPECIFIER \*\* Delete references from the list below that are not actually required by the text of the edited section.

* + 1. ANSI Z21.44 - Gas-Fired Gravity and Fan Type Direct Vent Wall Furnaces.
    2. ANSI Z21.88 - Vented Gas Fireplace Heaters.
    3. UL 127 - Standard for Factory-Built Fireplaces.
    4. NFPA - 70 - National Electric Code.
    5. NFPA 54 - National Fuel Gas Code.
    6. CSA B149.1 - Natural Gas and Propane Installation Code.
    7. CSA B149.2 - Propane Storage and Handling Code.
    8. CSA C22.1 - Canadian Electrical Code.
    9. CSA 2.33 - Vented Gas Fireplace Heaters.
    10. CAN/ULC S610 - Factory-Built Fireplaces.
  1. SUBMITTALS
     1. Submit under provisions of Section 01 30 00 - Administrative Requirements.
     2. Product Data: Manufacturer's data sheets on each product to be used, including:
        1. Preparation instructions and recommendations.
        2. Storage and handling requirements and recommendations.
        3. Installation methods. Including:
           1. Fireplace unit rough opening dimensions, rough opening sizes for flue, and installation details.
           2. Fireplace unit cabinet dimensions, clearances required from adjacent construction, and applicable regulatory agency approvals

\*\* NOTE TO SPECIFIER \*\* Delete the following paragraphs if LEED is not applicable.

* + 1. LEED Submittals: Provide documentation of how the requirements of Credit will be met:
       1. Product Data for Credit MR 2.1 and 2.2: For products being recycled, documentation of total weight of project waste diverted from landfill.
       2. Product Data for Credit MR 4.1 and MR 4.2: For products that have recycled content, documentation including percentages by weight of post-consumer and preconsumer recycled content
          1. Include statement indicating costs for each product having recycled content.
       3. Product Data for Credit MR 5.1 and Credit MR 5.2: Submit data, including location and distance from Project of material manufacturer and point of extraction, harvest or recovery for main raw material.
          1. Include statement indicating cost for each regional material and the fraction by weight that is considered regional.
    2. Manufacturer's Certificates: Certify products meet or exceed specified requirements.
    3. Closeout Submittals: Provide manufacturer's maintenance instructions that include recommendations for periodic checking and adjustment and periodic cleaning and maintenance of all components.
  1. QUALITY ASSURANCE
     1. Manufacturer Qualifications: Manufacturer with a minimum of 10 years documented experience with the types of products specified.
     2. Installer Qualifications: Installer with a minimum 5 years documented experience with the type of products specified and approved by the manufacturer or Certified by the National Fireplace Institute.

\*\* NOTE TO SPECIFIER \*\* Include a mock-up if the project size and/or quality warrant taking such a precaution. The following is one example of how a mock-up on a large project might be specified. When deciding on the extent of the mock-up, consider all the major different types of work on the project.

* + 1. Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
       1. Finish areas designated by Architect.
       2. Do not proceed with remaining work until workmanship, color, and finishes are approved by Architect.
       3. Refinish mock-up area as required to produce acceptable work.
  1. DELIVERY, STORAGE, AND HANDLING
     1. Store products in manufacturer's unopened packaging until ready for installation.
     2. Store products in covered area, well protected from weather.
  2. SEQUENCING
     1. Ensure that locating templates and other information required for installation of products of this section are furnished to affected trades in time to prevent interruption of construction progress.
     2. Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
  3. PROJECT CONDITIONS
     1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
  4. WARRANTY

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs for indoor or outdoor fireplaces and delete the one not required.

* + 1. Provide manufacturer's limited lifetime warranty covering combustion chamber heat exchanger, stainless steel burner, logs, ceramic glass against thermal breakage, gold plated parts against tarnishing, porcelain enameled surfaces and aluminum extrusion trim.
    2. Provide manufacturer's limited 5 year warranty covering outdoor fireplace combustion chamber heat exchanger, stainless steel burner, logs, ceramic glass against thermal breakage, gold plated parts against tarnishing, porcelain enameled surfaces and aluminum extrusion trim.

1. PRODUCTS
   1. MANUFACTURERS
      1. Acceptable Manufacturer: Napoleon Fireplaces, which is located at: Wolf Steel USA 103 Miller Dr.; Crittenden, KY 41030; Toll Free Tel: 800-461-5581 ; Email: [request info (jspray@napoleonproducts.com)](https://admin.arcat.com/users.pl?action=UserEmail&company=Napoleon+Fireplaces&coid=45452&rep=&fax=&message=RE:%20Spec%20Question%20(10305nap):%20%20&mf=); Web: <https://www.napoleon.com/en/us/fireplaces>

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions.

* + 1. Substitutions: Not permitted.
    2. Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.

\*\* NOTE TO SPECIFIER \*\* Select from the wood burning, gas burning or electric manufactured fireplaces below. Select the units required and delete those not required. If more than one unit is required clearly indicate locations on the Drawings. Consult manufacturers literature for product options and features. Delete article below if not required.

* 1. GAS BURNING INDOOR VENT FREE FIREPLACES - GRANDVILLE SERIES
     1. Comply with applicable building codes.

\*\* NOTE TO SPECIFIER \*\* Delete model not required. Vent Free units are not approved in Canada and some states. Contact manufacturer for additional information.

* + 1. Model: Grandville GVF36 Series. Type: Vent free. BTU: 30,000.

\*\* NOTE TO SPECIFIER \*\* Delete fuel type not required.

* + - 1. Fuel Type: Natural gas.
      2. Fuel Type: Propane.
      3. Dimensions (WxHxD): 27.38 x 35.50 x 13.25 inches (695 x 902 x 337 mm).
      4. Features:
         1. Safety screen.
         2. Fireplace screen.
         3. Flame and Heat Adjustment: 50 percent.
         4. SAFEGUARD Gas Control System: 100 percent.
         5. Oxygen depletion sensor (ODS).
         6. Pre-wired for wall switch.
         7. Millivolt wall thermostat.
         8. Battery back-up control system.
         9. Media Kit: PHAZER log set.
         10. YELLOW DANCING FLAMES.

\*\* NOTE TO SPECIFIER \*\* Delete options below not required.

* + - * 1. Remote control.
        2. Finish: Metallic black.
        3. Finish: Porcelain enamel majolica brown.
        4. Ornamental Insets. Brushed stainless steel.
        5. Ornamental Insets. Antique brass.
        6. Ornamental Insets. Painted black.
        7. Louvers: Finish brushed stainless steel.
        8. Louvers: Finish antique brass.
        9. Louvers: Finish painted black.
        10. Trim 3 inch: Finish brushed stainless steel.
        11. Trim 3 inch: Finish textured painted black.
        12. Trim 6 inch: Finish brushed stainless steel.
        13. Trim 6 inch: Finish textured painted black.
        14. Surrounds: Cast Iron. Painted black.
        15. Decorative Panels: MIRRO-FLAME porcelain reflective radiant panels.
        16. Decorative Panels: Sandstone brick.
        17. Decorative Panels: Slate brick.
        18. Laval rick cinders.
        19. Andirons. Painted black.
        20. Trivets: Cast iron.
        21. Heat circulating blower kit.
        22. On/off or modulating remote with digital screen.
    1. Model: Grandville GVF42 Series. Type: Vent free. BTU: 30,000.

\*\* NOTE TO SPECIFIER \*\* Delete fuel type not required.

* + - 1. Fuel Type: Natural gas.
      2. Fuel Type: Propane.
      3. Dimensions (WxHxD): 42 x 38.50 x 22 inches (1067 x 978 x 559 mm)
      4. Features:
         1. Safety screen.
         2. Fireplace screen.
         3. Flame and Heat Adjustment: 50 percent.
         4. SAFEGUARD Gas Control System: 100 percent.
         5. Oxygen depletion sensor (ODS).
         6. Pre-wired for wall switch.
         7. Battery back-up control system.

\*\* NOTE TO SPECIFIER \*\* Delete options below not required.

* + - * 1. Remote control.
        2. Millivolt wall thermostat.
        3. Louvers: Finish brushed stainless steel.
        4. Louvers: Finish painted black.
        5. Decorative Panels: MIRRO-FLAME porcelain reflective radiant panels.
        6. Decorative Panels: Sandstone brick.
        7. Andirons. Painted black.
        8. Heat circulating blower kit.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required.

* 1. GAS BURNING INDOOR DIRECT VENT FIREPLACES - VITTORIA SERIES
     1. Comply with applicable building codes.
        1. Comply with ANSI Z21.88/CSA 2.33. WHI listed.
        2. Safety Barriers are "Safety Barrier Approved."
     2. Model: Vittoria GD19. Direct Vent Gas Fireplace. BTU: 11,500.
        1. Dimensions (WxHxD): 21.50 x 34.12 x 13 inches (546 x 867 x 330 mm).
        2. Viewing Area: 16.63 x 24 inches (422 x 610 mm).

\*\* NOTE TO SPECIFIER \*\* Delete fuel type not required.

* + - 1. Fuel type: Natural gas.
      2. Fuel type: Propane. Provided with conversion kit.
      3. Features:
         1. Accent lights.
         2. Night light.
         3. Safety barrier.
         4. Electronic ignition.
         5. Heat radiating ceramic glass.
         6. Back-up control system.
         7. SAFEGUARD gas control system. 100 percent.

\*\* NOTE TO SPECIFIER \*\* Delete the following items not required.

* + - * 1. Remote control.
        2. Room Settings: Transitional.
        3. Room Settings: Contemporary.
        4. Room Settings: Traditional.
        5. Room Settings: Rustic.
        6. Decorative Panels: MIRRO-FLAME porcelain reflective radiant panels.
        7. Decorative Panels: Sandstone.
        8. Media Kit: PHAZER log set.
        9. Media Kit: River rock stone set.
        10. Surrounds: Traditional metallic black.
        11. Surrounds: Contemporary black.
        12. Decorative Fronts: Traditional black.
        13. Decorative Fronts: Contemporary stainless.
        14. Decorative Fronts: Contemporary black.
        15. Ornamental Insets: Brushed stainless Victorian.
        16. Ornamental Insets: Black Victorian.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required.

* 1. GAS BURNING INDOOR DIRECT VENT FIREPLACES - PARK AVENUE SERIES
     1. Comply with applicable building codes.
        1. Comply with ANSI Z21.88/CSA 2.33. WHI listed.
        2. Safety Barriers are "Safety Barrier Approved."
     2. Model: Park Avenue GD82NT-PAESB. Direct Vent Gas Fireplace. BTU: 26,000.
        1. Dimensions (WxHxD): 28 x 58 x 22.13 inches (711 x 1473 x 562 mm).
        2. Viewing Area: 22 x 29 inches (559 x 737 mm).

\*\* NOTE TO SPECIFIER \*\* Delete fuel type not required.

* + - 1. Fuel type: Natural gas.
      2. Fuel type: Propane. Provided with conversion kit.
      3. Features:
         1. Accent lights.
         2. Hearth Pad: Brushed stainless steel.
         3. Media Kit: PHAZER log set.
         4. Andirons: Painted black.
         5. Safety Barrier: Black.
         6. Back-up control system.
         7. SAFEGUARD gas control system: 100 percent.
         8. Remote control.

\*\* NOTE TO SPECIFIER \*\* Delete the following items not required.

* + - * 1. Room Settings: Transitional.
        2. Room Settings: Contemporary.
        3. Room Settings: Traditional.
        4. Room Settings: Rustic.
        5. Decorative Fronts: Arched Heritage.
        6. Decorative Fronts: Rectangular black.
        7. Decorative Panels: MIRRO-FLAME porcelain reflective radiant panels.
        8. Decorative Panels: Herringbone sandstone.
        9. Surround: Arched black heritage pattern.
        10. Surround: Brushed stainless steel.
        11. Surround: Rectangular black.
        12. Millivolt wall thermostat.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model and fuel type not required.

* 1. GAS BURNING INDOOR DIRECT VENT FIREPLACES - ALTITUDE X SERIES
     1. Altitude X Series: Type: Indoor.
        1. Model AX36 Series: BTU: 36,500.
           1. Fuel Type: Natural gas.
           2. Fuel Type: Propane.
           3. One Side (WxHxD): 35.25 x 42.44 x 18.75 inches (895 x 1078 x 476 mm).
           4. Viewing Areas (WxH): 35.25 x 33 inches (895 x 838 mm).
        2. Model AX42 Series: BTU: 38,000.
           1. Fuel Type: Natural gas.
           2. Fuel Type: Propane.
           3. One Side (WxHxD): 42.25 x 45.44 x 18.63 inches (1073 x 1154 x 473 mm).
           4. Viewing Areas (WxH): 42.25 x 36 inches (1073 x 914 mm).
     2. Features:
        1. Safety barrier. Black.
        2. Glass door.
        3. SIT Proflame II System.
        4. Electronic ignition.
        5. Dual night lights.
        6. Heat circulating blower with variable speed and thermostatic control.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Controls: On/Off switch. Not supplied.
      2. Controls: Battery holder and switch.
      3. Controls: Remote control. Standard.
      4. Controls: eFIRE Bluetooth app.
      5. AMBIENT-GLOW metal fibers.
      6. Door Trim: Black.
      7. Door Trim: Stainless steel.
      8. Decorative Panels: Reflective Radiant: MIRRO-FLAME porcelain radiant panels.
      9. Decorative Panels: Black illusion glass.
      10. Decorative Panels: Westminster Herringbone.
      11. Decorative Panels: Westminster.
      12. Decorative Panels: Old Town Red.
      13. Decorative Panels: Old Town Red Herringbone.
      14. Decorative Panels: Newort.
      15. Room Settings: Transitional.
      16. Room Settings: Contemporary.
      17. Room Settings: Traditional.
      18. Room Settings: Rustic.
      19. Media Kits: Driftwood log.
      20. Media Kits: Birch log.
      21. Media Kits: Split oak.
      22. Media Kits: Maple log
      23. Front Trim: Whitney.
      24. Front Trim: Denali
      25. Front Trim: Charcoal Zen
      26. Front Trim: Black finish.
      27. Front Trim: Charcoal finish.
      28. Front Trim: Copper finish.
      29. Front Trim: Gunmetal finish.
      30. Front Trim: Beveled.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model and fuel type not required.

* 1. GAS BURNING INDOOR DIRECT VENT FIREPLACES - ELEVATION SERIES
     1. Elevation Models: Type: Indoor.
        1. Model: Elevation X36.
           1. Fuel Type: Natural gas. BTU: 37,500.
           2. Fuel Type: Propane. BTU: 34,000.
        2. Dimension (WxHxD): 38.62 x 43.56 x 22.56 inches (981 x 1106 x 573 mm).
        3. Model: Elevation X42.
           1. Fuel Type: Natural gas. BTU: 45,000.
           2. Fuel Type: Propane. BTU: 39,000.
        4. Dimension (WxHxD): 44.62 x 47.56 x 22.50 inches (1133 x 1208 x 572 mm).
     2. Features:
        1. Clean face with full firebox flame.
        2. Safety Barrier: Standard black.
        3. Modulating ENDLESS EMBERS electric ember bed fills the floor below the log set and are visible from every angle.
        4. Heat circulating blower.
        5. Controls: Remote control included controls flame modulation, split-flow, ember bed lights and blower.
        6. Controls: eFIRE Bluetooth app.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Dynamic heat control and dynamic heat control plus.
      2. Room Settings: Transitional.
      3. Room Settings: Contemporary.
      4. Room Settings: Traditional.
      5. Room Settings: Rustic.
      6. Decorative Panels: Westminster Herringbone.
      7. Decorative Panels: Westminster Standard.
      8. Decorative Panels: Old town red herringbone brick.
      9. Decorative Panels: Old town red standards brick.
      10. Decorative Panels: Glacier herringbone brick.
      11. Decorative Panels: Glacier standard brick.
      12. Decorative Panels: Antique ledgestone brick.
      13. Decorative Panels: Newport standard.
      14. Decorative Panels: Black Illusion glass.
      15. Decorative Panels: MIRRO-FLAME porcelain reflective radiant panel
      16. Media Kits: Birch log set.
      17. Media Kits: Driftwood log set.
      18. Media Kits: Split Oak log set.
      19. Front: Premium Denali.
      20. Front: Whitney.
      21. Front: Zen front - black.
      22. Trim Finish: Black.
      23. Trim Finish: Charcoal.
      24. Trim Finish: Copper.
      25. Trim Finish: Gunmetal.
      26. Trim Finish: Beveled Black.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required.

* 1. GAS BURNING INDOOR DIRECT VENT FIRELPLACES - HIGH DEFINITION SERIES
     1. High Definition See Though Series. Type: Indoor. Certified to CSA 2.22 and ANSI Z21.50.
        1. Model High Definition HD81NT-1. Fuel Type: Natural gas. BTU: 60,000.
           1. One Side (WxHxD): 54.25 x 49.25 x 28.75 inches (1378 x 1251 x 730 mm).
           2. Viewing Areas (WxH): 36.75 x 30.75 inches (933 x 781 mm).
     2. Features:
        1. Clean face design.
        2. Accent lights.
        3. Andirons: Black
        4. Proflame 2 electronic gas valve.
        5. YELLOW DANCING FLAMES.
        6. Safety barrier: Black.
        7. Remote control.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Room Settings: Transitional.
      2. Room Settings: Contemporary.
      3. Room Settings: Traditional.
      4. Room Settings: Rustic.
      5. Decorative Panels: MIRRO-FLAME porcelain reflective.
      6. Decorative Panels: Sandstone decorative.
      7. Burner Assembly: Log set.
      8. Burner Assembly: River rock set.
      9. Burner Assembly: Glass embers.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model and model numbers not required.

* 1. GAS BURNING INDOOR DIRECT VENT FIREPLACES - ASCENT SERIES
     1. Ascent Series. Type: Indoor. Certified to CSA 2.22 and ANSI Z21.50.
        1. Model Ascent 30. Fuel Type: Natural gas. BTU: 15,000.
           1. Model No: B30NTR-1. Millivolt ignition.
           2. Model No: B30NTRE-1. Electronic ignition.
           3. One Side (WxHxD): 30 x 34.63 x 14 inches (762 x 880 x 356 mm).
           4. Viewing Areas (WxH): 25.69 x 23.69 inches (653 x 602 mm).
        2. Model Ascent 36.
           1. Model No: B36NTR-1. Millivolt ignition. Fuel Type: Natural gas. BTU: 15,000.
           2. Model No: B36PTR-1. Millivolt ignition. Fuel Type: Propane. BTU: 18,000.
           3. Model No: B36PTRE-1. Electronic ignition. Fuel Type: Propane. BTU: 18,000.
           4. One Side (WxHxD): 35 x 34.63 x 15.75 inches (762 x 880 x 400 mm).
           5. Viewing Areas (WxH): 30.69 x 23.69 inches (779 x 602 mm).
           6. Surround: Wrought iron.
           7. Surround: Matte black clean face.
        3. Model Ascent 42. Fuel Type: Natural Gas. BTU: 22,000.
           1. Model No: B42NTR. Millivolt ignition.
           2. Model No: B42NTRE. Electronic ignition.
           3. One Side (WxHxD): 42 x 34.63 x 18.31 inches (1067 x 88 x 465 mm).
           4. Viewing Areas (WxH): 37.69 x 23.69 inches (957 x 602 mm).
           5. Surround: Wrought iron
        4. Model Ascent 42. Fuel Type: Propane. BTU: 22,000.
           1. Model No: B42PTR. Millivolt ignition.
           2. Model No: B42PTRE. Electronic ignition.
           3. One Side (WxHxD): 42 x 34.63 x 18.31 inches (1067 x 880 x 465 mm).
           4. Viewing Areas (WxH): 37.69 x 23.69 inches (957 x 602 mm).
           5. Surround: Wrought iron.
        5. Model Ascent 46. Fuel Type: Natural Gas. BTU: 22,000.
           1. Model No: B46NTR. Millivolt ignition.
           2. Model No: B46NTRE. Electronic ignition.
           3. One Side (WxHxD): 46 x 34.63 x 18.31 inches (1067 x 88 x 465 mm).
           4. Viewing Areas (WxH): 41.69 x 23.69 inches (1059 x 602 mm).
           5. Mobile home approved.
     2. Features:
        1. Pan style burner.
        2. Back-Up control system.
        3. Glass door.
        4. Controls: Pre-Wired for wall switch.
        5. Controls: Remote control.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Room Settings: Transitional.
      2. Room Settings: Contemporary.
      3. Room Settings: Traditional.
      4. Room Settings: Rustic.
      5. Decorative Panels: MIRRO-FLAME porcelain reflective.
      6. Decorative Panels: Old Town red herringbone.
      7. Decorative Panels: Sandstone decorative.
      8. Decorative Panels: Westminster herringbone.
      9. Decorative Panels: Westminster standard.
      10. Media Kits: PHAZER Log Set. Standard.
      11. Media Kits: Beach Fire.
      12. Media Kits: Mineral Rock.
      13. Media Kits: Shore Fire.
      14. Safety Barrier: Black Heritage.
      15. Safety Barrier: Black Zen.
      16. Safety Barrier: Standard Black.
      17. Trim: Black 2.
      18. Trim: Black 3 Premium Beveled.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model and model numbers not required.

* 1. GAS BURNING INDOOR DIRECT VENT FIRELPLACES - ASCENT X SERIES
     1. Ascent X-Series. Type: Indoor. Certified to CSA 2.22 and ANSI Z21.50.
        1. Model Ascent X 36:
           1. Model No: GX36NTR-1. Millivolt ignition. Fuel Type: Natural gas. BTU: 26,000.
           2. Model No: GX36NTRE-1. Electric ignition. Fuel Type: Natural gas. BTU: 26,000.
           3. Model No: GX36PTR-1. Millivolt ignition. Fuel Type: Propane. BTU: 26,000.
           4. Model No: GX36PTRE-1. Electric ignition. Fuel Type: Propane. BTU: 26,000.
           5. One Sided (WxHxD): 35 x 34.63 x 15.75 inches (889 x 880 x 400 mm).
           6. Viewing Areas (WxH): 30.69 x 23.69 inches (780 x 602 mm).
        2. Model Ascent X 42
           1. Model No: GX42NTRE-1. Electric ignition. Fuel Type: Natural gas. BTU: 30,000.
           2. Model No: GX42PTRE-1. Electric ignition. Fuel Type: Propane. BTU: 30,000.
           3. One Sided (WxHxD): 42 x 40.88 x 18.31 inches 1067 x 1038 x 465 mm).
           4. Viewing Areas (WxH): 34.80 x 20.94 inches (884 x 32 mm).

\*\* NOTE TO SPECIFIER \*\* Feature below apply to the Ascent X 36 and X 42 models above

* + - 1. Features:
         1. Exclusive PHAZER log set and glowing ember bed.
         2. Pan style burner.
         3. Safety Barrier: Standard premium.
         4. Glass door.
         5. Back-up control system.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - * 1. Controls: Pre-Wired for wall switch.
        2. Controls: Battery holder and switch.
        3. Controls: Remote control.
        4. Controls: eFIRE remote app.
        5. Room Settings: Transitional.
        6. Room Settings: Contemporary.
        7. Room Settings: Traditional.
        8. Room Settings: Rustic.
        9. Decorative Panels: MIRRO-FLAME porcelain reflective.
        10. Decorative Panels: Sandstone decorative.
        11. Decorative Panels: Westminster herringbone.
        12. Decorative Panels: Newport decorative.
        13. Media Kits: PHAZER Log Set. Standard.
        14. Media Kits: Beach fire.
        15. Media Kits: Mineral rock.
        16. Media Kits: Shore fire.
        17. Trim: Black 2.
        18. Trim: Black 3 Premium beveled.
      1. Model Ascent X 70
         1. Model No: GX70NTE-1. Electric ignition. Fuel Type: Natural gas. BTU: 35,000.
         2. Model No: GX70PTE-1. Electric ignition. Fuel Type: Propane. BTU: 35,000.
         3. One Sided (WxHxD): 35 x 34.63 x 18.51 inches (889 x 880 x 470 mm).
         4. Viewing Areas (WxH): 30.69 x 23.69 inches (780 x 602 mm).
         5. Features:

Exclusive PHAZER log set and glowing ember bed.

Pan style burner.

Glass door.

Back-up control system.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

Controls: Pre-Wired for wall switch.

Controls: Battery holder and switch.

Controls: Remote control.

Controls: eFIRE remote app.

Room Settings: Transitional.

Room Settings: Contemporary.

Room Settings: Traditional.

Room Settings: Rustic.

Decorative Panels: MIRRO-FLAME porcelain reflective.

Decorative Panels: Newport decorative.

Decorative Panels: Old town red decorative.

Media Kits: PHAZER Log Set. Standard.

Safety Barrier: Black Heritage.

Safety Barrier: Black Zen.

Safety barrier: Premium black.

Surround: back with operable screen.

Surround: Matte black clean face.

Surround: Scalloped wrought from decorative.

Surround: Wrought iron.

Trim: Black 2.

Trim: Black 3 premium beveled.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model numbers not required.

* 1. GAS BURNING INDOOR DIRECT VENT FIRELPLACES - ASCENT DEEP SERIES
     1. Ascent Deep-Series. Type: Indoor. Certified to CSA 2.22 and ANSI Z21.50.
        1. Model Ascent Deep 42:
           1. Model No: D42NTRE. Fuel Type: Natural gas. BTU: 26,000.

One Sided (WxHxD): 40.25 x 37.44 x 23.75 inches (1022 x 951 x 603 mm).

Viewing Areas (WxH): 33.25 x 24 inches (845 x 610 mm).

Tempered heat resistant glass.

\*\* NOTE TO SPECIFIER \*\* The following paragraph is optional. Delete if not required.

Control: Remote. Blower.

* + - * 1. Model No: D42PTRE. Fuel Type: Propane. BTU: 26,000.

One Sided (WxHxD): 40.25 x 37.44 x 23.75 inches (1022 x 951 x 603 mm).

Viewing Areas (WxH): 33.25 x 24 inches (845 x 610 mm).

Tempered heat resistant glass

Control: Remote.

Blower.

* + - * 1. Model No: DX42NTRE. Fuel Type: Natural gas. BTU: 31,000.

One Sided (WxHxD): 40.25 x 37.44 x 23.75 inches (1022 x 951 x 603 mm).

Viewing Areas (WxH): 33.25 x 24 inches (845 x 610 mm ).

Ceramic glass.

\*\* NOTE TO SPECIFIER \*\* The following paragraph is optional. Delete if not required.

Control: Remote. Blower.

* + - * 1. Model No: DX42PTRE. Fuel Type: Propane. BTU: 31,000.

One Sided (WxHxD): 40.25 x 37.44 x 23.75 inches (1022 x 951 x 603 mm).

Viewing Areas (WxH): 33.25 x 24 inches (845 x 610 mm ).

Ceramic glass.

Control: Remote.

Blower.

* + 1. Features:
       1. Allows Rigid and Flex venting.
       2. Safety barrier.
       3. Night light.
       4. Battery back-up, USB charge.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Heat Management for reduced clearance to combustible.
      2. Room Settings: Transitional.
      3. Room Settings: Contemporary.
      4. Room Settings: Traditional.
      5. Room Settings: Rustic.
      6. Decorative Panels: MIRRO-FLAME porcelain reflective.
      7. Decorative Panels: Newport decorative.
      8. Decorative Panels: Sandstone decorative.
      9. Decorative Panels: Old town red decorative.
      10. Decorative Panels: Old town red herringbone.
      11. Decorative Panels: Westminster herringbone.
      12. Decorative Panels: Westminster.
      13. Media Kits: Beach Fire.
      14. Media Kits: Mineral Rock.
      15. Media Kits: Shore Fire.
      16. Trim: Zen Black.
      17. Trim: Black beveled.
      18. Trim: Black.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model numbers not required.

* 1. GAS BURNING INDOOR DIRECT VENT FIRELPLACES - ASCENT MULTI-VIEW SERIES
     1. Ascent Multi-View Series. Type: Indoor 3-sided peninsula. Certified to CSA 2.22 and ANSI Z21.50.
        1. Model No: BHD4PN: Fuel Type: Natural gas. BTU: 30,000.

One Sided (WxHxD): 43.25 x 38.25 x 15.13 inches (1099 x 972 x 384 mm).

Viewing Areas (WxH): 35.5 x 28.50 inches (902 x 724 mm).

Burner Assembly: PHAZER log set

Burner Assembly: Fire cradle.

* + - 1. Model No: BHD4PGN: Fuel Type: Natural gas. BTU: 30,000.

One Sided (WxHxD): 43.25 x 38.25 x 15.13 inches (1099 x 972 x 384 mm).

Viewing Areas (WxH): 35.5 x 28.50 inches (902 x 724 mm).

Burner Assembly: Crystalline ember bed.

Burner Assembly: Fire cradle.

Glass Media: Beads.

Glass Media: Embers.

Color: Amber.

Color: Black.

Color: Blue.

Color: Clear.

Color: Topaz.

Decorative Media: Iron globes.

Decorative Media: Nickel stix.

Decorative Media: Rock media.

* + - 1. Model No: BHD4STN: See through. Fuel Type: Natural gas. BTU: 30,000.

One Sided (WxHxD): 45 x 38.25 x 25.13 inches (1143 x 971 x 638 mm).

Viewing Areas (WxH): 35.5 x 28.50 inches (902 x 724 mm).

Burner Assembly: PHAZER log set.

Burner Assembly: Fire cradle.

* + - 1. Model No: BHD4PFCN: Fuel Type: Natural gas. BTU: 30,000

One Sided (WxHxD): 45 x 38.25 x 25.13 inches (1143 x 971 x 638 mm).

Viewing Areas (WxH): 35.5 x 28.50 inches (902 x 724 mm).

Burner Assembly: Crystalline ember bed.

Burner Assembly: Fire cradle.

Glass Media: Beads.

Glass Media: Embers.

Color: Amber.

Color: Black.

Color: Blue.

Color: Clear.

Color: Topaz.

* + - 1. Model No: BHD4STGN: See though. Fuel Type: Natural gas. BTU: 30,000

One Sided (WxHxD): 45 x 38.25 x 25.13 inches (1143 x 971 x 638 mm).

Viewing Areas (WxH): 35.5 x 28.50 inches (902 x 724 mm).

Burner Assembly: PHAZER log set.

Burner Assembly: Crystalline ember bed.

Burner Assembly: Fire cradle.

Glass Media: Beads.

Glass Media: Embers.

Color: Amber.

Color: Black.

Color: Blue.

Color: Clear.

Color: Topaz.

Decorative Media: Iron globes.

Decorative Media: Nickel stix.

Decorative Media: Rock media.

* + - 1. Model No: BHD4STFCN: See though. Fuel Type: Natural gas. BTU: 30,000.

One Sided (WxHxD): 45 x 38.25 x 25.13 inches (1143 x 971 x 638 mm).

Viewing Areas (WxH): 35.5 x 28.50 inches (902 x 724 mm).

Burner Assembly: PHAZER log set.

Burner Assembly: Fire cradle.

Burner Assembly: CRYSTALINE ember bed.

Glass Media: Beads.

Glass Media: Embers.

Color: Amber.

Color: Black.

Color: Blue.

Color: Clear.

Color: Topaz.

* + 1. Features:
       1. Safety Barrier: Standard black.
       2. Safety screen.
       3. AMBIENT-GLOW metal fibers.
       4. Ignition: Electric with battery backup.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Remote control.
      2. Room Settings: Transitional.
      3. Room Settings: Contemporary.
      4. Room Settings: Traditional.
      5. Room Settings: Rustic.
      6. Decorative Panels: MIRRO-FLAME porcelain reflective.
      7. Decorative Panels: Newport deluxe decorative.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete models not required.

* 1. GAS BURNING LINEAR INDOOR DIRECT VENT FIRELPLACES - ASCENT LINEAR
     1. Comply with applicable building codes.
        1. Comply with ANSI Z21.88/CSA 2.33.
        2. WHI listed.
        3. Safety Barriers are "Safety Barrier Approved."
     2. Ascent Linear Models: Type: Indoor.
        1. Model: Linear 36NTE.
           1. Fuel Type: Natural gas. BTU: 17.500.
           2. One Side (WxHxD): 35.94 x 39.06 x 15.75 inches (913 x 992 x 400 mm).
           3. Viewing Areas (WxH): 30.75 x 16.75 inches (781 x 425 mm).
        2. Model: Linear 36NTEA.
           1. Fuel Type: Natural gas. BTU: 17.500.
           2. One Side (WxHxD): 35.94 x 39.06 x 15.75 inches (913 x 992 x 400 mm).
           3. Viewing Areas (WxH): 30.75 x 16.75 inches (781 x 425 mm).
        3. Model: Linear 46NTE.
           1. Fuel Type: Natural gas. BTU: 24,000.
           2. One Side (WxHxD): 46.94 x 39.06 x 18.31 inches (1192 x 992 x 464 mm).
           3. Viewing Areas (WxH): 41.75 x 16.75 inches (1060 x 425 mm).
     3. Features:
        1. Safety barrier.
        2. Firebox glass door.
        3. SIT Proflame II System.
        4. Electronic ignition.
        5. Easy access air control.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Propane conversion kit.
      2. Controls: On/Off switch. Not supplied.
      3. Controls: Battery holder and switch.
      4. Controls: Remote control.
      5. Controls: eFIRE Bluetooth app.
      6. Door Trim: Black.
      7. Door Trim: Stainless steel.
      8. Surround: Classic black.
      9. Surround: Premium brushed stainless steel.
      10. Reflective Radiant Panels: MIRRO-FLAME porcelain.
      11. Room Settings: Transitional.
      12. Room Settings: Contemporary.
      13. Room Settings: Traditional.
      14. Room Settings: Rustic.
      15. Media Kits: Beach Fire.
      16. Media Kits: Mineral Rock.
      17. Media Kits: Shore Fire.
      18. Glass Beads Media: Amber.
      19. Glass Beads Media: Black.
      20. Glass Beads Media: Blue.
      21. Glass Beads Media: Clear.
      22. Glass Beads Media: Red.
      23. Glass Beads Media: Topaz.
      24. Glass Embers Media: Amber.
      25. Glass Embers Media: Black.
      26. Glass Embers Media: Blue.
      27. Glass Embers Media: Clear.
      28. Glass Embers Media: Red.
      29. Glass Embers Media: Topaz.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete models not required.

* 1. GAS BURNING LINEAR INDOOR DIRECT VENT FIRELPLACES - VECTOR
     1. Vector Models: Type: Indoor.
        1. Model LV38 Series. Vector 38 Direct Vent Gas Fireplace:
           1. Fuel Type: Natural gas. BTU: 30,000.
           2. One Side (WxHxD): 53.31 x 41.19 x 18.89 inches (1354 x 1046 x 480 mm).
           3. See Through (WxHxD): 53.31 x 41.19 x 16.19 inches (1354 x 1046 x 411 mm).
           4. Viewing Areas (WxH): 40.75 x 18.62 inches (1035 x 473 mm).
        2. Model LV50 Series. Vector 50 Direct Vent Gas Fireplace:
           1. Fuel Type: Natural gas. BTU: 36,000.
           2. One Side (WxHxD): 65.31 x 41.19 x 19.89 inches (1760 x 1046 x 505 mm).
           3. See Through (WxHxD): 65.31 x 41.19 x 16.19 inches (1760 x 1046 x 411 mm).
           4. Viewing Areas (WxH): 52.75 x 18.62 inches (1340 x 473 mm).
        3. Model LV62 Series. Vector 62 Direct Vent Gas Fireplace:
           1. Fuel Type: Natural gas. BTU: 36,000.
           2. One Side (WxHxD): 73.31 x 41.19 x 19.89 inches (2065 x 1046 x 505 mm).
           3. See Through (WxHxD): 77.31 x 41.19 x 16.19 inches (1964 x 1046 x 411 mm).
           4. Viewing Areas (WxH): 64.75 x 18.62 inches (1645 x 473 mm).
        4. Model LV74 Series. Vector 74 Direct Vent Gas Fireplace:
           1. BTU: 50,000.
           2. Fuel Type: Natural gas.
           3. Fuel Type: Propane.
           4. One Side (WxHxD): 93.31 x 41.19 x 17.19 inches (2065 x 1046 x 437 mm).
           5. See Through (WxHxD): 93.31 x 41.19 x 16.19 inches (2065 x 1046 x 411 mm).
           6. Viewing Areas (WxH): 78.12 x 18.62 inches (1984 x 473 mm)
     2. Features:
        1. Dynamic Heat Control: Allows controls to be placed above fireplace and specific heat management or select rooms.
        2. Firebox glass door.
        3. Night light system.
        4. Divinity flame pattern.
        5. Electronic ignition.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Controls: On/Off switch. Not supplied.
      2. Controls: Battery holder and switch.
      3. Controls: Remote control.
      4. Controls: eFIRE Bluetooth app. Standard.
      5. Door Trim: Black.
      6. Door Trim: Stainless steel.
      7. Surround: Premium black.
      8. Surround: Brushed stainless steel.
      9. Safety Barrier: Premium black.
      10. Safety Barrier: Brushed stainless steel.
      11. Decorative Front: Stainless steel.
      12. Decorative Front: Stainless steel trim.
      13. Decorative Front: Stainless steel two-tone.
      14. Decorative Front: Black.
      15. Decorative Front: Black trim.
      16. Reflective Radiant Panels: MIRRO-FLAME porcelain.
      17. Room Settings: Transitional.
      18. Room Settings: Contemporary.
      19. Room Settings: Traditional.
      20. Room Settings: Rustic.
      21. Media Kits: Beach Fire.
      22. Media Kits: Birch Log.
      23. Media Kits: Contemporary Log.
      24. Media Kits: Mineral Rock.
      25. Media Kits: Nickel Stix.
      26. Media Kits: Shore Fire.
      27. Media Kits: Wrought Iron Globe.
      28. Glass Beads Media: Amber.
      29. Glass Beads Media: Black.
      30. Glass Beads Media: Blue.
      31. Glass Beads Media: Clear.
      32. Glass Beads Media: Red.
      33. Glass Beads Media: Topaz.
      34. Glass Embers Media: Amber.
      35. Glass Embers Media: Black.
      36. Glass Embers Media: Blue.
      37. Glass Embers Media: Clear.
      38. Glass Embers Media: Red.
      39. Glass Embers Media: Topaz.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model not required.

* 1. GAS BURNING LINEAR INDOOR DIRECT VENT FIRELPLACES - LUXURIA
     1. Luxuria Models: Type: Indoor
        1. Model LVX38 Series. Luxuria 38 Direct Vent Gas Fireplace:
           1. Fuel Type: Natural gas. BTU: 32,000.
           2. One Side (WxHxD): 57.31 x 41.19 x 17.19 inches (1456 x 1046 x 437 mm).
           3. See Through (WxHxD): 57.31 x 41.19 x 16.19 inches (1456 x 1046 x 411 mm).
           4. Viewing Areas (WxH): 41.12 x 18.62 inches (1044 x 473 mm).
        2. Model LVX50 Series. Luxuria 50 Direct Vent Gas Fireplace:
           1. Fuel Type: Natural gas. BTU: 36,000.
           2. One Side (WxHxD): 69.31 x 41.19 x 17.19 inches (1456 x 1046 x 437 mm).
           3. See Through (WxHxD): 69.31 x 41.19 x 16.19 inches (1456 x 1046 x 411 mm).
           4. Viewing Areas (WxH): 54.12 x 18.62 inches (1375 x 473 mm).
        3. Model LVX62 Series. Luxuria 62 Direct Vent Gas Fireplace:
           1. Fuel Type: Natural gas. BTU: 44,000.
           2. One Side (WxHxD): 81.31 x 41.19 x 17.19 inches (2065 x 1046 x 437 mm).
           3. See Through (WxHxD): 81.31 x 41.19 x 16.19 inches (2065 x 1046 x 411 mm).
           4. Viewing Areas (WxH): 66.12 x 18.62 inches (1679 x 473 mm).
        4. Model LVX74 Series. Luxuria 74 Direct Vent Gas Fireplace:
           1. BTU: 50,000.
           2. Fuel Type: Natural gas or propane.
           3. Fuel Type: Propane.
           4. One Side (WxHxD): 93.31 x 41.19 x 17.19 inches (2065 x 1046 x 437 mm).
           5. See Through (WxHxD): 93.31 x 41.19 x 16.19 inches (2065 x 1046 x 411 mm).
           6. Viewing Areas (WxH): 78.12 x 18.62 inches (1984 x 473 mm).
     2. Features:
        1. Dynamic Heat Control: Allows controls to be placed above fireplace and specific heat management or select rooms.
        2. Premium glass guard system and heat rail.
        3. Door trim.
        4. Firebox glass door.
        5. Night light system.
        6. Divinity flame pattern.
        7. Electronic ignition.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Controls: On/Off switch. Not supplied.
      2. Controls: Battery holder and switch.
      3. Controls: Remote control.
      4. Controls: eFIRE Bluetooth app. Standard.
      5. Reflective Radiant Panels: MIRRO-FLAME porcelain.
      6. Room Settings: Transitional.
      7. Room Settings: Contemporary.
      8. Room Settings: Traditional.
      9. Room Settings: Rustic.
      10. Media Kits: Beach Fire.
      11. Media Kits: Birch Log.
      12. Media Kits: Contemporary Log.
      13. Media Kits: Mineral Rock.
      14. Media Kits: Nickel Stix.
      15. Media Kits: Shore Fire.
      16. Media Kits: Wrought Iron Globe.
      17. Glass Beads Media: Amber.
      18. Glass Beads Media: Black.
      19. Glass Beads Media: Blue.
      20. Glass Beads Media: Clear.
      21. Glass Beads Media: Red.
      22. Glass Beads Media: Topaz.
      23. Glass Embers Media: Amber.
      24. Glass Embers Media: Black.
      25. Glass Embers Media: Blue.
      26. Glass Embers Media: Clear.
      27. Glass Embers Media: Red.
      28. Glass Embers Media: Topaz.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete mounting type and model not required.

* 1. ELECTRIC INDOOR FIREPLACES - ALLURE VERTICAL
     1. General: Comply with applicable building codes. UL listed.
     2. Model: Allure Vertical. Electric. BTU: 5000. Watts: 1,500 Maximum.
        1. Mounting Type: Surface.
        2. Mounting Type: Partially recessed.
        3. Model NEFVC32H (WxHxD): 15.25 x 32 x 5.5 inches (387x 813 x 140 mm).
           1. Viewing Area (WxH): 16 x 20 inches (406 x 508 mm).
        4. Model NEFVC38H (WxHxD): 16 x 38 x 5.5 inches (406 x 965 x 140 mm).
           1. Viewing Area (WxH): 16 x 26 inches (406 x 660 mm).
     3. Features:
        1. Trim: Black.
        2. Control Panel, touch screen.
        3. Remote Control: Adjusts flame height, heat and on/off.
        4. Flame speed control.
        5. Flame brightness control.
        6. Front facing vents.
        7. Quiet Blower with Boost Function Included.

\*\* NOTE TO SPECIFIER \*\* Select the options required from the following paragraphs and delete those not required.

* + - 1. Plug-in, 120 VAC.
      2. Hardwired, 120 or 240 VAC.
      3. Room Settings: Transitional.
      4. Room Settings: Contemporary.
      5. Room Settings: Traditional.
      6. Room Settings: Rustic.
      7. Flame Color: Blue.
      8. Flame Color: Multicolor.
      9. Flame Color: Orange.
      10. Flame Color: Yellow.
      11. Media Kit: Birch log.
      12. Media Kit: Crystal clear cube.
      13. Ember Bed Lights: Yellow Lights Logs.
      14. Ember Bed Lights: White Lights Logs.
      15. Ember Bed Lights: Red Lights Logs.
      16. Ember Bed Lights: Purple Lights Logs.
      17. Ember Bed Lights: Green Lights Logs
      18. Ember Bed Lights: Blue Lights Logs
      19. Accent Lights: Yellow.
      20. Accent Lights: White.
      21. Accent Lights: Red.
      22. Accent Lights: Purple.
      23. Accent Lights: Green.
      24. Accent Lights: Blue.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete models not required.

* 1. ELECTRIC INDOOR FIREPLACES - ALLURAVISION
     1. Model: Alluravision NEFL42CH Series 42. Comply with applicable building codes. UL listed.
        1. Slim (WxHxD): 44.5 x 17 x 4.25 inches (1130 x 432 x 108 mm). BTU: 5000
        2. Deep (WxHxD): 44.44 x 17.32 x 5.81 inches (1128 x 440 x 148 mm). BTU: 9000
        3. Viewing Areas (WxH): 40.25 x 11 inches (1022 x 279 mm).
     2. Model: Alluravision NEFL50CH Series 50. Comply with applicable building codes. UL listed.
        1. Slim (WxHxD): 52.69 x 17.32 x 4.25 inches (1338 x 440 x 108 mm). BTU: 5000
        2. Deep (WxHxD): 52.69 x 17.32 x 5.81 inches (1338 x 440 x 148 mm). BTU: 9000
        3. Viewing Areas (WxH): 48.50 x 11 inches (1232 x 279 mm).
     3. Model: Alluravision NEFL60CH Series 60. Comply with applicable building codes. UL listed.
        1. Slim (WxHxD): 62.56 x 17.32 x 4.25 inches (1589 x 440 x 108 mm). BTU: 5000
        2. Deep (WxHxD): 62.56 x 17.32 x 5.81 inches (1589 x 440 x 148 mm). BTU: 9000
        3. Viewing Areas (WxH): 58.50 x 11 inches (1486 x 279 mm).
     4. Model: Alluravision NEFL74CH Series 74. Comply with applicable building codes. UL listed.
        1. Slim (WxHxD): 76.75 x 17.32 x 4.25 inches (1943 x 440 x 108 mm). BTU: 5000
        2. Deep (WxHxD): 76.75 x 17.32 x 5.81 inches (1943 x 440 x 148 mm). BTU: 9000
        3. Viewing Areas (WxH): 72.50 x 11 inches (1841 x 279 mm).
     5. Model: Alluravision NEFL100CH Series 100. Comply with applicable building codes. UL listed.
        1. Deep (WxHxD): 102.69 x 17.32 x 5.81 inches (2608 x 440 x 148 mm). BTU: 9000
        2. Viewing Areas (WxH): 98.50 x 11 inches (2502 x 279 mm).
     6. Features:
        1. Power requirements: 120 VAC.
        2. Trim: Black.
        3. Control Panel, touch screen.
        4. Remote Control: Adjusts flame height, heat and on/off.
        5. Flame speed control.
        6. Flame brightness control.
        7. Front facing vents.
        8. Quiet blower with boost function included.

\*\* NOTE TO SPECIFIER \*\* Select the options required from the following paragraphs and delete those not required.

* + - 1. Type: Electric wall mount.
      2. Type: Recessed.
      3. Plug-in, 120 VAC.
      4. Hardwired, 120 or 240 VAC.
      5. Room Settings: Transitional.
      6. Room Settings: Contemporary.
      7. Room Settings: Traditional.
      8. Room Settings: Rustic.
      9. Glass Media: Crystal clear cubes.
      10. Flame Color: Blue.
      11. Flame Color: Multicolor.
      12. Flame Color: Orange.
      13. Flame Color: Yellow.
      14. LED Lights: Blue.
      15. LED Lights: Green.
      16. LED Lights: Purple.
      17. LED Lights: Red.
      18. LED Lights: Yellow.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete models not required.

* 1. ELECTRIC INDOOR FIREPLACES - ENTICE
     1. Entice Series. Electric. BTU: 5000.
        1. Model: NEFL36CFH (WxHxD): 36 x 16.94 x 5.44 inches (914 x 430 x 138 mm).
           1. Viewing Areas (WxH): 32 x 12 inches (813 x 305 mm).
        2. Model: NEFL42CFH (WxHxD): 41.75 x 16.94 x 5.44 inches (1060 x 430 x 138 mm).
           1. Viewing Areas (WxH): 38 x 12 inches (965 x 305 mm).
        3. Model: NEFL50CFH (WxHxD): 49.69 x 16.94 x 5.44 inches (1262 x 430 x 138 mm).
           1. Viewing Areas (WxH): 45.75 x 12 inches (1162 x 305 mm).
        4. Model: NEFL60CFH (WxHxD): 59.69 x 16.94 x 5.44 inches (1516 x 430 x 138 mm).
           1. Viewing Areas (WxH): 55.75 x 12 inches (1416 x 305 mm).
        5. Model: NEFL72CFH (WxHxD): 71.69 x 16.94 x 5.44 inches (1821 x 430 x 138 mm).
           1. Viewing Areas (WxH): 67.75 x 12 inches (1721 x 305 mm).
     2. Features:
        1. Trim: Black.
        2. Control Panel, touch screen.
        3. Remote Control: Adjusts flame height, heat and on/off.
        4. Flame speed control.
        5. Flame brightness control.
        6. Front facing vents.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Type: Wall mount.
      2. Type: Partially recessed.
      3. Type: Recessed.
      4. Plug-in, 120 V,
      5. Hardwired, 120 or 240 V.
      6. Room Settings: Transitional.
      7. Room Settings: Contemporary.
      8. Room Settings: Traditional.
      9. Room Settings: Rustic.
      10. Media Kits: Driftwood log,
      11. Media Kits: Birch log.
      12. Media Kits: Crystal clear.
      13. Flame Color: Blue.
      14. Flame Color: Multicolor.
      15. Flame Color: Orange.
      16. Lights, Crystal: Blue.
      17. Lights, Crystal: Green.
      18. Lights, Crystal: Orange.
      19. Lights, Crystal: Purple.
      20. Lights, Crystal: Red.
      21. Lights, Crystal: Yellow.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model not required.

* 1. ELECTRIC INDOOR FIREPLACES - CLEARION ELITE
     1. Certified to CSA C22.2 No. 46 and UL 2021. BTU: 10,000.
        1. Model NEFBD50HE. CLEARion Elite 50. See through electric recessed wall mount.
           1. Dimensions (WxHxD): 50 x 18.38 x 9.06 inches (1270 x 467 mm)
           2. Viewing Area (WxH): 43.63 x 12 inches (1108 x 305 mm)
        2. Model NEFBD60HE. CLEARion Elite 60. See through electric recessed wall mount.
           1. Dimensions (WxHxD): 60 x 20.44 x 9.19 inches (1524 x 519 x 233 mm)
           2. Viewing Area (WxH): 53.50 x 14 inches (1359 x 356 mm)
     2. Features
        1. Privacy Glass: Instantaneously switch between transparent, semi-transparent, and fully opaque.
        2. Five different flame speed options
        3. Simple framing specifications. 8 inch (203 mm) wall thickness.
        4. Full feature remote control. Adjustable flame and ember light control with nightlight.
        5. Clear Glass Ember Bed.
        6. Safety Barrier: Standard barrier.
        7. Hardwired, 120 or 240 VAC.
        8. Surround: Black.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Controls: On/Off switch. Not supplied.
      2. Controls: Battery holder and switch.
      3. Controls: Remote control. Standard.
      4. Controls: eFIRE Bluetooth app.
      5. Type: Wall mount.
      6. Type: Partially recessed.
      7. Type: Recessed.
      8. Room Settings: Transitional.
      9. Room Settings: Contemporary.
      10. Room Settings: Traditional.
      11. Room Settings: Rustic.
      12. Glass Settings: See through.
      13. Glass Settings: Translucent.
      14. Glass Settings: Opaque.
      15. Flame Colors: Blue.
      16. Flame Colors: Orange.
      17. Flame Colors: Multicolor.
      18. Lights - Log Set: Blue.
      19. Lights - Log Set: Magenta.
      20. Lights - Log Set: Red.
      21. Lights - Log Set: Orange.
      22. Lights - Log Set: Yellow.
      23. Lights - Log Set: Green.
      24. Lights - Log Set: White.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model not required.

* 1. ELECTRIC INDOOR FIREPLACES - STYLUS SERIES
     1. Certified to CSA C22.2 No. 46 and UL 2021.
        1. Model Stylus Cara. No: NEFP32-5019W. Electric. Wall hanging. BTU: 5,000.
           1. Dimensions (WxHxD): 59.13. x 20.31 x 11 inches (1502 x 511 x 279 mm)
           2. Viewing Area (WxH): 31.75 x 12 inches (806 x 305 mm)
        2. Model Stylus Steinfeld. No: NEFP32-5020BW. Electric. Wall hanging. BTU: 5,000.
           1. Dimensions (WxHxD): 53.13 x 19.81 x 10.25 inches (1350 x 503 x 260 mm)
           2. Viewing Area (WxH): 32 x 12 inches (813 x 305 mm)
     2. Features:
        1. Plug-in, 120 VAC.
        2. Combination birch log set and crystal media.
        3. Accent shelf light with color and brightness settings.
        4. USB: 2 inputs with charging status color indication.
        5. Flame Color Settings: Four. Brightness adjustment options.
        6. Ember Bed Color Settings: 6 cycles. Fade-in and fade-out.
        7. Timer Settings: 9 different. From 30 minutes up to 8 hours.
        8. All Season Usage: Operates with or without heat.
        9. Disable heat function.
        10. Controls: Thermostat. Touch control panel. Multi-function remote.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete models not required.

* 1. ELECTRIC INDOOR FIREPLACES - TRIVISTA SERIES
     1. Certified to CSA C22.2 No. 46 and UL 2021.
        1. Trivista Models: Electric. 3-sided. BTO: 10,000
        2. Model: Trivista Primis 50. Wall mounted. No: NEFB50H-3SV
           1. Dimensions (WxHxD): 50 x 21.50 x 9.50 inches 1270 x 546 x 241 mm)
           2. Viewing Area (WxH): 48.50 x 15 inches (1232 x 381 mm)
        3. Model: Trivista Primis 60. Wall mounted. No: NEFB60H-3SV
           1. Dimensions (WxHxD): 60 x 20.50 x 9.50 inches (1524 x 521 x 241 mm)
           2. Viewing Area (WxH): 58.50 x 15 inches (1456 x 381 mm)
     2. Features:
        1. All seasons use.
        2. LED top lights.
        3. Northern Woods log set and crystal media.
        4. Controls: Remote.
        5. Controls: Touchscreen.
        6. Controls: Motion Proximity sensor.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. End panels.
      2. Ember Bed Color: Royal Blue.
      3. Ember Bed Color: Clear.
      4. Ember Bed Color: Dark Orange.
      5. Ember Bed Color: Fuschia.
      6. Ember Bed Color: Green.
      7. Ember Bed Color: Light Blue.
      8. Ember Bed Color: Lime.
      9. Ember Bed Color: Orange.
      10. Ember Bed Color: Purple.
      11. Ember Bed Color: Red.
      12. Ember Bed Color: Teal.
      13. Ember Bed Color: Yellow.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model not required.

* 1. ELECTRIC INDOOR FIREPLACES - ASCENT ELECTRIC SERIES
     1. Certified to CSA C22.2 No. 46 and UL 2021.
        1. Model Ascent 33 Electric. No: NEFB33H. Electric. BTU: 9,000.
           1. Dimensions (WxHxD): 40.37 x 32 x 14 inches (1025 x 813 x 356 mm)
           2. Viewing Area (WxH): 38 x 27 inches (965 x 686 mm)
        2. Model Ascent 40 Electric. No: NEFB40H Electric. BTU: 9,000.
           1. Dimensions (WxHxD): 40.37 x 32 x 14 inches (1025 x 813 x 356 mm)
           2. Viewing Area (WxH): 38 x 27 inches (965 x 686 mm)
     2. Features:
        1. Can be recessed or hung on a wall.
        2. All seasons use.
        3. ULTRA BRIGHT LED lighting
        4. WHISPER QUIET fan and heater.
        5. Non-reflective backing.
        6. Can be set to Fahrenheit or Celsius settings.
        7. Self-trimming flange.
        8. Realistic brick panels, glowing logs, and ember bed.
        9. Self-diagnostic LED Light Indicates when any issues arise.
        10. Controls: Remote.
        11. Controls: Touchscreen.
        12. Controls: Motion Proximity sensor.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Plug in 120 / 240 VAC.
      2. Hardwire 120 / 240 VAC.
      3. Room Settings: Transitional.
      4. Room Settings: Contemporary.
      5. Room Settings: Traditional.
      6. Room Settings: Rustic.
      7. Night Light: Blue.
      8. Night Light: Orange.
      9. Night Light: Purple.
      10. Night Light: White.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required.

* 1. ELECTRIC INDOOR FIREPLACES - ELEMENT SERIES
     1. Certified to CSA C22.2 No. 46 and UL 2021.
        1. Model: Element. No: NEFB36H-BS. Electric. BTU: 10,000.
           1. Dimensions (WxHxD): 36.13 x 31.88 x 11.25 inches (918 x 810 x 286 mm)
           2. Viewing Area (WxH): 33.5 x 25.5 inches (851 x 648 mm)
     2. Features:
        1. Vivid flame effect with brightness adjustment.
        2. Self-trimming.
        3. Top light LEDs in 7 color settings.
        4. All season usage: flames operate with or without heat.
        5. Ember bed light.
        6. Decorative brick side panels.
        7. Disable heat function as child safety feature.
        8. Thermostatic control.
        9. Remote Control: Multi-function.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Plug in 120 / 240 VAC.
      2. Hardwire 120 / 240 VAC.
      3. Room Settings: Transitional.
      4. Room Settings: Contemporary.
      5. Room Settings: Traditional.
      6. Room Settings: Rustic.
      7. Accent Lights: Multicolor.
      8. Accent Lights: Blue.
      9. Accent Lights: Orange.
      10. Accent Lights: Red.
      11. Accent Lights: Yellow.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model not required.

* 1. ELECTRIC INDOOR FIREPLACES - CINEVIEW SERIES
     1. Certified to CSA C22.2 No. 46 and UL 2021.
        1. Model: Cineview. No: NEFB26H. Electric. BTU: 5,000.
           1. Dimensions (WxHxD): 26 x 20.25 x 7.75 inches ( mm)
           2. Viewing Area (WxH): 24 x 15.25 inches ( mm)
        2. Model: Cineview. No: NEFB30H. Electric. BTU: 5,000.
           1. Dimensions (WxHxD): 30 x 20.25 x 7.75 inches ( mm)
           2. Viewing Area (WxH): 28 x 15.25 inches ( mm)
     2. Features:
        1. Remote control.
        2. Control panel.
        3. Front vents allow unit to be fully recessed.
        4. Media: Burnt Oak Logs and Crystal media.
        5. Brick side panel detail.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Plug in 120 / 240 VAC.
      2. Hardwire 120 / 240 VAC.
      3. Ember Bed Color: Black.
      4. Ember Bed Color: Blue.
      5. Ember Bed Color: Green.
      6. Ember Bed Color: Purple/Pink.
      7. Ember Bed Color: Red.
      8. Ember Bed Color: Teal.
      9. Ember Bed Color: Topaz.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete models not required.

* 1. WOOD BURNING INDOOR FIREPLACES - HIGH COUNTRY SERIES
     1. General: Comply with applicable building codes.
        1. Tested and listed by Intertek Testing Services Ltd. as per North American standards: ULC S610, UL 127 for factory built fireplaces.
     2. Model: High Country NZ3000H. Includes a catalytic converter. EPA 2020 Certified.
        1. Standards Compliance:
           1. EPA 2020 Certified.
           2. Factory Built Appliances: ULC S629, ULC S610 and UL103 HT.
           3. Steel Liner Assemblies for Solid Fuel Burning Appliances: ULC S640, ULC S639 and UL 1777.
        2. Type: Wood Burning. BTU: 60,000.
        3. Dimensions (WxHxD): 42 x 48 x 29.25 inches (1067 x 1219 x 743 mm).
           1. Viewable Area (WxH): 12.5 x 17 inches (317 x 432 mm).
        4. Flue Diameter: 7 inches (178 mm).
        5. Combustion Air: Indoor or outdoor.
        6. Features:
           1. Catalytic converter.
           2. Digital catalyst temperature monitor.
           3. Advanced air wash system.
           4. Cast iron bypass door and baffle.
           5. Andirons: Painted black.

\*\* NOTE TO SPECIFIER \*\* Delete the following items not required.

* + - * 1. Room Settings: Transitional.
        2. Room Settings: Contemporary.
        3. Room Settings: Traditional.
        4. Room Settings: Rustic.
        5. Surrounds: Black.
        6. Surrounds: Wrought iron.
        7. Doors: Arched cast iron black double doors.
        8. Doors: Arched wrought iron double doors.
        9. Blower Kit. 318 cfm
    1. Model: High Country NZ5000 T.
       1. Standards Compliance:
       2. Type: Wood Burning.
       3. Dimensions (WxHxD): 41.94 x 73.38 x 29.75 inches (1065 x 1864 x 756 mm).
          1. Viewable Area (WxH): 36.67 x 26.67 inches (931 x 677 mm).
       4. Flue Diameter: 8 inches (203 mm).
       5. Features:
          1. Andirons: Painted black.
          2. Door: Zero gravity glass doors. Swing open.
          3. Safety Barrier: Cast iron grate.
          4. Chimney: 10 inch (254 mm) diameter.
          5. Combustion Air: Outdoor.

\*\* NOTE TO SPECIFIER \*\* Delete the following items not required.

* + - * 1. Room Settings: Transitional.
        2. Room Settings: Contemporary.
        3. Room Settings: Traditional.
        4. Room Settings: Rustic.
        5. Decorative Panels: Smooth decorative.
        6. Decorative Panels: Traditional decorative.
    1. Model: High Country NZ6000.
       1. Type: Wood Burning. BTU: 60,000.
       2. Dimensions (WxHxD): 44.94 x 50.13 x 27.19 inches (1065 x 1273 x 691 mm).
       3. Flue Diameter: 8 inches (203 mm).
       4. Outside Air for Combustion: Yes.
       5. Standard Features:
          1. Andirons: Cast iron. Painted black finish.
          2. Safety Barrier: Arched screen kit.
          3. Grate: Cast iron.
          4. Napoleon Insignia.
          5. WHISPER QUIET blower system.
          6. Firebrick lined Firebox with a cast Napoleon insignia.
          7. Heavy duty welded 1/4 inch (6 mm) boiler plate construction.
          8. Decorative Panels: Smooth.

\*\* NOTE TO SPECIFIER \*\* Delete the following items not required.

* + - * 1. Room Settings: Transitional.
        2. Room Settings: Contemporary.
        3. Room Settings: Traditional.
        4. Room Settings: Rustic.
        5. Media Kits: Real firewood display.
        6. Media Kits: Country Crane and Hearth Pot.
        7. Surround: Wrought iron.
        8. Surround: Arched black.
        9. Arched Double Doors: Wrought iron finish.
        10. Arched Double Doors: Painted black finish.
        11. Arched Faceplate: Upper Grill and Keystone, wrought iron finish.
        12. Arched Faceplate: Painted black finish.
        13. Arched Upper Grill: Painted black finish.
        14. Keystone: Painted black finish.
        15. Country Crane and Hearth Pot.
        16. Air circulating blower system with decorative grill and washable filter.
    1. Model: High Country NZ8000.
       1. Type: Wood burning.
       2. Dimensions (WxHxD): 59.63 x 80.81 x 30.31 inches (1515 x 2053 x 770 mm).
          1. Viewing Area (WxH): 42 x 28.5 inches (1067 x 724 mm).
       3. Flue Diameter: 10 inches (254 mm).
       4. Flue damper and outside air damper close 100 percent when not in use.
       5. Outside Air for Combustion: Yes.
       6. Standard Features:
          1. Andirons painted black finish.
          2. Refractory brick lined.
          3. Zero gravity glass and screen door.
          4. ZERO GRAVITY door system.

\*\* NOTE TO SPECIFIER \*\* Delete options below not required.

* + - * 1. Room Settings: Transitional.
        2. Room Settings: Contemporary.
        3. Room Settings: Traditional.
        4. Room Settings: Rustic.
        5. Decorative Panels: Herringbone decorative.
        6. Decorative Panels: Smooth decorative.
        7. Decorative Panels: Traditional decorative.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete models not required.

* 1. GAS BURNING STOVES, DIRECT VENT - DISTINCT STOVE SERIES
     1. Comply with applicable building codes, CSA 2.22, and ANSI Z21.50
     2. Distinct Stove Series:
        1. Model Haliburton GDS28-1NE: Pedestal Gas Stove. Fuel Type: Natural gas. BTU: 30,000.
           1. Dimensions (WxHxD): 22.50 x 26.75 x 18.50 inch (572 x 679 x 470 mm)
           2. Viewing Area (WxH): 24.50 x 11.38 inches (622 x 289 mm)

\*\* NOTE TO SPECIFIER \*\* Delete trivets not required.

* + - * 1. Trivets: Black.
        2. Trivets: Stainless steel.
        3. Trivets: Brass.
      1. Model Haliburton GDS28-1NSB: Pedestal Gas Stove. Fuel Type: Natural gas. BTU: 30,000.
         1. Dimensions (WxHxD): 22.50 x 26.75 x 18.50 inch (572 x 679 x 470 mm)
         2. Viewing Area (WxH): 24.50 x 11.38 inches (622 x 289 mm)

\*\* NOTE TO SPECIFIER \*\* Delete trivets not required.

* + - * 1. Trivets: Black.
        2. Trivets: Stainless steel.
        3. Trivets: Brass.
      1. Model Havelock GDS50-1NE: Pedestal Gas Stove. Fuel Type: Natural gas. BTU: 44,000.
         1. Dimensions (WxHxD): 28.25 x 30.75 x 21.63 inch (718 x 781 x 549 mm)
         2. Viewing Area (WxH): 22.50 x 12.63 inches (572 x 321 mm)
         3. Backup control system.
      2. Model Havelock GDS50-1NSB: Pedestal Gas Stove. Fuel Type: Natural gas. BTU: 44,000.
         1. Dimensions (WxHxD): 28.25 x 30.75 x 21.63 inch (718 x 781 x 549 mm)
         2. Viewing Area (WxH): 22.50 x 12.63 inches (572 x 321 mm)
         3. Backup control system.
    1. Features:
       1. Easy access hidden controls.
       2. Media Kit: Hand-painted logs.
       3. Heat radiating ceramic glass.
       4. No electricity required.
       5. Triple flame burner.
       6. Flame/Heat adjustment.
       7. YELLOW DANCING FLAMES.
       8. 100 percent SAFEGUARD gas control system.
       9. Safety screen.
       10. Blower kit.
       11. Mobile home certified.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Color Finish: Metallic black.
      2. Color Finish: Porcelain enamel majolica brown.
      3. Remote control.
      4. Andirons: Painted black.
      5. Doors: Satin chrome plated.
      6. Doors: Metallic black.
      7. Gas conversion kit.
      8. Vent adapter kits.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete models not required.

* 1. GAS BURNING STOVES, DIRECT VENT - CAST IRON STOVE SERIES
     1. Cast Iron Stove Series: Comply with applicable building codes, CSA 2.22, and ANSI Z21.50.
        1. Model Arlington GDS20 Series: Fuel Type: Natural gas. BTU: 20,000.
           1. Dimensions (WxHxD): 19.25 x 25.38 x 18.50 inch (489 x 645 x 470 mm).

Viewing Area (WxH): 14 x 13 inches (356 x 330 mm).

* + - * 1. Color: Metallic black.
        2. Color: Majolica brown.
        3. No electricity required.
        4. Easy access hidden controls.
        5. Reflective Radiant Panels: MIRRO-FLAME porcelain.
      1. Model Bayfield GDS25 Series: Fuel Type: Natural gas. BTU: 24,500.
         1. Dimensions (WxHxD): 23.50 x 25.63 x 17.50 inch (597 x 651 x 445 mm).

Viewing Area (WxH): 18 x 15 inches (457 x 381 mm).

* + - * 1. Ignition: Electronic.
        2. Color: Metallic black.
        3. Color: Majolica Brown.
        4. Color: Winter frost.
        5. Battery backup control system.
        6. Glowing NIGHT LIGHT.
        7. Reflective Radiant Panels: MIRRO-FLAME porcelain.
        8. Remote control.
      1. Model Castlemore GDS26 Series: Fuel Type: Natural gas. BTU: 25,000.
         1. Dimensions (WxHxD): 23.56 x 35.50 x 19.19 inch (598 x 902 x 487 mm).

Viewing Area (WxH): 16.63 x 24 inches (422 x 610 mm).

* + - * 1. Ignition: Electronic.
        2. Color: Metallic black.
        3. Color: Majolica Brown.
        4. Color: Summer Moss.
        5. Battery backup control system.
        6. Glowing NIGHT LIGHT.
        7. Reflective Radiant Panels: MIRRO-FLAME porcelain.
        8. Reflective Radiant Panels: Sandstone brick.
        9. Remote control.
        10. Top or rear vent configuration.
      1. Model Knightsbridge GDS60-1NNSB: Fuel Type: Natural gas. BTU: 35,000.
         1. Dimensions (WxHxD): 27 x 37 x 19.50 inch (686 x 940 x 495 mm).

Viewing Area (WxH): 21 x 18.75 inches (533 x 476 mm).

* + - * 1. Color: Majolica brown.
        2. Battery backup control system.
        3. Andirons.
        4. Anti-condensation switch.
        5. YELLOW DANCING FLAMES.
    1. Features:
       1. Media Kit: Hand-painted logs.
       2. Log Set: Realistic, Ceramic Fiber, Light-Weight Molded PHAZER Logs
       3. Heat radiating ceramic glass.
       4. PHAZERMATIC burner system.
       5. Flame/Heat adjustment.
       6. Safety Screen Included.
       7. 100 percent SAFEGUARD gas control system.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Remote control.
      2. Blower kit.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model not required.

* 1. WOOD BURNING STOVES, DIRECT VENT - CAST IRON STOVE SERIES
     1. S Series: Tested and certified to EPA 2020 cord wood requirements
        1. Model S20: Pedestal Wood Stove. Contemporary medium sized wood stove completed with cast door, cast ash lip, and cast pedestal base.
           1. Fuel Type: Wood. BTU: 54.127.
           2. Dimensions (WxHxD): 26 x 34.25 x 20.5 inches (660 x 870 x 521 mm).

Viewing Area (WxH): 15.63 x 9.75 inches (397 x 248 mm).

Firebox: 1.9 cu ft (0.03 cu m).

* + - * 1. Weighted average emissions rate: 2.25 grams per hour.
        2. Weighted average overall efficiency: 72 percent.
      1. Model S25: Pedestal Wood Stove. Contemporary medium sized wood stove completed with cast door, cast ash lip, and cast pedestal base.
         1. Fuel Type: Wood. BTU: 65,000.
         2. Dimensions (WxHxD): 28.75 x 37.50 x 27 inch (730 x 953 x 686 mm).

Viewing Area (WxH): 18.50 x 11 inches (470 x 279 mm).

Firebox: 2.5 cu ft (0.07 cu m).

* + - * 1. Weighted average emissions rate: 1.3 grams per hour.
        2. Weighted average overall efficiency: 76 percent.
    1. Features
       1. Cast iron door with hidden hinges.
       2. Precision Easy glide drawer with removable ash pan.
       3. Refractory lined firebox.
       4. Heavy duty 5/16 inches (8 mm) firebox top.
       5. Ceramic fiber baffle system.
       6. Top and rear heat shield.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Blower kit.
      2. Ash pan lid.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete series and models not required.

* 1. GAS BURNING FIREPLACE INSERTS, GAS - OAKVILLE SERIES
     1. Fiberglow Series: Gas fireplace inserts.
        1. Model Oakville 3, GDI3N. Fuel Type: Natural Gas. BTU: 24,500.
           1. Dimensions (WxHxD): 28.63 x 20.94 x 18.31 inch (727 x 532 x 465 mm).

Viewing Area (WxH): 22.63 x 15 inches (575 x 381 mm)

* + - * 1. Media Kit: Split Oak Log Set.
      1. Model Oakville 3, GDI3NE. Fuel Type: Natural Gas. BTU: 24,500.
         1. Dimensions (WxHxD): 28.50 x 21 x 18.50 inch (724 x 533 x 470 mm).

Viewing Area (WxH): 22.63 x 15 inches (575 x 381 mm)

* + - * 1. Directional baffles increase air flow for maximum blower efficiency.
        2. Media Kit: Split Oak Log Set.
      1. Model Oakville X3, GDIX3N. Fuel Type: Natural Gas. BTU: 30,000.
         1. Dimensions (WxHxD): 28.63 x 20.94 x 18.31 inch (727 x 532 x 465 mm).

Viewing Area (WxH): 22.63 x 15 inches (575 x 381 mm)

* + - * 1. Directional baffles increase air flow for maximum blower efficiency.
        2. SIT Proflame II electronic ignition
        3. Exclusive NIGHT LIGHT included
        4. Media Kit: Split Oak Log Set.
      1. Model Oakville 3 Glass, GDIG3N. Fuel Type: Natural Gas. BTU: 30,000.
         1. Dimensions (WxHxD): 28.63 x 20.94 x 18.31 inch (727 x 532 x 465 mm).

Viewing Area (WxH): 22.63 x 15 inches (575 x 381 mm)

* + - * 1. Sparkling topaz crystaline ember bed.
        2. Directional baffles increase air flow for maximum blower efficiency.
        3. SIT Proflame II electronic ignition.
        4. Exclusive NIGHT LIGHT included.
        5. Media Kit: Split Oak Log Set.
        6. eFIRE Controller app.
        7. Remote control.
      1. Model Oakville X4, GDIX3N. Fuel Type: Natural Gas. BTU: 40,000.
         1. Dimensions (WxHxD): 34.13 x 24.56 x 18.75 inch (866 x 624 x 476 mm).

Viewing Area (WxH): 27.75 x 11.69 inches (705 x 297 mm).

* + - * 1. Directional baffles increase air flow for maximum blower efficiency.
        2. SIT Proflame II electronic ignition.
        3. Exclusive NIGHT LIGHT included.
        4. Media Kit: Split Oak Log Set.
        5. Media Kit: Driftwood Log Set.
        6. Media Kit: Birch Log Set.
    1. Features: Fiberglow series.
       1. High Performance "H" Style Burner Provides Complete Firebox Width Flame Display.
       2. Simple and robust millivolt control system.
       3. Safety barrier.
       4. Glass door.
       5. Riser box.
       6. Surround: Cast iron.
       7. Battery backup control system.
       8. Can be hardwired for switch control.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Remote control.
      2. Blower kit.
      3. Room Settings: Transitional.
      4. Room Settings: Contemporary.
      5. Room Settings: Traditional.
      6. Room Settings: Rustic.
      7. Backer Plate: Large 4 sided.
      8. Backer Plate: Large 3 sided.
      9. Backer Plate: Medium 3 sided.
      10. Backer Plate: Small 3 sided.
      11. Decorative Panels: MIRRO-FLAME porcelain reflective.
      12. Decorative Panels: Newport standard.
      13. Decorative Panels: Old town red brick.
      14. Decorative Panels: Westminster standard.
      15. Faceplate: 3-Sided.
      16. Faceplate: 4-Sided.
      17. Faceplate Finish: Small black.
      18. Faceplate Finish: Small charcoal.
      19. Faceplate Finish: Small copper.
      20. Faceplate Finish: Small gun metal.
      21. Faceplate Finish: Large black.
      22. Faceplate Finish: Large charcoal.
      23. Faceplate Finish: Large copper.
      24. Faceplate Finish: Large gun metal.
    1. Inspiration Series: Gas fireplace inserts.
       1. Model Inspiration ZC, GDIZC-NSB. Fuel Type: Natural Gas. BTU: 24,000.
          1. Dimensions (WxHxD): 36 x 24.13 x 15.50 inch ( mm).

Viewing Area (WxH): 18.13 x 15.63 inches ( mm)

* + - * 1. Media Kit: Split Oak Log Set.
      1. Features:
         1. Andirons.
         2. Media Kits: Realistic, ceramic fiber, light-weight molded PHAZER Log Set and charcoal ember bed.
         3. YELLOW DANCING FLAMES.
         4. Blower.
         5. Decorative Panels: MIRRO-FLAME porcelain reflective.
         6. Decorative Panels: Sandstone.
         7. Surrounds: Cast iron black.
         8. Surrounds: Brushed copper.
         9. Surrounds: Brushed stainless.
         10. Surrounds: Black.
         11. Surrounds: 4 sided flashing.
         12. Surrounds: 3 sided flashing.
         13. Decorative Fronts: 3 sided black.
         14. Decorative Fronts: 4 sided black.
         15. Decorative Fronts: Contemporary.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete models not required.

* 1. GAS BURNING LOG SETS
     1. Fiberglow Series: Vented Gas log sets
        1. Model Fiberglow 18, GL18NE. Fuel Type: Natural Gas. BTU: 55,000.
           1. Dimensions (WxHxD): 22 x 18 x 14 inch (559 x 457 x 356 mm).
        2. Model Fiberglow VF18, GVFL18N. Fuel Type: Natural Gas. BTU: 40,000.
           1. Dimensions (WxHxD): 24 x 18 x 13.25 inch (610 x 457 x 337 mm).
        3. Model Fiberglow VF18, GVFL18P. Fuel Type: Propane. BTU: 40,000.
           1. Dimensions (WxHxD): 24 x 18 x 13.25 inch (610 x 457 x 337 mm).
        4. Model Fiberglow 24, GL24NE. Fuel Type: Natural Gas. BTU: 60,000.
           1. Dimensions (WxHxD): 28 x 20 x 14 inch (711 x 508 x 356 mm).
        5. Model Fiberglow VF24, GVFL24N. Fuel Type: Natural Gas. BTU: 40,000.
           1. Dimensions (WxHxD): 28 x 18 x 13.25 inch (711 x 508 x 337 mm).
        6. Model Fiberglow VF24, GVFL24P. Fuel Type: Propane. BTU: 40,000.
           1. Dimensions (WxHxD): 28 x 18 x 13.25 inch (711 x 508 x 337 mm).
        7. Model Fiberglow 30, GL30NE. Fuel Type: Natural Gas. BTU: 65,000.
           1. Dimensions (WxHxD): 34 x 22 x 14 inch (864 x 559 x 337 mm).
        8. Model Fiberglow VF30, GVFL30N. Fuel Type: Natural Gas. BTU: 40,000.
           1. Dimensions (WxHxD): 34 x 18 x 13.25 inch (864 x 508 x 337 mm).
        9. Model Fiberglow VF30, GVFL30P. Fuel Type: Propane. BTU: 40,000.
           1. Dimensions (WxHxD): 24 x 18 x 13.25 inch (610 x 508 x 337 mm).
     2. Features:
        1. Solid cast iron andirons and grate.
        2. Electronic ignition 100 percent.
        3. Battery Back-up control system.
        4. Flame/Heat adjustment.
        5. Media Kit: Logs.
        6. Media Kit: Lava rocks.
        7. Andirons.

\*\* NOTE TO SPECIFIER \*\* Delete remote control if not required.

* + - 1. Remote control.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required.

* 1. WOOD BURNING FIREPLACE INSERTS - S SERIESI
     1. S Series: Wood burning fireplace inserts. Contemporary wood stove complete with contemporary cast door and cast pedestal base.
        1. Standards Compliance: ULC S628, UL 1482, ASTM E3053, ASTM E2515
        2. EPA Tested to 2020 cord wood requirement
        3. Model S20i. Fuel Type: Wood. BTU: 54,127.
           1. Dimensions (WxHxD): 41 x 30 x 26.50 inch (1041 x 762 x 673 mm).

Viewing Area (WxH): 15.5 x 9.75 inches (394 x 248 mm)

Firebox Capacity: 1.9 cu ft (0.05 cu m)

* + - * 1. Minimum Fireplace Opening: 25.88 x 22 x 14 inches (657 x 558 x 356 mm)
      1. Weighted average emissions rate: 2.25 grams per hour.
      2. Weighted average overall efficiency: 72 percent
      3. Features:
         1. Refractory lined firebox.
         2. Dual Blower system.
         3. Backer plate. Metallic charcoal.
         4. Door: Cast iron.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete models not required.

* 1. ELECTRIC LOG SETS
     1. Woodland Series:
        1. Model Woodland 18, NEFI18H. Plug and play electric fireplace that fills an old, pre-existing masonry fireplace opening.
           1. Dimensions (WxHxD): 18 x 13.50 x 13 inch (457 x 343 x 330 mm).
        2. Model Woodland 18, NEFI24H. Plug and play electric fireplace that fills an old, pre-existing masonry fireplace opening.
           1. Dimensions (WxHxD): 24 x 15.50 x 14 inch (610 x 394 x 356 mm).
        3. Model Woodland 18, NEFI27H. Plug and play electric fireplace that fills an old, pre-existing masonry fireplace opening.
           1. Dimensions (WxHxD): 27 x 15.50 x 14 inch (686 x 394 x 356 mm).
     2. Features
        1. Fuel Type: Electric. BTU: 5,000.
        2. Five piece hand painted resin log set.
        3. Customizable glow. Realistic flames.
        4. High intensity LED lights.
        5. Safe to touch - never hot enough to burn.
        6. Eco-friendly.
        7. Remote control.

\*\* NOTE TO SPECIFIER \*\* Delete power option not required.

* + - 1. Power: Plugged in 120 VAC.
      2. Power: Hardwired 120 VAC.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model if not required.

* 1. GAS BURNING OUTDOOR FIREPLACES - GALAXY SERIES
     1. Galaxy Series: Outdoor fireplaces.
        1. Model Galaxy, GSS48. Stainless Steel Outdoor Fireplace. Fuel Type: Natural Gas. BTU: 55,000.
           1. Dimensions (WxHxD): 50.50 x 24.50 x 19.50 inch (1283 x 622 x 495 mm).

Viewing Area (WxH): 46.75 x 16.50 inches (1187 x 419 mm)

* + - 1. Model Galaxy, GSS48SDT. Stainless Steel Outdoor See Through Fireplace. Fuel Type: Natural Gas. BTU: 55,000.
         1. Dimensions (WxHxD): 50.50 x 24.50 x 19.50 inch (1283 x 622 x 495 mm).

Viewing Area (WxH): 46.75 x 16.50 inches (1187 x 419 mm)

* + 1. Features:
       1. Surround: Stainless steel.
       2. Cover: Stainless steel.
       3. Ember bed
       4. LED light strip
       5. Burner: Stainless steel.
       6. Wind deflector.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Room Settings: Transitional.
      2. Room Settings: Contemporary.
      3. Room Settings: Traditional.
      4. Room Settings: Rustic.
      5. Media Kits: Driftwood Logs.
      6. Media Kits: Rocks.
      7. Glass Media Kits: Topaz Embers.
      8. Glass Media Kits: Red Embers.
      9. Glass Media Kits: Clear Embers.
      10. Glass Media Kits: Blue Embers.
      11. Glass Media Kits: Black Embers.
      12. Glass Media Kits: Amber Embers.
      13. Glass Media Kits: Topaz Beads.
      14. Glass Media Kits: Red Beads.
      15. Glass Media Kits: Clear Beads.
      16. Glass Media Kits: Blue Beads.
      17. Glass Media Kits: Black Beads.
      18. Glass Media Kits: Amber Beads.
      19. LED Lighting: Blue.
      20. LED Lighting: Red.
      21. LED Lighting: Green.
      22. LED Lighting: Yellow.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete model not required.

* 1. GAS BURNING OUTDOOR FIREPLACES - RIVERSIDE SERIES
     1. Riverside Series: Outdoor fireplaces. Certified to ANSI Z21.97 and CSA 2.41
        1. Model Riverside 36 Clean Face, GSS36CFN. Stainless Steel Outdoor Fireplace. Fuel Type: Natural Gas. BTU: 40,000.
           1. Dimensions (WxHxD): 42 x 35.50 x 20.25 inch (1067 x 902 x 514 mm).

Viewing Area (WxH): 16.38 x 20.18 inches (416 x 513 mm).

* + - * 1. Decorative Panels: Old Town Herringbone.
        2. Decorative Panels: Westminster/
        3. Media Kits: Birch Log Set.
        4. Media Kits: Oak Log Set.
      1. Model Riverside 42 Clean Face, GSS42CFN. Stainless Steel Outdoor Fireplace. Fuel Type: Natural Gas. BTU: 65,000.
         1. Dimensions (WxHxD): 46.5 x 35.50 x 21.25 inch (181 x 902 x 540 mm).

Viewing Area (WxH): 16.38 x 20.18 inches (416 x 513 mm)

* + - * 1. Decorative Panels: Sandstone.
        2. Media Kits: PHAZER Log Set.
        3. Cover: Stainless steel.
    1. Features:
       1. Ignition: Push button.
       2. Controls: Flame and heat.
       3. No venting or chimney required.
       4. Safety screen.
       5. Doors: Outdoor cover.
       6. Doors: Traditional glass door.
       7. Tempered glass cover.

\*\* NOTE TO SPECIFIER \*\* Delete the following options not required.

* + - 1. Remote control.
      2. Room Settings: Transitional.
      3. Room Settings: Contemporary.
      4. Room Settings: Traditional.
      5. Room Settings: Rustic.
      6. Gas conversion kit.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required.

* 1. ELECTRIC FIREPLACE MANTEL - DECOR SERIES
     1. Electric Fireplace Mantel Package:
        1. Model: The Taylor. No: NEFP33-0214W. Traditional mantel with white finish, comes with Electric Indoor Fireplace, Ascent 33.
           1. Dimensions (WxHxD): 55 x 45.25 x 18 inches (1397 x 1149 x 457 mm).
           2. Viewing Area (WxH): 31 x 23 inches (787 x 584 mm).
        2. Features:
           1. Classic white finish.
           2. Black slate styled surround.
           3. Pedestal base.
           4. Decorative dentil accent molding.

1. EXECUTION
   1. EXAMINATION
      1. Do not begin installation until substrates have been properly prepared.
      2. If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.

\*\* NOTE TO SPECIFIER \*\* Include the following paragraph if powered ventilators are provided. Delete if not required.

* + 1. Verify proper power supply and fuel source are available.
  1. PREPARATION
     1. Clean surfaces thoroughly prior to installation.
     2. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
  2. INSTALLATION
     1. Install in accordance with manufacturer's instructions, ANSI Z21.44 and the requirements of authorities having jurisdiction.
     2. Use manufacturer's guidelines for minimum clearances to combustibles, walls, and finishes.
     3. Set fireplace units plumb, level, and rigid
     4. Anchor all components firmly in position.

\*\* NOTE TO SPECIFIER \*\* Include the following for following two paragraphs for natural gas fireplaces.

* + 1. Connect to natural gas system in accordance with NFPA 54.
    2. Connect to natural gas system in accordance with CSA B149.1.

\*\* NOTE TO SPECIFIER \*\* Include the following for following two paragraphs for propane fireplaces.

* + 1. Connect to propane system in accordance with NFPA 54.
    2. Connect to propane system in accordance with CSA B149.1 and B149.2.

\*\* NOTE TO SPECIFIER \*\* Include one of the following two paragraphs for electric fireplaces and for wood or gas and wood fireplaces equipped with electric controls or blowers.

* + 1. Connect to power supply and control wiring in accordance with NFPA 70.
    2. Connect to power supply and control wiring in accordance with CSA C221.
    3. Upon completion of installation, visually inspect all exposed surfaces. Touch up scratches and abrasions with touch up paint recommended by the manufacturer; make imperfections invisible to the unaided eye from 5 feet (1524 mm).
  1. PROTECTION
     1. Protect installed products until completion of project.
     2. Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION