SECTION 09 30 00

TILE

Display hidden notes to specifier. (Don't know how? [Click Here](http://www.arcat.com/sd/display_hidden_notes.shtml))

*Copyright 2004 - 2019 ARCAT, Inc. - All rights reserved*

\*\* NOTE TO SPECIFIER \*\* Endicott Clay Products Company, clay tile.  
This section is based on the products of Endicott Clay Products Company, which is located at:  
 57120 707th Road  
 Endicott, NE 68350  
 Tel: (402) 729-3315  
 Fax: (402) 729-5804  
 Email: [endicott@endicott.com](mailto:endicott@endicott.com)   
 Website: [www.endicott.com](http://www.endicott.com)   
Endicott Clay Products Company manufactures face brick, pavers, glazed units, pool copings, thin brick, and sculptured brick murals. This section covers their thin brick products. Note that code requirements vary between municipalities; check local code authorities for applicability of thin brick systems.

1. GENERAL
   1. SECTION INCLUDES
      1. Clay tile.
      2. Transition tile.
      3. Tile step treads.
   2. RELATED SECTIONS
      1. Section 04 27 23 - Cavity Wall Unit Masonry.
      2. Section 05 40 00 - Cold-Formed Metal Framing.
      3. Section 06 10 00 - Rough Carpentry.
      4. Section 09 21 16.33 - Gypsum Board Area Separation Wall Assemblies.
      5. Section 09 30 50 - Tile Setting Materials and Accessories\*.
   3. REFERENCES
      1. ANSI A137.1 - American National Standard for Ceramic Tile.
   4. SUBMITTALS
      1. Submit under provisions of Section 01 30 00 - Administrative Requirements.
      2. [ Product Data ]: Manufacturer's catalog data, detail sheets, and specifications.
      3. Selection Samples: For each product requiring color/texture selection, provide full size samples for final selection.
      4. Verification Samples: For each product, color, and texture selected, provide two full-size units representing actual color and texture of products to be installed.
   5. SAMPLE PANELS
      1. Construct sample panel at location indicated or directed, and as follows:
         1. Size: 4 feet by 4 feet (1.2 m by 1.2 m).
         2. Include all unit types and sizes to be used, and mortar joint treatment.
      2. Obtain architect's acceptance of sample panel before beginning construction activities of this section.
      3. Do not remove sample panel until construction activities of this section have been accepted by architect.
   6. DELIVERY, STORAGE, AND HANDLING
      1. Deliver products of this section on pallets, with individual faces protected; keep dry.
      2. Store tile in protected area or under cover on level ground; keep dry. Do not double-stack pallets.
2. PRODUCTS
   1. MANUFACTURERS
      1. Acceptable Manufacturer: Endicott Clay Products Co., which is located at: 57120 707th Rd.; Endicott, NE 68350; Tel: 402-729-3315; Fax: 402-729-5804; Email: [request info (endicott@endicott.com)](http://admin.arcat.com/users.pl?action=UserEmail&company=Endicott+Clay+Products+Co&coid=32282&rep=&fax=402-729-5804&message=RE:%20Spec%20Question%20(09300end):%20%20&mf=); Web: <http://www.endicott.com>
      2. Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
      3. Substitutions: Not permitted.
   2. TILE
      1. Clay Tile: ANSI 137.1.
         1. Size: 2-1/4 inches (57.2 mm) by 7-5/8 inches (193.7 mm), 1/2 inch (12.7 mm) thick.
         2. Size: 3-5/8 inches (92.1 mm) by 3-5/8 inches (92.1 mm), 1/2 inch (12.7 mm) thick.
         3. Size: 3-5/8 inches (92.1 mm) by 7-5/8 inches (193.7 mm), 1/2 inch (12.7 mm) thick.
         4. Size: 3-5/8 inches (92.1 mm) by 11-5/8 inches (295.3 mm), 1/2 inch (12.7 mm) thick.
         5. Size: 7-5/8 inches (193.7 mm) by 7-5/8 inches (193.7 mm), 1/2 inch (12.7 mm) thick.
         6. Texture: Smooth.
         7. Texture: Wirecut.
         8. Texture: Velour.
         9. Color: As selected by Architect from manufacturer's full range.
      2. Transition Tiles: TT 488, 3-5/8 inches (92.1 mm) by 7-5/8 inches (193.7 mm), tapering from 1/2 inch (12.7 mm) thickness to 1/4 inch (6.3 mm) thick rounded edge along the long edge.
         1. Color: As selected by Architect from manufacturer's full range.
      3. Tile Step Treads:TST488, Bullnosed front edge, grooved top surface to increase slip resistance; 3-5/8 inches (92.1 mm) by 7-5/8 inches (193.7 mm), 1/2 inch (12.7 mm) thick.
         1. Color: As selected by Architect from manufacturer's full range.
3. EXECUTION
   1. INSTALLATION
      1. Install units in accordance with manufacturer's instructions, approved submittals and in proper relationship with adjacent construction.

END OF SECTION