SECTION 10 50 00

STORAGE SPECIALTIES - WEAPONS, COMPUTERS, SECURE MEDIA, SECURITY GEAR

Display hidden notes to specifier. (Don't know how? [Click Here](https://www.arcat.com/sd/display_hidden_notes.shtml))

*Copyright 2021 - 2021 ARCAT, Inc. - All rights reserved*

\*\* NOTE TO SPECIFIER \*\* DASCO Storage Solutions; secure storage lockers.  
This section is based on the products of DASCO Storage Solutions, which is located at:  
346 Orenda Rd.  
Brampton, ON, Canada L6T 1G1  
Toll Free Tel: 800-387-2468  
Tel: 905-792-7080  
Fax: 905-792-9166  
Email: [request info (info@dascostorage.com)](https://admin.arcat.com/users.pl?action=UserEmail&company=DASCO+Storage+Solutions&coid=50089&rep=&fax=905-792-9166&message=RE:%20Spec%20Question%20(10500dss):%20%20&mf=)  
Web: <http://www.dascostorage.com>   
 [ [Click Here](https://www.arcat.com/arcatcos/cos50/arc50089.html) ] for additional information.  
At Dasco Storage Solutions, we pride ourselves on delivering the best products, along with top notch customer service. Our products are installed around the world - from the Arctic to New Zealand and many places in between.  
We are always developing new solutions to meet changing secure-storage needs. Find out why our customers love the Dasco Experience.

1. GENERAL
   1. SECTION INCLUDES
      1. Weapon storage.
      2. Computer storage.
      3. Secure media storage.
      4. Gear Storage.
      5. E-Lockers.
      6. Miscellaneous storage equipment.
   2. RELATED SECTIONS

\*\* NOTE TO SPECIFIER \*\* Delete any sections below not relevant to this project; add others as required.

* + 1. Section 05 50 00 - Metal Fabrications.
    2. Section 06 10 00 - Rough Carpentry.
  1. SUBMITTALS
     1. Submit under provisions of Section 01 30 00 - Administrative Requirements.
     2. Product Data:
        1. Manufacturer's data sheets on each product to be used.
        2. Preparation instructions and recommendations.
        3. Storage and handling requirements and recommendations.
        4. Typical installation methods.

\*\* NOTE TO SPECIFIER \*\* Delete if not applicable to product type.

* + 1. Verification Samples: Two representative units of each type, size, pattern, and color.
    2. Shop Drawings: Include details of materials, construction, and finish. Include relationship with adjacent construction.
  1. QUALITY ASSURANCE
     1. Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience.
     2. Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
     3. Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.

\*\* NOTE TO SPECIFIER \*\* Include mock-up if the project size or quality warrant the expense. The following is one example of how a mock-up on might be specified. When deciding on the extent of the mock-up, consider all the major different types of work on the project.

* + 1. Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
       1. Intent of mock-up is to demonstrate quality of workmanship and visual appearance.
       2. If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
       3. Retain mock-up during construction as a standard for comparison with completed work.
       4. Do not alter or remove mock-up until work is completed or removal is authorized.
  1. PRE-INSTALLATION CONFERENCE
     1. Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
  2. DELIVERY, STORAGE, AND HANDLING
     1. Store and handle in strict compliance with manufacturer's written instructions and recommendations.
     2. Protect from damage due to weather, excessive temperature, and construction operations.
  3. PROJECT CONDITIONS
     1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
  4. WARRANTY
     1. Manufacturer's standard limited warranty unless indicated otherwise.

1. PRODUCTS
   1. MANUFACTURERS
      1. Acceptable Manufacturer: DASCO Storage Solutions, which is located at: 346 Orenda Rd.; Brampton, ON, Canada L6T 1G1; Toll Free Tel: 800-387-2468; Tel: 905-792-7080; Fax: 905-792-9166; Email: [request info (info@dascostorage.com)](https://admin.arcat.com/users.pl?action=UserEmail&company=DASCO+Storage+Solutions&coid=50089&rep=&fax=905-792-9166&message=RE:%20Spec%20Question%20(10500dss):%20%20&mf=); Web: <http://www.dascostorage.com>

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs: coordinate with requirements of Division 1 section on product options and substitutions.

* + 1. Substitutions: Not permitted.
    2. Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete weapon storage unit paragraphs not required.

* 1. WEAPON STORAGE
     1. Expandable Weapon Rack: Can be extended and re-configured to suit a growing armory. Outfit with solid steel components that slide into a universal back panel.
        1. Universal Back Panel: Tailor system using solid-steel adjustable components.

\*\* NOTE TO SPECIFIER \*\* Delete configuration option not required.

* + - 1. Configuration: Single Sided.
      2. Configuration: Double Sided.

\*\* NOTE TO SPECIFIER \*\* Delete size options not required. Increase the height using 12 inch and 34 inch post and panel add-ons

* + - 1. Size (HxW): 50 x 34 inch (1270 x 864 mm); 10 long guns wide.
      2. Size (HxW): 50 x 40 inch (1270 x 1016 mm); 12 long guns wide.
      3. Size (HxW): 84 x 34 inch (2134 x 864 mm); 10 long guns wide.
      4. Size (HxW): 84 x 40 inch (2134 x 1016 mm); 12 long guns wide.
      5. Components:

\*\* NOTE TO SPECIFIER \*\* Delete components not required.

* + - * 1. Barrel Saddle: Single-capacity.
        2. Barrel Saddle: Single-capacity seismic.
        3. Barrel Saddle: Double-wide.
        4. Barrel Saddle: Double-wide seismic.
        5. Barrel Saddle: Extended.
        6. Barrel Saddle: Extended seismic.
        7. Barrel Saddle: Padlock.
        8. Barrel Saddle: 2-capacity spare.
        9. Barrel Saddle: Single-capacity spare - reversable.
        10. Bayonet Holder: Single-capacity.
        11. Bayonet Holder: 5-capacity.
        12. Carl Gustav base.
        13. Carl Gustav top.
        14. C-16 grenade launcher base
        15. Drop-Down Bracket: Single-capacity.
        16. Drop-Down Bracket: 10-capacity.
        17. Drop-Down Bracket: 12-capacity.
        18. Drop-Down Bracket: 16-capacity.
        19. Horizontal Mounts: 2-capacity.
        20. Horizontal Mounts: 3-capacity.
        21. Horizontal Mounts: 4-capacity.
        22. M2 Receiver and Barrel Storage: Single-capacity.
        23. MK19 grenade launcher base.
        24. MK19 grenade launcher top.
        25. Magazine Box: 3 inch wide.
        26. Magazine Box: 6 inch wide.
        27. Magnetic inventory tags.
        28. Mortar Storage: 60 mm.
        29. Mortar Storage: 80 mm.
        30. Pistol Pac: Single-capacity.
        31. Pistol Pac: 6-capacity.
        32. Pistol Pac: 8-capacity.
        33. Pistol Pac: 6-capacity lockable.
        34. Pistol Pac: 8-capacity lockable.
        35. Pistol Pac: Single-capacity and mag storage.
        36. Pistol Pac: 6-capacity and mag storage.
        37. Pistol Pac: 8-capacity and mag storage,
        38. Pistol Peg: Single-capacity. Store 9 mm and .22 Cal weapons.
        39. Pistol Peg: 8-capacity. Organize eight 9 mm and .22 Cal weapons
        40. Pistol Peg: 6-capacity. Organize six 9 mm and .22 Cal weapons.
        41. Plain Shelf: 34 inch wide.
        42. Plain Shelf: 40 inch wide.
        43. Radio Cradle: 6-capacity.
        44. Secure eyelet.
        45. Security screwdriver.
        46. Stock Shelf: Single-capacity.
        47. Stock Shelf: 5-capacity.
        48. Stock Shelf: 6-capacity.
        49. Stock Shelf: 10-capacity.
        50. Stock Shelf: 12-capacity.
        51. Storage Box: 3 inch wide.
        52. Storage Box: 6 inch wide.
        53. Storage Box: 12 inch wide.
        54. Sword Holder.
        55. TASER Device Pac: Single-capacity.
        56. TASER Device Pac: 6-capacity.
        57. TASER Device Pac: 8-capacity.
        58. Velcro Pass Thru Bracket: Single.
        59. Velcro Pass Thru Bracket: Double. Two brackets with a 25 inch Velcro strap.
        60. Vest Holder: 3-capacity.
    1. Weapon Storage Wall: Made with reinforced steel panels. Outfit with over 50 components to build a tailored solution. Mount weapons vertically with a mix of shelves above a workbench for maintenance station or showcase weapons with horizontal long gun mounts.
       1. Universal Back Panel: Tailor system using solid-steel adjustable components.

\*\* NOTE TO SPECIFIER \*\* Delete size option not required.

* + - 1. Size (HxW): 24 x 34 inch (610 x 864 mm); 10 long guns wide.
      2. Size (HxW): 24 x 40 inch (610 x 1016 mm); 12 long guns wide.
      3. Components:

\*\* NOTE TO SPECIFIER \*\* Delete Components not required.

* + - * 1. Barrel Saddle: Single-capacity.
        2. Barrel Saddle: Single-capacity seismic.
        3. Barrel Saddle: Double-wide.
        4. Barrel Saddle: Double-wide seismic.
        5. Barrel Saddle: Extended.
        6. Barrel Saddle: Extended seismic.
        7. Barrel Saddle: Padlock.
        8. Barrel Saddle: 2-capacity spare.
        9. Barrel Saddle: Single-capacity spare - reversable.
        10. Bayonet Holder: Single-capacity.
        11. Bayonet Holder: 5-capacity.
        12. Drop-Down Bracket: Single-capacity.
        13. Drop-Down Bracket: 10-capacity.
        14. Drop-Down Bracket: 12-capacity.
        15. Drop-Down Bracket: 16-capacity.
        16. Horizontal Mounts: 2-capacity.
        17. Horizontal Mounts: 3-capacity.
        18. Horizontal Mounts: 4-capacity.
        19. Magazine Box: 3 inch wide.
        20. Magazine Box: 6 inch wide.
        21. Magnetic inventory tags.
        22. Pistol Pac: Single-capacity.
        23. Pistol Pac: 6-capacity.
        24. Pistol Pac: 8-capacity.
        25. Pistol Pac: Single-capacity and mag storage.
        26. Pistol Pac: 6-capacity and mag storage.
        27. Pistol Pac: 8-capacity and Mag storage,
        28. Pistol Pac: 6-capacity lockable.
        29. Pistol Pac: 8-capacity lockable.
        30. Pistol Peg: Single-capacity. Store 9 mm and .22 Cal weapons.
        31. Pistol Peg: 6-capacity. Organize six 9 mm and .22 Cal weapons.
        32. Pistol Peg: 8-capacity. Organize eight 9 mm and .22 Cal weapons
        33. Plain Shelf: 34 inch wide.
        34. Plain Shelf: 40 inch wide.
        35. Radio Cradle: 6-capacity.
        36. Secure eyelet.
        37. Security screwdriver.
        38. Stock Saddle: Single-capacity.
        39. Stock Shelf: Single-capacity.
        40. Stock Shelf: 5-capacity.
        41. Stock Shelf: 6-capacity.
        42. Stock Shelf: 10-capacity.
        43. Stock Shelf: 12-capacity.
        44. Storage Box: 3 inch wide.
        45. Storage Box: 6 inch wide.
        46. Storage Box: 12 inch wide.
        47. Sword holder.
        48. TASER Device Pac: Single-capacity.
        49. TASER Device Pac: 6-capacity.
        50. TASER Device Pac: 8-capacity.
        51. Velcro Pass Thru Bracket: Single.
        52. Velcro Pass Thru Bracket: Double. Two brackets with a 25 inch Velcro strap.
        53. Vest Holder: 3-capacity.
    1. Bi-Fold Weapon Racks: Perforated steel bi-folding gates. Low-tolerance doors and multi-point lock system. Can be bolted to floor, side-to-side, back-to-back, or to a wall and can stack on top of each other.
       1. Universal Back Panel: Tailor system using solid-steel adjustable components.

\*\* NOTE TO SPECIFIER \*\* Delete height and width options not required.

* + - 1. Height: 48 inch (1219 mm).
      2. Height: 64.5 inch (1638 mm).
      3. Height: 72 inch (1829 mm).
      4. Height: 84 inch (2134 mm).
      5. Width: 36 inches (914 mm); 10 long guns wide.
      6. Width: 42 inches (12 long guns wide).
      7. Depth: 15 inches (381 mm).
      8. Size: 84 inches (2134 mm).
      9. Finish: Powder coat.
      10. Components:

\*\* NOTE TO SPECIFIER \*\* Delete components not required.

* + - * 1. Barrel Saddle: Single-capacity.
        2. Barrel Saddle: Single-capacity seismic.
        3. Barrel Saddle: Double-wide.
        4. Barrel Saddle: Double-wide seismic.
        5. Barrel Saddle: Extended.
        6. Barrel Saddle: Extended seismic.
        7. Barrel Saddle: Padlock.
        8. Barrel Saddle: 2-capacity spare.
        9. Barrel Saddle: Single-capacity spare - reversable.
        10. Bayonet Holder: Single-capacity.
        11. Bayonet Holder: 5-capacity.
        12. Bi-fold weapon rack.
        13. Bi-Fold Weapon Rack: Bolt drawer weapon storage component.
        14. BWR: Ammo/storage shelf.
        15. BWR: Bolt drawer.
        16. BWR: Drawer with locking lid.
        17. BWR: Roll-out drawer.
        18. Carl Gustav base.
        19. Carl Gustav top.
        20. C-16 grenade launcher base
        21. Drop-Down Bracket: Single-capacity.
        22. Drop-Down Bracket: 10-capacity.
        23. Drop-Down Bracket: 12-capacity.
        24. Drop-Down Bracket: 16-capacity.
        25. Horizontal Mounts: 2-capacity.
        26. Horizontal Mounts: 3-capacity.
        27. Horizontal Mounts: 4-capacity.
        28. M2 Receiver and Barrel Storage: Single-capacity.
        29. MK19 grenade launcher base.
        30. MK19 grenade launcher top.
        31. Magazine Box: 3 inch wide.
        32. Magazine Box: 6 inch wide.
        33. Magnetic inventory tags.
        34. Mortar Storage: 60 mm.
        35. Mortar Storage: 80 mm.
        36. Stock Shelf: Single-capacity.
        37. Stock Shelf: 5-capacity.
        38. Stock Shelf: 6-capacity.
        39. Stock Shelf: 10-capacity.
        40. Stock Shelf: 12-capacity.
        41. Stock Saddle: Single-capacity
        42. Storage Box: 3 inch wide.
        43. Storage Box: 6 inch wide.
        44. Storage Box: 12 inch wide.
        45. Sword holder.
        46. Pistol Pac: Single-capacity.
        47. Pistol Pac: 6-capacity.
        48. Pistol Pac: 8-capacity.
        49. Pistol Pac: 6-capacity lockable.
        50. Pistol Pac: 8-capacity lockable.
        51. Pistol Pac: Single-capacity and mag storage.
        52. Pistol Pac: 6-capacity and mag storage.
        53. Pistol Pac: 8-capacity and mag storage,
        54. Pistol Peg: 8-capacity. Organize eight 9 mm and .22 Cal weapons
        55. Pistol Peg: 6-capacity. Organize six 9 mm and .22 Cal weapons.
        56. Radio Cradle: 6-capacity.
        57. Secure 3-compartment handgun insert w/Abloy locks.
        58. Secure eyelet.
        59. Security screwdriver
        60. Velcro Pass Thru Bracket: Single.
        61. Velcro Pass Thru Bracket: Double. Two brackets with a 25 inch Velcro strap.
        62. Vest Holder: 3-capacity.
        63. TASER Device Pac: Single-capacity.
        64. TASER Device Pac: 6-capacity.
        65. TASER Device Pac: 8-capacity.
        66. Locks:

Abloy Lock and 2 keys.

Abloy Key only (single).

Abloy Master key.

Abloy Padlock.

Abloy Padlock and 2 keys.

Combi-Lock 3-digit.

Combi-Lock 4-digit.

Comp-X digital lock

Comp-X digital lock with Audit Trail

Real Lock-Combo 3-Digit.

Wesko Lock and 2 Keys.

Wesko Keys only (2/set).

Wesko Master Key.

* + 1. Stackable Weapon Locker Storing guns and accessories for teams. Can be bolted in banks - side-to-side, back-to-back, on top of each other - and can be secured to the floor and wall.
       1. Dimensions (HxWxD): 48 x 14 x 15 inch (1219 x 356 x 381 mm); 3 long guns wide.
       2. Universal Back Panel: Tailor system using solid-steel adjustable components.
       3. Components:

\*\* NOTE TO SPECIFIER \*\* Delete components not required.

* + - * 1. Barrel Saddle: Single-capacity.
        2. Barrel Saddle: Single-capacity seismic.
        3. Barrel Saddle: Double-wide.
        4. Barrel Saddle: Double-wide seismic.
        5. Barrel Saddle: Extended.
        6. Barrel Saddle: Extended seismic.
        7. Barrel Saddle: Padlock.
        8. Barrel Saddle: 2-capacity spare.
        9. Barrel Saddle: Single-capacity spare - reversable.
        10. Bayonet Holder: Single-capacity.
        11. Bayonet Holder: 5-capacity.
        12. Carl Gustav base.
        13. C-16 grenade launcher base
        14. Drop-Down Bracket: Single-capacity.
        15. M2 Receiver and Barrel Storage: Single-capacity.
        16. MK19 grenade launcher base.
        17. MK19 grenade launcher top.
        18. Magazine Box: 3 inch wide.
        19. Magazine Box: 6 inch wide.
        20. Magnetic inventory tags.
        21. Mortar Storage: 60 mm.
        22. Mortar Storage: 80 mm.
        23. Pistol Pac: Single-capacity.
        24. Pistol Pac: Single-capacity and mag storage.
        25. Pistol Peg: Single-capacity. Store 9 mm and .22 Cal weapons.
        26. Radio Cradle: 6-capacity.
        27. Secure eyelet.
        28. Security screwdriver.
        29. Stock Saddle: Single capacity.
        30. Stock Shelf: Single-capacity.
        31. Storage Box: 3 inch wide.
        32. Storage Box: 6 inch wide.
        33. Storage Box: 12 inch wide.
        34. Sword Holder.
        35. TASER Device Pac: Single-capacity.
        36. Velcro Pass Thru Bracket: Single.
        37. Velcro Pass Thru Bracket: Double. Two brackets with a 25 inch Velcro strap.
    1. Medium Stackable Weapon Rack: Stores weapons, ammo, and accessories. Can be bolted in banks - side-to-side, back-to-back, on top of each other - and can be secured to the floor and wall.
       1. Dimensions (HxWxD): 48 x 42 x 15 inch (1219 x 1067 x 381 mm); 12 long guns wide.
       2. Doors: Perforated with multi-point lock mechanism. Doors handle additional locking mechanisms for maximum security.
       3. Universal back panel: Tailor system using solid-steel adjustable components.
       4. Components:

\*\* NOTE TO SPECIFIER \*\* Delete components not required.

* + - * 1. Barrel Saddle: Single-capacity.
        2. Barrel Saddle: Single-capacity seismic.
        3. Barrel Saddle: Double-wide.
        4. Barrel Saddle: Double-wide seismic.
        5. Barrel Saddle: Extended.
        6. Barrel Saddle: Extended seismic.
        7. Barrel Saddle: Padlock.
        8. Barrel Saddle: 2-capacity spare.
        9. Barrel Saddle: Single-capacity spare - reversable.
        10. Bayonet Holder: Single-capacity.
        11. Bayonet Holder: 5-capacity.
        12. Carl Gustav base.
        13. Carl Gustav top.
        14. C-16 grenade launcher base
        15. Drop-Down Bracket: Single-capacity.
        16. Drop-Down Bracket: 10-capacity.
        17. Drop-Down Bracket: 12-capacity.
        18. Drop-Down Bracket: 16-capacity.
        19. Horizontal Mounts: 2-capacity.
        20. Horizontal Mounts: 3-capacity.
        21. Horizontal Mounts: 4-capacity.
        22. M2 Receiver and Barrel Storage: Single-capacity.
        23. MK19 grenade launcher base.
        24. MK19 grenade launcher top.
        25. Magazine Box: 3 inch wide.
        26. Magazine Box: 6 inch wide.
        27. Magnetic inventory tags.
        28. Mortar Storage: 60 mm.
        29. Mortar Storage: 80 mm.
        30. Pistol Pac: Single-capacity.
        31. Pistol Pac: 6-capacity.
        32. Pistol Pac: 8-capacity.
        33. Pistol Pac: 6-capacity lockable.
        34. Pistol Pac: 8-capacity lockable.
        35. Pistol Pac: Single-capacity and mag storage.
        36. Pistol Pac: 6-capacity and mag storage.
        37. Pistol Pac: 8-capacity and mag storage,
        38. Pistol Peg: 8-capacity. Organize eight 9 mm and .22 Cal weapons
        39. Pistol Peg: 6-capacity. Organize six 9 mm and .22 Cal weapons.
        40. Plain Shelf: 34 inch wide.
        41. Plain Shelf: 40 inch wide.
        42. Radio Cradle: 6-capacity.
        43. Secure 3-compartment handgun insert w/Abloy locks
        44. Secure eyelet.
        45. Security screwdriver.
        46. Stock Saddle: Single-capacity.
        47. Stock Shelf: Single-capacity.
        48. Stock Shelf: 5-capacity.
        49. Stock Shelf: 6-capacity.
        50. Stock Shelf: 10-capacity.
        51. Stock Shelf: 12-capacity.
        52. Storage Box: 3 inch wide.
        53. Storage Box: 6 inch wide.
        54. Storage Box: 12 inch wide.
        55. Sword holder.
        56. TASER Device Pac: Single-capacity.
        57. TASER Device Pac: 6-capacity.
        58. TASER Device Pac: 8-capacity.
        59. Velcro Pass Thru Bracket: Single.
        60. Velcro Pass Thru Bracket: Double. Two brackets with a 25 inch Velcro strap.
        61. Vest Holder: 3-capacity.
    1. Large Stackable Weapon Rack: Stores 32 long guns. Bolt racks back-to-back and side-to-side, to the floor, or wall.
       1. Dimensions (HxWxD): 64.5 x 42 x 15 inch (1638 x 1067 x 381 mm); 12 long guns wide.
       2. Construction: Steel. All welded.
       3. Doors: Perforated. One piece full length door hinges.
       4. Built-in side carry handles.
       5. Interior security eyelet for cable locks.
       6. Universal Back Panel: Tailor system using 55 solid-steel adjustable components.
       7. Increase vertical storage space with a 12-capacity drop-down bracket for stock shelves.
       8. Components:

\*\* NOTE TO SPECIFIER \*\* Delete Components not required.

* + - * 1. 3-Compartment Secure Handgun Insert w/Abloy locks
        2. Barrel Saddle: Single-capacity.
        3. Barrel Saddle: Single-capacity seismic.
        4. Barrel Saddle: Double-wide.
        5. Barrel Saddle: Double-wide seismic.
        6. Barrel Saddle: Extended.
        7. Barrel Saddle: Extended seismic.
        8. Barrel Saddle: Padlock.
        9. Barrel Saddle: 2-capacity spare.
        10. Barrel Saddle: Single-capacity spare - reversable.
        11. Bayonet Holder: Single-capacity.
        12. Bayonet Holder: 5-capacity.
        13. Carl Gustav base.
        14. Carl Gustav top.
        15. C-16 grenade launcher base
        16. Drop-Down Bracket: Single-capacity.
        17. Drop-Down Bracket: 10-capacity.
        18. Drop-Down Bracket: 12-capacity.
        19. Drop-Down Bracket: 16-capacity.
        20. Horizontal Mounts: 2-capacity.
        21. Horizontal Mounts: 3-capacity.
        22. Horizontal Mounts: 4-capacity.
        23. M2 Receiver and Barrel Storage: Single-capacity.
        24. MK19 grenade launcher base.
        25. MK19 grenade launcher top.
        26. Mortar Storage: 60 mm.
        27. Mortar Storage: 80 mm.
        28. Pistol Pac: Single-capacity.
        29. Pistol Pac: 6-capacity.
        30. Pistol Pac: 8-capacity.
        31. Pistol Pac: Single-capacity and mag storage.
        32. Pistol Pac: 6-capacity and mag storage.
        33. Pistol Pac: 8-capacity and mag storage,
        34. Pistol Pac: 6-capacity lockable.
        35. Pistol Pac: 8-capacity lockable.
        36. Pistol Peg: Single-capacity. Store 9 mm and .22 Cal weapons.
        37. Pistol Peg: 6-capacity. Organize six 9 mm and .22 Cal weapons.
        38. Pistol Peg: 8-capacity. Organize eight 9 mm and .22 Cal weapons
        39. Plain Shelf: 34 inch wide.
        40. Plain Shelf: 40 inch wide.
        41. Radio Cradle: 6-capacity.
        42. Secure eyelet.
        43. Security screwdriver.
        44. Stock Saddle: Single-capacity.
        45. Stock Shelf: Single-capacity.
        46. Stock Shelf: 5-capacity.
        47. Stock Shelf: 6-capacity.
        48. Stock Shelf: 10-capacity.
        49. Stock Shelf: 12-capacity.
        50. Storage Box: 3 inch wide.
        51. Storage Box: 6 inch wide.
        52. Storage Box: 12 inch wide.
        53. Sword holder.
        54. TASER Device Pac: Single-capacity.
        55. TASER Device Pac: 6-capacity.
        56. TASER Device Pac: 8-capacity.
        57. Velcro Pass Thru Bracket: Single.
        58. Velcro Pass Thru Bracket: Double. Two brackets with a 25 inch Velcro strap.
        59. Vest Holder: 3-capacity.
    1. Weapon Storage Cabinet: Heavy-duty steel cabinet.
       1. Size (HxWxD): 60 x 36 x 22 inches (1524 x 914 x 559 mm).
       2. Size (HxWxD): 66 x 36 x 22 inches (1676 x 914 x 559 mm).
       3. Size (HxWxD): 72 x 36 x 22 inches (1829 x 914 x 559 mm).
       4. Size (HxWxD): 83 x 36 x 22 inches (2108 x 914 x 559 mm).
       5. Doors: Bi-parting steel tambour door.
          1. Built-in padlock bar and lift handles on door.
       6. Multi-point locking mechanism.
       7. All-welded steel body.
       8. Adjustable levels: 4.
       9. Internal component adjustments: 1/2 inch (13 mm) increments.
       10. Universal back panel accommodates over 55 components to customize your weapon storage solution.
       11. Finish: Powder coat.
       12. Reinforced Universal Back Panel: Tailor system using steel adjustable components.
       13. Components:

\*\* NOTE TO SPECIFIER \*\* Delete Components not required.

* + - * 1. 3-Compartment Secure Handgun Insert w/Abloy locks
        2. Barrel Saddle: Single-capacity.
        3. Barrel Saddle: Single-capacity seismic.
        4. Barrel Saddle: Double-wide.
        5. Barrel Saddle: Double-wide seismic.
        6. Barrel Saddle: Extended.
        7. Barrel Saddle: Extended seismic.
        8. Barrel Saddle: Padlock.
        9. Barrel Saddle: 2-capacity spare.
        10. Barrel Saddle: Single-capacity spare - reversable.
        11. Bayonet Holder: Single-capacity.
        12. Bayonet Holder: 5-capacity.
        13. Carl Gustav base.
        14. Carl Gustav top.
        15. C-16 grenade launcher base
        16. Drop-Down Bracket: Single-capacity.
        17. Drop-Down Bracket: 10-capacity.
        18. Drop-Down Bracket: 12-capacity.
        19. Drop-Down Bracket: 16-capacity.
        20. Floor anchors.
        21. High-Security 3-compartment insert
        22. High-Security single-compartment locker
        23. Horizontal Mounts: 2-capacity.
        24. Horizontal Mounts: 3-capacity.
        25. Horizontal Mounts: 4-capacity.
        26. Low profile bin drawer.
        27. M2 Receiver and Barrel Storage: Single-capacity.
        28. MK19 grenade launcher base.
        29. MK19 grenade launcher top.
        30. Magazine Box: 3 inch wide.
        31. Magazine Box: 6 inch wide.
        32. Magnetic inventory tags.
        33. Mortar Storage: 60 mm.
        34. Mortar Storage: 80 mm.
        35. Pistol Pac: Single-capacity.
        36. Pistol Pac: 6-capacity.
        37. Pistol Pac: 8-capacity.
        38. Pistol Pac: Single-capacity and mag storage.
        39. Pistol Pac: 6-capacity and mag storage.
        40. Pistol Pac: 8-capacity and mag storage,
        41. Pistol Pac: 6-capacity lockable.
        42. Pistol Pac: 8-capacity lockable.
        43. Pistol Peg: Single-capacity. Store 9 mm and .22 Cal weapons.
        44. Pistol Peg: 6-capacity. Organize six 9 mm and .22 Cal weapons.
        45. Pistol Peg: 8-capacity. Organize eight 9 mm and .22 Cal weapons
        46. Plain shelf.
        47. Plain Shelf: Heavy duty.
        48. Radio Cradle: 6-capacity.
        49. Secure eyelet.
        50. Secure 3-Compartment
        51. Secure 2-Compartment
        52. Secure 6-Compartment
        53. Security Gate: 50 inches (1270 mm) height; for 60 and 66 inch (1524 and 1676 mm) high cabinets.
        54. Security screwdriver.
        55. Stock Saddle: Single-capacity.
        56. Stock Shelf: Single-capacity.
        57. Stock Shelf: 5-capacity.
        58. Stock Shelf: 6-capacity.
        59. Stock Shelf: 10-capacity.
        60. Stock Shelf: 12-capacity.
        61. Storage Box: 3 inch wide.
        62. Storage Box: 6 inch wide.
        63. Storage Box: 12 inch wide.
        64. Sword holder.
        65. Taclane bin drawer with locking lid.
        66. TASER Device Pac: Single-capacity.
        67. TASER Device Pac: 6-capacity.
        68. TASER Device Pac: 8-capacity.
        69. Universal Back Panel: 50 inches (1270 mm).
        70. Velcro Pass Thru Bracket: Single.
        71. Velcro Pass Thru Bracket: Double. Two brackets with a 25 inch Velcro strap.
        72. Vest Holder: 3-capacity.
        73. Locks:

Abloy Lock and 2 keys.

Abloy Key only (single).

Abloy Master key

Combi-Lock 3-Digit

Combi-Lock 4-Digit

Comp-X Digital Lock

Comp-X Digital Lock with Audit Trail

Real Lock-Combo 3-Digit.

Wesko Lock and 2 Keys.

Wesko Keys only (2/set).

Wesko Master Key.

* + 1. Mobile Weapon Storage Cart: Transport 20 long guns and accessories.
       1. Size (HxWxD): 49.5 x 34.25 x 26.75 inches (1257 x 870 x 679 mm); 10 long guns wide.
       2. Steering welded handles and heavy duty locking wheels.
       3. Security eyelets for cable locks and added security.
       4. Double sided universal back panel with over 55 weapon storage components.
       5. Components:

\*\* NOTE TO SPECIFIER \*\* Delete components not required.

* + - * 1. Barrel Saddle: Single-capacity.
        2. Barrel Saddle: Single-capacity seismic.
        3. Barrel Saddle: Double-wide.
        4. Barrel Saddle: Double-wide seismic.
        5. Barrel Saddle: Extended.
        6. Barrel Saddle: Extended seismic.
        7. Barrel Saddle: Padlock.
        8. Barrel Saddle: 2-capacity spare.
        9. Barrel Saddle: Single-capacity spare - reversable.
        10. Carl Gustav base.
        11. Carl Gustav top.
        12. C-16 grenade launcher base
        13. Drop-Down Bracket: Single-capacity.
        14. Drop-Down Bracket: 10-capacity.
        15. Drop-Down Bracket: 12-capacity.
        16. Drop-Down Bracket: 16-capacity.
        17. Horizontal Mounts: 2-capacity.
        18. Horizontal Mounts: 3-capacity.
        19. Horizontal Mounts: 4-capacity.
        20. M2 Receiver and Barrel Storage: Single-capacity.
        21. MK19 grenade launcher base.
        22. MK19 grenade launcher top.
        23. Magazine Box: 3 inch wide.
        24. Magazine Box: 6 inch wide.
        25. Magnetic inventory tags.
        26. Mortar Storage: 60 mm.
        27. Mortar Storage: 80 mm.
        28. Pistol Pac: Single-capacity.
        29. Pistol Pac: 6-capacity.
        30. Pistol Pac: 8-capacity.
        31. Pistol Pac: 6-capacity lockable.
        32. Pistol Pac: 8-capacity lockable.
        33. Pistol Peg: Single-capacity. Store 9 mm and .22 Cal weapons.
        34. Pistol Peg: 8-capacity. Organize eight 9 mm and .22 Cal weapons
        35. Pistol Peg: 6-capacity. Organize six 9 mm and .22 Cal weapons.
        36. Radio Cradle: 6-capacity.
        37. Secure eyelet.
        38. Security screwdriver.
        39. Stock Saddle: Single-capacity.
        40. Stock Shelf: Single-capacity.
        41. Stock Shelf: 5-capacity.
        42. Stock Shelf: 6-capacity.
        43. Stock Shelf: 10-capacity.
        44. Stock Shelf: 12-capacity.
        45. Storage Box: 3 inch wide.
        46. Storage Box: 6 inch wide.
        47. Storage Box: 12 inch wide.
        48. Sword Holder.
        49. TASER Device Pac: Single-capacity.
        50. TASER Device Pac: 6-capacity.
        51. TASER Device Pac: 8-capacity.
        52. Velcro Pass Thru Bracket: Single.
        53. Velcro Pass Thru Bracket: Double. Two brackets with a 25 inch Velcro strap.
        54. Vest Holder: 3-capacity.
    1. Pistol Storage Cabinet: 5-drawer steel cabinet. Store and organize 150 pistols and ammo.
       1. Size (HxWxD): 45 x 41.5 x 25 inch (1143 x 1054 x 635 mm).
       2. All-welded steel construction.
       3. Different drawer configurations to suit storage needs.
       4. Rubber matting in each drawer.
       5. Integrated 5-drawer locking mechanism.
       6. 5 Purpose-built storage inserts.
       7. Drawer Hardware: Easy-glide full-suspension.
       8. Leveling Feet: Built-in.
       9. Components:

\*\* NOTE TO SPECIFIER \*\* Delete components not required.

* + - * 1. Handgun insert.
        2. Pistol magazine insert.
        3. Bolt insert.
        4. Baton insert.
        5. Rifle magazine insert.
        6. Storage dividers.
        7. Pistol cabinet left to right dividers.
        8. Pistol cabinet compartment divider.
        9. 30-capacity pistol and magazine insert.
        10. Protective rubber matting - for top.
    1. TASER Device Storage Cabinet: Stores 20 non-lethal side arms. 2 TASER Devices per drawer. Stackable to maximize space.
       1. Size (HxWxD): 26 x 23 x 22 inch (660 x 584 x 559 mm).
       2. Construction: Steel.
       3. Compartments: Individually lockable.
       4. Optional power outlets.
       5. Easy-glide roll-out drawers.
       6. Components: Provide more storage space for other side arms and equipment.

\*\* NOTE TO SPECIFIER \*\* Delete components not required.

* + - * 1. Single-Capacity TASER Device Pac.
        2. 6-Capacity TASER Device Pac.
        3. Double-Wide Non-Powered TASER Device Storage Drawer.
        4. Double-Wide Powered TASER Device Storage Drawer.
        5. TASER Device Storage Shelf.
        6. TASER Device Storage Cabinet Riser.
    1. 4-Compartment Sidearm Locker: Store multiple pistols or TASER Devices in separate secure compartments.
       1. Size (HxWxD): 12.5 x 14 x 15 x inches (317 x 356 x 381 mm).
       2. Compartments (HxWxD): 5.25 x 6 x 14 inches (133 x 152 x 356 mm). Accommodate large pistols, magazines, and accessories.
          1. Lock: 3-digit combination.
          2. Interior rubber matting.
       3. Configuration, 4 compartments in a 2X2 configuration.
       4. Secure to a wall, attached together, or mount on a weapon locker.
       5. Locks:

\*\* NOTE TO SPECIFIER \*\* Delete lock options not required.

* + - * 1. Abloy Lock and 2 keys.
        2. Abloy Key only (single).
        3. Abloy Master key.
        4. Abloy Padlock and 2 keys.
        5. Wesko Lock and 2 keys.
        6. Wesko Keys only (2/set).
        7. Wesko Master Key.
        8. REAL Lock-Combo 3-Digit.
        9. Combi-Lock 3-Digit.
        10. Combi-Lock 4-Digit.
        11. Comp-X Digital Lock.
        12. Comp-X Digital Lock with Audit Trail.
    1. 4-Compartment Sidearm Tower: For storing handguns and TASER Devices.
       1. Construction: Welded steel.
       2. Configuration: 4x1 stacked. 4 individual compartments with space to store your sidearms, ammo, charges, and accessories.
       3. Size (HxWxD): 22.75 x 12 x 8 inches (22.75 x 305 x 203 mm).
       4. Compartment Size (HxWxD): 5 x 10.5 x 8 inch (127 x 267 x 203 mm) equipped with lock.
          1. Interior protective rubber matting.
       5. Mounting: To wall, stacked on each other, and attached side-to-side.
       6. Locks:

\*\* NOTE TO SPECIFIER \*\* Delete lock options not required.

* + - * 1. Abloy Lock and 2 keys.
        2. Abloy Key only (single).
        3. Abloy Master key.
        4. Abloy Padlock and 2 keys.
        5. Combi-Lock 3-Digit.
        6. Combi-Lock 4-Digit.
        7. Comp-X Digital Lock.
        8. Comp-X Digital Lock with Audit Trail.
        9. REAL Lock-Combo 3-Digit.
        10. Wesko Lock and 2 keys.
        11. Wesko Keys only (2/set).
        12. Wesko Master key.
  1. COMPUTER STORAGE
     1. Laptop Tower: 7-compartment tower for compact powered laptop storage. Keeps laptops and power cords secure, charged and ventilated in a small space. Towers can be attached side-to-side and stack on each other.
        1. Tower Size (HxWxD): 34 x 15 x 18 inch (864 x 381 x 457 mm).
        2. Compartments (HxWxD): 4 x 13.5 x 17 inch (102 x 343 x 432 mm).
           1. Can be keyed uniquely with an option for a master key.
           2. Vented at back to provide air flow.
           3. Inside is a single 110v outlet to keep gear fully charged.
        3. Construction: Heavy-duty steel, all-welded.
        4. Finish: Powder Coat. Color: Beige.
        5. Locks:

\*\* NOTE TO SPECIFIER \*\* Delete lock options not required.

* + - * 1. Abloy Lock and 2 keys.
        2. Abloy Key only (single).
        3. Abloy Master key.
        4. Abloy Padlock and 2 keys.
        5. Combi-Lock 3-Digit.
        6. Combi-Lock 4-Digit.
        7. Comp-X Digital Lock.
        8. Comp-X Digital Lock with Audit Trail.
        9. REAL Lock-Combo 3-Digit.
        10. Wesko Lock and 2 keys.
        11. Wesko Keys only (2/set).
        12. Wesko Master key.
    1. Single-Wide Powered Laptop Cabinet: Stores and secures 14 laptops. An optional 550 CFM fan and louvered side vents for ventilation.Charge laptops while stored with powered roll-out drawers; 110v power outlet and fits big and small laptops.
       1. Cabinet Size (HxWxD): 66 x 25 x 24 inch (1676 x 635 x 610 mm).
       2. Components:

\*\* NOTE TO SPECIFIER \*\* Delete components not required.

* + - * 1. Top-mounted 550 CFM fan.
        2. 9-Outlet power bar.
        3. Single-Wide powered laptop drawer (no lids).
        4. Single-Wide secure powered laptop drawer.
        5. Single-Wide bin storage drawer.
        6. Cable management raceway.
        7. Cable management arms (Set of 2).
        8. Network cable installed (CAT5 or 6)
        9. Single-Wide switch shelf.
    1. Double-Wide Powered Laptop Cabinet: Stores and secures 28 laptops. An optional top-mount 550 CFM fan and louvered vents for ventilation. Charge laptops while stored with powered roll-out drawers; 110v power outlet and fits big and small laptops.
       1. Cabinet Size (HxWxD): 66 x 36 x 24 inch (1676 x 914 x 610 mm).
       2. Components:

\*\* NOTE TO SPECIFIER \*\* Delete components not required.

* + - * 1. Top-mounted 550 CFM fan.
        2. 9-Outlet power bar.
        3. Caster base for double-wide laptop cabinet.
        4. Double-wide switch shelf.
        5. Double-wide powered laptop drawer (no lids).
        6. Double-wide secure powered laptop drawer.
        7. Doublewide bin storage drawer.
        8. Cable management raceway.
        9. Cable management arms (Set of 2).
        10. Network cable installed (CAT5 or 6).
        11. Double-Wide laptop cabinet floor anchors.
    1. PC-Stor: A secure desktop workstation on wheels. Heavy-duty steel cabinet stores and transports workstation hardware. Louvered vents on each side and 6-outlet power bar.
       1. Cabinet Size (HxWxD): 60 x 36 x 25 inch (1524 x 914 x 635 mm).
       2. Multi-point locking mechanism.
       3. All-steel bi-parting tambour door.
       4. Vented side panels.
       5. 6-outlet power bar.
       6. Components:

\*\* NOTE TO SPECIFIER \*\* Delete components not required.

* + - * 1. Top-mounted 550 CFM fan
        2. Thermostat controls.
        3. Full-Suspension rotating shelf.
        4. Fixxed perforated shelf.
        5. Roll-Out keyboard perforated shelf with wings.
        6. Roll-Out perforated shelf.
        7. Abloy Lock and 2 Keys.
        8. Wesko Lock and 2 Keys.
        9. Floor anchors.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete storage paragraphs not required.

* 1. SECURE MEDIA STORAGE
     1. Secure Storage Cabinets: All-welded steel cabinets includes a bi-parting steel tambour door for total media and file security.
        1. Changeable configuration.
        2. Padlock Bar for additional security.
        3. Adjustable leveling feet.

\*\* NOTE TO SPECIFIER \*\* Delete size, finish and components options not required.

* + - 1. Size (HxWxD): 36 x 36 x 22 inches (914 x 914 x 559 mm).
      2. Size (HxWxD): 55 x 36 x 22 inches (1397 x 914 x 559 mm).
      3. Size (HxWxD): 60 x 36 x 22 inches (1524 x 914 x 559 mm).
      4. Size (HxWxD): 66 x 36 x 22 inches (1676 x 914 x 559 mm).
      5. Size (HxWxD): 72 x 36 x 22 inches (1829 x 914 x 559 mm).
      6. Size (HxWxD): 83 x 36 x 22 inches (2108 x 914 x 559 mm).
      7. Finish: Powder Coat. Color: Beige.
      8. Finish: Powder Coat. Color: Grey.
      9. Finish: Powder Coat. Color: Black.
      10. Components: Adjustable in 1/2 inch (13 mm) increments.
          1. High-Security single-compartment locker.
          2. Low profile bin drawer.
          3. Multi-Media roll-out shelf.
          4. Roll-out reference shelf.
          5. CD/DVD roll-out shelf.
          6. Filing bin drawer.
          7. Plain Shelf: Heavy duty.
          8. Back plate and (5) divider set.
          9. Mail sorter insert.
          10. Secure 6-compartment.
          11. Laptop/Notebook secure 3-compartment.
          12. Laptop/Notebook secure 2-compartment.
          13. Floor anchors.
          14. Caster base.
          15. Taclane bin drawer with locking lid.
          16. Protective matting for reference shelf.
          17. Locks:

\*\* NOTE TO SPECIFIER \*\* Delete lock options not required.

Abloy Lock and 2 keys.

Abloy Key only (single).

Abloy Master key.

Abloy Padlock and 2 keys.

Combi-Lock 3-Digit.

Combi-Lock 4-Digit.

Comp-X Digital Lock.

Comp-X Digital Lock with Audit Trail.

REAL Lock-Combo 3-Digit.

Wesko Lock and 2 keys.

Wesko Keys only (2/set).

Wesko Master key.

* + 1. Media Storage Rack: Multi-media shelves are adjustable in 1 inch (25 mm) increments and come with 2 adjustable dividers. When adding on to the left or right a common post is used.
       1. Rack Width: 32.5 inches (925 mm).
       2. Standard Finish: Powder Coat. Color: Black Santex.

\*\* NOTE TO SPECIFIER \*\* Delete single-sided or doubled sided option, whichever is not required.

* + - 1. Single-Sided: Customize and re-configure your storage system with our versatile media storage wall. This open system provides open access and easy organization.
         1. Single sided post.
         2. Joiner bars. One per storage rack.
         3. Media Shelf Dividers (HxWxD): 4 x 32 x 5 inch (102 x 813 x 127 mm). Minimum of 2 per rack.
         4. Height: 54 inches (1372 mm).
         5. Height: 84 inches (2134 mm).
      2. Double-Sided: Customize and re-configure your storage system with our versatile component wall. This open system provides open access and easy organization.
         1. Double sided post.
         2. Joiner bars. One per storage rack.
         3. Media Shelf Dividers (HxWxD): 4 x 32 x 5 inch (102 x 813 x 127 mm). Minimum of 2 per rack.
         4. Height: 54 inches (1372 mm).
         5. Height: 84 inches (2134 mm).
      3. Media Types:
         1. DLT (All types). Capacity/Shelf: 25. Space Required: 6 inches (152 m).
         2. LTO (All types). Capacity/Shelf: 30. Space Required: 6 inches (152 mm).
         3. CD/DVD (jewel case). Capacity/Shelf: 78. Space Required: 7 inches (178 mm).
         4. CD/DVD (slim case). Capacity/Shelf: 156. Space Required: 7 inches. (178 mm)
         5. 4MM. Capacity/Shelf: 52. Space Required: 5 inches (127 mm).
         6. 8MM. Capacity/Shelf: 40. Space Required: 5 inches (127 mm).
         7. VHS (sleeve or case). Capacity/Shelf: 30. Space Required: 9 inches (229 mm).
         8. Optical 5.25 inch (133 mm). Capacity/Shelf: 45. Space Required: 7 inches (178 mm).
         9. 3480/3490/3590. Capacity/Shelf: 32. Space Required: 6 inches (152 mm).
         10. Mini-DV. Capacity per Shelf: 64. Space Required: 5 inches (127 mm).
         11. DV cam- small. Capacity per Shelf: 43. Space Required: 5 inches (127 mm).
         12. DV cam- large. Capacity per Shelf: 40. Space Required: 5 inches (127 mm).
         13. Beta- Small. Capacity per Shelf: 25. Space Required: 8 inches (203 mm).
         14. Beta- Large. Capacity per Shelf: 25. Space Required: 13 inches (330 mm).
    1. Multi-Media Mobile Cart: Solid-steel frame. Two sides of multi-level storage to organize and transport files. Welded handles, 4 heavy-duty wheels, and corner bumpers.
       1. Inside U sable Space: 38.5 inches (978 mm).
       2. Shelves: Quantity of 8, adjustable in 1 inch increments.
       3. Dividers: Quantity of 16. Add more for larger media transportation needs.
       4. Finish: Powder coat. Color: Black Santex.
       5. Media Types: Capacity per wall rack.
          1. DLT (All Types): 125.
          2. LTO (All Types): 150.
          3. CD/DVD (jewel case): 390.
          4. CD/DVD (Slim Line): 780.
          5. 3480/3490/3590: 160.
          6. 4MM: 260.
          7. 8MM: 200.
          8. OPTICAL5.25 inch: 225.
          9. 16MM FILM: 160.
          10. 35MM FILM: 100.
    2. Multi-Media Wall Rack: Open-rack system provides quick access and easy organization. Store different media without taking up valuable floor space.
       1. Dimensions (HxWxD): 34 x 33-3/4 x 9-3/4 inch (864 x 857 x 248 mm).
       2. Adjustable Shelves: 5 shelves and support frame.
       3. Rack Frame is preset to 12, 16, and 24 inch (305, 406, and 610 mm) stud centers.
       4. Finish: Powder coat. Color: Black Santex.
       5. Media Types: Capacity per wall rack.
          1. DLT (All Types): 125.
          2. LTO (All Types): 150.
          3. CD/DVD (jewel case): 390.
          4. CD/DVD (Slim Line): 780.
          5. 3480/3490/3590: 160.
          6. 4MM: 260.
          7. 8MM: 200.
          8. OPTICAL5.25 inch: 225.
          9. 16MM FILM: 160.
          10. 35MM FILM: 100.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required or delete product paragraphs not required.

* 1. GEAR STORAGE
     1. TA-50 Gear Storage Locker Fully-welded secure locker. Perforated sides and gates. Pre-installed heavy-duty wardrobe shelf. 3 hooks. Back panel lets you store weapons in same locker. Multi-point lock mechanism, including a built-in padlock hasp bar which accepts a 3/8 inch shackle. No assembly required, no frame bolts to tighten repeatedly. Fully-adjustable shelves.

\*\* NOTE TO SPECIFIER \*\* Delete size option not required.

* + - 1. Size (HxWxD): 78 x 36 x 24 inches (1981 x 914 x 610mm).
      2. Size (HxWxD): 78 x 42 x 24 inches (1981 x 1067 x 610 mm).
      3. Finish: Powder Coat. Color: Black Sandtex.
      4. Components:

\*\* NOTE TO SPECIFIER \*\* Delete components not required.

* + - * 1. Barrel Saddle: Single-capacity.
        2. Barrel Saddle: Single-capacity seismic.
        3. Barrel Saddle: Extended.
        4. Barrel Saddle: Extended seismic.
        5. Barrel Saddle: Padlock.
        6. Barrel Saddle: 2-Capacity spare
        7. Barrel Saddle: Single-capacity spare - reversable
        8. Bayonet Holder: Single-capacity
        9. Bayonet Holder: 5-capacity
        10. Magnetic inventory tags.
        11. Pass Thru Bracket: Single Velcro.
        12. Pass Thru Bracket: Double Velcro.
        13. Pistol Pac: Single-capacity.
        14. Pistol Pac: Single-capacity and mag storage.
        15. Pistol Peg: Single-capacity.
        16. Radio Cradle: 6-capacity.
        17. Secure eyelet.
        18. Security screwdriver
        19. Stock Shelf: Single-capacity.
        20. Stock Saddle: Single-capacity.
        21. Sword holder.
        22. TASER Device Pac: Single-capacity.
        23. Vest Holder: 3-capacity.
    1. Two-Tier TA-50 Gear Storage Locker: Two locking compartments. Fully-welded secure locker. Perforated sides and gates. Each compartment has a multi-point lock mechanism, including a built-in padlock hasp bar which accepts a 3/8 inch (10 mm) shackle. No assembly required. Fully-adjustable shelves.
       1. Dimensions (HxWxD): 78 x 36 x 24 inches (1981 x 914 x 610 mm).
       2. Dimensions (HxWxD): 78 x 42 x 24 inches (1981 x 1067 x 610 mm).
       3. Finish: Powder Coat. Color: Black Sandtex.
       4. Components:

\*\* NOTE TO SPECIFIER \*\* Delete components not required.

* + - * 1. Barrel Saddle: Single-capacity.
        2. Barrel Saddle: Single-capacity seismic.
        3. Stock Shelf: Single-capacity.
        4. Stock Saddle: Single-capacity.
        5. Barrel Saddle: Padlock.
        6. Barrel Saddle: 2-Capacity spare
        7. Barrel Saddle: Single-capacity spare - reversable
        8. Bayonet Holder: Single-capacity
        9. Magnetic inventory tags.
        10. Pistol Pac: Single-capacity.
        11. Pistol Pac: Single-capacity and mag storage.
        12. Pistol Peg: Single-capacity.
        13. Pass Thru Bracket: Single Velcro.
        14. Pass Thru Bracket: Double Velcro.
        15. Secure eyelet.
        16. Sword holder.
        17. Security Screwdriver.
        18. TASER Device Pac: Single-capacity.
    1. Constable Locker aka Tactical Locker: Two compartment bench design for storing gear and weapons. Both compartments are vented.
       1. Top Compartment: Heavy-duty shelf, hooks, hang bar and universal back panel for jackets, vests, accessories, and weapons.
       2. Bottom Compartment: Roll-out drawer for boots and heavy objects.

\*\* NOTE TO SPECIFIER \*\* The wooden butcher block bench is optional. Delete if not required.

* + - 1. Wooden butcher's block bench
      2. Dimensions (HxW): 72 x 18 inches (1829 x 457 mm).
         1. Depth of Top Compartment: 24 inches (610 mm).
         2. Depth of Bottom Compartment: 32 inches (813 mm).
      3. Dimensions (HxW): 72 x 24 inches (1829 x 610 mm).
         1. Depth of Top Compartment: 24 inches (610 mm).
         2. Depth of Bottom Compartment: 32 inches (813 mm).
      4. Components:

\*\* NOTE TO SPECIFIER \*\* Delete components if not required.

* + - * 1. Barrel Saddle: Single-capacity.
        2. Barrel Saddle: Single-capacity seismic.
        3. Barrel Saddle: Double-wide.
        4. Barrel Saddle: Double-wide seismic.
        5. Barrel Saddle: Extended.
        6. Barrel Saddle: Extended seismic.
        7. Barrel Saddle: Padlock.
        8. Barrel Saddle: 2-capacity spare.
        9. Barrel Saddle: Single-capacity spare - reversable.
        10. Bayonet Holder: Single-capacity.
        11. Bayonet Holder: 5-capacity.
        12. Drop-Down Bracket: Single-capacity.
        13. Magazine Box: 3 inch wide.
        14. Magazine Box: 6 inch wide.
        15. Magnetic inventory tags.
        16. Pistol Pac: Single-capacity.
        17. Pistol Pac: 6-capacity.
        18. Pistol Pac: 8-capacity.
        19. Pistol Pac: Single-capacity and mag storage.
        20. Pistol Pac: 6-capacity and mag storage.
        21. Pistol Pac: 8-capacity and mag storage,
        22. Pistol Pac: 6-capacity lockable.
        23. Pistol Pac: 8-capacity lockable.
        24. Pistol Peg: Single-capacity. Store 9 mm and .22 Cal weapons.
        25. Pistol Peg: 6-capacity. Organize six 9 mm and .22 Cal weapons.
        26. Pistol Peg: 8-capacity. Organize eight 9 mm and .22 Cal weapons
        27. Radio Cradle: 6-capacity.
        28. Secure eyelet.
        29. Security screwdriver.
        30. Stock Saddle: Single-capacity.
        31. Stock Shelf: Single-capacity.
        32. Stock Shelf: 5-capacity.
        33. Stock Shelf: 6-capacity.
        34. Storage Box: 3 inch wide.
        35. Storage Box: 6 inch wide.
        36. Storage Box: 12 inch wide.
        37. Sword holder.
        38. TASER Device Pac: Single-capacity.
        39. TASER Device Pac: 6-capacity.
        40. TASER Device Pac: 8-capacity.
        41. Velcro Pass Thru Bracket: Single.
        42. Velcro Pass Thru Bracket: Double.
        43. Vest Holder: 3-capacity.
    1. Duty Bag Locker All-welded steel construction. Top 3 compartments are equipped with full-length interior hinges. Bottom compartment has a full-extension easy-glide roll-out drawer. Padlock or keylock.
       1. Finish: Grey Santex powder-coat.
       2. Dimensions (HxWxD): 78 x 18 x 24 inches (1981 x 457 x 610 mm).
       3. Full-length concealed interior hinges on top 3 compartments.
       4. Easy-glide full-suspension bottom drawer.
       5. All-welded steel construction.
       6. Locking Mechanism: Padlock.
       7. Locking Mechanism: Built-in lock.
    2. Excalibur Locker: For change rooms or hallways. Manufactured with 16 ga, sheet steel for security and durability.
       1. Doors: Double-walled pan door and quiet-close door technology. Dorr frame venting
       2. Lock: A single-point latch.
       3. Hinge: Full length piano hinge.
       4. Finish: Graffiti-resistant powder coat. Color: \_\_\_\_\_\_\_\_.
       5. Shelves: Metal. 16 gauge galvanneal.
       6. Tops: Sloped.
       7. Coat hooks.
       8. Hanger bar.
       9. Sizes:

\*\* NOTE TO SPECIFIER \*\* there are 4 height, 4 width, 5 depth, and 6 tier configuration options available. Contact the manufacturer for more detailed information.'

* + - * 1. Height: \_\_\_ inches (\_\_\_ mm).
        2. Width: \_\_\_ inches (\_\_\_ mm).
        3. Depth: \_\_\_ inches (\_\_\_ mm).
        4. Tier Configuration: \_\_\_
    1. Event Locker: For change rooms or hallways. Manufactured with 16 ga, sheet steel for security and durability. Ventilated locker storage solution. Vented doors and sides for airflow.
       1. Doors: Double-walled pan door and quiet-close door technology. Door frame venting
       2. Lock: A single-point latch.
       3. Hinge: Full length piano hinge.
       4. Finish: Graffiti-resistant powder coat. Color: \_\_\_\_\_\_\_\_.
       5. Shelves: Metal.
       6. Tops: Sloped.
       7. Coat hooks.
       8. Hanger bar.
       9. Sizes:

\*\* NOTE TO SPECIFIER \*\* there are 4 height, 4 width, 5 depth, and 6 tier configuration options available. Contact the manufacturer for more detailed information.'

* + - * 1. Height: \_\_\_ inches (\_\_\_ mm).
        2. Width: \_\_\_ inches (\_\_\_ mm).
        3. Depth: \_\_\_ inches (\_\_\_ mm).
        4. Tier Configuration: \_\_\_
    1. Laptop Tower: For securely storing toughbooks, tablets and other powered accessories in offices, armories, and deployment rooms. All-welded steel construction.
       1. Dimensions (HxWxD): 34 x 15 x 18 inch (864 x 381 x 457 mm).
       2. Compartments (HxWxD): 4 x 13.5 x 17 inch (102 x 343 x 432 mm). Seven compartments.
          1. Each Compartment: 110 v outlet for charging. Vented at back for increased airflow. Outfitted with lock so access to laptops, body cameras and tablets is limited.
       3. Towers can be attached side-to-side and stack on each other.
       4. Finish: Powder coated. Color: \_\_\_\_\_\_\_\_.
       5. Locks:

\*\* NOTE TO SPECIFIER \*\* Delete lock options not required.

* + - * 1. Abloy Lock and 2 keys.
        2. Abloy Key only (single).
        3. Abloy Master key.
        4. Abloy Padlock and 2 keys.
        5. Combi-Lock 3-Digit.
        6. Combi-Lock 4-Digit.
        7. Comp-X Digital Lock.
        8. Comp-X Digital Lock with Audit Trail.
        9. REAL Lock-Combo 3-Digit.
        10. Wesko Lock and 2 keys.
        11. Wesko Keys only (2/set).
        12. Wesko Master key.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required.

* 1. E-LOCKERS
     1. E-Locker Secure Storage Locker Systems:
        1. A minimum of one Access Point Kiosk including a touchscreen industrial PC. Lockers are connected and controlled from the Access Point Kiosk touchscreen. Each locker system is comprised of various specified compartment sizes.
           1. Touchscreen Display: 12.1 inch (308 mm) high resolution.

Multiple languages available.

Two-factor authentication options available.

Audio and visual "Open Locker" warnings.

Built-in security camera option available for kiosks.

Customize kiosk screen display colors and logo.

Intel J1900 quad-core processor.

Operating System: Windows 10 IOT.

RAM: 4 GB.

ROM: 64 GB.

PCAP: 10 point touch.

Power Consumption: Less than 48 W X 86.

* + - 1. Compartments are indicated on associated plan. Compartment identification is managed by software. Each compartment is equipped with electronic cabinet lock.
      2. E-Lockers systems are powered by E-Lockers Inc. 2.0 Electronic Locker Software 2021. Software is configurable by registered admins for traceability and reporting functions, authentication type to open lockers, appearance, and customer usage guidelines. Tracking Abilities, secure monitoring, and 24/7 customer support. Configure to send alerts, track usage and limit/extend storage duration.
         1. Private Software: Used in facilities with regular, non-paying users.
         2. Public Software: Used in facilities wanting pay-per-use systems.
      3. Power Supply: 120V AC, 10A/12V DC, intermittent plus or minus 10 percent.
         1. Kiosk and cabinets must have direct power supply.

\*\* NOTE TO SPECIFIER \*\* Delete Uninterruptible Power Supply if not required.

* + - * 1. Uninterruptible Power Supply.
      1. An internet connection is required.
    1. Access Point Kiosk:

\*\* NOTE TO SPECIFIER \*\* Delete kiosk and depth options not required.

* + - 1. Standard Kiosk: PIN entry on touchscreen to open locker doors.
         1. Height x Width: 72 x 18 inches (1828 x 457 mm).
         2. Depth: 18 inches (457 mm).
         3. Depth: 24 inches (610 mm).
         4. Private software.
      2. Kiosk with RFID Reader: Standard kiosk with mounted RFID reader to open locker doors.
         1. Height x Width: 72 x 18 inches (1828 x 457 mm).
         2. Depth: 18 inches (457 mm).
         3. Depth: 24 inches (610 mm).
         4. RFID cards available.
         5. Private Software
      3. Kiosk with Barcode Reader: Standard kiosk with recessed barcode reader to open locker doors.
         1. Height x Width: 72 x 18 inches (1828 x 457 mm).
         2. Depth: 18 inches (457 mm).
         3. Depth: 24 inches (610 mm).
         4. Private Software
      4. Kiosk with Card Payment Reader: Standard kiosk with mounted card reader to open locker doors.
         1. Height x Width: 72 x 18 inches (1828 x 457 mm).
         2. Depth: 18 inches (457 mm).
         3. Depth: 24 inches (610 mm).
         4. Public Software
      5. Kiosk Electrical Components:
         1. Touchscreen Industrial PC (Windows 10 IoT OS).
         2. Power supply.
         3. Control board assembly
         4. Buzzer: Audio and Visual Alert

\*\* NOTE TO SPECIFIER \*\* Delete the camera and UPS are optional. Delete options not required.

* + - * 1. Camera.
        2. Uninterruptible Power Supply: 30 Minutes.
    1. Lockers:
       1. Cabinet Locks: CE and RoHS certification compliant. Heavy-duty metal construction with chrome-plated steel housing. Three-bolt regular triangle mounting enables high security. Mechanical override enables manual release during power failure.
          1. Operation Voltage: 12V DC intermittent plus or minus 10 percent.
          2. Power Consumption: 12V DC 1500 mA.
          3. Operation Mode: Fail locked.
          4. Holding Force: 150 kg.
          5. Maximum power on time: Less than 1 second.
          6. Solenoid: Rated for intermittent use.
          7. Cycle Rating: More than 1,000,000 times.
          8. MS Contact Rating: 2 A at 25 V.
          9. Mechanical Override: 7 mm hole.
          10. Dimensions (LxWxH): (72 x5 6 x14 mm).
          11. Gross Weight: 250 grams.
          12. Protection Class: IP20.

\*\* NOTE TO SPECIFIER \*\* Delete locker and depth options not required.

* + - 1. E-Locker 2 Door: 1 tier x 2 door locker module.
         1. Height x Width: 72 x 33.5 inches (1828 x 851 mm).
         2. Depth: 18 inches (457 mm).
         3. Depth: 24 inches (610 mm).
         4. Number Plates: 2.
         5. Coat Hooks: 3 per compartment.
         6. Shelves: 1 per compartment.
      2. E-Locker 4 Door: 2 tier x 2 door locker module.
         1. Height x Width: 72 x 33.5 inches (1828 x 851 mm).
         2. Depth: 18 inches (457 mm).
         3. Depth: 24 inches (610 mm).
         4. Number Plates: 4.
         5. Coat Hooks: 3 per compartment
      3. E-Locker 4 Door X-Wide: Extra wide 2 tier x 2 door locker module.
         1. Height x Width: 72 x 55.1 inches (1828 x 1400 mm).
         2. Depth: 24 inches (610 mm).
         3. Number Plates: 4.
      4. E-Locker 8 Door: 4 tier x 2 door locker module.
         1. Height x Width: 72 x 33.5 inches (1828 x 851 mm).
         2. Depth: 18 inches (457 mm).
         3. Depth: 24 inches (610 mm).
         4. Number Plates: 8.
      5. E-Locker 12 Door: 6 tier x 2 door locker module.
         1. Height x Width: 72 x 33.5 inches (1828 x 851 mm).
         2. Depth: 18 inches (457 mm).
         3. Depth: 24 inches (610 mm).
         4. Number Plates: 12.
      6. E-Locker 24 Door: 12 tier x 2 door locker module.
         1. Height x Width: 72 x 33.5 inches (1828 x 851 mm).
         2. Depth: 18 inches (457 mm).
         3. Depth: 24 inches (610 mm).
         4. Number Plates: 24.
    1. Fabrication: Asbestos free. Zero VOCs.

\*\* NOTE TO SPECIFIER \*\* Delete finish options not required.

* + - 1. Finish: Powder coated Black Sandtex (501); standard.
      2. Finish: Powder coated Charcoal Sandtex (633)
      3. Finish: Powder coated Flagstone Sandtex (803)
      4. Finish: Powder coated Slate Grey Sandtex (827)
      5. No exposed fasteners on locker door fronts and frames.
      6. End Panels: Two 16 gauge steel end panels included for every bank of lockers specified.
      7. Locker modules include levelers at base.
      8. Mounting: Necessary hardware included to connect locker modules to form locker bank.

\*\* NOTE TO SPECIFIER \*\* Delete mounting kit option not required.

* + - * 1. Mounting Kits: Floor.
        2. Mounting Kits: Wall.
      1. Each E-Locker system includes a 4-outlet extension cord reel.
      2. Components: 16 and 18-gauge carbon steel.
      3. Door hinge pins, locking pins and doors springs: Stainless steel.
      4. Each Cabinet: Has a 3.5 inch W channel for wiring and locks.

\*\* NOTE TO SPECIFIER \*\* Delete article if not required. Or delete product paragraphs not required.

* 1. MISCELLANEOUS STORAGE EQUIPMENT
     1. Weapon Work Bench For cleaning, maintaining, and repairing weapons.
        1. Construction: Stainless steel.
        2. A large flat workspace with protective matting.
        3. Tool trough and slide out drawer for tool or component storage.
        4. Supported by stainless steel legs.
        5. Universal back panel that accommodates storage components, which can be reconfigured to suit your needs.
        6. Storage Components:
           1. Barrel Saddle: Single-capacity.
           2. Barrel Saddle: Single-capacity seismic.
           3. Barrel Saddle: Double-wide.
           4. Barrel Saddle: Double-wide seismic.
           5. Barrel Saddle: Extended.
           6. Barrel Saddle: Extended seismic.
           7. Barrel Saddle: Padlock.
           8. Barrel Saddle: 2-capacity spare.
           9. Barrel Saddle: Single-capacity spare - reversable.
           10. Bayonet Holder: Single-capacity.
           11. Bayonet Holder: 5-capacity.
           12. Drop-Down Bracket: Single-capacity.
           13. Drop-Down Bracket: 10-capacity.
           14. Drop-Down Bracket: 12-capacity.
           15. Drop-Down Bracket: 16-capacity.
           16. Horizontal Mounts: 2-capacity.
           17. Horizontal Mounts: 3-capacity.
           18. Horizontal Mounts: 4-capacity.
           19. Magazine Box: 3 inch wide.
           20. Magazine Box: 6 inch wide.
           21. Magnetic inventory tags.
           22. Pistol Pac: Single-capacity.
           23. Pistol Pac: 6-capacity.
           24. Pistol Pac: 8-capacity.
           25. Pistol Pac: 6-capacity lockable.
           26. Pistol Pac: 8-capacity lockable.
           27. Pistol Pac: 6-capacity and mag storage.
           28. Pistol Pac: 8-capacity and mag storage,
           29. Pistol Peg: Single-capacity. Store 9 mm and .22 Cal weapons.
           30. Pistol Peg: 8-capacity. Organize eight 9 mm and .22 Cal weapons
           31. Pistol Peg: 6-capacity. Organize six 9 mm and .22 Cal weapons.
           32. Plain Shelf: 34 inch wide.
           33. Plain Shelf: 40 inch wide.
           34. Radio Cradle: 6-capacity.
           35. Secure eyelet.
           36. Security screwdriver.
           37. Stock Saddle: Single-capacity.
           38. Stock Shelf: Single-capacity.
           39. Stock Shelf: 5-capacity.
           40. Stock Shelf: 6-capacity.
           41. Stock Shelf: 10-capacity.
           42. Stock Shelf: 12-capacity.
           43. Storage Box: 3 inch wide.
           44. Storage Box: 6 inch wide.
           45. Storage Box: 12 inch wide.
           46. Sword Holder.
           47. TASER Device Pac: Single-capacity.
           48. TASER Device Pac: 6-capacity.
           49. TASER Device Pac: 8-capacity.
           50. Velcro Pass Thru Bracket: Single.
           51. Velcro Pass Thru Bracket: Double. . Two brackets with a 25 inch Velcro strap.
           52. Vest Holder: 3-capacity.
     2. High-Security Single Compartment Locker: Can be added to any secure cabinet.
        1. All-steel with 3-point locking mechanism. Cannot be accessed without a key.
        2. Doors: Perforated steel for visual inspections.
        3. Compartments: Include a rubber matting inlay.
     3. Vehicle Secure Storage Drawers: For storage of weapons in tactical vehicles. Mounts in most vehicle trunks but specifically for tactical SUVs. Holds 6 rifles, shotguns or carbines with room left over for accessories and ammunition.
        1. Construction: All Steel.
        2. Full-suspension easy-glide hardware.
        3. Lock: Knob-style.
        4. Pre-configured with barrel saddles.
     4. Hi-Density Storage Systems: Hold more weapons in a smaller area. Heavy-duty steel components for horizontal storage and drop-down systems.
        1. Drop-Down System: Allows more storage in a limited vertical space by re-envisioning the stock component.
     5. Evidence Storage Systems:
        1. Construction: Heavy-gauge steel for body and components.
        2. Storage Front: Multiple double-lined doors that can be individually locked.
        3. Doors: From 6 to 18 with quiet-close and stay-closed technology.

\*\* NOTE TO SPECIFIER \*\* Delete configuration and locks options not required.

* + - 1. Configuration: Closed-back.
      2. Configuration: Pass-through.
      3. Locks: Electronic lock.
      4. Locks: Padlocks.
    1. Parachute Holders: Store parachutes together with heavy-duty component that works with integrated wall system.
    2. Low-Profile Bin Drawer: Adds an extra level of security to any cabinet with a steel lid and key lock. The drawer slides out of cabinets on full-suspension easy-glide drawer hardware to make accessing valuables simple.
       1. Lid: All-steel lid equipped with your choice of keylock.
       2. Drawer Interior: Rubber matting inlay.
    3. COMP-X Digital Locks: Available on all cabinets and lockers. Locks use a key-pad combination for access and come available with Audit Trail to know who has accessed your storage system.

1. EXECUTION
   1. EXAMINATION
      1. Do not begin installation until substrates have been properly constructed and prepared.
      2. If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
   2. PREPARATION
      1. Clean surfaces thoroughly prior to installation.
      2. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
   3. INSTALLATION
      1. Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
   4. FIELD QUALITY CONTROL
      1. Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.

\*\* NOTE TO SPECIFIER \*\* Include if manufacturer provides field quality control with onsite personnel for instruction or supervision of product installation, application, erection, or construction. Delete if not required.

* + 1. Manufacturer's Services: Coordinate manufacturer's services in accordance with appropriate sections in Division 01.
  1. CLEANING AND PROTECTION
     1. Clean products in accordance with the manufacturer's recommendations.
     2. Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION