SECTION 11 68 13

PLAYGROUND EQUIPMENT

Display hidden notes to specifier. (Don't know how? [Click Here](https://www.arcat.com/sd/display_hidden_notes.shtml))

*Copyright 2024 - 2024 ARCAT, Inc. - All rights reserved*

\*\* NOTE TO SPECIFIER \*\* American Playground and Recreation Company; playground structures and equipment.
This section is based on products of American Playground and Recreation Company, which is located at:
47061 Charlotte Ct.
Sioux Falls, SD 57108
Phone: 605-401-4250
Email: \_\_\_\_\_\_\_\_.
Web: theamericanplayground.com
[Click Here] for additional information.
When you want a complete solution to your playground and recreational activity needs without sweating the small stuff, choose American Playground & Recreation Company- we make it easy. Our experienced team can assist from a needs assessment to design consultations, CAD drawings, and installation to keep your project on track, on budget, and on time
American Playground & Recreation Company has one of the largest support teams in the Nation. Our lineup of professionals is diverse and support the entire Midwest. Our core leadership team are trained experts not only in the playground industry but across many trades in construction..

1. GENERAL
	1. SECTION INCLUDES

\*\* NOTE TO SPECIFIER \*\* Delete items below not required for project.

* + 1. Playground Structures and Equipment:
			1. Playground structures.
			2. Freestanding elements.
			3. Inclusive elements.
			4. Playground screenings.
			5. Sports equipment.
			6. Surfacing.
			7. Site amenities.
			8. Fitness equipment.
			9. Versacourt.
			10. Swings.
			11. Dock parks,
			12. Shades and shelters.
	1. RELATED SECTIONS

\*\* NOTE TO SPECIFIER \*\* Delete any sections below not relevant to this project; add others as required.

* + 1. Section 03 30 00 - Cast-in-Place Concrete.
		2. Section 05 50 00 - Metal Fabrications.
		3. Section 06 10 00 - Rough Carpentry.
	1. SUBMITTALS
		1. Submit under provisions of Section 01 30 00.
		2. Product Data:
			1. Manufacturer's data sheets on each product to be used.
			2. Preparation instructions and recommendations.
			3. Storage and handling requirements and recommendations.
			4. Typical installation methods.

\*\* NOTE TO SPECIFIER \*\* Delete if not applicable to product type.

* + 1. Verification Samples: Two representative units of each type, size, pattern, and color.
		2. Shop Drawings: Include details of materials, construction, and finish. Include relationship with adjacent construction.
	1. QUALITY ASSURANCE
		1. Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum of five years documented experience.
		2. Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
		3. Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
	2. PRE-INSTALLATION CONFERENCE
		1. Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
	3. DELIVERY, STORAGE, AND HANDLING
		1. Store and handle in strict compliance with manufacturer's written instructions and recommendations.
		2. Protect from damage due to weather, excessive temperature, and construction operations.
	4. PROJECT CONDITIONS
		1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
	5. WARRANTY
		1. Manufacturer's standard limited warranty unless indicated otherwise.
1. PRODUCTS
	1. MANUFACTURERS
		1. Acceptable Manufacturer: American Playground & Recreation Company, which is located at: 47061 Charlotte Ct.; Sioux Falls, SD 57108; Tel: 605-401-4250; Email: [request info (customerservice@theamericanplayground.com)](https://admin.arcat.com/users.pl?action=UserEmail&company=American+Playground+%26+Recreation+Company&coid=54037&rep=&fax=&message=RE:%20Spec%20Question%20(11683apr):%20%20&mf=); Web: <https://theamericanplayground.com>

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions.

* + 1. Substitutions: Not permitted.
		2. Requests for substitutions will be considered in accordance with the provisions of Section 01 60 00.
	1. PLAYGROUND STRUCTURES AND EQUIPMENT

\*\* NOTE TO SPECIFIER \*\* Delete paragraph if not required, or delete items not required.

* + 1. Playground Structures:
			1. Shaded Tower Playground, 10 ft Square: Model FXT-50002. ADA: Yes. Age-appropriate climbers, slides, and panels. Slotted barrier panels for safety and visibility.
				1. Ages: 5-12 years. Capacity: 115 individuals. Estimated Timber Count: 48.
				2. Size: 43 x 34 ft. Use Zone: 58 x 47 ft. Fall Height: 10 ft.
			2. Hex Tower, 12 ft: ADA: Yes. Model FXT-50012. Ages: 5-12 years. Capacity: 55.
			3. Octo Tower Play Structure, 13 ft: Model FXT-50003. ADA: Yes. Slides, climbers, and play panels.
				1. Ages: 5-12 years. Capacity: 115. Estimated Timber Count: 49.
				2. Size: 49 x 43 ft. User Zone: 62 x 57 ft. Fall Height: 13 ft.
			4. Hex Tower Plat Structure,14 ft: Model FXT-50000. ADA: Yes. Designed with slides, climbers, and interactive play panels. Slotted Barrier Panels: For safety and visibility.
				1. Ages: 5-12 Years. Capacity: 82. Estimated Timber Count: 46.
				2. Size: 41 x 33 ft. User Zone: 56 x 46 ft. Fall Height: 14 ft.
			5. ADA HEX Shaded Tower Playground: Model FXT-50010. Ramp provides access to play activities for children of all abilities.
				1. Ages: 5-12 years. Capacity: 88. Estimated Timber Count: 44.
				2. Size: 45 x 31 ft. Use Zone: 51 x 40 ft. Fall Height: 10 ft.
			6. Adventures in Growing Series: Model AIG010-SRP. Challenges infants to climb stairs and rewards them with see-through panels and full slide once reaching the top. Primary or natural color schemes.
				1. Ages: 6-23 months. Capacity: 6 children.
				2. Size: 11 x 3 ft. User Zone: 24 x 15 inches.
			7. Playground Structures: Model AIG031-SRP. Educational and interactive for infants. Panel-based unit for exploration of texture, shapes, and sound. Infants use the texture climber to climb or crawl to the top and slide back down to explore panels and musical play pieces closer to the ground. Primary or natural color schemes.
				1. Dimensions: 11 x 9 ft. Use Zone: 24 x 21 ft.
			8. Bayonne Police Car: Model SRPFX-50333. ADA: Yes. Police car-themed.
				1. Ages: 2-12 years. Capacity: 54 children. Estimated Timber Count: 29.
				2. Structure Size: 24 x 20 ft. User Zone: 36 x 30 ft. Fall Height: 4 ft.
			9. Fighter Jet Steel Playground: Model SRPFX-50308-S1-E. ADA: Yes. Climbers, slides, and interactive panels to encourage dramatic, physical, and social play.
				1. Ages: 5-12 years. Capacity: 172 children.
				2. Structure Size: 48 x 30 ft. Use Zone: 61 x 42 ft. Fall Height: 7 ft.
			10. Firehouse with Tower: Model SRPFX-50303-02. Steel outdoor playground with tower and spiral slide connected to a shaded structure.
				1. Ages: 5-12 years. Capacity: 112 children. Estimated Timber Count: 40.
				2. Size: 44 x 43 ft. Use Zone: 56 x 32 ft. Fall Height: 10 ft.
			11. Floral Nature: Model SRPFX-50127-R1. ADA: Yes. Floral post-top accents, giant cattails, and log climbing elements. Climbing challenges, tunnels, bridges, and slides.
				1. Ages: 2- 12 years. Capacity: 174 children. Estimated Timber Count: 50.
				2. Structure Size: 47 x 42 ft. Use Zone: 59 x 54 ft. Fall Height: 6 ft.
			12. Playground Structures: Model GFP-10020-2. ADA: Yes.
				1. Ages: 2-12 Years. Capacity: 35 to 40 children. Estimated Timber Count: 31.
				2. User Zone: 27 x 21 ft. Structure Zone: 39 x 33 ft. Fall Height: 6 ft.
			13. Playground Structures: Model GFP-10044. ADA: Yes.
				1. Ages: 2-12 years. Capacity: 25-30 children. Estimated Timber Count: 24.
				2. User Zone: 17 x 15 ft. Structure Zone: 29 x 27 ft. Fall Height: 4 ft.
			14. Playground Structures: Model GFP-10069. ADA: Yes.
				1. Ages: 2-5 Years. Capacity: 25-30. Estimated Timber Count: 28.
				2. Structure Size: 22 x 21 ft. User Zone: 34 x 33 ft. Fall Height: 5 ft.
			15. Playground Structures: Model GFP-20125-2. ADA: Yes.
				1. Ages: 2-5 Years. Capacity: 15-20. Estimated Timber Count: 21.
				2. Structure Size: 12 x 15 ft. User Zone: 24 x 27 ft. Fall Height: 3 ft.
			16. Playground Structures: Model GFP-20128-4. ADA: Yes.
				1. Ages: 5-12 Years. Capacity: 50-55. Estimated Timber Count: 34.
				2. User Zone: 31 x 21 ft. Structure Zone: 43 x 33 ft. Fall Height: 7 ft.
			17. Playground Structures: Model GFP-20178. ADA: Yes.
				1. Ages: 5-12 years. Capacity: 30-35. Estimated Timber Count: 40.
				2. Structure Size: 39 x 31 ft. Use Zone: 51 x 43 ft. Fall Height: 7 ft.
			18. Playground Structures: Model GFP-20182. ADA: Yes.
				1. Capacity: 45-50. Estimated Timber Count: 30.
				2. User Zone: 36 x 35 ft. Structure Zone: 24 x 23 ft. Fall Height: 5 ft.
			19. Playground Structures: Model GFP-20229. ADA: Yes.
				1. Ages: 5-12 Years. Capacity: 35-40. Estimated Timber Count: 31.
				2. User Zone: 28 x 21 ft. Structure Zone: 40 x 33 ft. Fall Height: 7 ft.
			20. Playground Structures: Model GFP-20427. ADA: Yes.
				1. Ages: 2-12 Years. Capacity: 25-30. Estimated Timber Count: 26.
				2. User Zone: 21 x 19 ft. Structure Zone: 33 x 31 ft. Fall Height: 5 ft.
			21. Playground Structures: Model GFP-20446. ADA: Yes.
				1. Ages: 5-12 years. Capacity: 35-40. Estimated Timber Count: 34.
				2. Structure Size: 29 x 23 ft. Use Zone: 41 x 35 ft. Fall Height: 7 ft.
			22. Playground Structures: Model GFP-20449-2. ADA: Yes.
				1. Ages: 2-12 Years. Capacity: 50-55. Estimated Timber Count: 34.
				2. User Zone: 28 x 28 ft. Structure Zone: 40 x 40 ft. Fall Height: 6 ft.
			23. Playground Structures: Model GFP-20595. ADA: Yes.
				1. Ages: 2-5 Years. Capacity: 40-45. Estimated Timber Count: 27.
				2. Structure Size: 22 x 19 ft. User Zone: 34 x 31 ft. Fall Height: 4 ft.
			24. Playground Structures: Model GFP-20685. ADA: Yes.
				1. Ages: 5-12 years. Capacity: 25-30. Estimated Timber Count: 31.
				2. Structure Size: 20 x 19 ft. Use Zone: 37 x 31 ft. Fall Height: 7 ft
			25. Playground Structures: Model GFP-20695. ADA: Yes.
				1. Ages: 2-5 Years. Capacity: 15-20. Timber Count: 29.
				2. Structure Size: 25 x 15 ft. User Zone: 38 x 37 ft. Fall Height: 3 ft.
			26. Playground Structures: Model GFP-30000. ADA: Yes.
				1. Ages: 5-12 years. Capacity: 40-45. Estimated Timber Count: 41.
				2. Structure Size: 38 x 21 ft. Use Zone: 50 x 33 ft. Fall Height: 7 ft.
			27. Playground Structures: Model GFP-30069. ADA: Yes.
				1. Ages: 5-12 years. Capacity: 70-75. Estimated Timber Count: 34.
				2. Structure Size: 42 x 21 ft. Use Zone: 54 x 33 ft. Fall Height: 7 ft.
			28. Playground Structures: Model GFP-30082. ADA: Yes.
				1. Age: 2-12 Years. Capacity: 25-30. Timber Count: 32.
				2. User Zone: 29 x 21 ft. Structure Zone: 41 x 33 ft. Fall Height: 6 ft.
			29. Playground Structures: Model GFP-30084. ADA: Yes.
				1. Ages: 2-5 Years. Capacity: 50-55. Timber Count: 34.
				2. Structure Size: 30 x 19 ft. User Zone: 42 x 31 ft. Fall Height: 6 ft.
			30. Playground Structures: Model GFP-30103. ADA: Yes.
				1. Ages: 5-12 years. Capacity: 45-50. Estimated Timber Count: 40.
				2. Structure Size: 32 x 27 ft. Use Zone: 44 x 39 ft. Fall Height: 7 ft.
			31. Playground Structures / Marsh: Model SRPFX-50372. ADA: Yes. Nature-themed playground features cattails, a large, enclosed spiral slide, log climbers, and an overhead ladder.
				1. Age Group: 5-12 Years. Capacity: 59. Estimated Timber Count: 35.
				2. Structure Size: 32 x 23 ft. Use Zone: 44 x 35 ft. Fall Height: 6 ft.
			32. Playground Structures: ADA: Yes. Model PA5-29292.
				1. Age group: 5-12 Years. Capacity: 5-10. Timber Count: 31.
				2. Size: 26 x 23 ft. User Zone: 38 x 35 ft. Fall Height: 8 ft.
			33. Playground Structures: Model PS3-31385-1. Featuring activity panels, slides, and a lily pad climber.
				1. Age Group: 2-5 years. Capacity: 25-30. Estimated Timber Count: \_\_\_\_.
				2. Structure Size: 21 x 13 ft. Use Zone: \_\_\_ ft. Fall Height: \_\_\_ ft.
			34. Playground Structures: Model PS3-31400-1. ADA: Yes.
				1. Age Group: 2-5 years old. Capacity: 20-25. Estimated Timber Count: 34.
				2. Structure Size: 24 x 15 ft. Use Zone: 36 x 27 ft. Fall Height: 5 ft.
			35. Playground Structures: Model PS3-31664. ADA: Yes. Features two lily pad step climbers, two slides and multiple activity panels as well as a shade to keep kids cool as they play. Also available with 5 inch posts and no shade.
				1. Age Group: 2- 12 Years. Capacity: 32.
				2. Structure Size: 31 x 19 ft. Use Zone: 43 x 31 ft. Fall Height: 5 ft.
			36. Playground Structures: Model PS5-31723. ADA: Yes. Incorporates into any environment and holds 25 children. Customize your choice of colors to match your facility's exterior or branding. Post: 5 inches is available.
				1. Age Group: 2-12 years. Capacity: 25-30. Estimated Timber Count: 25.
				2. Structure Size: 25 x 10 ft. Use Zone: 37 x 22 ft. Fall Height: 6 ft.
			37. Playground Structures: Model PS3-31861. ADA: Yes. Steel playground. Talk tubes, slides, three climbing challenges, and space-themed play panels.
				1. Age Group: 2-12 years. Capacity: 30-35. Estimated Timber Count: 37.
				2. Structure Size: 31 x 19 ft. Use Zone: 43 x 31 ft. Fall Height: 5 ft.
			38. Playground Structures: Yes. Model PS3-31905. ADA: Yes.
				1. Age Group: 2-12 years. Capacity: 20-24. Estimated Timber Count: 25.
				2. Structure Size: 18 x 18 ft. Use Zone: 30 x 30 ft. Fall Height: 7 ft.
			39. Playground Structures: Model PS3-31908. Model PS5-31908: ADA: Yes. Available with a 5 inch Post.
				1. Age Group: 2-12 years. Capacity: 35-40. Estimated Timber Count: 32.
				2. Structure Size: 23 x 17 ft. Use Zone: 35 x 29 ft. Fall Height: 4'
			40. Playground Structures: Model PS3-32207. ADA: Yes
				1. Age Group: 5-12 years. Capacity: 15-20. Estimated Timber Count: 30.
				2. Structure Size: 18 x 18 ft. Use Zone: 30 x 30 ft. Fall Height: 7 ft.
			41. Playground Structures: Model PS3-32851. ADA: Yes. Offers shade and activities to be social with each other in the play environment.
				1. Use Zone: 18 x 10 ft. Fall Height: 3 ft.
				2. Comes in a 3.5 inch and 5 inch post option.
				3. Ages: 6-23 month. Capacity: 10 children.
			42. Playground Structures: Model PS3-33461-2. ADA: Yes. Many slides and climbing features. Durable steel frame. A platform to allow children of all abilities to play on and explore the structure.
				1. Age Group: 2-12 years. Capacity: 35-40. Estimated Timber Count: 39.
				2. Structure Size: 47 x 16 ft, Use Zone: 59 x 28 ft. Fall Height: 6 ft.
			43. Playground Structures: Model PS3-33726. ADA: Yes.
				1. Age Group: 5-12 years old. Capacity: 45-50. Estimated Timber Count: 36.
				2. Structure Size: 37 x 22 ft. Use Zone: 49 x 34 ft. Fall Height: 6 ft.
			44. Playground Structures: Model PS3-70058. ADA: Yes. Featuring a climbing net, lily pad climbers, two slides, and shades.
				1. Age Group: 5-12 years old. Capacity: 32. Estimated Timber Count: 37.
				2. Structure Size: 31 x 22 ft. Use Zone: 43 x 34 ft. Fall Height: 5 ft.
			45. Playground Structures: Model PS3-70243. ADA: Yes. Steel playground. Talk tubes, slides, four climbing challenges, and space-themed play panels.
				1. Age Group: 5-12 years old. Capacity: 45-50. Estimated Timber Count: 32.
				2. Structure Size: 34 x 13 ft. Use Zone: 46 x 25 ft. Fall Height: 7 ft.
			46. Playground Structures: Model PS3-70570. ADA: Yes.
				1. Age Group: 2-12 years old. Capacity: 20-25. Estimated Timber Count: 28.
				2. Structure Size: 27 x 21 ft. Use Zone: 39 x 29 ft. Fall Height: 6 ft.
			47. Playground Structures: Model PS3-70645. ADA: Yes.
				1. Age Group: 5-12 years old. Capacity: 25-30. Estimated Timber Count: 30.
				2. Structure Size: 18 x 22 ft. Use Zone: 30 x 34 ft. Fall Height: 7 ft.
			48. Playground Structures: Model PS3-70675. ADA: Yes.
				1. Age Group: 2-12 years old. Capacity: 40. Estimated Timber Count: 30.
				2. Structure Size: 30 x 18 ft. Use Zone: 42 x 30 ft. Fall Height: 6 ft.
			49. Playground Structures: Model PS3-70693. ADA: Yes.
				1. Age Group: 2-5 years old. Capacity: 16. Estimated Timber Count: 22.
				2. Structure Size: 20 x 10 ft. Use Zone: 32 x 22 ft. Fall Height: 3 ft.
			50. Playground Structures: Model PS3-70836 with Shade; Model PS3-70836-1 without Shade. ADA: Yes. Steel playground. Slides, climbing challenges, and space accented panels. An ADA transfer platform makes it accessible for all abilities.
				1. Age Group: 5-12. Capacity: 67. Estimated Timber Count: 38.
				2. Structure Size: 35 x 29 ft. Use Zone: 47 x 41 ft. Fall Height: 7 ft.
			51. Playground Structures: Model PS3-70845. ADA: Yes.
				1. Age Group: 5-12 years old. Capacity: 15-20. Estimated Timber Count: 35.
				2. Structure Size: 27 x 19 ft. Use Zone: 37 x 31 ft. Fall Height: 7 ft.
			52. Playground Structures: Model PS3-70971 with shade. Model PS3-70971-2 without shade. ADA: Yes. For small spaces. Includes a horizontal ladder, two climbers, a sliding pole, ADA transfer station, and a slide.
				1. Age Group: 5-12 years old. Capacity: 21. Estimated Timber Count: 26.
				2. Structure Size: 17 x 17 ft. Use Zone: 29 x 29 ft. Fall Height: 7 ft.
			53. Playground Structures: ADA: Yes. Model PS3-71031. Obstacle course-like steel playground. Provides kids with multiple opportunities for fun.
				1. Age Group: 5-12 years old. Capacity: 30-35. Estimated Timber Count: 40.
				2. Structure Size: 38 x 22 ft. Use Zone: 50 x 34 ft. Fall Height: 7 ft.
			54. Playground Structures: Model PS3-71039. ADA: Yes.
				1. Age Group: 2-5 years old. Capacity: 20-25. Estimated Timber Count: 27.
				2. Structure Size: 24 x 13 ft. Use Zone: 36 x 25 ft. Fall Height: 3 ft.
			55. Playground Structures: Model PS3-71043-1 without shade. Model PS3-71043 with shade. ADA: Yes. Age-appropriate challenges. Climbers, slides, and interactive play panels.
				1. Age Group: 2-5 years old. Capacity: 30-35. Estimated Timber Count: 29.
				2. Structure Size: 22 x 21 ft. Use Zone: 34 x 33 ft. Fall Height: 4 ft.
			56. Playground Structures: Model PS3-71098. ADA: Yes. Designed for developmental needs of younger children. Slides, play panels, and climbers. Select desired colors.
				1. Age Group: 2-5 years old. Capacity: 30-35. Estimated Timber Count: 30.
				2. Structure Size: 26 x 19 ft. Use Zone: 38 x 31 ft. Fall Height: 3 ft.
			57. Playground Structures: Model PS3-71103. ADA: Yes.
				1. Age Group: 5-12 years old. Capacity: 30-35. Estimated Timber Count: 30.
				2. Structure Size: 18 x 23 ft. Use Zone: 30 x 35 ft. Fall Height: 7 ft.
			58. Playground Structures: Model PS3-71143. ADA: Yes.
				1. Age Group: 5-12 years old. Capacity: 45-50. Estimated Timber Count: 52.
				2. Structure Size: 58 x 35 ft. Use Zone: 70 x 47 ft. Fall Height: 8 ft.
			59. Playground Structures: Model PS3-71401. ADA: Yes.
				1. Age Group: 2-5 years old. Capacity: 35-40. Estimated Timber Count: 27.
				2. Structure Size: 18 x 21 ft. Use Zone: 30 x 33 ft. Fall Height: 3 ft.
			60. Playground Structures: Model PS3-71407. ADA: Yes.
				1. Age Group: 5-12 years old. Capacity: 45-50. Estimated Timber Count: 35.
				2. Structure Size: 36 x 20 ft. Use Zone: 48 x 32 ft. Fall Height: 7 ft.
			61. Playground Structures: Model PS3-71449. ADA: Yes.
				1. Age Group: 2-12 years old. Capacity: 40-45. Estimated Timber Count: 35.
				2. Structure Size: 32 x 21 ft. Use Zone: 44 x 33 ft. Fall Height: 5 ft.
			62. Playground Structures: Model PS3-71462. ADA: Yes.
				1. Age Group: 2-12 years old. Capacity: 45-50. Estimated Timber Count: 37.
				2. Structure Size: 29 x 19 ft. Use Zone: 41 x 31 ft. Fall Height: 4 ft.
			63. Playground Structures: Model PS3-71488. ADA: Yes.
				1. Age Group: 5-12 years old. Capacity: 40-45. Estimated Timber Count: 33.
				2. Structure Size: 28 x20 ft. Use Zone: 40 x 32 ft. Fall Height: 7 ft.
			64. Playground Structures: Model PS3-71493. ADA: Yes.
				1. Age Group: 2-5 years old. Capacity: 25-30. Estimated Timber Count: 33.
				2. Structure Size: 30 x 16 ft. Use Zone: 42 x 28 ft. Fall Height: 4 ft.
			65. Playground Structures: Model PS3-71586. ADA: Yes.
				1. Age Group: 2-5 years old. Capacity: 25-30. Estimated Timber Count: 28.
				2. Structure Size: 17 x 16 ft. Use Zone: 29 x 28 ft. Fall Height: 4 ft.
			66. Playground Structures: Steel Playground. Model PS5-34365-1. ADA: Yes. Over 8 different climbing and balancing challenges.
				1. Ages: 5-12 years. Capacity: 65 to 70. Estimated Timber Count: 48.
				2. Structure Size: 41 x 36 ft. Use Zone: 53 x 48 ft. Fall Height: 7 ft.
			67. Playground Structures: Model PS5-70148. Unique dueling eclipse shade. The structure is set with a vertical square delta climber, a deep rung climber, and various panels. Panels low to the ground make it easy for children of all abilities to access the playground's features. Series: Commercial Playgrounds: Expedition (Large Posts).
				1. Ages: 2-12. Capacity: 42 children.
				2. Dimensions: 25 x 23 ft. Use Zone: 37 x 35 ft. Dimensions Width: 5 ft.
			68. Playground Structures: Model PS5-70150. ADA: Yes. Includes an ADA transfer point with a half gate and large ramps leading to a half push panel, zipper climber, and several different slides fit for every child. A below deck bench. A USA map panel and the spelling panel promote learning while engaging with others and playing. Adding necessary surfacing, makes this environment completely accessible for children of all abilities. This structure is available in any color scheme best fit for you.
				1. Age Group: 5-12 Years. Capacity: 115. Estimated Timber Count: 64.
				2. Structure Size: 53 x 53 ft. Use Zone: 65 x 65 ft. Fall Height: 5 ft.
			69. Playground Structures: Model PS5-70630. ADA: Yes. Steel playground. Play structure provides kids with multiple opportunities for fun while keeping them safe.
				1. Age Group: 5-12 years old. Capacity: 35-40. Estimated Timber Count: 37.
				2. Structure Size: 31 x 19 ft. Use Zone: 43 x 31 ft. Fall Height: 5 ft.
			70. Playground Structures: Model PS5-70720. ADA: Yes.
				1. Age group: 5-12 Years. Capacity: 15-20. Estimated Timber Count: 26.
				2. Size: 17 x 17 ft. User Zone: 29 x 29 ft. Fall Height: 7 ft.
			71. Playground Structures: Model PS5-71105. ADA: Yes.
				1. Age Group: 2-12 years old. Capacity: 50-60. Estimated Timber Count: 47.
				2. Structure Size: 39x39 ft. Use Zone: 51x51 ft. Fall Height: 7 ft. Inclusive: Yes.
			72. Playground Structures: Model PS5-71112. ADA: Yes. Features wide, inclusive ramps that allow children of all abilities to play and explore together. With slides, interactive play panels, and climbing challenges.
				1. Age Group: 2-12 years old. Capacity: 75-80. Estimated Timber Count: 49.
				2. Structure Size: 43 x 33 ft. Use Zone: 55 x 45 ft. Fall Height: 7 ft.
			73. Playground Structures: Model PS5-71361.
				1. Age Group: 5-12 years old. Capacity: 30-35. Estimated Timber Count: 45.
				2. Structure Size: 38 x 43 ft. Use Zone: 40 x 55 ft. Fall Height: 7 ft.
			74. Playground Structures: Model PS5-71362.
				1. Age group: 5-12 Years. Capacity: 30-35. Estimated Timber Count: 58.
				2. Size: 58 x25 ft. User Zone: 70 x37 ft. Fall Height: 10 ft.
			75. Playground Structures: Model PS5-71363
				1. Age Group: 5-12 years old. Capacity: 30-35. Estimated Timber Count: 43.
				2. Structure Size: 35 x 35 ft. Use Zone: 47 x 47 ft. Fall Height: 11 ft.
			76. Playground Structures: Model PS5-71364
				1. Ages: 5-12 Years. Capacity: 25-30. Estimated Timber Count: 40.
				2. Size: 26 x 36 ft. User Zone: 38 x 48 ft. Fall Height: 7 ft.
			77. Playground Structures: Model PS5-71365.
				1. Age Group: 5-12 years old. Capacity: 20-25. Estimated Timber Count: 35.
				2. Structure Size: 39 x 13 ft. Use Zone: 51 x 25 ft. Fall Height: 7 ft.
			78. Playground Structures: ADA: Yes. Model PS5-71464.
				1. Age Group: 5-12 years old. Capacity: 35-40. Estimated Timber Count: 34.
				2. Structure Size: 39 x19 ft. Use Zone: 51 x 29 ft. Fall Height: 6 ft.
			79. Playground Structures: Model PS5-71477. ADA: Yes.
				1. Age Group: 2-12 years old. Capacity: 25-30. Estimated Timber Count: 30.
				2. Structure Size: 24 x 20 ft. Use Zone: 36 x 32 ft. Fall Height: 5 ft.
			80. Playground Structures: Model RFX-30157. ADA: Yes. R-Town Cottage playground. Slides, climbers, and panels.
				1. Age Range: 2-12. Capacity: 82. Estimated Timber Count: 35.
				2. Size: 32 x 25 ft. Use Zone: 44 x 37 ft. Fall Height: 6 ft.
			81. Playground Structures: Model R3-20446. Recycled reliable recreation equipment. Bedrock climber, double chute slide, open spiral slide, deep rung arch climber, rung ladder, disk climber, arch bridge, and more. At the end of the rung ladder there is a chin bar, a turn bar, and a crunch bar.
				1. Ages: 5-12. Capacity: 30-45. Size: 27 x 23 ft. Use Zone: 41 x 37 ft.
			82. Playground Structures: Model R3FX-30029-R1. ADA: Yes. Train Fueling Station. Made from recycled materials. Climbing elements, slides, and interactive play panels.
				1. Age Group: 5-12 years old. Capacity: 120. Estimated Timber Count: 46.
				2. Structure Size: 49 x 36 ft. Use Zone: 61 x 47 ft. Fall Height: 7 ft.
			83. Playground Structures: Model R3FX-30038-R1. ADA: Yes. Barn-themed. Made from recycled materials, two climbers, crawl tunnel, slides, and interactive tic-tac-toe panel.
				1. Age Group: 2-5 years old. Capacity: 35. Estimated Timber Count: 26.Structure Size: 22 x 15 ft. Use Zone: 34 x 27 ft. Fall Height: 4 ft.
			84. Playground Structures: Model R3FX-30074. ADA: Yes. `Large Barn Recycled Playground. Accessible, wide ramps, climbers, slides, and interactive play panels
				1. Age Group: 5-12 years old. Capacity: 140. Estimated Timber Count: 67.
				2. Structure Size: 63 x 46 ft. Use Zone: 77 x 58 ft. Fall Height: 7 ft.
			85. Playground Structures: Model R3FX-30076-A-R3. ADA: Yes. Small Shipwreck-Themed playground. Themed panels, climbers, and slides. Made from recycled materials. Corrosion resistant.
				1. Age Group: 2-5 years old. Capacity: 53. Estimated Timber Count: 24.
				2. Structure Size: 20 x 16 ft. Use Zone: 32 x 28 ft. Fall Height: 4 ft.
			86. Playground Structures: Model R3FX-30076-B. ADA: Yes. Pirate ship structure with themed climbers, slides, play panels.
				1. Age Group: 5-12 years old. Capacity: 129. Estimated Timber Count: 43.
				2. Structure Size: 44 x 22 ft. Use Zone: 59 x 35 ft. Fall Height: 8 ft.
			87. Playground Structures: Model R3FX-30082-R1. ADA: Yes. Treehouse playground. Incorporates slides, climbing elements, and musical play panels for maximum fun.
				1. Age Group: 5-12 years old. Capacity: 99. Estimated Timber Count: 32.
				2. Structure Size: 31 x 28 ft. Use Zone: 43 x 38 ft. Fall Height: 6 ft.
			88. Playground Structures: Model R3FX-30093-R2. ADA: Yes. Train-themed play structure. Age-appropriate slides, climbers, activity panels, and detailed train accents.
				1. Age Group: 2-12 years old. Capacity: 40-45. Estimated Timber Count: 32.
				2. Structure Size: 33 x 20 ft. Use Zone: 45 x 32 ft. Fall Height: 5 ft.
			89. Playground Structures: Model R3FX-30099. ADA: Yes. Western-themed playground made from recycled materials. Play panels, slides, and climbing elements.
				1. Age Group: 2-5 years old. Capacity: 36. Estimated Timber Count: 30.
				2. Structure Size: 28 x 20 ft. Use Zone: 40 x 32 ft. Fall Height: 5 ft.
			90. Playground Structures: Model SRPFX-50195-R1. Two-story Rail Station-themed playground with connected water tower and train structures, along with climbers, tunnels, and slides.
				1. Age Group: 5-12 years old. Capacity: 127. Estimated Timber Count: 41.
				2. Structure Size: 35 x 31 ft. Use Zone: 47 x 45 ft. Fall Height: 8 ft.
			91. Playground Structures: Model SRPFX-50043-R1. ADA: Yes. Marsh themes playground. Giant cattails and log climbing blocks It also offers an overhead ladder and a large, enclosed spiral slide.
				1. Age Group: 5-12 years old. Capacity: 59. Estimated Timber Count: 35.
				2. Structure Size: 32 x 23 ft. Use Zone: 44 x 35 ft. Fall Height: 6 ft.
			92. Playground Structures: Model SRPFX-50115. ADA: Yes. Steel playground. Nature-themed structure. Featuring accessible wide ramps, talk tubes, activity panels, short slides, and climbers. Tree-topped posts and rustic treehouse accents.
				1. Age Group: 5-12. Capacity: 257. Estimated Timber Count: 73.
				2. Structure Size: 72 x 43 ft. Use Zone: 84 x 55 ft. Fall Height: 6 ft.
			93. Playground Structures: Model SRPFX-50159-R1. ADA: Yes. Ship-themed playground. Cargo net, treasure maze, and Alpine Thunder Slide.
				1. Age Group: 5-12 years old. Capacity: 72. Estimated Timber Count: 33.
				2. Structure Size: 32' x 23 ft. Use Zone: 44' x 35 ft. Fall Height: 7ft.
			94. Playground Structures: Model SRPFX-50183. ADA: Yes. Helicopter-themed. Climbing elements, slides, and interactive panels. Control panels for two young pilots.
				1. Age Group: 2-12. Capacity: 68. Estimated Timber Count: 33.
				2. Structure Size: 33 x 23 ft. Use Zone: 45 x 35 ft. Fall Height: 5 ft.
			95. Playground Structures: Model SRPFX-50218. ADA: Yes. Nature-themed, steel play structure. Three slides, climbing elements, and tree-house accents.
				1. Age Group: 5-12 years old. Capacity: 82. Estimated Timber Count: 34.
				2. Structure Size: 33 x 25 ft. Use Zone: 45 x 37 ft. Fall Height: 6 ft.
			96. Playground Structures: Model SRPFX-50221. ADA: Yes. Treehouse-themed steel play structure. Leafy post tops, tree trunk decorative accents, and picket-style panels. Slides, climbers, bridges, and other interactive panels.
				1. Age Group: 5-12. Capacity: 108. Estimated Timber Count: 44.
				2. Structure Size: 41 x 28 ft. Use Zone: 54 x 43 ft. Fall Height: 14 ft.
			97. Playground Structures: Model SRPFX-50222. ADA: Yes. Two levels. Baseball-themed. Double spiral slides, obstacle course, and climbing elements.
				1. Age Group: 5-12. Capacity: 210. Estimated Timber Count: 51.
				2. Structure Size: 53 x 44 ft. Use Zone: 66 x 57 ft. Fall Height: 13 ft.
			98. Playground Structures: Model SRPFX-50308-S1-E. ADA: Yes. Fighter jet-themed play structure. Steel frames and posts. Climbers, slides, interactive play panels, and an imagination-sparking cockpit.
				1. Age Group: 5-12. Capacity: 172. Estimated Timber Count: 42.
				2. Structure Size: 48 x 30 ft. Use Zone: 61 x 42 ft. Fall Height: 7 ft.
			99. Playground Structures: Model TFR0520XX. Tot-Trek Base Unit. Add on components based. Design your own. Three sample tot-lots: Color: Primary or natural scheme.
				1. Phase I: 5 children. Size: 8 x 6 ft. Base model features stairs, slide, bubble window, texture panel, and climber.
				2. Phase II: 10 children. Measures 12 x 8 ft. Phase I plus bridge, climber, stairs, and activity panels.
				3. Phase III: 15 children. Phase II plus crawl tube, slide, and activity panels.
				4. Ages: 6-23 months. Capacity: 0-15.

\*\* NOTE TO SPECIFIER \*\* Delete paragraph if not required, or delete items not required.

* + 1. Freestanding Elements:
			1. Playground Structures / Western Town Playground: Model SRPFX-50074. ADA: Yes. Two slides and multiple themed panels Featured dramatic play activity panels include the Federal Reserve Bank, Post Office, and more.
				1. Age Group: 5-12 Years. Capacity: 88. Estimated Timber Count: 37.
				2. Structure Size: 39 x 22 ft. Use Zone: 50 x 32 ft. Fall Height: 6 ft.
			2. 3 ft Double Straight Slide: Model AFR0221XX - 3 ft.
				1. Ages: 2-12 years. User Zone: 17 x 24 ft.
			3. 360 degrees Orbital Ladder: Model EFR0072XX.
				1. Ages: 5-12 years. User Zone: 23 x 21 ft.
			4. 4 ft Double Straight Slide: Model AFR0222XX - 4 ft.
				1. Ages: 2-12 years. User Zone: 17 x 27 ft.
			5. 5 ft Double Straight Slide: Model AFR0224XX - 5 ft.
				1. Ages: 2-12 years. User Zone: 17 x 28 ft.
			6. 6 ft Double Straight Slide: Model AFR0224XX - 6 ft.
				1. Ages: 2-12 years. User Zone: 17 x 29 ft.
			7. NetMax SpiderNet Small: Nylon covered steel core cables provide reinforced strength and are comfortable to touch. Black cabling. Galvanized posts.
				1. Ages: 5-12 years. User Zone: 29 x 29 ft. Weight: 773 lbs.
			8. NetMax SpiderNet Medium: Model 65160. Nylon covered steel cables provide reinforced strength and are comfortable to touch. Black cabling. Galvanized posts.
				1. Age: 5-12. Space Required: 41 x 41 ft. Weight: 1124 lbs.
			9. NetMax SpiderNet Large: Model 65161. Nylon covered steel cables provide reinforced strength and are comfortable to touch. Black cabling. Galvanized posts.
				1. Ages: 5-12 years. Space Required: 57 x 51 ft.
			10. Double Diamond Spinner: Model 65186. Ages: 5-12. Capacity: 6-10.
				1. Space Required: 21 ft 1 inch x 21 ft 1 inch. Weight: 927 lbs.
			11. Spyro Spinner Model 65188. Age Group: 5-12 years old. Capacity: 6-8.
				1. Space Required: 19 ft 9 inch x 19 ft 9 inch. Weight: 741 lbs.
			12. Inclusive Orbit: Model 65218. Ground level whirl sits flush with playground surfacing, allowing smooth and easy access for mobility devices.
				1. Age Group: 5-12 years. Space Required: 18 ft 9 inch x 18 ft 9 inch.
			13. Air Glider: Model 65219. Age Group: 5-12 years.
				1. Space Required: 22 ft 4 inch x 22 ft 4 inch.
			14. Large Boulder: Model 68196. Age: 5-12 years.
				1. Space Required: 18 x 16 ft. Weight: 631 lbs.
			15. Alligator Rider: Model TFR0510XX. Age Group: 2-5 years.
				1. User Zone: 17 x 17 ft.
			16. Ascend 10 ft Web Whirl: Model RC-2000-FSR. Age Group: 5-12 years.
				1. User Zone; 22 ft 10 inch x 22 ft 10 inch. Fall Height: 10 ft.
			17. Ascend 11 ft Tower: Model RC-101-1SR. Age Group: 5-12 years.
				1. User Zone; 27 ft 2 inch x 27 ft 2 inch. Fall Height 11 inch.
			18. Ascend 13 ft Tower: Model RC-101SR. Age Group: 5-12 years.
				1. User Zone; 30 ft 7 inch x 30 ft 7 inch. Fall Height: 13 inch.
			19. Ascend 13 ft Peak: Model RC-802-1SR. Made of 20 mm rope and a steel frame
				1. Height: 13 and 14 ft. Use Zone: 24 ft 2 inch x 24 ft 2 inch Fall Height: 7 ft.
			20. Ascend 14 ft Web Whirl: Model RC-2100-FSR.
				1. Age Group: 5-12 years. User Zone; 22 ft 10 inch x 22 ft 10 inch. Fall Height: 14 ft.
			21. Ascend 14 ft Peak: Model RC-802SR. Made of sturdy 20 mm rope and a steel frame.
				1. Height: 13 and 14 ft. Use Zone: 25 ft 9 inch x 25 ft 9 inch. Fall Height: 8 ft.
			22. Ascend 15 ft Peak Max: Model: RC-804SR. Height: 15 ft. Offers expanded climbing activities for children. Construction: Steel frame and durable 20mm cabling.
				1. Use Zone: 31 ft x 31 ft. Fall Height: 7 ft.
			23. Ascend 15 ft Tower: Model RC-102-1SR.
				1. Age Group: 5-12 years. User Zone: 37 ft 6 inch x 37 ft 6 inch. Fall Height: 7 ft.
			24. Ascend 18 ft Peak Max: Model RC-805SR. Height: 18 ft. Offers expanded climbing activities for children. Construction: Steel frame and durable 20 mm cabling.
				1. Use Zone: 29 ft 2 inch x 29 ft 2 inch. Fall Height: 6 ft.
			25. Ascend 19 ft Tower: Model: RC-102SR. Age Group: 5-12 years.
				1. User Zone: 44 ft 6 inch x 44 ft 6 inch. Fall Height: 7 ft.
			26. Ascend 25 ft Tower: Model: RC-103SR. Age Group: 5-12 years.
				1. User Zone: 52 ft 2 inch x 52 ft 2 inch. Fall Height: 7 ft.
			27. Ascend 9 ft Web Whirl: Model: RC-1200SR. Age Group: 5-12 years old.
				1. User Zone: 9 ft Web Whirl: 18 ft 7 inch x 18 ft 7 inch. Fall Height: 4 ft.
			28. Ascend Arch: Model: RC-909SR. Freestanding 13 x 13 ft net structure made of soft-to-touch rope and steel arches. Ages Group: 5-12 years old.
				1. Use Zone: 25 ft 6 inch x 25 ft 6 inch. Fall Height: 6 ft.
			29. Ascend Atom: Model: RC-903SR. Freestanding climber. Solid steel structure shaped like an atom. Age Group: 5-12 years.
				1. Use Zone: 26 ft 4 inch x 24 ft 9 inch. Fall Height: 7 ft.
			30. Ascend 10 ft Conquer Max: Model: RC-SM03SR. 400 sq ft of climbing space.
				1. Age Group: 5-12 years. Use Zone: 32 ft 10 inch x 32 ft 10 inch. Fall Height: 5 ft.
			31. Ascend Conquer- 10 ft: Model: RC-SM01SR. Freestanding play climbing structure. Made with soft, strong 20mm rope and is available in two different heights.
				1. Age Group: 5-12. Use Zone: 26 ft 7 inch x 24 ft 7 inch. Fall Height: 6 ft.
			32. Ascend Conquer- 9 ft: Model: RC-SM02SR. Freestanding play climbing structure. Made with soft, strong 20 mm rope and is available in two different heights.
				1. Age Group 5-12. Use Zone: 26 ft 5 inch x 26 ft 5 inch. Fall Height: 5 ft.
			33. Ascend Dual Treefort: Model: RC-NTS2001. Leaf accented decks, climbers and slide. Made from 20 mm rope and steel posts.
				1. Age Group: 5-12. Use Zone: 38 ft 5 inch x 36 ft 9 inch. Fall Height: 7 ft.
			34. Ascend Funnel Web: Model: RC-L005-SR.
				1. Ages: 5-12. Use Zone: 73 ft x 70 ft 5 inch. Fall Height: 9 ft.
			35. Ascend Hammock: Model Number: RC-U001-1SR. Made of soft, strong rope and steel frame. Customizable color options.
				1. Age Group: 5-12. Use Zone: 25 ft 7 inch x 15 ft 6 inch. Fall Height: 3 ft.
			36. Ascend Helix: Model: RC-TS006-SR.
				1. Ages: 5- 12. Use Zone: 33 ft 4 inch x 22 ft 4 inch. Fall Height: 7 ft.
			37. Ascend Low Loop Track: Model: RC-M001SR. Course is made with soft, strong 20 mm cabling and a sturdy steel frame. Transfer platform with grip handles.
				1. Age Group 5-12. Use Zone: 31 ft 3 inch x 28 ft 1 inch. Fall Height: 5 ft.
			38. Ascend Low Wave Track Model: RC-M006SR. Its steel frame and durable cabling comes with an attached slide and transfer platform with grip handles.
				1. Age Group: 5-12. Use Zone: 41 ft 7 inch x 34 ft 10 inch. Fall Height: 5 ft.
			39. Ascend Orbiter: Model: RC-923-SR.
				1. Ages: 5- 12. Use Zone: 37 ft 9 inch x 36 ft 11 inch. Fall Height: 10 ft.
			40. Ascend Overlook Without Slide: Model: RC-SH101SR. Four net walls to enter the overlook tower. Made from durable steel posts and 20 mm rope.
				1. Ages: 5- 12. Use Zone: 22 ft 10 inch x 22 ft 10 inch. Fall Height: 5 ft.
			41. Ascend Overlook with Slide: Model: RC-SH102SR.Four net walls to enter the overlook tower. Made from durable steel posts and 20 mm rope.
				1. Ages: 5- 12. Use Zone: 38 ft 7 inch x 27 ft 4 inch. Fall Height: 7 ft.
			42. Ascend Quad Rope: Model: RC-RW1002SR. Low to ground and made with sturdy 20 mm cabling. This product comes in three options: single, triple and quad.
				1. Ages: 5-12. Use Zone: 34 ft 5 inch x 20 ft 6 inch. Fall Height: 2 ft.
			43. Ascend Quest 11 Course: Model: RC-A011SR. Six different climbing experiences. Constructed with durability in mind, the course is comprised of 20 mm rope and steel posts to provide lasting climbing fun.
				1. Ages: 5-12. Use Zone: 70 ft 8 inch x 53 ft 10 inch. Fall Height: 7 ft.
			44. Ascend Quest 14 Course: Model: RC-A014SR. Using durable steel posts and soft, strong 20mm rope. Net walls, hammocks, and other climbers in this course.
				1. Ages: 5 -12. Use Zone: 44 ft 5 inch x 43 ft 2 inch. Fall Height: 7 ft.
			45. Ascend Quest 15 Course: Model: RC-A015SR. Six climbing challenges made from sturdy steel posts and 20 mm rope and designed to be flexible and accessible.
				1. Ages: 5 - 12. Use Zone: 56 ft 2 inch x 39 ft 4 inch. Fall Height: 7 ft.
			46. Ascend Quest 5 Course: Model: RC-A005SR. Expansive rope course. Its net walls, accessible surface, hammock, and variety of climbing elements provide children with endless opportunities.
				1. Ages: 5-12. Use Zone: 70 ft 8 inch x 53 ft 10 inch. Fall Height: 7 ft.
			47. Ascend Quest 7 Course: Model: RC-A007SR. Made from 20 mm rope and steel posts. Four different climbing experiences.
				1. Ages: 5-12. Use Zone: 26 ft 8 inch x 26 ft 8 inch. Fall Height: 7 ft.
			48. Ascend Quest 8 Course: Model: RC-A008SR. Seven walls of climbing. The course is constructed with steel posts and 20 mm rope for safety and durability.
				1. Ages: 5-12. Use Zone: 34 ft 7 inch x 32 ft 5 inch. Fall Height: 7 ft.
			49. Ascend Quest 9 Course: Model: RC-A009SR. Eight different climbing elements ranging from hammocks to net walls and other climbers. Made from 20 mm rope and steel posts.
				1. Ages: 5-12. Use Zone: 44 ft 5 inch x 42 ft 3 inch. Fall Height: 7 ft.
			50. Ascend Rope Bridges: Made using a steel frame and soft, strong 20 mm rope. Available in single, dual, or triple options.
				1. Ascend Rope Bridge. Model RC-7001HSR.

Use Zone: 22 ft 4 inch x 15 ft 5 inch. Fall Height: 3 ft.

* + - * 1. Ascend Dual Rope Bridge. Model RC-7002HSR.

Use Zone: 32 ft 2 inches x 15 ft 5 inches. Fall Height: 6 ft.

* + - * 1. Ascend Triple Rope Bridge. Model RC-7003HSR.

Use Zone: 42 ft x 15 ft 5 inch. Fall Height: 6 ft.

* + - 1. Ascend Single Rope: Model RC-RW1001SR. Low to the ground and made with sturdy 20 mm cabling. Comes in three options: single, triple and quad.
				1. Ages: 5-12. Use Zone: 26 ft 8 inch x 13 ft 6 inch. Fall Height: 2 ft.
			2. Ascend Tall Loop Track: Model: RC-R003SR. A rope race and climbing course. Supported by a solid steel frame. Transfer platform with grip handles. A flexible accessible playing surface.
				1. Ages: 5-12. Use Zone: 40 ft 10 inch x 40 ft 10 inch. Fall Height: 8 ft.
			3. Ascend Tall Wave Track: Combines a rope race and climbing course into one structure. Utilizes a transfer platform with grip handles. A flexible and accessible playing surface.
				1. Ages: 5-12, Use Zone: 53 ft 1 inch x 40 ft 10 inch. Fall Height: 7 ft.
			4. Ascend Thrill Tower: Model: RC-X2SR.
				1. Ages: 5-12 years. User Zone: 23 ft 3 inch x 22 ft 11 inch. Fall Height: 10 ft.
			5. Ascend Thrill Tower with Slide: Model: RC-1601-2SR.
				1. Ages: 5-12 years. User Zone: 45 ft 11 inch x 22 ft 10 inch. Fall Height: 7 ft.
			6. Ascend Thrill X Tower: Model: RC-1601-1SR. A freestanding solid steel structure and 20 mm rope.
				1. Ages: 5-12. Use Zone: 22 ft 10 inch x 22 ft 10 inch. Height: 24 ft. Fall Height: 6 ft.
			7. Ascend Treefort: Model: RC-NTS1002. Leaf panel accents, steel posts and 20 mm rope. Two climbing challenges and a slide.
				1. Ages: 5-12. Use Zone: 35 ft 10 inch x 29 ft 7 inch. Fall Height: 7 ft.
			8. Ascend Triple Rope: Model: RC-RW1003SR. Low to the ground and made with sturdy 20 mm cabling. Comes in three options: single, triple and quad.
				1. Ages: 5-12. Use Zone: 27 ft 9 inch x 25 ft 10 inch. Fall Height: 2 ft.
			9. Bear Rider: Model: TFS0020XX.
				1. Ages: 12-23 months, 2-5 years old. User Zone: 17 x 17 ft.
			10. Blue Tang Rider: Model: TFS0040XX. For ocean-themed playground.
				1. Ages: 2- 5. Use Zone: 16 x 14 ft.
			11. Spider Pyramid 6-4 Net Climber: Model: BSN-0002. Constructed from six-strand steel core rope that's also soft to the touch. Netting is only available in black. The center post color is subject to change.
				1. Ages: 5-12. Use zone of 53 x 53 ft. Fall Height: 6 ft.
			12. Chin Bar: Options: 1 bar, 2 bars, 3 bars.
				1. Ages: 5-12.
			13. Clownfish Rider: Model Number: TFS0039XX.
				1. Age Group: 2-5 years old. User Zone: 16 x 14 ft.
			14. Cozy Camper: Model Number: DRM00059XX.
				1. Ages: 2-12 Years. User Zone: 26 x 19 ft.
			15. Cozy Pod Spinner: Series: Independent Play: Motion Events.
				1. Ages: 5-12. Use Zone: 22 x 22 ft.
			16. Criss Cross: Model Number: 87000034XX.
				1. Age: 5-12 Years. User Zone: 25 x 16 ft. Fall Height: 6 ft.
			17. Daisy Dash Game: Play against the clock to touch each daisy sensor as it lights up. See how many lights you can touch before the clock runs out. Turn the rotator on the leaf panel to begin.
				1. Features:

Inclusive design.

Shaded electronic reactions game.

Includes 1 control panel and 5 sensors.

Powered by user rotating control panel.

Rotation charges internal battery cell.

Timer lasts 20 seconds.

Shade includes our Glide Elbow.

Patent-pending.

* + - * 1. Mounting Type: In-Ground.
				2. Color Scheme: Powder coat and fabric colors.
				3. Material Type: Powder coated steel posts and shade fabric.
				4. Surfacing: Requires 12 inches of surfacing.
			1. Double Curve Slide: Model: AFR0220XX.
				1. Ages: 5-12 years old. User Zone: 19 x 29 ft. Fall Height: 5 ft.
			2. EMS Rider: Model: TFS0015XX.
				1. Age: 2-5 Years. User Zone: 17 x 17 ft.
			3. Fire Station Climber: Model: TFR05580XX. Fosters whole body muscular strength, endurance, and flexibility.
				1. Ages: 5-12 Years. User Zone: 26 x 26 ft.
			4. Fire Truck Rider: Model Number: TFS0022XX.
				1. Age: 2-5 Years. User Zone: 17 x 17 ft.
			5. Frog Rider: Model: 90018202XX.
				1. Ages: 2-12. Use Zone: 17 x 17 ft.
			6. Musical Flowers: 4 different models. Sound like soft gongs and add a fun architectural element to any outdoor musical space. Each flower is a different size, height, color and has 4 different notes.
				1. Dimensions: 26-1/4 x 15-1/2 x 48-1/2 inch.
				2. Mounting Options: In-Ground, Surface, and Portable.
			7. Half Arch: Model Number: 87000014XX.
				1. Ages: 5-12 Years.
				2. User Zone: 26 x 20 ft. Fall Height: 5 ft.
			8. Half Dome Matrix Climber: Model: 87000024XX. Tall climber, designed for children. Two different ways to the top. Large hand and foot openings.
				1. Age: 5-12 Years
				2. User Zone: 27 x 20 ft. Fall Height: 10 ft
			9. Horse Rider: Model: TFS0026XX
				1. Age Group: 12-23 months, 2-5 years old
				2. User Zone: 17 x 17 ft
			10. Hump Camel Climber: Kids can climb up and down the ladder using the looped rungs and handrail for support.
				1. Ages: 5-12 Years: Model TFR16968XX. User Zone: 17x14 ft.
				2. Ages: 2-5 Years: Model TFR16985XX. User Zone: 17x14 ft.
			11. Hump Matrix Climber: Model 87000020XX.
				1. Ages: 5-12 Years. User Zone: 24 x 24 ft. Fall Height: 2 ft/
			12. Lion Rider: For Safari themed playground. Ages: 12 month to 5 years old.
			13. Metro Fire Truck: Models: Spring Mounted: 46514. Post Mounted: 49220.
				1. Ages: 2-5 years. User Zone: 20 x 16 ft.
			14. Mini Arch: Model Number: 87000011XX.
				1. Ages: 5-12 Years. User Zone: 20 x17 ft. Fall Height: 4 ft.
			15. Mini Half Dome Climber: Model: 87000026XX. Climb to top two different ways. Large hand and foot openings.
				1. Ages: 5-12 Years. User Zones: 20 x 18 ft. Fall Height: 6 ft.
			16. Mole Hill: Model Number: 87000010XX.
				1. Age: 5-12 Years. User Zone: 26 x 26 ft. Fall Height: \_\_\_.
			17. Motorcycle Rider: Model Numbers: 1 Seat: TFS0025XX. 2 Seat: TFS0023XX.
				1. Age: 2-5 Years. User Zone: 17 x 17 ft.
			18. Mound: Model Number: 87000016XX.
				1. Ages: 5-12 Years. User Zone: 27 x 27 ft. Fall Height: 8 ft
			19. Off-Road Military Vehicle: Model Number: RECF0032XX.
				1. Ages: 2-12 Years. User Zone: 16 x 12 ft.
			20. Off-Road Truck: Model Number: 49222.
				1. Ages: 2-5 Years. User Zone: 26 x 11 ft.
			21. Open Spiral Slide: Model Number: AFR0243XX.
				1. Age Group: 5-12 years old. User Zone: 18 x 25 ft. Fall Height: 6 ft.
			22. Pig Rider: Model Number: TFS0027XX.
				1. Age Group: 12-23 months, 2-5 years old. User Zone: 17 x 17 ft.
			23. Post Mounted Ambulance: Model Number: 47507.
				1. Ages: 2-5 Year. User Zone: 20 x 16 ft.
			24. Spring Mounted Ambulance: Model Number: 46520.
				1. Ages: 2-5 Years. User Zone: 20 x 16 ft.
			25. Quad Saw: A unique 4 corner spring rider designed with a center platform.
				1. Ages: 5-12. Use Zone: 22 x 18 ft.
			26. Retro Rocker: 2-Seat spring rocker.
				1. Ages: 2- 5. Use Zone: 13 x 17 ft.
			27. Right/Left Curve Slide: 4 ft. Model Numbers: Right: AFR0217XX. Left: AFR0218XX.
				1. Age: 2-5 years old. User Zone: 18 x 28 ft.
			28. Rockface Climber:
				1. Ages: 5-12 Years. User Zone: 21 x 17 ft
			29. Sensory Roller Table: Freestanding table is equitable to overhead climbers and is designed with 44 precision-milled rollers to provide a smooth ride.
				1. Ages: 5-12. Color Options: Red or Blue. Weight: 512 lbs.
			30. Stegosaurus Rider: Model Number: TFS0032XX. Ages: 2-5.
			31. Straight Slide: Age Group: 2-12 years old.

\*\* NOTE TO SPECIFIER \*\* Delete model options not required.

* + - * 1. Model: 3 ft: AFR0211XX. User Zone: 16 x 24 ft.
				2. Model: 4 ft: AFR0212XX. User Zone: 16 x 27 ft.
				3. Model: 5 ft: AFR0213XX. User Zone: 16 x 29 ft.
				4. Model: 6 ft: AFR0214XX. User Zone: 16 x 30 ft.
			1. Trapeze Ring: Model Number: AFR0098XX
				1. Ages: 5-12 Years Old. User Zone: 16 x 21 ft.
			2. Tri-Hex: Model: 87000022XX. Triple Hexagon Plastic Climber. One junction point creates its distinctive shape. Each Tortoise climbing panel has hand and foot holes that make gripping and climbing safe and easy.
				1. Ages: 5-12 Years. User Zone: 18 x 15 ft. Fall Height: 4 ft.
			3. Tri-Pent: Model: 87000023XX.
				1. Age: 5-12 Years. User Zone: 21 x 21 ft. Fall Height: 4 ft.
			4. Tri-Rung: Model: TRT-10. Triple Toss game.
				1. Options: Curved, Inverted Arch, Straight, Zig-Zag.
				2. Ages: 2-12. User Zone: 16 x 21 ft.
			5. Trout Rider: Model: TFS0029XX. For bayou or river-themed park.
				1. Ages: 12 months to 5 years old.
			6. Vertical Spider Net Climber: Model Number: EFR0103XX. Freestanding and made of durable, powder coated steel and easy-to-grip six-strand steel core rope. Large selection of powder coat colors.
				1. Ages:5-12 Years. User Zone: 21 x 12 ft. Fall Height: 9 ft.
			7. Whirl and Twirl: One child rides and the other spins them about. Tilted design adds to the spinning momentum. Rounded top helps children as they get in and out of the bowl.
				1. Ages 5-12 years. Use zone: 15 ft 7 inch x 15 ft 7 inch.
			8. Zip Line: Durable cable system and comfortable seat. Designed to help the rider gain momentum at the start and slow down at the landing.
				1. Ages: 5-12. Mounting Type: In-Ground.
				2. Lengths: Available in 75 and 100 ft.
				3. Color Scheme: Powder coat colors.
				4. Material Type: Steel posts.
				5. Surfacing: Requires 60 inches of impact attenuation.
				6. Critical Fall Height: 10 ft.

\*\* NOTE TO SPECIFIER \*\* Delete paragraph if not required, or delete items not required.

* + 1. Inclusive Elements:
			1. Aria Playgound Instrument: Model: ARIA-IG-REC-SRP. ADA accessible. Features nine notes in C major.
				1. Includes: In-Ground Mount Kit, Recycled Post.
				2. Ages: All Ages.
				3. Sizes: Available in small, medium, and large.
			2. Butterfly Outdoor Instruments: Model: BFLY-#-IG-SRP. Each sold separately Available In different color options to match outdoor aesthetic.
				1. Toddler Size Also Available
			3. Calypso Drum Outdoor Instrument: Model: CPSO-#-SM-SRP. Reminiscent of steel drums from Caribbean islands. Stainless Steel. 9 notes. Range is alto/soprano in an F Major Pentatonic scale.
				1. Silver post is standard. Green is available.
				2. Ages: All.
				3. Sizes: Available in small, medium, and large.
				4. Colors: Steel Gray or Green.
			4. Musical Flowers: Model: FWR-#-IG-SRP. Sound like soft gongs.
				1. Colors: indigo, orange, turquoise, and yellow.
				2. Each flower has a different musical chord, size, height, and color.
				3. Wheelchair accessible.
				4. Includes attached mallets.
				5. Mounting: In-ground mount, surface mount, or portable.
				6. Construction: Powder-coated steel frame. Anodized aluminum flower petals. Stainless steel hardware.
			5. Flush Mount Ramp System: Model Number: 2BY2HR#.Single-side ADA ramp.
				1. ADA Half Ramp System for 12 and 8 inch Border Timbers.
				2. Includes: (5) Spikes, (2) End Caps, Hardware.
				3. Dimensions (L x W): 60 x 43 inches.
				4. Steel or flex spikes.
			6. Full Ramp System: Model Number: 2BY2FR#-F.
				1. ADA Full Ramp System for 12 and 8 inch Border Timbers.
				2. Includes: (9) Spikes, (2) End Caps.
				3. Steel or flex spikes.
				4. Dimensions (L x W): 120 x 43 inch.
			7. Glockenspiel: Model: 77131-IG.
				1. Includes: In-Ground Mount.
				2. Extra mallets (77003) are also available.
			8. Harp: Model: HRP-IG-SRP. Each chime creates sounds perfectly tuned; C major pentatonic. A sculptural shape. Construction: Powder-coated steel frame, Anodized aluminum chimes. Stainless steel hardware. Mounting: In-ground mount, surface mount, or portable.
				1. Wheelchair accessible. Attached mallets.
			9. Imbarimba: Model: IMBA-IG-REC-SRP. C major and A minor pentatonic. The design was inspired by the marimba, and the kalimba. Location of upper and lower notes is designed to allow children to easily access all of them.
				1. HDPE frame. Coated fiberglass bars. Anodized aluminum resonators.
				2. Stainless steel hardware.
				3. Wheelchair accessible. Includes two attached mallets.
				4. In-ground mount, surface mount, or portable.
			10. Inclusive Atom Spinner: Model: TFR0659XX.
				1. Ages: 2-5 and 5-12. Capacity: 6.
				2. Use Zone: 9 ft+ Radius Recommended.
			11. Inclusive Swing: Model: BSIS-25. Seat is designed for children who need support to maintain a seated position. Each seat comes with galvanized chain. Available in any rotomolded plastic color with a yellow or beige brace.
				1. Ages: 2-5 or 5-12.
			12. Lady Bug Drum: Model: 77149.
			13. Manta Ray Metallophone: Model: MRAY-IG-SRP. Individual chime tubes suspended by nylon-coated stainless steel cable. Steel powder-coated frame. Chimes on both sides are the same 18 notes. Sizes: Available in small, medium, and large.
				1. Portable and Surface Mount: Height of 44 inches. For children 5 and up.
				2. In-Ground Mount: Finished height of 39 inches. For children ages 3 and up.
				3. Mounting: Surface or In-Ground.
				4. Ages: All Ages.
			14. Melody Playground Instrument: Model: MELD-IG-REC-SRP.
				1. Compact instrument with nine keys that play in C major scale. Made of anodized aluminum bars. Two mallets attached with a nylon-coated stainless steel cable. Sizes: Available in small, medium, and large.
				2. Ages: All Ages.
			15. Mushroom Musical Instrument: Model: MUSH-#-SM-SRP.
				1. Age Group: All Ages.
				2. Size: Available in Small, Medium, and Large.
			16. Pegasus Metallophone: Model: PEG-IG-REC-SRP. A large metallophone with 23 anodized aluminum bars in both C major and A minor. When struck, it creates resonating sounds similar to a gong. Includes: In-Ground Mount Kit, Recycled Post.
				1. Sizes: Available in small, medium, and large.
				2. Ages: All Ages.
			17. Inclusive Orbit: Model: PLD0010XX. Stainless steel independent freestanding playground equipment that allows for easy wheelchair accessibility by the surface-level platform.
				1. Ages: 5-12 years. Use Zone: 20 x 20 ft.
			18. Single Post Bongos: Model: 77136-IG.
			19. Includes: In-Ground Mount.
			20. Tuned Drums: Model: TD-IG-N-SRP. Each drum is a different size including 15, 12, 10, 8, and 6 inch. Tallest drum makes the deepest sound, while the shortest makes the highest sound. Can be arranged and installed in any location and pattern. Must be installed less than 3 inches or more than 9 inches apart for children's safety. For wheelchair accessibility, leave 36 inch clearance around the entire drum arrangement.
				1. HDPE frame. Anodized aluminum chimes and resonators. Stainless steel hardware. C major and A minor. Wheelchair accessible. Includes two attached mallets. In-ground mount, surface mount, or portable. Normal or toddler size.

\*\* NOTE TO SPECIFIER \*\* Delete paragraph if not required, or delete items not required.

* + 1. Playground Screening:
			1. Playsafe Artistic Cut: Playground screen. No sharp corners or edges.
				1. Square Steel Posts: 4 inches. Base Plate: 3/4 inch round beveled plates.
				2. Structural Aluminum Angle Framework: 3 x 3 x 1/4 inch.
				3. Solid Infill: 36 inches and lower.
				4. Openings: No smaller than 1/2 inch and no openings greater than 1-3/4 inches.
				5. Your design, logo or cartoon characters that compliment your playground.
				6. Gates with lock sets at 48 inch heights.
				7. Panic hardware, fire exit and alarmed devices: Available and factory installed.
				8. Gate Closures: Available and factory installed.
				9. Hardware: Button head stainless steel screws. No hex head.
			2. Playsafe Semi-Private: Playground screen. No sharp corners or edges.
				1. Square Steel Posts: 4 inches. Base Plate: 3/4 inch round beveled plates.
				2. Structural Aluminum Angle Framework: 3 x 3 x 1/4 inch.
				3. Solid Infill: 36 inches and lower.
				4. Semi-private upper infill slates. Openings: No greater than 1-3/4 inches.
				5. Gates with lock sets at 48 inch heights.
				6. Panic Hardware, Fire Exit and Alarmed Devices: Factory installed.
				7. Gate Closures: Factory installed.
				8. Hardware: Button head stainless steel screws. No hex head.
			3. Playsafe Solid: Playground screen. No sharp corners or edges.
				1. Square Steel Posts: 4 inches. Base Plate: 3/4 inch round beveled plates.
				2. Vehicle Barrier Protection: 6 inch square steel posts. 3/4 inch beveled plates. Continuous W-beam guardrail.
				3. Structural Aluminum Angle Framework Screen Panels: 3 x 3 x 1/4 inch.
				4. Solid Infill: 36 inches and lower.
				5. Openings: No smaller than 1/2 inch and no openings greater than 1-3/4 inches.
				6. Gates with lock sets at 48 inch heights.
				7. Panic hardware, fire exit and alarmed devices: Available and factory installed.
				8. Gate closures available and factory installed.
				9. Button head stainless steel screws. No sharp bolts or screws.
			4. Playsafe Vehicle Barrier: Prevent mobile equipment from skidding off the road by redirecting it. Minimize the damage of errant vehicles. High quality material and anti-rust and corrosion resistant surfaces for longer service life. Can be repaired quickly after accident
				1. Shape: Two waves.
				2. Material: Q235 (equivalent to S235JR / DIN EN10025 and Gr.D / ASTM A283M), Q345 (S355JR / ASTM A529M 1994), Q255JR, etc.
				3. Surface: Hot dipped galvanized or powder coating.
				4. Standard: AASHTO M-180, EN1317, RAL-RG620, JT/T 281-1995, JT/T 281-2007, JT/T 457-2007, SPS98S, EU, USA, AS/NZS, or any other International Standards.
				5. Certificate: GB/T9001-2000, ISO 9001-2000.

\*\* NOTE TO SPECIFIER \*\* Delete paragraph if not required, or delete items not required.

* + 1. Sports Equipment:
			1. Soccer Goals: Classic Alumagoal 6.5 x 12 ft. White. Model 145SS.
				1. Elite Club Goals: Available in multiple sizes.
				2. Ground anchors and 3 mm white nets are included.
			2. Portable Welded Aluminum Bleachers: Length: 15 ft. 3 Row. SKU No. 129-1214-3.
				1. Durable, lightweight, low-rise, aluminum construction. Weight: 206 lbs.
				2. Single 2 x 10 inch footboards and 2 x 12 inch clear anodized seat planks.
				3. Understructure Options:

Welded aluminum.

Aluminum tube angle understructure.

Heavy-duty galvanized steel understructure.

* + - * 1. Designed in accordance with the IBC 2014 and ICC 300 building codes.
			1. GaGa Ball Pit, 15 ft. Comes with the following items: Borders: 12 inch. Qty: 23. Spikes: 36 inches. Qty: 12. End Caps: 6 inch. Qty: 2.
			2. Ultimate Playground Goal - Basketball: Model Number: 176SS. Ages: 5-12
			3. Game Series Breakaway Goal; Basketball: Model: 179SS. A ball-and-socket breakaway design prevents player injury due to aggressive dunks. Powder-coated steel rim, competition net, and mounting hardware. Universal mounting back plate fits all glass backboards.
				1. Ages: 5-12. Material: Steel. Rim Thickness: 3/5 inches. Weight: 26 lbs.
			4. Grizzly Adjustable Basketball-Breakaway Goal: Model Number: 186SS.
			5. Official Aluminum Backboard: Model Number: 191SS.
			6. Offset Gooseneck Post, Aluminum backboard, Double Rim: Model: 194SS. Built to withstand extra-heavy use. A double rim, steel chain net, and a shooter's square.
				1. Ages: 5-12.
			7. 20 ft GaGa Ball Pit: Model: 2BY2GAGA20-IG.
				1. Comes with the Following: (31) 12 inch borders, (16) 34 inch spikes, (2) 6 inch end caps.
			8. 21 ft Welded Aluminum 3 Row Sideline Series: Model: 129-1214-4. Durable, lightweight, low-rise, portable aluminum bleachers. Built per IBC 2014 and ICC 300 building codes. Features: Single 2 x 10 inch footboards and 2 x 12 inch clear anodized seat planks.

\*\* NOTE TO SPECIFIER \*\* Delete understructure options not required.

* + - * 1. Understructure: Welded aluminum.
				2. Understructure: Aluminum tube angle understructure.
				3. Understructure: Heavy-duty galvanized steel understructure.
				4. Length: 21 ft. Weight: 286 lbs. Capacity: 42.
			1. 27 ft Welded Aluminum 3 Row Sideline Series: Model: 129-1214-5. Durable, lightweight, low-rise, portable aluminum bleachers. Built per IBC 2014 and ICC 300 building codes. Features: Single 2 x 10 inch footboards and 2 x 12 inch clear anodized seat planks.

\*\* NOTE TO SPECIFIER \*\* Delete understructure options not required.

* + - * 1. Understructure: Welded aluminum.
				2. Understructure: Aluminum tube angle understructure.
				3. Understructure: Heavy-duty galvanized steel understructure.
				4. Length: 27 ft. Weight: 366 lbs. Capacity: 54.
			1. High School Gooseneck Goal Posts (White): Model: 250SS.
			2. Football/Soccer Combo Goal: Model: 256SS.
			3. 26 ft GaGa Ball Pit: Model: 2BY2GAGA26-IG.
				1. Includes: (39) 12 inch borders, (20) 36 inch spikes, (2) 6 ft end caps
			4. Fence Guard: Model: 312SS/
			5. Foul Pole: Model: 313SS/
			6. Ryan Express Batting Cage: Model: 326SS. Dual coach observation platforms. Ricochet padding for overhead framework. Lockable dolly lift system for portability.
				1. Dimensions (WxDxH): 18 x 22 x 12 ft. Shipping Weight: 555 lbs.
			7. Pro Tunnel Nets: Model: 350SS. 100 percent waterproof and UV treated. Material: 2.5 mm No. 42 twisted knotted polyethylene. To be used with 353 Pro Tunnel Frames.
				1. Sizes: 70 x 14 x 12 ft, 70 x 12 x 12 ft, 55 x 14 x 14 ft, 55 x 14 x 12 ft, and 55 x 12 x 12 ft.
			8. Foldable, Portable Batting Cage: Model: 358SS.
			9. 7.5 ft Welded Aluminum 3 Row Sideline Series: Model: 129-1214-1. Durable, lightweight, low-rise, portable bleachers. All aluminum construction. Built per IBC 2014 and ICC 300 building codes. Features: Single 2 x 10 inch footboards and 2 x 12 inch clear anodized seat planks.

\*\* NOTE TO SPECIFIER \*\* Delete understructure options not required.

* + - * 1. Understructure: Welded aluminum.
				2. Understructure: Aluminum tube angle understructure.
				3. Understructure: Heavy-duty galvanized steel understructure.
				4. Length: 7.5 ft. Weight: 109 lbs. Capacity: 15.
			1. 9 ft Welded Aluminum 3 Row Sideline Series: Model: 129-1214-2. Durable, lightweight, low-rise, portable bleachers. All aluminum construction. Built per IBC 2014 and ICC 300 building codes. Features: Single 2 x 10 inch footboards and 2 x 12 inch clear anodized seat planks.

\*\* NOTE TO SPECIFIER \*\* Delete understructure options not required.

* + - * 1. Understructure: Welded aluminum.
				2. Understructure: Aluminum tube angle understructure.
				3. Understructure: Heavy-duty galvanized steel understructure.
				4. Length: 9 ft. Weight: 126 lbs. Capacity: 18.
			1. Single-Sided Basketball Scoreboard: Model: BB-2153. Displays: Period time to 99:59. HOME and GUEST scores to 199. PERIOD to nine. PLYR (player) number to 99. Player FOUL to nine. Team FLS (fouls) to 19 and indicates possession and bonus. T.O.L. (time outs left) to nine are optional. Electronic captions automatically change when volleyball and wrestling modes are selected.
				1. Sports Scored: Basketball, Volleyball, and Wrestling.
				2. Digit Sizes: 10, 7, 3 inches.
				3. Dimensions (H x W x D): 6 ft x 8 ft x 6 inches.
				4. Control: All Sports 5000 Wireless.
				5. Caption Options: Vinyl, Team Name Message Centers.
				6. Digit Colors: White, Mixed (Red, Amber).
				7. Digit Technology: Panaview.
				8. Construction: Durable lightweight aluminum Tuff Sport cabinet.
				9. Cabinet Color: 20 Standard Colors or Custom Pantone.
			2. Four-Sided LED Scoreboard: Model: BB-2154. Period Time Display: To 99:59. HOME and GUEST Scores: To 199. PERIOD: To 9. PLYR (player) Number: To 99. Player FOUL: To 9. Team FLS (fouls) to 19 and indicates possession and bonus. T.O.L. (time outs left) to 9 are optional. Electronic Captions: Change when basketball, volleyball and wrestling modes are selected.
				1. Sports: Basketball, Volleyball, and Wrestling.
				2. Digit Sizes: 10, 7, 3 inches.
				3. Dimensions (H x W x D): 6 ft 2 inches x 10 ft 10 inches x 10 ft 10 inches.
				4. Control: All Sports 5000
				5. Caption Options: Vinyl, Team Name Message Centers.
				6. Digit Colors: White or Mixed; Red and Amber.
				7. Digit Technology: PanaView.
				8. Construction: Durable, lightweight aluminum Tuff Sports cabinet.
				9. Cabinet Color: 20 Standard Colors or Custom Pantone.
			3. Single-Sided LED Scoreboard. Model BB-2155. Period Time Display: To 99:59. HOME and GUEST Scores: To 199. PERIOD: To 9. PLAYER Number: To 99. Player FOUL: To 9. Team FOULS: To 19. Time Outs Left (TOL): To 9. Indicates possession and bonus. Electronic Captions: Change when volleyball or wrestling modes are selected.
				1. Sports: Basketball, Volleyball, and Wrestling.
				2. Digit Sizes: 10 or 13 inches.
				3. Dimensions (H x W x D): 6 ft x 10 ft x 6 inches.
				4. Control: All Sports 5000.
				5. Digit Colors: White or Mixed; Red and Amber.
				6. Digit Technology: PanaView.
				7. Construction: Durable, lightweight aluminum Tuff Sports cabinet.
				8. Cabinet Color: 20 Standard Colors or Custom Pantone.
			4. Four-Sided LED Basketball Scoreboard: Model Number: BB-2156. Period Time Display: To 99:59. HOME and GUEST Scores: To 199. PERIOD: To 9. PLAYER Number: To 99. Player FOUL: To 9. Team FOULS: To 19. Time Outs Left (TOL): 9. Indicates possession and bonus. Electronic Captions: Change when basketball, volleyball, and wrestling modes are selected.
				1. Sports: Basketball, Volleyball, and Wrestling.
				2. Digit Sizes: 10 and 13 inches.
				3. Dimensions (H x W x D): 6 ft 2 inch x 12 ft 10 inch x 12 ft 10 inch.
				4. Control: All Sports 5000.
				5. Caption Options: Vinyl, Team Name Message Centers.
				6. Digit Colors: White or Mixed; Red and Amber.
				7. Digit Technology: PanaView.
				8. Construction: Durable, lightweight aluminum Tuff Sports cabinet.
				9. Cabinet Color: 20 Standard Colors or Custom Pantone.
			5. T-Rex Americana: Model Number: BA898AG. Breakaway Rim: Model BA3180S. Safe Play Area: At 10 ft: 96 inches.
				1. Glass Backboard Size: 42 x 72 inches.
				2. Beam Size: 6 inches square.
				3. Ballast Weight: 1100 lbs. Total Weight: 2686 lbs.
				4. Padded Base Dimension (WxL): 52 x 80 inches.

Base Color: Bright White.

Front Base Padding: 4 inch Thick Premium Sewn. Colors: 16.

* + - * 1. Wheels: Diameter: 8 inches. Width: 2 inches. Qty: 4 front and 4 rear.
				2. Stored Dimensions (WxLxH): 76 x 176 x 83 inches.
				3. Beam Padding.
				4. Backboard Padding. Colors: 17.
				5. Rear Hold Down and Deadlock Device.
				6. Front Levelers: Automatic.
				7. Floor Load Transport: Front: 330 lbs. Rear: 342 lbs.
				8. Floor Load Playing: Front: 535 lbs. Rear: 137 lbs.
				9. Minimum Required Floor Space Outside Court: 169 inches.
			1. T-Rex Club: Model BA894GSR. Breakaway Rim: BA35S. Satisfies programs looking for a spring-assisted portable system with full-size glass backboard and breakaway goal. The base is downsized. Factory-installed hidden ballast: 950 lbs. Tip-over stability without rear hold downs. Its lighter overall weight and size allow easier set up, tear down, transport, and storage. Safe Play Area: 10 ft: 54 inches.
				1. Glass Backboard Size: 42 x 72 inches.
				2. Beam Size: 4 inches square.
				3. Ballast Weight: 950 lbs. Total Weight: 1700 lbs.
				4. Padded Base Dimension (WxL): 40 x 65 inches.

Base Color: Bright White.

Base Padding: 2 inches Thick Stapled. Colors: 16.

* + - * 1. Wheels: Diameter: 8 inches. Width: 2 inches. Qty. Front: 2. Qty Rear: 2.
				2. Stored Dimensions (WxLxH): 76 x 124 x 78 inches.
				3. Beam Padding.
				4. Backboard Padding. Colors: 17.
				5. Rear Hold Down Optional.
				6. Front Levelers: Lead Screw.
				7. Floor Load Transport: N/A. Floor Load Playing: N/A.
				8. Minimum Required Floor Space Outside Court: 72 inches.
			1. T-Rex Competition. Model BA898G. Breakaway Rim: BA3180S. Safe Play Area: At 10 ft: 96 inches.
				1. Glass Backboard Size: 42 x 72 inches.
				2. Beam Size: 4 inches square.
				3. Ballast Weight: 1000 lbs. Total Weight: 2350 lbs.
				4. Padded Base Dimension (WxL): 40 x 74 inches.

Base Color: Bright White.

\*\* NOTE TO SPECIFIER \*\* Delete padding option not required.

Front Base Padding: 2 inch Thick Premium Sewn.

Front Base Padding: 4 inch thick on FIBA Models.

* + - * 1. Wheels: Diameter: 8 inches. Width: 2 inches. Qty: 2 front and 4 rear.
				2. Stored Dimensions (WxLxH): 76 x 160 x 78 inches.
				3. Beam Padding.
				4. Backboard Padding. Colors: 17.
				5. Rear Hold Down and Deadlock Device.
				6. Front Levelers: Automatic.
				7. Floor Load Transport: Front: 450 lbs. Rear: 725 lbs.
				8. Floor Load Playing: Front: 700 lbs. Rear: 475 lbs.
				9. Minimum Required Floor Space Outside Court: 130 inches.
			1. T-Rex International: Model: BA8910IG. Breakaway Rim: BA3180S. Safe Play Area at 10 ft: 128 inches.
				1. Glass Backboard Size: 42 x 72 inches.
				2. Beam Size: 6 inch square.
				3. Ballast Weight: 1500 lbs. Total Weight: 3228 lbs.
				4. Padded Base Dimension (WxL): 52 x 80 inches.

Base Color: Bright White.

Front Base Padding: 4 inch Thick Premium Sewn.

* + - * 1. Wheels: Diameter: 8 inches. Width: 2 inches. Qty: 4 front and 4 rear.
				2. Stored Dimensions (WxLxH): 76 x 204 x 83 inches.
				3. Beam Padding.
				4. Backboard Padding. Colors: 17.
				5. Rear Hold Down and Deadlock Device.
				6. Front Levelers: Automatic.
				7. Floor Load Transport: Front: 386 lbs. Rear: 421 lbs.
				8. Floor Load Playing: Front: 634 lbs. Rear: 173 lbs.
				9. Minimum Required Floor Space Outside Court: 202 inches.
			1. T-Rex Recreational: Model BA894USR for indoor. BA894USRO for outdoor. Breakaway Rim: BA35S. Safe Play Area: 10 ft: 54 inches. Identical to T-Rex Club except the backboard is 1/2 inch thick clear, polycarbonate. Locking device to eliminate unwanted and unsupervised raising and lowering of the basket.
				1. Outdoor Version: Substitutes OSB board as backing for base padding system.
				2. Polycarbonate Backboard Size: 42 x 72 inches.
				3. Beam Size: 4 inches square.
				4. Ballast Weight: 950 lbs. Total Weight: 14700 lbs.
				5. Padded Base Dimension (WxL): 40 x 65 inches.

Base Color: Bright White.

Base Padding: 2 inch Thick Stapled. Colors: 16.

* + - * 1. Wheels: Diameter: 8 inches. Width: 2 inches. Qty: 2 front and 2 rear.
				2. Stored Dimensions (WxLxH): 76 x 124 x 78 inches.
				3. Beam Padding.
				4. Backboard Padding.
				5. Rear Hold Down is Optional.
				6. Front Levelers: Lead Screw.
				7. Floor Load Transport: N/A.
				8. Floor Load Playing: N/A.
				9. Minimum. Required Floor Space Outside Court: 72 inches.
			1. T-Rex Slide Court. Model BA895G. Breakaway Rim Model BA35S. Safe Play Setback: 5-1/2 ft. Safe Play Area at 10 ft: 66 inches. Less storage room, and less space outside the court end line.
				1. Glass Backboard Size: 42 x 72 inches.
				2. Beam Size: 4 inches square.
				3. Ballast Weight: 800 lbs. Total Weight: 1900 lbs.
				4. Padded Base Dimension (WxL): 40 x 74 inches.

Base Color: Bright White.

Base Padding: 2 inch Thick Sewn. Colors: 16.

* + - * 1. Wheels: Diameter: 8 inches. Width: 2 inches. Qty: 2 front and 2 rear.
				2. Stored Dimensions (WxLxH): 76 x 130 x 78 inches.
				3. Beam Padding.
				4. Backboard Padding. Colors: 17.
				5. Rear Hold Down and Deadlock Device, both optional.
				6. Floor Load Transport: Front: 350 lbs. Rear: 600 lbs.
				7. Floor Load Playing: Front: 575 lbs. Rear: 375 lbs.
				8. Minimum. Required Floor Space Outside Court: 100 inches.

\*\* NOTE TO SPECIFIER \*\* Delete paragraph if not required, or delete items not required.

* + 1. Surfacing:
			1. Border Timbers: Model: 2BY240. Includes galvanized steel spike.
				1. Dimensions (LxWxH): 52 x 4 x 12 inches. Spike to Spike: 48 inches.
			2. Engineered Wood Fiber: Non-toxic and does not contain paint, chemicals, or additives. Contains minimal bark and is free of twigs, leaf debris, and other organic material.
			3. Evirofill: Acrylic-coated, round sand infused with Microban technology that is used as synthetic turf infill in landscape systems.
			4. Filler End Caps for Border Timbers: Model: 2BY2EC#. Two Sizes: 6 and 4 inches.
				1. Border Timber Filler End Caps are for 12 and 8 inch Border Timbers and all ramp systems. Made with recycled plastic.
			5. Galvanized Steel Spikes: Model: 2BY2STEEL##. For use with 12 and 8 inch Border Timbers, ADA ramps. Three Sizes: 28.5, 20, and 12 inch.
			6. Loose Fill Rubber Surfacing: Safe and affordable playground surfacing. Softer alternative to wood mulch. Properly maintained, it meets ASTM standards. Made from 100 percent recycled shredded rubber tires. Surface is clean, wire-free, non-toxic, and will not leach into groundwater. Drainage and weed-control accessories are available. Five different colors are available. High wear resistance and impact attenuation rating.
				1. Mold, animal, and insect resistant
			7. Nordot Turf Glue 34N-2: One-part, solvent-based urethanes with high "Green Strength" (grab, tack, grip) during installation, Superior water-resistance and proven long-term durability in climates worldwide after cure. Use year-round in sub-freezing cold to desert heat.
			8. Poured in Place Rubber: For colorful and customized surfacing. Poured onsite. Creatively combine colors and patterns to create graphical play areas that include game markings, graphics, or logos. Non-skid surface. Rubber is soft, durable, and low maintenance. Available in a variety of colors that can be mixed and matched.
			9. Recycled Bonded Rubber: Cean, recycled, shredded rubber coated and mixed with a polyurethane binder creating a unified and bonded surface that doesn't require refilling and maintenance like loose fill materials. Can be poured in one step. Allows water to flow through. Available in a variety of solid and blended colors.
			10. SurfaceMax Premium Recycled Rubber Tile Surfacing: A safe, soft surface material for indoor and outdoor applications. Available in a variety of thicknesses to ensure adequate impact attenuation for falls. Interlocking and non-interlocking tiles. Easy to maintain, replace, and install. Available in a variety of colors. ADA accessible ramp tiles and custom edging options are available.
			11. Synthetic Artificial Play Turf: Rolls: 15 ft wide x Length as ordered.
				1. A variety of pile heights and face weights available.
				2. Resilient material that offers a cooler play surface. Drains water. Available in a variety of colors. ADA accessible playground surfacing.
			12. Turf Seam Tape Adhesive seam tape to bond edges of artificial grass together. Engineered for sealing the seams in putting greens and over-concrete installations.

\*\* NOTE TO SPECIFIER \*\* Delete paragraph if not required, or delete items not required.

* + 1. Site Amenities:
			1. Classic Bike Bollard: Model 2633. Diameter: 6 and 8 inch. Height: 3 and 4 ft. Mounting: In-ground or surface. Finish: Powder coated in a variety of colors.
			2. Hamilton Table Tabletop: Model 30SM-5. Solid 36 inch round. Freestanding Seats: 24 inch vertical slatted. Seats available in quantities of 2, 3, or 4. Mounting: In-ground or vertical mount. Finish: Powder coating available in a variety of colors.
			3. Canopy Table: Model 320-P6. Permanent 6 ft picnic table with integrated canopy. providing a shaded seating area. Diamond perforations. Coating for Tabletop, Canopy and Seat Planks: UltraCoat thermoplastic. Supports and Framing: Powder coated in a variety of colors.
			4. Kensington Square Table: Model 40SM-S 46. Size: 46 inch square. Mounting: In-ground or surface mount. Tabletop: Rolled vertical slat. Seats: 4 seats fabricated from 1/4 inch steel plate with rolled slats. Finish: Powder coat in a variety of colors.
			5. Flare Bike Rack: Model 5030. Holds two bicycles. Mounting: In-ground or surface mount. Finish: Powder coat finish in a variety of colors.
			6. Contemporary Loop Bike Rack: Mounting: In-ground or surface mount. One piece. No assembly required. Finish: Hot-dipped galvanized or powder coat in a variety of colors.

\*\* NOTE TO SPECIFIER \*\* Delete model options not required.

* + - * 1. Model 5801. Loops: 1.
				2. Model 5803. Loops: 3.
				3. Model 5805. Loops: 5.
				4. Model 5807. Loops: 7.
				5. Model 5809. Loops: 9.
				6. Model 5811. Loops: 11.
				7. Model 5813. Loops: 13.
			1. 6 ft Basic Standard Bench without Back: Model: B6ULX. Frame: 2-3/8 inch black powder-coated. Glossy, thermoplastic seat in blue, red, green, and black. Seat Width: 10 inch. Seat Height: 17 inch.
				1. Mounting: Portable, Surface, or In-ground.
			2. DuraLight DualDrop High Capacity Cart: Model 60. Allows the most amount of room for collections while still being able to push it around comfortably on 4 inch casters.
			3. High Fire Ring with Adjustable Grate: Model: 612. An in-ground mounted 4 level adjustable cooking grate with cooling coil handles and a 300 square inch cooking area with a durable, high-temp, rust-resistant, back powder coat firebox. The Fire Ring only option and the ADA accessible double fire ring option is also available.
			4. Rotating Flip-Back Pedestal Grill: Model 616. Convenient flip-back grate. The 4 level adjustable cooking grate with cool-coil handles along with the full 360-degree rotation provides ease-of-use while operating the 280 square inches of cooking space. The high-temp black powder coated firebox is rust-resistant, ensuring longevity and durability in outdoor environments.
				1. Size (LxDxH): 20 x 14 x 8 inches. MIG welded 7 ga. base plate with 10 ga. side plates with an inground galvanized iron post mount. Available with an optional hot-dip galvanized firebox and utility shelf. ADA version is also available.
			5. Rotating Pedestal Grill: ADA: Yes. Model 620-630: 4 level adjustable cooking grate with cool-coil handles. 360 degree rotation. 280 square inches of cooking space. Firebox: High-temp black powder coated, rust-resistant, ensuring longevity and durability in outdoor environments. Lockable grill cover and utility shelf are available.
				1. Size (LxDxH): 20 x 14 x 8 inches. MIG welded 7 ga. base plate with 10 ga. side plates with an inground galvanized iron post mount. Available with an optional hot-dip galvanized firebox and utility shelf. ADA version is also available. Mounting: 2-3/8 inch O.D. inground post.
			6. Regal Accessible Rectangular Portable Table: Model: T#RCHDCP. Replace (#) with length desired. Default Length: 6 ft. ADA Accessibility Overhang: 24 inches.
				1. Frame: 2-3/8 inch powder-coated. Pre-drilled surface mount holes.
				2. Textured polyethylene table top and seats. Standard or centered seats.
				3. Anti-vandalism brace.
			7. Textilene Umbrella: Model 758A-75. Compatible with most thermoplastic round and square tables. Tilt: 3-position. Select manual or crank lift. A variety of color choices, or alternating colors. Post Diameter: 1-5/8 inch O.D.
				1. Material: 7-1/2 ft Grade A Open Weave or Grade B Closed Weave.
			8. 8 ft Basic Standard Bench without Back:

\*\* NOTE TO SPECIFIER \*\* Delete model options not required.

* + - * 1. Model B8ULP: 8 ft UltraLeisure Bench without Back, Portable.
				2. Model B8ULS: 8 ft UltraLeisure Bench without Back, In-Ground Mount.
				3. Model B8ULSM: 8 ft UltraLeisure Bench without Back, Surface Mount.
				4. Frame: 2-3/8 inch black powder-coated. Seat Width x Height: 10 x 17 inches.
				5. Material: Glossy, thermoplastic seat available in blue, red, green, and black.
			1. Straight Bench: Model 800-VS3. Available in two or three individual seat sections. When placed side-by-side, the individual seat sections can be used to create straight or oval seat configurations. Available with or without backs. Comes with perforated, diamond or rod pattern options. Finish: Thermoplastic. Frame: Powder coated. Comes in a variety of colors.
			2. Convex Bench: Model 830/730. A semi-circle seating arrangement with 30 degree angle between seats. Mounting: Portable, In-Ground, or Surface. Diamond or perforated patterns. Finish: Thermoplastic. Frame: Powder coated. Comes in a variety of colors. Backless is also available.
			3. Oxford Bench without Back: Model 85-S6. Lengths: 4 and 6 inches. A variety of colors. Finish: UltraCoat thermoplastic. Mounting: Portable or surface. Fully-welded with 7 ga steel seat and 3/8 inch steel plate legs. Ships fully assembled.
			4. 8 ft Regal Accessible Rectangular Portable Table: Model: T#RCHDCP-1. Replace (#) with length desired. Default Length: 8 ft. Frame: 2-3/8 inch, powder-coated. Pre-drilled surface mount holes. ADA Accessibility Overhang: 24 inches.
				1. Table Top and Seats: Textured polyethylene. Seats: Standard or centered.
				2. Includes anti-vandalism brace.
			5. Extra-Heavy Duty Bench without Back: Model 942-V10. Mounting: Portable, inground, surface, or wall. Available in 6, 8, 10, and 15 inches. Frame-only available. Finish: Thermoplastic with powder coated frames. Available in a variety of colors and patterns. Diamond and perforated roll pattern are available in lengths 6 and 8 inches.
			6. Charleston Recycled Bench with Back: Model 964-BRN6. Lengths: 6 and 8 ft. Manufactured with recycled plank seating and decorative 1-1/2 inch aluminum cast frame. Finish: Thermoplastic. Available in a variety of colors. Mounting: Portable or surface mounted.
			7. 974-s4 Wilmington Bench: High-arching arms. Choice of vertical or horizontal slats. The MIG welded cast aluminum frame is powder coated and available in a variety of colors. Safe mount stainless steel hardware included.
			8. Basic Round Pedestal Table: UltraLeisure Model: T46RACSPEC. Glossy, thermoplastic table top and seats available in blue, red ,green, and black.
				1. Table Top: 46 inch diameter with umbrella hole. Seats: 3 to 4.
				2. Frame: Heavy-duty 4 inch square black powder-coated. Mounting: In-ground.
			9. Basic Round Pedestal Table: UltraLeisure Model: T46RACSPED-3S. Glossy, thermoplastic table top and seats available in blue, red, green, and black.
				1. Table Top: 46 inch diameter with umbrella hole. Seats: 3. Wheelchair Accessible.
				2. Frame: Heavy-duty 4 inch square black powder-coated. Mounting: In-ground.
			10. Basic Round Pedestal Table. UltraLeisure Model: T46RACSPEDSM. Glossy, thermoplastic table top and seats available in blue, red, green, and black.
				1. Table Top: 46 inch diameter with umbrella hole. Seats: 3 to 4.
				2. Frame: Heavy-duty 4 inch square black powder-coated. Mounting: Surface.
			11. Basic Standard Bench with Back: Model: B#WBUL.
			12. Basic Metal Trash Receptacle: UltraLeisure Model: TR32UL. Glossy, thermoplastic coating available in blue, red, green, and black. Capacity: 32-gallon. Lid and liner.
				1. Mounting: Surface and in-ground.
			13. Bollard Plastic Covers: 6 year manufacturer Anti-Fade Warranty. Self-adhesive foam strips are included for slip-on installation. Choose from a variety of colors.
			14. Buddy Bench: Model: B6WBPERFP-BB. Colored backing plate is optional.
			15. Classic Swing Door Receptacle: Model: CL-36FT. Features a convenient swing door with latch for access to the 36 gallon receptacle liner. Powder coat finish comes in a variety of colors. Multiple lid options, including the flat top, ash urn, and rain bonnet..
				1. Hardware: Stainless-steel for portable or surface mount.
			16. CollectionPoint 24 inch Outdoor Recycling Receptacle:
			17. CollectionPoint 24 inch Trash Container: Trash receptacles by Kingsley.
			18. Drive Up Book Returns, C Series System: Specifically for curbside vehicle returns from cars, trucks, and SUVs. Also used for ADA compliant walk-ups when properly installed. Extra security, safety, and convenience features.
			19. Drive Up Book Returns: C Series Supermax DualDrop: 70 C and 80 C Series are only available in the Supermax DualDrop model. Specifically for curbside vehicle returns from cars, trucks, and SUVs. Also used for ADA compliant walk-ups when properly installed. Extra security, safety, and convenience features.
			20. High Capacity Carts: With 4 inch diameter wheels to allow the most amount of room for collections while still being able to push it around comfortably.
			21. Receptacle Mounting Kits: Model: IG KIT. All trash receptacles are portable and can be converted into either inground (IG) or surface mount (SM). Kits fit 32, 36 (IG only), and 55 gallon receptacles.
				1. 2-3/8 inch O.D. all MIG welded pipe. Powder-coated black.
			22. Integrated Bench Shade: Model: STS765BA. Attaches to Standard Benches With Backs. Available for in-ground or surfacing mounting options.
			23. K-Series KwikDrop Outdoor Depository: 70K and 80K Series are only available in the Supermax model. Accept More Than Books: Wide mouth depository for large reference materials, bulk deposits of multiple books, magazines, packages, and donations.
			24. Dual Lexington Trash Receptacle: Model: LX-72FT.Holds two 32 gallon liners and lids. Smooth, vertical slats coordinate with many of our benches, seats, and tables. Finish: Powder coat comes in a variety of colors with multiple lettering and decal options, including "Cans", "Plastics", "Trash", and "Recycle". Hardware: Stainless-steel. Mounting: Portable and/or surface mount.
			25. PL-Receptacle Liner: Model: LINER55. Heavy-duty black plastic liner fits most 32 and 55 gallon trash receptacles. Finish: Thermoplastic.

\*\* NOTE TO SPECIFIER \*\* Delete can size option not required.

* + - * 1. 32-Gallon: 21-7/8 inches wide x 27-1/2 inches tall.
				2. 55-Gallon: 23-3/8 inches wide x 31-3/8 inches tall.
			1. Portable Casino Bench with Back: Legs and Arms: 1-1/2 inch square textured polyethylene. Seat and Contoured Seat Back: Textured polyethylene. Seat Height: 15-1/2 inches. Pre-drilled holes for optional surface mounting.
				1. Custom center armrest, optional.
			2. Rainier Bench with Back: Model: B#WBRN. High arching armrests. Crafted of steel with cast aluminum frame; fully welded. Lengths: 6 or 8 ft lengths. Finish: Choice of powder coat color. Slats: Vertical. Combined portable/surface mount frame with pre-drilled surface mount holes.
			3. Rectangular Portable Table: Frame: 2-3/8 inch powder-coated with pre-drilled surface mount holes.. Table Top and Seats: Textured polyethylene, with or without seat backs.
			4. Round Portable Cafe Table: Model Number: T36round. Commercial-grade table for outdoor use seating up to four people. Diameter: 36 or 46 inches. Tabletop: Expanded metal, textured polyethylene coated finish, resists rust, corrosion, and fading from UV rays. Includes Hole for Umbrella. Frame: 1-5/8 inch Steel, powder-coated.
			5. Round Portable Table: Model T46ULRACS. Frame: 1-5/8 inch, powder-coated, with pre-drilled surface mount holes. Table Top and Seats: Textured polyethylene. Diameter: 46 inches with umbrella hole. Top: solid or expanded metal.
			6. Post Mounted Sanitizer/Receptacle: Model SANT01: Outdoor hand sanitation. 20 ga aluminum locking enclosures. Dispenser: Pump, lever, or automatic touchless.
				1. Usage instructions: In English and Spanish.
				2. Attached receptacle: Available.
				3. Finish: Can customize post and box colors.
				4. Sanitizer: Not included.
			7. Post Mounted Sanitizer and Receptacle, Surface Mount: Model SANT01SM: Locking Enclosure: 20-gauge aluminum. Dispenser: Pump, lever, or automatic touchless.
				1. Usage Instructions: In English and Spanish.
				2. Attached receptacle available.
				3. Finish: Can customize post and box colors.
				4. Sanitizer: Not included.
			8. Post Mounted Sanitizer: Model: SANT02. Outdoor hand sanitation. 20 ga aluminum locking enclosures. Dispenser: Pump, lever, or automatic touchless.
				1. Usage Instructions: In English and Spanish.
				2. Attached Receptacle: Available.
				3. Finish: Can customize post and box colors.
				4. Sanitizer: Not included.
			9. Post Mounted Sanitizers, Surface Mount: SANT02SM. Outdoor hand sanitation. 20 gauge aluminum locking enclosures. Pump, lever, or automatic touchless.
				1. Usage Instructions: In English and Spanish.
				2. Attached Receptacle: Available.
				3. Finish: Can customize post and box colors.
				4. Sanitizer: Not included.
			10. Post Mounted Automatic Holder: Model: SANT04. Outdoor hand sanitation. 20 gauge aluminum locking enclosures. Pump, lever, or automatic touchless.
				1. Usage Instructions: In English and Spanish.
				2. Attached Receptacle: Available.
				3. Finish: Can customize post and box colors.
				4. Sanitizer: Not included.
			11. Post Mounted Automatic Holder, Surface Mount: Model: SANT04SM. Outdoor hand sanitation. 20 gauge aluminum locking enclosures. Pump, lever, or automatic touchless.
				1. Usage Instructions: In English and Spanish.
				2. Attached Receptacle: Available.
				3. Finish: Can customize post and box colors.
				4. Sanitizer: Not included.
			12. Post Mounted Automatic Holder and Receptacle: Model: SANT05. Outdoor hand sanitation. 20 gauge aluminum locking enclosures. Pump, lever, or automatic touchless.
				1. Usage Instructions: In English and Spanish.
				2. Attached Receptacle: Available.
				3. Finish: Can customize post and box colors.
				4. Sanitizer: Not included.
			13. Post Mounted Automatic Holder and Receptacle, Surface Mount: Model SANT05SM Outdoor hand sanitation. 20 gauge aluminum locking enclosures. Pump, lever, or automatic touchless.
				1. Usage Instructions: In English and Spanish.
				2. Attached Receptacle: Available.
				3. Finish: Can customize post and box colors.
				4. Sanitizer: Not included.
			14. Seat Portable: Model: SF-133.
			15. Seat Surface Mount: Model: SF-134.
			16. Standard Picnic Table: Model: SF-169.
			17. Single Ped Table 46 inch Ingr: Model: SF-173.
			18. Single Ped Table Ada Ingr: Model: SF-174.
			19. Single Ped Table 46 inch Smt: Model: SF-175.
			20. Single Ped Table Ada Smt: Model: SF-176.
			21. 46 inch Square Web Table: Model: T46WEBS. Fream: 2-3/8 powder-coated. Standard umbrella hole. Mounting: Surface or in-ground.
				1. Finish: Textured polyethylene table top and seats.
			22. 6 ft Basic Standard Bench with Back: UltraLeisure Model: B6WBULP.
			23. 6 ft Standard Bench with Back, Portable: UltraLeisure Model: B6WBULS.
			24. 6ft Standard Bench with Back, In-Ground Mount: UltraLeisure Model: B6WBULSM.
			25. 6ft Standard Bench with Back, Surface Mount: UltraLeisure. Glossy, thermoplastic back and seat available in blue, red, green, and black. Frame: 2-3/8 inch black powder-coated. Seat Width: 10 inches. Seat Height: 17 inches.
				1. Mounting: Portable, Surface, or In-ground.
			26. Standard Trash Receptacle: Model Number: TR##. Finish: Textured polyethylene coated. Capacity: 32 and 55 gallon. Lid and liner available but not included.
				1. Mounting: Surface and in-ground.
			27. UltraLeisure Rectangular Portable Table: Model: T#UL. Extra Heavy-Duty Rectangular Table. Diamond and Perforated Rolled Edges. Finish: Choice of 22 powder coat frame and 8 UltraCoat planking colors,
				1. Mounting: Portable and/or surface mounted. Lengths: 6 and 8 ft.
			28. Walk Up Book Return: Model: S-Series. ADA compliant. Can be put on the curb and used for drive-ups.
			29. Walk Up Book Return. Model 70 S-Series. DualDrop Each side can hold 380 standard size (6 x 9 inch) books or 950 media cases for a combined total of 760 standard size (6x9 inch) books or 1900 media cases. Label one side for books and one for media.
			30. Wave Bike Rack, 3-Hump: Model: MSBR3-SM. Mounting: In-ground or surface. An all-in-one piece, no assembly required, with 5 loops. Finish: Hot-dipped galvanized or powder coat in a variety of colors.

\*\* NOTE TO SPECIFIER \*\* Delete paragraph if not required, or delete items not required.

* + 1. Fitness Equipment:
			1. Cardio Walker: Model: UP164SM. Users stand upright and alternate their legs in a striding, smooth motion. Aerobic, muscle, and core fitness, and balance/flexibility. Extra wide handle bar allows for comfortable grip and provides support. Steel construction with rust resistant coating. Heavy duty, vandal resistant housings.
				1. Ages: 13 and Up.
			2. ActionFit Compact Course: Model: UP198. Efficiently addresses muscle fitness and core. Available in in-ground mount only. Traditional color options.
				1. Ages: 13 and Up.
				2. Minimum Area: 350 sq ft. Weight: 1102 lbs.
			3. Overhead Ladder: Model: UP199. An intense upper body and core workout. Step-up provides an extra boost for those who need assistance reaching the bars. Modern design. Metallic and black color scheme similar to indoor fitness equipment. Steel construction. Rust resistant coating. Available in in-ground mount.
				1. Ages: 13 and Up.
			4. Hand Cycle: Model: UP216S. A nylon seat and ergonomically designed handholds for an aerobic and muscle upper body workout. A magnetic resistance mechanism provides smooth and balanced exercise. Meets ASTM standards for outdoor fitness equipment.
				1. Ages: 13 and Up.
			5. Hand Cycle Accessible: Model: UP2175. Ergonomically designed handholds provide easy grip for an aerobic upper body and workout. A magnetic resistance mechanism provides smooth and balanced exercise. ADA version excludes a seat to allow for a user of a mobility device easy access and comfort. Meets ASTM standards for outdoor fitness equipment.
				1. Ages: 13 and Up.
			6. Combination Hub: Model: UP221S. Four fitness configurations for upper and lower body while promoting core strength, endurance, and grip strength. Includes variations of Chin-Up Station, Push-Up Station, and a Horizontal Chin-Up Station.
				1. Ages: 13 and Up.
			7. Push Up Station Combo: Model: UP222S. A strength workout at two height variations for upper body. Hand grip curvatures offer multiple grip positions to vary workout and challenge levels.
				1. Ages: 13 and Up.
			8. Push Up Station, Low: Model: UP223S. For enhancing upper body strength. Hand grip curvatures offer multiple grip positions to vary workout and challenge levels.
				1. Ages: 13 and Up.
			9. Push Up Station, High: Model: UP224S. For enhancing upper body strength. Hand grip curvatures offer multiple grip positions to vary workout and challenge levels.
				1. Ages: 13 and Up.
			10. T Bar Station: Model: UP256. Provides a full body strength work-out as the user slowly moves through plank positions. Freestanding instructional sign included. Available as in-ground mount only.
				1. Ages: 13 and Up. Dimensions: 50 x 4 x 27 inches. Minimum Sq Ft: 1
			11. Knee Lift Station: Model: UP257, Encourages balance and flexibility as the user must lift their knees to waist level and hold for a count. Available as in-ground mount only.
				1. Ages: 13 and Up. Dimensions: 30 x 30 x 91 inches. Minimum Area: 6 sq ft.
			12. Vault Bar Station: Model: UP258. Builds muscle strength. User must grasp one end for support and hop from side to side. Advanced users can jump over the bar for more challenge. Freestanding instructional sign. Available as in-ground mount only.
				1. Age: 13 and up. Dimensions: 111 x 3 x 52 inches. Minimum Area: 2 sq ft.
			13. Traditional Horizontal Chin-Up Station: Model: UP259. Encourages muscle strength in the upper body, arms, back, and abdominals. Available as in-ground mount only.
				1. Age: 13 and up. Dimensions: 96 x 43 x 56 inch. Minimum Area: 29 sq ft.
			14. Joint Use Pull Bar Station: Model: UP261. Allows users to work on upper body strength. Three bars at different heights. Available as in-ground mount only.
				1. Age: 13 and up. Dimensions: 126 x 4 x 86 inches. Minimum Area: 4 sq ft.
			15. Body Curl Station: Model: UP262. Traditional core exercise. User lays on their back and grasps the bar with both hands. Core engages as user lifts their heels off of the bench. Freestanding instructional sign included. Available as in-ground mount only.
				1. Age: 13 and up. Dimensions: 84 x 16 x 34 inches. Minimum Area: 9 sq ft.
			16. Parallel Bar Station: Model UP263. User must grasp both bars and use their upper and lower body to raise their body until arms are straight. Freestanding instructional sign included. Available as in-ground mount only.
				1. Age: 13 and up. Dimensions: 119 x 22 x 46 inches. Minimum Area: 18 sq ft.
			17. Step Up Station Model UP264. An aerobic activity, user steps up and down engaging the lower body and increasing their heart rate. Freestanding instructional sign included. Available as in-ground mount only
				1. Age: 13 and up. Dimensions: 36 x 20 x 40 inches. Minimum Area: 5 sq ft.
			18. ActionFit Endurance Course: Model UP307S. A Cardio Walker and series of Plyometric Boxes. Addresses all four fitness elements: aerobic, muscle fitness, balance/flexibility, and core. 10 piece pre-configured outdoor fitness package.
				1. Minimum Area: 900 sq ft. Weight: 1197 lbs. Age: 13 and up.
			19. ActionFit Performance Course: Model UP312S. Fitness Line: FitTech Packages
				1. Color Options: ActionFit. Age: 13 and up. Weight: 1292 lbs.
			20. ActionFit Training Course: Model UP314S. Features 6 FitTech products which focus on all four fitness elements, aerobic, muscle fitness, balance/flexibility, and core.
				1. Age: 13 and up. Minimum Sq Ft: 625. Weight: 902 lbs.

\*\* NOTE TO SPECIFIER \*\* Delete paragraph if not required, or delete items not required.

* + 1. VersaCourt:
			1. VersaCourt: Court system. An outdoor/ indoor athletic surface of interlocking copolymer tiles. Durable and safe playing surface for sports and activities. A forgiving playing surface reduces body stress without sacrificing action.
				1. Suitable for: Basketball, Tennis, Soccer, Futsal, Shuffleboard, Volleyball, Pickleball, Multi-game courts, Portable Courts, Playground Surfacing, Roller Derby, and Inline Hockey.
			2. Active Court Tile: For building courts on driveways or parking areas. Tiles measure 15-3/4 inch squared and withstand 60,000 lbs of rollover weight. Two-tone, checkerboard appearance and flat surface. Ideal for outdoor volleyball and many multi-purpose courts such as: Basketball, Volleyball, Shuffleboard, and Multi Sport Game Courts
			3. Boost Outdoor Tile: Durable, safe, and functional game court for commercial spaces. Made from specially blended, high-impact, copolymer polypropylene that lasts for years. Applications: Basketball, Shuffleboard, and Multi Sports Game Court.
			4. Compete Indoor Tile: Safe, durable, high-performance indoor sports surfacing system for a wide variety of activities. Requires little to no maintenance. Applications Include: Volleyball, Basketball, Tennis, and Multi-Sport Game Court.
			5. VersaCourt Game Outdoor Court Tile: Designed and developed for outdoor multi-sport applications. Tile design and six-point locking system creates a seamless playing surface allowing consistent ball bounce, response, and playability.
				1. Recommended Applications: Basketball, Pickleball, Futsal, Tennis, Shuffleboard, and Multi-Sport Game Court.
			6. VersaCourt Pro Indoor Court Tile: For indoor multi-sports applications. The tile design and six-point locking system creates a seamless playing surface allowing consistent ball bounce, response, and playability.
				1. Recommended Applications: Basketball, Futsal, Volleyball, Multi-Sport Game Court.
			7. Speed Outdoor Tile: VersaCourt Speed Outdoor court tile for outdoor inline hockey, roller sports, and multi-sport applications. Design offers wheel grip and excellent traction for multi-sport activities.

\*\* NOTE TO SPECIFIER \*\* Delete paragraph if not required, or delete items not required.

* + 1. Swings:
			1. Spinning Seat: Model 68156. Proprioceptive movement experiences. Encourages cooperation. Supportive seats and handles to help users sustain engagement.
				1. Ages: 2-5 and 5-12. Weight: 75 lbs.
			2. Arch Swing Frame: Constructed from 3.5 inches diameter steel and stands 8 ft tall.
				1. Seats: Belt, bucket, and tire for all ages and in a variety of colors.
				2. Four bay options and an add-a-bay option to ensure you have an available option for any number of children.
				3. Fall Height: 8 ft. Use Zone: Starts at 24 x 32 ft. (Varies Based on Bay Count).
				4. Age Range: All ages, Dependent Upon Seat Style.
				5. Post Diameter: 3.5 and 5 inch.
			3. Arch Tire Swing Frame: Made from 5 inch steel tubing.
			4. Molded Belt Seat: Galvanized triangle hardware and high carbon steel spring inserts to resist vandalism. Available in red, yellow, green, blue, black, and tan. Galvanized or Yellow PVC coated chain is available. Sold as a set of two.
				1. Model Number: 90015108XX. Ages: 5-12.
			5. Bucket Seats: High backs and full stainless steel inserts. For ages 24 to 47 months. 54 inch chain in red, yellow, green, blue, or black. Sold as a set of two.
				1. Model Number: 90015130XX. Ages: 24 to 47 months.
			6. Inclusive Swing: Model: BSIS-25. For children who need support to maintain a seated position. Each seat comes with galvanized chain. Available in any rotomolded plastic color with a yellow or beige brace. Ages: 2-12 years.
			7. Painted 10 ft Tripod Swing Add-A-Bay. Model: P68033. 3-1/2 inch upright posts and swing beam. Swings sold separately. Ages: 2-5 and 5-12. Weight: 151 lbs
			8. See Me Swing: Model: TFR0662XX. Tandem-mounted swing allows parents and other family members to swing face-to-face with a toddler. A sturdy welded and powder-coated frame. Customizable colors. Age Group: 24-47 months.
			9. Single Post Swing Frames Constructed from 5 inch (without shade) or 6-5/8 inch (with shade) diameter steel. Frames Height: 8 ft. Shade Version: IPEMA Certified and ASTM F1487-17 Compliant. Swing Seats and Swing Chain Sold Separately.
			10. Standard Bi-Pod Swing Frames: Constructed from 2-3/8 inch galvanized steel tubing with cast aluminum junctions. Height: 8 or 10 ft.
			11. Tire Swing: Model TFR0612XX. One Tire: Surable, black roto-molded plastic. Steel Chain and Hardware: Galvanized.
			12. Tri-Pod Swing:
				1. Galvanized 8 ft: Model 90015108XX.
				2. Galvanized 10 ft: Model 90015110XX.
				3. Yellow PVC 8 ft: Model 90015208XX.
				4. Yellow PVC 10 ft: 90015210XX.

\*\* NOTE TO SPECIFIER \*\* Delete paragraph if not required, or delete items not required.

* + 1. Dog Parks:
			1. Classic Dog Park Bench: Model B6WBCLASSIC.
				1. Length: 6 ft. Design: Paws or bone. Seat Back: Contoured.
				2. Frame: Cast aluminum, powder coated. Portable with pre-drilled holes for surface mounting.
				3. Finish: Textured polyethylene seat and seat backs.
			2. Classic Wingline Dog Park Bench: Model B6WBCLASSICWINGLINE#-1.
				1. Length: 6 ft. Design: Paws or bone. Seat Back and Arm Rests: Contoured.
				2. Frame: Heavy-duty 2-3/8 inch aluminum, powder coated.
				3. Mounting: Portable, Surface, and In-ground.
				4. Finish: Textured polyethylene seat and seat back.
				5. Seat height: 18 inches.
			3. Standard Dog Park Bench: Model B6WBUL#-1.
				1. Length: 6 ft. Design: Paws or bone. Seat Back and Arm Rests: Contoured.
				2. Frame: Heavy-duty 2-3/8 inch aluminum, powder coated.
				3. Mounting: Portable, Surface, and In-ground.
				4. Finish: Textured polyethylene seat and seat back
				5. Seat Height: 17 inches. Seat Width: 10 inches.
			4. Camel Hump Climber: Model RECF0001XX.
				1. Dimensions (WxHxD): 11 ft 7-1/2 inches x 24-3/4 inches x 16 inches. Weight: 269 lbs.
			5. Custom Logo, Emblem, or Insignia Amenities:
				1. Add logo, emblem, insignia, or theme to market your dog park. We offer lettering from our selection of fonts, as well as more intricate designs.
				2. Upcharge per piece
				3. Powder coated backing plates are available for an additional charge
				4. Customization available on most products
			6. Dog Park Trash Receptacle: Model TR32-1.
				1. Capacity: 32 gal. Design: Paws or bone. Mounting: Surface and in-ground options. Coating: Textured polyethylene. Lid and liner.
			7. Home Sweet Home: Model RECF0010XX.
				1. Dimensions (W x H): 36 x 65-3/8 x 47 inches. Weight: 416 lbs.
			8. Hurdle Jump: Model RECF0007XX.
				1. Dimensions (W x H): 24 x 5-11/16 inches. Weight: 68 lbs
			9. Over and Under: Model RECF0012XX.
				1. Dimensions (W x H): 42-1/2 x 34-1/2 inches. Weight: 109 lbs.
			10. Pet and Owner Drinking Fountain: Model BSW-0007XX. Meets ADA requirements.
				1. Stainless steel. Push-button mechanism. Anti-rotation non-squirt bubbler.
			11. Pet Only Drinking Fountain: Model BSW-0010XX.
				1. Stainless steel. Push-button mechanism. Anti-rotation non-squirt bubbler.
			12. Pup Turf: Safe for the environment, humans, and pets.
				1. Extra strength against wear from paws and claws.
				2. Envirofill Microban Protection to help fight the spread of bacteria.
				3. Perforated turf layer provides for rapid drainage.
				4. Odors easily flush away with water.
				5. Shades and shelters.

\*\* NOTE TO SPECIFIER \*\* Delete paragraph if not required, or delete items not required.

* + 1. Shades and Shelters:
			1. 2-Tier Gable: Rectangular design. Provides protection from the elements with an open-air atmosphere. Roof Pitch: 4:12. Available in a variety of colors. Can be designed to meet specific local codes. Size (WxL): Up to 30 x 44 ft in 1 ft increments.
				1. Humidity Resistance, ASTM D2247-D2: 5,000 hrs. No blistering or adhesion loss. Color/UV Resistance, ASTM G154-04: 2,000 hrs exposure. No chalking. Roofing Panel Protection: Kynar 500 coating. Structural Steel Tubing: ASTM A500 Grade B. Plates: A36 steel. Welds: By AWS welders.
			2. 1 or 2-Tier Hexagon Shelters: Traditional six-column frame. Roof Pitch: 6:12.
				1. Size: Available in 1 ft increments up to 30 ft in diameter. Available in a variety of colors. Can be designed to meet specific local codes.
				2. Humidity Resistance, ASTM D2247-D2: 5,000 hrs. No blistering or adhesion loss. Color/UV Resistance, ASTM G154-04: 2,000 hrs exposure. No chalking. Roofing Panel Protection: Kynar 500 coating. Structural Steel Tubing: ASTM A500 Grade B. Plates: A36 steel. Welds: By AWS welders.
			3. 2-Tier Square Shelter: Roof Pitch: 6:12. Size: Available in 1 ft increments up to 30 ft. Available in a variety of colors. Can be designed to meet specific local codes.
				1. Humidity Resistance, ASTM D2247-D2: 5,000 hrs. No blistering or adhesion loss. Color/UV Resistance, ASTM G154-04: 2,000 hrs exposure. No chalking. Roofing Panel Protection: Kynar 500 coating. Structural Steel Tubing: ASTM A500 Grade B. Plates: A36 steel. Welds: By AWS welders.
			4. Custom Sails Shade Canopies: Available in a variety of colors. Can be designed to meet specific local codes.
				1. Withstands 5 psf snow load and wind gusts up to 90 mph (ASCE-7) with fabric intact. Up to 150 mph wind gusts with fabric removed.

Zinc rich primer: 1-2 mil thickness.

Polyester Powder Coat: oven baked to a 2-4 mil thickness.

* + - 1. Dual Column Freestanding Umbrella Shade: Heights: 8 and 10 ft.
				1. Sizes: 16 x 12 ft, 18 x 12 ft, 20 x 10 ft, 20 x 12 ft, and 24 x 14 ft.
			2. Freestanding Hanging Cantilever Shade:
				1. Heights: 8 ft. Sizes: 20 x10 ft, 20 x12 ft, and 24 x12 ft.
			3. Freestanding Hexagon Shade: With six column uprights.
				1. Heights: 8, 10, and 12 ft. Sizes: From 20 to 40 ft. Weight: 600 lbs.
			4. Freestanding Hexagon Single Column Umbrella Shade:
				1. Heights: 8 and 10 feet. Sizes: 10 to 27 ft. Weight: 600 lbs.
			5. Freestanding Rectangular Four Column Shade:
				1. Heights: 8, 10, and 12 ft.
				2. Sizes: 10 x 15 ft, 10 x 20 ft, 13 x 15 ft, 13 x 20 ft, 15 x 25 ft, 18 x 24 ft, 18 x 28 ft, 18 x 32 ft, 18 x 36 ft, 20 x 26 ft, 20 x 30 ft, 20 x 34 ft, 20 x 38 ft, 24 x 30 ft, 24 x 34 ft, 24 x 38 ft, 24 x 40 ft, 28 x 34 ft, and 28 x 38 ft. Weight: 600 lbs.
			6. Freestanding Square Four Column Shade:
				1. Heights: 8, 10, and 12 ft. Limited sizes available in 14 ft height.
				2. Sizes: 10 x 10 ft up to 30 x 30 ft. Weight: 600 lbs.
			7. Freestanding Square Umbrella Shade:
				1. Heights: 8 and 10 ft.
				2. Sizes: 10 x 10 ft, 12 x 12 ft, 14 x 14 ft, 16 x 16 ft, 18 x 18 ft, 20 x 20 ft, 22 x 22 ft, and 24 x 24 ft. Weight: 600 lbs.
			8. Gable: Provides open-air atmosphere and protection from the elements.
				1. Roof Pitch: 4:12. Size (WxL): 1 ft increments up to 30 x 84 ft.
				2. Available in a variety of colors. Can be designed to meet specific local codes.
				3. Humidity Resistance, ASTM D2247-D2: 5,000 hrs. No blistering or adhesion loss. Color/UV Resistance, ASTM G154-04: 2,000 hrs exposure. No chalking. Roofing Panel Protection: Kynar 500 coating. Structural Steel Tubing: ASTM A500 Grade B. Plates: A36 steel. Welds: By AWS welders.
			9. Hexagon: 1 or 2 tiers. Traditional six-column frame.
				1. Roof Pitch: 6:12. Size: 1 ft increments up to 30 ft in diameter.
				2. Available in a variety of colors. Can be designed to meet specific local codes.
				3. Humidity Resistance, ASTM D2247-D2: 5,000 hrs. No blistering or adhesion loss. Color/UV Resistance, ASTM G154-04: 2,000 hrs exposure. No chalking. Roofing Panel Protection: Kynar 500 coating. Structural Steel Tubing: ASTM A500 Grade B. Plates: A36 steel. Welds: By AWS welders.
			10. Hexagon Shade: Traditional 6 column frame with a fabric top. Available in a variety of colors. Can be designed to meet specific local codes.
				1. Withstands 5 psf snow load and wind gusts up to 90 mph (ASCE-7) with fabric intact. Up to 150 mph wind gusts with fabric removed.

Zinc rich primer: 1-2 mil thickness.

Polyester Powder Coat: oven baked to a 2-4 mil thickness.

* + - 1. Hip Rectangle Shelters: For any open outdoor area.
				1. Roof pitch: 4:12. Size (WxL): 1 ft increments up to 30 x 84 ft.
				2. Available in a variety of colors. Can be designed to meet specific local codes.
				3. 4Humidity Resistance, ASTM D2247-D2: 5,000 hrs. No blistering or adhesion loss. Color/UV Resistance, ASTM G154-04: 2,000 hrs exposure. No chalking. Roofing Panel Protection: Kynar 500 coating. Structural Steel Tubing: ASTM A500 Grade B. Plates: A36 steel. Welds: By AWS welders.
			2. Hip Rectangular Double Dome Shade: For parks and large spaces. Available in a variety of colors. Can be designed to meet specific local codes.
				1. Withstands 5 psf snow load and wind gusts up to 90 mph (ASCE-7) with fabric intact. Up to 150 mph wind gusts with fabric removed.

Zinc rich primer: 1-2 mil thickness.

Polyester Powder Coat: oven baked to a 2-4 mil thickness.

* + - 1. Hyper Rectangular Sail: Available in a variety of colors. Can be designed to meet specific local codes.
				1. Withstands 5 psf snow load and wind gusts up to 90 mph (ASCE-7) with fabric intact. Up to 150 mph wind gusts with fabric removed.

Zinc rich primer: 1-2 mil thickness.

Polyester Powder Coat: oven baked to a 2-4 mil thickness.

* + - 1. Mini Gable Shelter:
				1. Roof pitch: 4:12. Size: 1 ft increments up to 12 ft in diameter.
				2. Available in a variety of colors. Can be designed to meet specific local codes.
				3. Humidity Resistance, ASTM D2247-D2: 5,000 hrs. No blistering or adhesion loss. Color/UV Resistance, ASTM G154-04: 2,000 hrs exposure. No chalking. Roofing Panel Protection: Kynar 500 coating. Structural Steel Tubing: ASTM A500 Grade B. Plates: A36 steel. Welds: By AWS welders.
			2. Octagon: Taking on the welcoming shape of the gazebo. Available in a variety of colors. Can be designed to meet specific local codes.
				1. Humidity Resistance, ASTM D2247-D2: 5,000 hrs. No blistering or adhesion loss. Color/UV Resistance, ASTM G154-04: 2,000 hrs exposure. No chalking. Roofing Panel Protection: Kynar 500 coating. Structural Steel Tubing: ASTM A500 Grade B. Plates: A36 steel. Welds: By AWS welders.
			3. Single Column Cantilever Umbrella Shade:
				1. Available Heights: 8, 10, and 12 ft. Sizes: 8, 10, 12, 14, 16, 18, and 20 ft.
				2. Weight: 600 lbs.
			4. Square Shade Structure: For shading a large area. Can be designed to meet specific local codes. Available in a variety of colors and sizes.
				1. Withstands 5 psf snow load and wind gusts up to 90 mph (ASCE-7) with fabric intact. Up to 150 mph wind gusts with fabric removed.

Zinc rich primer: 1-2 mil thickness.

Polyester Powder Coat: oven baked to a 2-4 mil thickness.

* + - 1. Square Shelter: A roof pitch of 6:12. Available in 1 ft increments up to 30 ft. Available in a variety of colors and sizes. Can be designed to meet specific local codes.
				1. Withstands 5 psf snow load and wind gusts up to 90 mph (ASCE-7) with fabric intact. Up to 150 mph wind gusts with fabric removed.

Zinc rich primer: 1-2 mil thickness.

Polyester Powder Coat: oven baked to a 2-4 mil thickness.

* + - 1. Square Umbrella: Available in a variety of colors, Can be designed to meet specific local codes.
				1. Withstands 5 psf snow load and wind gusts up to 90 mph (ASCE-7) with fabric intact. Up to 150 mph wind gusts with fabric removed.

Zinc rich primer: 1-2 mil thickness.

Polyester Powder Coat: oven baked to a 2-4 mil thickness.

* + - 1. Standard Cantilever: For areas requiring shadows in direct locations. Can be designed to meet local codes. Available in a variety of colors.
				1. Withstands 5 psf snow load and wind gusts up to 90 mph (ASCE-7) with fabric intact. Up to 150 mph wind gusts with fabric removed.

Zinc rich primer: 1-2 mil thickness.

Polyester Powder Coat: oven baked to a 2-4 mil thickness.

* + - 1. T-Cantilever: For areas requiring shadows in direct locations. Can be designed to meet local codes in your area. Available in a variety of colors.
				1. Withstands 5 psf snow load and wind gusts up to 90 mph (ASCE-7) with fabric intact. Up to 150 mph wind gusts with fabric removed.

Zinc rich primer: 1-2 mil thickness.

Polyester Powder Coat: oven baked to a 2-4 mil thickness.

* + - 1. Triangle Sail Shade Canopies: Add customized shade and UV protection to any outdoor space. Can be designed to meet local codes. Available in a variety of colors.
				1. Withstands 5 psf snow load and wind gusts up to 90 mph (ASCE-7) with fabric intact. Up to 150 mph wind gusts with fabric removed.

Zinc rich primer: 1-2 mil thickness.

Polyester Powder Coat: Oven baked to a 2-4 mil thickness.

* + - 1. Wave: Multi-level shade structure providing a cool, shaded area. Designed to meet local codes. Available in a variety of colors.
				1. Withstands 5 psf snow load and wind gusts up to 90 mph (ASCE-7) with fabric intact. Up to 150 mph wind gusts with fabric removed.

Zinc rich primer: 1-2 mil thickness.

Polyester Powder Coat: oven baked to a 2-4 mil thickness.

1. EXECUTION
	1. EXAMINATION
		1. Do not begin installation until the substrates have been properly constructed and prepared.
		2. If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
	2. PREPARATION
		1. Clean surfaces thoroughly prior to installation.
		2. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
	3. INSTALLATION
		1. Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
	4. FIELD QUALITY CONTROL
		1. Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.

\*\* NOTE TO SPECIFIER \*\* Include if manufacturer provides field quality control with onsite personnel for instruction or supervision of product installation, application, erection, or construction. Delete if not required.

* + 1. Manufacturer's Services: Coordinate manufacturer's services in accordance with appropriate sections in Division 01.
	1. CLEANING AND PROTECTION
		1. Clean products in accordance with the manufacturers recommendations.
		2. Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION