SECTION 12 93 00

SITE FURNISHINGS

Display hidden notes to specifier. (Don't know how? [Click Here](http://www.arcat.com/sd/display_hidden_notes.shtml))

*Copyright 2006 - 2015 ARCAT, Inc. - All rights reserved*

\*\* NOTE TO SPECIFIER \*\* DuMor, Inc.; Site Furnishing products.  
.  
This section is based on the products of DuMor, Inc., which is located at:  
P. O. Box 142  
Mifflintown, PA 17059-0142  
Toll Free Tel: 800-598-4018  
Tel: 717-436-2106  
Fax: 717-436-9839  
Email: [request info (sales@dumor.com)](http://admin.arcat.com/users.pl?action=UserEmail&company=DuMor,+Inc.&coid=32084&rep=&fax=717-436-9839&message=RE:%20Spec%20Question%20(02870dum):%20%20&mf=)  
Web: [www.dumor.com](http://www.dumor.com)   
 [ [Click Here](http://www.arcat.com/arcatcos/cos32/arc32084.html) ] for additional information.  
DuMor Site Furnishings, Inc., one of America's most prominent producers of site furnishings, is adding several new site furnishings to our already extensive line for 2006. For over 20 years, DuMor Site Furnishings has been designing stylish and functional site furnishings for parks and common areas across the country. Site furnishings by DuMor Site Furnishings are available with a variety of polyester powder finishes, heavy-duty support options, recycled plastic colors, as well as high-grade woods.

1. GENERAL
   1. SECTION INCLUDES

\*\* NOTE TO SPECIFIER \*\* Delete items below not required for project.

* + 1. Trash receptacles.
    2. Picnic tables.
    3. Planters.
    4. Bike racks.
  1. RELATED SECTIONS

\*\* NOTE TO SPECIFIER \*\* Delete any sections below not relevant to this project; add others as required.

* + 1. Section 12 93 43.13 - Site Seating.
    2. Section 03 30 00 - Cast-in-Place Concrete.
  1. REFERENCES

\*\* NOTE TO SPECIFIER \*\* Delete references from the list below that are not actually required by the text of the edited section.

* + 1. ADA - Americans with disabilities act requirements.
  1. SUBMITTALS
     1. Submit under provisions of Section 01 30 00 - Administrative Requirements.
     2. Product Data: Manufacturer's data sheets on each product to be used, including:
        1. Preparation instructions and recommendations.
        2. Storage and handling requirements and recommendations.
        3. Installation methods.
     3. Shop Drawings: Complete details of layout and assembly, showing member sizes and part identification, fasteners, anchors, and fittings.

\*\* NOTE TO SPECIFIER \*\* Delete the following paragraphs if LEED is not applicable.

* + 1. LEED Submittals: Provide documentation of how the requirements of Credit will be met:
       1. Product Data for Credit MR 2.1 and 2.2: For products being recycled, documentation of total weight of project waste diverted from landfill.
       2. Product Data for Credit MR 4.1 and MR 4.2: For products having recycled content, documentation including percentages by weight of post consumer and preconsumer recycled content
          1. Include statement indicating costs for each product having recycled content.
       3. Product Data for Credit MR 5.1 and Credit MR 5.2: Submit data, including location and distance from Project of material manufacturer and point of extraction, harvest or recovery for main raw material.
          1. Include statement indicating cost for each regional material and the fraction by weight that is considered regional.
    2. Selection Samples: Color selections shall be made from the manufacturer's brochure representing manufacturer's full range of available colors and patterns.
    3. Manufacturer's Certificates: Certify products meet or exceed specified requirements.
    4. Manufacturers warranties.
  1. QUALITY ASSURANCE
     1. Manufacturer Qualifications: Minimum of 15 years experience manufacturing site furnishings.
     2. Installer Qualifications: Minimum of 5 years experience assembling and installing site furnishings.

\*\* NOTE TO SPECIFIER \*\* Include a mock-up if the project size and/or quality warrant taking such a precaution. The following is one example of how a mock-up on a large project might be specified. When deciding on the extent of the mock-up, consider all the major different types of work on the project.

* + 1. Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
       1. Finish areas designated by Architect.
       2. Do not proceed with remaining work until workmanship, color, and sheen are approved by Architect.
       3. Refinish mock-up area as required to produce acceptable work.
  1. DELIVERY, STORAGE, AND HANDLING
     1. Store products in manufacturer's unopened packaging until ready for installation.
     2. Do not deliver until conditions are ready for installation.
  2. PROJECT CONDITIONS
     1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
  3. WARRANTY
     1. Limited twenty-year warranty against structural failure of all table frames, litter receptacle frames, and steel planters.
     2. Limited five-year warranty against structural failure of douglas fir, redwood, western red cedar and ipe products.
     3. Limited ten-year warranty against structural failure of recycled plastic; it is further warrantied not to degrade, split, crack, or splinter during this period.
     4. Limited 3 year warranty on structural failure of all bike racks.

1. PRODUCTS
   1. MANUFACTURERS
      1. Acceptable Manufacturer: DuMor, Inc., which is located at: P. O. Box 142; Mifflintown, PA 17059-0142; Toll Free Tel: 800-598-4018; Tel: 717-436-2106; Fax: 717-436-9839; Email: [request info (sales@dumor.com)](http://admin.arcat.com/users.pl?action=UserEmail&company=DuMor,+Inc.&coid=32084&rep=&fax=717-436-9839&message=RE:%20Spec%20Question%20(02870dum):%20%20&mf=); Web: [www.dumor.com](http://www.dumor.com)

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions.

* + 1. Substitutions: Not permitted.
    2. Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.

\*\* NOTE TO SPECIFIER \*\* Select one or more site furnishings required from the following paragraphs; delete paragraphs that are not required. Visit the manufacturer's web site at [www.dumor.com](http://www.dumor.com) for photos of standard designs. Contact the manufacturer for non-standard and custom products.

* 1. TRASH RECEPTACLES
     1. Steel Trash Receptacles.
        1. DuMor Receptacle 17. Companion to bench 94.
           1. Height: 28-1/2 inches (724 mm).
           2. Width/Length: 26-1/2 inches (673 mm) square.
           3. Frame: Steel tubing, 2 inches (51 mm) square by 11 gauge (3.17 mm) wall and 2 inch (51 mm) by 1 inch (25 mm) by 13 gauge (2.38 mm) wall.
           4. Panel: 1/2 inch (12.5 mm) steel.
           5. Internal Liner: 18 gauge (1.27 mm) steel.
           6. Cover: 14 gauge (1.98 mm) steel.
           7. Liner: 22 gallon (100 l) plastic.
           8. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Embed 18 inches (457 mm) into a cast in place concrete foundation.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 84-22. Companion to Urn 80.
         1. Height: 32-1/2 inches (826 mm).
         2. Diameter: 28-1/4 inches (718 mm).
         3. Top Edge: Steel bar, 5/8 inch (63 mm) diameter.
         4. Vertical Straps: 1/4 inch by 1-1/2 inch (6 by 38 mm) steel bar.
         5. Reveal Strip: 1/4 inch by 3 inch (6 by 76 mm) steel bar.
         6. Liner: 22 gallon (100 l) plastic.
         7. Cover: Spun 14 gauge (1.98 mm) steel with vinyl coated cable.
         8. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 84-32. Companion to Urn 80.
         1. Height: 37-3/8 inches (949 mm).
         2. Diameter: 31-1/2 inches (800 mm).
         3. Top Edge: Steel bar, 5/8 inch (63 mm) diameter.
         4. Vertical Straps: 1/4 inch by 1-1/2 inch (6 by 38 mm) steel bar.
         5. Reveal Strip: 1/4 inch by 3 inch (6 by 76 mm) steel bar.
         6. Liner: 32 gallon (145 l) plastic.
         7. Cover: Spun 14 gauge (1.98 mm) steel with vinyl coated cable.
         8. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 87-22.
         1. Height: 33-1/4 inches (845 mm).
         2. Diameter: 28 inches (711 mm).
         3. Top and Bottom Edges: Steel bar, 5/8 inch (63 mm) diameter.
         4. Body: 1/4 inch by 1 inch (6 by 25 mm) and 1/4 inch by 2 inch (6 by 51 mm) steel bar.
         5. Liner: 22 gallon (100 l) plastic.
         6. Cover: Spun 14 gauge (1.98 mm) steel, hinged with nylon stops.
         7. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 89.
         1. Height: 32-1/4 inches (819 mm).
         2. Diameter: 26-3/4 inches (697 mm).
         3. Frame: 1/4 inch by 2 inch (25 by 51 mm), 3/8 by 2 inch (9.5 by 51 mm) and 1/4 inch by 1-1/2 inch (25 by 38 mm) steel bar.
         4. Body: 16 gauge (1.58 mm) perforated steel.
         5. Reveal Strip: 1/4 inch (6 mm) by 5 inch (127 mm) steel bar.
         6. Cover: 14 gauge (1.98 mm) spun steel with a 10 inch (254 mm) diameter opening and secured with vinyl coated cable.
         7. Liner: 32 gallon (145 l) plastic.
         8. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 102-22. With hinged door for liner removal.
         1. Height: 32-3/4 inches (832 mm).
         2. Diameter: 26-1/2 inches (673 mm).
         3. Top and Bottom Edges: Steel bar, 3/8 by 2-1/2 inch (38 635 mm) steel.
         4. Centerband: 3/8 inch (9.5 mm) by 2 inch (51 mm) steel.
         5. Vertical Straps: 3/8 inch by 1 inch (9.5 by 25 mm) steel bar.
         6. Reveal Strip: 1/4 inch by 2 inch (25 by 51 mm) steel bar.
         7. Rosettes: 4-1/4 inch (108 mm) diameter, 3/4 inch (19 mm) cast iron.
         8. Opening: 3/8 inch (9.5 mm) steel plate with 10 inch (254 mm) diameter opening.
         9. Liner: 22 gallon (100 l) plastic.

\*\* NOTE TO SPECIFIER \*\* Internal shield is optional delete if not required.

* + - * 1. Internal Shield: 18 gauge (1.27 mm) CR steel.
        2. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 102-32. With hinged door for liner removal.
         1. Height: 36 inches (832 mm).
         2. Diameter: 28 inches (711 mm).
         3. Top and Bottom Edges: Steel bar, 3/8 by 2-1/2 inch (9.5 by 63.5 mm) steel.
         4. Vertical Straps: 1/2 by 1 inch (12.5 by 25 mm) steel bar.
         5. Reveal Strip: 1/4 inch by 2 inch (25 by 51 mm) steel bar.
         6. Rosettes: 4-1/4 inch (108 mm) diameter, 3/4 inch (19 mm) cast iron.
         7. Opening: 3/8 inch (9.5 mm) steel plate with 10 inch (254 mm) diameter opening.
         8. Liner: 32 gallon (145 l) plastic.

\*\* NOTE TO SPECIFIER \*\* Internal shield is optional delete if not required.

* + - * 1. Internal Shield: 18 gauge (1.27 mm) CR steel.
        2. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 107-22. Extra heavy duty.
         1. Height: 32-3/4 inches (832 mm).
         2. Diameter: 29 inches (737 mm).
         3. Top Edge: Steel bar, 5/8 inch (63 mm) diameter.
         4. Vertical Straps: 3/8 by 3/4 inch (9.5 by 19 mm) and 3/8 by 1-1/4 inch (9.5 by 32 mm) steel bar.
         5. Reveal Strip: 1/4 inch by 3 inch (6 by 76 mm) steel bar.
         6. Liner: 22 gallon (100 l) plastic.
         7. Cover: Spun 14 gauge (1.98 mm) steel with vinyl coated cable and 10 inch (254 mm) diameter opening.
         8. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 107-32. Extra heavy duty.
         1. Height: 37 inches (940 mm).
         2. Diameter: 32-3/4 inches (832 mm).
         3. Top Edge: Steel bar, 5/8 inch (63 mm) diameter.
         4. Vertical Straps: 3/8 by 3/4 inch (9.5 by 19 mm) and 3/8 by 1-1/4 inch (9.5 by 32 mm) steel bar.
         5. Reveal Strip: 1/4 inch by 3 inch (6 by 76 mm) steel bar.
         6. Liner: 32 gallon (145 l) plastic.
         7. Cover: Spun 14 gauge (1.98 mm) steel with vinyl coated cable and 10 inch (254 mm) diameter opening.
         8. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 116.
         1. Height: 28-1/2 inches (724 mm).
         2. Width/Length: 26-1/2 inches (673 mm) square.
         3. Frame: Steel tubing, 2 inches (51 mm) square by 11 gauge (3.17 mm) wall and 2 inch (51 mm) by 1 inch (25 mm) by 13 gauge (2.38 mm) wall.
         4. Panel: 3/8 inch (9.5 mm) steel.
         5. Internal Liner: 18 gauge (1.27 mm) steel.
         6. Cover: Hinged 14 gauge (1.98 mm) steel.
         7. Liner: 22 gallon (100 l) plastic.
         8. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Embed 18 inches (457 mm) into a cast in place concrete foundation.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle/Ash Urn 129.
         1. Height: 27-15/16 inches (710 mm).
         2. Diameter: 13-3/8 inches (340 mm).
         3. Frame: 1 inch (25 mm) schedule 40 pipe and 1/4 inch (25 mm) by 2 inch (51 mm) HR steel.
         4. Ash Pan: Spun aluminum, 10 inch (254 mm) diameter.
         5. Liner: 5 gallon (23 l) galvanized steel.
         6. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 133. Companion to planter 134 and ash urn 135.
         1. Height: 36-1/2 inches (927 mm).
         2. Diameter: 30-5/16 inches (770 mm)
         3. Top Edge: 1 inch (25 mm) schedule 40 steel pipe.
         4. Vertical Straps: 3/8 by 1-1/4 inch (9.5 by 32 mm) steel bar.
         5. Reveal Strip: 1/4 inch by 3 inch (6 by 76 mm) steel bar.
         6. Liner: 32 gallon (145 l) plastic.
         7. Cover: Hinged, 14 gauge (1.98 mm) spun steel with a 10 inch (254 mm) diameter opening.
         8. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 148-22. With hinged door for liner removal.
         1. Height: 32-3/4 inches (832 mm).
         2. Diameter: 26-1/2 inches (673 mm).
         3. Top and Bottom Edges: Steel bar, 3/8 by 2-1/2 inch (9.5 by 63.5 mm) steel.
         4. Vertical Straps: 3/8 by 1 inch (9.5 by 25 mm) steel bar.
         5. Reveal Strip: 3/8 by 2 inch (9.5 by 51 mm) steel bar.
         6. Star Disk: 4-1/4 inch (108 mm) diameter, 3/4 inch (19 mm) cast iron.
         7. Cover: 3/8 inch (9.5 mm) steel with a 10 inch (254 mm) diameter opening.
         8. Liner: 22 gallon (100 l) plastic.

\*\* NOTE TO SPECIFIER \*\* Internal shield is optional delete if not required.

* + - * 1. Internal Shield: 18 gauge (1.27 mm) CR steel.
        2. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 148-32. With hinged door for liner removal.
         1. Height: 36 inches (832 mm).
         2. Diameter: 28 inches (711 mm).
         3. Top and Bottom Edges: Steel bar, 3/8 by 2-1/2 inch (9.5 by 63.5 mm) steel.
         4. Vertical Straps: 1/2 by 1 inch (12.5 by 25 mm) steel bar.
         5. Reveal Strip: 1/4 inch by 2 inch (25 by 51 mm) steel bar.
         6. Star Disk: 4-1/4 inch (108 mm) diameter, 3/4 inch (19 mm) cast iron.
         7. Cover: 3/8 inch (9.5 mm) steel with a 10 inch (254 mm) diameter opening.
         8. Liner: 32 gallon (145 l) plastic.

\*\* NOTE TO SPECIFIER \*\* Internal shield is optional delete if not required.

* + - * 1. Internal Shield: 18 gauge (1.27 mm) CR steel.
        2. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 157-22. With hinged door for liner removal.
         1. Height: 40-11/16 inches (1038 mm).
         2. Diameter: 26-1/8 inches (634 mm).
         3. Top Edge: Steel bar, 5/8 inch (63 mm) diameter.
         4. Vertical Straps: 1/4 inch by 1-1/2 inch (6 by 38 mm) steel bar.
         5. Reveal Strip: 1/4 inch by 2 inch (6 by 51 mm) steel bar.
         6. Internal Steel Shield: 18 gauge (1.27 mm) CR steel.
         7. Liner: 22 gallon (100 l) plastic.
         8. Bonnet Cover: Spun 12 gauge (2.77 mm) steel with 3/8 by 1 inch (9.5 by 25 mm) steel bar supports.
         9. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 157-32. With hinged door for liner removal.
         1. Height: 45-1/2 inches (1156 mm).
         2. Diameter: 33-1/8 inches (841 mm)
         3. Top Edge: Steel bar, 5/8 inch (63 mm) diameter.
         4. Vertical Straps: 1/4 inch by 1-1/2 inch (6 by 38 mm) steel bar.
         5. Reveal Strip: 1/4 inch by 2 inch (6 by 51 mm) steel bar.
         6. Internal Steel Shield: 18 gauge (1.27 mm) CR steel.
         7. Liner: 32 gallon (145 l) plastic.
         8. Bonnet Cover: Spun 12 gauge (2.77 mm) steel with 3/8 by 1 inch (9.5 by 25 mm) steel bar supports.
         9. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 158-22. Heavy duty type. Companion to bench 19 and planter 159.
         1. Height: 34-3/16 inches (884 mm).
         2. Diameter: 29-13/16 inches (757 mm).
         3. Top Edge: Steel bar, 5/8 inch (63 mm) diameter.
         4. Vertical Straps: Steel bar, 5/8 inch (63 mm) diameter.
         5. Reveal Strip: 1/4 inch by 3 inch (6 by 76 mm) steel bar.
         6. Internal Steel Shield: 18 gauge (1.27 mm) CR steel.
         7. Liner: 22 gallon (100 l) plastic.
         8. Cover: Spun 14 gauge (1.98 mm) steel with 10 inch (254 mm) diameter opening secured with a vinyl coated cable.
         9. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 158-32. Heavy duty type. Companion to bench 19 and planter 159.
         1. Height: 39-1/4 inches (997 mm).
         2. Diameter: 33 inches (838 mm)
         3. Top Edge: Steel bar, 5/8 inch (63 mm) diameter.
         4. Vertical Straps: Steel bar, 5/8 inch (63 mm) diameter.
         5. Reveal Strip: 1/4 inch by 3 inch (6 by 76 mm) steel bar.
         6. Liner: 32 gallon (145 l) plastic.
         7. Internal Steel Shield: 18 gauge (1.27 mm) CR steel.
         8. Cover: Spun 14 gauge (1.98 mm) steel with 10 inch (254 mm) diameter opening secured with a vinyl coated cable.
         9. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 170
         1. Height: 30-9/16 inches (776 mm).
         2. Diameter: 28-1/2 inches (724 mm).
         3. Frame: 1/4 inch by 1-1/2 inch (25 by 38 mm), 3/8 by 2 inch (9.5 by 51 mm) and 1-5/16 inch (49 mm) O.D. steel pipe
         4. Body: 16 gauge (1.58 mm) slotted perforated steel.
         5. Cover: 14 gauge (1.98 mm) spun steel with a 10 inch (254 mm) diameter opening and secured with vinyl coated cable.
         6. Liner: 32 gallon (145 l) plastic.
         7. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 182-32-BT: Companion to bench 181-60.
         1. Height: 43-1/2 inches (1105 mm).
         2. Width/Length: 22 inches (559 mm) square.
         3. Frame: Extruded aluminum and 1/8 inch thick (3 mm) aluminum plate.
         4. Panel: 14 gauge slotted steel.
         5. Reveal Strip: 1/4 inch by 1-1/2 inch (6 mm by 38 mm) aluminum bar.
         6. Cover: 10 gauge aluminum bonnet with 10-1/2 by 16 inch (267 mm by 406 mm) opening and vinyl coated steel cable.
         7. Liner: 32 gallon (145 l) plastic.
         8. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 183-22: Companion to Planter 184.
         1. Height: 30-7/8 inches (784 mm).
         2. Diameter: 32-1/2 inches (826 mm).
         3. Top and bottom edges: 5/8 inch (16 mm) diameter steel bar.
         4. Vertical Straps: 1/4 inch by 1-1/2 inch (6 mm by 38 mm) steel bar.
         5. Liner: 22 gallon (100 l) plastic.
         6. Cover: Spun 14 gauge (1.96 mm) steel with vinyl coated cable.
         7. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 183-32: Companion to Planter 184.
         1. Height: 35-9/16 inches (903 mm).
         2. Diameter: 35-5/8 inches (905 mm).
         3. Top and bottom edges: 5/8 inch (16 mm) diameter steel bar.
         4. Vertical Straps: 1/4 inch by 1-1/2 inch (6 mm by 38 mm) steel bar.
         5. Liner: 32 gallon (145 l) plastic.
         6. Cover: Spun 14 gauge (1.96 mm) steel with vinyl coated cable.
         7. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 200.
         1. Body: 1/4 inch (6 mm) steel with 18 gauge internal steel shield.
         2. Height: 33 inches (838 mm).
         3. Diameter: 26-1/4 inches (667 mm).
         4. Top and Bottom Edge: 1/4 inch by 2 inch (25 by 51 mm) steel bar.
         5. Liner: 32 gallon (145 l) plastic.
         6. Internal Steel Shield: 18 gauge (1.27 mm) CR steel.

\*\* NOTE TO SPECIFIER \*\* Select one the following design types as required and delete those not required.

* + - * 1. Design Type:

201.

203.

204.

208.

209.

210.

211.

Custom design as selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Custom lettering is optional, delete if not required.

Provide with custom lettering as selected by the Architect.

* + - * 1. Cover: 14 gauge (1.98 mm) spun steel with a 10 inch (254 mm) diameter opening.
        2. Liner: 32 gallon (145 l) plastic.
        3. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Receptacle 300 with hinged side door.
         1. Body: 1/4 inch (6 mm) steel with 18 gauge internal steel shield.
         2. Height: 34-1/2 inches (876 mm).
         3. Diameter: 26-1/4 inches (667 mm).
         4. Top and Bottom Edge: 1/4 inch by 2 inch (25 by 51 mm) steel bar.
         5. Liner: 32 gallon (145 l) plastic.

\*\* NOTE TO SPECIFIER \*\* Select one the following design types as required and delete those not required.

* + - * 1. Design Type:

301.

303.

304.

308.

309.

310.

311.

Custom design as selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* Custom lettering is optional, delete if not required.

Provide with custom lettering as selected by the Architect.

* + - * 1. Cover: 14 gauge (1.98 mm) spun steel with a 10 inch (254 mm) diameter opening.
        2. Liner: 32 gallon (145 l) plastic.
        3. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

* + - * 1. Metal Finish and Colors: Powder coated.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + 1. Recycled Plastic Receptacles.
       1. DuMor Plastic Receptacle 41PL:
          1. Height: 22 gallon, 33-13/16 inches (859 mm).
          2. Height: 32 gallon, 37-15/16 inches (964 mm).
          3. Diameter: 22 gallon, 24-11/16 inches (627 mm).
          4. Diameter: 32 gallon, 28-1/2 inches (724 mm).
          5. Supports: 2-3/8 inch (60 mm) and 2-7/8 inch (73 mm) O.D. steel pipe.
          6. Internal Frame: 3/16 by 1-1/4 inch (5 by 32 mm) and 3/8 by 1 inch (9.5 mm by 25 mm) steel bar.
          7. Fasteners: Stainless steel.

\*\* NOTE TO SPECIFIER \*\* Select one the following sizes as required and delete the one not required.

* + - * 1. Liner: 22 gallon (100 l) plastic.
        2. Liner: 32 gallon (145 l) plastic.
        3. Cover: Polyethylene with vinyl coated cable and 10 inch (254 mm) opening.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

* + - * 1. Mounting:

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 2 by 3 inch (51 by 76 mm) recycled plastic. Plastic Colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

* + - * 1. Metal Finish and Colors: Black polyester finish.
      1. DuMor Plastic Receptacle 44PL:
         1. Height: 37-3/4 inches (959 mm).
         2. Diameter: 25-1/2 inches (648 mm).
         3. Internal Frame: 3/16 inch (5 mm) by 4 inch (102 mm) and 3/16 inch (5 mm) by 1-1/4 inch (32 mm) steel bar.
         4. Fasteners: Stainless steel.
         5. Liner: 22 gallon (100 l) plastic.
         6. Cover: Flat polyethylene plastic with vinyl coated cable and sand urn.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

* + - * 1. Mounting:

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 1-1/2 inch thick (38 mm) recycled plastic. Plastic Colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

* + - * 1. Metal Finish and Colors: Black polyester finish.
      1. DuMor Plastic Receptacle 70PL:
         1. Height: 30-11/16 inches (779 mm).
         2. Diameter: 25-7/16 inches (646 mm).
         3. Internal Frame: 3/16 inch (5 mm) by 4 inch (102 mm) steel bar.
         4. Fasteners: Stainless steel.
         5. Liner: 22 gallon (100 l) plastic.
         6. Cover: Flat polyethylene plastic with vinyl coated cable and a 10 inch (254 mm) diameter opening.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

* + - * 1. Mounting:

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 1-1/2 inch thick (38 mm) recycled plastic. Plastic Colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Plastic Receptacle 85PL:
         1. Height: 31-11/16 inches (805 mm).
         2. Diameter: 24-7/8 inches (632 mm).
         3. Supports: 1/2 by 3 inch (12.5 by 76 mm) steel bar.
         4. Internal Frame: 3/16 by 1-1/4 inch (5 by 32 mm) and 1/4 inch by 1 inch (6 by 25 mm) steel bar.
         5. Fasteners: Stainless steel.
         6. Liner: 22 gallon (100 l) plastic.
         7. Cover: Flat polyethylene plastic with vinyl coated cable.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

* + - * 1. Support/Mounting:

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Gull Wing: 1/2 by 3 inch (12.5 by 76 mm) steel bar with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Embed 24 inches (610 mm) into a cast in place concrete foundation.

Subfloor 4 inches (102 mm) into a cast in place concrete floor.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 2 by 3 inch (51 by 76 mm) recycled plastic. Plastic Colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Plastic Receptacle 124PL: Companion to bench 57PL.
         1. Height: 36 inches (914 mm).
         2. Diameter: 28 inches (711 mm).
         3. Top and Bottom Bands: 3/8 inch by 2 inch (9.5 by 51 mm) steel bar.
         4. Rosettes: 4-1/4 inch (108 mm) diameter, 3/4 inch (19 mm) cast iron.
         5. Cover: 14 gauge (1.98 mm) spun steel with a 10 inch (254 mm) diameter opening and secured with vinyl coated cable.
         6. Fasteners: Stainless steel.
         7. Liner: 31 gallon (141 l) galvanized.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

* + - * 1. Mounting:

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 2 by 4 inch (51 by 102 mm) recycled plastic. Plastic Colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Plastic Receptacle 152PL: Companion to bench 142 and planter 153.
         1. Height: 36 inches (914 mm).
         2. Diameter: 28 inches (711 mm).
         3. Top and Bottom Bands: 3/8 inch by 2-1/4 inch (9.5 by 57 mm) steel bar.
         4. Center Band: 3/8 inch by 2 inch (9.5 by 51 mm) steel bar.
         5. Rosettes: 4-1/4 inch (108 mm) diameter, 3/4 inch (19 mm) cast iron.
         6. Cover: 14 gauge (1.98 mm) spun steel with a 10 inch (254 mm) diameter opening and secured with vinyl coated cable.
         7. Fasteners: Stainless steel.
         8. Liner: 31 gallon (141 l) galvanized.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

* + - * 1. Mounting:

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 2 by 4 inch (51 by 102 mm) recycled plastic. Plastic Colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Plastic Receptacle 179PL; Companion to bench 177PL.
         1. Height: 31-3/8 inches (797 mm).
         2. Width/Length: 26 inches (660 mm) square.
         3. Top band: 1/4 inch by 3 inch (6.25 mm by 76 mm steel plate.
         4. Bottom Plate: 1/4 inch (6.25 mm) by 26 inch (660 mm) square plasma cut steel plate.
         5. Decorative rings: 4-1/2 inch (114 mm) diameter by 1/2 inch (12.5 mm) wall by 1/2 inch (12.5 mm) thick.
         6. Opening: 1/4 inch (6.25 mm) steel plate with 10 inch (254 mm) diameter opening.
         7. Frame: 1/4 inch (6.25 mm) plasma cut steel plate.
         8. Fasteners: Stainless Steel.
         9. Liner: 22 gallon (100 l) plastic.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

* + - * 1. Mounting:

Free standing.

Surface Plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 2 by 3 inch (51 by 76 mm) nom, and profiled recycled plastic. Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Plastic Receptacle 187-32PL; Companion to bench 185PL.
         1. Height: 32 inches (713 mm).
         2. Width/Length: 23-1/2 inches (597 mm) square.
         3. Corner supports: Cast iron.
         4. Frame: 1/4 inch by 2 inch (6.25 mm by 51 mm) steel bar.
         5. Cover: 12 gauge steel with vinyl coated cable and a 10 inch (254 mm) square opening.
         6. Fasteners: Stainless Steel.
         7. Liner: 32 gallon (145 l) plastic.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

* + - * 1. Mounting:

Free standing.

Surface Plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 2 by 3 inch (51 by 76 mm) nom, and profiled recycled plastic. Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + 1. Wood Receptacles:
       1. DuMor Wood Receptacle 41:

\*\* NOTE TO SPECIFIER \*\* Select the height and diameter for the capacity required and delete the ones not required.

* + - * 1. Height: 22 gallon (100 l), 33-13/16 inches (859 mm).
        2. Height: 32 gallon (145 l), 37-5/16 inches (964 mm).
        3. Diameter: 22 gallon (100 l), 24-11/16 inches (624 mm).
        4. Diameter: 32 gallon (145 l), 28-3/4 inches (730 mm).
        5. Supports: 2-3/8 inch (60 mm) and 2-7/8 inch (73 mm) O.D. steel pipe.
        6. Internal Frame: 3/16 by 1-1/4 inch (5 by 32 mm) and 3/8 by 1 inch (9.5 by 25 mm) steel bar.
        7. Fasteners: Stainless steel.

\*\* NOTE TO SPECIFIER \*\* Select one the following sizes as required and delete the one not required.

* + - * 1. Liner: 22 gallon (100 l) plastic.
        2. Liner: 32 gallon (145 l) plastic.

\*\* NOTE TO SPECIFIER \*\* Select one the following cover options as required and delete the one not required.

* + - * 1. Cover: Molded polyethylene with vinyl coated cable and 10 inch (254 mm) diameter opening.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

* + - * 1. Mounting:

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Embed 12 inches (305 mm) into a cast in place concrete foundation.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 3 inch (51 by 76 mm):

Redwood.

Douglas Fir.

As selected by the Architect from manufacturer's standard materials.

* + - * 1. Metal Finish and Colors: Powder coated, black polyester.
      1. DuMor Wood Receptacle 43:
         1. Height: 22 gallon (100 l), 23-2/16 inches (527 mm).
         2. Height: 32 gallon (145 l), 36-5/8 inches (905 mm).
         3. Diameter: 22 gallon (100 l), 24-13/16 inches (630 mm).
         4. Diameter: 32 gallon (145 l), 28-5/8 inches (724 mm).
         5. Internal Frame: 3/16 by 1-1/4 inch (5 by 32 mm) and 3/8 by 1 inch (9.5 by 25 mm) steel bar.
         6. Fasteners: Stainless steel.

\*\* NOTE TO SPECIFIER \*\* Select one the following sizes as required and delete the one not required.

* + - * 1. Liner: 22 gallon (100 l) plastic.
        2. Liner: 32 gallon (145 l) plastic.
        3. Cover: Molded polyethylene with vinyl coated cable and 10 inch (254 mm) diameter opening.
        4. Mounting: Free standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 3 inch (51 by 76 mm):

Redwood.

Douglas Fir.

As selected by the Architect from manufacturer's standard materials.

* + - * 1. Metal Finish and Colors: Black polyester.
      1. DuMor Wood Receptacle 44:
         1. Height: 37-1/2 inches (953 mm).
         2. Diameter: 25-1/2 inches (648 mm).
         3. Internal Frame: 3/16 inch (5 mm) by 4 inch (102 mm) steel bar.
         4. Fasteners: Stainless steel.
         5. Liner: 22 gallon (100 l) plastic.
         6. Cover: Flat polyethylene plastic with vinyl coated cable and sand urn.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

* + - * 1. Mounting:

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 3 inch (51 by 76 mm):

Redwood.

Douglas Fir.

As selected by the Architect from manufacturer's standard materials.

* + - * 1. Metal Finish and Colors: Black polyester.
      1. DuMor Wood Receptacle 70:
         1. Height: 30-1/2 inches (775 mm).
         2. Diameter: 25-1/2 inches (648 mm).
         3. Internal Frame: 3/16 inch (5 mm) steel bar.
         4. Fasteners: Stainless steel.
         5. Liner: 22 gallon (100 l) plastic.
         6. Cover: Flat polyethylene plastic with vinyl coated cable.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

* + - * 1. Mounting:

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 3 inch (51 by 76 mm):

Redwood.

Douglas Fir.

As selected by the Architect from manufacturer's standard materials.

* + - * 1. Metal Finish and Colors: Black polyester.
      1. DuMor Wood Receptacle 85:
         1. Height: 31-11/16 inches (805 mm).
         2. Diameter: 24-7/8 inches (632 mm).
         3. Supports: 1/2 by 3 inch (12.5 by 76 mm) steel bar.
         4. Internal Frame: 3/16 by 1-1/4 inch (5 by 32 mm) and 3/8 inch by 1 inch (9.5 by 25 mm) steel bar.
         5. Fasteners: Stainless steel.
         6. Liner: 22 gallon (100 l) plastic.
         7. Cover: Black polyethylene with vinyl coated cable and 10 inch (254 mm) diameter opening.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

* + - * 1. Support/Mounting:

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Gull Wing: 1/2 by 3 inch (12.5 by 76 mm) steel bar with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Embed 18 inches (457 mm) into a cast in place concrete foundation.

Subfloor 4 inches (102 mm) into a cast in place concrete floor.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 3 inch (51 by 76 mm):

Redwood.

Douglas Fir.

As selected by the Architect from manufacturer's standard materials.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Wood Receptacle 124: Companion to bench 57.
         1. Height: 36 inches (914 mm).
         2. Diameter: 28 inches (711 mm).
         3. Top and Bottom Bands: 3/8 inch by 2 inch (9.5 by 51 mm) steel bar.
         4. Rosettes: 4-1/4 inch (108 mm) diameter, 3/4 inch (19 mm) cast iron.
         5. Cover: 14 gauge (1.98 mm) spun steel with a 10 inch (254 mm) diameter opening and secured with vinyl coated cable.
         6. Fasteners: Stainless steel.
         7. Liner: 31 gallon (141 l) galvanized.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

* + - * 1. Mounting:

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 3 inch (51 by 76 mm):

Redwood.

Douglas Fir.

Ipe.

As selected by the Architect from manufacturer's standard materials.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Wood Receptacle 152: Companion to bench 142 and planter 153.
         1. Height: 36 inches (914 mm).
         2. Diameter: 28 inches (711 mm).
         3. Top and Bottom Bands: 3/8 inch by 2-1/4 inch (9.5 by 57 mm) steel bar.
         4. Center Band: 3/8 inch by 2 inch (9.5 by 51 mm) steel bar.
         5. Rosettes: 4-1/4 inch (108 mm) diameter, 3/4 inch (19 mm) cast iron.
         6. Cover: 14 gauge (1.98 mm) spun steel with a 10 inch (254 mm) diameter opening and secured with vinyl coated cable.
         7. Fasteners: Stainless steel.
         8. Liner: 31 gallon (141 l) galvanized.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

* + - * 1. Mounting:

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 3 inch (51 by 76 mm):

Redwood.

Douglas Fir.

Ipe.

As selected by the Architect from manufacturer's standard materials.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Model 187-32; Companion to bench 185:
         1. Height: 32 inches (813 mm).
         2. Width/Length: 23-1/2 inches (597 mm) square.
         3. Corner supports: Cast iron.
         4. Frame: 1/4 inch by 2 inch (6.25 mm by 51 mm) steel bar.
         5. Cover: 12 gauge steel with vinyl coated cable and a 10 inch (254 mm) square opening.
         6. Fasteners: Stainless Steel
         7. Liner: 32 gallon (145 l) plastic

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

* + - * 1. Mounting:

Free standing

Surface Plate with 1/2 inch by 3-3/4 inch (12.5 mm by 95 mm) stainless steel expansion bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 3 inch (51 by 76 mm) nom, and profiled.

Redwood.

Douglas Fir.

Ipe.

As selected by the Architect from manufacturer's standard materials.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

\*\* NOTE TO SPECIFIER \*\* The following covers are optional in lieu of the covers specified above. Select optional covers as required or delete if not required. Custom colors are available at additional cost.

* + 1. Receptacle Covers:
       1. DuMor Recycled Lid.
       2. Bonnet Top.
       3. Bonnet Top with Ash Urn.
       4. Dome Top.
       5. Dome Top with Ash Urn.
       6. Dome Top with Self-Closing Door.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - 1. Metal Finish and Colors: Powder coated.
         1. As selected by the Architect from manufacturer's 11 standard colors.
         2. Custom color as selected by the Architect.
  1. TABLES
     1. Pedestal Tables:
        1. DuMor Free Standing Steel Table 101:
           1. Diameter: 42 inch (1067 mm).
           2. Top: 10 gauge (3.57 mm) steel.
           3. Seats: 14 gauge (1.98 mm) perforated steel.
           4. Supports: 2 inch (51 mm) schedule 40 steel pipe, 1/2 by 2 inch (12.5 by 51 mm) and 3/8 by 2-1/2 inch (9.5 by 64 mm) steel bar.
           5. Mounting: Free standing.
           6. Fasteners: Stainless steel.
           7. Pedestal Seats:

\*\* NOTE TO SPECIFIER \*\* Select paragraph for the number of seats required, delete those not required.

Two seats.

Three seats.

Four seats.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Free Standing Steel Table 126:
         1. Diameter: 42 inch (1067 mm).
         2. Top: 10 gauge (3.57 mm) steel.
         3. Table Supports: 5/8 by 3 inch (16 by 76 mm) steel bar.
         4. Seats: 14 gauge (1.98 mm) perforated steel.
         5. Seat Supports: 3/4 inch (19 mm) schedule 40 steel pipe, 1 inch (25.5 mm) square steel tube and 3/8 by 2 inch (9.5 by 51 mm) steel bar.
         6. Mounting: Free standing.
         7. Fasteners: Stainless steel.
         8. Free Standing Seats:

\*\* NOTE TO SPECIFIER \*\* Select paragraph for the number of seats required, delete those not required.

Two seats.

Three seats.

Four seats.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Plastic Pedestal Table 76PL:
         1. Size: 48 inch (1219 mm) square.
         2. Frame: 2-1/2 inch by 1/4 inch (64 by 6 mm) steel tube and 1/4 inch (6 mm) steel angle.
         3. Center Post: 4 inch (102 mm) by 3/16 inch (5 mm).
         4. Fasteners: Stainless steel.

\*\* NOTE TO SPECIFIER \*\* Select one the following slat sizes as required and delete the one not required.

* + - * 1. Slats: Recycled plastic.

3 by 4 inch (76 by 102 mm).

4 by 4 inch (102 by 102 mm).

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut.

As selected by the Architect from manufacturer's standard colors.

* + - * 1. Pedestal Seats:

\*\* NOTE TO SPECIFIER \*\* Select paragraph for the number of seats required, delete those not required.

Two seats.

Three seats.

Four seats.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required. For embedded mount use 30 inches for 3 by 4 inch slat model and 31 inches for the 4 by 4 inch model.

* + - * 1. Mounting:

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Embed 30 inches (762 mm) into a cast in place concrete foundation.

Embed 31 inches (787 mm) into a cast in place concrete foundation.

Subfloor 4 inches (102 mm) into a cast in place concrete floor.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Wood Pedestal Table 76:
         1. Size: 48 inch (1219 mm) square.
         2. Frame: 2-1/2 inch by 1/4 inch (64 by 6 mm) steel tube and 1/4 inch (6 mm) steel angle.
         3. Center Post: 4 inch (102 mm) by 3/16 inch (5 mm).
         4. Fasteners: Stainless steel.
         5. Wood Slats:

\*\* NOTE TO SPECIFIER \*\* Select one the following slat sizes as required and delete the one not required.

2 by 4 inch (51 by 102 mm).

3 by 4 inch (76 by 102 mm.

4 by 4 inch (102 by 102 mm.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

Redwood.

Douglas Fir.

As selected by the Architect from manufacturer's standard materials.

* + - * 1. Pedestal Seats:

\*\* NOTE TO SPECIFIER \*\* Select paragraph for the number of seats required, delete those not required.

Two seats.

Three seats.

Four seats.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required. For embedded mount use 29 inched for 2 by 4 inch slats, 30 inches for 3 by 4 inch slat model and 31 inches for the 4 by 4 inch model.

* + - * 1. Mounting:

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Embed 29 inches (637 mm) into a cast in place concrete foundation.

Embed 30 inches (762 mm) into a cast in place concrete foundation.

Embed 31 inches (787 mm) into a cast in place concrete foundation.

Subfloor 4 inches (102 mm) into a cast in place concrete floor.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + 1. Picnic Tables:
       1. DuMor Plastic Picnic Table 71PL:

\*\* NOTE TO SPECIFIER \*\* Select one the following size paragraphs and delete the ones not required.

* + - * 1. Size:

59 inches (1499 mm) wide by 71 inches (1803 mm) long.

59 inches (1499 mm) wide by 95 inches (2413 mm) Long.

59 inches (1499 mm) wide by 95 inches (2413 mm) Long, handicapped accessible.

* + - * 1. Frame: 1-5/8 inch (41 mm) O.D. steel tube and 1/4 inch (6 mm) by 1 inch (25.5 mm) steel braces.
        2. Fasteners: Stainless steel.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 2 by 10 inch (51 by 254 mm) recycled plastic. Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

* + - * 1. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

Metal hot dip galvanized.

* + - 1. DuMor Plastic Picnic Table 72PL:

\*\* NOTE TO SPECIFIER \*\* Select one the following size paragraphs and delete the one not required.

* + - * 1. Size:

59 inches (1499 mm) wide by 71 inches (1803 mm) long.

59 inches (1499 mm) wide by 95 inches (2413 mm) Long.

59 inches (1499 mm) wide by 95 inches (2413 mm) Long, handicapped accessible.

* + - * 1. Frame: 2-3/8 inch (60 mm) O.D. galvanized steel pipe and 1-5/8 inch (41 mm) O.D. galvanized steel pipe braces and 2 inch by 1 inch by 1/8 inch (51 by 35 by 3 mm) center channel.
        2. Fasteners: Stainless steel.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 2 by 10 inch (51 by 254 mm) recycled plastic. Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

* + - * 1. Mounting: Free Standing.
        2. Metal Finish: Triple layer, zinc flowcoat.
      1. DuMor Plastic Picnic Table 77PL:

\*\* NOTE TO SPECIFIER \*\* Select one the following size paragraphs and delete the one not required.

* + - * 1. Size:

59 inches (1499 mm) wide by 71 inches (1803 mm) long.

59 inches (1499 mm) wide by 95 inches (2413 mm) Long.

59 inches (1499 mm) wide by 95 inches (2413 mm) Long, handicapped accessible.

* + - * 1. Frame: 2-3/8 inch (60 mm) O.D. steel pipe, 1-5/8 inch (41 mm) O.D. galvanized steel pipe braces and 2 by 1 by 1/8 inch (51 by 25.5 by 3 mm) center channel.
        2. Fasteners: Stainless steel.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 2 by 10 inch (51 by 254 mm) recycled plastic. Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

* + - * 1. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

Metal hot dip galvanized.

* + - 1. DuMor Plastic Picnic Table 100PL:

\*\* NOTE TO SPECIFIER \*\* Select one the following size paragraphs and delete the one not required.

* + - * 1. Size:

30 inches (1219 mm) wide by 71 inches (1803 mm) long.

30 inches (1219 mm) wide by 95 inches (2413 mm) Long.

30 inches (1219 mm) by 95 inches (2413 mm) Long, handicapped accessible.

* + - * 1. Supports: 3 inch (76 mm) by 1/4 inch (6 mm) thick square steel tube, 1/2 by 3 inch (12.5 by 76 mm) steel bar, 1-5/16 inch (33 mm) O.D. steel pipe and 2 by 1 by 1/8 inch (51 by 25 by 3 mm) steel channel.
        2. Fasteners: Stainless steel.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 3 by 4 inch (76 by 102 mm) and 3 by 6 inch (76 by 152 mm) recycled plastic. Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

* + - * 1. Mounting:

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Embed 23-1/2 inches (597 mm) into a cast in place concrete foundation.

Subfloor 4 inches (102 mm) into a cast in place concrete floor.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Wood Picnic Table 71:

\*\* NOTE TO SPECIFIER \*\* Select one the following size paragraphs and delete the one not required.

* + - * 1. Size:

59 inches (1499 mm) wide by 71 inches (1803 mm) long.

59 inches (1499 mm) wide by 95 inches (2413 mm) Long.

59 inches (1499 mm) wide by 95 inches (2413 mm) Long, handicapped accessible.

* + - * 1. Frame: 1-5/8 inch (41 mm) O.D. steel tube and 1/4 inch (6 mm) by 1 inch (25.5 mm) steel braces.
        2. Fasteners: Stainless steel.
        3. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 10 inch (51 by 254 mm):

Yellow Pine.

Douglas Fir.

Aluminum Slats.

As selected by the Architect from manufacturer's standard materials.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

Metal hot dip galvanized.

* + - 1. DuMor Wood Picnic Table 72:

\*\* NOTE TO SPECIFIER \*\* Select one the following size paragraphs and delete the one not required.

* + - * 1. Size:

59 inches (1499 mm) wide by 71 inches (1803 mm) long.

59 inches (1499 mm) wide by 95 inches (2413 mm) Long.

59 inches (1499 mm) wide by 95 inches (2413 mm) Long, handicapped accessible.

* + - * 1. Frame: 2-3/8 inch (60 mm) O.D. galvanized steel pipe and 1-5/16 inch (33 mm) O.D. galvanized steel pipe braces.
        2. Fasteners: Stainless steel.
        3. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 10 inch (51 by 254 mm):

Yellow Pine.

Douglas Fir.

Aluminum Slats.

As selected by the Architect from manufacturer's standard materials.

* + - * 1. Metal Finish: Triple layer, zinc flowcoat.
      1. DuMor Wood Picnic Table 75:

\*\* NOTE TO SPECIFIER \*\* Select one the following size paragraphs and delete the one not required.

* + - * 1. Size:

30 inches (1219 mm) wide by 71 inches (1803 mm) long.

30 inches (1219 mm) wide by 95 inches (2413 mm) Long.

30 inches (1219 mm) wide by 95 inches (2413 mm) Long, handicapped accessible.

* + - * 1. Supports: 3 inch (76 mm) by 1/4 inch (6 mm) thick square steel tube, 1/2 by 3 inch (12.5 by 76 mm) steel bar.
        2. Fasteners: Stainless steel.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 3 by 4 inch (76 by 102 mm) and 3 by 8 inch (76 by 204 mm):

Redwood.

Douglas Fir.

As selected by the Architect from manufacturer's standard materials.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

* + - * 1. Mounting:

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Embed 23-1/2 inches (597 mm) into a cast in place concrete foundation.

Subfloor 4 inches (102 mm) into a cast in place concrete floor.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Wood Picnic Table 77:

\*\* NOTE TO SPECIFIER \*\* Select one the following size paragraphs and delete the one not required.

* + - * 1. Size:

59 inches (1499 mm) wide by 71 inches (1803 mm) long.

59 inches (1499 mm) wide by 95 inches (2413 mm) Long.

59 inches (1499 mm) wide by 95 inches (2413 mm) Long, handicapped accessible.

* + - * 1. Frame: 2-3/8 inch (60 mm) O.D. steel pipe, 1-5/16 inch (33 mm) O.D. galvanized steel pipe braces and 2 by 1 by 1/8 inch (51 by 25.5 by 3 mm) center channel.
        2. Fasteners: Stainless steel.
        3. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 10 inch (51 by 254 mm):

Yellow Pine.

Douglas Fir.

Aluminum Slats.

As selected by the Architect from manufacturer's standard materials.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

Metal hot dip galvanized.

* + - 1. DuMor Aluminum Picnic Table 156PL:

\*\* NOTE TO SPECIFIER \*\* Select one the following size paragraphs and delete the one not required.

* + - * 1. Size:

59 inches (1499 mm) wide by 71 inches (1803 mm) long.

59 inches (1499 mm) wide by 95 inches (2413 mm) long.

59 inches (1499 mm) wide by 95 inches (2413 mm) long, handicapped accessible.

* + - * 1. Frame: 1-7/8 inch (48 mm) O.D. aluminum pipe and 3 by 2 by 3/16 inch (76 by 51 by 5 mm) aluminum angles.
        2. Table Top Brace: 1-5/16 inch (33 mm) O.D. aluminum pipe braces and 3 by 2 by 3/16 inch (76 by 51 by 5 mm) aluminum angles.
        3. Seat Brace: 3 by 2 by 3/16 inch (76 by 51 by 5 mm) aluminum angles.
        4. Fasteners: Stainless steel.
        5. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following color paragraphs as required and delete those not required.

* + - * 1. Plastic Slats: 2 by 10 inch (51 by 254 mm). recycled plastic. Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Mill finish is standard powder coat is optional. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

Mill finish.

Powder Coat: Color as selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + 1. Game Tables:
       1. DuMor Plastic Game Table 78PL:
          1. Size: 25-1/4 inch (641 mm) square.
          2. Frame: 1/4 inch (6 mm) thick steel angle.
          3. Center Post: 3 inch (76 mm) by 1/4 inch (6 mm).
          4. Seat Supports: 2-1/2 inch (57 mm) by 1/4 inch (6 mm) wall steel tube with 3/8 by 6 inch (9.5 by 152 mm) steel bar.
          5. Fasteners: Stainless steel.
          6. Game Board: 14 gauge (1.98 mm) aluminum.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 3 by 4 inch (76 by 102 mm) or 3 by 6 inch (76 by 152 mm) recycled plastic. Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

* + - * 1. Seats:

\*\* NOTE TO SPECIFIER \*\* Select paragraph for the number of seats required, delete the one not required.

Two seats.

Three seats.

Four seats.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

* + - * 1. Mounting:

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Embed 24 inches (610 mm) into a cast in place concrete foundation.

Subfloor 4 inches (102 mm) into a cast in place concrete floor.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Wood Game Table 78:
         1. Size: 25-1/4 inch (641 mm) square.
         2. Frame: 1/4 inch (6 mm) thick steel angle.
         3. Center Post: 3 inch (76 mm) by 1/4 inch (6 mm).
         4. Seat Supports: 2-1/2 inch (57 mm) by 1/4 inch (6 mm) wall steel tube with 3/8 by 6 inch (9.5 by 152 mm) steel bar.
         5. Fasteners: Stainless steel.
         6. Game Board: 14 gauge (1.98 mm) aluminum.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 3 by 4 inch (76 by 102 mm):

Redwood.

Douglas Fir.

As selected by the Architect from manufacturer's standard materials.

* + - * 1. Seats:

\*\* NOTE TO SPECIFIER \*\* Select paragraph for the number of seats required, delete the one not required.

Two seats.

Three seats.

Four seats.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

* + - * 1. Mounting:

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Embed 24 inches (610 mm) into a cast in place concrete foundation.

Subfloor 4 inches (102 mm) into a cast in place concrete floor.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* 1. PLANTERS
     1. Steel Planters.
        1. DuMor Planter 114: Companion to receptacle 84 and ash urn 80.
           1. Size: 28-1/4 inch (718 mm) diameter.
           2. Top Edge: 5/8 inch (16 mm) steel bar.
           3. Vertical Straps: 1/4 inch by 1-1/2 inch (6 by 38 mm) steel bar.
           4. Reveal Strip: 1/4 inch by 3 inch (6 by 76 mm) steel bar.
           5. Liner: Polyethylene.
           6. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter 115: Companion to bench 117 and receptacle 116.
         1. Size: 26-1/2 inch (673 mm) square.
         2. Frame: 2 by 1 inch (51 by 25.5 mm) by 13 gauge wall and 2 inch (51 mm) square 11 gauge steel tubing.
         3. Panel: 3/8 inch (9.5 mm) steel.
         4. Liner: 18 gauge (1.27 mm) steel.
         5. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter 122: Companion to receptacle 102 and ash urn 123.
         1. Size: 28 inch (711 mm) diameter.
         2. Top and Bottom Bands: 3/8 by 2-1/2 inch (9.5 by 64 mm) steel bar.
         3. Center Band: 3/8 by 2 inch (9.5 by 51 mm) steel.
         4. Vertical Straps: 1/2 by 1 inch (12.5 by 25 mm) steel bar.
         5. Reveal Strip: 1/4 inch by 2 inch (6 by 51 mm) steel bar.
         6. Rosettes: 4-1/4 inch (108 mm) diameter by 3/4 inch (19 mm) thick cast iron.

\*\* NOTE TO SPECIFIER \*\* Internal shield is optional delete if not required.

* + - * 1. Internal Shield: 18 gauge (1.27 mm) steel.
        2. Liner: Polyethylene.
        3. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter 128: Companion to receptacle 89.
         1. Size: 26-3/4 inch (679 mm) diameter.
         2. Frame: 1/4 inch by 2 inch (6 by 51 mm), 3/8 by 2 inch (9.5 by 51 mm) and 3/8 by 1 inch (9.5 by 25 mm) steel.
         3. Reveal Strip: 1/4 inch by 5 inch (6 by 127 mm) steel.
         4. Body: 16 gauge (1.58 mm) perforated steel.
         5. Liner: Polyethylene.
         6. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter 134: Companion to receptacle 133 and ash urn 135.
         1. Size: 30-5/16 inch (770 mm) diameter.
         2. Top Edge: 1 inch (25 mm) schedule 40 steel pipe.
         3. Vertical Straps: 3/8 by 1-1/2 inch (9.5 by 38 mm) steel bar.
         4. Reveal Strip: 1/4 inch by 3 inch (6 by 76 mm) steel bar.
         5. Liner: Polyethylene.
         6. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter 149: Companion to receptacle 148.
         1. Size: 28 inch (711 mm) diameter.
         2. Top and Bottom Bands: 3/8 by 2-1/2 inch (9.5 by 64 mm) steel bar.
         3. Center Band: 3/8 by 2 inch (9.5 by 51 mm) steel.
         4. Vertical Straps: 1/2 by 1 inch (12.5 by 25 mm) steel bar.
         5. Reveal Strip: 1/4 inch by 2 inch (6 by 51 mm) steel bar.
         6. Star Disks: 4-1/4 inch (108 mm) diameter by 3/4 inch (19 mm) thick cast iron.

\*\* NOTE TO SPECIFIER \*\* Internal shield is optional delete if not required.

* + - * 1. Internal Shield: 18 gauge (1.27 mm) steel.
        2. Liner: Polyethylene.
        3. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter 159: Companion to bench 19 and receptacle 158.
         1. Size: 29-3/4 inch (756 mm) diameter.
         2. Top Edge: 5/8 inch (16 mm) steel bar.
         3. Vertical Slats: 5/8 inch (16 mm) steel bar.
         4. Reveal Strip: 1/4 inch by 3 inch (6 by 76 mm) steel bar.
         5. Internal Shield: 18 gauge (1.27 mm) steel.
         6. Liner: Polyethylene.
         7. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter 171: Companion to receptacle 170.
         1. Size: 25-1/2 inch (648 mm) diameter.
         2. Frame: 1/4 inch by 1-1/2 inch (6 by 38 mm), 3/8 by 1-1/2 inch (9.5 by 38 mm) and 1-5/16 inch (33 mm) O.D. steel pipe Strip: 1/4 inch by 3 inch (6 by 127 mm) steel.
         3. Body: 16 gauge (1.58 mm) slotted perforated steel.
         4. Liner: Polyethylene.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required.

* + - * 1. Mounting:

Free Standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter 184: Companion to Receptacle 183
         1. Size: 32-1/2 inches (826 mm) diameter
         2. Top and bottom bands: 5/8 (16 mm) diameter steel bar.
         3. Vertical Straps: 1/4 inch by 1-1/2 inch (6 mm by 38 mm) steel bar.
         4. Liner: Polyethylene.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required.

* + - * 1. Mounting:

Free Standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter 189: Companion to Receptacle 182
         1. Height: 23 inches (584 mm)
         2. Width/Length: 25 inches (635 mm) square.
         3. Frame: Extruded aluminum and 1/8 inch thick (3 mm) aluminum plate
         4. Panel: 14 gauge slotted steel.
         5. Reveal strip: 1/4 inch by 1-1/2 inch (6 mm by 38 mm aluminum bar.
         6. Liner: Polyethylene.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required.

* + - * 1. Mounting:

Free Standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + 1. Plastic Planters.
       1. DuMor Planter 113PL: Companion to receptacle 44 or 70.
          1. Size: 24-13/16 inch (630 mm) diameter.
          2. Frame: 3/16 inch (5 mm) steel.
          3. Floor: 1/4 inch (6 mm) steel plate.
          4. Liner: 6 mil plastic.
          5. Fasteners: Stainless steel.
          6. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 1-1/2 inch (38 mm) thick recycled plastic. Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter 151PL: Companion to bench 57 and receptacle 124.
         1. Size: 28 inch (711 mm) diameter.
         2. Top and Bottom Bands: 3/8 by 2-1/4 inch (9.5 by 57 mm) steel bar.
         3. Center Band: 3/8 by 2 inch (9.5 by 51 mm) steel.
         4. Rosettes: 4-1/4 inch (108 mm) diameter by 3/4 inch (19 mm) thick cast iron.
         5. Liner: Polyethylene.
         6. Fasteners: Stainless steel.
         7. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 1-1/2 inch (38 mm) thick recycled plastic. Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter 153PL: Companion to bench 143 and receptacle 152.
         1. Size: 28 inch (711 mm) diameter.
         2. Top and Bottom Bands: 3/8 by 2-1/4 inch (9.5 by 57 mm) steel bar.
         3. Center Band: 3/8 by 2 inch (9.5 by 51 mm) steel.
         4. Rosettes: 4-1/4 inch (108 mm) diameter by 3/4 inch (19 mm) thick cast iron.
         5. Liner: Polyethylene.
         6. Fasteners: Stainless steel.
         7. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 2 by 4 inch (51 by 102 mm) recycled plastic. Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Model 180PL; Companion to receptacle 179PL.
         1. Dimensions: 23-3/4 inches (603 mm) by 24 inches (610 mm) square
         2. Top band: 1/4 inch by 3 inch (6.25 mm by 76 mm) steel plate.
         3. Bottom Plate: 1/4 inch (6.25 mm) by 26 inch (660 mm) square plasma cut steel plate.
         4. Decorative rings: 4-1/2 inch (114 mm) diameter by 1/2 inch (12.5 mm) wall by 1/2 inch (12.5 mm) thick.
         5. Frame: 1/4 inch by 1-1/2 inch (6.25 mm by 38 mm) steel bar.
         6. Fasteners: Stainless Steel.
         7. Liner: Polyethylene.
         8. Fasteners: Stainless steel.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required and delete the one not required.

* + - * 1. Mounting:

Free Standing.

Surface Plate with 1/2 inch by 3-3/4 inch (12.5 mm by 95 mm) stainless steel expansion bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 2 by 3 inch (51 by 76 mm) nom, and profiled recycled plastic. Plastic colors:

Cedar

Green

Gray

Redwood

Walnut

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + 1. Wood Planters.
       1. DuMor Planter 151: Companion to bench 57 and receptacle 124.
          1. Size: 28 inch (711 mm) diameter.
          2. Top and Bottom Bands: 3/8 by 2-1/4 inch (9.5 by 57 mm) steel bar.
          3. Center Band: 3/8 by 2 inch (9.5 by 51 mm) steel.
          4. Rosettes: 4-1/4 inch (108 mm) diameter by 3/4 inch (19 mm) thick cast iron.
          5. Liner: Polyethylene.
          6. Fasteners: Stainless steel.
          7. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 4 inch (51 by 102 mm) wood:

Redwood.

Douglas Fir.

Ipe.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter 153: Companion to bench 143 and receptacle 152.
         1. Size: 28 inch (711 mm) diameter.
         2. Top and Bottom Bands: 3/8 by 2-1/4 inch (9.5 by 57 mm) steel bar.
         3. Center Band: 3/8 by 2 inch (9.5 by 51 mm) steel.
         4. Rosettes: 4-1/4 inch (108 mm) diameter by 3/4 inch (19 mm) thick cast iron.
         5. Liner: Polyethylene.
         6. Fasteners: Stainless steel.
         7. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 2 by 4 inch (51 by 102 mm) wood:

Redwood.

Douglas Fir.

Ipe.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* 1. ASH URNS
     1. Steel Ash Urns.
        1. DuMor Ash Urn 18: Companion to receptacle 158.
           1. Size: 18-1/8 inch (460 mm) diameter by 28 inches (711 mm) high.
           2. Top Edge: 5/8 inch (16 mm) round steel bar.
           3. Vertical Straps: 5/8 inch (16mm) steel bar.
           4. Reveal Strip: 3/16 by 5 inch (4.8 mm by 127 mm) steel bar.
           5. Ash Pan: 10 inch (254 mm) diameter spun aluminum

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required.

* + - * 1. Mounting:

Free Standing.

Surface plate with 1/2 inch by 3-3/4 inch (12.5 mm by 95 mm) stainless steel anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Ash Urn 80: Companion to receptacle 84.
         1. Size: 16-5/8 inch (422 mm) diameter.
         2. Top Edge: 5/8 inch (16 mm) steel bar.
         3. Vertical Straps: 1/4 inch by 1-1/2 inch (6 by 38 mm) steel bar.
         4. Reveal Strip: 3/16 by 3 inch (4.8 mm by 76 mm) steel bar.
         5. Ash Pan: 10 inch (254 mm) diameter spun aluminum.
         6. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Ash Urn 123: Companion to receptacle 102 and planter 122.
         1. Size: 17-1/2 inch (445 mm) diameter.
         2. Top and Bottom Bands: 3/8 by 2-1/2 inch (9.5 by 64 mm) steel bar.
         3. Center Band: 3/8 by 2 inch (9.5 by 51 mm) steel.
         4. Rosettes: 4-1/4 inch (108 mm) diameter by 3/4 inch (19 mm) thick cast iron.

\*\* NOTE TO SPECIFIER \*\* Internal shield is optional, delete if not required.

* + - * 1. Internal Shield: 20 gauge steel.
        2. Ash Pan: 10 inch (254 mm) diameter spun aluminum.
        3. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Planter/Trash Receptacle 129: Companion to planter 128.
         1. Body: 18 gauge (1.2 mm) slotted perforated steel.
         2. Size: 13-3/8 inch (340 mm) diameter.
         3. Frame: 1 inch (25 mm) schedule 40 steel pipe and 1/4 inch by 2 inch (6 by 51 mm) steel.
         4. Body: 18 gauge (1.27 mm) perforated steel.
         5. Ash Pan: 10 inch (254 mm) diameter spun aluminum.
         6. Liner: 5 gal (22 l) galvanized steel.
         7. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Ash Urn 135: Companion to planter 134 and receptacle 133.
         1. Size: 13-3/8 inch (340 mm) diameter.
         2. Top Edge: 1 inch (25 mm) schedule 40 steel pipe.
         3. Vertical Straps: 3/8 by 1-1/4 inch (9.5 by 32 mm) steel bar.
         4. Reveal Strip: 1/4 inch by 3 inch (6 by 76 mm) steel bar.
         5. Ash Pan: 10 inch (254 mm) diameter spun aluminum.
         6. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Ash Urn 150: Companion to receptacle 148 and planter 149.
         1. Size: 17-1/2 inch (445 mm) diameter.
         2. Top and Bottom Bands: 3/8 by 2-1/2 inch (9.5 by 64 mm) steel bar.
         3. Center Band: 3/8 by 2 inch (9.5 by 51 mm) steel.
         4. Vertical Straps: 1/2 by 1 inch (12.5 by 25 mm) steel straps.
         5. Star Disk: 4-1/4 inch (108 mm) diameter by 3/4 inch (19 mm) thick cast iron.

\*\* NOTE TO SPECIFIER \*\* Internal shield is optional, delete if not required.

* + - * 1. Internal Shield: 20 gauge steel.
        2. Ash Pan: 10 inch (254 mm) diameter spun aluminum.
        3. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Ash Urn 172.
         1. Body: 18 gauge (1.2 mm) slotted perforated steel.
         2. Height: 27-15/16 inches (710 mm).
         3. Diameter: 13-3/8 inches (340 mm).
         4. Frame: 1 inch (25 mm) schedule 40 pipe, 1/4 inch (25 mm) by 2 inch (51 mm) and 1/7 inch (25 mm) by 3 inch (76 mm) HR steel.
         5. Ash Pan: Spun aluminum, 10 inch (254 mm) diameter.
         6. Mounting:

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

Free standing.

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Ash Urn 175: Companion to receptacle 107.
         1. Size: 15-7/8 inch (403 mm) diameter by 27-15/16 inches (710 mm) high
         2. Top Edge: 5/8 inch (16 mm) round steel bar
         3. Vertical Straps: 1/4 inch by 3/4 inch (6 mm by 19 mm) and 1/4 by 1-1/4 inch (6 mm by 32 mm) steel bar.
         4. Reveal Strip: 3/16 by 3 inch (4.8 mm by 76 mm) steel bar.
         5. Ash Pan: 10 inch (254 mm) diameter spun aluminum.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required.

* + - * 1. Mounting:

Free Standing.

Surface plate with 1/2 inch by 3-3/4 inch (12.5 mm by 95 mm) stainless steel anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + - 1. DuMor Ash Urn 176: Companion to receptacle 89.
         1. Size: 11-1/4 inch (340 mm) diameter by 26-1/2 inches (673 mm) high.
         2. Top Edge: 1/4 inch by 2 inch (6 mm by 51 mm) steel bar.
         3. Body: 18 gauge perforated steel.
         4. Reveal Strip: 3/16 by 3 inch (4.8 mm by 76 mm) steel bar.
         5. Ash Pan: 10 inch (254 mm) diameter spun aluminum.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required.

* + - * 1. Mounting:

Free Standing.

Surface plate with 1/2 inch by 3-3/4 inch (12.5 mm by 95 mm) stainless steel anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + 1. Plastic Ash Urns.
       1. DuMor Ash Urn 23PL:
          1. Size: 13-1/2 inch (343 mm) diameter by 25 inches (635 mm) high.
          2. Frame: 3/16 inch (5 mm) steel.
          3. Ash Pan: 10 inch (254 mm) diameter spun aluminum.
          4. Fasteners: Stainless steel.
          5. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following colors paragraphs as required and delete those not required.

* + - * 1. Slats: 1-1/2 inch (38 mm) recycled plastic. Plastic colors:

Cedar.

Green.

Gray.

Redwood.

Walnut Plastic.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* + 1. Wood Ash Urns.
       1. DuMor Ash Urn 23:
          1. Size: 13-1/2 inch (343 mm) diameter by 25 inches (635 mm) high.
          2. Frame: 3/16 inch (5 mm) steel.
          3. Ash Pan: 10 inch (254 mm) diameter spun aluminum.
          4. Fasteners: Stainless steel.
          5. Mounting: Free Standing.

\*\* NOTE TO SPECIFIER \*\* Select one the following wood paragraphs as required and delete those not required.

* + - * 1. Wood Slats: 1-1/2 inch (38 mm) thick:

Redwood.

Douglas Fir.

As selected by the Architect from manufacturer's standard colors.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the one not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors: Powder coated.

As selected by the Architect from manufacturer's 11 standard colors.

Custom color as selected by the Architect.

* 1. BIKE RACKS
     1. Bike Racks.
        1. DuMor Bike Racks 81 and 82 Series:

\*\* NOTE TO SPECIFIER \*\* Select one the following models and delete the one not required.

* + - * 1. Series 81: Single side entry bike rack.
        2. Series 82: Dual side entry bike rack.

\*\* NOTE TO SPECIFIER \*\* Select one the following size paragraphs and delete the one not required.

* + - * 1. Size:

61 inches (1549 mm) long.

121 inches long (3073 mm) long.

* + - * 1. Frame: 1-5/8 inch (41 mm) galvanized steel pipe.
        2. Vertical Wheel Supports: 5/8 inch (16 mm) galvanized steel pipe.
        3. Caps: Domed plated steel welded in place.
        4. Metal Finish: Triple layer, zinc flowcoat.
        5. Fasteners: Stainless steel.
        6. Mounting: Free Standing.
      1. DuMor Bike Racks 83-00 / 83-00G Series:
         1. Size: 16-1/2 inches (419 mm) by 35-1/2 inch (902 mm) high.
         2. Frame: 2-3/8 inch (41 mm) O.D. by 11 gauge (3.17 mm) wall galvanized steel pipe.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete those not required.

* + - * 1. Mounting:

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm)stainless steelexpansion anchor bolts.

Embed 12 inches (305 mm) into a cast in place concrete foundation.

Subfloor 4 inches (102 mm) into a cast in place concrete floor.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the ones not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors:

Powder coated as selected by the Architect from manufacturer's 11 standard colors.

Metal Finish: Triple layer, zinc flowcoat.

Powder coated custom color as selected by the Architect.

* + - 1. DuMor Bike Racks 125 and 130 Series:

\*\* NOTE TO SPECIFIER \*\* Select one the following size paragraphs as required, delete those not required.

* + - * 1. Size Model 125: 2-7/8 inch (73 mm) O.D. schedule 40 steel pipe frame.

5 Bike.

7 Bike.

9 Bike.

11 Bike.

13 Bike.

* + - * 1. Size Model 130: 2-3/8 inch (41 mm) O.D. schedule 40 steel pipe.

5 Bike.

7 Bike.

9 Bike.

11 Bike.

13 Bike.

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

* + - * 1. Mounting:

Surface plate with 1/2 by 3-3/4 inch (12.5 by 95 mm) stainless steel expansion anchor bolts.

Embed 24 inches (610 mm) into a cast in place concrete foundation.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the ones not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors:

Powder coated as selected by the Architect from manufacturer's 11 standard colors.

Hot dip galvanized.

Powder coated custom color as selected by the Architect.

* + - 1. DuMor Bike Rack 188

\*\* NOTE TO SPECIFIER \*\* Select one the following size paragraphs as required, delete those not required.

* + - * 1. Size:

41-1/4 inches (1048 mm) long, 5 openings.

57-1/4 inches (1454) long, 7 openings.

73-1/4 inches (1861 mm) long, 9 openings.

89-1/4 inches (2267 mm) long, 11 openings.

105-1/4 inches (2673 mm) long, 13 openings.

121-1/4 inches (3080 mm) long, 15 openings.

* + - * 1. Frame: 2 inch by 1 inch by 13 gauge (51 mm by 12.5 mm by 2.28 mm) and 2 inch square by 11 gauge (51 mm square by 3.17 mm) steel tube
        2. Vertical wheel supports: 3/4 inch square by 11 gauge (19 mm square by 3.17 mm) steel tube.
        3. Caps: Cast iron

\*\* NOTE TO SPECIFIER \*\* Select one the following mounting types as required and delete the one not required.

* + - * 1. Mounting:

Embedment

Surface plate with 1/2 inch by 3-3/4 inch (12.5 mm by 95 mm) stainless steel anchor bolts.

\*\* NOTE TO SPECIFIER \*\* Select one the following paragraphs as required, delete the ones not required. Custom colors are available at additional cost.

* + - * 1. Metal Finish and Colors:

Powder coated as selected by the Architect from manufacturer's 11 standard colors.

Hot dip galvanized.

Powder coated custom color as selected by the Architect.

1. EXECUTION
   1. EXAMINATION
      1. Do not begin installation until substrates have been properly prepared.
      2. If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
   2. PREPARATION
      1. Clean surfaces thoroughly prior to installation.
      2. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
   3. INSTALLATION
      1. Install in accordance with manufacturer's instructions.
      2. Embedded mounting. Material is to be extended a minimum of 12 inches (305 mm) below finish surface and cast in concrete.
      3. Surface mounting. Location and drilling of holes for inserts included. Anchor bolts and inserts provided by others.
   4. PROTECTION
      1. Protect installed products until completion of project.
      2. Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION