SECTION  10 57 36

BARN DOOR ASSEMBLIES

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2026 -  2026 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Hall 3-Lite Barn Door Assembly.
B.	Salinas Z-Design.
C.	Cristo 1-Lite Barn Door Assembly.
D.	Stone-K Design Barn Door Assembly.
E.	Sagrada Double-X Design Barn Door Assembly.
F.	Pavilion 5-Lite Barn Door Assembly.
G.	Herringbone Chevron Design Barn Door Assembly.
H.	Easy-Build, Stone K-Design Barn Door Assembly.
I.	Easy Build, Langley Arrow Design Barn Door Assembly.
J.	Easy-Build, Salinas Z-Design Barn Door Assembly.
K.	Easy-Build, Pavilion 5-LIte Barn Door Assembly.
L.	Easy-Build, Authentic Cross-Brace Design Barn Door Assembly.
M.	Tribeca 6-Lite Barn Door Assembly.
N.	Tribeca 8-Lite Barn Door Assembly.
O.	Stone K Design Barn Door Assembly.
1.2	RELATED SECTIONS
A.	Section 08 14 16 - Flush Wood Doors
B.	Section 08 14 33 - Stile and Rail Wood Doors
C.	Section 08 71 00 - Door Hardware.
1.3	REFERENCES
A.	International Code Council (ICC):
1.	International Building Code, 2024 Edition.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Verification Samples: Two representative units of each type, size, pattern, and color.
D.	Shop Drawings: Include details of materials, construction, and finish. Include relationship with adjacent construction.
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum of five (5) years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two (2) years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
D.	Latching hardware complies with requirements of 2024 IBC, paragraph 1010.2.1 for single motion unlatching.
E.	Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
1.	The intent of a mock-up is to demonstrate quality of workmanship and visual appearance.
2.	If the mock-up is not acceptable, rebuild the mock-up until satisfactory results are achieved.
3.	Retain mock-up during construction as a standard for comparison with completed work. 
4.	Do not alter or remove mock-up until work is completed or removal is authorized.
1.6	PRE-INSTALLATION CONFERENCE
A.	Convene a conference approximately two (2) weeks before scheduled commencement of the Work. Attendees include Architect, Contractor and trades involved. Agenda includes schedule, responsibilities, critical path items and approvals.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.8	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.9	WARRANTY
A.	Manufacturer's standard limited warranty unless indicated otherwise.
B.	RENIN/ACME warrants products for a period of five (5) years from date of purchase. 
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Renin/Acme, which is located at:<BR />110 Walker Dr.<BR />Brampton, ON, Canada L6T 4H6<BR />Tel: 905-791-7930<BR />Fax: 905-791-3813<BR />Email: request info (info@renin.com);Web: https://www.renin.com | https://www.renin.com/us/wholesale-commercial/acme-hardware-systems/ 
B.	Acceptable Manufacturer: Renin/Acme, which is located at:<BR />110 Walker Dr.<BR />Brampton, ON, Canada L6T 4H6<BR />Tel: 905-791-7930<BR />Fax: 905-791-3813<BR />Email: request info (info@renin.com);Web: https://www.renin.com | https://www.renin.com/us/wholesale-commercial/acme-hardware-systems/ 
C.	Substitutions: Not permitted.
D.	Requests for substitutions will be considered in accordance with the provisions of Section 01 60 00.
2.2	HALL 3-LITE BARN DOOR ASSEMBLY
A.	Basis of Design: Model BD061. Hall 3-Lite Barn Door Assembly, as manufactured and supplied by Renin.
1.	Door Assembly: Prefinished solid engineered wood sliding barn door with three glass lites, door slab only. 
2.	Door Assembly: Prefinished solid engineered wood sliding barn door with three glass lites, complete assembly with hanging system and hardware. 
3.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
4.	Door Thickness: 1-3/8 inches (35 mm).
5.	Door Style and Color:
a.	Finish: Bright White with a scratch resistant smooth finish - requires no painting or staining.
b.	Finish: Espresso with a scratch resistant smooth wood grain look - requiring no painting or staining.
c.	Finish: Iron Age with a scratch resistant smooth wood grain look - requiring no painting or staining.
6.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle, and floor guide in a Rustic Matte Black finish.
a.	Soft Close hardware.
b.	Easy Latch Privacy Lock.
c.	Tear Drop Latch.
2.3	SALINAS Z-DESIGN BARN DOOR ASSEMBLY
A.	Basis of Design: Model BD053. Salinas Z-Design Barn Door Assembly, as manufactured and supplied by Renin.
1.	Door Assembly: Unfinished rustic solid pine sliding barn door with Z-design, door slab only.
2.	Door Assembly: Unfinished rustic solid pine sliding barn door with Z-design, complete assembly with hanging system and hardware.
3.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
4.	Door Dimensions (HxW): 42 x 84 inches (1067 x 2134 mm).
5.	Door Thickness: 1-3/8 inches (35 mm).
6.	Door Style and Color: Z-Design, unfinished.
7.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle and floor guide in a Rustic Matte Black finish.
2.4	CRISTO 1-LITE BARN DOOR ASSEMBLY.
A.	Basis of Design: Model BD054. Cristo 1-Lite Barn Door Assembly, as manufactured and supplied by Renin.
1.	Door Assembly: Prefinished solid engineered wood sliding barn door with one glass lite, door slab only. 
2.	Door Assembly: Prefinished solid engineered wood sliding barn door with one glass lite, complete assembly with hanging system and hardware. 
3.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
4.	Door Thickness: 1-3/8 inches (35 mm).
5.	Door Style and Color: Iron Age with a scratch resistant smooth wood grain look - requiring no painting or staining.
6.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle and floor guide in a Rustic Matte Black finish.
a.	Soft Close hardware.
b.	Easy Latch Privacy Lock Hardware Kit.
c.	Tear Drop Latch.
2.5	STONE-K DESIGN BARN DOOR ASSEMBLY
A.	Basis of Design: Model BD052. Stone K-Design Barn Door Assembly, as manufactured and supplied by Renin.
1.	Door Assembly: Prefinished wood sliding barn door with K-design, door slab only.
2.	Door Assembly: Prefinished wood sliding barn door with K-design, complete assembly with hanging system and hardware. 
3.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
4.	Door Dimensions (HxW): 42 x 84 inches (1067 x 2134 mm).
5.	Door Thickness: 1-3/8 inches (35 mm).
6.	Door Style and Color:
a.	Finish: Off White with a scratch resistant smooth finish - requires no painting or staining.
b.	Finish: Sandstone with a scratch resistant smooth wood grain look - requiring no painting or staining.
c.	Finish: Silver Oak with a textured wood grain look - requires no painting or staining.
d.	Finish: Iron Age with a scratch resistant smooth wood grain look - requiring no painting or staining.
7.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle and floor guide in a Rustic Matte Black finish.
a.	Soft Close hardware.
2.6	SAGRADA DOUBLE-X DESIGN BARN DOOR ASSEMBLY
A.	Basis of Design: Model BD060. Sagrada Double X-Design Barn Door Assembly, as manufactured and supplied by Renin.
1.	Door Assembly: Prefinished wood sliding barn door with double X-design, door slab only.
2.	Door Assembly: Prefinished wood sliding barn door with double X-design, complete assembly with hanging system and hardware.
3.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
4.	Door Thickness: 1-3/8 inches (35 mm).
5.	Door Style and Color:
a.	Finish: Cherry smooth wood grain look, requires no painting or staining.
b.	Finish: Gunstock Oak with a textured wood grain look, requires no painting or staining.
6.	Hardware: All hardware included. Hardened steel, bent strap hardware,matching handle and floor guide in a Rustic Matte Black finish.
2.7	PAVILION 5-LITE BARN DOOR ASSEMBLY
A.	Basis of Design: Model BD062. Pavilion 5-Lite Barn Door Assembly, as manufactured and supplied by Renin.
1.	Door Assembly: Prefinished wood sliding barn door with five tempered frosted glass inserts, door slab only.
2.	Door Assembly: Prefinished wood sliding barn door with five tempered frosted glass inserts, complete assembly with hanging system and hardware.
3.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
4.	Door Thickness: 1-3/8 inches (35 mm).
5.	Door Style and Color:
a.	Finish: Bright White with a textured wood grain look - requires no painting or staining.
b.	Finish: Iron Age smooth wood grain look - requires no painting or staining.
6.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle and floor guide in a Rustic Matte Black finish.
2.8	HERRINGBONE CHEVRON DESIGN BARN DOOR ASSEMBLY
A.	Basis of Design: Model BD059. Herringbone Chevron-Design Barn Door Assembly, as manufactured and supplied by Renin.
1.	Door Assembly: Prefinished wood sliding barn door with chevron plank design, door slab only.
2.	Door Assembly: Prefinished wood sliding barn door with chevron plank design, complete assembly with hanging system and hardware.
3.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
4.	Door Thickness: 1-3/8 inches (35 mm).
5.	Door Style and Color:
a.	Finish: Satin Nickel Grey - Hand-Stained Solid Wood Finish, requires no painting or staining. 
b.	Finish: Ashen Grey with a scratch resistant smooth finish, requires no painting or staining.
c.	Finish: Ashen White with a scratch resistant smooth finish, requires no painting or staining.
6.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle and floor guide in a Rustic Matte Black finish.
a.	Soft Close hardware.
b.	Easy Latch Privacy Lock Hardware Kit.
c.	Tear Drop Latch.
2.9	EASY-BUILD, STONE K-DESIGN BARN DOOR KIT
A.	Basis of Design: Model BD052. Easy Build, Stone K-Design Barn Door Kit, as manufactured and supplied by Renin.
1.	Prefinished wood sliding barn door kit with K-design.
2.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
3.	Door Dimensions (HxW): 42 x 84 inches (1067 x 2134 mm).
4.	Door Thickness: 1-3/8 inches (35 mm).
5.	Door Style and Color:
a.	Finish: Bright White with a textured wood grain look - requires no painting or staining.
6.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle and floor guide in a Rustic Matte Black finish.
2.10	EASY BUILD, LANGLEY ARROW DESIGN BARN DOOR KIT
A.	Basis of Design: Model BD136. Easy Build, Langley Arrow Design Barn Door Kit, as manufactured and supplied by Renin.
1.	Prefinished wood sliding barn door kit with Arrow-design.
2.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
3.	Door Thickness: 1-3/8 inches (35 mm).
4.	Door Style and Color:
a.	Finish: Graphite Gray with a wood grain painted look, requires no painting or staining.
5.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle and floor guide in a Rustic Matte Black finish.
2.11	EASY-BUILD, SALINAS Z-DESIGN BARN DOOR KIT
A.	Basis of Design: Model BD053. Easy Build, Salinas Z-Design Barn Door Kit, as manufactured and supplied by Renin.
1.	Unfinished rustic solid pine sliding barn door with Z-design.
2.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
3.	Door Thickness: 1-3/8 inches (35 mm).
4.	Door Style and Color:
a.	Finish: Natural wood treated with a thin coat of clear primer - requires painting or staining.
5.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle and floor guide in a Rustic Matte Black finish.
2.12	EASY-BUILD, PAVILION 5-LITE BARN DOOR KIT
A.	Basis of Design: Model BD062. Pavilion 5-Lite Barn Door Kit, as manufactured and supplied by Renin.
1.	Prefinished wood sliding barn door kit with five tempered frosted glass inserts.
2.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
3.	Door Thickness: 1-3/8 inches (35 mm).
4.	Door Style and Color:
a.	Finish: Bright White with a textured wood grain look, requires no painting or staining.
5.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle and floor guide in a Rustic Matte Black finish.
2.13	EASY-BUILD, AUTHENTIC CROSS-BRACE DESIGN BARN DOOR KIT
A.	Basis of Design: Model BD069. Authentic Cross-Brace Design Barn Door Kit, as manufactured and supplied by Renin.
1.	Prefinished wood sliding barn door kit with cross-brace design.
2.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
3.	Door Thickness: 1-3/8 inches (35 mm).
4.	Door Style and Color:
a.	Finish: Bright White with a textured wood grain look, requires no painting or staining.
b.	Finish: Iron Age Grey with a smooth wood grain look, requires no painting or staining.
5.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle and floor guide in a Rustic Matte Black finish.
2.14	TRIBECA 6-LITE BARN DOOR ASSEMBLY
A.	Basis of Design: Model BD073. Contemporary 6-Lite Barn Door Assembly, as manufactured and supplied by Renin.
1.	Door Assembly: Prefinished aluminum frame with six tempered frosted glass inserts, door slab only.
2.	Door Assembly: Prefinished aluminum frame with six tempered frosted glass inserts, complete assembly with hanging system and hardware.
3.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
4.	Door Thickness: 1-3/8 inches (35 mm).
5.	Door Style and Color:
a.	Finish: Matte Black finish, requires no painting or staining.
6.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle and floor guide in a Rustic Matte Black finish.
2.15	TRIBECA 8-LITE BARN DOOR ASSEMBLY
A.	Basis of Design: Model BD074. Contemporary 8-Lite Barn Door Assembly, as manufactured and supplied by Renin.
1.	Door Assembly: Prefinished aluminum frame with eight tempered frosted glass inserts, door slab only.
2.	Door Assembly: Prefinished aluminum frame with eight tempered frosted glass inserts, complete assembly with hanging system and hardware.
3.	Door Dimensions (HxW): 36 x 84 inches (914 x 2134 mm).
4.	Door Thickness: 1-3/8 inches (35 mm).
5.	Door Style and Color:
a.	Finish: Matte Black finish, requires no painting or staining.
6.	Hardware: All hardware included. Hardened steel, bent strap hardware, matching handle and floor guide in a Rustic Matte Black finish.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until the substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install barn door assemblies in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
3.4	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturer's recommendations. 
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION