SECTION 28 25 00

VIDEO SURVEILLANCE POSITIONING EQUIPMENT

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2024 -  2024 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Security Camera Poles:
1.	SteadyMax poles.
2.	Square, 4 inch poles.
3.	Square Direct Bury poles.
B.	Building mounts.
1.	HD corner mount.
2.	HD parapet wall camera mount.
3.	Arm with dual gussets, 2 foot.
4.	Fly-out mount.
5.	Fly-over mount.
6.	Parapet PTZ camera mount.
7.	Reacher mount, 5 foot.
8.	Camera mounts with built-in junction box.
9.	Wall mount bracket.
10.	Surface mount pole and plate.
C.	Keypad and Reader Pedestals:
1.	Dual height keypad pedestals.
2.	Touch-less reader pedestals.
3.	Gooseneck direct-burial keypad pedestals.
4.	Heavy duty architectural keypad and reader pedestals.
5.	Gooseneck keypad and reader pedestals.
D.	LED Lighting:
1.	Select-A-Watt LED area lights.
2.	LED area lights.
E.	Accessories.
1.2	RELATED SECTIONS
A.	Section 03 30 00 - Cast-in-Place Concrete.
B.	Section 07 84 13 - Penetration Firestopping.
C.	Section 26 05 48 - Vibration and Seismic Controls for Electrical Systems.
D.	Section 27 05 29 - Hangers and Supports for Communications Systems.
1.3	REFERENCES
A.	American Association of State Highway and Transportation Officials (AASHTO):
1.	AASHTO LTS - Standard Specifications for Structural Supports for Highway Signs, Luminaires and Traffic Signals 2013 (Revised 2019).
B.	Florida Building Code 2017.
C.	Institute of Electrical and Electronics Engineers (IEEE):
1.	IEEE C2 - National Electrical Safety Code 2017.
D.	National Electrical Contractors Association (NECA):
1.	NECA 1 - Standard for Good Workmanship in Electrical Construction 2015.
2.	NECA 303 - Standard for Installing and Maintaining Closed-Circuit Television (CCTV) Systems 2019.
E.	National Electrical Manufacturers Association (NEMA):
1.	NEMA/UL Enclosure Ratings.
F.	Underwriters Laboratories (UL).
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Verification Samples: Two representative units of each type, size, pattern and color.
D.	Shop Drawings: Include details of materials, construction and finish. Include relationship with adjacent construction. 
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
D.	Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
1.	Intent of mock-up is to demonstrate quality of workmanship and visual appearance.
2.	If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
3.	Retain mock-up during construction as a standard for comparison with completed work. 
4.	Do not alter or remove mock-up until work is completed or removal is authorized.
1.6	PRE-INSTALLATION CONFERENCE
A.	Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.8	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.9	WARRANTY
A.	Manufacturer's standard limited warranty unless indicated otherwise.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: StrongPoles, which is located at:<BR />203 N. Elm St.<BR />Kemp, TX 75143<BR />Toll Free Tel: 844-669-3537<BR />Tel: 903-498-0980<BR />Fax: 844-319-3025<BR />Email: request info (sales@strongpoles.com);Web: https://www.strongpoles.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	SECURITY CAMERA POLES
A.	Performance Requirements:
1.	Standards Compliance: 
a.	AASHTO LTS.
2.	Wind Load: Include effective projected area (EPA) of cameras, supports, and accessories to be installed.
a.	Design Wind Speed: 190 mph (306 kph).
b.	Design Wind Speed: 150 mph (241 kph).
c.	Design Wind Speed: As indicated on Drawings.
d.	Design Wind Speed: As required by Code.
e.	Design Wind Speed: ____ mph (____ kph).
f.	Gust Factor: 1.3.
3.	Dead Load: Include weight of proposed cameras, supports, and accessories.
B.	General:
1.	Provide poles suitable for cameras, supports, and accessories to be installed.
2.	Included Parts:
a.	Hand hole at 18 inches (457 mm) from base.
b.	Hand hole at 48 inches (1219 mm) from base.
c.	Ground lug, accessible from handhole.
d.	Top cap.
e.	Anchor bolts with leveling nuts or leveling shims.
f.	Anchor base cover.
g.	Pole-top tenon, size as required for installed camera/bracket.
h.	Cables as indicated or as required for connections between system components.
i.	Accessory racks and cabinets as indicated or as required for equipment mounting.
3.	Mounting: Install on concrete foundation, unless otherwise indicated.
C.	Basis of Design: SteadyMax Camera Poles; as manufactured by StrongPoles, LLC.
1.	Pole Configuration: As indicated on Drawings.
2.	Pole Configuration:
a.	Shape: Round.
1)	Diameter: 6 inches (152 mm).
2)	Diameter: 8 inches (203 mm).
b.	Tapered.
c.	Straight, not tapered.
d.	Height: 12 feet (3658 mm).
e.	Height: 16 feet (4877 mm).
f.	Height: 20 feet (6096 mm).
g.	Height: 25 feet (7620 mm).
h.	Height: _____.
3.	Features:
a.	Factory installed vibration suppression system.
b.	Maximum movement of 3 percent.
4.	Material: 6063-T6 aluminum.
5.	Finish: White powder coat.
6.	Finish: Dark bronze powder coat.
D.	Basis of Design: SteadyMaxFL Camera Poles; as manufactured by StrongPoles, LLC.
1.	Standards Compliance: 
a.	Florida Building Code 2017.
2.	Pole Configuration: As indicated on Drawings.
3.	Pole Configuration:
a.	Shape: Round.
b.	Diameter: 6 inches (152 mm).
c.	Straight, not tapered.
d.	Height: 12 feet (3658 mm).
4.	Features:
a.	Factory installed vibration suppression system.
b.	Maximum movement of 3 percent.
5.	Material: 6063-T6 aluminum.
6.	Finish: White powder coat.
7.	Finish: Dark bronze powder coat.
E.	Basis of Design: 4 inch Square Camera Poles; as manufactured by StrongPoles, LLC.
1.	Pole Configuration: As indicated on Drawings.
2.	Pole Configuration:
a.	Shape: Square.
b.	Size: 4 inches (102 mm).
c.	Straight, not tapered.
d.	Height: 5 feet (1524 mm).
e.	Height: 8 feet (2438 mm).
f.	Height: 12 feet (3658 mm).
g.	Height: _____.
3.	Mounting Base: Fixed base.
4.	Mounting Base: Tilt over base.
5.	Anchor Basket: None.
6.	Anchor Basket: Fixed anchor basket.
7.	Anchor Basket: Tilt over anchor basket.
8.	Hand Hole Cover: Blank.
9.	Hand Hole Cover: Single 1 inch (25 mm) hole.
10.	Hand Hole Cover: Two 1 inch (25 mm) holes.
11.	Material: 6005-T5 aluminum.
12.	Finish: White powder coat.
13.	Finish: Dark bronze anodized.
F.	Basis of Design: Square Direct Bury Poles; as manufactured by StrongPoles, LLC.
1.	Pole Configuration: As indicated on Drawings.
2.	Pole Configuration:
a.	Shape: Square.
b.	Size: 4 inches (102 mm).
1)	Height: 12 feet (3658 mm), buried 4 feet (1219 mm).
2)	Height: 16 feet (4877 mm), buried 5 feet (1524 mm).
3)	Height: 20 feet (6096 mm), buried 5 feet (1524 mm).
4)	Height: _____.
c.	Size: 5 inches (127 mm).
1)	Height: 8 feet (2438 mm), buried 4 feet (1219 mm).
2)	Height: 11 feet (3353 mm), buried 4 feet (1219 mm).
3)	Height: 16 feet (4877 mm), buried 5 feet (1524 mm).
4)	Height: 20 feet (6096 mm), buried 5 feet (1524 mm).
5)	Height: 25 feet (7620 mm), buried 5 feet (1524 mm).
6)	Height: _____.
d.	Straight, not tapered.
3.	Material: Aluminum.
4.	Finish: White powder coat.
5.	Finish: Dark bronze powder coat.
2.3	BUILDING MOUNTS
A.	Basis of Design: HD Corner Mount; as manufactured by StrongPoles, LLC.
1.	Description: Mounts to exterior corner of building.
2.	Dimensions: 11 x 9 x 9 inches (279 x 229 x 229 mm).
3.	Color: White.
4.	Color: Dark Bronze.
B.	Basis of Design: HD Parapet Wall Camera Mount; as manufactured by StrongPoles, LLC.
1.	Description: For mounting PTZ security cameras and wireless devices to parapet walls. Mounts to interior of parapet walls.
2.	Dimensions: 62 x 28 x 6 inches (1575 x 711 x 152 mm).
3.	Features:
a.	Folds back to parapet interior to allow easy access to mounted equipment.
b.	Adjustable angle.
4.	Included Options:
a.	Parapet extension.
b.	Twin PTZ adapter.
5.	Color: White.
6.	Color: Dark Bronze.
C.	Basis of Design: 2 Foot Arm with Dual Gussets; as manufactured by StrongPoles, LLC.
1.	Description: Supports any PTZ, camera, or accessory that fits 1-1/2 inch (38 mm) NPT fitting.
2.	Mounting Plate: 3.5 x 6 inches (89 x 162 mm).
3.	Dimensions: 24 x 4 x 6 inches (610 x 102 x 152 mm).
4.	Flourish: None.
5.	Flourish: Included.
6.	Color: White.
7.	Color: Dark Bronze.
D.	Basis of Design: Fly-Out Mount; as manufactured by StrongPoles, LLC.
1.	Description: Supports any PTZ, camera, or accessory that fits 1-1/2 inch (38 mm) NPT fitting.
2.	Mounting Plate: 3 x 6 inches (76 x 152 mm).
3.	Dimensions: 36 x 21 x 6 inches (914 x 533 x 152 mm).
4.	Wall Mount Bracket: None.
5.	Wall Mount Bracket: Included.
6.	Color: White.
7.	Color: Dark Bronze.
E.	Basis of Design: Fly-Over Mount; as manufactured by StrongPoles, LLC.
1.	Description: Designed to get structure as far away from the camera as possible, 1-1/2 inch (38 mm) NPT fitting.
2.	Mounting Plate: 3 x 6 inches (76 x 152 mm).
3.	Dimensions: 52 x 28 x 6 inches (1321 x 711 x 152 mm).
4.	Color: White.
5.	Color: Dark Bronze.
F.	Basis of Design: Parapet PTZ Camera Mount; as manufactured by StrongPoles, LLC.
1.	Description: For mounting PTZ security cameras and wireless devices to parapet walls. Mounts to interior of parapet walls.
2.	Dimensions: 52 x 28 x 6 inches (1321 x 711 x 152 mm).
3.	Features:
a.	Folds back to parapet interior to allow easy access to mounted equipment.
b.	Adjustable angle.
4.	Attachments:
a.	Dome camera mount.
b.	Dual dome camera mount.
c.	Twin adapter.
5.	Color: White.
6.	Color: Dark Bronze.
G.	Basis of Design: 5 Foot Reacher Mount; as manufactured by StrongPoles, LLC.
1.	Description: Designed to reach out over a property line or fence.
2.	Dimensions: 65 x 16 x 16 inches (1651 x 406 x 406 mm).
3.	Mounting: Pole mount, 6-7 inch (152-178 mm) round.
4.	Mounting: Pole mount, 4 inch (102 mm) square.
5.	Mounting: Pole mount, 5 inch (127 mm) square.
6.	Mounting: Corner mount.
7.	Mounting: Flat mount.
8.	Color: White.
9.	Color: Dark Bronze.
H.	Basis of Design: Camera Mounts with Built-In Junction Box; as manufactured by StrongPoles, LLC.
1.	Description: Provides three different faces for camera mounting.
2.	Dimensions: 14 x 11 x 8 inches (356 x 279 x 203 mm).
3.	Mounting: Corner mount.
4.	Mounting: Flat mount.
5.	Color: White.
6.	Color: Dark Bronze.
I.	Basis of Design: Wall Mount Bracket; as manufactured by StrongPoles, LLC.
1.	Description: For mounting 4 inch (102 mm) square poles to wall or parapet.
2.	Dimensions: 13 x 13 x 5 inches (330 x 330 x 127 mm).
3.	Color: White.
4.	Color: Dark Bronze.
J.	Basis of Design: Surface Mount Pole and Plate; as manufactured by StrongPoles, LLC.
1.	Description: For mounting under building eaves or from building faces.
2.	Length: 15 inches (381 mm).
3.	Length: 30 inches (762 mm).
4.	Length: 48 inches (1219 mm).
5.	Color: White.
6.	Color: Dark Bronze.
7.	Color: Hammered Black.
2.4	KEYPAD AND READER PEDESTALS
A.	Basis of Design: Dual Height Keypad Pedestals; as manufactured by StrongPoles, LLC.
1.	Description: Dual height pad mounted pedestal for cars and big trucks.
2.	Dimensions: 79 x 19 x 9 inches (2007 x 483 x 229 mm).
3.	Color: White.
4.	Color: Dark Bronze.
B.	Basis of Design: Touch-Less Reader Pedestals; as manufactured by StrongPoles, LLC.
1.	Description: For mounting single or multiple contact-less card readers, RFID, or reader antennas.
2.	Dimensions: 54 x 9 x 9 inches (1372 x 229 x 229 mm).
3.	Top: Pyramid.
4.	Top: Flat.
5.	Color: White.
6.	Color: Dark Bronze.
C.	Basis of Design: Gooseneck Direct-Burial Keypad Pedestals; as manufactured by StrongPoles, LLC.
1.	Description: Can be buried 2 feet (610 mm).
2.	Dimensions: 70 x 13 x 13 inches (1778 x 330 x 330 mm).
3.	Features:
a.	Anti-turn paddles.
b.	Below ground wire gland.
4.	Color: White.
5.	Color: Dark Bronze.
D.	Basis of Design: Heavy Duty Architectural Keypad and Reader Pedestals; as manufactured by StrongPoles, LLC.
1.	Dimensions: 54 x 19 x 9 inches (1372 x 483 x 229 mm).
2.	Top: Pyramid.
3.	Color: White.
4.	Color: Dark Bronze.
E.	Basis of Design: Gooseneck Keypad and Reader Pedestals; as manufactured by StrongPoles, LLC.
1.	Model: 36 inch (914 mm) curb-mount.
2.	Model: 42 inch (1067 mm) pad-mount.
3.	Model: 48 inch (1219 mm) pad-mount.
4.	Model: 42 inch (1067 mm) direct burial.
5.	Color: Black hammered.
2.5	LED LIGHTING
A.	Basis of Design: Select-A-Watt LED Area Light; as manufactured by StrongPoles, LLC.
1.	Compliance: UL Certified.
2.	Description : Switchable LED lights.
3.	Dimensions: 24 x 18 x 8 inches (610 x 457 x 203 mm).
4.	Body Material: Die-cast aluminum.
5.	Color Temperature: 3000K.
6.	Color Temperature: 4000K.
7.	Color Temperature: 5000K.
8.	Color Temperature: 5700K.
9.	Optics: Type III.
10.	Optics: Type IV.
11.	Optics: Type V.
12.	Mounting: Square and round pole mount.
13.	Mounting: Adjustable square and round pole mount.
14.	Mounting: Slip fitter mount.
15.	Mounting: Trunnion mount.
16.	Voltage: AC120-277.
17.	Wattage: 80-150W.
18.	Wattage: 240-310W.
19.	Minimum Temperature Rating: Minus 40 degrees F (minus 40 degrees C).
20.	Finish: Dark Bronze.
21.	Accessories:
a.	External half glare shield.
b.	External 360 full visor.
c.	Photocell control.
d.	Shorting cap control.
e.	PIR motion sensor control.
f.	Surge protection device.
B.	Basis of Design: LED Area Lights; as manufactured by StrongPoles, LLC.
1.	Compliance: UL Listed.
2.	Dimensions: 20 x 17 x 6 inches (508 x 432 x 152 mm).
3.	Color Temperature: 4000K.
4.	Color Temperature: 5000K.
5.	Optics: Type III.
6.	Voltage: AC120-277.
7.	Wattage: 100W.
8.	Wattage: 150W.
9.	Wattage: 200W.
10.	Wattage: 250W.
11.	Wattage: 300W.
2.6	ACCESSORIES
A.	Camera Pole Anchor Basket, 4 inch (102 mm):
1.	Description: For anchoring to a poured concrete foundation.
2.	Fixed base anchor basket.
3.	Tilt over anchor basket.
B.	Pole Top Mounting Pedestal:
1.	Dimensions: 13 x 10 x 4 inches (330 x 254 x 102 mm).
2.	Color: White.
3.	Color: Dark Bronze.
C.	Antenna Top Mount Mast:
1.	Dimensions: 48 x 4 x 4 inches (1219 x 102 x 102 mm).
2.	Color: White.
3.	Color: Dark Bronze.
D.	Antenna Mast for Birdhouse:
1.	Dimensions: 40 x 12 x 12 inches (1016 x 305 x 305 mm).
2.	Color: White.
3.	Color: Dark Bronze.
E.	Side Mount Antenna Mast use:
1.	Dimensions: 36 x 6 x 3 inches (914 x 152 x 76 mm).
2.	Color: White.
3.	Color: Dark Bronze.
F.	Wrap Around Mount:
1.	Dimensions: 16 x 9 x 9 inches (406 x 229 x 229 mm).
2.	Mount: With RR mount.
3.	Mount: Without RR mount.
4.	Color: White.
5.	Color: Dark Bronze.
G.	Fence-Guard Mount:
1.	Dimensions: 49 x 16 x 16 inches (1245 x 406 x 406 mm).
2.	Mount: Pole.
3.	Mount: Corner.
4.	Mount: Flat.
5.	Color: White.
6.	Color: Dark Bronze.
H.	Square Pedestal, 8 inch (203 mm) :
1.	Dimensions: 8 x 8 x 8 inches (203 x 203 x 203 mm).
2.	Top Mount Pedestal: Single mount.
3.	Top Mount Pedestal: HD single mount.
4.	Top Mount Pedestal: HD twin mount.
5.	Color: White.
6.	Color: Dark Bronze.
I.	Junction Box, 6 x 6:
1.	Dimensions: 8 x 8 x 8 inches (203 x 203 x 203 mm).
2.	Color: White.
3.	Color: Dark Bronze.
J.	Birdhouse Mounting Platform:
1.	Size: 8 x 10 inches (203 x 254 mm).
2.	Size: 8 x 16 inches (203 x 406 mm).
3.	Mount: With SP-RR mount.
4.	Mount: Without SP-RR mount.
5.	Color: White.
6.	Color: Dark Bronze.
K.	Light Pole Adapter:
1.	Dimensions: 20 x 20 x 15 inches (508 x 508 x 381 mm).
2.	Hardware: Without hardware.
3.	Hardware: With 5/8 inch (16 mm) pole mounting hardware.
4.	Shims: With shims.
5.	Shims: Without shims.
6.	Color: White.
7.	Color: Dark Bronze.
L.	SteadyMax Pole Enclosure Mounts:
1.	Mounting Bar Length: 8 inches (203 mm).
2.	Mounting Bar Length: 16 inches (406 mm).
3.	Caps: White.
4.	Caps: Black.
5.	Caps: None.
6.	Clamp Size: Regular, 4 to 8 inches (102 to 203 mm).
7.	Clamp Size: XL, 4 to 12 inches (102 to 305 mm).
M.	Panoramic Camera Mount:
1.	Dimensions: 11 x 9 x 9 inches (279 x 229 x 229 mm).
2.	Color: White.
3.	Color: Dark Bronze.
N.	StrongMount-44:
1.	Compliance: NEMA/UL 4X.
2.	Material: Polycarbonate.
3.	Camera Mounting Area: 4 x 4 inches (102 x 102 mm).
4.	Inside Depth: 2-1/2 inches (64 mm).
5.	Finish: High gloss.
O.	StrongMount-55:
1.	Compliance: NEMA/UL 6P.
2.	Material: Polycarbonate.
3.	Camera Mounting Area: 4-3/4 x 4-3/4 inches (121 x 121 mm).
4.	Inside Depth: 3 inches (76 mm).
5.	Finish: High gloss.
P.	StrongMount-66:
1.	Compliance: NEMA/UL 6P.
2.	Material: Polycarbonate.
3.	Camera Mounting Area: 5-3/4 x 5-3/4 inches (146 x 146 mm).
4.	Inside Depth: 3 inches (76 mm).
5.	Finish: High gloss.
Q.	StrongMount-86:
1.	Compliance: NEMA/UL 6P.
2.	Material: Polycarbonate.
3.	Camera Mounting Area: 7-3/4 x 5-3/4 inches (197 x 146 mm).
4.	Inside Depth: 3 inches (76 mm).
5.	Finish: High gloss.
R.	StrongMount-98:
1.	Compliance: NEMA/UL 6P.
2.	Material: Polycarbonate.
3.	Camera Mounting Area: 8-1/2 x 7-1/2 inches (216 x 190 mm).
4.	Inside Depth: 2-1/2 inches (64 mm).
5.	Finish: High gloss.
S.	StrongMount-2016:
1.	Compliance: NEMA/UL 6P.
2.	Material: Polycarbonate.
3.	Camera Mounting Area: 20 x 16 inches (508 x 406 mm).
4.	Inside Depth: 8-1/2 inches (216 mm).
5.	Finish: High gloss.
T.	Dome Camera Mount:
1.	Dimensions: 13 x 10 x 4 inches (330 x 254 x 102 mm).
2.	Color: White.
3.	Color: Dark Bronze.
U.	Dual Camera Mount with PTZ Adapter:
1.	Dimensions: 12 x 8 x 6 inches (305 x 203 x 152 mm).
2.	Color: White.
3.	Color: Dark Bronze.
V.	Side Mount Platform:
1.	Dimensions: 7 x 7 x 4 inches (178 x 178 x 102 mm).
2.	Color: White.
3.	Color: Black.
W.	Dual Dome/Bullet Adapter:
1.	Dimensions: 12 x 8 x 6 inches (305 x 203 x 152 mm).
2.	Color: White.
3.	Color: Dark Bronze.
X.	Horizontal Tenon, 6 inch:
1.	Dimensions: 7 x 7 x 4 inches (178 x 178 x 102 mm).
2.	Color: White.
3.	Color: Dark Bronze.
Y.	Vertical Tenon, 4 inch:
1.	Dimensions: 12 x 7 x 5 inches (305 x 178 x 127 mm).
2.	Color: White.
3.	Color: Dark Bronze.
Z.	Twin PTZ Adapter:
1.	Dimensions: 19 x 8 x 3 inches (483 x 203 x 76 mm).
2.	Color: White.
3.	Color: Dark Bronze.
AA.	Modular Accessory Platform:
1.	Dimensions: 10 x 10 x 13 inches (254 x 254 x 330 mm).
2.	Bottom Plate: 1-1/2 inch (38 mm) threaded connector.
3.	Bottom Plate: Blank plate.
4.	Color: White.
5.	Color: Black.
AB.	Modular Junction Box:
1.	Bottom Plate: 1-1/2 inch (38 mm) threaded connector.
2.	Bottom Plate: Blank plate.
3.	Color: White.
4.	Color: Black.
AC.	Junction Box with Side Mounts:
1.	Dimensions: 13 x 10 x 4 inches (330 x 254 x 102 mm).
2.	Plates: Threaded top and bottom plates.
3.	Plates: Threaded top plate, solid bottom plate.
4.	Color: White.
5.	Color: Black.
AD.	Pipe Clamp Strong Strut Mounting Bars:
1.	Mounting Bar Length: 8 inches (203 mm).
2.	Mounting Bar Length: 16 inches (406 mm).
3.	Cap Color: White.
4.	Cap Color: Black.
5.	Cap Color: None.
AE.	Beam Clamp Strong Strut Mounting Bars:
1.	Mounting Bar Length: 8 inches (203 mm).
2.	Mounting Bar Length: 16 inches (406 mm).
3.	Cap Color: White.
4.	Cap Color: Black.
5.	Cap Color: None.
AF.	Egyptian Style Strong Strut Mounting Bars. :
1.	Mounting Bar Length: 8 inches (203 mm).
2.	Mounting Bar Length: 16 inches (406 mm).
3.	Bar: Single bar.
4.	Bar: Double bar.
5.	Cap Color: White.
6.	Cap Color: Black.
7.	Cap Color: None.
AG.	TV Mount Bolts.
AH.	TV Mount:
1.	Dimensions: 4 x 4 x 4 inches (102 x 102 x 102 mm).
2.	Color: White.
3.	Color: Black.
AI.	Junction and MAP Hand Hole Gasket:
1.	Color: White.
2.	Color: Black.
AJ.	Junction and MAP 4 x 4 inch Gasket:
1.	Dimensions: 4 x 4 inches (102 x 102 mm).
2.	Color: White.
3.	Color: Black.
AK.	Strong Strut Nut without Spring, 3/8 inch (9.5 mm).
AL.	MP810 1.5 inch (38 mm) Cap, Main Holes:
1.	Color: White.
2.	Color: Black.
AM.	MP68 1-1/8 inch (29 mm) Cap, Main Holes:
1.	Color: White.
2.	Color: Black.
AN.	MP68 Multi-Purpose Hand Hole Cover with 2 Screws:
1.	Holes: One.
2.	Holes: Two.
3.	Holes: None.
4.	Color: White.
5.	Color: Dark Bronze.
AO.	MAP Caps, Small Holes:
1.	Color: White.
2.	Color: Black.
AP.	MAP 1.5 inch (38 mm) Cap, Main Holes:
1.	Color: White.
2.	Color: Black.
AQ.	MAP Main Body:
1.	Dimensions: 13 x 10 x 4 inches (330 x 254 x 102 mm).
2.	Color: White.
3.	Color: Black.
AR.	Junction 5/8-11x1 BH Torx Screw.
AS.	Junction Hand Hole Cover with 2 Screws:
1.	Color: White.
2.	Color: Black.
AT.	Junction and MAP Top Plate with 1.5 inch (38 mm) Threaded Cover:
1.	Color: White.
2.	Color: Black.
AU.	Junction and MAP Full Bottom Plate with 4 Holes:
1.	Color: White.
2.	Color: Black.
AV.	Junction Main Body:
1.	Dimensions: 4 x 4 x 7 inches (102 x 102 x 178 mm).
2.	Color: White.
3.	Color: Black.
AW.	Strong Strut - 10 foot (3048 mm):
1.	Round: Short round.
2.	Round: Long round.
AX.	TV Suspension Mounts:
1.	Type: Single.
2.	Type: Pair.
AY.	CamBlox - No Drill Solutions:
1.	Type: Single wide, 8 x 8 x 3 inches (203 x 203 x 76 mm).
2.	Type: Double wide, 8 x 12 x 3 inches (203 x 305 x 76 mm).
3.	Type: Triple wide, 8 x 16 x 3 inches (203 x 406 x 76 mm).
4.	Mount: Beam clamp.
5.	Mount: Pipe clamp.
6.	Mount: Pendant mount.
7.	Color: White.
8.	Color: Dark Bronze.
AZ.	Multi-Purpose 6 x 8 Box, MP-68:
1.	Color: White.
2.	Color: Black.
BA.	Egyptian-Style Ceiling Mount:
1.	Color: White.
2.	Color: Black.
BB.	Pipe Drop with 1.5 inch to 1.5 inch (38 mm to 38 mm) Double Alum Pipe Coupler with 2 Set Screws:
1.	Length: 8 inches (203 mm).
2.	Length: 19-1/2 inches (495 mm).
3.	Length: 4 feet (1219 mm).
4.	Length: 6 feet (1829 mm).
5.	Length: 8 feet (2438mm).
6.	Length: 10 feet (3048 mm).
7.	Color: White.
8.	Color: Dark Bronze.
BC.	NPT Female to Female Coupler, 1-1/2 inch (38 mm):
1.	Color: White.
2.	Color: Dark Bronze.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Verify that field measurements are as indicated.
B.	Verify that ratings and configurations of system components are consistent with the indicated requirements.
C.	Verify that mounting surfaces are ready to receive system components.
D.	Verify that branch circuit wiring installation is completed, tested, and ready for connection to system where applicable.
E.	Verify that conditions are satisfactory for installation prior to starting work.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
B.	Install video surveillance system in accordance with NECA 1, general workmanship, and NECA 303.
C.	Provide required support and attachment in accordance with Division 26.
D.	Pole-Mounted Cameras:
1.	Maintain the following minimum clearances:
a.	Comply with IEEE C2.
b.	Comply with utility company requirements.
2.	Foundation-Mounted Poles:
a.	Provide cast-in-place concrete foundations for poles as indicated; see Section 03 30 00 - Cast-in-Place Concrete.
1)	Install anchor bolts plumb using template furnished by pole manufacturer.
2)	Position conduits to enter pole shaft.
b.	Install foundations plumb.
c.	Install poles plumb, using leveling nuts or shims as required to adjust to plumb.
d.	Tighten anchor bolt nuts to manufacturer's recommended torque.
e.	Install nonshrink grout between pole anchor base and concrete foundation, leaving small channel for condensation drainage.
f.	Install anchor base covers or anchor bolt covers as indicated.
3.	Embedded Poles: Install poles plumb.
E.	Provide grounding and bonding in accordance with Division 26.
F.	Install firestopping to preserve fire resistance rating of partitions and other elements, using materials and methods specified in Section 07 84 13 - Penetration Firestopping.
G.	Identify system wiring and components in accordance with Division 26.
3.4	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.
3.5	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturer's recommendations. 
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION