SECTION 14 42 00

WHEELCHAIR LIFTS - VERTICAL

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2008 -  2026 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Vertical Permanently-Installed Wheelchair Lifts.
1.	Virtuoso 5460F.	 
2.	Protege 5442F.	 
B.	Vertical Permanently-Installed Wheelchair Lifts with Upper Landing Gate.		 
1.	Virtuoso 5460FG.	 
2.	Protege 5442FG.	 
C.	Vertical Portable Wheelchair Lifts.
1.	Virtuoso 5460P. 
2.	Protege 5442P.
1.2	RELATED SECTIONS
A.	Section 14 42 16 - Vertical Wheelchair Lifts.
B.	Section 26 05 00 - Common Work Results for Electrical.
1.3	REFERENCES
A.	ADA Accessibility Guidelines for Buildings and Facilities (ADAAG).
B.	ASME A17.5 - Elevator and Escalator Electrical Equipment.
C.	ASME A18.1 - Safety Standard for Platform Lifts and Stairway Chairlifts.
D.	ANSI A117.1 - Accessible and Usable Buildings and Facilities.
E.	NFPA 70 (NEC) - National Electrical Code.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings: Drawings will show dimensional and wiring requirements.
D.	Verification Samples: For each finish product specified, two samples, 2 x 3 inches (50 x 75 mm) representing actual product, color, and patterns.
1.5	QUALITY ASSURANCE
A.	Manufacturer will have not less than twenty years of experience in the design and manufacture of vertical wheelchair lifts.
B.	Installer Qualifications: Minimum 2 year experience installing similar products.
1.6	PRE-INSTALLATION MEETINGS
A.	Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees will include Architect, Contractor and trades involved. Agenda will include schedule, responsibilities, critical path items and approvals.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Deliver and store products in manufacturer's unopened packaging bearing the brand name and manufacturer's identification until ready for installation.
B.	Handle materials to avoid damage.
1.8	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.9	SEQUENCING
A.	Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
1.10	WARRANTY
A.	Manufacturer will provide a warranty for a period of ten years on the drive train, four years on all other components, and 90 days on labor, starting from the date of installation.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Ascension, a division of AGM, which is located at: 3526 E. Ft. Lowell Rd.; Tucson, AZ 85716; ASD Toll Free Tel: 800-459-0400; Tel:  520-881-3993. Fax: 520-881-4983; Email: WebSales@ascension-lift.com. Web: https://www.ascension-lift.com.
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	VERTICAL PERMANENTLY-INSTALLED WHEELCHAIR LIFTS (Virtuoso 5460F)
A.	Lift Product: Virtuoso 5460F as manufactured by Ascension. Unenclosed, self-contained vertical wheelchair lift for use by individuals with disabilities. Raises and lowers platform and occupant providing accessibility to stages, platforms, or similar elevated surfaces.
1.	Low Profile: No machine tower, to maintain viewing lines.
2.	Platform: Supported by an electro-hydraulic lifting mechanism.
3.	Independent Use: By individuals with disabilities.
4.	ADA Compliant: Includes applicable operating and safety devices.
5.	Platform Floor: Low-profile facilitating entry to the lift. Eliminates need for an installation pit or an access ramp at lower landing end. 
6.	Self-supported Unit: No anchoring to facility beyond anchors at base of lift. 
B.	Physical Characteristics:
1.	Lifting capacity: 750 lbs (340 kg).
2.	Weight of Lift: 1025 lbs (465 kg) maximum.
3.	Vertical Speed: 7 ft per min (2.1 mpm).
4.	Vertical Travel: 12 to 60 inches (305 to 1524 mm), infinitely adjustable.
C.	Platform Gate Configuration:
1.	Lower Gate:
a.	Manual Operation: Left handed. Hydraulic door closer.
b.	Manual Operation: Right handed. Hydraulic door closer.
c.	Automatic Operation: Left handed. Powered door operators.
d.	Automatic Operation: Right handed. Powered door operators.
2.	Upper Gate: 
a.	Manual Operation: Left handed. Hydraulic door closer.
b.	Manual Operation: Right handed. Hydraulic door closer.
c.	Automatic Operation: Left handed. Powered door operators.
d.	Automatic Operation: Right handed. Powered door operators.
D.	Dimensions:
1.	No part of lift to be over 44 inches (1117 mm) high when platform is on the ground; except when equipped with optional stage guard.
2.	Required Clear Space (WxL): 51.25 x 64.25 inches (1302 x 1632 mm).
3.	Lift Dimensions (WxLxH): 47.25 x 62.75 x 44 inches (1200 x 1594 x 1118 mm).
4.	Platform Clear Space: 36 x 54 inches (914 x 1371 mm). 
a.	Sidewalls and Platform Gates: 43 inches (1092 mm) high.
E.	Materials:
1.	Platform, Base Frame, and Lifting Device: ASTM A 36 or similar low-carbon steel.
2.	Windows: 1/4 inch (6 mm) thick high impact strength clear thermoplastic.
3.	Safety Skirt: Constructed from neoprene-coated nylon with PVC stiffeners.
F.	Finish:
1.	Exposed Metal Surfaces: Finished by powder coating.
a.	Color: Black.
b.	Color: ______.
G.	Drive Configuration: Direct-acting hydraulic.
1.	Synchronized Dual Hydraulic Cylinders: Evenly support both sides of lift platform.
2.	Hydraulic Power Unit: Mounted on vibration-isolating supports minimizing vibration transmission and reducing frame-borne noise.
H.	Electrical Requirements:
1.	Amperage Draw per Lift:  15 Amps maximum.
2.	Service Line:  120 VAC, 60 hertz. Amperage capacity:  15 Amps.
3.	Motor:  1/2 hp, 115 V AC single phase.
4.	Control Circuits: 24 VDC. 
5.	Electrical System:  Certified to ASME A17.5 by independent testing laboratory.
I.	Lift Safety Devices: 
1.	Lift Construction:  Meet applicable requirements of ASME A18.1, ASME A17.5, ADAAG, ANSI 117.1, and NFPA 70 (NEC). 
2.	Included Safety Features: For passenger and general public protection.
a.	Safety Skirt: Completely encloses and protects area under platform.
1)	Switches:  Stop platform movement in case of excess skirt deflection.
b.	Operating Switches:  Constant pressure.
c.	Emergency Stop Button:  Lighted, sounds audible alarm.
d.	Electro-Mechanical Interlock:  Prevents accidental opening of lower platform gate, and if provided, the upper landing gate.
e.	Gate Switches:  Prevent operation if either platform gate is open.
f.	Hand Pump:  Allows platform to manually be raised or lowered.
g.	Sidewalls and Platform Gates:  43 inches (1092 mm) high.
1)	Visibility:  Unobstructed view. Transparent sidewalls and platform gates.
h.	Lift platform stop height sensor.
i.	Platform Floor:  Low profile and slip resistant surface. 
j.	No installation pit or external access ramp at the lower landing.
k.	Full length frame integrated grab bar.
J.	Compression Capability: May be compressed to 33 inches (838 mm) wide facilitating relocation through a 36 inch (914 mm) wide doorway.
1.	Compression Tool Kit: Recommended to facilitate compression of the lift. From Ascension.
K.	Add-Ons: 
1.	Automatic Standby Power (Battery Backup):  Minimum 5 lift cycles at full load during power outage events. 
2.	Two-Way Communication:  Hands-free autodialing phone on platform. 
3.	Universal Keys:  Limits lift use to authorized persons.
4.	Auxiliary Lighting: Provides lighting when facility power is lost. 
5.	Safety Pan: Safely stops lift if platform is obstructed during downward travel.
2.3	VERTICAL PERMANENTLY-INSTALLED WHEELCHAIR LIFTS (Protege 5442F)
A.	Lift Product: Protege 5442F as manufactured by Ascension. Unenclosed, self-contained vertical wheelchair lift for use by individuals with disabilities. Raises and lowers platform and occupant providing accessibility to stages, platforms, or similar elevated surfaces.
1.	Requires minimal modifications to using facility. 
2.	Low Profile: No machine tower to maintain viewing lines. 
3.	Platform: Supported by an electro-hydraulic lifting mechanism. 
4.	Independent Use: By individuals with disabilities
5.	ADA Compliant: Includes applicable operating and safety devices.
6.	Platform Floor: Low-profile facilitating entry to the lift. Eliminates need for a pit or access ramp at the lower landing end. 
7.	Self-supported Unit: No anchoring to facility beyond anchors at base of lift.  
B.	Physical Characteristics: 
1.	Lifting Capacity: 900 pounds (408 kg).
2.	Weight of Lift: 850 pounds maximum (386 kg).
3.	Vertical Speed: 5 fpm (1.5 mpm).
4.	Vertical Travel: 4 to 42 inches (102 to 1067 mm), infinitely adjustable.
C.	Platform Gate Configuration:
1.	Lower Gate:
a.	Manual Operation: Left handed. Hydraulic door closer.
b.	Manual Operation: Right handed. Hydraulic door closer.
c.	Automatic Operation: Left handed. Powered door operators.
d.	Automatic Operation: Right handed. Powered door operators.
2.	Upper Gate: 
a.	Manual Operation: Left handed. Hydraulic door closer.
b.	Manual Operation: Right handed. Hydraulic door closer.
c.	Automatic Operation: Left handed. Powered door operators.
d.	Automatic Operation: Right handed. Powered door operators.
D.	Dimensions:
1.	No part of lift to be over 49 inches (1245 mm) high when platform is on the ground except when equipped with optional stage guard.
2.	Required Clear Space (WxL): 51.63 x 60.75 inches (1311 x 1543 mm).
3.	Lift Dimensions (WxLxH): 47.63 x 58.25 x 49 inches (1210 x 1480 x 1245 mm).
4.	Platform Clear Space: 36 x 54 inches (914 x 1372 mm).
E.	Materials:
1.	Platform, Base Frame, and Lifting Device: ASTM A 36 or similar low-carbon steel.
2.	Windows: 1/4 inch (6 mm) thick high impact strength clear thermoplastic.
3.	Platform Sheet Metal and Under-Platform Safety Pan: 1/16 inch (1.6 mm) aluminum alloy.
F.	Finish:
1.	Exposed Metal Surfaces: Finished by powder coating.
a.	Color: Black.
b.	Color: ______.
2.	Base Frame: Hot-dip galvanized.
G.	Drive Configuration: Direct-acting hydraulic.
1.	Synchronized Dual Hydraulic Cylinders: Evenly support both sides of lift platform.
2.	Hydraulic Power Unit: Mounted on vibration-isolating supports minimizing vibration transmission and reducing frame-borne noise.
H.	Electrical Requirements:
1.	Amperage Draw per Lift:  13 Amps maximum.
2.	Service Line:  120 VAC, 60 hertz. Amperage capacity:  Exceeding 13 Amps.
3.	Motor:  1/2 hp, 115 V AC single phase.
4.	Control Circuits: 24 VDC. 
5.	Electrical System:  Certified to ASME A17.5 by independent testing laboratory.
I.	Lift Safety Devices:
1.	Lift Construction:  Meet applicable requirements of ASME A18.1, ASME A17.5, ADAAG, ANSI 117.1, and NFPA 70 (NEC). 
2.	Included Safety Features:  For passenger and general public protection.
a.	Operating Switches:  Constant pressure.
b.	Emergency Stop Button:  Lighted, sounds audible alarm.
c.	Electro-Mechanical Interlock:  Prevents accidental opening of lower platform gate, and if provided, the upper landing gate.
d.	Gate Switches:  Prevent operation if either platform gate is open.
e.	Hand Pump:  Allows platform to manually be raised or lowered.
f.	Sidewalls and Platform Gate Heights:  48 inches (1220 mm).
1)	Visibility:  Unobstructed view. Transparent sidewalls and platform gates.
g.	Lift platform stop height sensor.
h.	Under-Platform Safety Pan:  Safely stops lift if platform is obstructed during downward travel.
i.	Platform Floor:  Low profile and slip resistant surface.
j.	No installation pit or external access ramp at the lower landing.
k.	Full length grab bar. 
J.	Compression Capability: May be compressed to 33 inches (838 mm) wide facilitating relocation through a 36 inch (914 mm) wide doorway.
1.	Compression Tool Kit: Recommended to facilitate compression of the lift. From Ascension.
K.	Add-Ons: 
1.	Automatic Standby Power (Battery Backup):  Minimum 5 lift cycles at full load during power outage events. 
2.	Two-Way Communication:  Hands-free autodialing phone on platform. 
3.	Universal Keys:  Limits lift use to authorized persons. 
4.	Shaftway Package:  For installation in a hoistway/shaftway. 
5.	Auxiliary Lighting: Provides lighting when facility power is lost.
2.4	VERTICAL PERMANENTLY-INSTALLED WHEELCHAIR LIFTS WITH UPPER LANDING GATE (Virtuoso 5460FG)			 
A.	Lift Product: Virtuoso 5460FG as manufactured by Ascension. Unenclosed, self-contained vertical wheelchair lift with a fixed upper landing gate for use by individuals with disabilities. Raises and lowers platform and occupant providing accessibility to stages, platforms, or similar elevated surfaces.		 
1.	Low Profile: No machine tower, to maintain viewing lines.	 
2.	Platform: Supported by an electro-hydraulic lifting mechanism.	 
3.	Independent Use: By individuals with disabilities.	 
4.	ADA Compliant: Includes applicable operating and safety devices.	 
5.	Platform Floor: Low-profile facilitating entry to the lift. Eliminates need for an installation pit or an access ramp at lower landing end.	 
6.	Self-supported Unit: No anchoring to facility beyond anchors at base of lift. 	 
B.	Physical Characteristics: 		 
1.	Lifting capacity: 750 lbs (340 kg).	 
2.	Weight of Lift: 1025 lbs (465 kg) maximum.	 
3.	Vertical Speed: 7 ft per min (2.1 mpm).	 
4.	Vertical Travel: 12 to 60 inches (305 to 1524 mm), infinitely adjustable.	 
C.	Platform and Upper Landing Gate Configuration:		 
1.	Lower Platform Gate:	 
a.	Manual Operation: Left handed. Hydraulic door closer. 
b.	Manual Operation: Right handed. Hydraulic door closer. 
c.	Automatic Operation: Left handed. Powered door operators. 
d.	Automatic Operation: Right handed. Powered door operators. 
2.	Upper Landing Gate: Stationary gate mounted at the upper landing that guards against falling onto the lift from the upper landing. For applications that require guard rails be installed at the upper landing.	 
a.	Manual Operation: Left handed. Hydraulic door closer. 
b.	Manual Operation: Right handed. Hydraulic door closer. 
c.	Automatic Operation: Left handed. Powered door operators. 
d.	Automatic Operation: Right handed. Powered door operators. 
D.	Dimensions:		 
1.	No part of lift to be over 44 inches (1117 mm) high when platform is on the ground; except when equipped with optional stage guard.	 
2.	Required Clear Space (WxL): 51.25 x 64.25 inches (1302 x 1632 mm).	 
3.	Lift Dimensions (WxLxH): 47.25 x 62.75 x 44 inches (1200 x 1594 x 1118 mm).	 
4.	Platform Clear Space: 36 x 54 inches (914 x 1371 mm). 	 
a.	Sidewalls and Platform Gates: 43 inches (1092 mm) high. 
E.	Materials:		 
1.	Platform, Base Frame, and Lifting Device: ASTM A 36 or similar low-carbon steel.	 
2.	Windows: 1/4 inch (6 mm) thick high impact strength clear thermoplastic.	 
3.	Safety Skirt: Constructed from neoprene-coated nylon with PVC stiffeners.	 
F.	Finish:		 
1.	Exposed Metal Surfaces: Finished by powder coating.	 
a.	Color: Black. 
b.	Color: ______. 
G.	Drive Configuration: Direct-acting hydraulic.		 
1.	Synchronized Dual Hydraulic Cylinders: Evenly support both sides of lift platform.	 
2.	Hydraulic Power Unit: Mounted on vibration-isolating supports minimizing vibration transmission and reducing frame-borne noise.	 
H.	Electrical Requirements: 	 
1.	Amperage Draw per Lift: 15 Amps maximum.	 
2.	Service Line: 120 VAC, 60 hertz. Amperage capacity: 15 Amps.	 
3.	Motor: 1/2 hp, 115 V AC single phase.	 
4.	Control Circuits: 24 VDC.	 
5.	Electrical System: Certified to ASME A17.5 by independent testing laboratory.	 
I.	Lift Safety Devices: 		 
1.	Lift Construction: Meet applicable requirements of ASME A18.1, ASME A17.5, ADAAG, ANSI 117.1, and NFPA 70 (NEC). 	 
2.	Included Safety Features: For passenger and general public protection.	 
a.	Safety Skirt: Completely encloses and protects area under platform. 
1)	Switches: Stop platform movement in case of excess skirt deflection.					 
b.	Operating Switches: Constant pressure. 
c.	Emergency Stop Button: Lighted, sounds audible alarm. 
d.	Electro-Mechanical Interlock: Prevents accidental opening of lower platform gate, and if provided, the upper landing gate. 
e.	Gate Switches: Prevent operation if either platform gate is open. 
f.	Hand Pump: Allows platform to manually be raised or lowered. 
g.	Sidewalls and Platform Gates: 43 inches (1092 mm) high. 
1)	Visibility: Unobstructed view. Transparent sidewalls and platform gates.					 
h.	Lift platform stop height sensor. 
i.	Platform Floor: Low profile and slip resistant surface.  
j.	No installation pit or external access ramp at the lower landing. 
k.	Full length frame integrated grab bar. 
J.	Compression Capability: May be compressed to 33 inches (838 mm) wide facilitating relocation through a 36 inch (914 mm) wide doorway.	 
1.	Compression Tool Kit: Recommended to facilitate compression of the lift. From Ascension.	 
K.	Add-Ons:		 
1.	Automatic Standby Power (Battery Backup): Minimum 5 lift cycles at full load during power outage events.	 
2.	Two-Way Communication: Hands-free autodialing phone on platform.	 
3.	Universal Keys: Limits lift use to authorized persons.	 
4.	Auxiliary Lighting: Provides lighting when facility power is lost.	 
5.	Safety Pan: Safely stops lift if platform is obstructed during downward travel.
2.5	VERTICAL PERMANENTLY-INSTALLED WHEELCHAIR LIFTS WITH UPPER LANDING GATE (Protege 5442FG)				 
A.	Lift Product: Protege 5442FG as manufactured by Ascension. Unenclosed, self-contained vertical wheelchair lift with a fixed upper landing gate for use by individuals with disabilities. Raises and lowers platform and occupant providing accessibility to stages, platforms, or similar elevated surfaces.			 
1.	Requires minimal modifications to using facility. 		 
2.	Low Profile: No machine tower to maintain viewing lines. 		 
3.	Platform: Supported by an electro-hydraulic lifting mechanism. 		 
4.	Independent Use: By individuals with disabilities		 
5.	ADA Compliant: Includes applicable operating and safety devices.		 
6.	Platform Floor: Low-profile facilitating entry to the lift. Eliminates need for a pit or access ramp at the lower landing end.		 
7.	Self-supported Unit: No anchoring to facility beyond anchors at base of lift. 		 
B.	Physical Characteristics: 			 
1.	Lifting Capacity: 900 pounds (408 kg).		 
2.	Weight of Lift: 850 pounds maximum (386 kg).		 
3.	Vertical Speed: 5 fpm (1.5 mpm).		 
4.	Vertical Travel: 4 to 42 inches (102 to 1067 mm), infinitely adjustable.		 
C.	Platform and Upper Landing Gate Configuration:			 
1.	Lower Platform Gate:		 
a.	Manual Operation: Left handed. Hydraulic door closer.	 
b.	Manual Operation: Right handed. Hydraulic door closer.	 
c.	Automatic Operation: Left handed. Powered door operators.	 
d.	Automatic Operation: Right handed. Powered door operators.	 
2.	Upper Landing Gate: Stationary gate mounted at the upper landing that guards against falling onto the lift from the upper landing. For applications that require guard rails be installed at the upper landing.		 
a.	Manual Operation: Left handed. Hydraulic door closer.	 
b.	Manual Operation: Right handed. Hydraulic door closer.	 
c.	Automatic Operation: Left handed. Powered door operators.	 
d.	Automatic Operation: Right handed. Powered door operators.	 
D.	Dimensions:			 
1.	No part of lift to be over 49 inches (1245 mm) high when platform is on the ground except when equipped with optional stage guard.		 
2.	Required Clear Space (WxL): 51.63 x 60.75 inches (1311 x 1543 mm).		 
3.	Lift Dimensions (WxLxH): 47.63 x 58.25 x 49 inches (1210 x 1480 x 1245 mm).		 
4.	Platform Clear Space; Upper Landing Gate Version: 36 x 58 inches (914 x 1473 mm).		 
E.	Materials:			 
1.	Platform, Base Frame, and Lifting Device: ASTM A 36 or similar low-carbon steel.		 
2.	Windows: 1/4 inch (6 mm) thick high impact strength clear thermoplastic.		 
3.	Platform Sheet Metal and Under-Platform Safety Pan: 1/16 inch (1.6 mm) aluminum alloy.		 
F.	Finish:			 
1.	Exposed Metal Surfaces: Finished by powder coating.		 
a.	Color: Black.	 
b.	Color: ______.	 
2.	Base Frame: Hot-dip galvanized.		 
G.	Drive Configuration: Direct-acting hydraulic.			 
1.	Synchronized Dual Hydraulic Cylinders: Evenly support both sides of lift platform.		 
2.	Hydraulic Power Unit: Mounted on vibration-isolating supports minimizing vibration transmission and reducing frame-borne noise.		 
H.	Electrical Requirements:			 
1.	Amperage Draw per Lift: 13 Amps maximum.		 
2.	Service Line: 120 VAC, 60 hertz. Amperage capacity: Exceeding 13 Amps.		 
3.	Motor: 1/2 hp, 115 V AC single phase.		 
4.	Control Circuits: 24 VDC.		 
5.	Electrical System: Certified to ASME A17.5 by independent testing laboratory.		 
I.	Lift Safety Devices:			 
1.	Lift Construction: Meet applicable requirements of ASME A18.1, ASME A17.5, ADAAG, ANSI 117.1, and NFPA 70 (NEC). 		 
2.	Included Safety Features: For passenger and general public protection.		 
a.	Operating Switches: Constant pressure.	 
b.	Emergency Stop Button: Lighted, sounds audible alarm.	 
c.	Electro-Mechanical Interlock: Prevents accidental opening of lower platform gate, and if provided, the upper landing gate.	 
d.	Gate Switches: Prevent operation if either platform gate is open.	 
e.	Hand Pump: Allows platform to manually be raised or lowered.	 
f.	Sidewalls and Platform Gate Heights: 48 inches (1220 mm).	 
1)	Visibility: Unobstructed view. Transparent sidewalls and platform gates. 
g.	Lift platform stop height sensor.	 
h.	Under-Platform Safety Pan: Safely stops lift if platform is obstructed during downward travel.	 
i.	Platform Floor: Low profile and slip resistant surface.	 
j.	No installation pit or external access ramp at the lower landing.	 
k.	Full length grab bar.	 
J.	Compression Capability: May be compressed to 33 inches (838 mm) wide facilitating relocation through a 36 inch (914 mm) wide doorway.			 
1.	Compression Tool Kit: Recommended to facilitate compression of the lift. From Ascension.		 
K.	Add-Ons:			 
1.	Automatic Standby Power (Battery Backup): Minimum 5 lift cycles at full load during power outage events.		 
2.	Two-Way Communication: Hands-free autodialing phone on platform.		 
3.	Universal Keys: Limits lift use to authorized persons.		 
4.	Shaftway Package: For installation in a hoistway/shaftway. 		 
5.	Auxiliary Lighting: Provides lighting when facility power is lost. 
2.6	VERTICAL PORTABLE WHEELCHAIR LIFTS (Virtuoso 5460P)				 
A.	Lift Product: Virtuoso 5460P as manufactured by Ascension. Portable lifting device, unenclosed and self-contained, requiring no additional components or facility modifications. Raises and lowers platform and occupant providing accessibility to stages, platforms, or similar elevated surfaces.			 
1.	Low Profile: No machine tower to maintain viewing lines.		 
2.	Platform: Supported on an electro-hydraulic lifting mechanism with built-in casters for portability.
3.	Casters: Permit easy movement of unoccupied lift over hard, level surfaces. 
a.	With Casters Removed: Lift to rest firmly on any hard, level surface, providing a stable base for operation of lift.
4.	Self-supported Unit: No anchoring to facility. 
5.	Independent Use: By individuals with disabilities
6.	ADA Compliant: Includes applicable operating and safety devices.
7.	Platform Profile: Low profile facilitating entry to the lift. Eliminates need for a pit or access ramp at lower landing.
B.	Physical Characteristics:
1.	Lifting Capacity: 750 pounds (340 kg).
2.	Weight of Lift: 1025 pounds (465 kg) maximum.
3.	Vertical Speed: 7 fpm (2.1 mpm).
4.	Vertical Travel: 12 to 60 inches (305 to 1524 mm), infinitely adjustable.
C.	Platform Gate Configuration:
1.	Lower Platform Gate:
a.	Manual Operation: Left handed. Hydraulic door closer.
2.	Upper Platform Gate: 
a.	Manual Operation: Right handed. Hydraulic door closer.
D.	Dimensions:
1.	No part of the lift to be over 44 inches (1117 mm) high when platform is on the ground except when equipped with optional stage guard.
2.	Space Requirements; Operational, Storage, and Transport (HxLxW): 44 x 66 x 48 inches (1117 x 1677 x 1219 mm). Height is for platform in the down position.
3.	Platform Clear Space: 36 x 54 inches (914 x 1372 mm). 
a.	Sidewalls and Platform Gates: 43 inches (1092 mm) high.
E.	Materials:
1.	Platform, Base Frame, and Lifting Device: ASTM A 36 or similar low-carbon steel.
2.	Windows: 1/4 inch (6 mm) thick high impact strength clear thermoplastic.
3.	Safety Skirt: Constructed from neoprene-coated nylon with PVC stiffeners.
F.	Finish:
1.	Exposed Metal Surfaces: Finished by powder coating.
a.	Color: Black.
b.	Color: ______.
G.	Drive Configuration: Direct-acting hydraulic.
1.	Synchronized Dual Hydraulic Cylinders: Evenly support both sides of lift platform.
2.	Hydraulic Power Unit: Mounted on vibration-isolating supports minimizing vibration transmission and reducing frame-borne noise.
H.	Electrical Requirements:
1.	Amperage Draw per Lift:  15 Amps maximum.
2.	Service:  120 VAC, 60 hertz, single phase, 15 amp service. Three prong grounded electrical cord. Length:  20 feet (6.1 m).
3.	A Ground Fault Circuit Interrupter (GFCI).
4.	Motor:  1/2 hp, 115 V AC single phase.
5.	Control Circuits: 24 VDC. 
6.	Electrical System:  Certified to ASME A17.5 by independent testing laboratory.
I.	Lift Safety Devices:
1.	Lift Construction:  Meet applicable requirements of ASME A18.1, ASME A17.5, ADAAG, ANSI 117.1, and NFPA 70 (NEC). 
2.	Included Safety Features:  For passenger and general public protection.
a.	Safety Skirt:  Completely encloses and protects area under platform.
1)	Switches:  Stop platform movement in case of excess skirt deflection.
b.	Operating Switches:  Constant pressure.
c.	Emergency Stop Button:  Lighted, sounds audible alarm.
d.	Electro-Mechanical Interlock:  Prevents accidental opening of lower platform gate, and if provided, the upper landing gate.
e.	Gate Switches:  Prevent operation if either platform gate is open.
f.	Hand Pump:  Allows platform to manually be raised or lowered.
g.	Sidewalls and Platform Gates:  43 inches (1092 mm) high.
1)	Visibility:  Unobstructed view. Transparent sidewalls and platform gates.
h.	Lift platform stop height sensor.
i.	Platform Floor:  Low profile and slip resistant surface. 
j.	No installation pit or external access ramp at the lower landing.
k.	Full length frame integrated grab bar.
J.	Portability:
1.	Casters: 3-1/2 inches (89 mm) diameter hard rubber. Attachable to platform without tools; stored in base frame when not in use. 
a.	Once attached, lift rolls easily over hard, smooth, level surfaces. 
2.	Lift may be moved via fork lift or fork truck.
K.	Operating Characteristics:
1.	Three Constant Pressure "UP/DOWN" Switches
2.	Platform Stop Height:  Adjustable without use of tools.
3.	Opening Upper Landing Platform Gate: Deploys a .190 inch (4.8 mm) aluminum dock plate that rests on the upper landing surface.
a.	Dock Plate:  Provides smooth transition between platform and upper landing. Closing upper landing platform gate retracts the dock plate.
L.	Compression Capability: May be compressed to 33 inches (838 mm) wide facilitating relocation through a 36 inch (914 mm) wide doorway. 
1.	Compression Tool Kit: Recommended to facilitate compression of the lift. From Ascension.
M.	Add-Ons:	 
1.	Automatic Standby Power (Battery Backup): Minimum 5 lift cycles at full load during power outage events. 
2.	Wireless Stanchions (Call Stations). 
3.	Oversized Casters. 
4.	Lift Cover. 
2.7	VERTICAL PORTABLE WHEELCHAIR LIFTS (Protege 5442P) 
A.	Lift Product: Protege 5442P as manufactured by Ascension. Portable lifting device, unenclosed, self-contained, requiring no additional components or facility modifications. Raises and lowers platform and occupant providing accessibility to stages, platforms, or similar elevated surfaces.
1.	Low Profile: No machine tower to maintain viewing lines. 
2.	Platform: Supported on an electro-hydraulic lifting mechanism with built-in casters for portability. 
3.	Casters: Permit easy movement of unoccupied lift over hard, level surfaces. 
a.	With Casters Removed: Lift to rest firmly on any hard, level surface, providing a stable base for operation of lift.
4.	Self-supported Unit: No anchoring to facility. 
5.	Independent Use: By individuals with disabilities
6.	ADA Compliant: Includes applicable operating and safety devices.
7.	Platform Profile: Slim profile frame eliminates need for pit or access ramp at lower landing and facilitate entry into lift directly at floor level by patrons.
B.	Physical Characteristics:
1.	Lifting Capacity: 900 pounds (408 kg).
2.	Weight of Lift: 850 pounds (386 kg) maximum.
3.	Vertical Speed: 5 fpm (1.5 mpm).
4.	Vertical Travel: 4 to 42 inches (102 to 1067 mm), infinitely adjustable.
C.	Platform Gate Configuration:
1.	Lower Platform Gate:
a.	Manual Operation: Left handed. Hydraulic door closer.
2.	Upper Platform Gate:
a.	Manual Operation: Right handed. Hydraulic door closer.
D.	Dimensions:
1.	No part of the lift to be over 49 inches (1245 mm) high when platform is on the ground except when equipped with optional stage guard.
2.	Space Requirements; Operational, Storage, and Transport (HxLxW): 49 x 61 x 48 inches (1245 x 1549 x 1219 mm). Height is for platform in the down position.
3.	Platform Clear Space: Size: 36 x 54 inches (914 x 1372 mm).
a.	Sidewalls and Platform Gates: 48 inches (1220 mm).
E.	Materials:
1.	Platform Frame, Base Frame, and Lifting Device: ASTM A 36 or similar low-carbon steel.
2.	Windows: 1/4 inch (6 mm) thick high impact strength clear thermoplastic.
3.	Platform Sheet Metal and Under-Platform Safety Pan: 1/16 inch aluminum alloy.
F.	Finish:
1.	Exposed Metal Surfaces: Finished by powder coating.
a.	Color: Black.
b.	Color: ______.
2.	Exposed Base Frame Metal Surfaces: Hot-dip galvanized.
G.	Drive Configuration: Direct-acting hydraulic.
1.	Synchronized Dual Hydraulic Cylinders: Evenly support both sides of lift platform.
2.	Hydraulic Power Unit: Mounted on vibration-isolating supports minimizing vibration transmission and reducing frame-borne noise.
H.	Electrical Requirements:
1.	Amperage Draw per Lift:  13 Amps maximum.
2.	Service:  120 VAC, 60 hertz, single phase, 15 amp service. Three prong grounded electrical cord. Length:  20 feet (6.1 m).
3.	A Ground Fault Circuit Interrupter (GFCI).
4.	Motor:  1/2 hp, 115 V AC single phase.
5.	Control Circuits: 24 VDC. 
6.	Electrical System:  Certified to ASME A17.5 by independent testing laboratory.
I.	Lift Safety Devices:
1.	Lift Construction:  Meet applicable requirements of ASME A18.1, ASME A17.5, ADAAG, ANSI 117.1, and NFPA 70 (NEC). 
2.	Included Safety Features:  For passenger and general public protection.
a.	Operating Switches:  Constant pressure.
b.	Emergency Stop Button:  Lighted, sounds audible alarm.
c.	Electro-Mechanical Interlock:  Prevents accidental opening of lower platform gate, and if provided, the upper landing gate.
d.	Gate Switches:  Prevent operation if either platform gate is open.
e.	Hand Pump:  Allows platform to manually be raised or lowered.
f.	Sidewalls and Platform Gate Heights:  48 inches (1220 mm).
1)	Visibility:  Unobstructed view. Transparent sidewalls and platform gates.
g.	Lift platform stop height sensor.
h.	Under-Platform Safety Pan:  Safely stops lift if platform is obstructed during downward travel.
i.	Platform Floor:  Low profile and slip resistant surface.
j.	No installation pit or external access ramp at the lower landing.
k.	Full length grab bar.
J.	Portability:
1.	Casters: 5 inches (127 mm) diameter. Attachable to platform without tools; stored in base frame when not in use. 
a.	Once attached, lift rolls easily over any hard, smooth, level surfaces.
2.	Lift may be moved via fork lift or fork truck.
K.	Operating Characteristics:
1.	Three Constant Pressure "UP/DOWN" Switches
2.	Platform Stop Height:  Adjustable without use of tools.
3.	Opening Upper Landing Platform Gate: Deploys a .190 inch (4.8 mm) aluminum dock plate that rests on the upper landing surface.
a.	Dock Plate:  Provides smooth transition between platform and upper landing. Closing upper landing platform gate retracts the dock plate.
L.	Compression Capability: May be compressed to 33 inches (838 mm) wide facilitating relocation through a 36 inch (914 mm) wide doorway. 
1.	Compression Tool Kit: Recommended to facilitate compression of the lift. From Ascension.
M.	Add-Ons:	 
1.	Automatic Standby Power (Battery Backup): Minimum 5 lift cycles at full load during power outage events. 
2.	Wireless Stanchions (Call Stations). 
3.	Oversized Casters. 
4.	Lift Cover.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Verify suitability of substrate preparation in accordance with approved manufacturer's drawings.
B.	Verify correct space requirements in accordance with approved manufacturer's drawings. Verify electrical service is of correct type and at correct location.
C.	Do not begin installation until substrates have been properly prepared. If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install lift in accordance with approved submittals, manufacturer's instructions, and ASME A18.1 requirements.
B.	Lift base will independently support the weight of the entire unit, and will be anchored to the pad at all four corners underneath the lift car. No part of the lift base frame will require anchoring to an adjacent wall for structural support.
3.4	FIELD QUALITY CONTROL
A.	Perform acceptance tests as required by code and the authority having jurisdiction. Place rated load on platform and operate for several cycles to verify correct installation and operation. No mechanical failures will occur and no wear that would affect the reliability of the lift will be detected.
3.5	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION