SECTION 08 33 00

COILING DOORS AND GRILLES

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2011 -  2020 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Service Doors: 
1.	Insulated Service Door. (Model CESD20).
2.	Non-Insulated Service Door. (Model CESD10).
3.	Labeled Fire Resistive Non-Insulated Door. (Model CERD10).
4.	Labeled Smoke Protection and Fire Resistive Non-Insulated Door. (Model CERD11).
5.	Labeled Fire Resistive Insulated Door. (Model CERD20).
6.	Labeled Smoke Protection and Fire Resistive Insulated Door. (Model CERD21).
B.	Counter Doors: 
1.	Standard Counter Door. (Model CESC10).
2.	Standard Counter Door with Integrated Frame. (Model CESC20).
3.	Standard Fire Rated Counter Door. (Model CERC10).
4.	Standard Fire Rated Counter Door with Integrated Frame. (Model CERC20).
C.	Security Grilles: 
1.	Overhead Glazed Rolling Grilles (Model: CESG11).
2.	Overhead Rolling Grilles (Model: CESG10 Straight Pattern).
3.	Overhead Rolling Grilles (Model: CESG12 Brick Pattern).
1.2	RELATED SECTIONS
A.	Section 05 50 00 - Metal Fabrications. Door opening jamb and head members.
B.	Section 06 10 00 - Rough Carpentry. Door opening jamb and head members.
C.	Section 08 31 16 - Access Panels and Frames. Access doors.
D.	Section 08 70 00 - Hardware.
E.	Section 09 91 00 - Painting. Field painting.
F.	Division 26 - Electrical wiring and conduit, fuses, disconnect switches, connection of operator to power supply, installation of control station and wiring, and connection to alarm system.
1.3	REFERENCES
A.	American Society of Civil Engineers (ASCE) 7 - Minimum Design Loads for Buildings and Other Structures.
B.	ASTM International (ASTM):
1.	ASTM A 123 - Standard Specification for Zinc (Hot-Dip Galvanized) Coatings on Iron and Steel Products.
2.	ASTM A 653/A 653M - Specification for Steel Sheet, Zinc-Coated (Galvanized) or Zinc-Iron Alloy-Coated (Galvannealed) by the Hot-Dip Process.
3.	ASTM A 924/A 924M - Specification for General Requirements for Steel Sheet, Metallic-Coated by the Hot-Dip Process.
4.	ASTM B 209/209M - Specification for Aluminum and Aluminum-Alloy Sheet and Plate.
5.	AST) B 221/221M - Specification for Aluminum and Aluminum-Alloy Extruded Bars, Rods, Wire, Profiles, and Tubes.
6.	ASTM C 612 - Standard Specification for Mineral Fiber Block and Board Thermal Insulation.
7.	ASTM C 665 - Standard Specification for Mineral-Fiber Blanket Thermal Insulation for Light Frame Construction and Manufactured Housing.
8.	ASTM D 3363 - Standard Test Method for Film Hardness by Pencil Test.
C.	National Electric Manufacturers Association (NEMA).
D.	National Fire Protection Association (NFPA) 80 - Standard for Fire Doors and Other Opening Protectives.
E.	National Fire Protection Association (NFPA) 105 - Standard for the Installation of Smoke Door Assemblies and Other Opening Protectives.
F.	Underwriters Laboratory (UL) 1784 - Air Leakage Tests of Door Assemblies.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
4.	Operation and maintenance data.
C.	Shop Drawings: Include special conditions not detailed in Product Data. Show interface with adjacent work.
D.	Quality Assurance/Control Submittals:
1.	Provide proof of manufacturer ISO 9001:2008 registration.
2.	Provide proof of manufacturer and installer qualifications.
E.	Closeout Submittals:
1.	Operation and Maintenance Manual.
2.	Certificate stating that installed materials comply with this specification.
1.5	QUALITY ASSURANCE
A.	Qualifications:
1.	Manufacturer Qualifications: ISO 9001:2008 registered and a minimum of five years experience in producing units of the type specified.
2.	Installer Qualifications: Manufacturer's approval.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Deliver all materials in their original sealed containers bearing manufacturer's name and identification of product.
B.	Do not store products in location with conditions outside manufacturer's absolute limits.
C.	Materials delivered to the site shall be examined for concealed damage or defects in shipping. Defects shall be noted and reported to the Owner's Representative in writing. 
1.7	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
1.8	WARRANTY
A.	Standard Warranty: Two years from date of shipment against defects in material and workmanship.
B.	Extended Warranty: Two year warranty against defects in materials and workmanship and five year finish warranty against fading, peeling, cracking, blistering, flaking or delaminating.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Clopay Corporation, which is located at:<BR />8585 Duke Blvd.<BR />Mason, OH 45040<BR />Toll Free Tel: 800-233-8366<BR />Tel: 513-770-4800<BR />Fax: 888-434-3193<BR />Email: request info (marketing@clopay.com);Web: https://www.clopaydoor.com | https://www.clopaycommercial.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00.
2.2	SERVICE DOORS
A.	Product:
1.	Insulated Service Door: Model CESD20 as manufactured by Clopay Corporation.
2.	Non-Insulated Service Door: Model CESD10 as manufactured by Clopay Corporation.
3.	Labeled Fire Resistive Non-Insulated Door: Model CERD10 as manufactured by Clopay Corporation.
4.	Labeled Fire Resistive Insulated Door: Model CERD20 as manufactured by Clopay Corporation.
5.	Labeled Smoke Protection and Fire Resistive Non-Insulated Door: Model CERD11 as manufactured by Clopay Corporation.
6.	Labeled Smoke Protection and Fire Resistive Insulated Door: Model CERD21 as manufactured by Clopay Corporation.
B.	Design Requirements:
1.	Wind Loading: Supply doors to withstand up to __ psf ( ___ Pa) maximum wind load.
2.	Cycle Life: Design doors of standard construction for normal use of up to 20 cycle per day maximum.
3.	Cycle Life: Design doors of special construction for high cycle use. Expected cycles of up to ____ per day.
4.	Provide doors with Underwriters' Laboratories, Inc. label for the fire rating classification:
a.	FR Classification: 4 hr.
b.	FR Classification: 3 hr.
c.	FR Classification: 1 1/2 hr.
d.	FR Classification: 1 hr.
e.	FR Classification: 3/4 hr.
f.	FR Classification: Factory Mutual 3 hour fire rating label.
5.	Provide doors with Underwriters' Laboratories, Inc. label for "Leakage Rated Assembly" or "S" label.
a.	Comply with NFPA 105 air leakage requirements.
b.	Pass UL test procedure 1784.
6.	Provide doors with seismic calculations for seismic performance per ASCE 7-05 to comply with Local Authority Having Jurisdiction (AHJ).
C.	Construction:
1.	Insulated Curtain:
a.	Slat Design: No. 6F, (Exterior/Interior): 
b.	Material: Galvanized Steel/Galvanized Steel: Grade 40, ASTM A 653 galvanized steel zinc coating.
1)	Material thickness: 24/24 gauge.
2)	Material thickness: 22/24 gauge.
3)	Material thickness: 20/24 gauge.
4)	Material thickness: 22/22 gauge.
5)	Material thickness: 18/24 gauge.
c.	Material: Stainless Steel/Galvanized Steel: 22 gauge AISI type 304 series stainless steel/24gauge, Grade 40, ASTM A 653 galvanized steel zinc coating.
d.	Material: Stainless Steel/Stainless Steel: 22/22 gauge AISI type 304 series stainless steel.
e.	Material: Aluminum/Aluminum: 0.040 inch (1.016 mm) aluminum.
f.	Total Slat Thickness: 15/16 inch (24 mm).
g.	Insulation Material: 7/8 inch (22 mm) foamed-in-place, closed cell urethane.
1)	Flame Spread Index of 0 and a Smoke Developed Index of 10 as tested per ASTM E84.
2)	Minimum Sound Transmission Class (STC) rating of 26 as tested per ASTM E90.
3)	Minimum R-value of 8.0 (U-factor of 0.125) as calculated using the ASHRAE Handbook of Fundamentals.
4)	Insulation to be CFC Free with an Ozone Depletion Potential (ODP) rating of zero.
h.	Bottom Bar: Reinforced extruded aluminum interior face with full depth insulation and exterior skin slat to match curtain material and gauge.
2.	Insulated Labeled Curtain:
a.	Slat Design: No. 6F, (Exterior/Interior): 
b.	Material: Galvanized Steel/Galvanized Steel: Grade 40, ASTM A 653 galvanized steel zinc coating.
1)	Material thickness: 24/24 gauge.
2)	Material thickness: 22/22 gauge.
c.	Material: Stainless Steel/Stainless Steel: 22/22 gauge AISI type 304 series stainless steel.
d.	Total Slat Thickness: 15/16 inch (24 mm).
e.	Insulation: 7/8 inch (22 mm) thick fire retardant mineral wool, ASTM C665-95 or ASTM C612-93.
1)	Flame Spread Index of 0 and a Smoke Developed Index of 0 as tested per ASTM E84.
2)	Minimum Sound Transmission Class (STC) rating of 27 as tested per ASTM E90. Results shall be indicative of testing a complete/operable door assembly.
3)	Minimum R-value of 2.75as calculated using the ASHRAE Handbook of Fundamentals.
f.	Bottom Bar: Two 2 inches by 2 inches by minimum 1/8 inch (51 by 51 by 3.2 mm) structural steel angles.
g.	Bottom Bar: Two 2 inches by 2 inches by minimum 1/8 inch (51 by 51 by 3.2 mm) AISI 300 series stainless steel angles.
3.	Curtain:
a.	Curtain Slats: No. 5F, Grade 40 steel, ASTM A 653 galvanized steel zinc coating.
1)	Material thickness: 22 gauge.
2)	Material thickness: 20 gauge.
3)	Material thickness: 18 gauge.
4)	Bottom Bar: Two 2 inches by 2 inches by minimum 1/8 inch (51 by 51 by 3.2 mm) structural steel angles.
b.	Curtain Slats: No. 5P, 20 gauge, Grade 40 steel, ASTM A 653 galvanized steel zinc coating perforated with 0.062 inch (1.6 mm) diameter openings at 0.094 inch (2.4 mm) staggered centers, approximately 22 percent free area.
1)	Bottom Bar: Two 2 inches by 2 inches by minimum 1/8 inch (51 by 51 by 3.2 mm) structural steel angles.
c.	Curtain Slats: No. 5F, 20 gauge AISI type 304 series stainless steel.
1)	Bottom Bar: Two 2 inches by 2 inches by minimum 1/8 inch (51 by 51 by 3.2 mm) AISI 300 series stainless steel angles.
d.	Curtain Slats: No. 5F, 0.050 inch (1.270 mm) aluminum.
1)	Bottom Bar: Two 2 inches by 2 inches by minimum 1/8 inch (51 by 51 by 3.2 mm) aluminum angles.
4.	Curtain Configuration: Standard Curtain configuration.
5.	Curtain Configuration: RapidResponse configuration with 3 feet (914 mm) of extra slats.
6.	Curtain Configuration: RapidResponse configuration with 6 feet (1829 mm) of extra slats.
7.	Bottom Bar Configuration: Standard Bottom Bar Configuration.
8.	Bottom Bar Configuration: RapidResponse Impactable Bottom Bar consisting of 2 steel angles with flexible connecting members.
9.	Breakaway Curtain Bottom Section: Bottom 25 inches (635 mm) of door curtain to be constructed of a reinforced vinyl laminated woven polyester fabric panel with a breakaway bottom bar constructed of back to back structural steel angles. Color of assembly to be safety orange. Design section to release upon impact avoiding most damage from accidents involving forklift trucks or other vehicles.
10.	Guide Configuration: Standard Guide Configuration.
11.	Guide Configuration: RapidResponse Guide Configuration with a 56 inches (1422 mm) removable lower guide section.
12.	Operator and Bracket Mechanism Cover: Provide sheet metal cover to provide weather resistance and to enclose exposed moving operating components at coil area of unit. Finish and material to match door hood.
13.	Nylon Endlocks: Fabricate interlocking sections with high strength nylon endlocks on alternate slats each secured with two 1/4 inch (6.35 mm) rivets. 
14.	Cast Iron Endlocks: Fabricate interlocking sections with high strength cast iron endlocks on alternate slats each secured with two 1/4 inch (6.35 mm) rivets. 
15.	Steel Endlocks: Fabricate interlocking continuous slat sections with high strength steel endlocks secured with two 1/4 inch (6.35 mm) rivets per UL requirements.
16.	Windlocks: Provide windlock bars of same material as guide material when windlocks are required to meet specified wind load. 
17.	Slat Finish: Coating System to include an ASTM A 653 galvanized base coating treated with dual process rinsing agents in preparation of a chemical bonding, light gray baked-on polyester base coat and a light gray baked-on polyester finish coat. Components include a limited two year finish warranty.
18.	Slat Finish: Coating System and phosphate treatment followed by baked-on polyester powder coat, minimum 2.5 mil (0.065 mm) cured film thickness; ASTM D-3363 pencil hardness: H or better.
a.	Color: Color as selected by Architect from manufacturer's standard color range, minimum 32 colors.
b.	Color: Custom color as selected by Architect.
19.	Slat Finish: Galvanized Steel - Phosphate and bonding treatment only, (no paint finish).
20.	Slat Finish: Stainless steel: No. 4 finish.
21.	Slat Finish: Aluminum - Mill finish.
22.	Slat Finish: Aluminum - Clear anodized.
23.	Slat Finish: Aluminum - Medium bronze anodized.
24.	Slat Finish: Aluminum - Dark bronze anodized.
25.	Slat Finish: Aluminum - Black anodized.
26.	Bottom Bar Finish: Steel: Phosphate treatment followed by a light gray baked-on polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
27.	Bottom Bar Finish: Steel - Phosphate treatment followed by corrosion inhibitive baked-on zinc-rich gray polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
28.	Bottom Bar Finish: Steel - ASTM A 123, Grade 85 zinc coating, hot-dip galvanized after fabrication.
29.	Bottom Bar Finish: Steel - Phosphate treatment followed by baked-on polyester powder coat, minimum 2.5 mil (0.065 mm) cured film thickness; ASTM D-3363 pencil hardness: H or better.
a.	Color: Color as selected by Architect from manufacturer's standard color range, minimum 32 colors.
b.	Color: Custom color as selected by Architect.
30.	Bottom Bar Finish: Stainless steel - No. 4 finish.
31.	Bottom Bar Finish: Aluminum - Mill finish.
32.	Bottom Bar Finish: Aluminum - Clear anodized.
33.	Bottom Bar Finish: Aluminum - Medium bronze anodized.
34.	Bottom Bar Finish: Aluminum - Dark bronze anodized.
35.	Bottom Bar Finish: Aluminum - Black anodized.
36.	Guide Material: Fabricate with 3/16 inch (4.8 mm) structural steel angles. 
37.	Guide Material: Fabricate with 3/16 inch (4.8 mm) stainless steel angles. 
38.	Guide Material: Fabricate with 3/16 inch (4.8 mm) aluminum angles. 
39.	Guide Material: Fabricate with 1/4 inch (6.35 mm) structural steel angles. 
40.	Top of inner and outer guide angles to be flared outwards to form bellmouth for smooth entry of curtain into guides. Provide removable guide stoppers to prevent over travel of curtain and bottom bar.
41.	Guide Top 16-1/2 inches (419 mm) of coil side guide angles shall be removable for curtain installation and curtain service.
42.	Guide Finish: Steel: Phosphate treatment followed by a light gray baked-on polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
43.	Guide Finish: Steel: Phosphate treatment followed by a corrosion inhibitive baked-on zinc-rich gray polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
44.	Guide Finish: Steel: ASTM A 123, Grade 85 zinc coating, hot-dip galvanized after fabrication.
45.	Guide Finish: Steel: Phosphate treatment followed by baked-on polyester powder coat, minimum 2.5 mil (0.065 mm) cured film thickness; ASTM D-3363 pencil hardness: H or better.
a.	Color: Color as selected by Architect from manufacturer's standard color range, minimum 32 colors.
b.	Color: Custom color as selected by Architect.
46.	Guide Finish: Stainless steel: No. 4 finish.
47.	Guide Finish: Stainless steel: Mill finish.
48.	Guide Finish: Aluminum - Mill finish.
49.	Guide Finish: Aluminum - Clear anodized.
50.	Guide Finish: Aluminum - Medium bronze anodized.
51.	Guide Finish: Aluminum - Dark bronze anodized.
52.	Guide Finish: Aluminum - Black anodized.
53.	Counterbalance Shaft Assembly:
a.	Barrel: Steel pipe capable of supporting curtain load with maximum deflection of 0.03 inches per foot (2.5 mm per meter) of width.
b.	Spring Balance: Oil-tempered, heat-treated steel helical torsion spring assembly designed for proper balance of door to ensure that maximum effort to operate will not exceed 25 lbs (110 N). Provide wheel for applying and adjusting spring torque.
54.	Brackets: Fabricate from minimum 3/16 inch (5 mm) steel plate with permanently lubricated ball or roller bearings at rotating support points to support counterbalance shaft assembly and form end closures.
55.	Brackets: Fabricate from minimum 1/4 inch (6.35 mm) steel plate with permanently lubricated ball or roller bearings at rotating support points to support counterbalance shaft assembly and form end closures.
56.	Bracket Finish: Steel - Phosphate treatment followed by a light gray baked-on polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
57.	Bracket Finish: Phosphate treatment followed by corrosion inhibitive baked-on zinc-rich gray polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
58.	Bracket Finish: ASTM A 123, Grade 85 zinc coating, hot-dip galvanized after fabrication.
59.	Bracket Finish: Phosphate treatment followed by baked-on polyester powder coat, minimum 2.5 mil (0.065 mm) cured film thickness; ASTM D-3363 pencil hardness: H or better.
a.	Color: Color as selected by Architect from manufacturer's standard color range, minimum 32 colors.
b.	Color: Custom color as selected by Architect.
60.	Hood: with reinforced top and bottom edges. Provide minimum 1/4 inch (6.35 mm) steel intermediate support brackets as required to prevent excessive sag.
61.	Hood Material: 24 gauge galvanized steel.
62.	Hood Material: 24 gauge stainless steel.
63.	Hood Material: 0.040 inch (1.016 mm) aluminum.
64.	Hood Finish: GalvaNex Coating System to include an ASTM A 653 galvanized base coating treated with dual process rinsing agents in preparation of a chemical bonding, light gray baked-on polyester base coat and a light gray baked-on polyester finish coat. The scientific organic material composition and chemical bonding process of GalvaNex produces a superior finish against corrosion and abrasion. GalvaNex components include a limited two year finish warranty.
65.	Hood Finish: GalvaNex Coating System and phosphate treatment followed by baked-on polyester powder coat, minimum 2.5 mil (0.065 mm) cured film thickness; ASTM D-3363 pencil hardness: H or better.
a.	Color: Color as selected by Architect from manufacturer's standard color range, minimum 32 colors.
b.	Color: Custom color as selected by Architect.
66.	Hood Finish: Stainless steel: No. 4 finish.
67.	Hood Finish: Aluminum - Mill finish.
68.	Hood Finish: Aluminum - Clear anodized.
69.	Hood Finish: Aluminum - Medium bronze anodized.
70.	Hood Finish: Aluminum - Dark bronze anodized.
71.	Hood Finish: Aluminum -Black anodized.
D.	Weatherstripping:
1.	Bottom Bar: Replaceable, bulb-style, compressible EDPM gasket extending into guides.
2.	Bottom Bar, Motor Operated Doors: Weather/sensing edge as specified.
3.	Guides: Vinyl strip sealing against fascia side of curtain.
4.	Hood: Neoprene/rayon baffle to impede air flow above coil.
5.	Lintel Seal: Nylon brush seal fitted at door header to impede air flow.
E.	Weather/Smoke Seal - Sensing Edge: 
1.	Provide an electric sensing edge device. Provide automatic control by an automatic sensing switch within neoprene or rubber astragal extending full width of door bottom bar. 
2.	Response: Contact before door fully closes shall cause door to immediately stop downward travel and reverse direction to the fully opened position. 
3.	Response: Contact before door fully closes shall cause door to immediately stop downward travel. 
4.	Type: Provide a self-monitoring wireless sensing edge connection to motor operator eliminating the need for a physical traveling electric cord connection between bottom bar sensing edge device and motor operator. Supervised system alters normal door operation preventing damage, injury or death due to an inoperable sensing edge system.
5.	Type: Provide a wireless sensing edge connection to motor operator eliminating the need for a physical traveling electric cord connection between bottom bar sensing edge device and motor operator.
6.	Type: Provide an electric sensing edge device. 
a.	Provide self-coiling cable connection to control circuit.
b.	Provide retracting safety cord and reel connection to control circuit.
7.	Type: Provide a pneumatic sensing edge device. 
a.	Provide self-coiling cable connection to control circuit.
b.	Provide retracting safety cord and reel connection to control circuit.
F.	Smoke Seals:
1.	Bottom Bar, Manual Operated Doors: Two, replaceable, UL listed, nylon pile smoke seals.
2.	Bottom Bar, Motor Operated Doors: Combination smoke seal/sensing edge as specified.
3.	Guides and Head: Replaceable, UL listed, nylon pile smoke seals sealing against fascia side of curtain.
G.	Locking:
1.	Locking: Manual Push-Up and Manual Crank Hoist - Padlockable slide bolt on coil side of bottom bar at each jamb extending into slots in guides.
2.	Locking: Manual Push-Up and Manual Crank Hoist - Padlockable slide bolt on fascia side of bottom bar at each jamb extending into slots in guides.
3.	Locking: Manual Chain Hoist - Padlockable chain keeper on guide.
4.	Padlockable slide bolt on coil side of bottom bar at each jamb extending into slots in guides. Provide interlock switches on motor operated units.
5.	Padlockable slide bolt on fascia side of bottom bar at each jamb extending into slots in guides. Provide interlock switches on motor operated units.
6.	Masterkeyable cylinder operable from coil side of bottom bar. Provide interlock switches on motor operated units. 
7.	Masterkeyable cylinder operable from fascia side of bottom bar. Provide interlock switches on motor operated units.
8.	Masterkeyable cylinder operable from both sides of bottom bar. Provide interlock switches on motor operated units.
H.	Vision Panels: 10 x 1-5/8 inches (254 x 41.28 mm) oval acrylic panes set with double sided foam glazing tape and secured with retaining clips and rivets. Refer to drawings for number and placement.
I.	Rated Vision Panels: 10 inches x 1-5/8 inches x 3/16 inch (254 x 41 x 4.76 mm) thick oval glass panes set in metal frames and mechanically fastened to slat. Refer to drawings for number and placement.
J.	Pass Doors: Provide pass door with hinge frame and hardware as scheduled.
K.	Graphics Door Image: 
1.	Flat face surface of door curtain slats, hood and fascia, as indicated, to include a factory applied color process, 2 mil (0.05 mm) thick vinyl graphic image, 3M or equal. 
2.	Color Process: 2 color.
3.	Color Process: 4 color.
4.	Graphic image to be selected and electronically supplied by customer. 
L.	Manual Operation/Non Labeled Doors:
1.	Manual Push-Up: Provide lift handles on bottom bar and pole with hook.
2.	Manual Chain Hoist: Provide chain hoist operator with endless steel chain, chain pocket wheel and guard, geared reduction unit, and chain keeper secured to guide.
3.	Manual Crank Hoist: Provide crank hoist operator including crank gear box, steel crank drive shaft and geared reduction unit. Fabricate gear box to completely enclose operating mechanism and be oil-tight.
M.	Control Station:
1.	Motor Control Station: Surface mounted, "Open/Close/Stop" push buttons; NEMA 1.
2.	Motor Control Station: Surface mounted, "Open/Close" push buttons; NEMA 1.
3.	Motor Control Station: Flush mounted, "Open/Close/Stop" push buttons; NEMA 1B.
4.	Motor Control Station: Flush mounted, "Open/Close" push buttons; NEMA 1B.
5.	Motor Control Station: Flush mounted, "Open/Close" key switch; NEMA 1B.
6.	Motor Control Station: Flush mounted, "Open/Close" key switch with "Stop" push button; NEMA 1B.
7.	Motor Control Station: Surface mounted, "Open/Close" key switch; NEMA 3R.
8.	Motor Control Station: Surface mounted, "Open/Close" key switch with "Stop" push button; NEMA 3R.
9.	Motor Control Station: Surface mounted, "Open/Close/Stop," push buttons with keyed lock-out, not masterkeyable; NEMA 4.
N.	Motor Operators/Non Labeled Doors:
1.	Motor Operator: Supply Clopay Model MG, industrial duty - rated for a maximum of 20 cycles per hour, cULus listed, Totally Enclosed Non Ventilated gear head operator(s) rated hp as recommended by door manufacture for size and type of door. Volts and Phase as available and scheduled.
a.	Provide complete with:
1)	Electric motor and factory pre-wired motor control terminals.
2)	Maintenance free solenoid actuated brake.
3)	Control station(s).
4)	Emergency manual chain hoist.
5)	Operator shall be equipped with a disconnect cable for auxiliary push-up operation. 
b.	Motor shall be high starting torque, industrial type, protected against overload with an auto-reset thermal sensing device. Primary speed reduction shall be heavy-duty, lubricated gears with mechanical braking to hold the door in any position. 
c.	Operator shall be equipped with an emergency manual chain hoist assembly that safely cuts operator power when engaged. A disconnect chain shall not be required to engage or release the manual chain hoist. 
d.	Operator drive and door driven sprockets shall be provided with #50 roller chain. 
e.	Provide an integral Motor Mounted Interlock system to prevent damage to door and operator when mechanical door locking devices are provided. 
f.	Operator shall be capable of driving the door at a speed of 8 to 9 inches per second (20 to 23 cm/sec). Fully adjustable, driven linear screw type cam limit switch mechanism shall synchronize the operator with the door. The electrical contractor shall mount the control station(s) and supply the appropriate disconnect switch, all conduit and wiring per the overhead door wiring instructions.
2.	Motor Operator: Supply Clopay Model SG, continuous duty, cULus listed, totally enclosed fan cooled gear head operator(s) rated hp as recommended by door manufacture for size and type of door. Volts and Phase as available and scheduled.
a.	Provide complete with electric motor and factory pre-wired motor control terminals, maintenance free solenoid actuated brake, emergency manual chain hoist provided up to 2 hp and control station(s). 
b.	Motor shall be high starting torque, industrial type, with overload protection. Primary speed reduction shall be heavy-duty gears running in grease or oil bath with mechanical braking to hold the door in any position. When equipped, the emergency manual chain hoist assembly is automatically disengaged when motor is energized. A disconnect chain shall not be required to engage or release the manual chain hoist. 
c.	Operator drive and door driven sprockets shall be provided with minimum #50 roller chain. Operator shall be capable of driving the door at a speed of 8 to 9 inches per second (20 to 23 cm/sec). Fully adjustable, driven linear screw type cam limit switch mechanism shall synchronize the operator with the door. The motor shall be removable without affecting the limit switch settings. The electrical contractor shall mount the control station(s) and supply the appropriate disconnect switch, all conduit and wiring per the overhead door wiring instructions.
O.	Motor Operators/Labeled Fire Doors:
1.	Motor Operated: Model CFD, UL listed and FM approved, NEMA 1 enclosure rating, horsepower as recommended by manufacture. Voltage and phase as available and scheduled. Provide open drip-proof motor, removable without affecting setting of limit switches; UL listed thermal overload protection; solenoid brake; planetary reduction gearing and rotary limit switches; transformer with 24 v control secondary; and all integral electrical components prewired to terminal blocks.
a.	Automatic closure shall be activated by fusible link.
b.	Automatic closure shall be activated by a local smoke/fire detector by means of a fail-safe releasing device. Doors shall not require a releasing device when activated by an alarm signal.
c.	Automatic closure shall be activated by a central smoke/fire alarm system by means of a fail-safe releasing device. Doors shall not require a releasing device when activated by an alarm signal.
d.	Doors shall maintain an average closing speed of not more than 9 inches (229 mm) per second during automatic closing. When automatic closure is activated, electric sensing edge and push button are inoperable.
1)	Doors shall be fail-safe and close upon power failure.
2)	Resetting of spring tension or mechanical dropouts shall not be required. Upon restoration of power, replacement of fusible link or clearing of the alarm signal, doors shall immediately reset by opening with the push button.
3)	The electrical contractor shall mount the control station(s) and supply the appropriate disconnect switch, all conduit and wiring per the overhead door wiring instructions.
2.	Battery Back-up System: Provide Model F-BBU Battery Back-Up System for CFD Motor Operator. Provides four hours of door open holding time in the event of a power failure. Can power local detectors and warning appliances. Allows for programming open/close obstruction cycling should the sensing edge encounter a stationary obstruction in the opening during AC power, alarm signal closing.
P.	Manual Operation/Labeled Fire Doors:
1.	Manual Chain Hoist: Provide combination chain / controlled closing system operator including endless steel chain, geared reduction unit and chain keeper.
a.	Provide a wall mounted Push To Close station located at floor level. Integral to the unit is a locking mechanism to hold the door at any position of travel during normal door operation mode and a governor to control automatic closing speed.
b.	Provide a combination close operation / automatic drop test cable located at floor level. Integral to the unit is a locking mechanism to hold the door at any position of travel during normal door operation mode and a governor to control automatic closing speed.
2.	Manual Crank Hoist: Provide combination crank / controlled closing system operator including removable hand crank and geared reduction unit.
a.	Provide a wall mounted Push To Close station located at floor level. Integral to the unit is a locking mechanism to hold the door at any position of travel during normal door operation mode and a governor to control automatic closing speed.
b.	Provide a wall mounted combination close operation / automatic drop test cable located at floor level. Integral to the unit is a locking mechanism to hold the door at any position of travel during normal door operation mode and a governor to control automatic closing speed.
3.	Manual Push-Up with Conventional Spring Release System: Provide lift handles on bottom bar and pole with hook.
4.	Automatic closure shall maintain an average closing speed of not less than 6 inches (152 mm) nor more than 24 inches (610 mm) per second during automatic closing per NFPA 80. Resetting of spring tension and mechanical dropouts by a trained door systems technician is required.
a.	Automatic closure shall be activated by fusible link.
b.	Automatic closure shall be activated by a local smoke/fire detector by means of a fail-safe releasing device. 
c.	Automatic closure shall be activated by a central smoke/fire alarm system by means of a fail-safe releasing device.
Q.	Fire Detectors:
1.	Provide Photoelectric Smoke/Heat Detector: UL listed.
2.	Provide Ionization Smoke Detector: UL listed.
R.	Fire Emergency Annunciator: 
1.	Provide ADA compliant horn/strobe fire emergency annunciator to give advanced warning that the fire door is about to close. Warning signal to activate upon alarm signal. 
2.	Provide Voice Warning Module fire emergency annunciator to give advanced warning that the fire door is about to close. Warning signal to activate upon alarm signal. 
S.	Automatic Closing and Speed Governor Mechanism:
1.	Motor Operated System:
a.	Activation: As specified.
b.	Operation: Motor operator shall close door upon signal from fire detector, power outage or melting of fusible link as specified.
c.	Closing Speed: Not more than 9 inches (229 mm) per second.
d.	Reset Procedure: Operation of control station after alarm is cleared or power is restored or replace fusible link. Resetting of spring tension or mechanical dropouts shall not be required.
2.	Manual Operation System:
a.	Operation: Hand chain and hand crank operation as scheduled and use of a wall mounted Push To Close station or combination close operation / automatic drop test cable as specified, located at floor level for normal use. When automatic closing is activated, integral brake and operator shall disengage. Integral governor controls closing speed.
1)	Activation: As specified.
2)	Average Closing Speed: Not more than 9 inches (229 mm) per second.
3)	Reset Procedure: Resetting of spring tension or mechanical dropouts shall not be required. 
a)	If tested by activating Push To Close station or automatic drop test cable, reset by releasing controller. 
b)	If activated by an automatic reset release device, clear alarm and/or restore power.
c)	If tested by activating a floor level reset release device, pull and hold floor level release reset cable for 3 seconds once alarm is cleared and/or power is restored.
d)	If tested by melting / cutting of fusible link, replace fusible link.
b.	Operation: Manual Push-Up.
1)	Product: Fusible Link.
2)	Activation: Melting of fusible link.
3)	Average Closing Speed: Not less than 6 inches (152 mm) nor more than 24 inches (610 mm) per second.
4)	Reset Procedure: Reset spring tension and mechanical dropouts; replace fusible link.
c.	Operation: Manual Push-Up.
1)	Product: Fusible Link with FireGard AR-D Release Device.
2)	Activation: Central alarm system or local smoke and heat detectors or power outage in excess of 10 seconds or melting of fusible link.
3)	Average Closing Speed: Not less than 6 inches (152 mm) nor more than 24 inches (610 mm) per second.
4)	Reset Procedure: Reset spring tension and mechanical dropouts; reset FireGard AR-D or replace fusible link.
d.	Operation: Manual Push-Up.
1)	Product: Fusible Link with FireGard BB Release Device.
2)	Activation: Central alarm system or local smoke and heat detectors or power outage in excess of 72 hours or melting of fusible link.
3)	Average Closing Speed: Not less than 6 inches (152 mm) nor more than 24 inches (610 mm) per second.
4)	Reset Procedure: Reset spring tension and mechanical dropouts; reset FireGard BB or replace fusible link.
e.	Operation: Manual Push-Up.
1)	Product: Fusible Link with FireGard DC Release Device.
2)	Activation: Central alarm system or local smoke and heat detectors or DC alarm system power outage or melting of fusible link.
3)	Average Closing Speed: Not less than 6 inches (152 mm) nor more than 24 inches (610 mm) per second.
4)	Reset Procedure: Reset spring tension and mechanical dropouts; reset FireGard DC or replace fusible link.
2.3	COUNTER DOORS
A.	Product: 
1.	Counter Door: Model CESC10 as manufactured by Clopay Corporation.
2.	Counter Door with Integrated Frame: Model CESC20 as manufactured by Clopay Corporation.
3.	Labeled Fire Resistive Door: Model CERC10 as manufactured by Clopay Corporation.
4.	Labeled Fire Resistive Door with Integrated Frame: Model CERC20 as manufactured by Clopay Corporation.
B.	Design Requirements:
1.	Wind Loading: Supply doors to withstand up to [ __ psf ( ___ Pa) maximum wind load.
2.	Cycle Life: Design doors of standard construction for normal use of up to 20 cycle per day maximum.
3.	Cycle Life: Design doors of special construction for high cycle use. Expected cycles of up to ____ per day.
4.	Provide doors with Underwriters' Laboratories, Inc. label for the fire rating classification:
a.	FR Classification: 3 hr.
b.	FR Classification: 1 1/2 hr.
c.	FR Classification: 1 hr.
d.	FR Classification: 3/4 hr.
5.	Provide doors with Underwriters' Laboratories, Inc. label for "Leakage Rated Assembly" or "S" label.
a.	Comply with NFPA 105 air leakage requirements.
b.	Pass UL test procedure 1784.
6.	Provide doors with seismic calculations for seismic performance per ASCE 7-05 to comply with Local Authority Having Jurisdiction (AHJ).
7.	Integrated Frame Fabrication: Factory weld components into a single unit, fully assembled, ready for installation.
a.	Integrated Frame Type: Built-in type.
b.	Integrated Frame Type: Slip-in type.
C.	Construction:
1.	Curtain: Continuous interlocking slat sections with galvanized steel endlocks riveted to slats as per UL requirements.
a.	Slat Type: Galvanized steel, No. 1F, interlocked flat-faced slats, 1-1/2 inches (38 mm) high by 1/2 inch (13 mm) deep, 22 gauge ASTM A 653, Commercial Quality, galvanized steel with plain steel bottom bar and vinyl astragal.
b.	Slat Type: Stainless Steel, No. 1F, interlocked flat-faced slats, 1-1/2 inches (38 mm) high by 1/2 inch (13 mm) deep, 22 gauge AISI type 304 series stainless steel with stainless steel bottom bar and vinyl astragal.
c.	Slats: No. 1F, interlocked flat-faced slats, 1-1/2 inches (38 mm) high by 1/2 inch (13 mm) deep, 0.040 inch (1.016 mm) aluminum with extruded tubular aluminum bottom bar with continuous lift handle and vinyl astragal.
d.	Slats: No. 1P ScreenGard interlocked flat-faced, perforated slats, 1-1/2 inches (38 mm) high by 1/2 inch (13 mm) deep, 22 gauge ASTM A 653, Commercial Quality, galvanized steel perforated with 0.062 inch (1.6 mm) diameter openings at 0.094 inch (2.4 mm) staggered centers, approximately 22 percent free area with extruded aluminum tubular bottom bar, continuous lift handle and vinyl astragal.
e.	Nylon Endlocks: Fabricate interlocking slat sections with high strength molded nylon endlocks riveted to ends of alternate slats.
f.	Steel Endlocks: Fabricate interlocking slat sections with high strength galvanized steel endlocks riveted to slats per UL requirements.
g.	Slat Finish: GalvaNex Coating System.
1)	Compliance: ASTM A 653 galvanized base coating treated with dual process rinsing agents in preparation for a chemical bonding.
2)	Base Coat: Light gray baked-on polyester base coat.
3)	Finish Coat: Light gray baked-on polyester finish coat.
4)	Finish Warranty: Limited two year finish warranty.
h.	Slat Finish: GalvaNex Coating System and phosphate treatment followed by baked-on polyester powder coat.
1)	ASTM D 3363 Pencil Hardness: H or better.
2)	Thickness: Minimum 2.5 mil (0.065 mm) cured film thickness.
3)	Color: As selected by Architect from manufacturer's standard color range, minimum 32 colors.
4)	Color: Custom color as selected by Architect.
i.	Slat Finish: Stainless steel, No. 4 finish.
j.	Slat Finish: Aluminum - Clear anodized.
k.	Slat Finish: Aluminum - Medium bronze anodized.
l.	Slat Finish: Aluminum - Dark bronze anodized.
m.	Slat Finish: Aluminum - Black anodized.
n.	Bottom Bar Finish: Steel, Phosphate treatment followed by a light gray baked-on polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
o.	Bottom Bar Finish: Steel, Phosphate treatment followed by a corrosion inhibitive baked-on zinc-rich gray polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
p.	Bottom Bar Finish: Steel, ASTM A 123, Grade 85 zinc coating, hot-dip galvanized.
q.	Bottom Bar Finish: Steel, Phosphate treatment followed by baked-on polyester powder coat.
1)	ASTM D-3363 Pencil Hardness: H or better. 
2)	Thickness: Minimum 2.5 mil (0.065 mm) cured film thickness.
3)	Color: As selected by Architect from manufacturer's standard color range, minimum 32 colors.
4)	Color: Custom color as selected by Architect.
r.	Bottom Bar Finish: Stainless steel, No. 4 finish.
s.	Aluminum Bar/Steel Slat with Baked Enamel Coating: Clear anodized.
t.	Aluminum Bar/Aluminum Slat: Match slat finish.
u.	Aluminum Bar/Steel Slat with Powder Coating: Match slat powder coating.
2.	Integrated Head and Jamb Frame: Integral welded with guide groove incorporated into jamb design. 
a.	Wall Thickness: As indicated on Drawings.
b.	Material: Steel, 16 gauge formed shapes.
c.	Material: Stainless steel, 16 gauge AISI 300 series formed shapes.
d.	Finish: Light gray shop prime coat; minimum 0.6 mil (0.015 mm) cured film thickness, steel.
e.	Finish: No. 4 finish, stainless steel.
3.	Guide Material: Fabricate with heavy duty extruded aluminum sections with snap-on cover to conceal fasteners. Provide polypropylene pile runners on both sides of curtain to eliminate metal to metal contact between guides and curtain.
4.	Guide Material: Fabricate with 12 gauge formed steel shapes.
5.	Guide Material: Fabricate with 12 gauge formed stainless steel shapes.
6.	Guide Finish: Aluminum Guide (for Steel Slat with Baked Enamel Coating): Clear anodized.
7.	Guide Finish: Aluminum Guide (for Steel Slat with Powder Coating): Match slat powder coating.
8.	Guide Finish: Aluminum Guide (with Aluminum Slat): Match slat finish.
9.	Guide Finish: Steel: Phosphate treatment followed by a light gray baked-on polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
10.	Guide Finish: Steel: Phosphate treatment followed by a corrosion inhibitive baked-on zinc-rich gray polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
11.	Guide Finish: Steel: ASTM A 123, Grade 85 zinc coating, hot-dip galvanized after fabrication.
12.	Guide Finish: Steel: Phosphate treatment followed by baked-on polyester powder coat, minimum 2.5 mil (0.065 mm) cured film thickness; ASTM D-3363 pencil hardness: H or better.
a.	Color: Color as selected by Architect from manufacturer's standard color range, minimum 32 colors.
b.	Color: Custom color as selected by Architect.
13.	Guide Finish: Stainless steel: No. 4 finish.
14.	Operator and Bracket Mechanism Cover: Provide sheet metal cover to provide weather resistance and to enclose exposed moving operating components at coil area of unit. Finish and material to match door hood.
15.	Counterbalance Shaft Assembly:
a.	Barrel: Steel pipe capable of supporting curtain load with maximum deflection of 0.03 inches per foot (2.5 mm per meter) of width.
b.	Spring Balance: Oil-tempered, heat-treated steel helical torsion spring assembly designed for proper balance of door to ensure that maximum effort to operate will not exceed 25 lbs (110 N), heel for applying and adjusting spring torque.
16.	Tube Motor Shaft Assembly:
a.	Barrel: Steel pipe capable of supporting curtain load with maximum deflection of 0.03 inches per foot (2.5 mm per meter) of width.
17.	Brackets: Fabricated from plate with bearings at rotating support points to support counterbalance shaft assembly and form end closures for hood.
a.	Bracket Material: Steel.
b.	Bracket Material: AISI 300 series stainless steel.
c.	Bracket Finish: Steel - Light gray shop prime coat; minimum 0.6 mils (0.015 mm) cured film thickness.
d.	Bracket Finish: Steel - Phosphate treatment followed by a light gray baked-on polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
e.	Bracket Finish: Phosphate treatment followed by corrosion inhibitive baked-on zinc-rich gray polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
f.	Bracket Finish: ASTM A 123, Grade 85 zinc coating, hot-dip galvanized after fabrication.
g.	Bracket Finish: Phosphate treatment followed by baked-on polyester powder coat, minimum 2.5 mil (0.065 mm) cured film thickness; ASTM D-3363 pencil hardness: H or better.
1)	Color: Color as selected by Architect from manufacturer's standard color range, minimum 32 colors.
2)	Color: Custom color as selected by Architect.
h.	Bracket Finish: No. 4 finish, stainless steel.
18.	Hood and Fascia: With reinforced top and bottom edges. Provide minimum 1/4 inch (6.35 mm) steel intermediate support brackets as required to prevent excessive sag.
a.	Hood and Fascia Material: 24 gauge stainless steel.
b.	Hood and Fascia Material: 24 gauge steel.
c.	Hood and Fascia Material: 0.040 inch (1.016 mm) aluminum.
d.	Hood and Fascia Finish: GalvaNex Coating System to include an ASTM A 653 galvanized base coating treated with dual process rinsing agents in preparation of a chemical bonding, light gray baked-on polyester base coat and a light gray baked-on polyester finish coat. The scientific organic material composition and chemical bonding process of GalvaNex produces a superior finish against corrosion and abrasion. GalvaNex components include a limited two year finish warranty.
e.	Hood and Fascia Finish: GalvaNex Coating System and phosphate treatment followed by baked-on polyester powder coat, minimum 2.5 mil (0.065 mm) cured film thickness; ASTM D-3363 pencil hardness: H or better.
1)	Color: Color as selected by Architect from manufacturer's standard color range, minimum 32 colors.
2)	Color: Custom color as selected by Architect.
f.	Hood and Fascia Finish: Stainless steel: No. 4 finish.
g.	Hood and Fascia Finish: Aluminum - Mill finish.
h.	Hood and Fascia Finish: Aluminum - Clear anodized.
i.	Hood and Fascia Finish: Aluminum - Medium bronze anodized.
j.	Hood and Fascia Finish: Aluminum - Dark bronze anodized.
k.	Hood and Fascia Finish: Aluminum -Black anodized.
19.	Hood and Fascia: Sheet brake metal with reinforced top and bottom edges. 
a.	Hood and Fascia Material: 16 gauge stainless steel.
b.	Hood and Fascia Material: 16 gauge steel.
c.	Hood and Fascia Finish: Stainless steel: No. 4 finish.
d.	Hood and Fascia Finish: Steel - Light gray shop prime coat; minimum 0.6 mils (0.015 mm) cured film thickness.
D.	Smoke Seals:
1.	Bottom Bar, Manual Operated Doors: UL Tested PVC double bulb seal.
2.	Bottom Bar, Motor Operated Doors: Combination smoke seal/sensing edge as specified.
3.	Guides and Head: Replaceable, UL listed, nylon pile smoke seals sealing against fascia side of curtain.
E.	Weather/Smoke Seal - Sensing Edge: 
1.	Provide an electric sensing edge device. Provide automatic control by an automatic sensing switch within neoprene astragal extending full width of door bottom bar. 
2.	Response: Contact before door fully closes shall cause door to immediately stop downward travel and reverse direction to the fully opened position. 
3.	Response: Contact before door fully closes shall cause door to immediately stop downward travel. 
4.	Type: Provide a self-monitoring wireless sensing edge connection to motor operator eliminating the need for a physical traveling electric cord connection between bottom bar sensing edge device and motor operator. Supervised system alters normal door operation preventing damage, injury or death due to an inoperable sensing edge system.
5.	Type: Provide a wireless sensing edge connection to motor operator eliminating the need for a physical traveling electric cord connection between bottom bar sensing edge device and motor operator.
6.	Type: Provide an electric sensing edge device. 
a.	Provide self-coiling cable connection to control circuit.
b.	Provide retracting safety cord and reel connection to control circuit.
F.	Locking:
1.	Locking: Locking thumb wing latch located on coil side of bottom bar at each jamb extending lock bolt through slots in guides. Keyed alike but not master keyed.
a.	Switches: Interlock switches on motor operated units.
2.	Locking: Padlockable slide bolt on coil side of bottom bar at each jamb extending into slots in guides.
a.	Switches: Interlock switches on motor operated units.
3.	Masterkeyable cylinder in bottom bar. 
a.	Configuration: Operable from coil side of bottom bar.
b.	Configuration: Operable from fascia side of bottom bar.
c.	Configuration: Operable from both sides of bottom bar.
d.	Switches: Interlock switches on motor operated units.
G.	Graphics Door Image: 
1.	Flat face surface of door curtain slats, hood and fascia, as indicated, to include a factory applied color process, 2 mil (0.05 mm) thick vinyl graphic image, 3M or equal. 
2.	Color Process: 2 color.
3.	Color Process: 4 color.
4.	Graphic image to be selected and electronically supplied by customer. 
H.	Countertops:
1.	Countertops: Integral, 14 gauge AISI 300 series stainless steel formed shape; No. 4 finish.
2.	Countertop: Plastic laminate covered, 1-1/4 inches (32 mm) thick, of size and configuration for opening size and wall construction. Color as selected by Architect from standard range of Wilson Art or Formica plastic laminates.
3.	Labeled Countertops: Non-Integral, 1-1/2 Hour UL Labeled, 1-5/8 inches (41 mm) thick, laminate covered, of size and configuration made for opening size and wall construction. Color as selected by Architect from standard range of manufacturer approved WilsonArt or Formica laminates.
I.	Manual Operation/Non Labeled Counter Doors:
1.	Manual Push-Up: Provide lift handles on bottom bar or pole with hook.
2.	Manual Crank Hoist: Provide crank hoist operator including crank gear box, steel crank drive shaft and geared reduction unit. Fabricate gear box to completely enclose operating mechanism and be oil-tight.
J.	Control Station:
1.	Motor Control Station: Surface mounted, "Open/Close/Stop" push buttons; NEMA 1.
2.	Motor Control Station: Surface mounted, "Open/Close" push buttons; NEMA 1.
3.	Motor Control Station: Flush mounted, "Open/Close/Stop" push buttons; NEMA 1B.
4.	Motor Control Station: Flush mounted, "Open/Close" push buttons; NEMA 1B.
5.	Motor Control Station: Flush mounted, "Open/Close" key switch; NEMA 1B.
6.	Motor Control Station: Flush mounted, "Open/Close" key switch with "Stop" push button; NEMA 1B.
7.	Motor Control Station: Surface mounted, "Open/Close" key switch; NEMA 3R.
8.	Motor Control Station: Surface mounted, "Open/Close" key switch with "Stop" push button; NEMA 3R.
9.	Motor Control Station: Surface mounted, "Open/Close/Stop," push buttons with keyed lock-out, not masterkeyable; NEMA 4.
K.	Motor Operators/Non Labeled Counter Doors:
1.	Motor Operator: Supply Clopay Model MG, industrial duty - rated for a maximum of 20 cycles per hour, cULus listed, Totally Enclosed Non Ventilated gear head operator(s) rated hp as recommended by door manufacture for size and type of door. Volts and Phase as available and scheduled.
a.	Provide complete with:
1)	Electric motor and factory pre-wired motor control terminals.
2)	Maintenance free solenoid actuated brake.
3)	Control station(s).
4)	Emergency manual chain hoist.
5)	Operator shall be equipped with a disconnect cable for auxiliary push-up operation. 
b.	Motor shall be high starting torque, industrial type, protected against overload with an auto-reset thermal sensing device. Primary speed reduction shall be heavy-duty, lubricated gears with mechanical braking to hold the door in any position. 
c.	Operator shall be equipped with an emergency manual chain hoist assembly that safely cuts operator power when engaged. A disconnect chain shall not be required to engage or release the manual chain hoist. 
d.	Provide an integral Motor Mounted Interlock system to prevent damage to door and operator when mechanical door locking devices are provided. 
e.	Operator shall be capable of driving the door at a speed of 6 to 9 inches per second (15 to 23 cm/sec). Fully adjustable, driven linear screw type cam limit switch mechanism shall synchronize the operator with the door. The electrical contractor shall mount the control station(s) and supply the appropriate disconnect switch, all conduit and wiring per the overhead door wiring instructions.
2.	Motor Operator: Supply Tube Motor Operator - rated for a maximum of 10 cycles per day, cULus recognized, rated as recommended by door manufacturer for size and type of door, 110 Volts, 1 Phase. Provide complete with electric tube motor, maintenance free electric brake, emergency manual crank hoist and control station(s). Motor shall be protected against overload with an auto-reset thermal sensing device. Operator shall be equipped with an emergency manual crank hoist assembly that safely cuts operator power when engaged. A disconnect chain shall not be required to engage or release the manual crank hoist. Operator shall be capable of 10-14 RPM. Fully adjustable, mechanical internal worm limit switch mechanism shall synchronize the operator with the door. The electrical contractor shall mount the control station(s) and supply the appropriate disconnect switch, all conduit and wiring per the overhead door wiring instructions.
L.	Motor Operators/Labeled Fire Doors:
1.	Motor Operated: Model FS, UL listed and FM approved, NEMA 1 enclosure rating, horsepower as recommended by manufacture. Voltage and phase as available and scheduled. Provide open drip-proof motor, removable without affecting setting of limit switches; UL listed thermal overload protection; solenoid brake; planetary reduction gearing and rotary limit switches; transformer with 24 v control secondary; and all integral electrical components prewired to terminal blocks.
a.	Automatic closure shall be activated by fusible link.
b.	Automatic closure shall be activated by a local smoke/fire detector by means of a fail-safe releasing device. Doors shall not require a releasing device when activated by an alarm signal.
c.	Automatic closure shall be activated by a central smoke/fire alarm system by means of a fail-safe releasing device. Doors shall not require a releasing device when activated by an alarm signal.
d.	Doors shall maintain an average closing speed of not more than 9 inches (229 mm) per second during automatic closing. When automatic closure is activated, electric sensing edge and push button are inoperable.
1)	Doors shall be fail-safe and close upon power failure.
2)	Resetting of spring tension or mechanical dropouts shall not be required. Upon restoration of power, replacement of fusible link or clearing of the alarm signal, doors shall immediately reset by opening with the push button.
3)	The electrical contractor shall mount the control station(s) and supply the appropriate disconnect switch, all conduit and wiring per the overhead door wiring instructions.
2.	Battery Back-up System: Provide Model F-BBU Battery Back-Up System for FS Motor Operator. Provides four hours of door open holding time in the event of a power failure. Can power local detectors and warning appliances. Allows for programming open/close obstruction cycling should the sensing edge encounter a stationary obstruction in the opening during AC power, alarm signal closing.
3.	Fire Emergency Annunciator: fire emergency annunciator to give advanced warning that the fire door is about to close. Warning signal to activate upon alarm signal.
a.	Fire Emergency Annunciator Type: ADA compliant horn/strobe.
b.	Fire Emergency Annunciator Type: Provide Voice Warning Module. 
4.	Fire Detection: Ionization Smoke Detector UL listed.
5.	Fire Detection: Photoelectric Smoke/Heat Detector UL listed.
M.	Manual Operation/Labeled Fire Doors:
1.	Manual Chain Hoist: Provide combination chain / controlled closing system operator including endless steel chain, geared reduction unit and chain keeper.
a.	Provide a wall mounted Push To Close station located at floor level. Integral to the unit is a locking mechanism to hold the door at any position of travel during normal door operation mode and a governor to control automatic closing speed.
b.	Provide a combination close operation / automatic drop test cable located at floor level. Integral to the unit is a locking mechanism to hold the door at any position of travel during normal door operation mode and a governor to control automatic closing speed.
2.	Manual Crank Hoist: Provide combination crank / controlled closing system operator including removable hand crank and geared reduction unit.
a.	Provide a wall mounted Push To Close station located at floor level. Integral to the unit is a locking mechanism to hold the door at any position of travel during normal door operation mode and a governor to control automatic closing speed.
b.	Provide a wall mounted combination close operation / automatic drop test cable located at floor level. Integral to the unit is a locking mechanism to hold the door at any position of travel during normal door operation mode and a governor to control automatic closing speed.
3.	Manual Push-Up with Conventional Spring Release System: Provide lift handles on bottom bar and pole with hook.
a.	Automatic closure shall maintain an average closing speed of not less than 6 inches (152 mm) nor more than 24 inches (610 mm) per second during automatic closing per NFPA 80. Resetting of spring tension and mechanical dropouts by a trained door systems technician is required.
b.	Automatic closure shall be activated by fusible link.
c.	Automatic closure shall be activated by a local smoke/fire detector by means of a fail-safe releasing device. 
d.	Automatic closure shall be activated by a central smoke/fire alarm system by means of a fail-safe releasing device.
4.	Fire Emergency Annunciator: fire emergency annunciator to give advanced warning that the fire door is about to close. Warning signal to activate upon alarm signal.
a.	Fire Emergency Annunciator Type: ADA compliant horn/strobe.
b.	Fire Emergency Annunciator Type: Provide Voice Warning Module. 
5.	Fire Detection: Ionization Smoke Detector UL listed.
6.	Fire Detection: Photoelectric Smoke/Heat Detector UL listed.
N.	Automatic Closing and Speed Governor Mechanism:
1.	Motor Operated System:
a.	Activation: As specified.
b.	Operation: Motor operator shall close door upon signal from fire detector, power outage or melting of fusible link as specified.
c.	Closing Speed: Not more than 9 inches (229 mm) per second.
d.	Reset Procedure: Operation of control station after alarm is cleared or power is restored or replace fusible link. Resetting of spring tension or mechanical dropouts shall not be required.
2.	Manual Operation System:
a.	Operation: Hand chain and hand crank operation as scheduled and use of a wall mounted Push To Close station or combination close operation / automatic drop test cable as specified, located at floor level for normal use. When automatic closing is activated, integral brake and operator shall disengage. Integral governor controls closing speed.
1)	Activation: As specified.
2)	Average Closing Speed: Not more than 9 inches (229 mm) per second.
3)	Reset Procedure: Resetting of spring tension or mechanical dropouts shall not be required. 
a)	If tested by activating Push To Close station or automatic drop test cable, reset by releasing controller. 
b)	If activated by an automatic reset release device, clear alarm and/or restore power.
c)	If tested by activating a floor level reset release device, pull and hold floor level release reset cable for 3 seconds once alarm is cleared and/or power is restored.
d)	If tested by melting / cutting of fusible link, replace fusible link.
b.	Operation: Manual Push-Up.
1)	Product: Fusible Link.
2)	Activation: Melting of fusible link.
3)	Average Closing Speed: not less than 6 inches (152 mm) or more than 24 inches (610 mm) per second.
4)	Reset Procedure: Reset spring tension and mechanical dropouts; replace fusible link.
c.	Operation: Manual Push-Up.
1)	Product: Fusible Link with FireGard AR-D Release Device.
2)	Activation: Central alarm system or local smoke and heat detectors or power outage in excess of 10 seconds or melting of fusible link.
3)	Average Closing Speed: Not less than 6 inches (152 mm) nor more than 24 inches (610 mm) per second.
4)	Reset Procedure: Reset spring tension and mechanical dropouts; reset FireGard AR-D or replace fusible link.
d.	Operation: Manual Push-Up.
1)	Product: Fusible Link with FireGard BB Release Device.
2)	Activation: Central alarm system or local smoke and heat detectors or power outage in excess of 72 hours or melting of fusible link.
3)	Average Closing Speed: Not less than 6 inches (152 mm) nor more than 24 inches (610 mm) per second.
4)	Reset Procedure: Reset spring tension and mechanical dropouts; reset FireGard BB or replace fusible link.
e.	Operation: Manual Push-Up.
1)	Product: Fusible Link with FireGard DC Release Device.
2)	Activation: Central alarm system or local smoke and heat detectors or DC alarm system power outage or melting of fusible link.
3)	Average Closing Speed: Not less than 6 inches (152 mm) nor more than 24 inches (610 mm) per second.
4)	Reset Procedure: Reset spring tension and mechanical dropouts; reset FireGard DC or replace fusible link.
2.4	SECURITY GRILLES
A.	Product: Overhead Glazed Rolling Grille: Model: CESG11 as manufactured by Clopay Corporation.
B.	Product: Overhead Rolling Grille: Model: CESG10 Straight Pattern as manufactured by Clopay Corporation.
C.	Product: Overhead Rolling Grille: Model: CESG12 Brick Pattern as manufactured by Clopay Corporation.
D.	Design Requirements:
1.	Cycle Life: Design grilles of standard construction for normal use of up to 5 cycles per day maximum.
2.	Cycle Life: Design grilles of special construction for high cycle use. Expected cycles of up to ____ per day.
E.	Curtain Construction - Open Design:
1.	Straight Pattern (Model CESG 10):
a.	Horizontal Rods: Solid 5/16 inch (8 mm) diameter, 5056 H32 aluminum alloy.
b.	Horizontal Rods: Solid 5/16 inch (8 mm) diameter, AISI 300 series stainless steel.
c.	Horizontal Rods: Solid 5/16 inch (8 mm) diameter galvanized steel.
d.	Vertical Spacing: 2 inches (50.8 mm) on center.
e.	Vertical Chains: Grommetted links, 3/4 inch (19 mm) wide, positioned by E-rings. Provide double E-rings on horizontal bars on both sides of end chains to retain curtain in guides.
f.	Vertical Chain Material: Aluminum.
g.	Vertical Chain Material: Stainless steel.
h.	Vertical Chain Spacing: 9 inch (228.6 mm) centers. 
i.	Vertical Chain Spacing: 6 inch (152.4 mm) centers. 
j.	Vertical Chain Spacing: 3 inch (76.2 mm) centers. 
2.	Brick Pattern (CESG 12):
a.	Horizontal Rods: Solid 5/16 inch (8 mm) diameter, 5056 H32 aluminum alloy sleeved with horizontal aluminum tube spacers to separate vertical links.
b.	Vertical Spacing 2 inches (50.8 mm).
c.	Vertical Links: Heavy duty aluminum links, 3/4 inch (19mm) wide, positioned by tube spacers on 9 inch (228.6 mm) staggered centers. End links to be held in place by self-locking retaining rings.
3.	Bottom Bar: 2 inches by 3-1/2 inches (50.8 mm by 88.9 mm) extruded aluminum tubular section.
4.	Reinforce bottom bar with 3 inches by 2 inches by 3/16 inch (76.2 by 50.8 by 4.76 mm) aluminum angle(s).
5.	Finish:
a.	Aluminum Curtain and Bottom Bar: 
1)	Curtain: Aluminum - Mill finish.
2)	Curtain: Aluminum - Clear anodized.
3)	Curtain: Aluminum - Medium bronze anodized.
4)	Curtain: Aluminum - Dark bronze anodized.
5)	Curtain: Aluminum - Black anodized.
6)	Bottom Bar: Aluminum - Mill finish.
7)	Bottom Bar: Aluminum - Clear anodized.
8)	Bottom Bar: Aluminum - Medium bronze anodized.
9)	Bottom Bar: Aluminum - Dark bronze anodized.
10)	Bottom Bar: Aluminum - Black anodized.
b.	Stainless Steel Curtain with Aluminum Bottom Bar:
1)	Curtain: Factory polished.
2)	Bottom Bar: Clear anodized.
3)	Bottom Bar: Mill finish.
c.	Stainless Steel Curtain with Stainless Steel Bottom Bar: Factory polished.
d.	Galvanized Steel Rods with Aluminum Chains and Bottom Bar:
1)	Rods: Galvanized steel, unpainted.
2)	Chains and Bottom Bar: Mill finish.
3)	Chains and Bottom Bar: Clear anodized.
F.	Curtain Construction - Clear Panel Design (CESG 11):
1.	Horizontal Rods: Solid 5/16 inch (8 mm) diameter, 5056 H32 aluminum alloy at 3 inches (76.2 mm) on center.
2.	Panel Module: 12 inches by 3 inches by 1/8 inch (304.8 by 76.2 by 3.2 mm) thick clear, flame retardant polycarbonate, secured to bronze colored molded nylon links. Lock end chains into guides to retain curtain ends.
3.	Bottom Bar: 2 inches by 3-1/2 inches (50.8 by 88.9 mm) extruded aluminum tubular section.
4.	Reinforce bottom bar with 3 inches by 2 inches by 3/16 inch (76.2 by 50.8 by 4.76 mm) aluminum angle(s).
5.	Finish:
a.	Curtain: Mill finish rods with bronze colored nylon links and clear polycarbonate panels.
b.	Curtain: Medium bronze anodized rods with bronze colored nylon links and clear polycarbonate panels.
c.	Curtain: Clear anodized rods with bronze colored nylon links and clear polycarbonate panels.
d.	Bottom Bar: Medium bronze anodized.
e.	Bottom Bar: Clear anodized.
f.	Bottom Bar: Mill finish.
G.	Guides, Wall Mounted: Heavy duty extruded sections.
1.	Guide Material: Aluminum.
2.	Provide snap-on cover to conceal fasteners on both sides of curtain. 
3.	Provide snap-on cover to conceal fasteners and polypropylene pile runners on both sides of curtain. 
4.	Provide steel mounting angle as required for face of wall installation.
5.	Provide aluminum mounting angle as required for face of wall installation.
H.	Guides, Tube Mounted: Heavy duty extruded aluminum sections. Provide tubes, floor saddles and hardware as recommended by manufacturer to support grille.
1.	Guide Material: Steel.
2.	Guide Material: Aluminum.
3.	Provide snap-on cover to conceal fasteners on both sides of curtain. 
4.	Provide snap-on cover to conceal fasteners and polypropylene pile runners on both sides of curtain. 
5.	Provide steel mounting angle as required for face of wall installation.
6.	Provide aluminum mounting angle as required for face of wall installation.
I.	Guide Finish:
1.	Aluminum: Mill finish.
2.	Aluminum: Clear anodized.
3.	Aluminum: Medium bronze anodized.
4.	Aluminum: Dark bronze anodized.
5.	Aluminum: Black anodized.
6.	Steel: Unpainted.
7.	Phosphate treatment followed by a light gray baked-on polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
8.	Phosphate treatment followed by a corrosion inhibitive baked-on zinc-rich gray polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
J.	Operator and Bracket Mechanism Cover: Provide sheet metal cover to provide weather resistance and enclose exposed moving operating components at coil area of unit as required or indicated. Finish matching grille hood. 
1.	Cover Material: 24 gauge galvanized steel.
2.	Cover Material: 24 gauge stainless steel.
3.	Cover Material: .0.040 inch (1.0 mm) aluminum.
K.	Counterbalance Shaft Assembly:
1.	Barrel: Steel pipe capable of supporting curtain load with maximum deflection of 0.03 inches per foot (2.5 mm per meter) of width.
2.	Spring Balance: Oil-tempered, heat-treated steel helical torsion spring assembly designed for proper balance of grille to ensure that maximum effort to operate will not exceed 25 lbs (110 N). Provide wheel for applying and adjusting spring torque.
L.	Brackets: Fabricate from minimum 3/16 inch (5 mm) steel plate with permanently lubricated ball or roller bearings at rotating support points to support counterbalance shaft assembly and form end closures.
1.	Bracket Finish: Phosphate treatment followed by a light gray baked-on polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
2.	Bracket Finish: Phosphate treatment followed by corrosion inhibitive baked-on zinc-rich gray polyester powder coat; minimum 2.5 mil (0.065 mm) cured film thickness.
3.	Bracket Finish: ASTM A 123, Grade 85 zinc coating, hot-dip galvanized after fabrication.
M.	Hood and Fascia: With reinforced top and bottom edges. Provide minimum 1/4 inch (6.35 mm) steel intermediate support brackets as required to prevent excessive sag.
1.	Hood Material: 24 gauge galvanized steel.
2.	Hood Material: 24 gauge stainless steel.
3.	Hood Material: 0.040 inch (1.016 mm) aluminum.
4.	Hood Finish: GalvaNex Coating System to include an ASTM A 653 galvanized base coating treated with dual process rinsing agents in preparation of a chemical bonding, light gray baked-on polyester base coat and a light gray baked-on polyester finish coat. The scientific organic material composition and chemical bonding process of GalvaNex produces a superior finish against corrosion and abrasion. GalvaNex components include a limited two year finish warranty.
5.	Hood Finish: Stainless steel: No. 4 finish.
6.	Hood Finish: Aluminum - Mill finish.
7.	Hood Finish: Aluminum - Clear anodized.
8.	Hood Finish: Aluminum - Medium bronze anodized.
9.	Hood Finish: Aluminum - Dark bronze anodized.
10.	Hood Finish: Aluminum - Black anodized.
N.	Locking:
1.	Manual Push-Up: Keyed cylinder locking into both jambs operable from both sides of curtain.
2.	Manual Crank Hoist: Keyed cylinder locking into both jambs operable from coil side of curtain.
3.	Motor Operated: Keyed cylinder locking into both jambs operable from both sides of curtain with motor interlock cutout switches.
4.	Emergency Egress Lock: Key cylinder locking from public side, thumb turn cylinder locking from tenant side, locking into both jambs. Provide an additional security panel in curtain. 
5.	Provide motor interlock cutout switches on motorized units.
O.	Manual Operation:
1.	Manual Push-Up: Provide pole with hook. 
2.	Manual Push-Up with EZ Lift Construction Package: Provide pole with hook. 
3.	Manual Crank Hoist: Provide crank hoist operator including crank gear box, steel crank drive shaft and geared reduction unit. Fabricate gear box to completely enclose operating mechanism and be oil-tight.
P.	Sensing Edge: 
1.	Provide an electric sensing edge device. Provide automatic control by an automatic sensing switch within neoprene or rubber astragal extending full width of grille bottom bar. 
2.	Response: Contact before grille fully closes shall cause grille to immediately stop downward travel and reverse direction to the fully opened position. 
3.	Response: Contact before grille fully closes shall cause grille to immediately stop downward travel. 
4.	Type: Provide a self-monitoring wireless sensing edge connection to motor operator eliminating the need for a physical traveling electric cord connection between bottom bar sensing edge device and motor operator. Supervised system alters normal grille operation preventing damage, injury or death due to an inoperable sensing edge system.
5.	Type: Provide a wireless sensing edge connection to motor operator eliminating the need for a physical traveling electric cord connection between bottom bar sensing edge device and motor operator.
6.	Type: Provide an electric sensing edge device. 
a.	Provide self-coiling cable connection to control circuit.
b.	Provide retracting safety cord and reel connection to control circuit.
Q.	Control Station:
1.	Motor Control Station: Flush mounted, "Open/Close" push buttons; NEMA 1B.
2.	Motor Control Station: Flush mounted, "Open/Close" key switch; NEMA 1B.
3.	Motor Control Station: Surface mounted, "Open/Close" push buttons; NEMA 1.
4.	Motor Control Station: Surface mounted, "Open/Close" key switch; NEMA 3R.
5.	Motor Control Station: Flush mounted, "Open/Close/Stop" push buttons; NEMA 1B.
6.	Motor Control Station: Flush mounted, "Open/Close" key switch with "Stop" push button; NEMA 1B.
R.	Motor Operators:
1.	Motor Operator: Supply Clopay Model MG, industrial duty - rated for a maximum of 20 cycles per hour, cULus listed, Totally Enclosed Non Ventilated gear head operator(s) rated hp as recommended by grille manufacture for size and type of grille. Volts and Phase as available and scheduled.
a.	Provide complete with:
1)	Electric motor and factory pre-wired motor control terminals.
2)	Maintenance free solenoid actuated brake.
3)	Control station(s).
4)	Emergency manual chain hoist.
5)	Operator shall be equipped with a disconnect cable for auxiliary push-up operation. 
b.	Motor shall be high starting torque, industrial type, protected against overload with an auto-reset thermal sensing device. Primary speed reduction shall be heavy-duty, lubricated gears with mechanical braking to hold the grille in any position. 
c.	Operator shall be equipped with an emergency manual chain hoist assembly that safely cuts operator power when engaged. A disconnect chain shall not be required to engage or release the manual chain hoist. 
d.	Operator drive and grille driven sprockets shall be provided with #50 roller chain. 
e.	Provide an integral Motor Mounted Interlock system to prevent damage to grille and operator when mechanical grille locking devices are provided. 
f.	Operator shall be capable of driving the grille at a speed of 8 to 9 inches per second (20 to 23 cm/sec). Fully adjustable, driven linear screw type cam limit switch mechanism shall synchronize the operator with the grille. The electrical contractor shall mount the control station(s) and supply the appropriate disconnect switch, all conduit and wiring per the overhead grille wiring instructions.
g.	Emergency Egress System: Provide wall mounted manual release system pull handle to disengage motor operator and automatically open grille for emergency egress without the use of electrical power. Release of pull handle will reset grille to normal motor operation.
2.	Motor Operator: Supply Clopay Model SG, continuous duty, cULus listed, totally enclosed fan cooled gear head operator(s) rated hp as recommended by grille manufacture for size and type of grille. Volts and Phase as available and scheduled.
a.	Provide complete with electric motor and factory pre-wired motor control terminals, maintenance free solenoid actuated brake, emergency manual chain hoist provided up to 2 hp and control station(s). 
b.	Motor shall be high starting torque, industrial type, with overload protection. Primary speed reduction shall be heavy-duty gears running in grease or oil bath with mechanical braking to hold the grille in any position. When equipped, the emergency manual chain hoist assembly is automatically disengaged when motor is energized. A disconnect chain shall not be required to engage or release the manual chain hoist. 
c.	Operator drive and grille driven sprockets shall be provided with minimum #50 roller chain. 
d.	Operator shall be capable of driving the grille at a speed of 8 to 9 inches per second (20 to 23 cm/sec). Fully adjustable, driven linear screw type cam limit switch mechanism shall synchronize the operator with the grille. The motor shall be removable without affecting the limit switch settings. The electrical contractor shall mount the control station(s) and supply the appropriate disconnect switch, all conduit and wiring per the overhead grille wiring instructions.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Examine wall and overhead areas, including opening framing and blocking, with installer present, for compliance with requirements for installation tolerances, clearances, and other conditions affecting performance of Work in this Section.
B.	If preparation is the responsibility of another installer, notify Architect of deviations from manufacturer's recommended installation tolerances and conditions.
C.	Do not proceed with installation until substrates have been properly prepared and deviations are corrected.
D.	Commencement of installation constitutes acceptance of conditions. 
3.2	INSTALLATION
A.	General: Install unit and operating equipment with necessary hardware, anchors, inserts, hangers and supports.
B.	Comply with NFPA 80 and follow manufacturer's installation instructions.
C.	Comply with NFPA80 and NFPA 105 and follow manufacturer's installation instructions.
3.3	ADJUSTING
A.	Following completion of installation, including related work by others, lubricate, test, and adjust doors for ease of operation, free from warp, twist, or distortion.
3.4	FIELD QUALITY CONTROL
A.	Site Drop Test: Test units for normal operation and automatic closing. Coordinate with authorities having jurisdiction to witness test and sign Drop Test Form.
3.5	DEMONSTRATION
A.	Demonstrate proper operation to Owner's Representative.
B.	Instruct Owner's Representative in maintenance procedures.
3.6	CLEANING
A.	Clean surfaces soiled by work as recommended by manufacturer.
B.	Remove surplus materials and debris from the site.
3.7	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION