SECTION 11 52 13

PROJECTION SCREENS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2026 -  2026 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Projection Screens:
1.	Electric.
2.	Fixed Frame.
3.	Portable.
4.	Manual.
1.2	RELATED SECTIONS
A.	Division 5 - Metal Fabrications: Suspension systems for projection screens.
B.	Section 06 40 23 - Interior Architectural Woodwork: Wood trim for recessed screen installation.
C.	Section 09 22 26 - Ceiling Suspension System: Supports and trim for suspended ceilings.
D.	Section 09 23 13 - Gypsum Plaster: Ceiling for recessed screen installation.
E.	Section 09 21 16.33 - Gypsum Board Assemblies: Ceiling for recessed screen installation.
F.	Section 09 51 23- Acoustical Tile Ceilings: Ceiling for recessed screen installation.
G.	Division 26 for electrical wiring, connections, and installation of remote-control switches for electrically operated projection screens.
1.3	SUBMITTALS
A.	Submit under provisions of Section 01 30 00.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Detail dimensional drawings and wiring diagrams.
3.	Preparation instructions and recommendations.
4.	Storage and handling requirements and recommendations.
5.	Typical installation instructions.
C.	Shop Drawings: Include details of materials, construction, and finish. Include relationship with adjacent construction.
1.4	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum of five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
1.5	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.6	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.7	WARRANTY
A.	Manufacturer's standard limited warranty unless indicated otherwise.
1.	Limited five-year warranty for all motorized projection screens.
2.	Limited five-year warranty for all fixed frame projection screens.
3.	Limited one-year warranty for all manual and portable projection screens.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Da-Lite, a brand of Legrand | AV, which is located at:<BR />10900 Red Circle Dr.<BR />Minnetonka, MN 55343<BR />Toll Free Tel: 866-977-3901<BR />Fax: 877-894-6918<BR />Email: request info (https://www.legrandav.com/contact_us/email_us);Web: https://www.legrandav.com/products/da-lite 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with the provisions of Section 01 60 00.
2.2	ELECTRIC PROJECTION SCREENS
A.	Basis of Design: Tensioned Advantage with Closure Door as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	90 x 160 inches (229 x 406 cm). Diagonal: 184 inches (467 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 60 inches (127 x 103 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches (480 cm).
i.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	43 x 57 inches (109 x 145 cm). Diagonal: 72 inches (183 cm).
b.	50 x 67 inches (127 x 170 cm). Diagonal: 84 inches (213 cm).
c.	60 x 80 inches (152 x 203 cm). Diagonal: 100 inches (254 cm).
d.	69 x 92 inches 175 x 234 cm). Diagonal: 120 inches (305 cm).
e.	87 x 116 inches (221 x 295 cm). Diagonal: 150 inches (381 cm).
f.	108 x 144 inches (274 x 366 cm). Diagonal: 180 inches (457 cm).
g.	120 x 160 inches (305 x 406 cm). Diagonal: 200 inches (508 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Certifications and Compliances: Listed by Underwriters' Laboratories.
5.	Two Motors: Door motor and screen motor.
a.	Door Motor:
1)	Mounting: In the roller.
2)	Electric: 120 volt (60 Hz) 1.2 amps max.
3)	Electric: 220 Volt (50 Hz) 1.2 amps max.
4)	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and electric brake to prevent coasting.
5)	Limit Switches: Preset and adjustable. Stops fabric door in the "down" position. As door lifts to the closed position, a microswitch cuts off the electrical current to the door motor.
b.	Screen Motor:
1)	Mounting: In the roller.
2)	Electric: 120 volt (60 Hz) 2.4 amps max.
3)	Electric: 220 Volt (50 Hz) 2.4 amps max.
4)	Motor Characteristics: Three wire with ground quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
5)	Limit Switches: Pre-set and adjustable. Stop picture surface in the "up" and "down" positions.
6.	Roller Material: Rigid aluminum.
7.	Housing: Extruded aluminum.
a.	Finish: Powder coated. Color: White.
b.	Housing Bottom: Self-trimming. Built-in flange around housing bottom.
1)	Hinged Aluminum Door: Opens and closes with the lowering and raising of projection screen.
2)	Balance of Housing Bottom: A second hinged aluminum access door for manual access.
3)	Hinges: Mounted in a concealed manner.
c.	Junction Box: Internally integrated into the housing. Housing may be installed and wired into the facility electrical system during construction.
d.	Quick Connector: Mounted in housing for plug-in connection to the motorized fabric and roller assembly.
e.	For use in environmental air space according to section 300-22 (c) of the National Electric Code, and sections 2-128, 12-010 (3) and 12-100 of the Canadian Electrical Code, part 1, CSA C22.1.
f.	Overall Housing Length Dimension: +/- 1/4 inches (6 mm).
8.	Motorized Fabric and Roller Assembly: Installs in the housing at the factory or at a later time at the job site. Roller Material: Rigid metal.
9.	Integrated Low Voltage Control Unit: 
a.	Three position control switch and cover plate.
10.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking borders.
f.	Fabric Sides: Radio Frequency welded tab guide cable system on each vertical side to maintain even lateral tension and hold surface flat.
g.	Custom Slat Bar: At bottom of fabric with added weight, maintains vertical tension on the screen surface.
h.	Slat Ends: Protected by heavy duty plastic caps enclosing a preset adjustable mechanism for screen tensioning.
i.	Black Drop at Top of Screen: 12 inches (30.5 cm).
j.	Black Drop at Top of Screen: 2 inches (5.1 cm).
k.	Viewing Surface: Parallax Pure 0.8. 
l.	Viewing Surface: Parallax Stratos 1.0. 
m.	Viewing Surface: HD Progressive 1.0. 
n.	Viewing Surface: HD Progressive 1.0 Perf. 
o.	Viewing Surface: HD Progressive 1.1 Contrast. 
p.	Viewing Surface: HD Progressive 1.3. 
q.	Viewing Surface: HD Progressive ReView 0.9 (Rear).
r.	Viewing Surface: Da-Mat. 
s.	Viewing Surface: Da-Tex (Rear).
11.	Accessories:
a.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger).
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
b.	Key Locking Cover Plate for LVC Switch.
B.	Basis of Design: Tensioned Advantage Series as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	90 x 160 inches (229 x 406 cm). Diagonal: 184 inches (467 cm).
h.	99 x 176 inches (251 x 447 cm). Diagonal: 202 inches (513 cm).
i.	108 x 192 inches (274 x 488 cm). Diagonal: 220 inches (559 cm).
j.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 60 inches (127 x 103 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches (480 cm).
i.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
j.	120 x 192 inches (305 x 488 cm). Diagonal: 226 inches (574 cm).
k.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	43 x 57 inches (109 x 145 cm). Diagonal: 72 inches (183 cm).
b.	50 x 67 inches (127 x 170 cm). Diagonal: 84 inches (213 cm).
c.	60 x 80 inches (152 x 203 cm). Diagonal: 100 inches (254 cm).
d.	69 x 92 inches (175 x 234 cm). Diagonal: 120 inches (305 cm).
e.	87 x 116 inches (221 x 295 cm). Diagonal: 150 inches (381 cm).
f.	108 x 144 inches (274 x 366 cm). Diagonal: 180 inches (457 cm).
g.	120 x 160 inches (305 x 406 cm). Diagonal: 200 inches (508 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Certifications and Compliances: Listed by Underwriters' Laboratories.
5.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor and an electric brake to prevent coasting.
6.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions. 
7.	Electrical Junction Box: Externally integrated into housing. Allows housing installation and wiring to facility's electrical system during construction. 
a.	A quick connector mounted in the housing for plug-in connection to the motorized fabric and roller assembly.
8.	Electrical Junction Box: External. Extends 2-1/8 inches (5.4 cm) past housing length on left end of case, and 1-1/8 inch (2.9 cm) past ceiling flange. Standard configuration.
9.	Electrical Junction Box: Internal. Will add 3-1/2 inches (8.9 cm) to overall case length and must be specified at time of order. Recommended for drywall installations.
10.	Electrical Junction Box: External on top of case. Will add 3-1/2 inches (8.9 cm) to overall case length and 1-7/8 inches (4.8 cm) to height at left end of case. Must be specified at time of order.
11.	Motorized Fabric and Roller Assembly: Installed in the housing at the factory or later at the job site. Roller Material: Rigid steel.
12.	Screen Fabric: 
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking borders.
f.	Fabric Sides: Radio Frequency welded tab guide cable system on each vertical side to maintain even lateral tension and hold surface flat.
g.	Custom Slat Bar: At bottom of fabric with added weight, maintains vertical tension on the screen surface.
h.	Slat Ends: Protected by heavy duty plastic caps enclosing a preset adjustable mechanism for screen tensioning.
13.	Housing, Top, Front and Back: Extruded aluminum.
a.	Finish: Powder coated. Color: White.
b.	End Caps: Heavy gauge steel.
1)	Finish: Powder coated. Color: White.
c.	Housing Bottom: To have a removable access door.
1)	Access Door: Extruded aluminum.
a)	Finish: Powder coated. Color: White.
2)	Self-trimming. Built-in flange around housing bottom.
d.	For use in environmental air space in accordance with section 300-22 (c) of the National Electric Code, and sections 2-128, 12-010 (3) and 12-100 of the Canadian Electrical Code, part 1, CSA C22.1.
e.	Overall Housing Length Dimensions: +/- 1/4 inches (6 mm).
14.	Integrated Low Voltage Control Unit:
a.	Three position control switch and cover plate.
15.	Projection Information:
a.	Black Drop at Top of Screen: 12 inch (30.5 cm).
b.	Black Drop at Top of Screen: 2 inch (5.1 cm).
c.	Surfaces will be seamless in the image area.
d.	Viewing Surface: Parallax Pure 0.8. 
e.	Viewing Surface: Parallax Stratos 1.0. 
f.	Viewing Surface: HD Progressive 1.0. 
g.	Viewing Surface: HD Progressive 1.0 Perf. 
h.	Viewing Surface: HD Progressive 1.1 Contrast. 
i.	Viewing Surface: HD Progressive 1.3. 
j.	Viewing Surface: HD Progressive ReView 0.9 (Rear). 
k.	Viewing Surface: Da-Mat. 
l.	Viewing Surface: Da-Tex (Rear). 
1)	Accessories:
m.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger)
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
n.	Key Locking Cover Plate for LVC Switch.
C.	Basis of Design: Tensioned Advantage with SightLine as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	87 x 153.75 inches (221 x 391 cm). Diagonal: 177 inches (450 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	96 x 153.75 inches (244 x 391 cm). Diagonal: 182 inches (462 cm).
i.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Certifications and Compliances: Listed by Underwriters' Laboratories.
4.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor and an electric brake to prevent coasting.
5.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
6.	Electrical Junction Box: External. Extends 2-1/8 inches (5.4 cm) past housing length on left end of case, and 1-1/8 inch (2.9 cm) past ceiling flange. Standard configuration.
7.	Electrical Junction Box: Internal. Will add 3-1/2 inches (8.9 cm) to overall case length and must be specified at time of order. Recommended for drywall installations.
8.	Electrical Junction Box: External on top of case. Will add 3-1/2 inches (8.9 cm) to overall case length and 1-7/8 inches (4.8 cm) to height at left end of case. Must be specified at time of order.
9.	Motorized Fabric and Roller Assembly: Installed in the housing at the factory or at a later time at the job site. Roller Material: Rigid steel.
a.	Suspension Cables: Roller to drop material from case on 1 mm diameter, 7/19 galvanized aircraft cable. 
b.	Adjustable Cable Drop:
1)	Overall Drop Length: 70 inches (178 cm) maximum.
2)	Factory Set Drop: 24 inches (6.1 cm).
3)	Field Adjustment: Set to desired drop distance at installation.
4)	Case Lengths up to 120 inches (305 cm): Screens drop from 3 cables.
5)	Case Lengths over 120 inches (305 cm): Screens drop from 4 cables.
10.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking borders.
f.	Fabric Sides: Radio Frequency welded tab guide cable system on each vertical side to maintain even lateral tension and hold surface flat.
g.	Custom Slat Bar: At bottom of fabric with added weight, maintains vertical tension on the screen surface.
h.	Slat Ends: Protected by heavy duty plastic caps enclosing a preset adjustable mechanism for screen tensioning.
11.	Housing Top, Front and Back: Extruded aluminum.
a.	Finish: Powder coated. Color: White.
b.	End Caps: Heavy gauge steel.
1)	Finish: Powder coated. Color: White.
c.	Housing Bottom: To have a removable access door.
1)	Access Door: Extruded aluminum.
a)	Finish: Powder coated. Color: White.
2)	Self-trimming, with built-in flange around housing bottom.
d.	Overall Housing Length Dimensions +/- 1/4 inches (6 mm).
e.	For use in environmental air space in accordance with section 300-22 (c) of the National Electric Code, and sections 2-128, 12-010 (3) and 12-100 of the Canadian Electrical Code, part 1, CSA C22.1.
12.	Integrated Low Voltage Control Unit:
a.	Three position control switch and cover plate.
13.	Electrical Junction Box: Extends 2-1/8 inches (5.4 cm) past housing length on left end of case, 1-1/8 inch (2.9 cm) past ceiling flange.
14.	Junction Box: Internal. Will add 3-1/2 inches (8.9 cm) to overall case length and must be specified at time of order, recommended for drywall installations.
15.	Junction Box: On top of housing. Will add 3-1/2 inches (8.9 cm) to overall case length and 1-7/8 inches (4.8 cm) to height at left end of case; must be specified at time of order.
16.	Projection Information:
a.	Black Drop at Top of Screen: 12 inch (30.5 cm).
b.	Black Drop at Top of Screen: 2 inch (5.1 cm).
c.	Surfaces will be seamless in the image area.
d.	Viewing Surface: Parallax Stratos 1.0. 
e.	Viewing Surface: HD Progressive 1.0. 
f.	Viewing Surface: HD Progressive 1.0 Perf. 
g.	Viewing Surface: HD Progressive 1.1 Contrast. 
h.	Viewing Surface: HD Progressive 1.3. 
i.	Viewing Surface: Da-Mat. Fire Retardant.
17.	Accessories:
a.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger).
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
b.	Key Locking Cover Plate for LVC Switch.
D.	Basis of Design: Tensioned Advantage over 14 ft (427 cm) Wide with Closure Door:
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	108 x 192 inches (274 x 488 cm). Diagonal: 220 inches (559 cm).
b.	121 x 216 inches (307 x 549 cm). Diagonal: 247 inches (627 cm).
c.	135 x 240 inches (343 x 610 cm). Diagonal: 275 inches (699 cm).
d.	146 x 260 inches (371 x 660 cm). Diagonal: 298 inches (757 cm).
e.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
b.	120 x 192 inches (305 x 488 cm). Diagonal: 226 inches (574 cm).
c.	135 x 216 inches (342 x 549 cm). Diagonal: 255 inches (648 cm).
d.	150 x 240 inches (381 x 610 cm). Diagonal: 283 inches (719 cm).
e.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	126 x 168 inches (320 x 427 cm). Diagonal: 210 inches (533 cm).
b.	132 x 176 inches (335 x 447 cm). Diagonal: 220 inches (559 cm).
c.	144 x 192 inches (366 x 488 cm). Diagonal: 240 inches (610 cm).
d.	162 x 216 inches (411 x 549 cm). Diagonal: 270 inches (686 cm).
e.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Certifications and Compliances: Listed by Underwriters' Laboratories.
5.	Two Motors: Door motor and screen motor.
a.	Door Motor:
1)	Mounting: In the roller.
2)	Electric: 120 volt (60 Hz) 1.2 amps max.
3)	Electric: 220 Volt (50 Hz) 1.2 amps max.
4)	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and electric brake to prevent coasting.
b.	Limit Switches: Preset and adjustable. Stops fabric door in the "down" position. As door lifts to the closed position, a microswitch cuts off the electrical current to the door motor.
c.	Screen Motor:
1)	Mounting: In the roller.
2)	Electric: 120 volt (60 Hz) 2.4 amps max.
3)	Electric: 220 Volt (50 Hz) 2.4 amps max.
4)	Motor Characteristics: Three wire with ground quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
d.	Limit Switches: Pre-set and adjustable. Stop picture surface in the "up" and "down" positions.
6.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking borders.
f.	Fabric Sides: Radio Frequency welded tab guide cable system on each vertical side to maintain even lateral tension and hold surface flat.
g.	Custom Slat Bar: At bottom of fabric with added weight, maintains vertical tension on the screen surface.
h.	Slat Ends: Protected by heavy duty plastic caps enclosing a preset adjustable mechanism for screen tensioning.
7.	Housing: Extruded aluminum.
a.	Finish: Powder coated. Color: White.
b.	Housing Bottom: Self-trimming. Built-in flange around housing bottom.
1)	Hinged Aluminum Door: Opens and closes with the lowering and raising of projection screen.
2)	Balance of Housing Bottom: A second hinged aluminum access door for manual access.
3)	Hinges: Mounted in a concealed manner.
c.	Overall Housing Length Dimension: +/- 1/4 inches (6 mm).
8.	Junction Box: Internally integrated into the housing. Housing may be installed and wired into the facility electrical system during construction.
a.	Quick Connector: Mounted in housing for plug-in connection to the motorized fabric and roller assembly.
9.	Motorized Fabric and Roller Assembly: Installs in the housing at the factory or at a later time at the job site. Roller Material: Rigid metal.
10.	For use in environmental air space according to section 300-22 (c) of the National Electric Code, and sections 2-128, 12-010 (3) and 12-100 of the Canadian Electrical Code, part 1, CSA C22.1.
11.	Integrated Low Voltage Control Unit: 
a.	Three position control switch and cover plate.
12.	Projection Information:
a.	Black Drop at Top of Screen: 12 inch (30.5 cm).
b.	Black Drop at Top of Screen: 2 inch (5.1 cm).
c.	Surfaces are to be seamless in the image area.
d.	Viewing Surface: Parallax Stratos 1.0. 
e.	Viewing Surface: HD Progressive 1.0. 
f.	Viewing Surface: HD Progressive 1.1 Contrast. 
g.	Viewing Surface: HD Progressive 1.3. 
h.	Viewing Surface: HD Progressive ReView 0.9 (Rear). 
i.	Viewing Surface: Da-Mat.
j.	Viewing Surface: Da-Tex (Rear). 
13.	Accessories:
a.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger).
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
b.	Key Locking Cover Plate for LVC Switch.
E.	Basis of Design: Tensioned Advantage; over 16 ft (488 cm) Wide.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	121 x 216 inches (307 x 549 cm). Diagonal: 247 inches (627 cm).
b.	135 x 240 inches (343 x 610 cm). Diagonal: 275 inches (699 cm).
c.	146 x 260 inches (371 x 660 cm). Diagonal: 298 inches (757 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	135 x 216 inches (342 x 549 cm). Diagonal: 255 inches (648 cm).
b.	150 x 240 inches (381 x 610 cm). Diagonal: 283 inches (719 cm).
c.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	162 x 216 inches (411 x 549 cm). Diagonal: 270 inches (686 cm).
b.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Certifications and Compliances: Listed by Underwriters' Laboratories.
5.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor and an electric brake to prevent coasting.
6.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
7.	Junction Box: Externally integrated into housing. Allows housing installation and wiring to facility's electrical system during construction.
a.	A quick connector mounted in the housing for plug-in connection to the motorized fabric and roller assembly.
8.	Motorized Fabric and Roller Assembly: Installed in the housing at the factory or at a later time at the job site. Roller Material: Rigid Steel.
9.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking borders.
f.	Fabric Sides: Radio Frequency welded tab guide cable system on each vertical side to maintain even lateral tension and hold surface flat.
g.	Custom Slat Bar: At bottom of fabric with added weight, maintains vertical tension on the screen surface.
h.	Slat Ends: Protected by heavy duty plastic caps enclosing a preset adjustable mechanism for screen tensioning.
10.	Housing: Extruded aluminum.
a.	Finish: Powder coated. Color: White.
b.	End Caps: Heavy gauge steel.
1)	Finish: Powder coated. Color: White.
c.	Housing Bottom: To have a removable access door.
1)	Access Door: Extruded aluminum.
a)	Finish: Powder coated. Color: White.
d.	Self-trimming. Built-in flange around the bottom of the case.
e.	For use in environmental air space in accordance with section 300-22 (c) of the National Electric Code, and sections 2-128, 12-010 (3) and 12-100 of the Canadian Electrical Code, part 1, CSA C22.1.
f.	Overall Housing Length Dimensions +/- 1/4 inches (6 mm).
11.	Junction Box: Internally integrated into the housing. Housing may be installed and wired into the facility electrical system during construction.
a.	Quick Connector: Mounted in housing for plug-in connection to the motorized fabric and roller assembly.
12.	Integrated Low Voltage Control Unit.
a.	Three position control switch and cover plate.
13.	Projection Information:
a.	Black Drop at Top of Screen: 12 inch (30.5 cm).
b.	Black Drop at Top of Screen: 2 inch (5.1 cm).
c.	Surfaces are to be seamless in the image area.
14.	Viewing Surface: Parallax Stratos 1.0.
15.	Viewing Surface: HD Progressive 1.0. 
16.	Viewing Surface: HD Progressive 1.1 Contrast. 
17.	Viewing Surface: HD Progressive 1.3. 
18.	Viewing Surface: HD Progressive ReView 0.9 (Rear). 
19.	Viewing Surface: Da-Mat.
20.	Viewing Surface: Da-Tex (Rear).
21.	Accessories:
a.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger)
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
b.	Key Locking Cover Plate for LVC Switch.
F.	Basis of Design: Advantage with Closure Door as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	90 x 160 inches (229 x 406 cm). Diagonal: 184 inches (467 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches (480 cm).
i.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	43 x 57 inches (109 x 145 cm). Diagonal: 72 inches (183 cm).
b.	50 x 67 inches (127 x 170 cm). Diagonal: 84 inches (213 cm).
c.	60 x 80 inches (152 x 203 cm). Diagonal: 100 inches (254 cm).
d.	69 x 92 inches (175 x 234 cm). Diagonal: 120 inches (305 cm).
e.	87 x 116 inches (221 x 295 cm). Diagonal: 150 inches (381 cm).
f.	105 x 140 inches (267 x 356 cm). Diagonal: 180 inches (457 cm).
g.	120 x 160 inches (305 x 406 cm). Diagonal: 200 inches (508 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Square. Viewing area (HxW).
a.	60 x 60 inches (152 x 152 mm).
b.	70 x 70 inches (178 x 178 cm).
c.	84 x 84 inches (213 x 213 mm).
d.	96 x 96 inches (244 x 244 mm).
e.	108 x 108 inches (274 x 274 mm).
f.	120 x 120 inches (305 x 305 mm).
g.	144 x 144 inches (366 x 366 mm).
h.	__ x __ inches (__ x __ cm).
5.	Certifications and Compliances: Listed by Underwriters' Laboratories.
6.	Two Motors: Door motor and screen motor.
a.	Door Motor:
1)	Mounting: In the roller.
2)	Electric: 120 volt (60 Hz) 1.2 amps max.
3)	Electric: 220 Volt (50 Hz) 1.2 amps max.
4)	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and electric brake to prevent coasting.
5)	Limit Switches: Preset and adjustable. Stops fabric door in the "down" position. As door lifts to the closed position, a microswitch cuts off the electrical current to the door motor.
b.	Screen Motor:
1)	Mounting: In the roller.
2)	Electric: 120 volt (60 Hz) 2.4 amps max.
3)	Electric: 220 Volt (50 Hz) 2.4 amps max.
4)	Motor Characteristics: Three wire with ground quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
a)	Quick Connect Male Plug-In Connector: On the motor.
5)	Limit Switches: Pre-set and adjustable. Stop picture surface in the "up" and "down" positions.
7.	Motorized Fabric and Roller Assembly: Factory installed in the housing or installed later at the job site.
a.	Roller Material: Rigid metal.
8.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking borders.
f.	Borders: None.
g.	Fabric Bottom: Formed into a pocket holding a metal rod.
h.	Heavy Duty Plastic Caps: Protects the rod ends.
9.	Housing: Extruded aluminum.
a.	Finish: Powder coated. Color: White.
b.	Housing Bottom: Self-trimming. Built-in flange around housing bottom.
1)	Hinged Aluminum Door: Opens and closes with the lowering and raising of projection screen.
2)	Balance of Housing Bottom: A second hinged aluminum access door for manual access.
3)	Hinges: Mounted in a concealed manner.
c.	For use in environmental air space in accordance with section 300-22 of the National Electric Code, and sections 2-128, 12-010 (3) and 12-100 of the Canadian Electrical Code, part 1, CSA C22.1.
d.	Overall Housing Length Dimension: +/- 1/4 inches (6 mm).
10.	Integrated Low Voltage Control Unit: Three position control switch and cover plate.
11.	Junction Box: Internally Integrated into the housing. Housing may be installed and wired to the building's electrical system during construction.
12.	Viewing Surfaces: GREENGUARD and GREENGUARD Gold Certified.
13.	Viewing Surface: Matte White:
a.	Horizontal seam required when both dimensions exceed 10 ft (305 cm).
14.	Viewing Surface: High Contrast Matte White:
a.	Available in sizes where both dimensions do not exceed 8 ft (243.8 cm).
15.	Total Surface Height Including Picture Area: 13 ft (396 cm) maximum.
a.	Black Drop at Top of Screen: 2 inch (5.1 cm).
b.	Black Drop at Top of Screen: ____ inch.
c.	White Drop at Top of Screen: ____ inch.
d.	Black Drop at Bottom of Screen: ____ inch.
e.	White Drop at Bottom of Screen: ____ inch.
16.	Accessories:
a.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger)
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
b.	Key Locking Cover Plate for LVC Switch.
G.	Basis of Design: Advantage Series as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	90 x 160 inches (229 x 406 cm). Diagonal: 184 inches (467 cm).
h.	99 x 176 inches (251 x 447 cm). Diagonal: 202 inches (513 cm).
i.	106 x 188 inches (269 x 478 cm). Diagonal: 216 inches (549 cm).
j.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches (480 cm).
i.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
j.	117.5 x 188 inches (298 x 478 cm). Diagonal: 222 inches (564 cm).
k.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	43 x 57 inches (109 x 145 cm). Diagonal: 72 inches (183 cm).
b.	50 x 67 inches (127 x 170 cm). Diagonal: 84 inches (213 cm).
c.	60 x 80 inches (152 x 203 cm). Diagonal: 100 inches (254 cm).
d.	69 x 92 inches (175 x 234 cm). Diagonal: 120 inches (305 cm).
e.	87 x 116 inches (221 x 295 cm). Diagonal: 150 inches (381 cm).
f.	108 x 144 inches (274 x 366 cm). Diagonal: 180 inches (457 cm).
g.	120 x 160 inches (305 x 406 cm). Diagonal: 200 inches (508 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Square. Viewing area (HxW).
a.	60 x 60 inches (152 x 152 cm).
b.	70 x 70 inches (178 x 178 cm).
c.	84 x 84 inches (213 x 213 cm).
d.	96 x 96 inches (244 x 244 cm).
e.	108 x 108 inches (274 x 274 cm).
f.	120 x 120 inches (305 x 305 cm).
g.	144 x 144 inches (366 x 366 cm).
h.	__ x __ inches (__ x __ cm).
5.	Certifications and Compliances: Listed by Underwriters' Laboratories.
6.	Screen Motor: 
a.	Mounting: In the roller. 
b.	Electric: 120 volt (60 Hz) 2.4 amps max. 
c.	Electric: 220 Volt (50 Hz) 2.4 amps max. 
d.	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor and an electric brake to prevent coasting. 
7.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions. 
8.	Electrical Junction Box: Externally integrated into housing. Allows housing installation and wiring to facility's electrical system during construction. 
a.	A quick connector mounted in the housing for plug-in connection to the motorized fabric and roller assembly.
9.	Electrical Junction Box: External. Extends 2-1/8 inches (5.4 cm) past housing length on left end of case, and 1-1/8 inch (2.9 cm) past ceiling flange. Standard configuration. 
10.	Electrical Junction Box: Internal. Will add 3-1/2 inches (8.9 cm) to overall case length and must be specified at time of order. Recommended for drywall installations. 
11.	Electrical Junction Box: External on top of case. Will add 3-1/2 inches (8.9 cm) to overall case length and 1-7/8 inches (4.8 cm) to height at left end of case. Must be specified at time of order. 
12.	Motorized Fabric and Roller Assembly: Installed in the housing at the factory or later at the job site. Roller Material: Rigid steel. 
13.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking borders.
f.	Borders: None.
g.	Fabric Bottom: Formed into a pocket holding a metal rod.
h.	Heavy Duty Plastic Caps: Protects the rod ends.
14.	Housing, Top, Front and Back: Extruded aluminum. 
a.	Finish: Powder coated. Color: White. 
b.	End Caps: Heavy gauge steel. 
1)	Finish: Powder coated. Color: White. 
c.	Housing Bottom: To have a removable access door. 
1)	Access Door: Extruded aluminum. 
a)	Finish: Powder coated. Color: White. 
2)	Self-trimming. Built-in flange around housing bottom. 
d.	For use in environmental air space in accordance with section 300-22 (c) of the National Electric Code, and sections 2-128, 12-010 (3) and 12-100 of the Canadian Electrical Code, part 1, CSA C22.1. 
e.	Overall Housing Length Dimensions: +/- 1/4 inches (6 mm). 
15.	Integrated Low Voltage Control Unit: 
a.	Three position control switch and cover plate. 
16.	Viewing Surfaces: 
a.	GREENGUARD and GREENGUARD Gold Certified.
17.	Viewing Surface: Matte White:
a.	Horizontal seam required when both dimensions exceed 10 ft (305 cm).
18.	Viewing Surface: High Contrast Matte White:
a.	Available in sizes where both dimensions do not exceed 8 ft (243.8 cm).
19.	Total Surface Height Including Picture Area: 13 ft (396 cm) maximum.
a.	Black Drop at Top of Screen: 2 inch (5.1 cm).
b.	Black Drop at Top of Screen: ____ inch.
c.	White Drop at Top of Screen: ____ inch.
d.	Black Drop at Bottom of Screen: ____ inch.
e.	White Drop at Bottom of Screen: ____ inch.
20.	Accessories:
a.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger).
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
b.	Key Locking Cover Plate for LVC Switch.
H.	Basis of Design: Advantage with Sightline as manufactured by Da-Lite.
1.	Format: HDTV (16:9)
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	90 x 160 inches (229 x 406 cm). Diagonal: 184 inches (467 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10)
a.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches (480 cm).
i.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Ultrawide (21:9). Viewing area (HxW)
a.	40.5 x 96 inches (103 x 244 cm). Diagonal: 104 inches (264 cm).
b.	50.75 x 120 inches (129 x 305 cm). Diagonal: 130 inches (330 cm).
c.	60.75 x 144 inches (154 x 366 cm). Diagonal: 156 inches (396 cm).
d.	64.75 x 153.75 inches (164 x 391 cm). Diagonal: 167 inches (424 cm).
4.	Certifications and Compliances: Listed by Underwriters' Laboratories.
5.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
1)	Quick Connect Male Plug-In Connector: On the motor.
6.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
7.	Motorized Fabric and Roller Assembly: Factory installed in the housing or installed later at the job site.
a.	Roller Material: Rigid metal.
b.	Aircraft Cabling: 1 mm, 7/19 galvanized. Length: 70 inch (178 cm) long maximum.
c.	Adjustable Cable Drop:
1)	Overall Drop Length: 70 inches (178 cm) maximum.
2)	Factory Set Drop: 24 inches (61 cm).
3)	Field Adjustment: Set to desired drop distance at installation.
4)	Case Lengths up to 120 inches (305 cm): Screens drop from 3 cables.
5)	Case Lengths over 120 inches (305 cm): Screens drop from 4 cables.
d.	Roller Mounting Brackets: Adjustable. Allows centering or offsetting of the screen within the case.
8.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking borders.
f.	Borders: None.
g.	Fabric Bottom: Formed into a pocket holding a metal rod.
h.	Heavy Duty Plastic Caps: Protects the rod ends.
9.	Housing Top, Front and Back: Extruded aluminum.
a.	Finish: Powder coated. Color: White.
b.	End Caps: Heavy gauge steel.
1)	Finish: Powder coated. Color: White.
c.	Housing Bottom: To have a removable access door.
1)	Door: Extruded aluminum.
a)	Finish: Powder coated. Color: White.
2)	Self-trimming, with built-in flange around housing bottom 
d.	Quick Connector: Mounted in housing for plug-in connection to the motorized fabric and roller assembly.
1)	For use in environmental air space in accordance with section 300-22 (c) of the National Electric Code, and sections 2-128, 12-010 (3) and 12-100 of the Canadian Electrical Code, part 1, CSA C22.1.
e.	Overall Housing Length Dimensions: +/- 1/4 inches (6 mm).
10.	Integrated Low Voltage Control Unit: 
a.	Three position control switch and cover plate.
11.	Electrical Junction Box: Externally integrated into the housing. Housing may be installed and wired to the building's electrical system during construction.
a.	Extends 2-1/8 inches (54 mm) past housing length on housing left end.
b.	Extends 1-1/8 inch (29 mm) past ceiling flange.
12.	Electrical Junction Box: Internally Integrated into the housing. Housing may be installed and wired to the building's electrical system during construction.
a.	Will add 3-1/2 inches (8.9 cm) to overall housing length.
13.	Electrical Junction Box: On top of Housing.
a.	Will add 3-1/2 inches (8.9 cm) to overall housing length.
b.	Will and 1-7/8 inches (4.8 cm) to height at left end of housing.
14.	Viewing Surfaces:
a.	Viewing Surface: Matte White:
1)	Seamless in all standard sizes.
b.	Viewing Surface: High Contrast Matte White:
1)	Available in sizes where both dimensions do not exceed 8 ft (243.8 cm).
15.	Accessories:
a.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger).
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
b.	Key Locking Cover Plate for LVC Switch.
I.	Basis of Design: Advantage, Over 14 ft (427 cm) Wide with Closure Door as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	106 x 188 inches (269 x 478 cm). Diagonal: 216 inches (549 cm).
b.	119 x 212 inches (302 x 538 cm). Diagonal: 243 inches (617 cm).
c.	133 x 236 inches (338 x 599 cm). Diagonal: 271 inches (688 cm).
d.	146 x 260 inches (371 x 660 cm). Diagonal: 298 inches (757 cm).
e.	160 x 284 inches (406 x 721 cm). Diagonal: 326 inches (828 cm).
f.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
b.	117.5 x 188 inches (283 x 478 cm). Diagonal: 222 inches (564 cm).
c.	132.5 x 212 inches (337 x 538 cm). Diagonal: 250 inches (635 cm).
d.	147.5 x 236 inches (375 x 599 cm). Diagonal: 278 inches (706 cm).
e.	162.5 x 260 inches (413 x 660 cm). Diagonal: 307 inches (780 cm).
f.	177.5 x 284 inches (451 x 721 cm). Diagonal: 335 inches (851 cm).
g.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	123 x 164 inches (312 x 417 cm). Diagonal: 210 inches (533 cm).
b.	141 x 188 inches (358 x 478 cm). Diagonal: 240 inches (610 cm).
c.	159 x 212 inches (404 x 538 cm). Diagonal: 265 inches (673 cm).
d.	177 x 236 inches (450 x 599cm). Diagonal: 295 inches (749 cm).
e.	213 x 284 inches (541 x 721 cm). Diagonal: 355 inches (902 cm).
f.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Square. Viewing area (HxW).
a.	168 x 168 inches (427 x 427 cm).
b.	192 x 192 inches (488 x 488 cm).
c.	216 x 216 inches (549 x 549 cm).
d.	240 x 240 inches (610 x 610 cm).
e.	264 x 264 inches (671 x 671cm).
f.	__ x __ inches (__ x __ cm).
5.	Certifications and Compliances: Listed by Underwriters' Laboratories.
6.	Two Motors: Door motor and screen motor.
7.	Door Motor:
a.	Mounting: In roller; 1.6 inches (4.1 cm) diameter aluminum.
b.	Electric: 120 volt (60 Hz) 1.2 amps max.
c.	Electric: 220 Volt (50 Hz) 1.2 amps max.
d.	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and electric brake to prevent coasting.
e.	Limit Switches: Preset and adjustable. Stops fabric door in the "down" position. As door lifts to the closed position, a microswitch cuts off the electrical current to the door motor.
8.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
1)	Quick Connect Male Plug-In Connector: On the motor.
e.	Limit Switches: Pre-set and adjustable. Stop picture surface in the "up" and "down" positions.
9.	Motorized Fabric and Roller Assembly: Factory installed in the housing or installed later at the job site.
a.	Roller Material: Rigid metal.
10.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking borders.
f.	Borders: None.
g.	Bottom of Fabric: Formed into a pocket holding a metal rod.
h.	Heavy Duty Plastic Caps: Protects the rod ends.
11.	Housing: Extruded aluminum.
a.	Finish: Powder coated. Color: White.
b.	Housing Bottom: Self-trimming. Built-in flange around housing bottom.
1)	Hinged Aluminum Door: Opens and closes with the lowering and raising of projection screen.
2)	Balance of Housing Bottom: A second hinged aluminum access door for manual access.
3)	Hinges: Mounted in a concealed manner.
c.	Quick Connector: Mounted in housing for easy plug-in connection to the motorized fabric and roller assembly.
d.	For use in environmental air space in accordance with section 300-22 (c) of the National Electric Code, and sections 2-128, 12-010 (3) and 12-100 of the Canadian Electrical Code, part 1, CSA C22.1.
12.	Electrical Junction Box: Internally Integrated into the housing.
a.	Housing may be installed and wired to the building's electrical system during construction.
13.	Overall Housing Length Dimension: +/- 1/4 inches (6 mm).
14.	Integrated Low Voltage Control Unit: 
a.	Three position control switch and cover plate.
15.	Viewing Surface: Matte White: 
a.	Horizontal seam required when both dimensions exceed 16 ft (488 cm).
16.	Total Surface Height Including Picture Area: 22 ft (671 cm) maximum.
a.	Screen Widths: Under 24 ft (731.5 cm) wide.
17.	Total Surface Height Including Picture Area: 18 ft (548.6 cm) maximum.
a.	Screen Widths: 24 ft (731.5 cm) wide.
b.	Black Drop at Top of Screen: 2 inch (5.1 cm).
c.	Black Drop at Top of Screen: __ inches (__ cm).
d.	White Drop at Top of Screen: __ inches (__ cm).
e.	Black Drop at Bottom of Screen: __ inches (__ cm).
f.	White Drop at Bottom of Screen: __ inches (__ cm).
18.	Accessories:
a.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger).
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
b.	Key Locking Cover Plate for LVC Switch.
J.	Basis of Design: Advantage, Over 16 ft (488 cm) Wide as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	119 x 212 inches (302 x 538 cm). Diagonal: 243 inches (617 cm).
b.	133 x 236 inches (338 x 599 cm). Diagonal: 271 inches (688 cm).
c.	146 x 260 inches (371 x 660 cm). Diagonal: 298 inches (757 cm).
d.	160 x 284 inches (406 x 721 cm). Diagonal: 326 inches (828 cm).
e.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	132.5 x 212 inches (337 x 538 cm). Diagonal: 250 inches (635 cm).
b.	147.5 x 236 inches (375 x 599 cm). Diagonal: 278 inches (706 cm).
c.	162.5 x 260 inches (413 x 660 cm). Diagonal: 307 inches (780 cm).
d.	177.5 x 284 inches (451 x 721 cm). Diagonal: 335 inches (851 cm).
e.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	159 x 212 inches (404 x 538 cm). Diagonal: 265 inches (673 cm).
b.	177 x 236 inches (450 x 599 cm). Diagonal: 295 inches (749 cm).
c.	213 x 284 inches (541 x 721 cm). Diagonal: 355 inches (902 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Square. Viewing area (HxW).
a.	216 x 216 inches (549 x 549 cm).
b.	240 x 240 inches (610 x 610 cm).
c.	264 x 264 inches (671 x 671cm).
d.	__ x __ inches (__ x __ cm).
5.	Certifications and Compliances: Listed by Underwriters' Laboratories.
6.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
1)	Quick Connect Male Plug-In Connector: On the motor.
7.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
8.	Motorized Fabric and Roller Assembly: Factory installed in the housing or installed later at the job site.
a.	Roller Material: Rigid metal.
b.	Roller Mounting Brackets: Adjustable to allow centering or offsetting of the screen within the housing.
9.	Screen Fabric:
a.	Mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Flame retardant.
e.	Borders: Black masking borders.
f.	Borders: None.
g.	Bottom of Fabric: Formed into a pocket holding a metal rod.
h.	Heavy Duty Plastic Caps: Protects the rod ends.
10.	Housing: Extruded aluminum.
a.	Finish: Powder coated. Color: White.
b.	End Caps: Heavy gauge steel.
1)	Finish: Powder coated. Color: White.
c.	Housing Bottom: To have a removable access door.
1)	Door: Extruded aluminum.
a)	Finish: Powder coated. Color: White.
2)	Self-trimming, with built-in flange around housing bottom. 
d.	Quick Connector: Mounted in housing for easy plug-in connection to the motorized fabric and roller assembly.
e.	Electrical Junction Box: Internally Integrated into the housing. Housing may be installed and wired to the building's electrical system during construction.
f.	For use in environmental air space in accordance with section 300-22 (c) of the National Electric Code, and sections 2-128, 12-010 (3) and 12-100 of the Canadian Electrical Code, part 1, CSA C22.1.
g.	Overall Housing Length Dimension: +/- 1/4 inches (6 mm).
11.	Integrated Low Voltage Control Unit: 
a.	Three position control switch and cover plate.
12.	Viewing Surface: Matte White: 
a.	Horizontal seam required when both dimensions exceed 16 ft (488 cm).
b.	Black Drop at Top of Screen: ___ inch (___ cm).
c.	Black Drop at Top of Screen: ___ inch (___ cm).
d.	White Drop at Top of Screen: ___ inch (___ cm).
e.	Black Drop at Bottom of Screen: ___ inch (___ cm)
f.	White Drop at Bottom of Screen: ___ inch (___ cm).
13.	Accessories:
a.	Radio Frequency (BLE) Remote.
b.	Infrared Remote.
c.	PoE Injector.
d.	Key Locking Cover Plate for LVC Switch.
K.	Basis of Design: Tensioned Contour Electrol as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	90 x 160 inches (229 x 406 cm). Diagonal: 184 inches (467 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches (480 cm).
i.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Ultrawide (21:9). Viewing Area (HxW).
a.	40.5 x 96 inches (103 x 244 cm). Diagonal: 104 inches (264 cm).
b.	50.75 x 120 inches (129 x 305 cm). Diagonal: 130 inches (330 cm).
c.	60.75 x 144 inches (154 x 366 cm). Diagonal: 156 inches (396 cm).
d.	67.5 x 160 inches (171 x 406 cm). Diagonal: 174 inches (442 cm).
e.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	43 x 57 inches (109 x 145 cm). Diagonal: 72 inches (183 cm).
b.	50 x 67 inches (127 x 170 cm). Diagonal: 84 inches (213 cm).
c.	60 x 80 inches (152 x 203 cm). Diagonal: 100 inches (254 cm).
d.	69 x 92 inches (175 x 234 cm). Diagonal: 120 inches (305 cm).
e.	87 x 116 inches (221 x 295 cm). Diagonal: 150 inches (381 cm).
f.	108 x 144 inches (274 x 366 cm). Diagonal: 180 inches (457 cm).
g.	120 x 160 inches (305 x 406 cm). Diagonal: 200 inches (508 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
5.	Certifications and Compliances: Listed by Underwriters' Laboratories.
6.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor and an electric brake to prevent coasting.
7.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
8.	Junction Box: Internally integrated into housing. Allows housing installation and wiring to facility's electrical system during construction.
a.	A quick connector mounted in the housing for plug-in connection to the motorized fabric and roller assembly.
9.	Roller Material: Metal.
10.	Screen Housing: Two piece extruded aluminum design.
a.	Finish: Powder coated.
1)	Color: White, lightly textured.
2)	Color: Black.
b.	Overall Housing Length Dimensions: +/- 1/4 inches (6 mm).
11.	Integrated Low Voltage Control Unit: 
a.	Three position control switch and cover plate.
12.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking borders.
f.	Fabric Sides: Radio frequency welded tab guide cable system on each vertical side to maintain even lateral tension and hold surface flat. 
g.	Fabric Bottom: Fabric to be inserted into a custom aluminum slat bar with added weight to provide vertical tension on the screen surface.
1)	Slat Ends: Protected by heavy duty plastic caps enclosing a preset adjustable mechanism for screen tensioning.
h.	Black Drop at Top of Screen: 12 inch (30.5 cm).
i.	Black Drop at Top of Screen: 2 inch (5.1 cm).
j.	Seamless in the image area.
13.	Accessories:
a.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger) 
1)	Radio Frequency (BLE) Remote. 
2)	Infrared Remote. 
3)	PoE Injector. 
b.	Key Locking Cover Plate for LVC Switch. 
L.	Basis of Design: Tensioned Cosmopolitan as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 60 inches (127 x 103 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	43 x 57 inches (109 x 145 cm). Diagonal: 72 inches (183 cm).
b.	50 x 67 inches (127 x 170 cm). Diagonal: 84 inches (213 cm).
c.	60 x 80 inches (152 x 203 cm). Diagonal: 100 inches (254 cm).
d.	69 x 92 inches (175 x 234 cm). Diagonal: 120 inches (305 cm).
e.	87 x 116 inches (221 x 295 cm). Diagonal: 150 inches (381 cm).
f.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Certifications and Compliances: Listed by Underwriters' Laboratories.
5.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
e.	Integrated Low Voltage Control (LVC).
f.	Silent motor. 
1)	Available in screen sizes up to 10 x 10 ft (305 x 305 cm).
g.	Silent motor with Integrated LVC. 
1)	Available in screen sizes up to 10 x 10 ft (305 x 305 cm).
6.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
7.	Motorized Fabric and Roller Assembly:
a.	Roller Material: Rigid metal.
8.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking.
f.	Borders: None.
g.	Fabric Sides: Radio frequency welded tab guide cable system on each vertical side to maintain even lateral tension and hold surface flat. 
h.	Fabric Bottom: Formed into a pocket holding a metal rod.
i.	Fabric Bottom: Fabric to be inserted into a custom aluminum slat bar with added weight to provide vertical tension on the screen surface.
1)	Slat Ends: Protected by heavy duty plastic caps enclosing a preset adjustable mechanism for screen tensioning.
9.	Housing: 21-gauge steel. Sectional Shape: Hexagonal with flat back.
a.	Finish: Powder coated.
1)	Color: White.
2)	Color: Black.
b.	End Caps: Heavy duty, allowing no exposed roller pins.
1)	Caps double as sturdy brackets for wall or ceiling mounting.
c.	Overall Housing Length Dimensions: +/- 1/4 inch (6 mm).
10.	Control Switch: 
a.	Three position with cover plate.
11.	Viewing Surface: Da-Mat. 
12.	Viewing Surface: Da-Tex (Rear). 
13.	Black Drop at Top of Screen: 12 inches (30.5 cm).
14.	Black Drop at Top of Screen: ___ inches.
15.	Accessories:
a.	External Low Voltage Control (LVC).
b.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger). Requires Integrated or External LVC.
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
c.	Key Locking Cover Plate for 120V or LVC Switch.
d.	Key Operated Switch for 120V only. Cannot be used with LVC.
e.	Floating Mounting Brackets. Recommended for drywall installations.
1)	Color: Black.
2)	Color: White.
f.	No. 6 Wall Bracket: 6 inch (15.2 cm) extension. Non-adjustable.
1)	Capacity: 140 lbs (63.5 kg) maximum per pair.
2)	Color: Black.
3)	Color: White.
g.	Ceiling Trim Kit: Built-in LVC recommended.
M.	Basis of Design: Tensioned Cosmopolitan, Over 12 ft (365.8 cm) as manufactured by Da-Lite.
1.	Format: HDTV (16:9).
a.	92 x 164 inches (234 x 417 cm). Diagonal: 188 inches (478 cm).
b.	108 x 192 inches (274 x 488 cm). Diagonal: 220 inches (559 cm).
c.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10).
a.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches (480 cm).
b.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
c.	120 x 192 inches (305 x 488 cm). Diagonal: 226 inches (574 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3).
a.	108 x 144 inches (274 x 366 cm). Diagonal: 180 inches (457 cm).
b.	120 x 160 inches (305 x 406 cm). Diagonal: 200 inches (508 cm).
c.	126 x 168 inches (320 x 427 cm). Diagonal: 210 inches (533 cm).
d.	132 x 176 inches (335 x 447 cm). Diagonal: 220 inches (559 cm).
e.	144 x 192 inches (366 x 488 cm). Diagonal: 240 inches (610 cm).
f.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Certifications and Compliances: Listed by Underwriters' Laboratories.
5.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
e.	Integrated Low Voltage Control (LVC); Built-in.
6.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
7.	Roller Material: Aluminum.
8.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking.
f.	Fabric Sides: Radio frequency welded tab guide cable system on each vertical side to maintain even lateral tension and hold surface flat. 
g.	Fabric Bottom: Fabric to be inserted into a custom aluminum slat bar with added weight to provide vertical tension on the screen surface.
1)	Slat Ends: Protected by heavy duty plastic caps enclosing a preset adjustable mechanism for screen tensioning.
9.	Housing: Two-piece extruded aluminum construction.
a.	Finish: Powder coated. Color: White.
b.	Finish: Powder coated. Color: Black.
c.	Overall Housing Length Dimensions: +/- 1/4 inch (6 mm).
10.	Control Switch: 
a.	Three position with cover plate.
11.	Viewing Surfaces: GREENGUARD and GREENGUARD Gold Certified.
a.	Viewing Surface: Parallax Stratos 1.0. 
b.	Viewing Surface: HD Progressive 1.0. 
c.	Viewing Surface: HD Progressive 1.1 Contrast.
d.	Viewing Surface: HD Progressive 1.3. 
e.	Viewing Surface: Da-Mat. Seamless.
f.	Viewing Surface: Da-Tex (Rear). 
g.	Viewing Surface: HD Progressive ReView 0.9 (Rear). 
12.	Black Drop at Screen Top: 12 inches (30.5 cm).
13.	Black Drop at Screen Top: ___ inches 
14.	Accessories:
a.	External Low Voltage Control (LVC).
b.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger). Requires Integrated or External LVC.
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
c.	Key Locking Cover Plate for 120V or LVC Switch.
d.	Key Operated Switch for 120V only. Cannot be used with LVC.
N.	Basis of Design: Tensioned Professional Electrol as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	92 x 164 inches (234 x 417 cm). Diagonal: 188 inches (478 cm).
b.	108 x 192 inches (274 x 488 cm). Diagonal: 220 inches (559 cm).
c.	121 x 216 inches (307 x 549 cm). Diagonal: 247 inches (627 cm).
d.	135 x 240 inches (343 x 610 cm). Diagonal: 275 inches (699 cm).
e.	146 x 260 inches (371 x 660 cm). Diagonal: 298 inches (757 cm).
f.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
b.	120 x 192 inches (305 x 488 cm). Diagonal: 226 inches (574 cm).
c.	135 x 216 inches (342 x 549 cm). Diagonal: 255 inches (648 cm).
d.	150 x 240 inches (381 x 610 cm). Diagonal: 283 inches (719 cm).
e.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	108 x 144 inches (274 x 366 cm). Diagonal: 180 inches (457 cm).
b.	120 x 160 inches (305 x 406 cm). Diagonal: 200 inches (508 cm).
c.	126 x 168 inches (320 x 427 cm). Diagonal: 210 inches (533 cm).
d.	132 x 176 inches (335 x 447 cm). Diagonal: 220 inches (559 cm).
e.	144 x 192 inches (366 x 488 cm). Diagonal: 240 inches (610 cm).
f.	162 x 216 inches (411 x 549 cm). Diagonal: 270 inches (686 cm).
g.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Certifications and Compliances: Listed by Underwriters' Laboratories.
5.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
1)	Secured in the housing with steel motor mount bracket.
6.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
7.	Roller Material: 4-1/2 inch (11.4 cm) diameter aluminum.
a.	Roller Mounting Heavy Duty Bracket: Equipped with self-aligning bearing.
8.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Fabric Sides: Radio frequency welded tab guide cable system on each vertical side to maintain even lateral tension and hold surface flat. 
f.	Fabric Bottom: To be inserted into a custom aluminum slat bar with added weight to provide vertical tension on the screen surface.
g.	Heavy Duty Plastic Caps: Protects the slat ends enclosing a preset adjustable mechanism for screen tensioning.
h.	Black Drop at the Top: 12 inches (30.5 cm) for all screen sizes unless specified otherwise.
i.	Black Drop at the Top: 2 inches (5.1 cm).
1)	Screen Size (HxW): 150 x 240 inches (381 x 610 cm). Diagonal: 283 inches (719 cm).
2)	Screen Size (HxW): 162 x 216 inches (411 x 549 cm). Diagonal: 270 inches (686 cm).
9.	Housing:
a.	Material: Wood, with double top for extra rigidity and strength.
b.	Finish: Black primer coat, ready to accept final finish by others.
c.	Heavy Duty Metal Brackets: For mounting screen to a ceiling or wall.
d.	Overall Housing Length Dimensions: +/- 1/4 inches (6 mm).
10.	Control Switch: Three position with cover plate.
11.	Viewing Surfaces: GREENGUARD and GREENGUARD Gold Certified.
a.	Viewing Surface: Parallax Stratos 1.0.
b.	Viewing Surface: HD Progressive 1.0. 
c.	Viewing Surface: HD Progressive 1.1 
d.	Viewing Surface: HD Progressive 1.3. 
e.	Viewing Surface: Da-Mat.
f.	Viewing Surface: Da-Tex (Rear). 
g.	Viewing Surface: HD Progressive ReView 0.9 (Rear). 
12.	Accessories:
a.	External Low Voltage Control (LVC).
b.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger). Requires Integrated or External LVC.
1)	Radio Frequency (BLE) Remote
2)	Infrared Remote
3)	PoE Injector
c.	Key Locking Cover Plate for 120V or LVC Switch
d.	Key Operated Switch for 120V only. Cannot be used with LVC.
e.	Key Operated Switch for 120 V only; cannot be used with LVC.
O.	Basis of Design: Contour Electrol as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	90 x 160 inches (229 x 406 cm). Diagonal: 184 inches (467 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 60 inches (127 x 103 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches (480 cm).
i.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	43 x 57 inches (109 x 145 cm). Diagonal: 72 inches (183 cm).
b.	50 x 67 inches (127 x 170 cm). Diagonal: 84 inches (213 cm).
c.	60 x 80 inches (152 x 203 cm). Diagonal: 100 inches (254 cm).
d.	69 x 92 inches (175 x 234 cm). Diagonal: 120 inches (305 cm).
e.	87 x 116 inches (221 x 295 cm). Diagonal: 150 inches (381 cm).
f.	105 x 140 inches (267 x 356 cm). Diagonal: 180 inches (457 cm).
g.	120 x 160 inches (305 x 406 cm). Diagonal: 200 inches (508 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Square. Viewing area (HxW).
a.	60 x 60 inches (152 x 152 cm).
b.	70 x 70 inches (178 x 178 cm).
c.	84 x 84 inches (213 x 213 cm).
d.	96 x 96 inches (244 x 244 cm).
e.	108 x 108 inches (274 x 274 cm).
f.	120 x 120 inches (305 x 305 cm).
g.	144 x 144 inches (366 x 366 cm).
h.	__ x __ inches (__ x __ cm).
5.	Certifications and Compliances: Listed by Underwriters' Laboratories.
6.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
7.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
8.	Roller Material: Rigid metal.
9.	Screen Housing: Two piece extruded aluminum design.
a.	Finish: Powder coated.
1)	Color: White, lightly textured.
2)	Color: Black.
10.	Control Switch: Three position with cover plate.
11.	Electrical Junction box: Integrated into the housing. Housing may be installed and wired to the building's electrical system during construction.
12.	Quick Connector: Mounted in housing for plug-in connection to the motorized fabric and roller assembly.
13.	Overall Housing Length Dimensions: +/- 1/4 inch (6 mm).
14.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking.
f.	Borders: None.
g.	Bottom of Fabric: Formed into a pocket holding a metal rod.
h.	Heavy Duty Plastic Caps: Protects the rod ends.
15.	Viewing Surfaces: GREENGUARD and GREENGUARD Gold Certified.
a.	Viewing Surface: Matte White:
1)	Horizontal seam required when both dimensions exceed 10 ft (305 cm).
b.	Viewing Surface: High Contrast Matte White:
1)	Available in sizes where both dimensions do not exceed 8 ft (243.8 cm).
16.	Total Surface Height Including Picture Area: 13 ft (396 cm) maximum.
a.	Black Drop at Top of Screen: 2 inch (5.1 cm).
b.	Black Drop at Top of Screen: ___inch (___ cm).
c.	White Drop at Top of Screen: ___inch (___ cm).
d.	Black Drop at Bottom of Screen: ___inch (___ cm).
e.	White Drop at Bottom of Screen: ___inch (___ cm).
17.	Accessories:
a.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger)
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
b.	Key Locking Cover Plate for LVC Switch.
P.	Basis of Design: Cosmopolitan Series as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 80 inches (127 x 103 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	43 x 57 inches (109 x 145 cm). Diagonal: 72 inches (183 cm).
b.	50 x 67 inches (127 x 170 cm). Diagonal: 84 inches (213 cm).
c.	60 x 80 inches (152 x 203 cm). Diagonal: 100 inches (254 cm).
d.	69 x 92 inches (175 x 234 cm). Diagonal: 120 inches (305 cm).
e.	87 x 116 inches (221 x 295 cm). Diagonal: 150 inches (381 cm).
f.	105 x 140 inches (267 x 356 cm). Diagonal: 180 inches (457 cm).
g.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Square. Viewing area (HxW).
a.	60 x 60 inches (152 x 152 cm).
b.	70 x 70 inches (178 x 178 cm).
c.	84 x 84 inches (213 x 213 cm).
d.	96 x 96 inches (244 x 244 cm).
e.	108 x 108 inches (274 x 274 cm).
f.	120 x 120 inches (305 x 305 cm).
g.	__ x __ inches (__ x __ cm).
5.	Certifications and Compliances: Listed by Underwriters' Laboratories.
6.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor and an electric brake to prevent coasting.
e.	Integrated Low Voltage Control (LVC).
f.	Silent motor. Available in screen sizes up to 10 x 10 ft (305 x 305 cm).
g.	Silent motor with Integrated LVC. Available in screen sizes up to 10 x 10 ft (305 x 305 cm).
7.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down"positions.
8.	Fabric Roller Material: Rigid metal.
9.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking.
f.	Borders: None.
g.	Bottom of Fabric: Formed into a pocket holding a metal rod.
10.	Housing: 21 gauge steel. Sectional Shape: Hexagonal with flat back.
a.	Finish: Powder coated.
1)	Color: White.
2)	Color: Black.
b.	End Caps: Heavy duty, allowing no exposed roller pins.
1)	Caps double as sturdy brackets for wall or ceiling mounting.
c.	Overall Housing Length Dimensions: +/- 1/4 inch (6 mm).
11.	Control Switch: Three position with cover plate.
12.	Viewing Surface: Matte White.
a.	Horizontal Seam: Required when both dimensions exceed 10 ft (305 cm).
13.	Viewing Surface: High Contrast Matte White.
a.	Available in sizes where both dimensions do not exceed 8 ft (243.8 cm).
14.	Options:
a.	Extra Drop: To lower picture area more than normal.
1)	Total Drop at Top: ___ inches (___ cm).
a)	Color: Black.
b)	Color: White.
2)	Total Drop at Bottom: ___ inches (___ cm).
a)	Color: Black.
b)	Color: White.
3)	Total Surface Height Including Picture Area: 13 ft (396 cm) maximum.
15.	Accessories:
a.	External Low Voltage Control (LVC).
b.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger). Requires Integrated or External LVC.
1)	Radio Frequency (BLE) Remote
2)	Infrared Remote
3)	PoE Injector
c.	Key Locking Cover Plate for 120V or LVC Switch
d.	Key Operated Switch for 120V only. Cannot be used with LVC.
e.	Floating Mounting Brackets. Recommended for drywall installations
1)	Color: Black.
2)	Color: White.
f.	No. 6 Wall Bracket: 6 inch (15.2 cm) extension. Non-adjustable.
1)	Capacity: 140 lbs (63.5 kg) maximum per pair.
2)	Color: Black.
3)	Color: White.
g.	Ceiling Trim Kit: Built-in LVC recommended.
Q.	Basis of Design: Cosmopolitan; over 12 ft (365.8 cm) Wide as manufactured by Da-Lite.
1.	Format: HDTV (16:9) . Viewing area (HxW).
a.	92 x 164 inches (234 x 417 cm). Diagonal: 188 inches (478 cm).
b.	106 x 188 inches (269 x 478 cm). Diagonal: 216 inches (549 cm).
c.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10) . Viewing area (HxW).
a.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches 480 cm).
b.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
c.	117.5 x 188 inches (298 x 478 cm). Diagonal: 222 inches (564 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3) . Viewing area (HxW).
a.	120 x 160 inches (305 x 406 cm). Diagonal: 200 inches (508 cm).
b.	123 x 164 inches (312 x 417 cm). Diagonal: 210 inches (533 cm).
c.	141 x 188 inches (358 x 478 cm). Diagonal: 240 inches (610 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Square. Viewing area (HxW).
a.	144 x 144 inches (366 x 366 cm). Diagonal: 153.5 inches (390 cm).
b.	168 x 168 inches (427 x 427 cm). Diagonal: 177.5 inches (451 cm).
c.	192 x 192 inches (488 x 488 cm). Diagonal: 201.5 inches (512 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
5.	Certifications and Compliances: Listed by Underwriters' Laboratories.
6.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor and an electric brake to prevent coasting.
7.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
8.	Fabric Roller Material: Aluminum.
9.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking.
f.	Borders: None.
g.	Screen Material: Matte White.
1)	Seamless in all standard sizes.
h.	Screen Material: High Contrast Matte White.
1)	Available in sizes where both dimensions do not exceed 8 ft (243.8 cm).
i.	Bottom of Fabric: Formed into a pocket holding a metal rod.
10.	Housing: A two-piece design made of extruded aluminum.
a.	Finish: Powder coated.
1)	Color: White.
2)	Color: Black.
b.	End Caps: Plastic, with integrated junction box.
c.	Overall Housing Length Dimensions: +/- 1/4 inch (6 mm).
11.	Control Switch: Three position with cover plate.
12.	Viewing Surface: Matte White.
a.	Seamless in all standard sizes.
13.	Viewing Surface: High Contrast Matte White.
a.	Available in sizes where both dimensions do not exceed 8 ft (243.8 cm).
14.	Options:
a.	Extra Drop: Available to lower picture area more than normal.
1)	Total Drop at Top: ___ inches (___ cm).
a)	Color: Black.
b)	Color: White.
2)	Total Drop at Bottom: ___ inches (___ cm).
a)	Color: Black.
b)	Color: White.
3)	Total Surface Height Including Picture Area: 16 ft (488 cm) maximum.
15.	Accessories:
a.	External Low Voltage Control (LVC).
b.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger). Requires Integrated or External LVC.
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
c.	Key Locking Cover Plate for 120V or LVC Switch.
d.	Key Operated Switch for 120V only. Cannot be used with LVC.
e.	Floating Mounting Brackets. Recommended for drywall installations.
1)	Color: Black.
2)	Color: White.
f.	No. 6 Wall Bracket: 6 inch (15.2 cm) extension. Non-adjustable.
1)	Capacity: 140 lbs (63.5 kg) maximum per pair.
2)	Color: Black.
3)	Color: White.
g.	Ceiling Trim Kit: Built-in LVC recommended.
R.	Basis of Design: Professional Electrol as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
b.	92 x 164 inches (234 x 417 cm). Diagonal: 188 inches (478 cm).
c.	106 x 188 inches (269 x 478 cm). Diagonal: 216 inches (549 cm).
d.	119 x 212 inches (302 x 538 cm). Diagonal: 243 inches (617 cm).
e.	133 x 236 inches (338 x 599 cm). Diagonal: 271 inches (688 cm).
f.	146 x 260 inches (371 x 660 cm). Diagonal: 298 inches (757 cm).
g.	160 x 284inches (406 x 721 cm). Diagonal: 326 inches (828 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
b.	117.5 x 188 inches (283 x 478 cm). Diagonal: 222 inches (564 cm).
c.	132.5 x 212 inches (337 x 538 cm). Diagonal: 250 inches (635 cm).
d.	147.5 x 236 inches (375 x 599 cm). Diagonal: 278 inches (706 cm).
e.	177.5 x 284 inches (451 x 721 cm). Diagonal: 335 inches (851 cm).
f.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	120 x 160 inches (305 x 406 cm). Diagonal: 200 inches (508 cm).
b.	123 x 164 inches (312 x 417 cm). Diagonal: 210 inches (533 cm).
c.	141 x 188 inches (358 x 478 cm). Diagonal: 240 inches (610 cm).
d.	159 x 212 inches (404 x 538 cm). Diagonal: 265 inches (673 cm).
e.	177 x 236 inches (450 x 599 cm). Diagonal: 295 inches (749 cm).
f.	195 x 260 inches (495 x 660 cm). Diagonal: 325 inches (826 cm).
g.	213 x 284 inches (541 x 721 cm). Diagonal: 355 inches (902 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Square. Viewing area (HxW).
a.	144 x 144 inches (366 x 366 cm).
b.	168 x 168 inches (427 x 427 cm).
c.	192 x 192 inches (488 x 488 cm).
d.	216 x 216 inches (549 x 549 cm).
e.	240 x 240 inches (610 x 610 cm).
f.	264 x 264 inches (671 x 671 cm).
g.	__ x __ inches (__ x __ cm).
5.	Certifications and Compliances: Listed by Underwriters' Laboratories.
6.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
1)	Secured in the housing with steel motor mount bracket.
7.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
8.	Rigid Metal Roller:
1)	Screens 12 ft (365.8 cm) Wide: Roll Diameter: 3 inches (7.6 cm).
2)	Screens 14 to 18 ft (427 x 549 cm) Wide: Roll Diameter: 5-3/4 inches (14.6 cm).
3)	Screens height or width is 20 ft (610 cm) or greater: Roller Diameter: 7 inches (17.8 cm).
a.	Roller Mounting Heavy Duty Bracket: Equipped with self-aligning bearing.
9.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking.
f.	Borders: None.
10.	Housing: Material: Wood, with double top for extra rigidity and strength.
a.	Finish: Black primer coat, ready to accept final finish by others.
b.	Finish: White primer coat, ready to accept final finish by others.
c.	Heavy Duty Metal Brackets: For mounting screen to a ceiling or wall.
d.	Overall Housing Length Dimensions: +/- 1/4 inch (6 mm).
11.	Control Switch: Three position with cover plate.
12.	Viewing Surface: Matte White. GREENGUARD and GREENGUARD Gold Certified.
a.	Horizontal seam required when width and height dimension exceed 16 ft (488 cm).
13.	Recessed Installation: Requires access to screen roller.
14.	Exposed Installation: May be covered with finished plywood, veneer, paneling, plastic wall covering or a valance.
15.	Options:
a.	Extra Drop: To lower picture area more than normal.
1)	Total Drop at Top: ___ inches (___ cm).
a)	Color: Black.
b)	Color: White.
2)	Total Drop at Bottom: ___ inches (___ cm)s.
a)	Color: Black.
b)	Color: White.
b.	Total Height Including Picture Area:
c.	The following applies to screen widths less than 24 ft.
1)	Total Height: 22 ft (671 cm) maximum.
2)	Total Height: 18 ft (549 cm) maximum.
16.	Accessories:
a.	External Low Voltage Control (LVC).
b.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger). Requires Integrated or External LVC.
1)	Radio Frequency (BLE) Remote
2)	Infrared Remote
3)	PoE Injector
c.	Key Locking Cover Plate for 120V or LVC Switch
d.	Key Operated Switch for 120 V only; cannot be used with LVC.
S.	Basis of Design: Myriad Reveal as manufactured by Da-Lite. An Automatic Electric Projection Screen Model.
1.	Model: Tensioned, SightLine Cable Drop.
2.	Model: Tensioned, Conventional Drop.
3.	Model: Non-Tensioned, SightLine Cable Drop.
4.	Model: Non-Tensioned, Conventional Drop.
5.	Format: HDTV (16:9). Viewing area (HxW).
a.	94.5 x 168 inches (240 x 427 cm). Diagonal: 193 inches x (490 cm)
b.	99 x 176 inches (251 x 447 cm). Diagonal: 202 inches (513 cm).
c.	108 x 192 inches (274 x 488 cm). Diagonal: 220 inches (559 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
6.	Format: Wide (16:10). Viewing area (HxW).
a.	105 x 168 inches (267 x 427 cm). Diagonal: 198 inches (503 cm)
b.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
c.	120 x 192 inches (305 x 488 cm). Diagonal: 226 inches (574 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
7.	Certifications and Compliances: Listed by Underwriters' Laboratories.
8.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
9.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
10.	Roller Material: Rigid metal.
11.	Junction Box: Internally integrated into the housing.
a.	Quick Connector: Mounted in the housing for easy plug-in connection to the motorized fabric and roller assembly.
12.	Housing: Single-piece design made of extruded aluminum.
a.	Finish: Powder coated. Lightly textured. 
1)	Color: White.
2)	Color: Black.
b.	Bottom of Housing: To have a removable access panel made of extruded aluminum.
c.	Overall Housing Length Dimensions: +/- 1/4 inch (6 mm).
13.	Integrated Low Voltage Control Unit.
14.	Control Switch: Decora-style, three-button wall switch with motor limit adjustment and third party control connections on the back.
a.	Dry contact interface.
b.	Projection Trigger: 5 to 12 Volts.
15.	Model: Tensioned.
a.	Screen Fabric:
1)	Seamless in the image area and mildew resistant.
2)	Front projection surfaces are black backed.
3)	GREENGUARD and GREENGUARD Gold Certified.
4)	Fire retardant.
5)	Borders: Black masking.
6)	Fabric Sides: Radio Frequency welded tab guide cable system on each vertical side. Maintains even lateral tension and holds screen fabric flat.
7)	Fabric Bottom: Inserted into a custom aluminum slat bar with added weight to provide vertical tension on the screen surface.
8)	Heavy Duty Plastic Caps: Protects the slat ends enclosing a preset adjustable mechanism for screen tensioning.
9)	Black Drop at Screen Top: 12 inches (30.5 cm).
b.	Viewing Surface: Parallax Stratos 1.0. Seamless. Black backing.
c.	Viewing Surface: HD Progressive 1.0. Seamless. Black backing.
d.	Viewing Surface: HD Progressive 1.1 Contrast. Seamless. Black backing.
e.	Viewing Surface: HD Progressive 1.3. Seamless. Black backing.
f.	Viewing Surface: HD Progressive ReView 0.9 (Rear). No black backing. Seamless.
g.	Viewing Surface: Da-Mat. Seamless. Black backing.
1)	Viewing Surface: Da-Tex (Rear). Seamless. No black backing.
16.	Model: Non-Tensioned.
a.	Screen Fabric:
1)	Mildew resistant.
2)	Front projection surfaces are black backed.
3)	GREENGUARD and GREENGUARD Gold Certified.
4)	Fire retardant.
5)	Borders: Black masking.
a)	Black masking.
b)	None.
6)	Fabric Bottom: Formed into a pocket holding a metal rod.
7)	Heavy Duty Vinyl Caps: Protects the ends of the rod.
8)	Black Drop at Screen Top: 2 inch (5.1 cm).
b.	Viewing Surface: Matte White. 
1)	Horizontal seam required when both dimensions exceed 10 ft (305 cm).
c.	Viewing Surface: High Contrast Matte White.
17.	Model: SightLine: Tensioned and Non-Tensioned.
a.	Roller drops material from case on four (4), 1.5 mm galvanized aircraft cables.
1)	Maximum Cable Drop: 16 ft (488 cm).
2)	Factory Set Cable Drop: 24 inches (61 cm).
3)	Final Cable Drop Setting: To be done in the field.
b.	Additional 22 inches of black at the top of screen for the following:
1)	Viewing Surface: HD Progressive 0.9. Seamless (Rear). No black backing.
2)	Viewing Surface: Da-Tex (Rear). Seamless. No black backing.
18.	Accessories: All models.
a.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger).
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
b.	Key Locking Cover Plate for LVC Switch.
T.	Basis of Design: Studio Electrol as manufactured by Da-Lite: Automatic Electric Projection Screen Model.
1.	Format: HDTV (16:9, 1.78:1). Viewing area (HxW).
a.	176 x 312 inches (447 x 792 cm). Diagonal: 359 inches (912 cm).
b.	189 x 336 inches (480 x 853 cm). Diagonal: 385 inches (978 cm).
c.	203 x 360 inches (516 x 914 cm). Diagonal: 414 inches (1052 cm).
d.	216 x 384 inches (549 x 975 cm). Diagonal: 440 inches (1118 cm).
e.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Cinemascope (21:9, 2.35:1). Viewing area (HxW).
a.	133 x 312 inches (338 x 792 cm). Diagonal: 340 inches (864 cm).
b.	143 x 336 inches (363 x 853 cm). Diagonal: 365 inches (927 cm).
c.	153 x 360 inches (389 x 914 cm). Diagonal: 391 inches (993 cm).
d.	163 x 384 inches (414 x 975 cm). Diagonal: 416 inches (1057 cm).
e.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3, 1.33:1). Viewing area (HxW).
a.	234 x 312 inches (594 x 792 cm). Diagonal: 390 inches (991 cm).
b.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 3.4 amps max.
c.	Motor Characteristics: Two wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
5.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
6.	Junction Box: Internally integrated into housing. Allows housing installation and wiring to facility's electrical system during construction.
7.	Motorized Fabric and Roller Assembly: Installed in the housing at the factory.
a.	Designed for left hand motor installation.
8.	Roller Material: Rigid steel, 7-5/8 inch (19.4 cm) diameter.
9.	Screen Fabric:
a.	Mildew resistant.
b.	GREENGUARD and GREENGUARD Gold Certified.
c.	Fire retardant.
d.	Fabric Bottom: Fitted with a metal slat covering.
e.	Heavy Duty Plastic Caps: Protect the metal slat ends.
10.	Housing: Structural steel tubing.
a.	Top: Aluminum metal coverings.
b.	Rear and Front: Aluminum profiles on rear and front.
c.	Side Coverings: Extruded aluminum.
d.	Bottom: Open.
e.	Overall Housing Length Dimensions: +/- 1/4 inch (6 mm).
f.	Finish: Powder coated. Gray.
g.	Finish: Powder coated. White.
h.	Finish: Powder coated. Black.
11.	Three-position radio remote control.
12.	Adjustable Mounting Brackets: For ceiling installation.
13.	Adjustable Mounting Brackets: For wall installation.
14.	Viewing Surfaces: GREENGUARD and GREENGUARD Gold Certified.
15.	Viewing Surface: Matte White:
a.	Horizontal seam required when height exceeds 75 inches (190.5 cm).
16.	Viewing Surface: Perforated Matte White:
a.	Horizontal seam required when height exceeds 75 inches (190.5 cm).
17.	Extra Drop to Lower Picture Area:
a.	Total White Drop at Top: ___ inches (___ cm).
b.	Total White Drop at Bottom: ___ inches (___ cm).
18.	Maximum Total Surface Height Including Picture Area: 19 ft 8 inches (600 cm).
U.	Basis of Design: Myriad Conceal as manufactured by Da-Lite. Automatic Electric Projection Screen Model.
1.	Model: Tensioned, SightLine Cable Drop.
2.	Model: Tensioned, Conventional Drop.
3.	Model: Non-Tensioned, SightLine Cable Drop.
4.	Model: Non-Tensioned, Conventional Drop.
5.	Format: HDTV (16:9). Viewing area (HxW).
a.	94.5 x 168 inches (240 x 427 cm). Diagonal: 193 inches x (490 cm)
b.	99 x 176 inches (251 x 447 cm). Diagonal: 202 inches (513 cm).
c.	108 x 192 inches (274 x 488 cm). Diagonal: 220 inches (559 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
6.	Format: Wide (16:10). Viewing area (HxW).
a.	105 x 168 inches (267 x 427 cm). Diagonal: 198 inches (503 cm)
b.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
c.	120 x 192 inches (305 x 488 cm). Diagonal: 226 inches (574 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
7.	Certifications and Compliances: Listed by Underwriters' Laboratories.
8.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 2.4 amps max.
c.	Electric: 220 Volt (50 Hz) 2.4 amps max.
d.	Motor Characteristics: Three wire with ground, quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
e.	Quick connect male plug-in connector on the motor.
9.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
10.	Motorized Fabric and Roller Assembly: Installed in the housing at the factory or at a later time at the job site. 
a.	Roller Material: Rigid metal.
11.	Junction Box: Internally integrated into the housing.
a.	Quick Connector: Mounted in the housing for easy plug-in connection to the motorized fabric and roller assembly.
12.	Housing: Extruded aluminum.
a.	Finish: Powder coated. Color: White.
b.	Finish: Powder coated. Color: Black.
c.	End Caps: Heavy gauge steel.
d.	Housing Bottom: Self-trimming. Built-in flange around housing bottom.
1)	Hinged Aluminum Door: Opens and closes with the lowering and raising of projection screen.
a)	Opens by gravity when screen is being lowered.
b)	When screen is being raised, the two ends of the slat at the bottom screen fabric engage two hooks on the door to lift it to the closed position.
2)	Balance of Housing Bottom: A second manually removable aluminum access door for access.
3)	Hinges: Mounted in a concealed manner.
e.	Quick Connector: Mounted in the housing for easy plug-in connection to the motorized fabric and roller assembly.
f.	Overall Housing Length: +/- 1/4 inches (6 mm).
g.	For use in environmental air space according to section 300-22 (c) of the National Electric Code, and sections 2-128, 12-010 (3) and 12-100 of the Canadian Electrical Code, part 1, CSA C22.1.
13.	Integrated Low Voltage Control Unit.
14.	Control Switch: Decora-style, three-button wall switch with motor limit adjustment and third party control connections on the back.
a.	Dry Contact Interface.
b.	Projection Trigger; 5 to 12V.
15.	Model: Tensioned.
a.	Screen Fabric:
1)	Seamless in the image area and mildew resistant.
2)	Front projection surfaces are black backed.
3)	GREENGUARD and GREENGUARD Gold Certified.
4)	Fire retardant.
5)	Borders: Black masking.
6)	Fabric Sides: Radio frequency tab guide cable system on each vertical side. Maintains even lateral tension and holds screen fabric flat.
7)	Fabric Bottom: To be inserted into a custom aluminum slat bar with added weight to provide vertical tension on the screen surface.
8)	Heavy Duty Plastic Caps: Protects the slat ends enclosing a preset adjustable mechanism for screen tensioning.
9)	Black Drop at Screen Top: 12 inches (30.5 cm).
b.	Viewing Surface: Parallax Stratos 1.0.
c.	Viewing Surface: HD Progressive 1.0. 
d.	Viewing Surface: HD Progressive 1.1 Contrast. 
e.	Viewing Surface: HD Progressive 1.3. 
f.	Viewing Surface: HD Progressive ReView 0.9 (Rear). 
g.	Viewing Surface: Da-Mat. 
h.	Viewing Surface: Da-Tex (Rear). 
16.	Model: Non-Tensioned.
a.	Screen Fabric:
1)	Mildew resistant.
2)	Front projection surfaces are black backed.
3)	GREENGUARD and GREENGUARD Gold Certified.
4)	Fire retardant.
5)	Borders: Black masking.
6)	Borders: None.
7)	Fabric Bottom: Formed into a pocket holding a metal rod.
8)	Heavy Duty Vinyl Caps: Protects the ends of the rod.
9)	Black Drop at Screen Top: 2 inch (5.1 cm).
b.	Viewing Surface: Matte White. 
1)	Horizontal seam required when both dimensions exceed 10 ft (305 cm).
c.	Viewing Surface: High Contrast Matte White.
17.	Model: SightLine: Tensioned and Non-Tensioned.
a.	Roller drops material from case on four (4), 1.5 mm galvanized aircraft cables.
1)	Maximum Cable Drop: 16 ft (488 cm).
2)	Factory Set Cable Drop: 24 inches (61 cm). 
3)	Final Cable Drop Setting: To be done in the field.
b.	Additional 22 in Black at the top of screen for the following:
1)	Viewing Surface: HD Progressive 0.9. Seamless. Black backing.
2)	Viewing Surface: Da-Tex (Rear). Seamless.
18.	Accessories: All models.
a.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger).
1)	Radio Frequency (BLE) Remote.
2)	Infrared Remote.
3)	PoE Injector.
b.	Key Locking Cover Plate for LVC Switch.
V.	Basis of Design: Designer Contour Electrol, Battery Operated as manufactured by Da-Lite: with Agility Battery Motor (Lithium-Ion).
1.	Model: Tensioned.
2.	Model: Non-Tensioned.
3.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 60 inches (127 x 103 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
5.	Screen Motor: Integrated lithium ion battery, 5V Micro-USB charging port.
a.	Mounting: Inside the roller.
b.	Motor Characteristics: Quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
6.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
7.	Screen Roller Material: Rigid metal.
8.	Housing: Two-piece extruded aluminum
a.	Finish: Powder coated: Lightly textured. Color: White.
b.	Finish: Powder coated: Lightly textured. Color: Black.
c.	Overall Housing Length Dimensions: +/- 1/4 inch (6 mm).
9.	Model: Tensioned Designer Contour:
a.	Black Drop at Top: 12 inches (30.5 cm).
b.	Screen Fabric: Flame retardant, mildew resistant, and seamless.
1)	Masking Borders: Black.
2)	Each Side of Screen Fabric: To have radio frequency welded tab guide cable system to maintain even lateral tension and hold flat.
3)	Screen Bottom: Inserted into custom slat bar with added weight that maintains vertical tension on the screen surface.
c.	Screen Fabric:
1)	Seamless in the image area and mildew resistant.
2)	Front projection surfaces are black backed.
3)	GREENGUARD and GREENGUARD Gold Certified.
4)	Fire retardant.
d.	Viewing Surface: HD Progressive 1.0. 
e.	Viewing Surface: Da-Mat. 
10.	Model: Designer Contour: Non-Tensioned.
a.	Black Drop at Top: 2 inches (5.1 cm).
b.	Screen Fabric:
1)	Seamless in the image area and mildew resistant.
2)	Front projection surfaces are black backed.
3)	GREENGUARD and GREENGUARD Gold Certified.
4)	Fire retardant.
5)	Masking Borders: Black.
6)	Screen Bottom: Formed into a pocket holding a metal rod.
a)	Heavy Duty Vinyl Caps: Protects rod ends.
1)	Viewing Surface: Matte White.
2)	Viewing Surface: High Contrast Matte White.
11.	Three-button radio frequency remote control with wall mount bracket.
12.	Accessories:
a.	WiFi Bridge.
b.	PoE 5V Micro-USB Adapter.
W.	Basis of Design: Designer Contour Electrol as manufactured by Da-Lite. With 120 V, 60 Hz, or 220-V, 50 Hz motor.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	37.5 x 67 inches (95 x 170 cm). Diagonal: 77 inches (196 cm).
b.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
c.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	43 x 57 inches (109 x 145 cm). Diagonal: 72 inches (183 cm).
b.	50 x 67 inches (127 x 170 cm). Diagonal: 84 inches (213 cm).
c.	60 x 80 inches (152 x 203 cm). Diagonal: 100 inches (254 cm).
d.	69 x 92 inches (175 x 234 cm). Diagonal: 120 inches (305 cm).
e.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Square. Viewing area (HxW).
a.	60 x 60 inches (152 x 152 cm).
b.	70 x 70 inches (178 x 178 cm).
c.	84 x 84 inches (213 x 213 cm).
d.	96 x 96 inches (244 x 244 cm).
e.	__ x __ inches (__ x __ cm).
4.	Certifications and Compliances: Listed by Underwriters' Laboratories.
5.	Screen Motor:
a.	Mounting: In the roller.
b.	Electric: 120 volt (60 Hz) 1.2 amps max.
c.	Electric: 220 Volt (50 Hz) 1.2 amps max.
d.	Motor Characteristics: Three wire with ground quick reversal type, oiled for life, with automatic thermal overload cutout, integral gears, capacitor, and an electric brake to prevent coasting.
6.	Limit Switches: Preset and adjustable. Stop picture surface in the "up" and "down" positions.
7.	Screen Roller Material: Rigid metal.
8.	Housing: Two-piece extruded aluminum.
a.	Finish: Powder coated: Lightly textured. Color: White.
b.	Finish: Powder coated: Lightly textured. Color: Black.
c.	Overall Housing Length Dimensions: +/- 1/4 inch (6 mm).
9.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking.
f.	Borders: None.
g.	Screen Bottom: Formed into a pocket holding a metal rod.
h.	Heavy Duty Vinyl Caps: Protects rod ends.
10.	Viewing Surface: Matte White.
11.	Viewing Surface: High Contrast Matte White.
12.	Three-position control switch and cover plate.
13.	Accessories:
a.	Single Motor Low Voltage Control (LVC); built-in.
1)	Adds 5 inches (12.7 cm) to housing length.
b.	External Low Voltage Control (LVC).
c.	Screen Controller (TCP/IP, RS232, Dry Contact, and VPI/Trigger). Requires Integrated or External LVC.
1)	Radio Frequency (BLE) Remote
2)	Infrared Remote
3)	PoE Injector
d.	Key Locking Cover Plate for 120V or LVC Switch
e.	Key Operated Switch for 120V only. Cannot be used with LVC.
2.3	FIXED FRAME PROJECTION SCREENS
A.	Basis of Design: Da-Snap. Wall mounted projection screen as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	37.5 x 67 inches (95 x 170 cm). Diagonal: 77 inches (196 cm).
b.	40.5 x 72 inches (103 x 183 cm). Diagonal: 82 inches (208 cm).
c.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
d.	49 x 87 inches (124 x 221 cm). Diagonal: 100 inches 254 cm).
e.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
f.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
g.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
h.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
i.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
j.	94.5 x 168 inches (240 x 427 Cm). Diagonal: 193 inches x (490 cm).
k.	108 x 192 inches (274 x 488 cm). Diagonal: 220 inches (559 cm).
l.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches 480 cm).
i.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
j.	120 x 192 inches (305 x 488 cm). Diagonal: 226 inches (574 cm).
k.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Cinemascope (2.35:1). Viewing area (HxW).
a.	37.5 x 88 inches (95 x 224 cm). Diagonal: 96 inches (244 cm).
b.	40.5 x 95 inches (103 x 241 cm). Diagonal: 103 inches (262 cm).
c.	45 x 106 inches (114 x 269 cm). Diagonal: 115 inches (292 cm).
d.	49 x 115 inches (124 x 292 cm). Diagonal: 125 inches (318 cm).
e.	52 x 122 inches (132 x 310 cm). Diagonal: 133 inches (338 cm).
f.	54 x 126 inches (137 x 320 cm). Diagonal: 138 inches (351 cm).
g.	58 x 136.5 inches (147 x 347 cm). Diagonal: 148 inches (376 cm).
h.	65 x 153 inches (165 x 389 cm). Diagonal: 166 inches (422 cm).
i.	78 x 183.5 inches (198 x 466 cm). Diagonal: 199 inches (505 cm).
j.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Reinforced Black Binding: All four sides.
f.	Frame Attachment: Metal snaps. Frame will conceal snaps and binding.
g.	Frame Attachment: Velcro.
h.	Screen Frame: 1-1/2 inch (3.81 cm) square aluminum.
1)	Finish: Powder coated. Color: Matte black.
2)	Finish: Pro-Trim Fabric Covering. A masked border that absorbs the light surrounds the viewing area.
3)	Walls: Ribbed for strength and light weight.
4)	Corners: Slip-jointed at corners and joints.
5)	Wall-Mounting Brackets: Included.
6)	Overall Dimensions: +/- 1/4 inches.
5.	Viewing Surface: HD Progressive 1.0. 
6.	Viewing Surface: HD Progressive 1.0 Perf. Sizes up to 8 ft (244 cm) high. 
7.	Viewing Surface: HD Progressive 1.3. 
8.	Viewing Surface: Da-Mat. 
9.	Viewing Surface: Da-Tex (Rear). 
10.	Viewing Surface: HD Progressive ReView 0.9 (Rear). 
11.	Accessory: T-Legs.
B.	Basis of Design: Cinema Contour. Wall mounted projection screen as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	37.5 x 67 inches (95 x 170 cm). Diagonal: 77 inches (196 cm).
b.	40.5 x 72 inches (103 x 183 cm). Diagonal: 82 inches (208 cm).
c.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
d.	49 x 87 inches (124 x 221 cm). Diagonal: 100 inches 254 cm).
e.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
f.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
g.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
h.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
i.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
j.	94.5 x 168 inches (240 x 427 Cm). Diagonal: 193 inches x (490 cm).
k.	108 x 192 inches (274 x 488 cm). Diagonal: 220 inches (559 cm).
l.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches 480 cm).
i.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
j.	120 x 192 inches (305 x 488 cm). Diagonal: 226 inches (574 cm).
k.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Ultrawide (21:9). Viewing area (HxW)
a.	40.5 x 96 inches (103 x 244 cm). Diagonal: 104 inches (264 cm)
b.	50.75 x 120 inches (129 x 305 cm). Diagonal: 130 inches (330 cm)
c.	60.75 x 144 inches (154 x 366 cm). Diagonal: 156 inches (396 cm)
d.	71 x 168 inches (180 x 427 cm). Diagonal: 182 inches (462 cm)
e.	81 x 192 inches (206 x 488 cm). Diagonal: 208 inches (528 cm)
f.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Cinemascope (2.35:1). Viewing area (HxW).
a.	37.5 x 88 inches (95 x 224 cm). Diagonal: 96 inches (244 cm).
b.	40.5 x 95 inches (103 x 241 cm). Diagonal: 103 inches (262 cm).
c.	45 x 106 inches (114 x 269 cm). Diagonal: 115 inches (292 cm).
d.	49 x 115 inches (124 x 292 cm). Diagonal: 125 inches (318 cm).
e.	52 x 122 inches (132 x 310 cm). Diagonal: 133 inches (338 cm).
f.	54 x 126 inches (137 x 320 cm). Diagonal: 138 inches (351 cm).
g.	58 x 136.5 inches (147 x 347 cm). Diagonal: 148 inches (376 cm).
h.	65 x 153 inches (165 x 389 cm). Diagonal: 166 inches (422 cm).
i.	78 x 183.5 inches (198 x 466 cm). Diagonal: 199 inches (505 cm).
j.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
5.	Viewing Surfaces:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Reinforced Black Binding: All four sides.
f.	Frame Attachment: Metal snaps. Frame will conceal snaps and binding.
g.	Frame Attachment: Velcro.
h.	Screen Frame (Width x Depth): 3 x 1-5/8 inch (7.6 x 4.1 cm) aluminum. A tapered front edge to reduce shadows on the viewing surface.
1)	Finish: Pro-Trim fabric covering. Color: Black.
2)	Finish: Textured Powder coated. Color: Black.
3)	Walls: Ribbed for strength and light weight.
i.	Overall Dimensions: +/- 1/4 inches (6 mm).
6.	Viewing Surface: Parallax Stratos 1.0. 
7.	Viewing Surface: HD Progressive 1.0. 
8.	Viewing Surface: HD Progressive 1.0 Perf. Sizes up to 8 ft (243.8 cm) high. 
9.	Viewing Surface: HD Progressive 1.1 Contrast.
10.	Viewing Surface: HD Progressive 1.3. 
11.	Viewing Surface: Da-Mat. 
12.	Viewing Surface: Da-Tex (Rear). 
13.	Viewing Surface: HD Progressive ReView 0.9 (Rear).
14.	Accessory: T-Legs.
C.	Basis of Design: UTB Contour. Wall mounted projection screen as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	37.5 x 67 inches (95 x 170 cm). Diagonal: 77 inches (196 cm).
b.	40.5 x 72 inches (103 x 183 cm). Diagonal: 82 inches (208 cm).
c.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
d.	49 x 87 inches (124 x 221 cm). Diagonal: 100 inches 254 cm).
e.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
f.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
g.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
h.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
i.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
j.	94.5 x 168 inches (240 x 427 Cm). Diagonal: 193 inches x (490 cm).
k.	108 x 192 inches (274 x 488 cm). Diagonal: 220 inches (559 cm).
l.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches 480 cm).
i.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
j.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Ultrawide (21:9). Viewing area (HxW).
a.	40.5 x 96 inches (103 x 244 cm). Diagonal: 104 inches (264 cm)
b.	50.75 x 120 inches (129 x 305 cm). Diagonal: 130 inches (330 cm)
c.	60.75 x 144 inches (154 x 366 cm). Diagonal: 156 inches (396 cm)
d.	71 x 168 inches (180 x 427 cm). Diagonal: 182 inches (462 cm)
e.	81 x 192 inches (206 x 488 cm). Diagonal: 208 inches (528 cm)
f.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Cinemascope (2.35:1). Viewing area (HxW).
a.	37.5 x 88 inches (95 x 224 cm). Diagonal: 96 inches (244 cm).
b.	40.5 x 95 inches (103 x 241 cm). Diagonal: 103 inches (262 cm).
c.	45 x 106 inches (114 x 269 cm). Diagonal: 115 inches (292 cm).
d.	49 x 115 inches (124 x 292 cm). Diagonal: 125 inches (318 cm).
e.	52 x 122 inches (132 x 310 cm). Diagonal: 133 inches (338 cm).
f.	54 x 126 inches (137 x 320 cm). Diagonal: 138 inches (351 cm).
g.	58 x 136.5 inches (147 x 347 cm). Diagonal: 148 inches (376 cm).
h.	65 x 153 inches (165 x 389 cm). Diagonal: 166 inches (422 cm).
i.	78 x 183.5 inches (198 x 466 cm). Diagonal: 199 inches (505 cm).
j.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
5.	Viewing Surfaces:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Reinforced Black Binding: All four sides.
f.	Frame Attachment: Metal snaps. Frame will conceal snaps and binding.
g.	Viewing Surface: Parallax Stratos 1.0. 
h.	Viewing Surface: HD Progressive 1.0. 
i.	Viewing Surface: HD Progressive 1.1 Contrast. 
j.	Viewing Surface: HD Progressive 1.3.
k.	Viewing Surface: Da-Mat. 
6.	Frame (W x D): 2-1/2 x 1-3/8 inch (6.3 x 3.5 cm) aluminum.
a.	Corners: Slip-jointed. Lip: 1/8 inch, to eliminate marks on the surface.
b.	Bezel: To conceal frame, grommets, and binding.
1)	Front Lip of Bezel: To be 1/4 inch (6 mm) all around viewing area surface.
2)	Material: Aluminum.
3)	Finish: Acid Etched Black.
c.	Wall Mounting Brackets: Included.
d.	Bottom back of screen to be secured, with a screw, to a bottom wall bracket.
e.	Overall dimensions +/- 1/4 inches (6 mm).
D.	Basis of Design: Parallax. Wall mounted projection screen as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	37.5 x 67 inches (95 x 170 cm). Diagonal: 77 inches (196 cm).
b.	40.5 x 72 inches (103 x 183 cm). Diagonal: 82 inches (208 cm).
c.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
d.	49 x 87 inches (124 x 221 cm). Diagonal: 100 inches 254 cm).
e.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
f.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
g.	59 x 104.5 inches (150 x 265 cm). Diagonal: 120 inches (305 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	44.5 x 71.5 inches (113 x 182 cm). Diagonal: 84 inches (213 cm).
b.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
c.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Ultrawide (21:9). Viewing area (HxW).
a.	40.5 x 96 inches (103 x 244 cm). Diagonal: 104 inches (264 cm).
b.	50.75 x 120 inches (129 x 305 cm). Diagonal: 130 inches (330 cm).
c.	59 x 140 inches (150 x 356 cm). Diagonal: 152 inches (386 cm).
d.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Cinemascope (2.35:1). Viewing area (HxW).
a.	37.5 x 88 inches (95 x 224 cm). Diagonal: 96 inches (244 cm).
b.	40.5 x 95 inches (103 x 241 cm). Diagonal: 103 inches (262 cm).
c.	45 x 106 inches (114 x 269 cm). Diagonal: 115 inches (292 cm).
d.	49 x 115 inches (124 x 292 cm). Diagonal: 125 inches (318 cm).
e.	52 x 122 inches (132 x 310 cm). Diagonal: 133 inches (338 cm).
f.	54 x 126 inches (137 x 320 cm). Diagonal: 138 inches (351 cm).
g.	58 x 136.5 inches (147 x 347 cm). Diagonal: 148 inches (376 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
5.	Screen Fabric:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Ambient light rejecting. Reinforced tabbed holes on all four sides that attach to frame with elastic rings. Frame is to conceal holes and rings.
6.	Screen Frame (W x D): 2-1/2 x 1-1/2 inch (6.3 x 3.8 cm).
a.	Tapered front edge to reduce shadows on the .
b.	Material: Aluminum.
1)	Finish: Pro-Trim fabric covering to enhance appearance and absorb light surrounding the viewing area. Color: Black.
c.	Slip-jointed at corners and joints.
d.	Wall Mounting Brackets: Included.
e.	Overall Dimensions: +/- 1/4 inches (6 mm).
7.	Viewing Surface: Parallax Pure 0.8. Seamless. 
8.	Viewing Surface: Parallax Pure UST 0.6. Seamless. 
E.	Basis of Design: Lace and Grommet as manufactured by Da-Lite. For a permanent fixed or fly screen with a user-supplied frame. Recommended for use with Da-Lite's Series 300 Lace and Grommet Frame.
1.	Viewing Area (H x W): ____ x ____ inches (____ x ____ cm).
2.	Features:
a.	Heavy-duty grommets for even screen tautness.
b.	Available with snap-button style for mounting on provided studs.
c.	Binding: Black.
d.	Binding: White.
e.	Available with lacing cord.
f.	Mildew resistant.
g.	Front projection surfaces are black backed.
h.	GREENGUARD and GREENGUARD Gold Certified.
i.	Fire retardant.
3.	Viewing Surface: HD Rental. Seamless up to 16 ft (488 cm). 
4.	Viewing Surface: Parallax Stratos 1.0. Seamless up to 16 ft (488 cm). 
5.	Viewing Surface: HD Progressive 1.0. Seamless up to 16 ft (488 cm). 
6.	Viewing Surface: HD Progressive 1.0 Perf. Seamless up to 8 ft (244 cm) high. 
7.	Viewing Surface: HD Progressive 1.1 Contrast. Seamless up to 16 ft (488 cm). 
8.	Viewing Surface: HD Progressive 1.3. Seamless up to 16 ft (488 cm). 
9.	Viewing Surface: Da-Mat. Seamless up to 16 ft (488 cm). 
10.	Viewing Surface: Da-Mat. Seamless up to 16 ft (488 cm). 
11.	Viewing Surface: HD Progressive ReView 0.9 (Rear). Seamless up to 16' (488 cm). 
12.	Viewing Surface: Da-Tex (Rear). Seamless up to 16 ft (488 cm). 
F.	Basis of Design: Series 300 Lace and Grommet Frame as manufactured by Da-Lite. Wall mounted projection screen.
1.	Screen Configuration: Flat.
2.	Screen Configuration: Curved.
a.	Specified to any degree of single-axis curve with a maximum width of 30 ft (914 cm).
3.	Viewing Area (H x W): ____ x ____ inches (____ x ____ cm).
4.	Frame: 3 inch (7.6 cm) diameter aluminum tubing with radius frame corners.
a.	Frame Sections: Slip fit at corners.
b.	Lacing Cord: Woven onto frame sections with preinstalled S-hooks for viewing surface attachment.
1)	Masking Cover: 7 inches (17.8 cm) wide. Conceals lace cord and hooks. Includes Pro-Trim to enhance appearance and absorb light surrounding the viewing area.
c.	Finish: Powder coated. Color: Black.
d.	Mounting: Suspended from ceiling.
1)	By means of included eyebolts installed on top frame section.
2)	Eye bolts included for ceiling installation.
e.	Mounting: Attached to wall.
1)	Wall mount brackets and eye bolts included for wall installation.
f.	Outside Dimension Greater than 20 ft 8 inch (630 cm). Will have two-piece top and bottom or side frame sections.
g.	Maximum Frame Outside Dimension; Height or Width:
1)	Front Projection: 90 ft (2743 cm) 
2)	Rear Projection: 40 ft (1219 cm).
h.	Maximum Screen Viewing Area; Height or Width:
1)	Front Projection: 88 ft 10 inch (2708 cm).
2)	Rear Projection: 38 ft 10 inch (1184 cm).
i.	Overall Frame Dimensions: +/- 1/4 inches (6 mm).
5.	Viewing surfaces:
a.	Mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Viewing Surface: HD Rental. Seamless up to 16 ft (488 cm).
f.	Viewing Surface: Parallax Stratos 1.0. Seamless up to 16 ft (488 cm). 
g.	Viewing Surface: HD Progressive 1.0. Seamless up to 16 ft (488 cm). 
h.	Viewing Surface: HD Progressive 1.0 Perf. Seamless up to 8 ft (244 cm) high. 
i.	Viewing Surface: HD Progressive 1.1 Contrast Seamless up to 16 ft (488 cm). 
j.	Viewing Surface: HD Progressive 1.3. Seamless up to 16 ft (488 cm). 
k.	Viewing Surface: Da-Mat. Seamless up to 16 ft (488 cm). 
l.	Viewing Surface: HD Progressive ReView 0.9 (Rear). Seamless up to 16 ft (488 cm). 
m.	Viewing Surface: Da-Tex (Rear). Seamless up to 16 ft (488 cm).
G.	Basis of Design: FullVision. Wall mounted projection screen as manufactured by Da-Lite.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	40.5 x 72 inches (103 x 183 cm). Diagonal: 82 inches (208 cm)
b.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
c.	49 x 87 inches (124 x 221 cm). Diagonal: 100 inches 254 cm).
d.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
e.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
f.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
g.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
h.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
i.	94.5 x 168 inches (240 x 427 Cm). Diagonal: 193 inches x (490 cm)
j.	108 x 192 inches (274 x 488 cm). Diagonal: 220 inches (559 cm).
k.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	100 x 160 inches (254 x 406 cm). Diagonal: 189 inches 480 cm).
i.	110 x 176 inches (279 x 447 cm). Diagonal: 208 inches (528 cm).
j.	120 x 192 inches (305 x 488 cm). Diagonal: 226 inches (574 cm).
k.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Screen Surface: Flexible, fire retardant and mildew resistant.
a.	Wraps completely around to the back of the fixed frame.
4.	Frame: Fixed. Material: Extruded aluminum.
5.	Border: None.
6.	Mounting: Steel mounting brackets for wall mounting or ceiling suspension.
7.	Assembly:
a.	Screen Depth: 13/16 inches (2 cm).
b.	Ships disassembled.
c.	Assembled by joining frame pieces using steel corner brackets, which are secured by setscrews using an Allen wrench.
d.	Attached by joining loop Velcro on the fabric to the hook Velcro on the frame.
e.	Overall Dimensions: +/- 1/4 inches (6 mm).
8.	Viewing Surfaces:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Viewing Surface: Parallax Stratos 1.0. 
f.	Viewing Surface: HD Progressive 1.0. 
g.	Viewing Surface: HD Progressive 1.1. Contrast. 
h.	Viewing Surface: HD Progressive 1.3. 
2.4	PORTABLE PROJECTION SCREENS
A.	Basis of Design: Fast-Fold Deluxe Screen System as manufactured by Da-Lite. Portable projection screen. Carrying Case: Wheeled polyethylene cases that meet or exceed Air Transport Association (ATA) Specification 300 standards.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	50.5 x 90.5 inches (128 x 230 cm).
b.	56.5 x 102.5 inches (144 x 261 cm).
c.	63.5 x 114.5 inches (161 x 291 cm).
d.	77.5 x 138.5 inches (197 x 352 cm).
e.	90.5 x 162.5 inches (230 x 413 cm).
f.	__ x __ inches (__ x __ cm).
2.	Format: HDTV (16:10). Viewing area (HxW).
a.	56.5 x 90.5 inches (144 x 261 cm).
b.	63.5 x 102.5 inches (161 x 291 cm).
c.	71.5 x 114.5 inches (197 x 352 cm).
d.	86.5 x 138.5 inches (220 x 352 cm).
e.	__ x __ inches (__ x __ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	66.5 x 90.5 inches (167 x 230 cm).
b.	84.5 x 114.5 inches (215 x 291 cm).
c.	102.5 x 138.5 inches (260 x 352 cm).
d.	120.5 x 162.5 inches (306 x 413 cm).
e.	__ x __ inches (__ x __ cm).
4.	Screen Surface: Flexible. Mildew resistant.
a.	Reinforced Black Binding: On all four sides.
b.	Attachment to Frame Front: Metal snaps.
c.	Seamless in the image area and mildew resistant.
d.	Front projection surfaces are black backed.
e.	GREENGUARD and GREENGUARD Gold Certified.
f.	Fire retardant.
5.	Frame Material: Lightweight, folding 1-1/4 inch (32 mm) square hard alloy aluminum tubing.
a.	Finish: Clear etched and anodized. Brushed and burr free.
b.	Finish: Black anodized. Brushed and burr free.
c.	Frame Sections: Joined with snap latch to allow for easy folding.
d.	Hardware: Steel and plated.
6.	Legs: Inverted "T" legs support the screen and allow height adjustments up or down in 6 inch (15 cm) increments.
a.	Supports the frame.
7.	Viewing Surface: HD Rental. Seamless. Black backing. Foldable.
8.	Viewing Surface: HD Progressive ReView 0.9 (Rear). Seamless. Foldable.
9.	Viewing Surface: Da-Tex (Rear). Seamless. Foldable.
10.	Accessories:
a.	HD Legs: Heavy duty legs add stability to larger screen sizes.
b.	Masking Panels: From 16:9 formatted screens to 4:3 format.
c.	Masking Panels: From 16:9 formatted screens to 16:10 format.
d.	Ultra Velour Drapery Presentation Kit: Adjustable Skirt Bar. Color: Black.
e.	Ultra Velour Drapery Presentation Kit: Adjustable Skirt Bar. Color: Blue.
f.	Ultra Velour Drapery Presentation Kit: Adjustable Skirt Bar. Color: Gray.
B.	Basis of Design: Heavy Duty Fast-Fold Deluxe Screen System as manufactured by Da-Lite. Portable projection screen.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	7.5 x 13.33 ft (229 x 406 cm).
b.	9 x 16 ft (274 x 488 cm).
c.	10 x 18 ft (305 x 549 cm).
d.	11.25 x 20 ft (343 x 610 cm).
e.	12 x 21.33 ft (366 x 650 cm).
f.	13.5 x 24 ft (411 x 732 cm).
g.	15 x 26.5 ft (457 x 808 cm).
h.	__ x __ inches (__ x __ cm).
2.	Format: HDTV (16:10). Viewing area (HxW).
a.	8.33 x 13.33 ft (254 x 406 cm).
b.	10 x 16 ft. (305 x 488 cm).
c.	13.25 x 18 ft. (343 x 549 cm).
d.	12.5 x 20 ft. (381 x 610 cm).
e.	__ x __ inches (__ x __ cm).
3.	Screen Surface: Flexible and mildew resistance.
a.	Reinforced Black Binding: On all four sides.
b.	Attachment to Frame Front: Metal snaps.
c.	Seamless in the image area and mildew resistant.
d.	Front projection surfaces are black backed.
e.	GREENGUARD and GREENGUARD Gold Certified.
f.	Fire retardant.
4.	Frames:
a.	Frame Sections:
1)	High Strength Aluminum Alloy Tube: 1-1/4 x 3-1/2 inch (3.2. x 8.9 cm).
2)	Frame Corners: Slip jointed with a cast speedy crank lock assembly.
b.	Hinged Sections: Joined with snap latch to allow for easy folding.
c.	Frame Legs: Heavy Duty Fast-Fold Deluxe with anti-sway braces.
1)	Supports the frame.
2)	Height Adjustments: Up or down in 6 inch (15.2 cm) increments.
d.	Larger Frames: Require additional bracing for rigidity and long life.
e.	Finish: Clear etched and anodized. Brushed and burr free.
f.	Finish: Black anodized. Brushed and burr free.
g.	Steel Hardware: To be plated.
5.	Wheeled Polyethylene Carrying Case: Must meet Air Transport Association (ATA) Specification 300 standard.
6.	Viewing Surface: HD Rental. Seamless. Foldable.
7.	Viewing Surface: HD Progressive ReView 0.9 (Rear). Foldable.
8.	Viewing Surface: Da-Tex (Rear). Foldable.
9.	Accessories:
a.	Drapery Presentation Kit. Color: Black.
b.	Drapery Presentation Kit. Color: Blue.
c.	Drapery Presentation Kit. Color: Gray.
d.	Masking Panels: To mask 16:9 formatted screens to 4:3 format.
C.	Basis of Design: Fast-Fold Truss Frame System as manufactured by Da-Lite: Portable projection screen.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	7.5 x 13.33 ft (229 x 406 cm).
b.	9 x 16 ft (274 x 488 cm).
c.	10 x 18 ft (305 x 549 cm).
d.	11.25 x 20 ft (343 x 610 cm).
e.	12 x 21.33 ft (366 x 650 cm).
f.	13.5 x 24 ft (411 x 732 cm).
g.	15 x 26.5 ft (457 x 808 cm).
h.	__ x __ inches (__ x __ cm).
2.	Format: HDTV (16:10). Viewing area (HxW).
a.	8.33 x 13.33 ft (254 x 406 cm).
b.	10 x 16 ft. (305 x 488 cm).
c.	13.25 x 18 ft. (343 x 549 cm).
d.	12.5 x 20 ft. (381 x 610 cm).
e.	__ x __ inches (__ x __ cm).
3.	Screen Surface: Flexible and mildew resistance.
a.	Reinforced Black Binding: On all four sides.
b.	Attachment to Frame Front: Metal snaps.
c.	Seamless in the image area and mildew resistant.
d.	Front projection surfaces are black backed.
e.	GREENGUARD and GREENGUARD Gold Certified.
f.	Fire retardant.
4.	Frames: 1 inch square aluminum tubing, heliarc welded to form a 6 x 1 truss member.
a.	Hinged Members: Joined with piano hinge to allow for folding.
b.	Truss Legs: 6 inches (15.2 cm) with anti-sway braces support the truss frame.
c.	Height adjustments: Up and down in 6 inch (15.2 cm) increments.
d.	Larger Frames: Require additional bracing for rigidity and long life.
e.	Finish: Clear etched and anodized. Brushed and burr free.
f.	Steel Hardware: To be plated.
5.	Wheeled Polyethylene Carrying Case: Meet Air Transport Association (ATA) Specification 300 standard.
6.	Viewing Surface: Da-Mat. Seamless up to 16 ft (488 cm). Foldable.
7.	Viewing Surface: Da-Tex (Rear). Foldable.
8.	Viewing Surface: HD Progressive ReView 0.9 (Rear). Foldable.
9.	Accessories:
a.	Drapery Presentation Kit. Color: Black.
b.	Drapery Presentation Kit. Color: Blue.
c.	Drapery Presentation Kit. Color: Gray.
d.	Adjustable Skirt Bar: For drapery presentation kits.
e.	Masking Panels: To mask 16:9 formatted screens to 4:3 format.
f.	Da-Mat Foldable Black Backed surface.
2.5	MANUAL PROJECTION SCREENS
A.	Model C as manufactured by Da-Lite. Manual spring roller type projection screen.
1.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
2.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	43 x 57 inches (109 x 145 cm). Diagonal: 72 inches (183 cm).
b.	50 x 67 inches (127 x 170 cm). Diagonal: 84 inches (213 cm).
c.	60 x 80 inches (152 x 203 cm). Diagonal: 100 inches (254 cm).
d.	69 x 92 inches (175 x 234 cm). Diagonal: 120 inches (305 cm).
e.	87 x 116 inches (221 x 295 cm). Diagonal: 150 inches (381 cm).
f.	105 x 140 inches (267 x 356 cm). Diagonal: 180 inches (457 cm).
g.	120 x 160 inches (305 x 406 cm). Diagonal: 200 inches (508 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Square (1:1). Viewing area (HxW).
a.	60 x 60 inches (152 x 152 cm).
b.	70 x 70 inches (178 x 178 cm).
c.	72 x 72 inches (183 x 183 cm).
d.	84 x 84 inches (213 x 213 cm).
e.	96 x 96 inches (244 x 244 cm).
f.	108 x 108 inches (274 x 274 cm).
g.	120 x 120 inches (305 x 305 cm).
h.	144 x 144 inches (366 x 366 cm).
i.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
5.	Screen Surface:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Border Masking: Black.
f.	Border Masking: None.
g.	Screen Fabric Mounting: Permanently attached onto a ball bearing rigid steel spring roller.
6.	Case: 21 gauge steel. Flat back design.
a.	Finish: Powder coated white 
b.	Finish: Powder coated black 
c.	Overall Case Length: Plus or minus 1/4 inch (6 mm).
d.	End Caps: Heavy-duty. Concealing roller ends with steel inner plates to support roller and provide added case strength.
1)	End caps function as sturdy brackets for wall or ceiling installations.
e.	Screen Bottom: Formed into pocket holding tubular metal slat.
1)	Steel Pull Bail: Attached to the slat.
f.	Heavy Duty Plastic Caps: Protect the ends of the slat.
g.	Bumper Stops: Built into case to prevent slat wedging inside case.
h.	Pull Cord: 6 ft with plastic knob.
i.	Extra Drop to lower viewing area more than normal. Maximum Total Surface Height Including Picture Area: 13 ft (396 cm) .
1)	Total Drop at Top: ___ inches (___ cm). Color: Black.
2)	Total Drop at Top: ___ inches (___ cm). Color: White.
3)	Total Drop at Bottom: ___ inches (___ cm). Color: Black.
4)	Total Drop at Bottom: ___ inches (___ cm). Color: White.
7.	Viewing Surface: Matte White.
a.	Horizontal Seam: When both dimensions exceed 10 ft (305 cm).
8.	Viewing Surface: High Contrast Matte White:
a.	Available in sizes where both dimensions do not exceed 10 ft (305 cm).
9.	Accessories:
a.	Extension Brackets: No. 6 wall brackets. 6 inches (15.2 cm) non-adjustable extension from wall. 140 lb. per pair maximum.
1)	Color: White
2)	Color: Black.
b.	Extension Brackets: No. 11 wall brackets. 10 inches (25 cm) or 14 inches (36 cm) non-adjustable extension from wall. 75 lb. per pair maximum.
1)	Color: White
2)	Color: Black.
c.	No. Extension Brackets: No. 23 adjustable wall brackets. 10 inches (25 cm), 14 inches (36 cm), 15.75 inches (40 cm), 18.25 inches (46 cm), 20 inches (51 cm) or 24 inches (61 cm) extension from wall. 75 lb. per pair maximum.
1)	Color: White
2)	Color: Black.
d.	Floating Mounting Bracket: For drywall installations.
1)	Color: Black.
2)	Color: White.
e.	Ceiling Trim Kit.
B.	Model C with CSR as manufactured by Da-Lite. Manual spring roller type projection screen.
1.	Controlled Screen Return (CSR): Controls return speed of screen back into the case.
2.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	43 x 57 inches (109 x 145 cm). Diagonal: 72 inches (183 cm).
b.	50 x 67 inches (127 x 170 cm). Diagonal: 84 inches (213 cm).
c.	60 x 80 inches (152 x 203 cm). Diagonal: 100 inches (254 cm).
d.	69 x 92 inches (175 x 234 cm). Diagonal: 120 inches (305 cm).
e.	87 x 116 inches (221 x 295 cm). Diagonal: 150 inches (381 cm).
f.	105 x 140 inches (267 x 356 cm). Diagonal: 180 inches (457 cm).
g.	120 x 160 inches (305 x 406 cm). Diagonal: 200 inches (508 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
5.	Format: Square (1:1). Viewing area (HxW).
a.	60 x 60 inches (152 x 152 cm).
b.	70 x 70 inches (178 x 178 cm).
c.	72 x 72 inches (183 x 183 cm).
d.	84 x 84 inches (213 x 213 cm).
e.	96 x 96 inches (244 x 244 cm).
f.	108 x 108 inches (274 x 274 cm).
g.	120 x 120 inches (305 x 305 cm).
h.	144 x 144 inches (366 x 366 cm).
i.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
6.	Screen Fabric Mounting: Permanently attached onto a ball bearing rigid steel spring roller.
7.	Case: 21 gauge steel. Flat back design.
a.	Finish: Powder coated white 
b.	Finish: Powder coated black 
c.	Overall Case Length: Plus or minus 1/4 inch (6 mm).
d.	End Caps: Heavy-duty. Concealing roller ends with steel inner plates to support roller and provide added case strength.
1)	End caps function as sturdy brackets for wall or ceiling installations.
e.	Screen Bottom: Formed into pocket holding tubular metal slat.
1)	Steel Pull Bail: Attached to the slat.
f.	Heavy Duty Plastic Caps: Protect the ends of the slat.
g.	Bumper Stops: Built into case to prevent slat wedging inside case.
h.	To be equipped with Controlled Screen Return (CSR) to control the return speed of the back into the case.
i.	Pull Cord: 6 ft with plastic knob.
j.	Extra Drop to lower viewing area more than normal. Maximum Total Surface Height Including Picture Area: 13 ft (396 cm) .
1)	Total Drop at Top: ___ inches (___ cm). Color: Black.
2)	Total Drop at Top: ___ inches (___ cm). Color: White.
3)	Total Drop at Bottom: ___ inches (___ cm). Color: Black.
4)	Total Drop at Bottom: ___ inches (___ cm). Color: White.
8.	Screen Surface:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
9.	Viewing Surface: Matte White.
a.	Horizontal Seam: When both dimensions exceed 10 ft (305 cm).
10.	Viewing Surface: High Contrast Matte White:
a.	Available in sizes where both dimensions do not exceed 10 ft (305 cm).
11.	Accessories:
a.	Extension Brackets: No. 6 wall brackets. 6 inches (15.2 cm) non-adjustable extension from wall. 140 lb. per pair maximum.
1)	Color: White
2)	Color: Black.
b.	Extension Brackets: No. 11 wall brackets. 10 inches (25 cm) or 14 inches (36 cm) non-adjustable extension from wall. 75 lb. per pair maximum.
1)	Color: White
2)	Color: Black.
c.	No. Extension Brackets: No. 23 adjustable wall brackets. 10 inches (25 cm), 14 inches (36 cm), 15.75 inches (40 cm), 18.25 inches (46 cm), 20 inches (51 cm) or 24 inches (61 cm) extension from wall. 75 lb. per pair maximum.
1)	Color: White
2)	Color: Black.
d.	Floating Mounting Bracket: For drywall installations.
1)	Color: Black.
2)	Color: White.
e.	Ceiling Trim Kit.
C.	Basis of Design: Advantage Manual With CSR - Ceiling Recessed as manufactured by Da-Lite. Manual projection screen.
1.	Controlled Screen Return (CSR): Controls return speed of screen back into the case.
2.	Format: HDTV (16:9). Viewing area (HxW).
a.	45 x 80 inches (114 x 203 cm). Diagonal: 92 inches (234 cm).
b.	52 x 92 inches (132 x 234 cm). Diagonal: 106 inches (269 cm).
c.	54 x 96 inches (135 x 244 cm). Diagonal: 110 inches (279 cm).
d.	58 x 104 inches (147 x 264 cm). Diagonal: 119 inches (302 cm).
e.	65 x 116 inches (165 x 295 cm). Diagonal: 133 inches (338 cm).
f.	78 x 139 inches (198 x 353 cm). Diagonal: 159 inches (404 cm).
g.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
3.	Format: Wide (16:10). Viewing area (HxW).
a.	50 x 80 inches (127 x 203 cm). Diagonal: 94 inches (239 cm).
b.	57.5 x 92 inches (146 x 234 cm). Diagonal: 109 inches (277 cm).
c.	60 x 96 inches (152 x 244 cm). Diagonal: 113 inches (287 cm).
d.	65 x 104 inches (165 x 264 cm). Diagonal: 123 inches (312 cm).
e.	69 x 110 inches (175 x 279 cm). Diagonal: 130 inches (330 cm).
f.	72.5 x 116 inches (184 x 295 cm). Diagonal: 137 inches (348 cm).
g.	87 x 139 inches (221 x 353 cm). Diagonal: 164 inches (417 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
4.	Format: Video (NTSC 4:3). Viewing area (HxW).
a.	43 x 57 inches (109 x 145 cm). Diagonal: 72 inches (183 cm).
b.	50 x 67 inches (127 x 170 cm). Diagonal: 84 inches (213 cm).
c.	60 x 80 inches (152 x 203 cm). Diagonal: 100 inches (254 cm).
d.	69 x 92 inches (175 x 234 cm). Diagonal: 120 inches (305 cm).
e.	87 x 116 inches (221 x 295 cm). Diagonal: 150 inches (381 cm).
f.	105 x 140 inches (267 x 356 cm). Diagonal: 180 inches (457 cm).
g.	108 x 144 inches (274 x 366 cm). Diagonal: 180 inches (457 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
5.	Format: Square (1:1). Viewing area (HxW).
a.	60 x 60 inches (152 x 152 cm).
b.	70 x 70 inches (178 x 178 cm).
c.	84 x 84 inches (213 x 213 cm).
d.	96 x 96 inches (244 x 244 cm).
e.	108 x 108 inches (274 x 274 cm).
f.	120 x 120 inches (305 x 305 cm).
g.	144 x 144 inches (366 x 366 cm).
h.	__ x __ inches (__ x __ cm). Diagonal: __ inches (__ cm).
6.	Mounting: Recessed ceiling.
7.	Screen Surface:
a.	Seamless in the image area and mildew resistant.
b.	Front projection surfaces are black backed.
c.	GREENGUARD and GREENGUARD Gold Certified.
d.	Fire retardant.
e.	Borders: Black masking.
f.	Borders: None.
g.	Screen Fabric: Permanently attached to roller.
h.	Bottom: Formed into pocket holding tubular metal slat.
1)	Steel Pull Ball: Attached to the slat.
2)	Heavy-Duty Plastic Caps: Protect the slat ends.
8.	Screen Roller: Ball bearing rigid steel spring roller.
9.	Housing:
a.	Top, Front, and Back: Extruded aluminum.
b.	End Caps: Heavy gauge steel.
c.	Bottom: To have a removable access door.
1)	Self-trimming. Built-in flange around the housing bottom.
d.	Finish: Powder coated. Color: White.
e.	Metal Bumper Stops: Built into housing to prevent the slat from getting wedged in the housing.
f.	To be equipped with Controlled Screen Return (CSR) to control the return speed of the back into the case.
g.	Pull Cord: 6 foot long with plastic knob.
h.	Overall Housing Length: +/- 1/4 inches (6 mm).
10.	For use in environmental air space in accordance with:
a.	Section 300-22 (c) of the National Electric Code.
b.	Sections 2-128, 12-010 (3) and 12-100 of the Canadian Electrical Code, part 1, CSA C22.1.
11.	Viewing Surface: Matte White.
a.	Horizontal Seam: When both dimensions exceed 10 ft (305 cm).
12.	Viewing Surface: High Contrast Matte White:
a.	Available in sizes where both dimensions do not exceed 8 ft (244 cm).
13.	Accessories:
a.	Extra Drop to lower viewing area more than normal. Maximum Total Surface Height Including Picture Area: 13 ft (396 cm).
1)	Total Drop at Top: ___ inches (___ cm). Color: Black.
2)	Total Drop at Top: ___ inches (___ cm). Color: White.
3)	Total Drop at Bottom: ___ inches (___ cm). Color: Black.
4)	Total Drop at Bottom: ___ inches (___ cm). Color: White.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until the substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
3.4	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.
B.	Manufacturer's Services: Coordinate manufacturer's services in accordance with appropriate sections in Division 01.
3.5	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturers recommendations.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION