SECTION 06 15 00

CONCEALED DECK FASTENERS AND ACCESSORIES

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2018 -  2018 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Hidden Deck Fasteners.
B.	Deck Screws.
C.	Wood Care Products.
D.	Deck Tools.
E.	Deck Accessories.
F.	Deck Tile Systems.
G.	Deck Tile Pedestals.
H.	Rainscreen Siding Clips.
I.	Deck Cable Railing.
1.2	RELATED SECTIONS
A.	Section 03 30 00 - Cast-in-Place Concrete.
B.	Section 04 27 23 - Cavity Wall Unit Masonry.
C.	Section 06 10 00 - Rough Carpentry.
D.	Section 06 20 00 - Finish Carpentry.
E.	Section 09 90 00 - Painting and Coating.
1.3	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings: Shop Drawings: Include details of construction and all materials.
D.	FSC Submittals: Provide documentation indicating manufacturer is FSC Chain-of-Custody certified.
E.	Verification Samples: For each finish product specified, two samples, minimum size 6 inches (150 mm) long, representing actual product, and color.
F.	Manufacturer's Certificates: Certify products meet or exceed specified requirements.
G.	Closeout Submittals: Provide manufacturer's maintenance instructions that include recommendations for periodic cleaning and maintenance of all components.
1.4	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with minimum 5 years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum 2 years documented experience.
C.	Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
1.	Finish areas designated by Architect.
2.	Do not proceed with remaining work until workmanship is approved by Architect.
3.	Rebuild mock-up area as required to produce acceptable work.
4.	Accepted mock-up shall be comparison standard for remaining Work.
1.5	DELIVERY, STORAGE, AND HANDLING
A.	Deliver and store products in manufacturer's unopened packaging bearing the brand name and manufacturer's identification until ready for installation.
B.	Protect from soiling, damage and construction operations. Allow for proper on site acclimation of wood materials.
1.6	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: DeckWise USA , which is located at:<BR />2111 58th Ave. E.<BR />Bradenton, FL  34203 <BR />Toll Free Tel: 866-427-2547 <BR />Tel: 941-896-9851	<BR />Email: request info (rkabel@deckwise.com);Web: https://www.deckwise.com | https://www.wisebond.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	HIDDEN DECK FASTENERS
A.	EXTREME Series Hidden Deck Fastener Clips by DeckWise: Malleable plastic with stainless steel insert:
1.	Made in the USA.
2.	Limited lifetime warranty.
3.	Casing: Virgin polypropylene resin, resistant to UV.
4.	Insert: Stainless steel with black oxide coating.
5.	Symmetrical edge groove for better board surface selections.
6.	Allows for expansion of width of hardwoods.
7.	Allows movement of length of composite and PVC decking.
8.	Unique square biscuit design ensures more contact surface area inside slot groove.
9.	Screws installed at 45 degrees provide maximum holding strength for hardwood decking.
10.	Screws installed straight down for composite and PVC decking allow these materials to naturally move on their length.
11.	Size: 1.0 x 1.0 x 0.390 inch (25.4 x 25.4 x 9.9 mm).
12.	Stainless Steel Insert: 0.883 x 0.883 x .036 inch (22.4 x 22.4 x 0.9 mm).
B.	Basis of Design: Ipe Clip EXTREME Hidden Deck Fastener Clip by DeckWise: Malleable plastic with stainless steel insert:
1.	Integrated spacer leg spaces deck boards at 3/32 inch (2.4 mm).
2.	For use with air-dried hardwood, composite, or PVC decking.
3.	Complete Kit Including:
a.	Fasteners: (175) Ipe Clip EXTREME Hidden Deck Fasteners.
b.	Screws: (190) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Plugs: (12) 3/8 inch tapered Ipe Plugs.
d.	Drill Bit: (1) 1/8 inch high speed drill bit.
e.	Drive Tip: (1) T15 star drive tip.
f.	Instruction sheet.
4.	100 Ct. Kit Including:
a.	Fasteners: (100) Ipe Clip EXTREME Hidden Deck Fasteners.
b.	Screws: (100) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Instruction sheet.
5.	2 Gal. Contractor Bucket Including:
a.	Fasteners: (525) Ipe Clip EXTREME Hidden Deck Fasteners.
b.	Screws: (565) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Drill Bit: (3) 1/8 inch high speed drill bit.
d.	Drive Tip: (3) T15 star drive tip.
e.	Instruction sheet.
6.	5 Gal. Contractor Bucket Including:
a.	Fasteners: (1050) Ipe Clip EXTREME Hidden Deck Fasteners.
b.	Screws: (1130) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Drill Bit: (5) 1/8 inch high speed drill bit.
d.	Drive Tip: (5) T15 star drive tip.
e.	Instruction sheet.
7.	Color: Shadowline Black.
8.	Color: Hardwood Brown.
9.	Color: Composite Grey.
10.	Color: To be selected by Architect.
C.	Basis of Design: Ipe Clip EXTREME-4 Hidden Deck Fastener Clip by DeckWise: Malleable plastic with stainless steel insert:
1.	Integrated spacer leg spaces deck boards at 5/32 inch (4 mm).
2.	For use with air-dried hardwood, kiln-dried hardwood, composite, or thermal wood decking.
3.	Complete Kit Including:
a.	Fasteners: (175) Ipe Clip EXTREME-4 Hidden Deck Fasteners.
b.	Screws: (190) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Plugs: (12) 3/8 inch tapered Ipe Plugs.
d.	Drill Bit: (1) 1/8 inch high speed drill bit.
e.	Drive Tip: (1) T15 star drive tip.
f.	Spacer Tools: (3) 5/32 inch spacer tools.
g.	Instruction sheet.
4.	100 Ct. Kit Including:
a.	Fasteners: (100) Ipe Clip EXTREME-4 Hidden Deck Fasteners.
b.	Screws: (100) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Spacer Tools: (3) 5/32 inch spacer tools.
d.	Instruction sheet.
5.	2 Gal. Contractor Bucket Including:
a.	Fasteners: (525) Ipe Clip EXTREME-4 Hidden Deck Fasteners.
b.	Screws: (565) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Drill Bit: (3) 1/8 inch high speed drill bit.
d.	Drive Tip: (3) T15 star drive tip.
e.	Spacer Tools: (6) 5/32 inch spacer tools.
f.	Instruction sheet.
6.	5 Gal. Contractor Bucket Including:
a.	Fasteners: (1050) Ipe Clip EXTREME-4 Hidden Deck Fasteners.
b.	Screws: (1130) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Drill Bit: (5) 1/8 inch high speed drill bit.
d.	Drive Tip: (5) T15 star drive tip.
e.	Spacer Tools: (6) 5/32 inch spacer tools.
f.	Instruction sheet.
7.	Color: Shadowline Black.
8.	Color: Hardwood Brown.
9.	Color: Composite Grey.
10.	Color: To be selected by Architect.
D.	Basis of Design: Ipe Clip EXTREME-KD Hidden Deck Fastener Clip by DeckWise: Malleable plastic with stainless steel insert:
1.	Integrated spacer leg spaces deck boards at 1/4 inch (6.4 mm).
2.	For use with kiln-dried hardwood, composite, or thermal wood decking.
3.	Hollow legs act as shock absorbers as kiln-dried materials expand.
4.	Complete Kit Including:
a.	Fasteners: (175) Ipe Clip EXTREME-KD Hidden Deck Fasteners.
b.	Screws: (190) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Plugs: (12) 3/8 inch tapered Ipe Plugs.
d.	Drill Bit: (1) 1/8 inch high speed drill bit.
e.	Drive Tip: (1) T15 star drive tip.
f.	Spacer Tools: (3) 1/4 inch spacer tools.
g.	Instruction sheet.
5.	100 Ct. Kit Including:
a.	Fasteners: (100) Ipe Clip EXTREME-KD Hidden Deck Fasteners.
b.	Screws: (100) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Spacer Tools: (3) 1/4 inch spacer tools.
d.	Instruction sheet.
6.	2 Gal. Contractor Bucket Including:
a.	Fasteners: (525) Ipe Clip EXTREME-KD Hidden Deck Fasteners.
b.	Screws: (565) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Drill Bit: (3) 1/8 inch high speed drill bit.
d.	Drive Tip: (3) T15 star drive tip.
e.	Spacer Tools: (6) 1/4 inch spacer tools.
f.	Instruction sheet.
7.	5 Gal. Contractor Bucket Including:
a.	Fasteners: (1050) Ipe Clip EXTREME-KD Hidden Deck Fasteners.
b.	Screws: (1130) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Drill Bit: (5) 1/8 inch high speed drill bit.
d.	Drive Tip: (5) T15 star drive tip.
e.	Spacer Tools: (6) 1/4 inch spacer tools.
f.	Instruction sheet.
8.	Color: Shadowline Black.
9.	Color: Hardwood Brown.
10.	Color: Composite Grey.
11.	Color: To be selected by Architect.
E.	Basis of Design: Standard Ipe Clip Hidden Deck Fastener Clip by DeckWise: Malleable plastic:
1.	Integrated spacer leg spaces deck boards at 3/32 inch (2.4 mm).
2.	For use with air-dried hardwood, composite, or thermal wood decking.
3.	Made in the USA.
4.	Limited lifetime warranty.
5.	Casing: Virgin polypropylene resin, resistant to UV.
6.	Symmetrical edge groove for better board surface selections.
7.	Allows for expansion of width of hardwoods.
8.	Allows movement of length of composite and PVC decking.
9.	Screws installed at 45 degrees provide maximum holding strength for hardwood decking.
10.	Screws installed straight down for composite and PVC decking allow these materials to naturally move on their length.
11.	Size: 1.0 inch diameter x 0.390 inch (25.4 mm diameter x 9.9 mm).
12.	Complete Kit Including:
a.	Fasteners: (175) Ipe Clip Standard Hidden Deck Fasteners.
b.	Screws: (190) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Plugs: (12) 3/8 inch tapered Ipe Plugs.
d.	Drill Bit: (1) 1/8 inch high speed drill bit.
e.	Drive Tip: (1) T15 star drive tip.
f.	Instruction sheet.
13.	100 Ct. Kit Including:
a.	Fasteners: (100) Ipe Clip Standard Hidden Deck Fasteners.
b.	Screws: (100) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Spacer Tools: (3) 5/32 inch spacer tools.
d.	Instruction sheet.
14.	2 Gal. Contractor Bucket Including:
a.	Fasteners: (525) Ipe Clip Standard Hidden Deck Fasteners.
b.	Screws: (565) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Drill Bit: (3) 1/8 inch high speed drill bit.
d.	Drive Tip: (3) T15 star drive tip.
e.	Instruction sheet.
15.	5 Gal. Contractor Bucket Including:
a.	Fasteners: (1050) Ipe Clip Standard Hidden Deck Fasteners.
b.	Screws: (1130) #8 x 2 inch colormatch black stainless steel star drive screws.
c.	Drill Bit: (5) 1/8 inch high speed drill bit.
d.	Drive Tip: (5) T15 star drive tip.
e.	Instruction sheet.
16.	Color: Shadowline Black.
17.	Color: Hardwood Brown.
18.	Color: Composite Grey.
19.	Color: To be selected by Architect.
2.3	DECK SCREWS
A.	#8 Trim-Head Stainless Steel Deck Screws: T15 stainless steel #8 trim-head deck screws.
1.	Type 17 point for ease of wood penetration.
2.	Material: 305 grade stainless steel.
3.	Material: 316 grade stainless steel.
4.	Head: T15 star drive finish heads.
5.	Length: 1 inch.
6.	Length: 1-1/2 inch.
7.	Length: 2 inch.
8.	Length: 2-1/2 inch.
9.	Length: 3-1/8 inch.
10.	Length: As indicated on Drawings.
11.	Color: Shadowline Black.
12.	Color: Hardwood Brown.
13.	Color: Stainless Steel.
14.	Color: Cedar.
15.	Color: Rosy Brown.
16.	Color: Outdoor Grey.
17.	Color: To be selected by Architect.
B.	#10 Bugle-Head Stainless Steel Deck Screws: T25 stainless steel #10 bugle-head deck screws.
1.	Double countersink flat bugle head with 6 nibs.
2.	6 lobe star drive reduces cam-out and increases torque.
3.	Chipboard thread screw with partial thread and triple spline.
4.	Type 17 point for ease of wood penetration.
5.	Material: 305 grade stainless steel.
6.	Material: 316 grade stainless steel.
7.	Head: T25 star drive finish heads.
8.	Length: 2-1/2 inch.
9.	Length: 3-1/8 inch.
10.	Length: As indicated on Drawings.
11.	Color: Hardwood Brown.
12.	Color: Stainless Steel.
13.	Color: Cedar.
14.	Color: Outdoor Grey.
15.	Color: To be selected by Architect.
C.	#10 Composite Stainless Steel Deck Screws: T20 stainless steel #10 star drive deck screws.
1.	Advanced type 17 point for ease of wood penetration.
2.	Reverse threads below head eliminate mushrooming of composite deck.
3.	Dual threads compress dust and pull decking tight to joists.
4.	Material: 305 grade stainless steel.
5.	Head: T20 star drive finish heads.
6.	Length: 2-1/2 inch.
7.	Color: Hardwood Brown.
8.	Color: Rosy Brown.
9.	Color: Cedar.
10.	Color: Composite Grey.
11.	Color: Composite Sand.
12.	Color: To be selected by Architect.
D.	#8 Heat-Treated Stainless Steel Deck Screws: T15 heat-treated stainless steel #8 self-drilling deck screws.
1.	Reduces stripping and snapping.
2.	Easy installation with TTAP T15 star drive.
3.	Type 17 point for ease of wood penetration.
4.	Material: 18-8 grade stainless steel.
5.	Serrated saw threads to remove sawdust.
6.	Length: 1-3/4 inch.
7.	Length: 2 inch.
8.	Length: As indicated on Drawings.
E.	#7 Self-Tapping Metal Joist Stainless Steel Deck Screws: Designed for metal joist applications.
1.	Specially engineered #3 drill point to penetrate metal joists with ease.
2.	Head: T15 star drive.
3.	Xylan coated for corrosion resistance.
4.	Material: 410 grade stainless steel.
5.	Auger tip for self-tapping.
6.	Length: 1-5/8 inch.
7.	Length: 2-1/4 inch.
8.	Length: As indicated on Drawings.
9.	Color: Shadowline Black.
10.	Color: Hardwood Brown.
11.	Color: Stainless Steel.
12.	Color: To be selected by Architect.
2.4	WOOD CARE PRODUCTS
A.	Basis of Design: Ipe Oil Harwood Oil Finish with UV Protectant by DeckWise: Oil-based natural hardwood finish for decking and siding.
1.	For use with exotic hardwoods and thermal woods.
2.	Exceptional penetration.
3.	Natural grain enhancement.
4.	Water repellant.
5.	Low VOC, maximum 250 g/L.
6.	Non-film forming.
7.	Inhibits mold, mildew, rot, and decay.
8.	Allows hardwoods to breath naturally.
9.	Provides UV protection.
10.	Reduces chance of warps and cracks.
11.	Made in the USA.
B.	Basis of Design: DeckWise WiseCoat Premium Hardwood Deck, Siding, and Fence Sealer by DeckWise: Zero-VOC, non-toxic waterproofing sealant for use on hardwood decking, siding, and fencing surfaces.
1.	Protects, preserves, and enhances all types of South American exotic hardwoods, American hardwoods, and most thermally modified wood.
2.	Guaranteed to prevent excessive water accumulation below the wood surface for up to six years on horizontal surfaces and up to 10 years on vertical surfaces.
3.	Amber tint for UV protection.
4.	Zero VOC.
5.	Non-toxic.
6.	Eco-friendly and harmless to plants, pets, and people.
7.	Odorless and non-flammable.
8.	Exceptional penetration at the cellular level.
9.	Non-film forming.
10.	Inhibits mold, mildew, rot, and decay.
11.	Allows hardwoods to breath naturally.
12.	Reduces chance of warps and cracks.
13.	Made in the USA.
C.	Basis of Design: Ipe Seal Hardwood End Grain Sealant by DeckWise: Seals ends of logs and lumber to protect against degradation during air-drying.
1.	For use with exotic hardwoods and thermal woods.
2.	Prevents joint swelling of composite decking material.
3.	Non-hazardous wax emulsion.
4.	Dries to the touch in 1-2 hours.
5.	Soap and water clean up.
6.	Not for use on walking surfaces.
7.	Made in the USA.
D.	Basis of Design: Deck and Wood Cleaner (Part 1) and Deck and Wood Brightener (Part 2) by DeckWise: Cleanses and brightens exterior wood.
1.	Removes surface dirt, mold, and mildew.
2.	Preps wood for finishing.
3.	Eliminates tannin stains.
4.	Biodegradable, easy to handle, and safe.
5.	Concentrated powders provide maximum strength. 
6.	Made in the USA.
E.	Basis of Design: Hardwood Deck and Siding Restoration All-in-One Kit by DeckWise: Includes:
1.	1 Gallon Ipe Oil Hardwood Finish.
2.	16 oz. DeckWise Deck and Wood Cleaner (Part 1).
3.	16 oz. DeckWise Deck and Wood Brightener (Part 2).
4.	1 Merit Pro 9 inch (22.9 cm) bright metal paint tray.
5.	1 Merit Pro 9 inch (22.9 cm) 5 wire roller frame with black handle.
6.	1 Merit Pro 9 inch (22.9 cm) x 3/8 inch (9.5 mm) woven roller cover.
7.	1 Merit Pro 2 inch (5.08 cm) painter's beavertail handle varnish brush.
8.	1 Merit Pro paint can opener. 
9.	3 American Paint paddle 12 inch (30.5 cm).
10.	10 Scott white pro rags.
2.5	DECK TOOLS
A.	Basis of Design: Hardwood Wrench Deck Board Straightener by DeckWise:
1.	Pushing Force: 1,100 lbs.
2.	Cam:
a.	Locks and holds planks in place.
b.	Aircraft grade anodized aluminum.
3.	Gripping Pins:
a.	Knurled stainless steel pins grip joists and furring strips.
b.	Long and short adjustable.
4.	Handle: American Ash wood, reverses to right or left hands.
5.	10 adjustable configurations to work in any space.
6.	Made in USA.
B.	Basis of Design: Drill & Drive by DeckWise: Rapid change drill bit set, includes:
1.	Quick change locking collar.
2.	(5) 3/8 inch countersink bits.
3.	(5) 1/8 inch drill bits.
4.	On-board hex key.
5.	(5) T15 star drive tips.
6.	Convenient carry case.
7.	Made in USA.
C.	Basis of Design: WiseGuides Deck Board Gap Spacer Tool by DeckWise: 
1.	Material: Hard plastic polymer resin for resistance and rigidity.
2.	Profile: V-shape to facilitate fitting and fast removal.
3.	Color coded spacer wedge sizes for easy use.
4.	Large grip blade guarantees ample resistance.
5.	Large handle opening allows easy access for fingers.
6.	Anti-marking ribs reduce plank contact surface.
7.	Made in USA.
8.	Gap Size: 1/8 inch.
9.	Gap Size: 5/32 inch.
10.	Gap Size: 13/64 inch.
11.	Gap Size: 1/4 inch.
12.	Gap Size: 5/16 inch.
D.	Basis of Design: DeckWise Router Bits by DeckWise: For use with handheld or table router:
1.	5/32 inch 4-wing cutter bit.
2.	Arbor Size: 1/4 inch diameter.
3.	Arbor Size: 1/2 inch diameter.
4.	Blade Diameter: 1-7/8 inches.
5.	Slot Width: 5/32 inch.
6.	Slot Depth: 1/2 inch.
E.	Basis of Design: DeckWise Premium Hardwood Plug Cutter by DeckWise: 
1.	Size: 3/8 inch.
2.	Size: 1/2 inch.
3.	Anti-skate design.
4.	Extra sharp cutting teeth.
5.	Made in USA.
2.6	DECK ACCESSORIES
A.	Basis of Design: Hardwood Plug Kit Complete System by DeckWise:
1.	Kit Includes:
a.	DeckWise Drill & Drive kit.
b.	Gorilla Glue, 4 ounce bottle.
c.	Hardwood plugs.
d.	Stainless steel trim-head screws.
2.	Quantity: 350 plugs and 350 screws.
3.	Quantity: 1050 plugs and 1050 screws.
4.	Design: Smooth tapered plugs.
a.	Size: 3/8 inch diameter.
b.	Species: Cumaru.
c.	Species: Tigerwood.
d.	Species: Ipe.
e.	Species: Massaranduba.
5.	Design: Extreme ribbed plugs.
a.	Manufactured with Tolerance Absorbing Rings to help fill the void in a hole that is not drilled perfectly round.
b.	Size: 3/8 inch diameter.
c.	Size: 10 mm diameter.
d.	Size: 12 mm diameter.
e.	Species: Cumaru.
f.	Species: Tigerwood.
g.	Species: Ipe.
h.	Species: Garapa.
i.	Species: Massaranduba.
B.	Basis of Design: WiseWrap JoistTape by DeckWise:
1.	Malleable polyethylene waterproof wood flashing material, using a rubberized asphalt mastic adhesive. 
2.	Roll Size: 3 inch wide by 75 feet long. 
3.	Thickness: 35-40 mil.
4.	Waterproof barrier protection.
5.	Prevents water intrusion between surfaces.
6.	Self-seals around screws.
7.	Prevents wood rot.
8.	Extends life of deck and joists.
9.	Corrosion blocker.
10.	Reduces noise.
11.	Made in USA.
C.	Basis of Design: WiseWrap LedgerTape by DeckWise:
1.	Malleable polyethylene waterproof wood flashing material, using a rubberized asphalt mastic adhesive. 
2.	Roll Size: 12 inch wide by 25 feet long. 
3.	Thickness: 35-40 mil.
4.	Waterproof barrier protection.
5.	Prevents water intrusion between surfaces.
6.	Self-seals around lags, bolts, and screws.
7.	Prevents wood rot.
8.	Extends life of ledger board.
9.	Corrosion blocker.
10.	Made in USA.
2.7	DECK TILE SYSTEMS
A.	Basis of Design: WiseTile Hardwood Deck Tiles by DeckWise: Modular solid hardwood tiles:
1.	Responsibly harvested.
2.	Assembled with stainless steel screws.
3.	100 percent all-natural, chemical-free hardwood.
4.	Low-maintenance and naturally resistant to mold, decay, and insects.
5.	Simple to remove, rearrange, and lay in new locations.
6.	Proven to last in extreme hot, dry, wet, and cold climates.
7.	Interchangeable patterns.
8.	Tile Size: 12 x 12 inches.
9.	Tile Size: 20 x 20 inches.
10.	Tile Size: 24 x 24 inches.
11.	FSC Certified.
12.	Species: Ipe.
13.	Species: Cumaru.
14.	Species: Tigerwood.
15.	Species: Massaranduba.
B.	Basis of Design: WiseTile Deck Tiles Connectors by DeckWise: Polyethylene connectors:
1.	Material: Chemical and UV resistant polyethylene resin.
2.	Integrated 3/16 inch gap spacers.
3.	Fasteners: 4 fasteners fit into bottom of deck tile.
4.	Corner pins secure tile placement.
5.	Pre-formed countersunk holes for attaching to substrates.
6.	Elevates deck tile above substrate.
7.	Easily divided into halves or quarters.
8.	Center drain hole provides runoff.
9.	Matte finish for enhanced appearance.
10.	Made in USA.
11.	Color: Shadowline Black.
12.	Color: Hardwood Brown.
13.	Color: Concrete Grey.
C.	Basis of Design: Hardwood Deck Tile Edge Trim by DeckWise:
1.	Predrilled to accept DeckWise Deck Tile Connectors.
2.	1/4 inch spacer in middle of trim piece for additional support.
3.	Tile Size: 12 x 12 inches.
4.	Tile Size: 20 x 20 inches.
5.	Tile Size: 24 x 24 inches.
6.	FSC Certified.
7.	Species: Ipe.
8.	Species: Cumaru.
9.	Species: Tigerwood.
10.	Species: Massaranduba.
11.	Responsibly harvested.
12.	Solid hardwood straight and mitered corner pieces.
13.	100 percent all-natural, chemical-free hardwood.
14.	Low-maintenance and naturally resistant to mold, decay, and insects.
15.	Simple to remove, rearrange, and lay in new locations.
16.	Proven to last in extreme hot, dry, wet, and cold climates.
2.8	DECK TILE PEDESTALS
A.	Basis of Design: DeckWise Altitudes Pedestal System by DeckWise: Elevates and levels structural 24 x 24 inch hardwood tiles over sloped or uneven surfaces:
1.	Minimum Height: 4-5/32 inches.
2.	Minimum Height: 2-21/32 inches.
3.	Minimum Height: 1-1/2 inches.
4.	Utilizes 4 inch diameter Schedule 40 PVC pipe.
5.	Base Type: Screw-jack base.
6.	Base Type: Non-screw-jack base.
7.	Head Type: Adjustable self-leveling head, compensates for slopes from 0 to 5 percent slope.
8.	Head Type: Stationary head.
9.	Heads have integrated gap spacers and corner fasteners.
10.	Heads and bases have pre-formed drainage holes.
11.	Maximum safe deck tile pedestal height: 24 inches.
12.	Warranted Live Load: 1,200 pounds.
13.	Resistant to freeze thaw cycles.
14.	20 percent talc added to polypropylene resin.
15.	Made in USA.
B.	Basis of Design: Lockit Down Washer by DeckWise: Locks hardwood deck tiles to the top of each pedestal when inserted into the corner kerf of deck tile:
1.	Material: Black oxide coated 305 grade stainless steel insert with glass-filled nylon plastic resin shell.
2.	Oblong center hole in washer allows easy installation.
3.	Screws: 3/32 inch screw included with washer.
4.	Hex Wrench: 3/32 inch hex wrench included in packaging.
5.	Made in USA.
2.9	RAINSCREEN SIDING CLIPS
A.	Basis of Design: DeckWise Hidden Siding Fasteners by DeckWise:
1.	Works with most 5/4 rainscreen hardwood siding profiles.
2.	Comes with 2 installation screw holes to allow for vertical, horizontal, and diagonal siding installation.
3.	Material: 304 grade stainless steel.
4.	No visible fasteners on the surface.
5.	Includes 305 grade stainless steel T15 #8 x 2 inch screws.
6.	Screws installed at 45 degree angle for added hold-down.
7.	Includes 304 grade stainless steel starter clips.
8.	Includes T15 star driver tips.
9.	Made in USA.
2.10	CABLE RAILING COMPONENTS
A.	Basis of Design: WiseRail 316 Grade Stainless Steel Deck Cable Railing System: 
1.	Pre-swaged cable ends for quick installations.
2.	Hardware: 316 grade stainless steel fittings.
3.	Fittings and Tensioners: Inside to inside.
4.	Fittings and Tensioners: Outside to outside.
5.	Length: 5 feet.
6.	Length: 10 feet.
7.	Length: 15 feet.
8.	Length: 20 feet.
9.	Length: 25 feet.
10.	Length: 30 feet.
11.	Length: 40 feet.
12.	Length: 50 feet.
13.	Unobstructed outward looking view.
14.	Patented push and pull locks including adjustable bodies.
15.	Virtually maintenance free with no painting.
16.	For use on hardwood decking with 4 x 4 inch wood posts.
17.	Warranty: 10 years.
18.	Made in USA.
B.	Pre-Packaged Kits: Basis of Design: WiseRail Pre-Packaged 316 Stainless Steel Deck Cable Rail Kits: 
1.	Kit Includes:
a.	Hardware fittings for ends.
b.	All necessary fasteners and washers.
c.	1/8 inch diameter 1x19 Type 316 stainless steel cable.
d.	Installation instructions.
2.	Kit: WiseRail WiseCable Legacy WC-LS: Cable railing on level straight runs.
3.	Kit: WiseRail WiseCable Legacy WC-LSS: Cable railing on a pitch or stair.
4.	Kit: WiseRail WiseCable Estate WC-ES: Cable railing on level straight runs.
5.	Kit: WiseRail WiseCable Estate WC-ES: Cable railing on a pitch or stair.
6.	Kit: WiseRail WiseCable Heritage WC-HS: Cable railing on level straight runs.
7.	Kit: WiseRail WiseCable Heritage WC-HS: Cable railing on a pitch or stair.
8.	Length: 5 feet.
9.	Length: 10 feet.
10.	Length: 15 feet.
11.	Length: 20 feet.
12.	Length: 25 feet.
13.	Length: 30 feet.
14.	Length: 40 feet.
15.	Length: 50 feet.
C.	Cable Rail Accessories: 
1.	Made in USA.
2.	Stainless steel post protector tube.
3.	Cable release key.
4.	Stainless steel crown end cap.
5.	Cut-off tool.
6.	Light-duty cable cutter.
7.	Heavy-duty cable cutter.
8.	Cable gripping pliers.
9.	Cable release key.
10.	Light-duty hanger bolt driver.
11.	Anodized aluminum cable brace.
12.	Anodized aluminum cable brace for stairs.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	Verify support framing is ready to receive decking. If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation. Coordinate placement of bearing or support items.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, approved submittals and in proper relationship with adjacent construction. Install accessories as recommended by manufacturer.
3.4	CLEANING AND PROTECTION
A.	Protect installed products until completion of project.
B.	Protect from damage during construction operations. Promptly repair any damaged surfaces. Remove and replace work which cannot be satisfactorily repaired.
C.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION