SECTION 12 93 13

BICYCLE RACKS AND LOCKERS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2016 -  2024 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Bicycle racks of the following types:
1.	Bike Hitch.
2.	Hoop Rack.
3.	Hoop Rack Heavy Duty.
4.	Swerve Rack.
5.	Downtown Rack.
6.	Round Rack.
7.	Arc Rack.
8.	Cycle Dock.
9.	Bike Bike Rack.
10.	Campus Rack.
11.	Ultra Space Saver Squared.
12.	Ultra Space Saver Single.
13.	Bike File.
14.	Dero Decker.
15.	Dero Duplex.
16.	Wall Rack.
B.	Bicycle accessories of the following types:
1.	Fixit Plus.
2.	Air Kit Prime
3.	Air Kit 4.
C.	Bicycle shelters of the following types:
1.	Kolo Shelter.
2.	Cycle Station.
3.	Vizor Shelter.
4.	Pocket Shelter.
D.	Bicycle lockers of the following types:
1.	Dero Locker.
2.	Veloport.
E.	Bicycle parking system: 
1.	Cycle Stall Basic.
F.	Electric bike charging racks.
1.	eBeam.
2.	eDowntown.
3.	eHitch.
4.	eSwerve.
1.2	RELATED SECTIONS
A.	Section 31 20 00 - Earth Moving.
B.	Section 33 40 00 - Stormwater Utilities.
C.	Section 12 93 13 - Bicycle Racks.
D.	Section 03 30 00 - Cast-in-Place Concrete.
1.3	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's product literature and technical data, including physical characteristics such as shape, dimensions, bicycle parking capacity, and finish for each product.
C.	Shop Drawings: Show installation details for each product.
D.	Samples for Verification: Submit finish samples for review and verification. 
E.	Maintenance Data: For each bicycle rack. Include recommended methods for repairing damage to the finish
1.4	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Minimum 2 years manufacturing similar products.
B.	Installer Qualifications: An experienced installer who has completed installation of products similar in material, design, and extent to that indicated for this project.
C.	Source Limitations: Obtain each color, finish, shape and type of product from a single source with resources to provide components of consistent quality in appearance and physical properties.
D.	Product Options: Drawings indicate size, shape and dimensional requirements of bicycle racks and are based on the specific system indicated.
1.5	DELIVERY, STORAGE, AND HANDLING
A.	Comply with manufacturer's recommendations.
B.	Upon delivery, before signing for shipment, inspect for any damages and notate on the B.O.L.
C.	Store products in original undamaged packages and containers until ready for installation.
1.6	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.7	WARRANTY
A.	Provide manufacturer's standard limited warranty against defects in materials and workmanship. 
1.	Bicycle racks carry a one year manufacturer's limited warranty against defects in materials and workmanship. The one year warranty period begins the date the product is shipped from the manufacturer.
2.	The air pump for the Dero Air Kits have limited operating temperatures ranges from -30 to 120 degrees F (minus 1 to 49 degrees C).
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Dero Bike Rack Co., a PlayCore Company, which is located at:<BR />5522 Lakeland Ave. N.<BR />Minneapolis, MN 55429<BR />Toll Free Tel: 888-337-6729<BR />Email: request info (sales@dero.com);Web: http://www.dero.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	BICYCLE RACKS
A.	Bike Hitch:
1.	Capacity: 2 bicycles.
2.	Center Beam: 2 inch diameter schedule 40 pipe.
3.	Ring: 1-1/2 inch O.D. 11 gauge tube.
4.	Logo: Custom logo, design to be provided by Architect.
5.	Logo: ______ 
6.	Logo: Custom logo as indicated on Drawings.
7.	Mounting: Surface-mounted.
8.	Mounting: In-ground mounted.
9.	Finish: Hot-dip galvanized.
10.	Finish: Stainless steel, 304 grade, with No. 4 finish and Spectra Shield.
11.	Finish: Stainless steel, 304 grade, with high luster electropolish finish and Spectra Shield.
12.	Finish: PVC dip.
13.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______
f.	Color: As indicated on Drawings.
B.	Hoop Rack:
1.	Capacity: 2 bicycles.
2.	Pipe: 1-1/2 inch schedule 40 pipe, 1.90 inch O.D.
3.	Logo: Custom logo, design to be provided by Architect.
4.	Logo: ______ 
5.	Logo: Custom logo as indicated on Drawings.
6.	Mounting: Surface-mounted.
7.	Mounting: In-ground mounted.
8.	Mounting: Rail rack: Hoops to be bolted to two parallel rails.
a.	Rail Material: AISI C3 x 4.1 steel channels.
9.	Finish: Hot-dip galvanized.
10.	Finish: Stainless steel, 304 grade, with No. 4 finish and Spectra Shield.
11.	Finish: Stainless steel, 304 grade, with high luster electropolish finish and Spectra Shield.
12.	Finish: PVC dip.
13.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
C.	Heavy Duty Hoop Rack:
1.	Capacity: 2 bicycles.
2.	Pipe: 2 inch schedule 40 pipe.
3.	Logo: Custom logo, design to be provided by Architect.
4.	Logo: ______ 
5.	Logo: Custom logo as indicated on Drawings.
6.	Mounting: Surface-mounted.
7.	Mounting: In-ground mounted.
8.	Mounting: Rail rack: Hoops to be bolted to two parallel rails.
a.	Rail Material: AISI C3 x 4.1 steel channels.
9.	Finish: Hot-dip galvanized.
10.	Finish: Stainless steel, 304 grade, with No. 4 finish and Spectra Shield.
11.	Finish: Stainless steel, 304 grade, with high luster electropolish finish and Spectra Shield.
12.	Finish: PVC dip.
13.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
D.	Swerve Rack:
1.	Capacity: 2 bicycles.
2.	Pipe: 1-1/2 inch schedule 40 pipe, 1.90 inch O.D.
3.	Logo: Custom logo, design to be provided by Architect.
4.	Logo: ______ 
5.	Logo: Custom logo as indicated on Drawings.
6.	Mounting: Surface-mounted.
7.	Mounting: In-ground mounted.
8.	Mounting: Rail rack: Hoops to be bolted to two parallel rails.
a.	Rail Material: AISI C3 x 4.1 steel channels.
9.	Finish: Hot-dip galvanized.
10.	Finish: Stainless steel, 304 grade, with No. 4 finish and Spectra Shield.
11.	Finish: Stainless steel, 304 grade, with high luster electropolish finish and Spectra Shield.
12.	Finish: PVC dip.
13.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
E.	Downtown Rack:
1.	Capacity: 2 bicycles.
2.	Square Tube: Mild steel, 2 inch (51 mm), 3/16 inch (55 mm) square tube.
3.	Square Tube: Stainless steel, 2 inch (51 mm), 11 gauge square tube.
4.	Logo: Custom logo, design to be provided by Architect.
5.	Logo: ______ 
6.	Logo: Custom logo as indicated on Drawings.
7.	Mounting: Surface-mounted.
8.	Mounting: In-ground mounted.
9.	Mounting: Rail rack: Hoops to be bolted to two parallel rails.
a.	Rail Material: AISI C3 x 4.1 steel channels.
10.	Finish: Hot-dip galvanized.
11.	Finish: Stainless steel, 304 grade, with No. 4 finish and Spectra Shield.
12.	Finish: Stainless steel, 304 grade, with high luster electropolish finish and Spectra Shield.
13.	Finish: PVC dip.
14.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
F.	Round Rack:
1.	Capacity: 2 bicycles.
2.	Pipe: 1-1/2 inch pipe.
3.	Logo: Custom logo, design to be provided by Architect.
4.	Logo: ______ 
5.	Logo: Custom logo as indicated on Drawings.
6.	Mounting: Surface-mounted.
7.	Mounting: In-ground mounted.
8.	Finish: Hot-dip galvanized.
9.	Finish: Stainless steel, 304 grade, with No. 4 finish and Spectra Shield.
10.	Finish: Stainless steel, 304 grade, with high luster electropolish finish and Spectra Shield.
11.	Finish: PVC dip.
12.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
G.	Arc Rack:
1.	Capacity: 2 bicycles.
2.	Tube: 2 inch by 11 gauge square tube.
3.	Logo: Custom logo, design to be provided by Architect.
4.	Logo: ______ 
5.	Logo: Custom logo as indicated on Drawings.
6.	Mounting: Surface-mounted.
7.	Mounting: In-ground mounted.
8.	Finish: Hot-dip galvanized.
9.	Finish: Stainless steel, 304 grade.
10.	Finish: PVC dip.
11.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
H.	Cycle Dock Rack:
1.	Capacity: 2 bicycles.
2.	Rack: 5/16 inch steel body and 1/2 inch steel base.
3.	Mounting: Surface-mounted.
4.	Finish: Hot-dip galvanized.
5.	Finish: Stainless steel, 304 grade.
6.	Finish: PVC dip.
7.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
I.	Bike Bike Rack:
1.	Capacity: 2 to 4 bicycles.
2.	Body: 1-1/2 inch O.D. 11 gauge steel tube.
3.	Feet: 1/4 x 2-1/2 x 6 inch.
4.	Seat: 1/4 inch plate steel.
5.	Ends: Capped and ground smooth.
6.	Logo: Custom logo, design to be provided by Architect.
7.	Logo: ______ 
8.	Logo: Custom logo as indicated on Drawings.
9.	Mounting: Surface-mounted.
10.	Mounting: In-ground mounted.
11.	Finish: Hot-dip galvanized.
12.	Finish: Stainless steel, 304 grade, with No. 4 finish and Spectra Shield.
13.	Finish: Stainless steel, 304 grade, with high luster electropolish finish and Spectra Shield.
14.	Finish: PVC dip.
15.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
J.	Campus Rack:
1.	Single Sided:
a.	S3: 3 bicycle capacity.
1)	Length: 64 inches.
b.	S4: 4 bicycle capacity.
1)	Length: 89 inches.
c.	S5: 5 bicycle capacity.
1)	Length: 115 inches.
d.	S6: 6 bicycle capacity.
1)	Length: 139 inches.
2.	Double Sided:
a.	D5: 5 bicycle capacity
1)	Length: 64 inches.
b.	D7: 7 bicycle capacity
1)	Length: 89 inches.
c.	D9: 9 bicycle capacity
1)	Length: 114 inches.
d.	D11: 11 bicycle capacity
1)	Length: 139 inches.
3.	Center Beam: 3 inch O.D. 11 gauge steel tube.
4.	Ears: 1-1/4 inch O.D. 11 gauge tube.
5.	Feet: C3 x 1.4 x 3/16 x 24 inch channels.
6.	Mounting: Surface-mounted.
7.	Mounting: In-ground mounted.
8.	Finish: Hot-dip galvanized.
9.	Finish: Stainless steel, 304 grade, with No. 4 finish and Spectra Shield.
10.	Finish: Stainless steel, 304 grade, with high luster electropolish finish and Spectra Shield.
11.	Finish: PVC dip.
12.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
K.	Ultra Space Saver Rack: Modular system, one bike per hanger.
1.	Single Sided:
a.	Capacity: ______ 
2.	Double Sided:
a.	Capacity: ______
3.	Hanger: 1 inch O.D. 11 gauge tube with 1/2 inch steel round bar.
4.	Upright: 2 x 2 x 11 gauge inch square tube.
5.	Feet: AISI C3 x 4.1 galvanized steel chan.
6.	Crossbeams: 1-1/4 inch schedule 40 galvanized pipe, 1.66 inch O.D.
7.	Spacers: 2-3/8 inch O.D. plastic tubes with .218 inch wall thickness.
8.	Mounting: Floor-mounted.
9.	Mounting: Wall-mounted.
10.	Finish: Hot-dip galvanized.
11.	Finish: PVC dip.
12.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: Black (standard).
e.	Color: To be selected by Architect.
f.	Color: ______ 
g.	Color: As indicated on Drawings.
L.	Ultra Space Saver Squared Rack: Modular system, one bike per hanger.
1.	Single Sided:
a.	Capacity: ______ 
2.	Double Sided:
a.	Capacity: ______
3.	Arm: 1 inch x 11 gauge square tube with 1/2 inch steel round bar.
4.	Upright: 2 x 2 x 11 gauge square tube.
5.	Feet: AISI C3 x 4.1 galvanized steel chan.
6.	Crossbeams: 1-1/4 inch schedule 40 galvanized pipe, 1.66 inch O.D.
7.	Mounting: Floor-mounted.
8.	Mounting: Wall-mounted.
9.	Finish: Hot-dip galvanized.
10.	Finish: PVC dip.
11.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: Black (standard).
e.	Color: To be selected by Architect.
f.	Color: ______ 
g.	Color: As indicated on Drawings.
M.	Ultra Space Saver Single Rack: 
1.	Capacity: One bicycle.
2.	Body: 1 inch O.D. 11 gauge tube with 1/2 inch steel round bar.
3.	Mounting Flange: 1/4 inch plate.
4.	Finish: Hot-dip galvanized.
5.	Finish: PVC dip.
6.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: Black (standard).
e.	Color: To be selected by Architect.
f.	Color: ______ 
g.	Color: As indicated on Drawings.
N.	Bike File Rack: 
1.	Capacity: Nine bicycles per 8 foot unit.
2.	Trolley Track: 12 gauge galvanized steel.
3.	Trolley Assembly: Steel, 1 inch 16 gauge arms.
4.	Mounting: Floor-mounted.
5.	Mounting: Wall-mounted.
6.	Mounting: Ceiling-mounted.
7.	Finish: Zinc-plated frame components and stainless steel trolleys.
O.	Dero Decker Rack: Modular system.
1.	Single Sided:
a.	Capacity: 4 bicycles.
b.	Capacity: 8 bicycles.
c.	Capacity: 12 bicycles.
2.	Double Sided:
a.	Capacity: 8 bicycles.
b.	Capacity: 16 bicycles.
c.	Capacity: 24 bicycles.
3.	Uprights: 4 inch by 12 gauge square tube.
4.	Upright Base: 1/4 inch plate.
5.	Crossbar: 4 inch by 7 gauge square tube.
6.	Cantilevers: 2 x 4 inch by 11 gauge tube.
7.	Cantilever Base: 1/4 inch plate.
8.	Trays: 1/8 inch plate, 1/2 inch round bar.
9.	Mounting: Floor-mounted.
10.	Finish: Hot-dip galvanized (standard).
11.	Finish: Stainless steel, 304 grade.
12.	Finish: PVC dip.
13.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
P.	Dero Duplex Rack: Modular system.
1.	Capacity:
2.	Main Frame: 2 inch by 11 gauge square tube.
3.	Connector Plates: 1/4 inch plate.
4.	Trays: 11 gauge plate.
5.	Finish: Hot-dip galvanized (standard).
6.	Finish: Stainless steel, 304 grade. 
7.	Finish: PVC dip.
8.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
Q.	Wall Rack:
1.	Capacity: 2 bicycles.
2.	Mounting: Wall-mounted.
3.	Color: Black.
2.3	BICYCLE ACCESSORIES
A.	Fixit Plus:
1.	Capacity: One bike.
2.	Capacity: Two bikes.
3.	Main body: 6 x 12 ga. tube.
4.	Bike Hanger: 1 inch (25 mm) solid round bar.
5.	Foot: 10 inch (254 mm) diameter x 0.25 inch (6 mm) plate.
6.	Tool Tethers: 3/16 inch (5 mm) stainless steel cable.
7.	Manual air pump.
8.	Hand Tools: 
a.	Screwdrivers: Philips and flat head.
b.	Allen Wrenches: 2.5, 3, 4, 5, 6, and 8 mm.
c.	Torx Wrench: T25.
d.	Headset Wrench: 32 mm.
e.	Pedal Wrench: 15 mm.
f.	Box Wrenches: 8, 9, 10, and 11 mm.
g.	Tire leversL Two.
9.	Mounting: Floor-mounted. Tamper-resistant fastener anchors; included.
10.	Finish: Hot-dip galvanized (standard).
11.	Finish: Powder coated.
a.	Epoxy primer.
b.	TGIC, UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect from Manufacturer's standard offering.
e.	Color: 
f.	Color: As indicated on Drawings.
12.	Cane Stop. 
B.	Air Kit Prime:
1.	Main Body: 3 inch x 11 ga tube.
2.	Foot: 1/4 inch (6 mm) steel.
3.	Top: 1/8 inch (3 mm) aluminum.
4.	Manual Air Pump: Dero made.
5.	Finish: Hot-dipped galvanized performed after fabrication.
6.	Finish: Powder Coating:
a.	Parts are hard sandblasting.
b.	Epoxy primer is electrostatically applied to parts.
c.	TGIC, UV resistant polyester powder coat is applied. 
1)	Final Coating Thickness: 6 mils minimum.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
7.	Finish: Powder Coating Over Hot Dipped Galvanized Performed After Fabrication.
a.	TGIC, UV resistant polyester powder coat is applied.
1)	Final Coating Thickness: 6 mils minimum.
b.	Color: To be selected by Architect.
c.	Color: ______ 
d.	Color: As indicated on Drawings.
8.	Setbacks: Air Kit to be installed on a concrete surface and be at 24 inches (610 mm) or more from any obstruction. 36 inches (914 mm) is recommended.
C.	Air Kit 4:
1.	Main Body: 6 inch x 12 ga tube.
2.	Foot: 1/4 inch steel.
3.	Top: 1/8 inchaluminum.
4.	Manual air pump. Dero-made.
5.	Finish: Powder Coating:
a.	Parts are hard sandblasting.
b.	Epoxy primer is electrostatically applied to parts.
c.	TGIC, UV resistant polyester powder coat is applied. 
1)	Final Coating Thickness: 6 mils minimum.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
6.	Finish: Powder Coating Over Hot Dipped Galvanized Performed After Fabrication.
a.	TGIC, UV resistant polyester powder coat is applied.
1)	Final Coating Thickness: 6 mils minimum.
b.	Color: To be selected by Architect.
c.	Color: ______ 
d.	Color: As indicated on Drawings.
7.	Setbacks: Air Kit to be installed on a concrete surface and be at 24 inches (610 mm) or more from any obstruction. 36 inches (914 mm) is recommended.
2.4	BICYCLE SHELTERS
A.	Kolo Shelter:
1.	Short Unit with Campus Rack D5: 5 bicycle capacity.
2.	Short Unit with Dero Decker Rack (14): 14 bicycle capacity.
3.	Short Unit with Ultra Space Saver Rack (6): 6 bicycle capacity.
4.	Short Unit with Ultra Space Saver Rack (9): 9 bicycle capacity.
5.	Medium Unit with Campus Rack D9: 9 bicycle capacity.
6.	Medium Unit with Dero Decker Rack (22): 22 bicycle capacity.
7.	Medium Unit with Ultra Space Saver Rack (12): 12 bicycle capacity.
8.	Medium Unit with Ultra Space Saver Rack (18): 18 bicycle capacity.
9.	Long Unit with Campus Rack D11: 11 bicycle capacity.
10.	Long Unit with Dero Decker Rack (30): 30 bicycle capacity.
11.	Long Unit with Ultra Space Saver Rack (16): 16 bicycle capacity.
12.	Long Unit with Ultra Space Saver Rack (24): 24 bicycle capacity.
13.	Uprights: 6 x 1/4 inch square tube.
14.	Center Member: 6 x 1/4 inch square tube, C6 channel.
15.	Feet: 1/2 inch plate.
16.	Rafter: 3/16 inch plate.
17.	Roof Panels: 1/2 inch UV resistant polycarbonate.
18.	Finish: Hot-dip galvanized (standard).
19.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______
f.	Color: As indicated on Drawings.
B.	Cycle Station:
1.	Capacity per unit with Campus Racks S4: 8 bicycles.
2.	Capacity per unit with Campus Racks S4 and side panels: 8 bicycles.
3.	Capacity per unit with Hoop Racks (6): 12 bicycles.
4.	Capacity per unit with Hoop Racks (5) and side panels: 10 bicycles.
5.	Capacity per unit with Space Saver Racks B5 and B7: 12 bicycles.
6.	Capacity per unit with Space Saver Racks B5 and B7 and side panels: 12 bicycles.
7.	Capacity per unit with Dero Decker (18): 18 bicycles.
8.	Capacity per unit with Dero Decker (16) and side panels: 16 bicycles.
9.	Uprights: 4 x 3/16 inch square tube.
10.	Feet: 1/2 inch plate.
11.	Roof Truss: 4 x 3 x 3/16 inch tube.
12.	Roof Purlins: 3 x 1/8 inch square tube.
13.	Roof Panels: 24 gauge Type S deck, galvanized steel.
14.	Panels: 1/4 inch polycarbonate with 1.77 inch square aluminum framing.
15.	Panels: 2 x 3/16 inch steel wire mesh with 2 inch steel framing.
16.	Finish: Hot-dip galvanized (standard).
17.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
C.	Vizor Shelter:
1.	Capacity per unit with Campus Rack S6: 6 bicycles.
2.	Capacity per unit with Hoop Racks (4): 8 bicycles.
3.	Uprights: 4 x 5/16 inch square tube.
4.	Feet: 5/8 inch plate.
5.	Rafter: 4 x 2 x 3/16 inch tube.
6.	Purlins: 4 x 2 x 3/16 inch tube.
7.	Roof Panels: 26 gauge Type S deck, galvanized steel.
8.	Finish: Hot-dip galvanized (standard).
9.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
D.	Bike Haven:
1.	Capacity per unit with Campus Rack S6: 8 bicycles.
2.	Capacity per unit with Hoop Racks (4): 8 bicycles.
3.	Capacity per unit with Space Savers B7 double-sided: 14 bicycles.
4.	Uprights: 4 x 3/16 inch square tube.
5.	Feet: 3/8 inch plate.
6.	Roof Member: 4 x 1/8 inch square tube.
7.	Roof Member Long: 4 x 2 x 3/16 inch tube.
8.	Roof Panels: 26 gauge Type S deck, galvanized steel.
9.	Panels: 1/4 inch clear polycarbonate with 1.77 inch square aluminum framing.
10.	Finish: Hot-dip galvanized (standard).
11.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
E.	Pocket Shelter:
1.	Capacity per unit with Ultra Space Saver Racks: 6 bicycles.
2.	Capacity per unit with Bike File Racks: 10 bicycles.
3.	Uprights: 2 x 3/16 inch square tube.
4.	Feet: 3/8 inch plate.
5.	Horizontal Member: 3/16 inch plate.
6.	Roof Member: 3/16 inch plate.
7.	Roof Panels: 26 gauge Type S deck, galvanized steel.
8.	Side Panels: 1/4 inch clear polycarbonate.
9.	Benches: Interior.
10.	Benches: Exterior.
11.	Finish: Hot-dip galvanized (standard).
12.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
2.5	BICYCLE LOCKERS
2.6	Customers can choose either a single-sided or double-sided model in a galvanized or powder coat finish. Ventilating windows on the doors allow for easy monitoring of the locker's contents. Installation is simple, with leveling feet for uneven surfaces. The Dero Bike Locker also ships flat to save on freight.
2.7	Delete if not required.
A.	Dero Bike Locker:
1.	Single Sided: 1 bicycle capacity.
2.	Double Sided: 2 bicycle capacity.
3.	Base: 1.5 inch x 14 gauge square tube.
4.	Corners: 14 gauge plate.
5.	Sides: 18 gauge plate.
6.	Doors: 16 gauge plate.
7.	Top: 16 gauge plate.
8.	Locking: Keyed lock.
9.	Locking: U-lock/padlock handle.
10.	Include floor.
11.	Finish: Hot-dip galvanized (standard).
12.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
B.	Veloport Locker:
1.	Capacity: 1 bicycle.
2.	Frame: 2 inch x 14 gauge square tube.
3.	Back: 18 gauge plate.
4.	Sides: 18 gauge plate.
5.	Doors: 12 gauge aluminum plate.
6.	Locking: Keyed lock.
7.	Locking: U-lock/padlock handle.
8.	Finish: Hot-dip galvanized (standard).
9.	Finish: Powder coated.
a.	Epoxy primer.
b.	UV resistant polyester powder coat.
c.	Minimum thickness: 6 mils.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
2.8	BICYCLE PARKING SYSTEMS
2.9	The Cycle Stall Basic kit covers the needs of cities and businesses that want to provide an on-street bike corral at a low cost and minimal changes to infrastructure. Kit includes parking delineators.
2.10	A variety of rack styles may be used to build your bike corral. Parks 10+ bikes.
2.11	Delete if not required.
A.	Cycle Stall Basic:
1.	Capacity with ___ rack: 
2.	Capacity with ___ rack: 
3.	Capacity with ___ rack: 
4.	Wheel Stops: 
5.	Bollards: 
6.	Color: Yellow.
2.12	ELECTRIC BIKE CHARGING RACKS
A.	Basis of Design: eBeam Charging Rack by Dero. A secure place to charge batteries while parked. Outlets on both sides of each rack. For indoor use only. Wire from ground or side. 
1.	Capacity: 2 e-Bikes
2.	Materials: 
a.	Rectangle Tube: 4 x 2 inches (102 x 51 mm). Wall thickness: 11 ga.
b.	Flat Bar: 2 x 3/8 inches (51 x 9.5 mm).
3.	Finishes: Powder Coat.
a.	1. Sandblast.
b.	2. Epoxy primer electrostatically applied.
c.	3. Final thick TGIC polyester powder coat.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
4.	Mounting: Surface Mount Only.
a.	Foot Mount: 0.25 inch (6 mm) thick steel foot with four anchors per foot. Specify foot mount for this option. 
b.	Fasteners: Tamper-resistant.
B.	Basis of Design: eDowntown Charging Rack by Dero. A secure place to charge batteries while parked. Outlets on both sides of each rack. For indoor use only. Wire from ground or side.
1.	Capacity: 2 e-Bikes
2.	Materials: 
a.	Rectangle Tube: 4 x 2 inches (102 x 51 mm). Wall thickness: 11 ga.
b.	Square Tube: 2 inch (51 mm) x 11 ga.
3.	Finishes: Powder Coat.
a.	1. Sandblast.
b.	2. Epoxy primer electrostatically applied.
c.	3. Final thick TGIC polyester powder coat.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
4.	Mounting: Surface Mount Only.
a.	Foot Mount: 0.25 inch (6 mm) thick steel feet with six anchors per foot. Specify foot mount for this option. 
b.	Fasteners: Tamper-resistant.
C.	Basis of Design: eHitch Charging Rack by Dero. A secure place to charge batteries while parked. Outlets on both sides of each rack. For indoor use only. Wire from ground or side.
1.	Capacity: 2 e-Bikes
2.	Materials: 
a.	Rectangle Tube: 4 x 2 inches (102 x 51 mm). Wall thickness: 11 ga.
b.	Flat Bar: 2 x 3/8 inches (51 x 9.5 mm).
3.	Finishes: Powder Coat.
a.	1. Sandblast.
b.	2. Epoxy primer electrostatically applied.
c.	3. Final thick TGIC polyester powder coat.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
4.	Mounting: Surface Mount Only.
a.	Foot Mount: 0.25 inch (6 mm) thick steel foot with four anchors per foot. Specify foot mount for this option. 
b.	Fasteners: Tamper-resistant.
D.	Basis of Design: eSwerve Charging Rack by Dero. A secure place to charge batteries while parked. Outlets on both sides of each rack. For indoor use only. Wire from ground or side.
1.	Capacity: 2 e-Bikes
2.	Materials: 
a.	Rectangle Tube: 4 x 2 inches (102 x 51 mm). Wall thickness: 11 ga.
b.	Square Tube: 2 inch (51 mm) x 11 ga.
3.	Finishes: Powder Coat.
a.	1. Sandblast.
b.	2. Epoxy primer electrostatically applied.
c.	3. Final thick TGIC polyester powder coat.
d.	Color: To be selected by Architect.
e.	Color: ______ 
f.	Color: As indicated on Drawings.
4.	Mounting: Surface Mount Only.
a.	Foot Mount: 0.25 inch (6 mm) thick steel feet with six anchors per foot. Specify foot mount for this option. 
b.	Fasteners: Tamper-resistant.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Verification of Conditions: Examine areas and conditions under which Work is to be performed and identify conditions that may be detrimental to proper or timely completion.
B.	Do not proceed until unsatisfactory conditions have been corrected.
3.2	INSTALLATION
A.	Install products in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
1.	Comply with manufacturer's published minimum setback dimensions and recommended mounting heights.
3.3	CLEANING AND PROTECTION
A.	Protect from damage during construction operations. Promptly repair any damaged surfaces. Remove and replace work which cannot be satisfactorily repaired.

END OF SECTION