SECTION 11 68 33.33

SPORTS FIELD EQUIPMENT

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2024 -  2024 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Za elective court equipment including the following:
1.	Ball park netting. 
2.	Ball park protective padding. 
3.	Baseball and softball windscreens. 
4.	Bases, home plates, pitching rubbers and accessories. 
5.	Batting cages and tunnels, tunnel nets, dividers, hitting stations, Indoor batting tunnel kits, and hitting backdrops:. 
6.	Outfield Products:
a.	Foul poles
b.	Fence guards and caps. 
c.	Distance markers
7.	Protective screens. 
8.	Replacement nets.
9.	Wheel kits. 
B.	Section 32 18 23 - Tennis Court Surfacing.
C.	Section 32 31 13.26 - Tennis Court Fences and Gates.
1.2	REFERENCES
A.	Selective court equipment in this Section complies with the following: 
1.	American Sports Builders Association (ASBA).
2.	United States Tennis Association (USTA).
3.	National Federation of State High School Associations (NFHS).
4.	National Collegiate Athletic Association (NCAA).
5.	International Amateur Athletic Association (IAFF).
1.3	SUBMITTALS
A.	Submit under provisions of Section 01 30 00.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Verification Samples: Two representative units of each type, size, pattern, and color.
D.	Shop Drawings: Include details of materials, construction, and finish. Include relationship with adjacent construction. 
1.4	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum of five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
1.5	PRE-INSTALLATION CONFERENCE
A.	Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.7	PROJECT CONDITIONS
A.	Maintain environmental temperature, humidity, and ventilation conditions within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.8	WARRANTY
A.	Manufacturer's standard Limited warranty unless indicated otherwise.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Douglas Industries, Inc. , which is located at:<BR />3441 S. 11th Ave.<BR />Eldridge, IA 52748<BR />Toll Free Tel: 800-553-8907<BR />Email: request info ();Web: http://www.douglas-sports.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with the provisions of Section 01 60 00.
2.2	FIELD EQUIPMENT
A.	Ball Park Netting:
1.	Douglas Standard Backstop Cable System: Item No. 66800. For use with Custom backstop wall padding.
a.	Poles: Steel. Outside Diameter: 10-3/4 inch (273 mm). Wall Thickness: 0.375 inch (9.53 mm). Finish: Powder coat. Color: Black. 
b.	Poles: Steel. Outside Diameter: ___ inch (___ mm). Wall Thickness: ___ inch (___ mm). Finish: Powder coat. Color: Black. 
c.	Netting: 1.4 mm, 1-3/4 inch sq. (44 mm), No. 12 Knotted Dyneema, ultra-high molecular polyethylene, UV, and weather resistant, with 1/4 inch (6 mm) solid braid sewn rope boarder. 94 percent visibility factor, 308 lbs. (139.71 kg) break strength, 1500 lbs. (680.39 kg) rope border break strength. 
d.	Netting: ________.
e.	Hardware: 1/4 inch (6 mm) cable, galvanized, with 6100 lbs.(2766.91 kg) break strength, 12 inch (305 mm) eyebolts, 12 inch (305 mm) turnbuckles, 1/4 inch (6 mm) cable clamps, 8 mm carabiner clips. 
f.	Digital printing.
2.	Douglas Standard Backstop Cable Hardware Kit: Item No. 66290. For use with custom netting and poles.
a.	Hardware: 1/4 inch (6 mm) cable, galvanized, with 6100 lbs. (2766.91 kg) break strength; 500 ft. (152.4 m), four 12 inch (305 mm) turnbuckles, four 6 inch (152 mm) turnbuckles, thirty 1/4 inch (6 mm) cable clamps, eight 6 inch (152 mm) eyebolts, four hundred 8 mm spring links. Hardware is zinc coated or stainless steel. 
3.	Douglas Suspended Backstop Cable System: Item No. 66805. For use with custom backstop wall padding.
a.	Poles: Stee. Outside Diameter: 10-3/4 inch (273 mm). Wall Thickness: 0.375 inch (10 mm). Finish: Powder coat. Color: Black.
b.	Poles: Steel. Outside Diameter: ___ inch (___ mm). Wall Thickness: ___ inch (___ mm). Finish: Powder coat. Color: Black. 
c.	Netting: 1.4 mm, 1-3/4 inch (44 mm), sq., No. 12 Knotted Dyneema, ultra-high molecular polyethylene, UV, and weather resistant, with 1/4 inch (6 mm) solid braid sewn rope boarder. 94 percent visibility factor, 308 lbs. (139.71 kg) break strength, 1500 lbs. (680.39 kg) rope border break strength. 
d.	Netting: ________. 
e.	Hardware: 1/4 inch (6 mm) cable, galvanized, with 6100 lbs.(2766.91 kg) break strength, 12 inch (305 mm) eyebolts, 12 inch (305 mm) turnbuckles, 1/4 inch (6 mm) cable clamps, 8 mm carabiner clips, galvanized. 
f.	Digital printing.
4.	Douglas Suspended Backstop Cable Hardware Kit, Tie-Back: Item No. 66295. To be used for custom netting and poles.
a.	Hardware: Cable: 1/4 inch (6 mm) galvanized steel; 600 ft. (189 m) Break Strength: 6100 lbs. (2766.91 kg). Six, 12 inch (305 mm) turnbuckles. Four, 6 inch (152 mm) turnbuckles. Forty, 1/4 inch (6 mm) cable clamps. Eight, 6 inch (152 mm) eyebolts. Four Hundred, 8 mm spring links. Hardware to be zinc coated or stainless steel. 
5.	Indoor Batting Tunnel Accessory Cable Hardware Kit: Item No. 66213. For use with batting tunnel nets.
a.	Hardware: Cable: 1/4 inch (6 mm); 500 ft. (152.4 m). Seventy steel c-snaps. Seventy split bracket pulleys. Six turnbuckles. Twelve 1/4 inch (6 mm) wire cable clamps. Six eyebolts. Hardware to be zinc coated or stainless steel. 
6.	Indoor Batting Tunnel Ceiling Suspension Kit: Item No. 66219. For use with batting tunnel nets.
a.	Hardware: Cable: One spool 1/4 inch (6 mm); 500 ft. (152.4 m). Two spools 1/8 inch (3 mm); 1000 ft. (309 m). Sixty 1/8 inch (3 mm) wire clamps. Twelve 1/4 inch (6 mm) wire cable clamps. Six turnbuckles. Six eyebolts. Seventy steel c-snaps. Thirty split bracket pulleys. Hardware to be zinc coated or stainless steel. 
7.	Indoor Batting Tunnel Tensioning Kit: Item No. 66200. For use with batting tunnel nets.
a.	Hardware: Six eyebolts. Six 8 mm spring link clips. Six 3/8 inch (10 mm) spring link clips. Six cables, 15 ft. (4.6 m) long. Three 50 ft. (15 m) lengths. Hoisting Rope: 3/8 inch (10 mm) high strength braided. Three cam lock pulley systems, Three swivel clamps. 
b.	Maximum Tension Load per Eyebolt: 200 lbs. (90.72 kg), with 24 inch (610 mm) sag in center for net. 
8.	BLR Braided Lacing Rope 3/16 Inches Poly-Pro, 1,000 Ft. Roll: Item No. 31601M.
a.	3/16 inch (5 mm) braided polypropylene lacing rope, black. UV and weather resistant. 550 lbs. (249.48 kg) break strength. 
9.	C-Snap, Steel Black: Item No. 32670. 3 inch Carabiner. 
10.	Cable 1/4 Inches GAC Galvanized Steel: Item No. 34728. 
a.	4200 lbs. (1905.09 kg) break strength. Cut to length, sold per foot. 
11.	Cable Clamp for 1/4 Inches Cable: Item No. 34725. 
12.	Cable 1/8 Inches Galvanized Steel: Item No. 15102. Cut to length, sold per foot. 
13.	Cable Clamp for 1/8 Inches Cable: Item No. 34726. 
14.	Douglas No. 12 Knotted Dyneema Black 1-3/4 Inches SQ: Item No. 26012. 
a.	1.4 mm, 1-3/4 inch (44 mm) sq., ultra-high molecular polyethylene, UV, and weather resistant, with 1/4 inch (6 mm) solid braid sewn rope boarder. 94 percent visibility factor, 308 lbs. (139.71 kg) break strength, 1500 lbs. (680.39 kg) rope border break strength. 
15.	Douglas No. 42 Knotted Ultra HDPE Netting, Black: Item No. 26142. 
a.	2.4 mm, 1-3/4 inch (44 mm) sq., knotted HDPE polyethylene, UV, and weather resistant, with 1/4 inch (6 mm) solid braid sewn rope boarder. 94 percent visibility factor, 424 lbs. (192.32 kg) break strength, 5/16 inch (8 mm) rope border, 1710 lbs. (775.64 kg) break strength. 
16.	Douglas No. 420 Knotless Pylon Netting, 1-1/2 Inches SQ: 
a.	Tape Bound with Grommets, Black Net: Item No. 22009.
b.	Tape Bound with Grommets, White Net: Item No. 22005.
1)	Netting: Weather treated for moisture and sunlight exposure. 125 lbs. (56.7 kg) breaking strength. 
2)	1-1/2 inch (38 mm) reinforced vinyl coated polyester, double sewn.
3)	Brass grommets.
4)	Grommet Spacing: 18 inches (457 mm) along top. 
5)	Grommet Spacing: ________. 
c.	Rope Bound: Item No. 22009R. 
17.	Douglas Complete Netting Systems: Item No. 67200.
a.	Poles: Steel. Outside Diameter: 10-3/4 inch (273 mm). Wall Thickness: 0.375 inch (10 mm). Finish: Powder coat. Color: Black.
b.	Poles: Steel. Outside Diameter: ___ inch (___ mm). Wall Thickness: ___ inch (___ mm). Finish: Powder coat. Color: Black. 
c.	Height: 40 ft. (12.2 m) maximum. For installation in minimum 24 inch (610 mm) wide concrete footing.
d.	Netting: Item No. 26012: No. 12 Knotted Dyneema. 1.4 mm, 1-3/4 inch (44 mm) sq., ultra-high molecular polyethylene, UV, and weather resistant, with 1/4 inch (6 mm) solid braid sewn rope boarder. 94 percent visibility factor, 308 lbs. (139.71 kg) break strength, 1500 lbs. (680.39 kg) rope border break strength. 
e.	Netting: Item No. 26142: Douglas No. 42 Knotted Ultra HDPE Netting. 2.4 mm, 1-3/4 inch (44 mm) sq., knotted HDPE polyethylene, UV, and weather resistant, with 1/4 inch (6 mm) solid braid sewn rope boarder. 94 percent visibility factor, 424 lbs. (192.32 kg) break strength, 5/16 inch (8 mm) rope border, 1710 lbs. (775.64 kg) break strength. 
f.	Netting: Item No. 36099B: Douglas Twisted Knotted Nylon Netting, 1-3/4 Inches SQ: No. 36 Medium Weight, Black: High tensile strength, black. UV and weather resistant, 5/16 inch (8 mm) rope border, 1710 lbs. (775.64 kg) break strength. 345 lbs. (156.49 kg) break strength.
g.	Netting: Douglas Premium 3.0 mm Knotless Polypropylene, 1-3/4 Inches SQ:
1)	High tenacity pylon netting, UV, and weather resistant, 250 lbs. (113.40 kg) break strength. 
a)	Color: Black, standard. 
b)	Color: Dark Green. 
c)	Color: White. 
2)	1-1/2 inch (38 mm) reinforced vinyl coated polyester edging, double-sewn. 
3)	Brass Grommet Spacing: 18 inches (457 mm) along top. 
4)	Brass Grommet Spacing: ________. 
5)	Sewn rope border, black.
h.	Netting: Douglas Premium 3.0 mm Knotless Polypropylene, 4 Inches SQ:
1)	High tenacity pylon netting, UV, and weather resistant, 250 lbs. (113.40 kg) break strength. 
a)	Color: Black, standard. 
b)	Color: Dark Green. 
c)	Color: White. 
2)	Netting: Item No. 25803B: 1-1/2 inch (38 mm) reinforced vinyl coated polyester edging, double-sewn,
3)	Brass Grommet Spacing: 18 inches (457 mm) along top. 
4)	Brass Grommet Spacing: ________. 
5)	Netting: Item No. 25803BR: Sewn rope border, black.
i.	Hardware: 1/4 inch (6 mm) GAC cable, galvanized, with 6100 lbs. (2766.91 kg) break strength, 12 inch (305 mm) eyebolts, TB-12 12 inch (305 mm) turnbuckles, TB-6 6 inch (152 mm) turnbuckles, 1/4 inch (6 mm) cable clamps, 8 mm carabiner clips, galvanized. 
18.	Douglas Premium 3.0 mm Knotless Polypropylene, 1-3/4 Inches SQ
1)	High tenacity pylon netting, UV, and weather resistant, 250 lbs. (113.40 kg) break strength. 
a)	Color: Black, standard. 
b)	Color: Dark Green. 
c)	Color: White. 
2)	1-1/2 inch (38 mm) reinforced vinyl coated polyester edging, double-sewn.
3)	Brass Grommet Spacing: 18 inches (457 mm) along top. 
4)	Brass Grommet Spacing: ________. 
5)	Sewn rope border, black.
19.	Douglas Premium 3.0 mm Knotless Polypropylene, 4 Inches SQ:
1)	High tenacity pylon netting, UV, and weather resistant, 250 lbs. (113.40 kg) break strength. 
a)	Color: Black, standard. 
b)	Color: Dark Green. 
c)	Color: White. 
2)	Item No. 25803B: 1-1/2 inch (38 mm) reinforced vinyl coated polyester edging, double-sewn.
3)	Brass Grommet Spacing: 18 inches (457 mm) along top. 
4)	Brass Grommet Spacing: ________. 
5)	Item No. 25803BR: Sewn rope border, black.
20.	Douglas Twisted Knotted Nylon Netting, 1-3/4 Inches SQ:
a.	High tensile strength, black. UV and weather resistant, 5/16 inch (8 mm) rope border, 1710 lbs. (775.64 kg). break strength. 
b.	Item No. 36099A: No. 21 Light Weight, Black: 237 lbs. (107.50 kg) break strength.
c.	Item No. 36099B: No. 36 Medium Weight, Black: 345 lbs.(156.49 kg) break strength.
d.	Item No. 36099C: No. 42 Heavy Weight, Black: 435 lbs. (197.31 kg) break strength. 
e.	Item No. 36099D: No. 48 Heavy Weight, Black: 472 lbs. (214.10 kg) break strength. 
f.	Item No. 36099E: No. 60 Heavy Weight, Black: 720 lbs. (326.59 kg) break strength. 
g.	Item No. 36099G: No. 72 Heavy Weight, Black: 862 lbs. (390.00 kg) break strength. 
h.	Item No. 36099F: No. 96 Heavy Weight, Black: 1112 lbs. (504.39 kg) break strength. 
21.	Eye Bolt, Steel, Galvanized. 1/2 x 6 Inches: Item No. 34730.
22.	Pully with Split Bracket, 1-7/8 Inch: Item No. 34721. 
23.	Spring Link Carabiner: 5mm: Item No. 32679. 
24.	Spring Link Carabiner: 6mm: Item No. 32680.
25.	Spring Link Carabiner: 8mm: Item No. 36000. 
26.	TB-12 Jaw and Eye Turnbuckle, 12 Inch: Item No. 34724. 
a.	Steel body and fittings, galvanized steel. 1/2 inch (13 mm) thread dia., 12 inch (305 mm) take-up. 
27.	TB-6 Jaw and Eye Turnbuckle, 6 Inch: Item No. 36986. 
a.	Steel body and fittings, galvanized steel. 3/8 inch (10 mm) thread dia., 6 inch (152 mm) take-up. 
B.	Ball Park Protective Padding:
1.	Logo Vinyl Rail Wraps: Item No. 29219.
a.	18 oz. vinyl, UV, and weather resistant. 
b.	Color: ________. 
c.	Color: As determined by the Architect.
d.	Digital Printed Graphics: Architect to provide vector graphics. 
2.	Douglas Custom 3 inch (76 mm) Pad. Thick Wood Back Bolt and Backup Plate. Item No. 26310. 
a.	Standards Compliance: NFHS, NCAA, IAFF, ASBA compliant. 
b.	Plywood Backing: 3/4 inch (19 mm), exterior marine grade.
c.	Padding: 3 inch (76 mm) thick, high impact, mildew resistant, polyurethane foam.
d.	Vinyl Covering: 18 oz. per sq. yd., UV, and weather resistant, for all locations and weather conditions.
e.	Back-Up Plates: Steel. Finish: Powder coated. Color: Black. 
1)	For attachment to back side of chain link fence and bolting to plywood back of padding. 
f.	Panel Size, Maximum: Up to 4 x 8 ft. (1.2 x 2.5 m).
g.	Finished Panel Size: ___ x ___ ft. (___ x ___ m).
h.	Color: Dark Green.
i.	Color: Black.
j.	Color: Royal Blue.
k.	Color: Navy Blue.
l.	Color: Red.
m.	Color: ________.
n.	Color: As determined by the Architect.
o.	Digital Printed Graphics: Architect to provide vector graphics. 
p.	Warranty: Manufacturer's Limited. 
3.	Douglas Custom 3 inch (76 mm) Pad: Thick Wood Back, Z-Clip Attachment for Concrete, Brick or Wood Walls. Item No. 26300. 
a.	Plywood Backing: 3/4 inch (19 mm), exterior marine grade. 
b.	Padding: 3 inch (76 mm) thick, high impact, mildew resistant, polyurethane foam.
c.	Vinyl Covering: 18 oz. per sq. yd., UV, and weather resistant, for all locations and weather conditions. 
d.	Attachment: 2-1/2 inch (64 mm) wide, 1/8 inch (3 mm) thick, extruded aluminum z-clip channel, anchored to top, and bottom length of plywood backing and exterior wall.
e.	Panel Size, Maximum: Up to 4 x 8 ft. (1.2 x 2.5 m).
f.	Finished Panel Size: ___ x ___ ft. (___ x ___ m).
g.	Color: Dark Green. 
h.	Color: Black. 
i.	Color: Royal Blue. 
j.	Color: Navy Blue. 
k.	Color: Red. 
l.	Color: ________.
m.	Color: As determined by the Architect.
n.	Digital Printed Graphics: Architect to provide vector graphics. 
o.	Warranty: Manufacturer's Limited. 
4.	Douglas Custom Sewn Padding with Grommets: Custom, vinyl wrapped, reinforced, double-sewn high-impact polyethylene foam.
a.	Foam Padding Thickness: Item No. 29218: 2 inch (51 mm).
b.	Foam Padding Thickness: Item No. 29218A: 3 inch (76 mm). 
c.	Foam Padding Thickness: Item No. 29218B: 4 inch (102 mm). 
d.	Solid Vinyl Covering: 18 oz. per sq. yd., UV, and weather resistant, antibacterial, antifungal, rot, and mildew resistant.
1)	Two, 1-1/2 inch (38 mm) sewn vinyl flaps.
2)	No. 2 brass grommets every 6 inches (152 mm), top and bottom.
3)	Black Velcro sewn along sides.
e.	Top and Bottom Hemmed Flap: Stitched with UV resistant high tensile strength polyester thread. 
f.	Panel Size, Maximum: Up to 4 x 8 ft. (1.2 x 2.5 m).
g.	Finished Panel Size: ___ x ___ ft. (___ x ___ m).
h.	Color: Forest Green. 
i.	Color: Black. 
j.	Color: Royal Blue. 
k.	Color: Navy Blue. 
l.	Color: Red. 
m.	Color: ________.
n.	Color: As determined by the Architect.
o.	Digital Printed Graphics: Architect to provide vector graphics. 
p.	Warranty: Manufacturer's Limited. 
5.	Douglas Baseball Dugout Rail Vinyl Covered Padding, Guard Rail Vinyl Covered Padding: Item No. 29217. 
a.	Standards Compliance: NFHS, NCAA, IAAF, and ASBA.
b.	Padding: 1 inch (25 mm) thick polyurethane 100 pus ILD high density foam.
c.	Vinyl Covering: 18 oz. sq. yd. UV and weather resistant, with 1-1/2 inch (38 mm) perimeter vinyl flap. 
1)	Double-sewn with high tensile strength thread.
2)	No. 2 brass grommets every 6 inch (152 mm). 
d.	Length: ___ft (___mm). Fitting up to 2 inch (51 mm) Dia. Pipe. 
e.	Color: Dark Green. 
f.	Color: Black. 
g.	Color: Royal Blue. 
h.	Color: Navy Blue. 
i.	Color: Red. 
j.	Color: ________. 
k.	Color: As determined by the Architect.
l.	UV Protected Tie Wraps.
m.	Digital Printed Graphics: UV digital printing, integrated into material. 
n.	Architect to provide vector graphics.
C.	Baseball and Softball Windscreens:
1.	Douglas VCP Windscreen: Warranty: 3 Year Limited. 
a.	Fabric: 9 x 12 weave. Windbreak: 80 percent. Material: 50 percent vinyl, 50 percent polyester open mesh, 8 oz. per sq. yd. Tensile Strength: 230 x 200.
b.	Hems: Three-ply, double-sewn, up to 1-1/2 inch (38 mm) wide, with No. 2 brass grommets spaced every 12 inches (305 mm) on panel side and every 18 inches (457 mm) along top and bottom. 
c.	Center Reinforcement: For screens over 6 ft. (1.9 m), secure with tie wraps. Screens over 6 ft. (1.9 m), high include a center tab with grommets. 
d.	Height: 6 ft. (1.9 m).
e.	Height: 9 ft. (2.7 m).
f.	Height: ________.
g.	Height: As detailed on the Drawings.
h.	Length: 60 ft. (18.3 m) maximum. 
i.	Length: ________.
j.	Length: As detailed on the Drawings.
k.	Air Vents: AVR Vents: 10 x 8 inch (254 x 203 mm) cut outs. Perimeter hemmed with polyester webbing. Placed at 10 ft. (3.05 m) intervals. 
l.	Air Vents: AV Vents: 5 x 8 inch (127 x 203 mm) die cut. Heat sealed. Placed at 10 ft. (3.05 m) intervals.
m.	Color: Dark Green.
n.	Color: Black.
o.	Color: Open Tournament Blue.
p.	Color: Royal Blue.
q.	Color: Navy Blue.
r.	Color: Red.
s.	Color: Purple. 
t.	Color: Orange.
u.	Color: Burgundy.
v.	Color: Gray.
w.	Color: Brown. 
x.	Douglas Digital Windscreen Printing: Item No. 39995. Warranty: 3-4 Years.
1)	UV resistant ink, full color, printed directly on material. Architect to provide vector graphics. 
2.	Douglas Poly Pro Plus Premium Open Mesh Windscreens. Item No. 21600. 
a.	Fabric: 28 x 14, 30-1/2 x 12 inch (775 x 305 mm) leno weave. Windbreak: 85 percent. Material: 100 percent polypropylene. Weather and UV resistant. Open mesh. 7 oz. per sq. yd. Tensile Strength: 380 x 185.
b.	Hems: Four-ply, double-sewn, up to 1-1/2 inch (38 mm) wide, with solid vinyl inserts and 18 oz. vinyl overlay. No. 2 brass grommets spaced every 12 inches (305 mm) on panel side and every 18 inches (457 mm) along top and bottom. 
c.	Center Reinforcement: For screens over 6 ft. (1.9 m), secure with tie wraps Screens over 6 ft. (1.9 m) high include a center tab, with double stitched 3 inch (76 mm) wide polyester webbing and grommets placed every 18 inches (457 mm). 
d.	Height: 6 ft. (1.9 m).
e.	Height: 9 ft. (2.7 m).
f.	Height: ________.
g.	Height: As detailed in the Drawings
h.	Length: 60 ft. (18.3 m) maximum. 
i.	Length: ________.
j.	Length: As detailed on the Drawings
k.	Air Vents: AVR Vents: 10 x 8 inch (254 x 203 mm) cut outs. Perimeter hemmed with polyester webbing. Placed at 10 ft. (3.05 m) intervals. 
l.	Color: Dark Green. 
m.	Color: Black. 
3.	Douglas Poly Pro Plus Premium -Closed Mesh: Warranty: 4 Year Limited.
a.	Design: 30 x 16 leno weave, 100 percent polypropylene, 95 percent blockage, 8 oz. per sq. yd. UV and weather treated. Tensile Strength: 450 x 215.
b.	Hems: Three-ply, double-sewn, up to 1-1/2 (38 mm) wide, seamed with solid vinyl inserts and No. 2 brass grommets spaced every 12 inches (305 mm) on panel side and every 18 inches (457 mm) along top and bottom. 
c.	Center Reinforcement: For screens over 6 ft. (1.9 m), secured with tie wraps. Screens over 6 ft. (1.9 m) high include a center tab double stitched with 3 inch (76 mm) wide polyester and, with grommets places every 18 inches (457 mm). 
d.	Height: 6 ft. (1.9 m).
e.	Height: 9 ft. (2.7 m).
f.	Height: ________.
g.	Height: As detailed on the Drawings.
h.	Length: 60 ft. (18.3 m) maximum. 
i.	Length: ________.
j.	Length: As detailed on the Drawings.
k.	Air Vents: AVR Vents: 10 x 8 inch (254 x 203 mm) cut outs. Perimeter hemmed with polyester webbing. Placed at 10 ft. (3.05 m) intervals. 
4.	Douglas VCP Max Windscreen. Warranty: 4 Year Limited. 
a.	Standards Compliance: ASBA, USTA Compliant.
b.	Fabric: 16 x 17 weave. Windbreak: 85 percent windbreak. Material: 50 percent vinyl, 50 percent polyester open mesh, 10 oz. per sq. yd. UV and weather treated. Tensile Strength: 395 x 401.
c.	Hems: Three-ply, double-sewn, up to 1-1/2 inch (38 mm) wide, with No. 2 brass grommets spaced every 12 inches (305 mm) on panel side and every 18 inches (457 mm) along top and bottom. 
d.	Center Reinforcement: For screens over 6 ft. (1.9 m), secured with tie wraps. Screens over 6 ft. (1.9 m) high include a center tab on vinyl coated polyester sewn with 18 oz. black vinyl, with grommets places every 18 inches (457 mm). 
e.	Height: 6 ft. (1.9 m).
f.	Height: 9 ft. (2.7 m).
g.	Height: ________.
h.	Height: As detailed on the Drawings.
i.	Length: 60 ft. (18.3 m) maximum. 
j.	Length: ________.
k.	Length: As detailed on the Drawings.
l.	Air Vents: AVR Vents: 10 x 8 inch (254 x 203 mm) cut outs. Perimeter hemmed with polyester webbing. Placed at 10 ft. (3.05 m) intervals. 
m.	Air Vents: AV Vents: 5 x 8 inch (127 x 203 mm) die cut. Heat sealed. Placed at 10 ft. (3.05 m) intervals.
n.	Color: Open Tournament Blue: Item No. 21644.
o.	Color: Black: Item No. 21642. 
p.	Color: Dark Green: Item No. 21640.
5.	Douglas Batter's Eye: Item No. 39995BE. 
a.	Open mesh, vinyl coated polyester screen. Windbreak: 80 percent. 
b.	Size, Maximum (HxL): Up to 20 x 40 ft (6.1 x 2.2 m)
c.	Size: ___ x ___ ft. (___ x ___ m).
d.	Custom Digital Printing: ________. 
6.	Douglas Bleacher Enclosures: Item No. 21620BZ. Custom fabricated.
a.	Standards Compliance: ASBA and USTA.
b.	Material: Vinyl coated polyester with three-ply hem, reinforced screen perimeters, and brass grommets spaced every 12 to 18 inches (305 x 457 mm). 
c.	Architect is to provide measurements, photos, and/or sketches of bleachers and facility layout. 
d.	Privacy Screen: 150 Ft. Rolls. Material: 85-90 percent knit raschel and 100 percent high density polyethylene, UV stabilized, mildew and mold resistant.
e.	Color: Dark Green. 
f.	Color: Black. 
g.	Color: Blue. 
h.	Color: Brown. 
i.	Color: Beige. 
j.	Role Height: 44 inch (1118 mm).
k.	Role Height: 68 inch (1727 mm).
l.	Role Height: 92 inch (2337 mm).
7.	Privacy Screen: Finished Panels. Material: 85 to 90 percent knit raschel and 100 percent high density polyethylene fiber, UV stabilized, mildew and mold resistant with hems and grommets.
a.	Panel Dimensions and Color:
1)	Size: 68 inch x 50 ft. (1727 mm x 15.25 m), Black. Item No. 26928B. 
2)	Size: 92 inch x 50 ft. (2337 mm x 15.25 m), Black. Item No. 26932B.
3)	Size: 68 inch x 50 ft. (1727 mm x 15.25 m), Dark Green. Item No. 26928G. 
4)	Size: 92 inch x 50 ft. (2337 mm x 15.25 m), Dark Green. Item No. 26932G.
b.	Tie Wrap: TR-120P. 8 inch. Item No. 31657. Pack of 100.
1)	Break Strength: 120 lbs. (54.43 kg).
c.	Tie Wrap: TR-120XL. 14 inch. Item No. 31655. Pack of 100.
1)	Break Strength: 120 lbs. (54.43 kg). 
d.	Tie Wrap: TR-120XL. 17 inch. Item No. 31652. Pack of 100.
1)	Break Strength: 120 lbs. (54.43 kg).
e.	Tie Wrap: TR-50P. 7 inch. Item No. 31656. Pack of 100.
1)	Break Strength: 50 lbs. (22.68 kg).
f.	Tie Wrap: TR-50XL. 14 inch. Item No. 31651. Pack of 100.
1)	Break Strength: 50 lbs. (22.68 kg).
D.	Bases, Home Plates, Pitching Rubbers and Accessories.
1.	Base Accessories:
a.	Dual Stanchion Ground Sleeve:
1)	Item No. 36592. Official Ground Sleeve. 24 inch (610 mm) length.
2)	Item No. 36593. Youth Ground Sleeve. 18 inch (457 mm) length.
b.	Base Plug with Indicator: Item No. 36514.
1)	High visibility feathered top. Fits into ground anchors. Indicator whisker colors vary.
c.	Dig Out Tool: Item No. 36560.
1)	Tempered steel with wooden handle. For dirt and debris removal from ground sleeves.
d.	Base Ground Sleeve: Item No. 36564. 1-1/2 inch n(38 mm) square steel tubing. 8 inch (203 mm) long.
e.	Round Orange Cap Base Anchor Plug: Item No. 36512.
1)	Plug: 1 x 1 inch, (25 x 25 mm.) Fits into the 1-1/2 inch (38 mm) Base Ground Sleeve. Safe or use with tractors, drags and rakes.
f.	Square Black Base Plug: Item No. 36513.
1)	Safe or use with tractors, drags and rakes. 
2.	Bases:
a.	Soft Touch Turf Bases: T Series . Item No. 36546B. Warranty: 1 Year. Rawlings, cut resistant polyurethane, molded, and compressible. For use on synthetic fields with 1 inch (25 mm) turf depth. Not for use with carpet style turf.
1)	Base Dimensions: 15 x 15 x 1-1/2 inch (381 x 381 x 38 mm).
2)	Accessory Items:
a)	Home plates.
b)	Pitching rubbers.
c)	Single orange base.
b.	Orange Soft Touch Turf Base. Item No. 36547. Warranty: 1 Year. Rawlings, cut resistant polyurethane, and compressible. For use with white T15 based on synthetic fields with 1 inch (25 mm) turf depth. Not for use with carpet style turf.
1)	Base Dimensions: 15 x 15 x 1-1/2 inch (381 x 381 x 38 mm).
2)	Accessory Items:
a)	Home plates.
b)	Pitching rubbers.
c)	Set of three white bases.
c.	Hollywood Impact Double First Base:
1)	Item No. 36528: Double Base. 
2)	Item No. 36530H: First Base with Two Bases. 
3)	Rawlings, double first base. Regulation sized white for fielders and orange for outside base. 6 inch (152 mm) stanchions attached to each base. Stabilized with chevron pattern on underside.
4)	Base Dimensions: Official 15 x 15 x 2-1/2 inch (381 x 381 x 64 mm).
5)	Accessory Items:
a)	Ground plugs.
b)	Anchors.
d.	Hollywood Impact First Base Set: Item No. 36526. Three bases.
1)	Rawlings, molded, compressible rubber. 6 inch (152 mm) stanchions attached to each base. Stabilized with chevron pattern on underside.
2)	Base Dimensions: Official 15 x 15 x 2-1/2 inch (381 x 381 x 64 mm).
3)	Accessory Items:
a)	Ground plugs.
b)	Anchors.
e.	Hollywood Impact Kwik-Release Base Sets: Babe Ruth League, Cal Ripken Baseball and approved for Little League play. 
1)	Double First Base with Two Bases, Youth: Item No. 36531.
2)	Rawlings, compressible base, disengages from platform upon hard impact. 
3)	Orange Platform: Includes 6 inch (152 mm) stanchion and soft tabs interconnected with tabs on underside of top base.
4)	Base Dimensions: Official 15 x 15 x 2-1/2 inch (381 x 381 x 64 mm).
5)	Accessory Items:
a)	Home plates.
b)	Pitching rubbers.
f.	Varsity Double First Base with Two Bases: Item No. 36531V.
1)	Rawlings compressible base. Disengages from platform upon hard impact. Orange Platform: Includes 6 inch (152 mm) stanchion and soft tabs interconnected with tabs on underside of top base.
2)	Base Dimensions: Official 15 x 15 x 2-1/2 inch (381 x 381 x 64 mm).
3)	Accessory Items:
a)	Ground plugs.
b)	Anchors.
g.	Impact Throw Down Bases, Set of 3: Item No. 36555. 
1)	Rawlings flexible, compressible bases with waffle bottom.
2)	Base Dimensions: Official 15 x 15 x 2-1/2 inch (381 x 381 x 64 mm).
h.	Original Jack Corbett MLB Hollywood Base: Item No. 36518. 
1)	Three bases with extended tapered lip. UV and weather resistant. Stanchions: 6 inch (152 mm.
2)	Size: 15 inch (381 mm) sq. 
3)	Size: 18 inch (457 mm) sq. 
4)	Accessory Items:
a)	Ground plugs.
b)	Anchors.
3.	Home Plates:
a.	Soft Touch Turf Home Plate: Item No. 36548. Warranty: 1 Year. 
1)	Cut resistant polyurethane, molded, compressible. For use on synthetic fields with 1 inch (25 mm) turf depth. Not for use with carpet style turf.
2)	Base Dimensions: 18-5/8 x 8-3/4 x 5/8 inch (473 x 222 x 16 mm), with 15/16 inch (24 mm) barbs.
3)	Accessory Items:
a)	Pitching rubber.
b)	Single orange.
c)	Set of 3 bases.
b.	Bury-All Home Plate: Item No. 36540.
1)	Rawlins, non-skid molded rubber with beveled edges, black, and stabilized waffle bottom. 
c.	Safety First Beveled Edge Five-Spike Home Base Plate: Item No. 36544.
1)	Rawlings home plate with beveled edge, black, and five metal spikes. 
2)	Plate Size: Official. 
d.	Anchor Home Plate: Item No. 36542. 
1)	Rawlings Pro, molded rubber with stanchion mounted steel plate and ground anchor.
e.	Hollywood MLB Bury-All Home Plate: Item No. 36540H. 
1)	Rawlings/MLB non-skid molded rubber with waffle bottom for permanent installation. 
f.	Hollywood MLB Pro Style Home Plate, Universal Mount: Item No. 36545.
1)	Rawlings, steel backed molded rubber plate with ground anchor and 6 inch (152 mm) stanchion for permanent installation and spikes, zinc plated, for temporary installation. Include one anchor and one plug. 
4.	Pitching Rubbers:
a.	Soft Touch Turf Pitching Rubber: Item No. 36549. Warranty: 1 Year.
1)	Material: Cut resistant polyurethane. For use on synthetic fields with 1 inch (25 mm) turf depth. Not for use with carpet style turf.
2)	Dimensions: 24-1/4 x 6-1/8 x 3/4 inch (616 x 156 x 19 mm) with 15/16 inch (24 mm) barbs.
3)	Accessories:
a)	Home plates.
b)	Orange base.
c)	Set of three bases.
b.	Official Size Hollywood 4-Way MLB Pitching Rubber: Item No. 36572H.
1)	Material: Molded rubber with interior aluminum tube. For burying in pitcher's mound.
2)	Size: 6 x 24 inch (152 x 610 mm). 
c.	Economy Pitcher's Rubber with Spikes and Metal Inserts:
1)	Item No. 36556: Size: Official: 6 x 24 inch (152 x 610 mm).
2)	Item No. 36558: Size: Youth: 4 x 18 inch (102 x 457 mm). 
3)	Rawlings, heavy-duty rubber with three metal spikes.
d.	Pro Step Down Pitching Rubber, Official Size: Item No. 36576H.
1)	Rawlings Pro, regulation size, heavy-duty rubber with waffle bottom.
e.	Step Down Pitching Rubber - Pitcher's Mound Rubber: 
1)	Item No. 36576: Official Size: 24 inch (610 mm).
2)	Item No. 36578: Youth Size: 18 inch (457 mm).
3)	Rawlings, heavy-duty rubber with solid bottom. 
E.	Batting Cages, Tunnels, Tunnel Nets and Dividers, Hitting Stations, Indoor Batting Tunnel Kit:
1.	Tunnel Frames
a.	Douglas Batting Tunnel Frames: Item No. 66216. 
b.	Douglas Double Batting Tunnel Frames: Item No. 66216D. 
c.	Douglas Triple Batting Tunnel Frames: Item No. 66216T.
d.	Warranty: 5 Year Limited. 
e.	Standards Compliance: NFHS, NCAA, IAAF, and ASBA. 
f.	Batting Tunnel Length: 55 ft. (16.75 m).
g.	Batting Tunnel Length: 70 ft. (21.3 m).
h.	Batting Tunnel Length: 75 ft. (22.9 m).
i.	Batting Tunnel Width: 12 ft. (3.7 m).
j.	Batting Tunnel Width: 14 ft. (4.3 m).
k.	Frame: Upright Poles: 
1)	Heavy-Duty Steel Tubing: Six, 4 inch (102 mm) square. Wall: 3/16 inch (5 mm). Height: 14 ft. (4.3 m).
2)	Reinforcement Steel Crossbars: 2-3/8 inch (60 mm) OD. Wall thickness: 7 ga. Finish: Zinc Flo-coat galvanized, for attachment of steel cables for net attachment, with cross cable. 
3)	Finish: Powder coated. Color: Black.
l.	Ground Sleeves: 4 inch (102 mm) sq., 24 inch (610 mm) aluminum. 
m.	Maximum Installed Net Height: 12 per ft. (3.7 per m).
n.	Hardware: 
1)	Cables: For attachment to net support crossbars. Includes quick links, turnbuckles, cable clamps and carabiner clips. 
2)	Cable Size: 1/4 inch (6 mm) diameter. Galvanized, UV, and weather resistant. Break Strength: 6100 lbs. (2766.91 kg). 
o.	Accessories:
1)	Batting tunnel nets. 
2.	Douglas Max Batting Tunnel Frames: Item No. 66470. Warranty: 7 Year Limited. 
a.	Standards Compliance: NFHS, NCAA, IAAF, and ASBA. 
b.	Upright Poles: Heavy-duty steel. 8-5/8 inch (219 mm) diameter. Wall Thickness: 0.322 inch (8 mm) wall thickness. Height: 16 ft. (4.9 m). Direct Bury: 4 ft. (1.23 m).
1)	Finish: Powder coated. Color: Black. 
c.	Maximum Installed Net Height: 11 ft. 6 inch (3.5 m). 
d.	Hardware: Cable: 1/4 inch (6 mm), galvanized, UV and weather resistant. Break Strength: 6100 lbs. (2766.91 kg). Quick links, turnbuckles, cable clamps and carabiner clips. 
e.	Accessories:
1)	Batting tunnel nets. 
3.	Douglas Max Double Batting Tunnel Frames: Item No. 66470D. Warranty: 7 Year Limited. 
a.	Standards Compliance: NFHS, NCAA, IAAF, and ASBA. 
b.	Included hardware installs two nets. 
c.	Upright Poles: Heavy-duty steel. 8-5/8 inch (219 mm). Wall Thickness: 0.322 inch (8 mm). Height: 16 ft. (4.9 m).
1)	Finish: Powder coated. Color: Black. 4 ft. (1.23 m) direct bury.
d.	Double T Poles: 8-5/8 inch (219 mm). Wall Thickness: 0.322 inch (8 mm).Wall Extensions: 6-5/8 x .25 inch (168 x 6 mm).
1)	Finish: Powder coated. Color: Black.
e.	Maximum Installed Net Height: 11 ft. 6 inch (3.5 m). 
f.	Hardware: 1/4 inch (6 mm) cable galvanized steel. UV and weather resistant, with 6100 lbs. (2766.91 kg) break strength. Quick links, turnbuckles, cable clamps and carabiner clips.
g.	Accessories:
1)	Batting tunnel nets. 
4.	Douglas Max Triple Batting Tunnel Frames: Item No. 66470T. Warranty: 7 Year Limited. 
a.	Standards Compliance: NFHS, NCAA, IAAF, and ASBA. 
b.	Included hardware installs three nets. 
c.	Upright Poles: Heavy-duty steel. 8-5/8 inch (219 mm). Wall Thickness: 0.322 inch (8 mm). Height: 16 ft. (4.9 m).
1)	Finish: Powder coated. Color: Black. 4 ft. (1.23 m) direct bury.
d.	Double T Poles: 8-5/8 inch (219 mm). Wall Thickness: 0.322 inch (8 mm).Wall Extensions: 6-5/8 x .25 inch (168 x 6 mm).
1)	Finish: Powder coated. Color: Black.
e.	Maximum Installed Net Height: 11 ft. 6 inch (3.5 m). 
f.	Hardware: 1/4 inch (6 mm) cable galvanized steel. UV and weather resistant, with 6100 lbs. (2766.91 kg) break strength. Quick links, turnbuckles, cable clamps and carabiner clips.
g.	Accessories: 
1)	Batting tunnel nets. 
5.	Douglas Hitting Station Systems: Warranty: 5 Years. 
a.	Item No. 66255: Two Poles, 55 ft. (16.75 m).
b.	Item No. 66270: Three Poles, 70 ft. (21.3 m) to 75 ft. (22.9 m).
c.	Poles: Heavy-duty steel, 4 inch (102 mm) sq. Height: 13 ft. (4 m).
1)	Buried in Ground Sleeve: 3 ft (0.9 m)
2)	Finish: Powder coated. Color: Black.
d.	Netting: No. 42 Twisted Knotted Nylon Black 1-3/4 inch (44 mm) SQ Mesh with Rope Border.
e.	Maximum Installed Net Height: 10 ft. (3.05 m).
f.	Hardware: Cable: 1/4 inch (6 mm), galvanized steel. UV and weather resistant. Break Strength: 6100 lbs. (2766.91 kg). Turnbuckles, c-snaps, collars, and ground sleeves.
6.	Indoor Batting Tunnel Accessory Cable Hardware Kit: Item No. 66213.
a.	Hardware required to set up and hang batting tunnel net for wall to wall installation:
1)	One Spool: 1/4 inch (6 mm) cable, 500 ft. (152.4 m).
2)	Seventy Steel C-Snaps. 
3)	Seventy Split Bracket Pulleys. 
4)	Six Turnbuckles. 
5)	Twelve 1/4 inch (6 mm) Wire Cable Clamps. 
6)	Six Eyebolts. 
7.	Indoor Batting Tunnel Ceiling Suspension Kit: Item No. 66219. 
a.	Hardware required to set up and hang batting tunnel net for wall to wall installation:
1)	One Spool: 1/4 inch (6 mm) cable, 500 ft. (152.4 m). 
2)	Two Spools: 1/8 inch (3 mm) cable, 1000 ft. (309 m). 
3)	Sixty 1/8 inch (3 mm) Wire Cable Clamps. 
4)	Twelve 1/4 inch (6 mm) Wire Cable Clamps. 
5)	Six Turnbuckles. 
6)	Six Eyebolts. 
7)	Seventy Steel C-Snaps. 
8)	Thirty Split Bracket Pulleys. 
8.	Indoor Batting Tunnel Tensioning Kit: Item No. 66200. 
a.	Hardware required to set up and hang batting tunnel net for wall to wall installation:
1)	Six Eyebolts. 
2)	Six 8 mm Spring Link Clips. 
3)	Six 3/8 inch (10 mm) Spring Link Clips. 
4)	Six Cables, 15 ft. (4.6 m).
5)	Three Pieces 3/8 inch (10 mm) High Strength Braided Hoisting Rope, 50 ft. (15.25 m). 
6)	Three Cam Lock Pulley Systems. 
7)	Three Swivel Clamps.
9.	Pole Pad 4-Sided for 4 inch square Batting Tunnel Pole: Item No. 39032. 
a.	Form Fitted Pole Protective Padding: For 4 inch (102 mm) square poles.
1)	Padding: 2 inch (51 mm) thick dense foam. UV and weather resistant. 
a)	Height: 72 inch (1829 mm).
2)	Cover: Vinyl. Secured by sewn-in Velcro straps. 
3)	Color: Dark Green.
4)	Color: Black. 
5)	Color: Royal Blue. 
6)	Color: Navy Blue. 
7)	Color: Red. 
10.	Vinyl Hitting Backdrop: Item No. 26460. 
a.	Material: 18 oz. sq. yd., vinyl. Color: Black. Reinforced perimeter hem with grommets. Size: 6 x 5 ft (1.9 x1.5 m). 
b.	Includes C-Snaps. 
c.	White printed hitting target. 
11.	Douglas No. 42 Knotted Twisted HDPE Batting Tunnel Nets: Warranty: 3 Years.
a.	Size: Item No. 36042: 12 x 12 x 35 ft. (3.7 x 3.7 x 10.7 m).
b.	Size: Item No. 36048: 12 x 12 x 55 ft. (3.7 x 3.7 x 16.75 m).
c.	Size: Item No. 36043: 12 x 12 x 70 ft. (3.7 x 3.7 x 21.3 m).
d.	Size: Item No. 36046: 12 x 14 x 55 ft. (3.7 x 4.3 x 16.75 m).
e.	Size: Item No. 36045: 12 x 14 x 70 ft. (3.7 x 4.3 x 21.3 m).
f.	Size: Item No. 36049: 12 x 14 x 75 ft. (3.7 x 4.3 x 22.9 m).
g.	Netting: No. 42 knotted, twisted HDPE, 1-3/4 inch (44 mm) sq. mesh. Sewn Rope Border: 5/16 inch (8 mm). Rope Tails: 6 inch (152 mm). Sewn hanging loops. Top center rope and overlap-style entryways. UV, weather, and mildew resistant. Break Strength: 290 lbs. (131.54 kg). 
12.	Douglas BT-PRO 3.5 Knotted Braided HDPE Batting Tunnel Nets: Warranty: 4 Years. 
a.	Size: Item No. 36038: 12 x 12 x 55 ft. (3.7 x 3;7 x 16.75 m).
b.	Size: Item No. 36033: 12 x 12 x 70 ft. (3.7 x 3.7 x 21.3 m).
c.	Size: Item No. 36036: 12 x 14 x 55 ft. (3.7 x 4.3 x 16.75 m).
d.	Size: Item No. 36035: 12 x 14 x 70 ft. (3.7 x 4.3 x 21.3 m).
e.	Size: Item No. 36039: 12 x 14 x 75 ft. (3.7 x 4.3 x 22.9 m).
f.	Size: __ x __ x __ ft. (__ x __ x ___ m)
g.	Standards Compliance: NFHS, NCAA, IAAF, and ASBA. 
h.	Netting: Knotted, braided HDPE, 1-3/4 inch (44 mm) sq. mesh with 5/16 inch (8 mm) sewn rope border. Top center rope and overlap-style entryways. UV, weather, and mildew resistant. Break Strength: 325 lbs. (147.42 kg)
1)	Reinforced vinyl top and center border. 
13.	Batting Tunnel Net Saver/Divider:
a.	Size: 12 x 12 ft. (3.7 x 3.7 m).
b.	Size: 12 x 14 ft. (3.7 x 4.3 m).
c.	Netting Panel: No. 48 knotted, twisted nylon netting, black. 1-3/4 inch (44 mm) sq. mesh with sewn rope border. UV and weather resistant. Break Strength: 459 lbs. (208.20 kg). 
F.	Outfield Products:
1.	Aluminum Foul Poles: Semi-permanent installation.
a.	Size: 15 ft. (4.6 m) Above Ground: Item No. 36651.
1)	Material: Aluminum, 4 inch (102 mm) OD pipe, with caps or base plate mounting system.
2)	Wing: 7 ft (2.1 m). Material: 1/8 inch (3 mm) stamped aluminum sheet wing with double reinforced bends, beginning at 8 ft. (2.5 m) above finished grade.
3)	Finish: Powder coated. Color: Yellow.
4)	Mounting: Ground sleeved.
5)	Mounting: Plate. 
b.	Size: 20 ft. (6.1 m) Above Ground: Item No. 36652.
1)	Material: Aluminum, 4 inch (102 mm) OD pipe, with caps or base plate mounting system.
2)	Wing: 12 ft. (3.7 m). Material: 1/8 inch (3 mm) stamped aluminum sheet wing with double reinforced bends, beginning at 8 ft. (2.5 m) above finished grade.
3)	Finish: Powder coated. Color: Yellow.
4)	Mounting: Ground sleeved.
5)	Mounting: Plate. 
c.	Size: ___ ft. (___ mm) Above Ground.
1)	Material: Aluminum, 4 inch (102 mm) OD pipe, with caps or base plate mounting system.
2)	Wing: ___ft., ___ m).Material: 1/8 inch (3 mm) stamped aluminum sheet wing with double reinforced bends, beginning at 8 ft. (2.5 m) above finished grade.
3)	Finish: Powder coated. Color: Yellow.
4)	Mounting: Ground sleeved.
5)	Mounting: Plate. 
d.	Size: 30 ft. (9.1 m) Above Ground: Item No. 36653. 
1)	Material: Aluminum, 6.625 inch (168 mm) OD pipe, with caps or base plate mounting system.
2)	Wing: 22 ft. (6.7 m). Material: 1/8 inch (3 mm) stamped aluminum sheet wing with double reinforced bends, beginning at 8 ft. (2.5 m) above finished grade.
3)	Finish: Powder coated. Color: Yellow.
4)	Mounting: Ground sleeved.
5)	Mounting: Plate. 
e.	Size: 40 ft. (12.2 m) Above Ground: Item No. 36654.
1)	Material: Aluminum, 6.625 inch (168 mm) OD pipe, with caps or base plate mounting system.
2)	Wing: 32 ft. (9.8 m). Material: 1/8 inch (3 mm) stamped aluminum sheet wing with double reinforced bends, beginning at 8 ft. (2.5 m) above finished grade.
3)	Finish: Powder coated. Color: Yellow.
4)	Mounting: Ground sleeved.
5)	Mounting: Plate. 
f.	Size: ___ ft. (___ m) Above Ground:
1)	Material: Aluminum, 6.625 inch (168 mm) OD pipe, with caps or base plate mounting system.
2)	Wing: ___ ft. (___ m). 1/8 inch (3 mm) stamped aluminum sheet wing with double reinforced bends, beginning at 8 ft. (2.5 m) above finished grade.
3)	Finish: Powder coated. Color: Yellow.
4)	Mounting: Ground sleeved.
5)	Mounting: Plate. 
2.	Protective Fence Guard for Chain Link Fences:
a.	Item No. 36982. Premium. Warranty: 3 Years.
1)	Size: Twelve, 4 x 2-5/8 inch (102 x 92 mm) x 7 ft. (2.1 m) sections. 84 ft. (25.6 m) total.
2)	Material: Heavy-duty polyethylene, teardrop profile. UV resistant. Pre-drilled every 24 inch (610 mm). Wall thickness 0.10 inches
3)	Zip-Ties: included. 
4)	Color: Forest Green. 
5)	Color: Red. 
6)	Color: Blue. 
7)	Color: Orange. 
8)	Color: White. 
9)	Color: Black. 
b.	Item No. 36984. Standard. Warranty: 5 Years. 
1)	Size: Twelve, 4-1/2 x 3 inch (114 x 76 mm) x 7 ft. (2.1 m) sections. 84 ft. (25.6 m) total.
2)	Material: Heavy-duty polyethylene, teardrop profile. UV resistant. Pre-drilled every 24 inch (610 mm). Wall thickness 0.07 inches
3)	Zip-Ties: included. 
4)	Color: Yellow. 
5)	Color: Red. 
6)	Color: Blue. 
3.	Poly-Cap, Protective Fence Cap for Chain-Link Fences: Warranty: 2 Years.
a.	Unit Size: Roll, 100 ft.: Item No. 36960.
b.	Unit Size: Roll, 250 ft.: Item No. 36966.
c.	Standards Compliance: ASBA.
d.	Material: 4-1/2 inch (114 mm) diameter and pre-slit. Polyethylene. UV and weather resistant.
e.	Color: Bright Safety Yellow.
f.	Color: Black.
4.	Professional Foul Pole Pairs: For direct bury or installation in ground sleeves. Heavy-Duty Steel. Warranty: 1 Year. 
a.	Size Above Ground: 12 ft. (3.7 m). Wings: 6 ft. (1.9 m). Item No. 36650B.
b.	Size Above Ground: 15 ft. (4.6 m). Wings: 8 ft. (2.5 m). Item No. 36650A. 
c.	Size Above Ground: 20 ft. (6.1 m) Wings: 12 ft. (3.7 m. Item No. 36650.
d.	Ground Sleeves: Item No. 36650GS.
e.	Standards Compliance: NFHS, NCAA, IAAF, and ASBA compliant. 
f.	Material: 3-1/2 inch (89 mm) OD. Wall thickness: 13 ga. 
1)	Wing: 18 inch (457 mm) wide expanded metal. 
g.	Finish: Powder coated. Color: Bright Safety Yellow.
5.	Vinyl Mesh Outfield Distance Markers:
a.	Windscreen/banner with reinforced, double-stitched perimeter and grommets. 
b.	Item No. 36815A. Each.
c.	Item No. 36815B. Set of Three.
d.	Item No. 36815C. Set of Five.
e.	Number Height: 16 inch (406 mm). Permanently UV printed. 
f.	Vertical Banner Dimensions: 60 x 24 inch (1524 x 610 mm). 
g.	Horizontal Banner Dimensions: 24 x 48 inch (610 x 1219 mm). 
h.	Banner Color: Black.
i.	Banner Color: Dark Green.
j.	Banner Color: Royal Blue.
k.	Banner Color: Navy Blue.
l.	Banner Color: Purple.
m.	Banner Color: Burgundy.
n.	Banner Color: Red.
o.	Banner Color: Brown.
p.	Banner Color: Orange.
q.	Banner Color: Yellow.
r.	Banner Color: Gray.
s.	Banner Color: ________.
t.	Banner Color: As determined by the Architect or as detailed on the Drawings.
u.	Printing Color: ________.
v.	Printing Color: As determined by the Architect or as detailed on the Drawings.
w.	Printed Numbers: ________.
x.	Printed numbers: As determined by the Architect or as detailed on the Drawings.
6.	Vinyl Outfield Distance Markers:
a.	Item No. 36816A. Each.
b.	Item No. 36816B. Set of Three.
c.	Item No. 36816C. Set of Five.
d.	Material: 18 oz. viny. Reinforced, double-stitched perimeter and grommets.
e.	Number Height: 16 inch (406 mm). Permanently UV printed. 
f.	Vertical Banner Dimensions: 60 x 24 inch (1524 x 610 mm). 
g.	Horizontal Banner Dimensions: 24 x 48 inch (610 x 1219 mm). 
h.	Banner Color: Black.
i.	Banner Color: Dark Green.
j.	Banner Color: Royal Blue.
k.	Banner Color: Navy Blue.
l.	Banner Color: Purple.
m.	Banner Color: Red.
n.	Banner Color: Yellow.
o.	Banner Color: Gray.
p.	Banner Color: White. 
q.	Banner Color: ________.
r.	Banner Color: As determined by the Architect or as detailed on the Drawings.
s.	Printing Color: ________.
t.	Printing Color: As determined by the Architect or as detailed on the Drawings.
u.	Printed Numbers: ________.
v.	Printed numbers: As determined by the Architect or as detailed on the Drawings.
G.	Protective Screens:
1.	Varsity Field Screen, 10 x 10 ft.: Item No. 36465.
a.	Frame: Steel tube. 1-1/2 inch (38 mm) OD. Welded gussets on each leg. Bolted installation. Finish: Powder coated. Color: Black.
b.	Net: No. 60. Braided. Color: Black. UV, and weather resistant. Pillow case style.
c.	Varsity Wheel Kit: Item No. 36469. Airless tires.
1)	Slip on and slip off installation with tightening screw.
2.	Varsity Field Screen, 6 x 4 ft.: Item No. 36468. 
a.	Frame: Steel tube, 1-1/2 inch (38 mm) OD. Welded gussets on each leg. Bolted installation. Finish: Powder coated. Color: Black.
b.	Net: No. 60. Braided. Color: Black. UV, and weather resistant. Pillow case style.
c.	Varsity Wheel Kit: Item No. 36469. Airless tires.
1)	Slip on and slip off installation with tightening screw.
3.	Varsity Field Screen, 7 x 7 ft.: Item No. 36463.
a.	Frame: Steel tube, 1-1/2 inch (38 mm) OD. Welded gussets on each leg, Bolted installation. Finish: Powder coated. Color: Black.
b.	Net: No. 60. Braided. Color: Black. UV, and weather resistant. Pillow case style.
c.	Varsity Wheel Kit: Item No. 36469. Airless tires.
1)	Slip on and slip off installation with tightening screw.
4.	Varsity Field Screen, 8 x 10 ft.: Item No. 36464.
a.	Frame: Steel tube, 1-1/2 inch (38 mm) OD. Welded gussets on each leg, Bolted installation. Finish: Powder coated. Color: Black. 
b.	Net: No. 60. Braided. Color: Black. UV, and weather resistant. Pillow case style. 
c.	Varsity Wheel Kit: Item No. 36469. Airless tires.
1)	Slip on and slip off installation with tightening screw. 
5.	Varsity L-Screen, 7 x 7 ft.: Item No. 36460.
a.	Frame: Steel tube, 1-1/2 inch (38 mm) OD. Welded gussets on each leg. 3 x 3 ft (0.9 m) cutout. Bolted installation. Finish: Powder coated. Color: Black.
b.	Net: No. 60. Braided. Color: Black. UV, and weather resistant. Pillow case style. 
c.	Varsity Wheel Kit: Item No. 36469. Airless tires.
1)	Slip on and slip off installation with tightening screw. 
6.	Varsity Mini L-Screen, 5 x 7 ft.: Item No. 36461. 
a.	Frame: Steel tube, 1-1/2 inch (38 mm) OD. Welded gussets on each leg. Bolted installation. Finish: Powder coated. Color: Black. 
b.	Net: No. 60. Braided. Color: Black. UV, and weather resistant. Pillow case style. 
c.	Varsity Wheel Kit: Item No. 36469. Airless tires.
1)	Slip on and slip off installation with tightening screw. 
7.	Varsity Sock Net Screen, 7 x 7 ft.: Item No. 36466.
a.	Frame: Steel tube, 1-1/2 inch (38 mm) OD. Welded gussets on each leg. Bolted installation. Finish: Powder coated. Color: Black. 
b.	Net: No. 60. Braided. Color: Black. UV, and weather resistant. Pillow case style. 
c.	Target: 49 x 53 inch (1245 x 1346 mm).
d.	Varsity Wheel Kit: Item No. 36469. Airless tires.
1)	Slip on and slip off installation with tightening screw. 
8.	Varsity Softball Pitching Screen, 7 x 7 ft.: Item No. 36467.
a.	Frame: Steel tube, 1-1/2 inch (38 mm) OD. Welded gussets on each leg. Bolted installation. Finish: Powder coated. Color: Black. 
b.	Net: No. 60. Braided. Color: Black. UV, and weather resistant. Pillow case style. 
c.	Cutout: 30 x 24 inch (762 x 610 mm), 21 inch (533 mm) from ground.
d.	Varsity Wheel Kit: Item No. 36469. Airless tires.
1)	Slip on and slip off installation with tightening screw. 
9.	Douglas Replacement Slip-On Style Net: 7x5 ft. Item No. 36446.
a.	3.5 mm knotless HTPP, 1-3/4 inch (44 mm) sq. mesh, with bottom lace cord. UV and weather resistant. 325 lbs. (147.42 kg) break strength. 
10.	Douglas Replacement Slip-On Style Net: 7x7 ft. Item No. 36449.
a.	3.5 mm knotless HTPP, 1-3/4 inch (44 mm) sq. mesh with bottom lace cord, UV, and weather resistant. 325 lbs.(147.42 kg) break strength.
11.	Douglas Replacement Slip-On Style Net: 7x7 ft. L-Screen. Item No. 36450.
a.	3.5 mm knotless HTPP, 1-3/4 inch (44 mm) sq. mesh with bottom lace cord, UV, and weather resistant. 325 lbs. (147.42 kg) break strength.
12.	Douglas Replacement Slip-On Style Net: 7x7ft. Sock Net. Item No. 36457.
a.	3.5 mm knotless HTPP, 1-3/4 inch (44 mm) sq. mesh with bottom lace cord, UV, and weather resistant. 325 lbs. (147.42 kg) break strength.
13.	Douglas Replacement Slip-On Style Net: 7x7 ft. Softball Pitching Net. Item No. 36462.
a.	3.5 mm knotless HTPP, 1-3/4 inch (44 mm) sq. mesh with bottom lace cord, UV, and weather resistant. 325 lbs. (147.42 kg) break strength.
14.	Douglas Replacement Slip-On Style Net: 8x8ft. L-Screen. Item No. 36451H. 
a.	3.5 mm knotless HTPP, 1-3/4 inch (44 mm) sq. mesh with bottom lace cord, UV, and weather resistant. 325 lbs. (147.42 kg) break strength.
15.	Varsity Wheel Kit: Item No. 36469. Airless tires.
a.	For use with 1-1/2 inch (38 mm) OD framed Varsity Screens. 
b.	Slip on and slip off installation with tightening screw. 
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until the substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
3.4	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.
B.	Manufacturer's Services: Coordinate manufacturer's services in accordance with appropriate sections in Division 01.
3.5	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturers recommendations. 
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION