SECTION 12 24 00

WINDOW SHADES

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2008 -  2026 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Manually operated, roll-up fabric interior window shades including mounting and operating hardware.
B.	Motorized, roll-up fabric interior window shades including motor operator, controls, and mounting hardware.
C.	Opaque window shade system: Manually operated, roll-up fabric opaque window shade system for complete blackout of window opening including side and bottom channels, headbox, manual operator, and mounting hardware.
D.	Opaque window shade system: Motorized, roll-up fabric opaque window shade system for complete blackout of window opening including side and bottom channels, headbox, motorized operator, controls, and mounting hardware.
1.2	RELATED SECTIONS
A.	Section 06 10 00 - Rough Carpentry.
B.	Section 07 90 00 - Joint Sealers.
C.	Section 09 21 16.33 - Gypsum Board Area Separation Wall Assemblies.
D.	Section 09 51 23 - Acoustical Tile Ceilings.
E.	Section 11 52 13.50 - Motorized Projection Screens.
F.	Section 11 52 13.50 - Motorized Projector Lifts.
G.	Division 16 [26] - Electrical.
1.3	REFERENCES
A.	NFPA 70 - National Electrical Code.
B.	NFPA 701-99 - Fire Tests for Flame-Resistant Textiles and Films.
C.	GREENGUARD Environmental Institute Gold.
D.	US Green Building Council.
E.	ANSI/WCMA A100.1-2022. For manual window shades with closed loop bead chains, all shades will meet all current standards mandated by the Consumer Product Safety Commission.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 33 26 - Submittal Procedures:
B.	Product Data: Manufacturer's data sheets on each product specified, including:
1.	Preparation instructions and recommendations.
2.	Installation and maintenance instructions.
3.	Styles, material descriptions, dimensions of individual components, profiles, features, finishes and operating instructions.
4.	NFPA Flame-Test: Passes NFPA 701 including certification from manufacturer that the fabrics sourced for this project comply with the test data provided.
5.	Storage and handling requirements and recommendations.
6.	Mounting details and installation methods.
7.	Typical wiring diagrams including integration of motor controllers with building management system, audiovisual and lighting control systems as applicable.
C.	Shop Drawings: Plans, elevations, sections, product details, installation details, operational clearances, wiring diagrams and relationship to adjacent work.
D.	LEED Submittals: Provide documentation of how the requirements of Credit will be met.
E.	Window Treatment Schedule: For all roller shades. Use same room designations as indicated on the Drawings, field verified window dimensions, quantities, type of shade, controls, fabric, and color, and include opening sizes and key to typical mounting details.
F.	Selection Samples: For each finish product specified, two complete sets of shade cloth options and aluminum finish color samples representing manufacturer's full range of available colors and patterns.
G.	Verification Samples: For each finish product specified, two complete sets of shade components, unassembled, demonstrating compliance with specified requirements. Shade fabric sample and aluminum finish sample as selected, representing actual product, color, and patterns. Mark face of material to indicate interior faces.
H.	Maintenance Data: Methods for maintaining roller shades, precautions regarding cleaning materials and methods, instructions for operating hardware and controls.
I.	Manufacturer's Certificates: Certify products meet or exceed specified requirements.
J.	Warranty: Properly executed manufacturers warranty.
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Obtain roller shades through one source from a single manufacturer with a minimum of twenty years documented experience in manufacturing products comparable to those specified in this section. Manufacturers that do not meet the required experience requirements must submit life cycle test data showing minimum 2000 complete operational cycles for each year of warranty showing no failure and that shade remains fit for use as a operable shade).
B.	NFPA Flame-Test: Passes NFPA 701. Materials tested shall be identical to products proposed for use.
C.	Mock-Up: Provide a mock-up of one of each type roller shade assembly specified for evaluation of mounting, appearance and accessories.
1.	Locate mock-up in window(s) designated by Architect.
2.	Do not proceed with remaining work until mock-up is accepted by Architect.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Do not deliver window shades until building is enclosed and construction within spaces where shades will be installed is substantially complete.
B.	Deliver products in manufacturer's original, unopened, undamaged containers with labels intact.
C.	Label containers and shades according to Window Shade Schedule.
D.	Store products in manufacturer's unopened packaging until ready for installation.
1.7	SEQUENCING
A.	Ensure that locating templates and other information required for installation of products of this section are furnished to affected trades in time to prevent interruption of construction progress.
B.	Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
1.8	PROJECT CONDITIONS
A.	Install roller shades after finish work and ambient temperature, humidity and ventilation conditions are maintained at levels recommended for project upon completion.
1.9	WARRANTY
A.	Hardware and Shade Fabric: Draper standard twenty-five year limited warranty.
B.	Motors and Controls: Draper standard five year limited warranty. 
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Draper Inc., which is located at:<BR />411 S. Pearl Street, P. O. Box 425<BR />Spiceland, IN 47385-0425<BR />Toll Free Tel: 800-238-7999<BR />Tel: 765-987-7999<BR />Fax: 866-637-5611<BR />Email: request info (drapercontract@draperinc.com);Web: http://www.draperinc.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements (01 60 00].
2.2	MANUALLY OPERATED WINDOW SHADES
A.	Manually Operated Window Shades with Independent Control: Manually operated, vertical roll-up, fabric window shade with components necessary for complete installation; Clutch-Operated FlexShade CLN as manufactured by Draper, Inc. 
1.	Operation: Bead chain and clutch operating mechanism allowing shade to stop when chain is released. Designed never to need adjustment or lubrication. Provide limit stops to prevent shade from being raised or lowered too far.
a.	Clutch mechanism: Fabricated from high carbon steel and molded fiberglass reinforced polyester or injected molded nylon. Minimum 20 lb. lifting capacity. White or Black color as selected by Architect.
b.	Spring-Assist Clutch: Adjustment-free system includes spring-assist components to reduce lifting forces required to raise the shade. Manufacturer shall provide estimated torque for shade unit. Spring-assist is recommended on estimated non-spring-assist torque above 6 lb-in; required on shades with an estimated torque higher than 15 lb-in.
c.	Bead chain loop: Polyester bead chain, Ivory.
d.	Bead chain loop: Polyester bead chain, Grey. 
e.	Bead chain loop: Polyester bead chain, White. 
f.	Bead chain loop: Polyester bead chain, Bronze. 
g.	Bead chain loop: Polyester bead chain, Black. 
h.	Bead chain loop: Stainless Steel.
i.	Bead Chain Hold Down: Spring-Loaded Tensioner complying with ANSI/WCMA A100.1-2022 safety standard.
j.	Idler Assembly: Provide roller idler assembly of molded nylon with adjustable or spring-loaded length idler pin to facilitate easy installation, and removal of shade for service.
2.	Single Roller Configuration:
a.	Mounting:
1)	Universal Mounting brackets.
2)	Endcaps only.
3)	Endcaps and fascia.
4)	Ceiling/Wall Style Headbox.
5)	Recessed Pocket Headbox.
b.	Brackets: Plated stamped steel. Provide size compatible with roller size.
1)	Mounted to ceiling.
2)	Mounted to wall.
3)	Mounted to jamb.
4)	Finish: White.
5)	Finish: Black.
c.	Endcaps: Stamped steel with universal design suitable for mounting to ceiling, wall, and jamb. Provide size compatible with roller size.
1)	Endcap covers: To match fascia or headbox color.
d.	Fascia: L shaped aluminum extrusion to conceal shade roller and hardware.
1)	Attachment: Snaps onto endcaps without requiring exposed fasteners of any kind. Fascia can be mounted continuously across two or more shade bands. No notching is required.
2)	Shape: Square Fascia Panel.
3)	Finish: Selected from Manufacturers standard range.
4)	Finish: Custom powder coat as selected by the Architect.
e.	Headbox Ceiling/Wall style: Aluminum fabrication with removable closure, endcaps, and back and top cover piece:
1)	Finish: Selected from Manufacturers standard range.
2)	Finish: Custom powder coat as selected by the Architect.
f.	Headbox, Pocket style: Aluminum fabrication with removable closure, endcaps, and U-shaped pocket:
1)	Selected from Manufacturers standard range
2)	Finish: Custom powder coat as selected by the Architect.
g.	Type D Shade pocket: Rectangular pocket and endcaps designed for recessed ceiling installation of window shades with ceiling tile lip.
1)	Material: Extruded aluminum alloy or steel with white finish.
2)	Size: 5 inches (127 mm) wide by 5-3/8 inches (137 mm) high.
3)	Closure Panel:
a)	1-1/2 (38 mm) closure dimension, recommended for bead chain operation.
4)	Pocket End Cap Kit: Metal endcaps with 7/8 inch (22 mm) lip for support of acoustical ceiling panel.
5)	Corners: Welded one-piece aluminum sections connecting to and matching pockets to allow continuous shade recess at ceiling corners.
h.	Wall Clip with Closure Panel: For site constructed ceiling recesses, provide removable closure panel to minimize slot for shade passage but allowing access to shade for maintenance.
1)	Material: Aluminum alloy with white epoxy paint finish.
2)	Tile Lip: Provide wall clip with 7/8 inch tile lip (22 mm).
3)	Closure width: 1-1/2 inches (38 mm).
4)	Closure width: 3 inches (76 mm).
5)	Closure Width: 5 inches (127 mm).
6)	Provide continuous wall clip, 1-3/4 (44 mm) by 3/16 inch (5 mm), for snap-in attachment of closure panel without fasteners.
i.	Aluminum Light Gap Reduction Channels: 
1)	L Angle - 3/4 inch by 1 inch (19 mm by 25 mm). 
2)	L Angle - 1 inch by 2-3/4 inches (25 mm by 70 mm). 
3)	U Channel - 1 inch by 2-1/2 inches (25 mm by 64 mm). 
4)	H Channel - 1 inch (25 mm) by 5 inches (127 mm). 
j.	Vinyl Light Gap Reduction Channels: 
1)	L Angle - 1-1/2 inches 3/4 inches (38 mm by 19 mm). 
k.	Interior Cable Guide Kit: 
1)	Interior cable hem bar finial. 
2)	Cable mount. 
3)	Cable. 
4)	Tension Stop. 
3.	Dual Roller Configuration / Mounting:
a.	Dual roller endcaps only. Endcaps for surface or recessed mounting of dual roller window shades. 1028 steel stamping.
b.	Dual roller fascia. Endcaps with fascia designed for surface mounting of dual roller window shades.
1)	Endcaps: 1028 steel stamping.
2)	Fascia: L-shaped cover of extruded aluminum, .060 wall. Assembly snaps onto endcaps without exposed fasteners.
3)	Size: Determined by manufacturer based on fabric size, weight, and thickness and window opening size.
4)	Finish: Selected from Manufacturers standard range.
5)	Finish: Custom powder coat as selected by the Architect.
c.	Dual roller with pocket headbox. Pocket and endcaps designed for recessed ceiling installation of dual roller window shades.
1)	Material: 18 gauge steel.
2)	Finish: White Inside/Grey Outside with white ceiling tile flange.
3)	Finish: Grey Inside/White Outside with white ceiling tile flange.
4)	Closure Panel Aluminum, without exposed fasteners:
a)	Front Tile Flange.
b)	Left Tile Flange.
c)	Right Tile Flange.
d)	Pre-drilled Mounting Holes.
e)	Pre-drilled Ventilation holes.
d.	Dual roller with ceiling/wall headbox. Fascia, L-shaped top/back, and endcaps designed for wall or ceiling installation of dual roller window shades.
1)	Endcaps: 1028 steel stamping.
2)	Fascia: L-shaped cover of extruded aluminum, .060 wall. Assembly snaps onto endcaps without exposed fasteners.
3)	Finish: Powder coat.
a)	Selected from Manufacturers standard range.
b)	Custom powder coat as selected by Design Professional
e.	Light Gap Reduction Channels. 
1)	Aluminum L Angle - 3/4 inch (19 mm) by 1 inch (25 mm). 
2)	Aluminum L Angle -1 inch (25 mm) by 2-3/4 inches (70 mm). 
3)	Vinyl L Angle-1-1/2 inches (38 mm) by 3/4 inch (19 mm). 
4)	U Channel -1 inch (25 mm) by 2-1/2 inches (64 mm) 
5)	H Channel - 1 inch (25 mm) by 5 inches (127 mm). 
4.	Roller Tube: Fabricated from extruded aluminum, galvanized steel, or enameled steel. Diameter, wall thickness, and material selected by manufacturer to accommodate shade type and size. Minimum roller diameter 1.5 inches. Tube diameters less than 1.5 inches shall not be acceptable unless manufacturer provides deflection analysis showing deflection limited to less than or equal to width (inches) /700 at 1.5X design load.
5.	Fabric connected to the roller tube with LSE (low surface energy) double sided adhesive specifically developed to attach coated textiles to metal. Adhesive attachment to eliminate horizontal impressions in fabric.
6.	Shade slat:
a.	Closed pocket elliptical slat: 1 inch (25 mm) aluminum elliptical slat inside of a 1-5/8 inch (41 mm) pocket with heat sealed ends.
b.	Open pocket elliptical slat: 1 inch (25mm) aluminum elliptical slat with plastic ends inside of a 1-5/8 inch (41 mm) pocket.
c.	Flat exposed hem bar: Small: 7/8 inch by 5/16 inch (22 mm by 8 mm) and Large 1-1/2 inch by 5/16 inch (38 mm by 8 mm) aluminum rectangular hem bar with plastic end caps. 
d.	Round exposed hem bar: Small 5/8 inch (16 mm) and Large 13/16 inch (21 mm) aluminum with plastic end caps.
B.	Heavy-Duty Manually Operated Window Shades with Independent Control: Manually operated, vertical roll-up, fabric window shade with components necessary for complete installation; Clutch-Operated FlexShade NEXD as manufactured by Draper, Inc. 
1.	Operation: Bead chain and clutch operating mechanism allowing shade to stop when chain is released. Designed never to need adjustment or lubrication. Provide limit stops to prevent shade from being raised or lowered too far.
a.	Spring-Assist Clutch: Adjustment-free system includes spring-assist components to reduce lifting forces required to raise the shade. Manufacturer shall provide estimated torque for shade unit. Spring-assist is recommended on estimated non-spring-assist torque above 6 lb-in; required on shades with an estimated torque higher than 15 lb-in.
b.	Bead chain loop: Polyester bead chain, Ivory.
c.	Bead chain loop: Polyester bead chain, Grey. 
d.	Bead chain loop: Polyester bead chain, White. 
e.	Bead chain loop: Polyester bead chain, Bronze. 
f.	Bead chain loop: Polyester bead chain, Black.
g.	Bead chain loop: Stainless Steel.
h.	Bead Chain Hold Down: Spring-Loaded Tensioner complying with ANSI/WCMA A100.1-2022 safety standard.
i.	Idler end: Height adjustable idler end allows fine leveling adjustments after installation-min plus or minus 1/8 inch without shimming brackets. Contains at least two entry points for the idler end. Safety engagement feature requires idler end pin to have a minimum engagement in bracket, ensuring that the idler end cannot fall out of the bracket due to lack of pin engagement.
2.	Single Roller Configuration:
a.	Mounting:
1)	Endcaps only.
2)	Endcaps and fascia.
3)	Endcaps and headbox.
4)	Cassette Headbox.
a)	Complete Cassette.
b)	Back only.
c)	Top only.
d)	Top and back only
5)	Cassette Style with Fascia.
a)	Back with Fascia.
b)	Top with Fascia.
c)	Top and back with Fascia.
b.	Endcaps: 1018 stamped steel. Suitable for mounting to ceiling, wall, and jamb. Field adjustable from ceiling to wall. No "L" angle required for wall mounting. Contains at least two entry points for the idler end.
1)	Endcap covers: To match fascia or headbox color.
2)	Mounted to ceiling.
3)	Mounted to wall.
4)	Mounted to jamb.
c.	Fascia: L shaped aluminum extrusion to conceal shade roller and hardware.
1)	Attachment: Snaps onto endcaps without requiring exposed fasteners of any kind. Fascia can be mounted continuously across two or more shade bands. Notching of fascia to provide for chain clearance is NOT acceptable. Fascia height to match throughout space unless specifically approved in advance by the Architect
2)	Selected from Manufacturers standard range.
3)	Finish: Custom powder coat as selected by the Architect.
d.	Headbox Ceiling/Wall style: Aluminum fabrication with a top/back cover and fascia with endcaps for mounting:
1)	Selected from Manufacturers standard range.
2)	Finish: Custom powder coat as selected by the Architect.
e.	Headbox, Pocket style: Aluminum fabrication with removable closure, endcaps, and U-shaped pocket:
1)	Selected from Manufacturers standard range.
2)	Finish: Custom powder coat as selected by the Architect.
f.	Type D Shade pocket: Rectangular pocket with ceiling tile lip designed for recessed ceiling installation of window shades.
1)	Material: Extruded aluminum alloy with white epoxy paint finish.
2)	Size: 5 inches (127 mm) by 5-3/8 inches (137 mm) high.
3)	Closure Panel:
a)	1-1/2 (38 mm) closure dimension.
b)	3 inch (78 mm)
4)	Pocket Endcap Kit: Endcaps with 7/8 inch (22 mm) lip for support of acoustical ceiling panel.
5)	Corners: Welded one-piece aluminum sections connecting to and matching pockets to allow continuous shade recess at ceiling corners.
6)	Pocket ends: Welded one-piece aluminum sections connecting to and matching pockets.
g.	Wall Clip with Closure panel: For site constructed ceiling recesses, provide removable closure panel to minimize slot for shade passage but allowing access to shade for maintenance.
1)	Material: Aluminum alloy with white epoxy paint finish.
2)	Tile Lip: Provide wall clip with 7/8 inch tile lip (22 mm).
3)	Closure width: 1-1/2 inches (38 mm).
4)	Closure width: 3 inches (75 mm).
5)	Closure Width: 5 inches (127 mm).
6)	Provide continuous wall clip, 1-3/4 (44 mm) by 3/16 inch (5 mm), for snap-in attachment of closure panel without fasteners.
h.	Cassette Headbox Fully assembled. Standard consists of fascia and two interlocking extrusions that form a back/top cover. Suitable for pocket installation. Size: 3-3/8 inch by 3-3/8 inch (86 mm by 86 mm):
1)	Finish: Selected from Manufacturers standard range.
2)	Finish: Custom powder coat as selected by the Architect.
i.	Cassette Style with Fascia. Standard consists of fascia and two interlocking extrusions that form a back/top cover. Size: 3-3/8 inch by 3-3/8 inch (86 mm by 86 mm):
1)	Finish: Selected from Manufacturers standard range.
2)	Finish: Custom powder coat as selected by the Architect.
j.	Roller Tube: Fabricated from extruded aluminum, galvanized steel, or enameled steel. Diameter, wall thickness, and material selected by manufacturer to accommodate shade type and size. Minimum roller diameter 1.5 inches. Tube diameters less than 1.5 inches shall not be acceptable unless manufacturer provides deflection analysis showing deflection limited to less than or equal to width (inches) /700 at 1.5X design load.
1)	Fabric to tube attachments: Spline fabric/roller attachment system to allow shade fabric to be removed from roller without having to remove roller from brackets.
k.	Shade slat:
1)	Closed pocket elliptical slat: 1 inch (25 mm) aluminum elliptical slat inside of a 1-5/8 inch (41 mm) pocket with heat sealed ends.
2)	Open pocket elliptical slat: 1 inch (25mm) aluminum elliptical slat with plastic ends inside of a 1-5/8 inch (41 mm) pocket.
3)	Flat exposed hem bar: Small: 7/8 inch by 5/16 inch (22 mm by 8 mm) and Large 1-1/2 inch by 5/16 inch (38 mm by 8 mm) aluminum rectangular hem bar with plastic end caps. 
4)	Round exposed hem bar: Small 5/8 inch (16 mm) and Large 13/16 inch (21 mm) aluminum with plastic end caps.
l.	Aluminum Light Gap Reduction Channels
1)	L Angle - 3/4 inch by 1 inch (19 mm by 25 mm).
2)	L Angle - 1 inch by 2-3/4 inches (25 mm by 70 mm).
3)	U Channel - 1 inch by 2-1/2 inches (25 mm by 64 mm).
4)	H Channel - 1 inch (25 mm) by 5 inches (127 mm).
m.	Vinyl Light Gap Reduction Channels
1)	L Angle - 1-1/2 inches 3/4 inches (38 mm by 19 mm).
n.	Interior cable guide kit
1)	Interior cable hem bar finial.
2)	Cable mount.
3)	Cable.
4)	Tension Stop
3.	Dual Roller Configuration / Mounting:
a.	Dual roller endcaps only. Endcaps for surface or recessed mounting of dual roller window shades. 1028 steel stamping.
b.	Dual roller fascia. Endcaps with fascia designed for surface mounting of dual roller window shades.
1)	Endcaps: 1028 steel stamping.
2)	Fascia: L-shaped cover of extruded aluminum, .060 wall. Assembly snaps onto endcaps without exposed fasteners.
3)	Size: 4-3/4 inches deep x 7 inches high x length required by window opening.
4)	Finish: Selected from Manufacturers standard range.
5)	Finish: Custom powder coat as selected by the Architect.
c.	Dual roller with pocket headbox. Pocket and endcaps designed for recessed ceiling installation of dual roller window shades.
1)	Material: 18 gauge steel.
2)	Finish: White Inside/Grey Outside with white ceiling tile flange.
3)	Finish: Grey Inside/White Outside with white ceiling tile flange.
4)	Closure Panel Aluminum, without exposed fasteners:
a)	Front Tile Flange.
b)	Left Tile Flange.
c)	Right Tile Flange.
d)	Pre-drilled Mounting Holes.
e)	Pre-drilled Ventilation holes.
d.	Dual roller with ceiling/wall headbox. Fascia, L-shaped top/back, and endcaps designed for wall or ceiling installation of dual roller window shades.
1)	Endcaps: 1028 steel stamping.
2)	Fascia: L-shaped cover of extruded aluminum, .060 wall. Assembly snaps onto endcaps without exposed fasteners.
3)	Finish: Powder coat.
a)	Selected from Manufacturers standard range.
b)	Custom powder coat as selected by Design Professional.
e.	Shade slat:
1)	Closed pocket elliptical slat: 1 inch (25 mm) aluminum elliptical slat inside of a 1-5/8 inch (41 mm) pocket with heat sealed ends.
2)	Open pocket elliptical slat: 1 inch (25mm) aluminum elliptical slat with plastic ends inside of a 1-5/8 inch (41 mm) pocket.
3)	Flat exposed hem bar: Small: 7/8 inch x 5/16 inch (22 mm x 8 mm) and Large 1-1/2 inch x 5/16 inch (38 mm x 8 mm) aluminum rectangular hem bar with plastic end caps. 
4)	Round exposed hem bar: Small 5/8 inch (16 mm) and Large 13/16 inch (21 mm) aluminum with plastic end caps.
f.	Light Gap Reduction Channels.
1)	Aluminum L Angle - 3/4 inch (19 mm) by 1 inch (25 mm).
2)	Aluminum L Angle -1 inch (25 mm) by 2-3/4 inches (70mm).
3)	Vinyl L Angle-1-1/2 inches (38 mm) by 3/4 inch (19 mm).
4)	U Channel -1 inch (25 mm) by 2-1/2 inches (64 mm).
5)	H Channel - 1 inch (25 mm) by 5 inches (127 mm).
4.	Bottom-Up Single Roller Configuration. Bottom-Up Single Roller Clutch-Operated FlexShade NEXD: Manually operated, vertical roll-up, fabric window shade with components necessary for complete installation, as manufactured by Draper, Inc.
a.	Brackets: Plated stamped steel. Provide size compatible with roller size.
1)	Mounted to ceiling.
2)	Mounted to wall.
3)	Mounted to jamb.
b.	Endcaps: Stamped steel with universal design suitable for mounting to ceiling, wall, and jamb. Provide size compatible with roller size.
1)	Endcap covers: To match fascia or headbox color.
c.	Fascia: L shaped aluminum extrusion to conceal shade roller and hardware.
1)	Attachment: Snaps onto endcaps without requiring exposed fasteners of any kind. Fascia can be mounted continuously across two or more shade bands. No notching is required.
2)	Selected from Manufacturers standard range
3)	Finish: Custom powder coat as selected by the Architect.
d.	Headbox Ceiling/Wall style: Aluminum fabrication with removable closure, endcaps, and back and top cover piece:
1)	Selected from Manufacturers standard range.
2)	Finish: Custom powder coat as selected by the Architect.
5.	Rollers: Extruded aluminum roller tube of appropriate diameter to support shade fabric with minimal deflection.
a.	Minimum Roller Tube Diameter: 1.5 inches (32 mm). Tube diameters less than 1.5 inches shall not be acceptable unless manufacturer provides deflection analysis showing deflection limited to less than or equal to width (inches) /700 at 1.5X design load.
b.	Fabric Connection to Roller Tube: Spline fabric/roller attachment system to allow shade fabric to be removed from roller without having to remove roller from brackets.
c.	Fabric Length: 6 inches (152 mm) greater than window height minimum.
d.	Orientation: Regular from back of roller.
e.	Orientation: Reverse from front of roller.
2.3	MOTORIZED WINDOW SHADES
A.	Type: Motorized vertical roll-up, fabric, window shade with motors, controls, mounting brackets, and other components necessary for complete installation; Motorized FlexShade as manufactured by Draper, Inc.
1.	Mounting brackets.
2.	Endcaps and fascia.
3.	Endcaps and headbox.
4.	Ceiling pocket.
B.	Shade Motor and Control System
1.	Motorized FlexShade I/O AC UL Listed if single roller configuration.
a.	IntelliFlex I/O 6Nm AC Motor: 120V AC, single phase, 60 HZ, 3-wire, 6nm or 15nm, at the manufacturer's discretion, instantly reversible, lifetime lubricated smart motor. Tubular motor concealed inside each shade roller tube. Equipped with internal thermal overload protector, and electric brake. Thermal protection: 4 minutes.
1)	Rated current: 1.0 Amps. Motors drawing greater than 1.0 amps shall not be acceptable without prior approval by Design Professional responsible for electrical design of project.
2)	Speed: 28RPM. All motors within a discrete control zone must operate at same speed.
3)	Sound level: 42dBA.
4)	UL Listing: UL325 and CSA C22.2 No. 247. Motors not listed as part of an entire shade assembly and control system shall not be acceptable.
5)	Encoded motors with two-way communication to network control devices. Motor/control networks that do not support two-way communication shall not be acceptable.
6)	Limits: Intermediate stopping points and presets.
b.	IntelliFlex I/O Network Devices.
1)	Network Device Connector. Connects lntelliFlex I/O devices into a network. Distributes power and communications between devices. One provided with each IntelliFlex I/O motor and network device. Approved for use in plenum spaces. LED Indicators indicate network status. Includes built-in terminating resistor, and network bypass switch for troubleshooting.
2)	Wireless Network Gateway. Allows wireless devices to control shades on the wired network. Required when using Radio Frequency handheld remote. LEDs indicate the status of both the wired and wireless networks. Allows wireless control of the entire network from a single receiving point.
3)	AV Gateway. Used to integrate with third party control systems. Single entry point must support RS-232 and RS-485 and contain at least 6 contact closure inputs, low voltage trigger, and IR receiver input. Approved for use in plenum spaces. LCD display allows for commissioning of serial groups.
4)	Contact Closure Interface. Allows up to 6 contact closure inputs to be connected to the network. These are grouped into 3 sets of Up/Down signals, each of which can control any number of shades on an lntelliFlex I/O network. Configuration must be done using onboard programming buttons, without rewiring or the use of external configuration devices. Power is provided through the lntelliFlex I/O network using a single Ethernet cable for power and communication.
5)	Sensor/Schedule Interface. Allows up to 4 sensors to be added to an IntelliFlex I/O network. Must include built-in support for brightness, wind, and precipitation sensors, and pyranometers. Must support up to 8 scheduled override events. Configuration must be done using on-board buttons and LCD display. Supports 0-10V, 4-20mA, photodiode and pulse sensors. External power input for sensors provides support for any sensor power requirements.
a)	SSI Transformer. To be used when adding third party sensors to the network.
6)	Sensor/Schedule Interface with Automated Glare Control. The IntelliFlex I/O Sensor / Scheduler Interface with automated glare control allows up to 4 sensors to be added to an IntelliFlex I/O network. Includes built-in support for brightness, temperature, wind, and precipitation sensors as well as pyranometers. Also provides support for up to 8 scheduled override events. Configuration is done using on-board buttons and LCD display. Supports 0-10V, 4-20mA, photodiode and pulse sensors. Configuration using built-in buttons and LCD display. Scheduled events can be configured to run on any combination of days of the week. External power input for sensors provides support for any sensor power requirements. Material: ABS plastic. Operating temperature: Ambient. Dimensions: 4-7/8 inches by 3 inches by 1 inch (124 by 83 by 32 mm). Mounting hardware provided.
7)	Central Network Controller. Touchscreen device to add advanced functionality to a network. It also acts as a router between the control network and a building IP network. Graphical user interfaces allow for the monitoring and override of motors and network devices. Automated glare control and scheduling. BACnet/IP integration. Interface to monitor and override network devices. Allows logging of shade movements, sensor readings, and user overrides. Input power: Micro USB. Operating temperature: ambient. Dimensions: 9-7/8 inches by 5-1/4 inches by 2 inches (251 by 146 by 51mm). Rough cutout: 8 inches by 5 inches by 1-3/4 inches (203 by 127 by 44 mm). Mounting hardware provided.
8)	IP Gateway. For connecting a network of IntelliFlex I/O devices to an IP network. Built-in two port network switch to allow direct connection to another IP Gateway creating a standalone network for access to all connected IntelliFlex I/O devices. Each IPG allows for an additional 120 devices to be added to the network. Configuration is done using the built-in buttons and display. Material: ABS plastic. Operating temperature: ambient. Dimensions: 4-7/8 inches by 3 inches by 1 inch (124 by 83 by 32 mm). Mounting hardware provided.
c.	IntelliFlex I/O Input Devices:
1)	Single Zone Wall Switch. Allows user to move roller shades to any position with a single touch. Swipe gestures must be recognized to move shades to fully open or closed positions. Power provided through lntelliFlex I/O network using a single Ethernet cable for power and communication. Switch is capable of controlling any number of shades on an lntelliFlex I/O network using onboard programming buttons without rewiring or the use of external configuration devices. Must allow unlimited number of preset alignment positions. Push button switches not permitted.
2)	Dual Zone Wall Switch. Allows user to control two independent zones of roller shades, moving them to any position with a single touch. Swipe gestures must also be recognized to move shades to fully open or closed positions. Power for switch must be provided through the lntelliFlex I/O network using a single Ethernet cable for power and communication. Each zone must be configured to control any number of shades on an lntelliFlex I/O network using the onboard programming buttons, without rewiring or the use of external configuration devices. Unlimited number of preset alignment positions. Push button switches not permitted.
3)	Radio Frequency Handheld Remote Control. Display must allow for any number of channels, up to 32 channels. Touch control to position the shades anywhere with one touch. Must be capable of serving as a simple commissioning tool. lntelliFlex I/O Wireless Network Gateway is required with remote. Range is 40 feet from closest IntelliFlex I/O device. Push button remotes not permitted.
4)	Infrared (IR) Remote Control Kit. Includes handheld remote transmitter and IR receiver. For use with AV Gateway.
d.	IntelliFlex I/O Sensors.
1)	External Brightness Sensor. For mounting on the exterior of the building. For use with Sensor/Schedule Interface.
2)	Wind Speed Sensor. For use with Sensor/Schedule Interface.
3)	Internal Brightness Sensor. To be mounted on the interior side of the window with adhesive or with provided mounting bracket. For use with Sensor/Schedule Interface.
2.	Motorized FlexShade AC UL Listed if single roller configuration
a.	Standard Motor: 120V AC, single phase, 60 HZ, instantly reversible, lifetime lubricated, and equipped with internal thermal overload protector, electric brake, and pre-set accessible limit switches. Tubular motor concealed inside each shade roller tube.
b.	Quiet 120V AC motor operates at 44 Db measured 3 feet from the motor. Tubular motor concealed inside each shade roller tube.
c.	Ultra Quiet 120V AC motor operates at 38 Db measured 3 feet from the motor. Tubular motor concealed inside each shade roller tube.
d.	Individual Control:
1)	Wall Switch - Toggle three position wall switch.
2)	Wall Switch - Key operated three position wall switch.
e.	Group Control:
1)	1 Motor Isolating Relay (1ISO) - One ISO relay per motor. Allows 110-120V group switching. Allows for up to 12 motors to be operated from a single 15 amp double throw switch, determined by motor size and circuit rating. Input Voltage: 120V AC/60Hz. Output Voltage: 120V AC/60Hz. Max Output Current: 4.0 Amps.
2)	1 Motor Controller. Single motor controller for use with motorized roller shades, Venetian blinds, and louver systems. Can be used as a standalone device or part of a network. When networked, can still be independently operated and can be configured to respond to wall switches, RF remotes, and signals from 3rd party systems. On-board contact closure interface. RS-485 network with built-in network termination. On-board buttons for testing and configuring motors. Pluggable terminal blocks. Input power: 110-230VAC @ 50 / 60Hz. Output power: Maximum 6A at input power. Material: ABS plastic. Operating temperature: 32 - 140 degree F (0 - 60 degree C). Dimensions: 2-3/4 inched by 3-1/2 inches by 2-1/8 inches (70 by 90 by 54 mm). Enclosure: 4 inches by 4 inches by 4 inches (102 by 102 by 102 mm).
3)	4 Motor Isolating Relay (GC4) - Panelized version with four ISO relays. Up to three GC4s can be linked together for control of up to 12 motors from any single 15 amp double throw wall switch, determined by motor size and circuit rating. Input Voltage: 120V AC/60Hz. Output Voltage: 120V AC/60Hz. Max Output Current: 4.0 Amps. Installed in a 8 inch by 8 inch by 4 inch (203 by 203 by 102 mm) box.
4)	4 Motor Controller. 4 motor controller for use with motorized roller shades, Venetian blinds and louver systems. Each port is independently operated and can be configured to respond to wall switches, RF remotes, and signals from 3rd party systems. RS-485 network with built-in network termination. Pluggable terminal blocks. Input power: 110-230VAC @ 50 / 60Hz. Output power: Maximum 6A at input power. Material: ABS plastic. Operating temperature: 32 - 140 degree F (0 - 60 degree C). Dimensions: 3-1.2 inches by 7 inches by 1-7/8 inches (89 by 178 by48 mm). Enclosure: 6 inches by 4 inches by 4 inches (152 by 102 by 102 mm).
f.	Individual and Group Control: IGC4N1. Individual and Group control of up to four motors with up to three intermediate positions per motor. Each motor output can be individually addressed and mapped to any of the 5 wall switch input ports using onboard dip switches
3.	FlexShade Recharge. Lithium-Ion battery powered motor with built-in radio receiver. Includes Ion Lithium batteries. No external wiring required. Tubular motor and batteries concealed inside each shade roller tube.
a.	12V Power Adapter.
b.	Solar Recharging Panel.
c.	Recharge Motor Cable Extender - 6 inches.
d.	Recharge Motor Cable Extender - 48 inches.
e.	Recharge Motor Cable Extender - 96 inches.
f.	Individual Control, Group Control and Individual and Group Control:
1)	Single channel wireless handheld radio frequency transmitter.
2)	Five channel wireless handheld radio frequency transmitter.
3)	15-Channel wireless handheld radio frequency transmitter.
4)	Single channel wireless wall switch for radio motor control.
5)	Five channel wireless wall switch for radio motor control.
6)	Fifteen channel wireless wall switch for radio motor control.
7)	Single channel dry contact interface.
8)	Screwless switch cover plate.
9)	Recharge Sun Sensor.
10)	Recharge Arc Wi-Fi to 433 2 way RF bridge kit
4.	Motorized FlexShade AC RTS. UL Listed if single roller configuration
a.	Standard Motor: 120V AC motor with built-in radio receiver. Tubular motor concealed inside each shade roller tube. 
b.	Quiet 120V AC RTS Motorized FlexShade. 120V AC quiet motor with built-in radio receiver. Operates at 44 dBA. Tubular motor concealed inside each shade roller tube.
c.	Individual Control, Group Control and Individual and Group Control:
1)	Single channel wireless handheld radio frequency transmitter.
2)	Single channel wireless handheld transmitter-Black.
3)	Four channel wireless handheld transmitter-White.
4)	Four channel wireless handheld transmitter-Black.
5)	16-Channel wireless handheld transmitter-White.
6)	16-Channel wireless handheld transmitter-Silver.
7)	Single channel wireless wall switch for radio motor control-White.
8)	Single channel wireless wall switch for radio motor control-Ivory.
9)	Four channel wireless wall switch for radio motor control-White.
10)	Four channel wireless wall switch for radio motor control-Ivory.
11)	RS-232/Dry Contact - Allows for full control of radio motor shade via RS-232/dry contact interface.
12)	Wireless Sun Sensor - Allows operation of one group of radio motors per sensor.
13)	Wireless Timer - Allows operation of one group of radio motors per timer.
14)	Repeater, 1 per project to extend range of transmitters.
15)	(URTSI II) Universal Interface - Allows for full control of radio motor shade via RS-232/485 or IR signals.
5.	FlexShade ST30 DC RTS. 24V DC quiet motor with built-in radio receiver. Tubular motor concealed inside each shade roller tube.
a.	Individual Control, Group Control and Individual and Group Control:
1)	Single channel wireless handheld transmitter-White.
2)	Single channel wireless handheld transmitter-Black.
3)	Four channel wireless handheld transmitter-White.
4)	Four channel wireless handheld transmitter-Black.
5)	16-Channel wireless handheld transmitter-White.
6)	16-Channel wireless handheld transmitter-Silver.
7)	Single channel wireless wall switch for radio motor control-White.
8)	Single channel wireless wall switch for radio motor control-Ivory.
9)	Four channel wireless wall switch for radio motor control-White.
10)	Four channel wireless wall switch for radio motor control-Ivory
11)	Dry Contact - Allows for full control of radio motor shade via dry contact interface.
12)	Wireless Sun Sensor - Allows operation of one group of radio motors per sensor.
13)	Wireless Timer - Allows operation of one group of radio motors per timer.
14)	Repeater, 1 per project to extend range of transmitters
15)	(URTSI II) Universal Interface - Allows for full control of radio motor shade via RS-232/485 or IR signals.
b.	Transformer (24V DC ONLY):
1)	Plug-In:
a)	1 Motor - Wall Type.
b)	1 Motor - Floor Type.
2)	Power Panel:
a)	5 Motors.
b)	10 Motors.
c)	15 Motors.
d)	20 Motors.
6.	Motorized FlexShade 50 RTS DC. 24V DC, UL Listed if single roller configuration quiet motor Quiet motor with built-in radio receiver. Tubular motor concealed inside each shade roller tube. 4 Nm of torque. Operates at 38 dBA.
a.	Individual Control, Group Control and Individual and Group Control:
1)	Single channel wireless handheld transmitter-White.
2)	Single channel wireless handheld transmitter-Silver.
3)	Four channel wireless handheld transmitter-White.
4)	Four channel wireless handheld transmitter-Silver
5)	16-Channel wireless handheld transmitter-White.
6)	16-Channel wireless handheld transmitter-Silver.
7)	Single channel wireless wall switch for radio motor control-White.
8)	Single channel wireless wall switch for radio motor control-Ivory.
9)	Four channel wireless wall switch for radio motor control-White.
10)	Four channel wireless wall switch for radio motor control-Ivory
11)	Dry Contact - Allows for full control of radio motor shade via dry contact interface.
12)	Wireless Sun Sensor - Allows operation of one group of radio motors per sensor.
13)	Wireless Timer - Allows operation of one group of radio motors per timer.
14)	Repeater, 1 per project to extend range of transmitters
15)	(URTSI II) Universal Interface - Allows for full control of radio motor shade via RS-232/485 or IR signals.
b.	Transformer (24V DC ONLY):
1)	Plug-In:
a)	1 Motor - Wall Type.
b)	1 Motor - Floor Type.
2)	Power Panel:
a)	10 Motors.
7.	FlexShade ST30 DC Dry Contact - 24V DC quiet motor with dry contact for connection to third party control systems. Tubular motor concealed inside each shade roller tube. 2 Nm of torque.
a.	Individual Control, Group Control, and Individual and Group Control:
1)	3-button dry contact switch (white) for up/stop/down control, limit setting, and motor speed control of a shade. Third party controllers can be connected to a secondary 4 wire terminal block located on the switch.
2)	3-button dry contact switch (ivory) for up/stop/down control, limit setting, and motor speed control of a shade. Third party controllers can be connected to a secondary 4 wire terminal block located on the switch.
3)	Dry contact motor limit setting tool.
b.	Transformer:
1)	Plug-In:
a)	1 Motor - Wall Type.
b)	1 Motor - Floor Type.
2)	Power Panel:
a)	5 Motors.
b)	10 Motors.
c)	15 Motors.
d)	20 Motors. 
8.	Motorized FlexShade AC 485. UL Listed if single roller configuration
a.	120V AC Intelligent Technology motor with built-in low voltage controller with 3-wire pig tail and data cable. No external motor controls are required. Available with optional three prong plug. Tubular motor concealed inside each shade roller tube.
b.	Quiet 120V AC Intelligent Technology Motor - 120V AC quiet motor with built-in low voltage controller with 3-wire pig tail and data cable. Motor operates at 44 dBA measured 3 feet from the motor. Makes no audible clicks when motor stops or starts. Available with optional three prong plug. Tubular motor concealed inside each shade roller tube.Ultra
c.	Ultra Quiet 120V AC Intelligent Technology Motor - 120V AC quiet motor with built-in low voltage controller with 3-wire pig tail and data cable. Motor operates at 38 dBA measured 3 feet from the motor. Makes no audible clicks when motor stops or starts. Available with optional three prong plug. Tubular motor concealed inside each shade roller tube.
d.	Individual Control, Group Control and Individual and Group Control:
1)	6 button RS 485 switch- for 2 groups up/stop/down or 1 group up/stop/down and 3 presets.
2)	8 button RS 485 switch- for 5 groups up/stop/down or 1 group up/stop/down and 5 presets.
3)	Somfy Digital Network. SDN system of window shades with intelligent motors linked to an IP interface box and other input devices for automated glare control.
4)	Bus Distribution
a)	Data Hub for 485 Motor
b)	5-Way RJ45 Splitter
c)	Building Controllers
d)	SDN Data Panel
5)	User Interfaces
a)	Somfy Connect BMS Interface
b)	Somfy Connect LTI
c)	Z Wave Digital Motor Interface (ZDMI)
d)	Zigbee to RS485 (ZBDMI)
e)	RTS Receiver for 485
f)	SDN 6 button wall switch (Preprogrammed for master control)
g)	SDN 8 button wall switch
h)	Somfy Connect UAI Plus
6)	Accessories
a)	Bus Power Supply, 24V, 1A
7)	32 point BACnet interface- Control of up to 32 groups with feedback via BACnet over IP.
9.	Model: FlexShade ST30 DC RS 485 Motor - 24V DC quiet motor with built-in intelligence for RS 485 control. Tubular motor concealed inside each shade roller tube. 4 Nm of torque.
a.	Individual Control, Group Control and Individual and Group Control:
1)	6 button RS 485 switch- for 2 groups up/stop/down or 1 group up/stop/down and 3 presets.
2)	8 button RS 485 switch- for 5 groups up/stop/down or 1 group up/stop/down and 5 presets
3)	Somfy Digital Network. SDN system of window shades with intelligent motors linked to an IP interface box and other input devices for automated glare control.
4)	Bus Distribution
a)	Data Hub for 485 Motor
5)	5-Way RJ45 Splitter
a)	Building Controllers
b)	SDN Data Panel
6)	User Interfaces
a)	Somfy Connect BMS Interface
b)	Somfy Connect LTI
c)	Z Wave Digital Motor Interface (ZDMI)
d)	Zigbee to RS485 (ZBDMI)
e)	RTS Receiver for 485
f)	SDN 6 button wall switch (Preprogrammed for master control)
g)	SDN 8 button wall switch
h)	Somfy Connect UAI Plus
7)	Accessories
a)	Bus Power Supply, 24V, 1A
8)	32-point BACnet interface-Control of up to 32 groups with feedback via BACnet over IP
b.	Transformer (24V DC ONLY):
1)	Plug-In:
a)	1 Motor - Wall Type.
b)	1 Motor - Floor Type.
2)	Power Panel:
a)	10 Motors.
10.	Motorized FlexShade 50 DC RS 485 UL Listed if single roller configuration 24V DC quiet motor with built-in intelligence for RS 485 control. Tubular motor concealed inside each shade roller tube. 4 Nm of torque.
a.	Individual Control, Group Control and Individual and Group Control:
1)	6 button RS 485 switch- for 2 groups up/stop/down or 1 group up/stop/down and 3 presets.
2)	8 button RS 485 switch- for 5 groups up/stop/down or 1 group up/stop/down and 5 presets
3)	Somfy Digital Network. SDN system of window shades with intelligent motors linked to an IP interface box and other input devices for automated glare control.
4)	Bus Distribution
a)	Data Hub for 485 Motor
5)	5-Way RJ45 Splitter
a)	Building Controllers
b)	SDN Data Panel
6)	User Interfaces
a)	Somfy Connect BMS Interface
b)	Somfy Connect LTI
c)	Z Wave Digital Motor Interface (ZDMI)
1)	Zigbee to RS485 (ZBDMI)
d)	RTS Receiver for 485
e)	SDN 6 button wall switch (Preprogrammed for master control)
f)	SDN 8 button wall switch
g)	Somfy Connect UAI Plus
7)	Accessories
a)	Bus Power Supply, 24V, 1A
8)	32-point BACnet interface-Control of up to 32 groups with feedback via BACnet over IP.
b.	Transformer:
1)	Plug-In:
a)	1 Motor - Wall Type.
b)	1 Motor - Floor Type.
2)	Power Panel:
a)	10 Motors.
C.	Configuration:
1.	Single Roller.
a.	Mounting.
1)	Endcaps: 1028 stamped steel with universal design suitable for mounting to ceiling, wall, and jamb. Provide size compatible with roller size. Endcap covers to match fascia/headbox finish.
2)	Brackets: 1018 stamped steel, black powder coat, idler height adjuster, field adjustable to wall or ceiling mount.
a)	Mounted to ceiling.
b)	Mounted to wall.
c)	Mounted to jamb.
3)	Fascia: L shaped aluminum extrusion to conceal shade roller and hardware.
a)	Attachment: Snaps onto end caps without requiring exposed fasteners of any kind. Fascia can be mounted continuously across two or more shade bands. 
b)	Finish: Selected from Manufacturers standard range.
c)	Finish: Custom powder coat as selected by the Architect.
4)	Headbox Ceiling/Wall Style: Aluminum fabrication with removable closure, endcaps, and back and top cover piece:
a)	Selected from Manufacturers standard range.
b)	Finish: Custom powder coat as selected by the Architect.
5)	Headbox, Pocket Style: Aluminum fabrication with removable closure, endcaps, and U-shaped pocket:
a)	Finish: Selected from Manufacturers standard range.
b)	Finish: Custom powder coat as selected by the Architect.
6)	Type D Shade pocket: Rectangular pocket with ceiling tile lip designed for recessed ceiling installation of window shades.
a)	Material: Extruded aluminum alloy with white epoxy paint finish.
b)	Size: 5 inches (127 mm) by 5-3/8 inches (137 mm) high.
c)	Closure Panel:
1)	1-1/2 (38 mm) closure dimension.
2)	3 inch (78 mm)
d)	Pocket Endcap Kit: Endcaps with 7/8 inch (22 mm) lip for support of acoustical ceiling panel.
e)	Corners: Welded one-piece aluminum sections connecting to and matching pockets to allow continuous shade recess at ceiling corners.
f)	Pocket ends: Welded one-piece aluminum sections connecting to and matching pockets.
7)	Wall Clip with Closure panel: For site constructed ceiling recesses, provide removable closure panel to minimize slot for shade passage but allowing access to shade for maintenance.
a)	Material: Aluminum alloy with white epoxy paint finish.
b)	Tile Lip: Provide wall clip with 7/8 inch tile lip (22 mm).
c)	Closure width: 1-1/2 inches (38 mm).
d)	Closure width: 3 inches (75 mm).
e)	Closure Width: 5 inches (127 mm).
f)	Provide continuous wall clip, 1-3/4 (44 mm) by 3/16 inch (5 mm), for snap-in attachment of closure panel without fasteners.
8)	Aluminum Light Gap Reduction Channels
a)	L Angle - 3/4 inch by 1 inch (19 mm by 25 mm).
b)	L Angle - 1 inch by 2-3/4 inches (25 mm by 70 mm).
c)	U Channel - 1 inch by 2-1/2 inches (25 mm by 64 mm).
d)	H Channel - 1 inch (25 mm) by 5 inches (127 mm). 
9)	Vinyl Light Gap Reduction Channels
a)	L Angle - 1-1/2 inches 3/4 inches (38 mm by 19 mm). 
10)	Interior cable guide kit
a)	Interior cable hem bar finial.
b)	Cable mount.
c)	Cable.
d)	Tension Stop.
11)	Shade slat:
a)	Closed pocket elliptical slat: 1 inch (25 mm) aluminum elliptical slat inside of a 1-5/8 inch (41 mm) pocket with heat sealed ends.
b)	Open pocket elliptical slat: 1 inch (25mm) aluminum elliptical slat with plastic ends inside of a 1-5/8 inch (41 mm) pocket.
c)	Flat exposed hem bar: Small: 7/8 inch x 5/16 inch (22 mm x 8 mm) and Large 1-1/2 inch x 5/16 inch (38 mm x 8 mm) aluminum rectangular hem bar with plastic end caps. 
d)	Round exposed hem bar: Small 5/8 inch (16 mm) and Large 13/16 inch (21 mm) aluminum with plastic end caps.
2.	Dual Roller.
a.	Mounting.
1)	Dual roller endcaps. Endcaps for surface or recessed mounting of dual roller window shades. 1028 steel stamping.
2)	Dual roller fascia. Endcaps with fascia designed for surface mounting of dual roller window shades.
a)	Endcaps: 1028 steel stamping.
b)	Fascia: L-shaped cover of extruded aluminum, .060 wall. Assembly snaps onto endcaps without exposed fasteners.
c)	Finish: Powder coat.
1)	Finish: Selected from Manufacturers standard range
2)	Finish: Custom powder coat as selected by the Architect.
3)	Dual roller with pocket headbox. Pocket and endcaps designed for recessed ceiling installation of dual roller window shades.
a)	Material: 18 gauge steel.
b)	Finish:
1)	White Inside/Grey Outside with white ceiling flange.
2)	Grey Inside/White Outside with white ceiling tile flange.
c)	Closure Panel Aluminum, without exposed fasteners:
1)	Front Tile Flange.
2)	Left Tile Flange.
3)	Right Tile Flange.
4)	Pre-drilled Mounting Holes.
5)	Pre-drilled Ventilation holes.
4)	Dual roller with ceiling/wall headbox. Fascia, L-shaped top/back, and endcaps designed for wall or ceiling installation of dual roller window shades.
a)	Endcaps: 1028 steel stamping.
b)	Fascia: L-shaped cover of extruded aluminum, .060 wall. Assembly snaps onto endcaps without exposed fasteners.
c)	Finish: Powder coat.
1)	Selected from Manufacturers standard range.
2)	Custom powder coat as selected by Design Professional.
b.	Aluminum Light Gap Reduction Channels
1)	L Angle - 3/4 inch by 1 inch (19 mm by 25 mm).
2)	L Angle - 1 inch by 2-3/4 inches (25 mm by 70 mm).
3)	U Channel - 1 inch by 2-1/2 inches (25 mm by 64 mm).
4)	H Channel - 1 inch (25 mm) by 5 inches (127 mm).
c.	Vinyl Light Gap Reduction Channels
1)	L Angle - 1-1/2 inches 3/4 inches (38 mm by 19 mm).
d.	Shade slat:
1)	Closed pocket elliptical slat: 1 inch (25 mm) aluminum elliptical slat inside of a 1-5/8 inch (41 mm) pocket with heat sealed ends.
2)	Open pocket elliptical slat: 1 inch (25mm) aluminum elliptical slat with plastic ends inside of a 1-5/8 inch (41 mm) pocket.
3)	Flat exposed hem bar: Small: 7/8 inch x 5/16 inch (22 mm x 8 mm) and Large 1-1/2 inch x 5/16 inch (38 mm x 8 mm) aluminum rectangular hem bar with plastic end caps. 
4)	Round exposed hem bar: Small 5/8 inch (16 mm) and Large 13/16 inch (21 mm) aluminum with plastic end caps.
3.	Bottom-Up Single Roller. Motorized Bottom-Up FlexShade.
a.	Brackets: Plated stamped steel. Provide size compatible with roller size.
1)	Mounted to ceiling.
2)	Mounted to wall.
3)	Mounted to jamb.
b.	Endcaps: Stamped steel with universal design suitable for mounting to ceiling, wall, and jamb. Provide size compatible with roller size.
1)	Endcap covers: To match fascia or headbox color.
c.	Fascia: L shaped aluminum extrusion to conceal shade roller and hardware.
1)	Attachment: Snaps onto endcaps without requiring exposed fasteners of any kind. Fascia can be mounted continuously across two or more shade bands. No notching is required.
2)	Shape: Square Fascia Panel.
3)	Finish: Selected from Manufacturers standard range.
4)	Finish: Custom powder coat as selected by the Architect.
d.	Headbox Ceiling/Wall style: Aluminum fabrication with removable closure, endcaps, and back and top cover piece:
1)	Selected from Manufacturers standard range.
2)	Finish: Custom powder coat as selected by the Architect.
e.	Hembar: Machine extruded aluminum, finished to match fascia.
4.	Bottom-Up Dual Roller. Motorized Bottom-Up Dual Roller FlexShade. Endcaps with fascia designed for surface mounting of dual roller window shades.
a.	Endcaps: 1028 steel alloy stamping.
b.	Fascia: L-shaped cover of extruded aluminum, .060 wall. Assembly snaps onto endcaps without exposed fasteners.
c.	Selected from Manufacturers standard range.
d.	Finish: Custom powder coat as selected by the Architect.
e.	Hembar: Extruded aluminum, finished to match fascia.
D.	Roller: Fabricated from extruded aluminum or steel. Wall thickness and material selected by manufacturer to accommodate shade size. Provide with roller idler assembly of molded nylon and zinc-plated steel pin. Sliding pin to allow easy installation and removal of roller. Fabric connected to the roller tube with LSE (low surface energy) double sided adhesive specifically developed to attach coated textiles to metal. Adhesive attachment to eliminate horizontal impressions in fabric.
E.	Coupling system: Couplings to join motorized shade rollers to allow operation by single motor. FlexShade Coupling System as manufactured by Draper, Inc. Provide endcaps to receive couplers and support multiple shades. Coupling system must be capable of up to 30-degree angles. 
2.4	INTERMEDIATE SIZE MOTORIZED WINDOW SHADES
A.	Type: Motorized vertical roll-up, fabric, window shade with motors, controls, mounting brackets, and other components necessary for complete installation; Motorized FlexShade 2 as manufactured by Draper, Inc.
1.	Mounting brackets.
2.	Endcaps and fascia.
3.	Endcaps and ceiling/wall headbox.
4.	Endcaps with pocket headbox
B.	Shade Motor and Control System
1.	Motorized FlexShade 2 AC
a.	FlexShade 2 120V AC motor. Single phase, 60 HZ, instantly reversible, lifetime lubricated, and equipped with internal thermal overload protector, electric brake, and pre-set accessible limit switches. Tubular motor concealed inside each shade roller tube.
b.	FlexShade 2 Quiet 120V AC motor. Operates at 44 Db measured 3 feet from the motor. Makes no audible clicks when motor stops or starts. Tubular motor concealed inside each shade roller tube.
c.	Individual Control:
1)	Wall Switch - Toggle three position wall switch.
2)	Wall Switch - Key operated three position wall switch.
d.	Group Control:
1)	1 Motor Isolating Relay (GC4) - One ISO relay per motor. Allows 110-120V group switching. Allows for up to 12 motors to be operated from on one a single 15 amp double throw switch, determined by motor size and circuit rating. Input Voltage: 120V AC/60Hz. Output Voltage: 120V AC/60Hz. Max Output Current: 4.0 Amps.
2)	1 Motor Controller. Single motor controller for use with motorized roller shades, Venetian blinds, and louver systems. Can be used as a standalone device or part of a network. When networked, can still be independently operated and can be configured to respond to wall switches, RF remotes, and signals from 3rd party systems. On-board contact closure interface. RS-485 network with built-in network termination. On-board buttons for testing and configuring motors. Pluggable terminal blocks. Input power: 110-230VAC @ 50 / 60Hz. Output power: Maximum 6A at input power. Material: ABS plastic. Operating temperature: 32 - 140 degree F (0 - 60 degree C). Dimensions: 2-3/4 inched by 3-1/2 inches by 2-1/8 inches (70 by 90 by 54 mm). Enclosure: 4 inches by 4 inches by 4 inches (102 by 102 by 102 mm).4 Motor Isolating Relay (GC4) - Panelized version with four ISO relays. Up to three 4ISOs can be linked together for control of up to 12 motors from any single 15 amp double throw wall switch, determined by motor size and circuit rating. Input Voltage: 120V AC/60Hz. Output Voltage: 120V AC/60Hz. Max Output Current: 4.0 Amps. Installed in a 8 inch by 8 inch by 4 inch (203 by 203 by 102 mm) box.
3)	4 Motor Controller. 4 motor controller for use with motorized roller shades, Venetian blinds and louver systems. Each port is independently operated and can be configured to respond to wall switches, RF remotes, and signals from 3rd party systems. RS-485 network with built-in network termination. Pluggable terminal blocks. Input power: 110-230VAC @ 50 / 60Hz. Output power: Maximum 6A at input power. Material: ABS plastic. Operating temperature: 32 - 140 degree F (0 - 60 degree C). Dimensions: 3-1.2 inches by 7 inches by 1-7/8 inches (89 by 178 by48 mm). Enclosure: 6 inches by 4 inches by 4 inches (152 by 102 by 102 mm).
4)	IGC4N1. Individual and Group control of up to four motors with up to three intermediate positions per motor. Each motor output can be individually addressed and mapped to any of the 5 wall switch input ports using onboard dip switches.
2.	FlexShade 2 I/O AC.
a.	IntelliFlex I/O AC smart motor: 120V AC, single phase, 60 HZ, 3-wire, 6nm or 15nm (at manufacturer's discretion), instantly reversible, lifetime lubricated smart motor. Equipped with internal thermal overload protector, and electric brake. 
1)	Thermal protection: 4 minutes.
2)	Rated current: 1.0 Amps. Motors drawing greater than 1.0 amps shall not be acceptable without prior approval by Design Professional responsible for electrical design of project.
3)	Speed: 28RPM. All motors within a discrete control zone must operate at same speed.
4)	Sound level: 42dBA.
5)	UL Listing: UL325 and CSA C22.2 No. 247. Motors not listed as part of an entire shade assembly and control system shall not be acceptable.
6)	Encoded motors with two-way communication to network control devices. Motor/control networks that do not support two-way communication shall not be acceptable.
7)	Limits: Intermediate stopping points and presets.
b.	IntelliFlex I/O Network Devices
1)	Network Device Connector. Connects lntelliFlex I/O devices into a network. Distributes power and communications between devices. One provided with each IntelliFlex I/O motor and network device. Approved for use in plenum spaces. LED Indicators indicate network status. Includes built-in terminating resistor, and network bypass switch for troubleshooting. Material: ABS plastic. Operating temperature: Ambient. Dimensions: 3-3/8 inches by 2 inches by 1-1/16 inches (90 by 31 by 27 mm). Mounting hardware provided. Indoor use only.
2)	Wireless Network Gateway. Allows wireless devices to control shades on the wired network. Required when using Radio Frequency handheld remote. LEDs indicate the status of both the wired and wireless networks. Allows wireless control of the entire network from a single receiving point. Material: ABS plastic. Operating temperature: Ambient. Dimensions: 3-3/8 inches by 2 inches by 1-1/16 inches (85 by 52 by 27 mm). Mounting hardware provided. Indoor use only.
3)	AV Gateway. Used to integrate with third party control systems. Single entry point must support RS-232 and RS-485 and contain at least 6 contact closure inputs, low voltage trigger, and IR receiver input. Approved for use in plenum spaces. LCD display allows for commissioning of serial groups. Material: ABS plastic. Operating temperature: Ambient. Dimensions: 4-7/8 inches by 3 inches by 1 inch (124 by 83 by 32 m). Mounting hardware provided. Indoor use only.
4)	Contact Closure Interface. Allows up to 6 contact closure inputs to be connected to the network. These are grouped into 3 sets of Up/Down signals, each of which can control any number of shades on an lntelliFlex I/O network. Configuration must be done using onboard programming buttons, without rewiring or the use of external configuration devices. Power is provided through the lntelliFlex I/O network using a single Ethernet cable for power and communication. Material: ABS plastic. Operating temperature: Ambient. Dimensions: 3 inches by 3 inches by 1 inch (76 by 76 by 25 mm). Mounting hardware provided. Indoor use only.
5)	Sensor/Schedule Interface. Allows up to 4 sensors to be added to an IntelliFlex I/O network. Must include built-in support for brightness, temperature, wind, and precipitation sensors, and pyranometers. Must support up to 8 scheduled override events. Configuration must be done using on-board buttons and LCD display. Supports 0-10V, 4-20mA, photodiode and pulse sensors. External power input for sensors provides support for any sensor power requirements. Material: ABS plastic. Operating temperature: Ambient. Dimensions: 4-7/8 inches by 3-1/4 inches by 1-1.4 inched (124 by 83 by 32 m). Mounting hardware provided. Indoor use only.
a)	SSI Transformer. To be used when adding third party sensors to the network.
6)	Sensor/Schedule Interface with Automated Glare Control. The IntelliFlex I/O Sensor / Scheduler Interface with automated glare control allows up to 4 sensors to be added to an IntelliFlex I/O network. Includes built-in support for brightness, temperature, wind, and precipitation sensors as well as pyranometers. Also provided support for up to 8 scheduled override events. Configuration is done using on-board buttons and LCD display. Supports 0-10V, 4-20mA, photodiode and pulse sensors. Configuration using built-in buttons and LCD display. Scheduled events can be configured to run on any combination of days of the week. External power input for sensors provides support for any sensor power requirements. Material: ABS plastic. Operating temperature: Ambient. Dimensions: 4-7/8 inches by 3 inches by 1 inch (124 by 83 by 32 m). Mounting hardware provided.
7)	Central Network Controller. Touchscreen device to add advanced functionality to a network. It also acts as a router between the control network and a building IP network. Graphical user interfaces on local touchscreen and remote access web interfaces allow for the monitoring and override of motors and network devices. Automated glare control and scheduling. BACnet/IP integration. Interface to monitor and override network devices. Allows logging of shade movements, sensor readings, and user overrides. Input power: Micro USB. Operating temperature: ambient. Dimensions: 9-7/8 inches by 5-1/4 inches by 2 inches (251 x 146 x 51 mm). Rough cutout: 8 inches by 5 inches by x 1-3/4 inches (203 by 127 by 44 mm). Mounting hardware provided.
8)	IP Gateway. For connecting a network of IntelliFlex I/O devices to an IP network. Built-in two port network switch to allow direct connection to another IP Gateway creating a standalone network for access to all connected IntelliFlex I/O devices. Each IPG is a BACnet/IP device and allows for an additional 120 devices to be added to the network. Configuration is done using the built-in buttons and display. Material: ABS plastic. Operating temperature: ambient. Dimensions: 4-7/8 inches by 3 inches by 1 inch (124 by 83 by 32 mm). Mounting hardware provided.
c.	IntelliFlex I/O User Input Devices.
1)	Single Zone Wall Switch. Allows user to move roller shades to any position with a single touch. Swipe gestures must be recognized to move shades to fully open or closed positions. Power provided through lntelliFlex I/O network using a single Ethernet cable for power and communication. Switch shall be capable of controlling any number of shades on an lntelliFlex I/O network using onboard programming buttons without rewiring or the use of external configuration devices. Must allow unlimited number of preset alignment positions. Push button switches not permitted.
2)	Dual Zone Wall Switch. Allows user to control two independent zones of roller shades, moving them to any position with a single touch. Swipe gestures must also be recognized to move shades to fully open or closed positions. Power for switch must be provided through the lntelliFlex I/O network using a single Ethernet cable for power and communication. Each zone must be configured to control any number of shades on an lntelliFlex I/O network using the onboard programming buttons, without rewiring or the use of external configuration devices. Unlimited number of preset alignment positions. Push button switches not permitted.
3)	Radio Frequency Handheld Remote Control. Display must allow for any number of channels, up to 32 channels. Touch control to position the shades anywhere with one touch. Must be capable of serving as a simple commissioning tool. lntelliFlex I/O Wireless Network Gateway is required with remote. Range is 40 feet from closest IntelliFlex I/O device. Push button remotes not permitted.
4)	Infrared (IR) Remote Control Kit. Includes handheld remote transmitter and IR receiver. For use with AV Gateway.
d.	IntelliFlex I/O Sensors.
1)	External Brightness Sensor. For mounting on the exterior side of the window. For use with Sensor/Schedule Interface.
2)	Wind Speed Sensor. For use with Sensor/Schedule Interface.
3)	Internal Brightness Sensor. To be mounted on the interior side of the window with adhesive or with provided mounting bracket. For use with Sensor/Schedule Interface.
3.	FlexShade 2 RTS AC.
a.	Standard Motor: 120V AC motor with built-in radio receiver. Tubular motor concealed inside each shade roller tube. 
b.	Individual Control, Group Control and Individual and Group Control:
1)	Single channel wireless handheld transmitter-White.
2)	Single channel wireless handheld transmitter-Black.
3)	Four channel wireless handheld transmitter-White.
4)	Four channel wireless handheld transmitter-Black.
5)	16-Channel wireless handheld transmitter-White.
6)	16-Channel wireless handheld transmitter-Silver.
7)	Single channel wireless wall switch for radio motor control-White.
8)	Single channel wireless wall switch for radio motor control-Ivory.
9)	Four channel wireless wall switch for radio motor control-White.
10)	Four channel wireless wall switch for radio motor control-Ivory.
11)	RS-232/Dry Contact - Allows for full control of radio motor shade via RS-232/dry contact interface.
12)	Wireless Sun Sensor - Allows operation of one group of radio motors per sensor.
13)	Wireless Timer - Allows operation of one group of radio motors per timer.
14)	Repeater, 1 per project to extend range of transmitters.
15)	(URTSI II) Universal Interface - Allows for full control of radio motor shade via RS-232/485 or IR signals.
4.	FlexShade 2 485 AC.
a.	120V AC motor with built-in low voltage controller with 3-wire pig tail and data cable. No external motor controls are required. Available with optional three prong plug. Tubular motor concealed inside each shade roller tube.
b.	Individual Control, Group Control and Individual and Group Control:
1)	6 button RS 485 switch- for 2 groups up/stop/down or 1 group up/stop/down and 3 presets.
2)	8 button RS 485 switch- for 5 groups up/stop/down or 1 group up/stop/down and 5 presets.
3)	Somfy Digital Network. SDN system of window shades with intelligent motors linked to an IP interface box and other input devices for automated glare control.
4)	Bus Distribution
a)	Data Hub for 485 Motor
b)	5-Way RJ45 Splitter
c)	Building Controllers
d)	SDN Data Panel
5)	User Interfaces
a)	Somfy Connect BMS Interface
b)	Somfy Connect LTI
c)	Z Wave Digital Motor Interface (ZDMI)
d)	Zigbee to RS485 (ZBDMI)
e)	RTS Receiver for 485
f)	SDN 6 button wall switch (Preprogrammed for master control)
g)	SDN 8 button wall switch
h)	Somfy Connect UAI Plus
6)	Accessories
a)	Bus Power Supply, 24V, 1A
7)	32 point BACnet interface- Control of up to 32 groups with feedback via BACnet over IP.
5.	Roller: Size 4 inch (102 mm) or 5 inch (127 mm) O.D. steel tube. Size at manufacturer's discretion.
6.	Roller Idler Assembly: Zinc-plated steel shaft supported by roller bearings in an aluminum housing.
7.	Slat: 13/16 inch aluminum dowel, encased in heat seamed hem.
8.	Mounting
a.	Endcaps: 1028 steel stamping. Complete with adapter roller bracket. Installs to wall, ceiling, or jamb. Accepts fascia or headbox.
b.	Brackets: 1018 plated steel stamping, suitable for mounting to wall, ceiling, or jamb. Brackets do not require additional adapters.
c.	Fascia: 6-1/2 inch by 6-1/2 inch (165 by 165 mm) square cover of extruded aluminum, 0.125 inch (3.175 mm) wall.
1)	Attachment: Snaps onto endcaps without requiring exposed fasteners of any kind.
2)	Finish: Selected from Manufacturers standard range.
3)	Finish: Custom powder coat as selected by Design Professional.
d.	Headbox Ceiling/Wall Style: 6-5/8 inches by 6-5/8 inches (168 by 168 mm) square fascia and L-shaped back/top cover to be fabricated of extruded aluminum:
1)	Finish: Selected from Manufacturers standard range.
2)	Finish: Custom powder coat as selected by the Architect.
e.	Pocket headbox constructed of extruded aluminum. Bottom of headbox fully enclosed except for slot allowing fabric passage. Bottom closure panel shall be extruded aluminum, finished white, and may be removed manually for access to roller and drive unit. Aluminum endplates with integrated steel brackets for suspended mounting shall be fastened to extruded headbox with thread-cutting screws.
1)	Ceiling Tile Flange: 12 foot (366 cm) extruded aluminum, finished white. Attaches to pocket headbox. Hardware for attachment to headbox included.
2)	Endcap Ceiling Tile Flange: Extruded aluminum, finished white. Available on one or both endcaps.
2.5	LARGE MOTORIZED WINDOW SHADES
A.	Type: FlexShade XL Motorized Roller shading systems: Electrically operated, motorized, vertical roll-up, fabric window shade. Assembly to include motor operator, controls, mounting hardware and other components necessary for complete installation; 
B.	Roller: 2.364 inch (60 mm) outside diameter aluminum. Roller assembly is integrated with floating bracketry
1.	Roller Idler Assembly: Plastic idle end insert into roller will fit over steel pin and rotate on pin with use of sealed bearing. Steel pin connects to bearing mounted to bracket mounted inside the headbox. Systems not using sealed bearings are not acceptable. 
2.	Fabric Connection to Roller Tube: Fabric panel to incorporate spline attachment at the top and hem pocket at the bottom to allow connection to the hem bar.
3.	Slat: 13/16 inch aluminum dowel, encased in heat seamed hem.
4.	Cradle System: Extrusion supports entire roller using cradle system to reduce roller deflection
C.	Headbox: Cassette-style extruded aluminum sections
1.	Size: 5 inches high by 5 inches deep by length required for shade being provided.
2.	Shape: Angled
3.	Shape: Curved.
4.	Finish: Selected from Manufacturers standard range.
5.	Finish: Custom powder coat as selected by the Architect
D.	Electric Operator: Tubular motor concealed inside shade roller tube;
1.	Standard Motor: Sonesse Radio Technology Motor: 110-120V AC, single-phase, 60 HZ, instantly reversible, lifetime lubricated motor with built-in radio receiver, equipped with internal thermal overload protector, electric brake, and pre-set accessible limit switches. (Compatible with Wireless Radio Technology Controls.)
2.	Wired Motor: Sonesse 110-120V AC, single-phase, 60 HZ, instantly reversible, lifetime lubricated, and equipped with internal thermal overload protector, electric brake, and pre-set accessible limit switches. Compatible with Intelliflex Controls.
3.	Location:
a.	Right hand
b.	Left hand
c.	As scheduled
4.	RTS Motor Controls:
a.	Individual Control, Group Control and Individual and Group Control:
b.	Single channel wireless handheld radio frequency transmitter.
c.	Single channel wireless handheld transmitter-Black.
d.	Four channel wireless handheld transmitter-White.
e.	Four channel wireless handheld transmitter-Black.
f.	16-Channel wireless handheld transmitter-White.
g.	16-Channel wireless handheld transmitter-Silver.
h.	Single channel wireless wall switch for radio motor control-White.
i.	Single channel wireless wall switch for radio motor control-Ivory.
j.	Four channel wireless wall switch for radio motor control-White.
k.	Four channel wireless wall switch for radio motor control-Ivory.
l.	RS-232/Dry Contact - Allows for full control of radio motor shade via RS-232/dry contact interface.
m.	Wireless Sun Sensor - Allows operation of one group of radio motors per sensor.
n.	Wireless Timer - Allows operation of one group of radio motors per timer.
o.	Repeater, 1 per project to extend range of transmitters.
p.	(URTSI II) Universal Interface - Allows for full control of radio motor shade via RS-232/485 or IR signals.
5.	Wired Motor Controls:
a.	Individual Control:
1)	Wall Switch - Toggle three position wall switch.
2)	Wall Switch - Key operated three position wall switch.
b.	Group Control:
1)	1 Motor Isolating Relay (1ISO) - One ISO relay per motor. Allows 110-120V group switching. Allows for up to 12 motors on one double throw switch. Input Voltage: 120V AC/60Hz. Output Voltage: 120V AC/60Hz. Max Output Current: 4.0 Amps.
2)	1 Motor Controller. Single motor controller for use with motorized roller shades, Venetian blinds, and louver systems. Can be used as a standalone device or part of a network. When networked, can still be independently operated and can be configured to respond to wall switches, RF remotes, and signals from 3rd party systems. On-board contact closure interface. RS-485 network with built-in network termination. On-board buttons for testing and configuring motors. Pluggable terminal blocks. Input power: 110-230VAC @ 50 / 60Hz. Output power: Maximum 6A at input power. Material: ABS plastic. Operating temperature: 32 - 140 degree F (0 - 60 degree C). Dimensions: 2-3/4 inched by 3-1/2 inches by 2-1/8 inches (70 by 90 by 54 mm). Enclosure: 4 inches by 4 inches by 4 inches (102 by 102 by 102 mm).
3)	4 Motor Isolating Relay (GC4) - Panelized version with four ISO relays. Up to three 4ISOs can be linked together for control of up to 12 motors from any single 15 amp double throw wall switch. Input Voltage: 120V AC/60Hz. Output Voltage: 120V AC/60Hz. Max Output Current: 4.0 Amps. Installed in a 8 inch by 8 inch by 4 inch (203 by 203 by 102 mm) box.
4)	4 Motor Controller. 4 motor controller for use with motorized roller shades, Venetian blinds and louver systems. Each port is independently operated and can be configured to respond to wall switches, RF remotes, and signals from 3rd party systems. RS-485 network with built-in network termination. Pluggable terminal blocks. Input power: 110-230VAC @ 50 / 60Hz. Output power: Maximum 6A at input power. Material: ABS plastic. Operating temperature: 32 - 140 degree F (0 - 60 degree C). Dimensions: 3-1.2 inches by 7 inches by 1-7/8 inches (89 by 178 by48 mm). Enclosure: 6 inches by 4 inches by 4 inches (152 by 102 by 102 mm).
c.	Individual and Group Control: IGC4N1. Individual and Group control of up to four motors with up to three intermediate positions per motor.
E.	Fabric: 
1.	1% 
2.	3% 
3.	5% 
4.	Soltis 92
2.6	OPAQUE WINDOW SHADE SYSTEM
A.	Operation Type: Motorized, vertical roll-up, fabric, opaque window shade system, complete with headbox, side and sill channels for total opacity; LightBloc FlexShade System as manufactured by Draper, Inc.
B.	Operation Type: Bead chain and clutch operated, vertical roll-up, fabric, opaque window shade system, complete with headbox, side and sill channels for total opacity; LightBloc FlexShade System as manufactured by Draper, Inc.
C.	Operation Type: Crank operated, vertical roll-up, fabric, opaque window shade system, complete with headbox, side and sill channels for total opacity; LightBloc FlexShade System as manufactured by Draper, Inc.
D.	Operation: Bead chain and clutch operating mechanism allowing shade to stop when chain is released. Designed never to need adjustment or lubrication. Provide limit stops to prevent shade from being raised or lowered too far.
1.	Clutch mechanism: Fabricated from high carbon steel and molded fiberglass reinforced polyester.
2.	Bead chain loop: Stainless steel bead chain hanging at side of window.
3.	Bead chain loop: Plastic bead chain hanging at side of window, Ivory, Grey, or Black color as selected by Architect.
4.	Idler Assembly: Provide roller idler assembly of molded nylon with adjustable length idler pin to facilitate easy installation, and removal of shade for service.
E.	Operation: Crank and gear box operated shades.
1.	Gear box: Die cast aluminum and steel construction. Injection molded nylon and steel crank insert installed in roller to engage gear box.
2.	Crank handle: 
a.	Detachable anodized aluminum and chrome plated steel handle.
b.	Permanently mounted anodized aluminum and chrome plated steel handle.
c.	Size: 4 feet (122 cm).
d.	Size: 6 feet (183 cm).
e.	Size: 10 feet (305 cm).
3.	Idler assembly: Provide roller idler assembly of molded nylon with adjustable length idler pin or spring-loaded idler to facilitate easy installation, and removal of shade for service.
F.	Shade Motor and Control System:
1.	Standard Motor: 110 VAC, single phase, 60 HZ, instantly reversible, lifetime lubricated, and equipped with internal thermal overload protector, electric brake, and pre-set accessible limit switches. Tubular motor concealed inside each shade roller tube.
2.	Quiet Standard Motor - 110 VAC motor operates at 38 dBA measured 3 feet from the motor. Makes no audible clicks when motor stops or starts. Tubular motor concealed inside each shade roller tube.
3.	Individual Control:
a.	Wall Switch - Toggle three position wall switch.
b.	Wall Switch - Key operated three position wall switch.
4.	Group Control:
a.	Motor Isolating Relay (1ISO) - One ISO relay per motor. Allows 110-120V group switching. Allows for up to 12 motors on one double throw switch. Input Voltage: 120V AC/60Hz. Output Voltage: 120V AC/60Hz. Max Output Current: 4.0 Amps.
b.	1 Motor Controller. Single motor controller for use with motorized roller shades, Venetian blinds, and louver systems. Can be used as a standalone device or part of a network. When networked, can still be independently operated and can be configured to respond to wall switches, RF remotes, and signals from 3rd party systems. On-board contact closure interface. RS-485 network with built-in network termination. On-board buttons for testing and configuring motors. Pluggable terminal blocks. Input power: 110-230VAC @ 50 / 60Hz. Output power: Maximum 6A at input power. Material: ABS plastic. Operating temperature: 32 - 140 degree F (0 - 60 degree C). Dimensions: 2-3/4 inched by 3-1/2 inches by 2-1/8 inches (70 by 90 by 54 mm). Enclosure: 4 inches by 4 inches by 4 inches (102 by 102 by 102 mm).
c.	4 Motor Isolating Relay (GC4) - Panelized version with four ISO relays. Up to three GC4s can be linked together for control of up to 12 motors from any single 15 amp double throw wall switch. Input Voltage: 120V AC/60Hz. Output Voltage: 120V AC/60Hz. Max Output Current: 4.0 Amps. Installed in a 8 inch by 8 inch by 4 inch (203 by 203 by 102 mm) box.
5.	4 Motor Controller. 4 motor controller for use with motorized roller shades, Venetian blinds and louver systems. Each port is independently operated and can be configured to respond to wall switches, RF remotes, and signals from 3rd party systems. RS-485 network with built-in network termination. Pluggable terminal blocks. Input power: 110-230VAC @ 50 / 60Hz. Output power: Maximum 6A at input power. Material: ABS plastic. Operating temperature: 32 - 140 degree F (0 - 60 degree C). Dimensions: 3-1.2 inches by 7 inches by 1-7/8 inches (89 by 178 by48 mm). Enclosure: 6 inches by 4 inches by 4 inches (152 by 102 by 102 mm)
a.	IGC4N1. Individual and Group control of up to four motors with up to three intermediate positions per motor.
6.	Radio Technology Motor- 110 VAC motor with built-in radio receiver. Tubular motor concealed inside each shade roller tube.
7.	Quiet Radio Technology Motor - 110 VAC motor with built-in radio receiver. Tubular motor concealed inside each shade roller tube.
8.	Individual Control, Group Control and Individual and Group Control:
a.	Single channel wireless handheld radio frequency transmitter.
b.	Single channel wireless handheld transmitter-Black.
c.	Four channel wireless handheld transmitter-White.
d.	Four channel wireless handheld transmitter-Black.
e.	16-Channel wireless handheld transmitter-White.
f.	16-Channel wireless handheld transmitter-Silver.
g.	Single channel wireless wall switch for radio motor control-White.
h.	Single channel wireless wall switch for radio motor control-Ivory.
i.	Four channel wireless wall switch for radio motor control-White.
j.	Four channel wireless wall switch for radio motor control-Ivory.
k.	RS-232/Dry Contact - Allows for full control of radio motor shade via RS-232/dry contact interface.
l.	Wireless Sun Sensor - Allows operation of one group of radio motors per sensor.
m.	Wireless Timer - Allows operation of one group of radio motors per timer.
n.	Repeater, 1 per project to extend range of transmitters.
o.	(URTSI II) Universal Interface - Allows for full control of radio motor shade via RS-232/485 or IR signals.
G.	Roller Tube: Fabricated from extruded aluminum, galvanized steel, or enameled steel. Diameter, wall thickness, and material selected by manufacturer to accommodate shade type and size. Fabric connected to the roller tube with LSE (low surface energy) double sided adhesive specifically developed to attach coated textiles to metal. Adhesive attachment to eliminate horizontal impressions in fabric.
H.	Headbox: Consists of extruded aluminum sections with endcaps and opacity plates.
1.	Size: 4-1/8 inches (105 mm) high by 3-1/2 inches (89 mm) wide by length required for shade being provided. 
2.	L-shaped removable front face and bottom cover and L-shaped back and top.
3.	U-shaped front, back, and top and removable bottom.
I.	Endcaps: Stamped steel with universal design suitable for mounting to ceiling, wall, and jamb. Provide size compatible with roller size.
J.	Side Channels: Double chamber fabricated from 0.06 inch (1.5 mm) thick extruded aluminum sections. One chamber accepts fabric and contains groove for fabric retainer. Other chamber accepts fabric guide and channel locator.
K.	Sill channel: 0.06 inch (1.5 mm) thick extruded aluminum channel to receive slat bar and prevent light leakage.
L.	Slat bar: Extruded aluminum bar attached to bottom of shade. Bar does not retract into headbox.
M.	Channel locator: Injected molded nylon insert to align side and sill channels with headbox.
N.	Fabric guide: Plated steel transition for fabric rolling into side channel.
O.	Fabric retainer: System designed to prevent disengagement of fabric from side channels due to normal variations of air pressure caused by doors opening, HVAC systems, and temperature differences between room and window well. System consists of horizontal steel stays installed in shade, covered with fabric, and spaced at regular intervals. Grommets installed through stays are held within groove of side channel chamber.
P.	Exposed aluminum finish:
1.	Finish: Selected from Manufacturers standard range.
2.	Custom powder coat as selected by the Architect.
2.7	FABRIC
A.	Light-Filtering Fabrics
1.	PVC Coated Fiberglass
a.	Basketweave
1)	E Screen 1% by Mermet: PVC coated fiberglass yarn woven in 2 by 2 basketweave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G21. 1 percent open, .020 inches thick, 13.3 oz/square yard.
2)	E Screen 3% by Mermet: PVC coated fiberglass yarn woven in 2 by 2 basketweave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G21. 3 percent open, .017 inches thick, 11.6 oz/square yard.
3)	E Screen 5% by Mermet: PVC coated fiberglass yarn woven in 2 by 2 basketweave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G21. 5 percent open, .016 inches thick, 10.7 oz/square yard.
4)	E Screen 10% by Mermet: PVC coated fiberglass yarn woven in 2 by 2 basketweave. .016 inches thick. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 10 percent open, .020 inches thick, 10.3 oz/square yd.
5)	E Screen 1% with KOOLBLACK by Mermet: PVC coated fiberglass yarn woven in 2 by 2 basketweave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 1 percent open, .021 inches thick. Weight: 12.95 oz/square yard.
6)	E Screen with KOOLBLACK. 3 percent open factor by Mermet: PVC coated fiberglass yarn woven in 2 by 2 basketweave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 3 percent open, .020 inches thick, 11.3 oz. per square yard.
7)	E Screen with KOOLBLACK. 5 percent open factor by Mermet: PVC coated fiberglass yarn woven in 2 by 2 basketweave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 5 percent open, .019 inches thick, 10.6 oz/square yard.
8)	E Screen Deco 1% by Mermet: PVC coated fiberglass yarn woven in 2 by 2 basketweave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 1 percent open, .022 inches thick. 12.30 oz/square yard.
9)	E Screen Deco 3% by Mermet: PVC coated fiberglass yarn woven in 2 by 2 basketweave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 3 percent open, .019 inches thick. 11.50 oz/square yard.
10)	E Screen Chroma by Mermet: PVC coated fiberglass yarn woven in 2 by 2 basketweave with metalized coating on outward side. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 3 percent open, .020 inches thick. 11.92 oz/square yard.
11)	Natte 5% by Mermet: PVC coated fiberglass yarn woven in 2 by 2 basketweave. NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 5% open. Thickness: 0.022 inches. Weight: 14.13 oz/square yard.
12)	Natte 10% by Mermet: PVC coated fiberglass yarn woven in 2 by 2 basketweave. NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 5% open. Thickness: 0.021 inches. Weight: 13.48 oz/square yard.
13)	S Screen 1% by Mermet: PVC coated fiberglass wrapped in polyester thread in a plain weave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 1 percent open, .041 inches thick, 19.10 oz/square yard.
14)	S Screen 4% by Mermet: PVC coated fiberglass wrapped in polyester thread in a plain weave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. ASTM E 2180 and ASTM G 21. Environmental benefits: RoHS - lead free. 4 percent open, .037 inches thick, 18.9 oz/square yard.
15)	S Screen Naturals 5% by Mermet: PVC coated fiberglass wrapped in polyester thread in a fancy weave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 5 percent open, .042 inches thick 15 oz/square yard.
16)	SheerWeave Series SW2000 by Phifer: 500 denier fiberglass, vinyl coated and woven into a 2 by 2 basket weave. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 14.26 oz/sq yd, .019 inches thick. Series SW2000 5 percent open.
17)	SheerWeave Series SW2100 by Phifer: 500 denier fiberglass, vinyl coated and woven into a 2 by 2 basket weave. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 14.26 oz/sq yd, .019 inches thick. Series SW2100 10 percent open.
18)	SheerWeave Series SW2400 (2410) by Phifer: 500 denier fiberglass, vinyl coated and woven into a 2 x 2 basket weave. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 3 percent open .019 inches thick. 14.1 oz/square yard.
19)	SheerWeave Series SW2500 by Phifer: 500 denier fiberglass, vinyl coated and woven into a 2 x 2 basket weave. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 1 percent open, .024 inches thick. 16.39 oz/square yard.
20)	SheerWeave Series SW2600 (2360) by Phifer: 500 denier fiberglass, vinyl coated and woven into a 2 x 2 basket weave. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 10 percent open, .017 inches thick. 10.4 oz/square yard.
21)	SheerWeave Series SW2900 (2390) by Phifer: 500 denier fiberglass, vinyl coated and woven into a 2 x 2 basket weave. Fire rating: California U.S. Title 19 (small scale), NFPA 101 (Class A Rating), BS 5867 Part 2 Type B Performance, CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80, NFPA 701 TM1 (small scale), IBC Section 803.1.1 (Class A Rating), NFPA 701 TM2 (large scale). Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 5 percent open. .017 inches thick. 11.8 oz/square yard.
22)	SheerWeave Basic 3% by Phifer. An economical alternative to traditional solar screen fabrics. Fire Rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, CAN/ULC-S 109 (large and small scale), NFPA 701 TM2 (large scale), CAN/CGSB2-4.162-M80. Bacteria and Fungal ResistanceASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental Certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 3 percent Open. Average Fabric Thickness: .025 inch. Average Fabric Weight: 16.4 ounces per square yard.
23)	SheerWeave Basic 5% by Phifer. An economical alternative to traditional solar screen fabrics. Fire Rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, CAN/ULC-S 109 (large and small scale), NFPA 701 TM2 (large scale), CAN/CGSB2-4.162-M80. Bacteria and Fungal ResistanceASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental Certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 5 percent Open. Average Fabric Thickness: 0.022 inch. Average Fabric Weight: 14.1 ounces per square yard.
24)	SheerWeave Performance+ 2500 by Phifer: 500 denier fiberglass, vinyl coated and woven into a 2 x 2 basket weave with metalized coating on outward side. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to GREENGUARD and GREENGUARD standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 1 percent open, .024 inches thick. 16.39 oz/square yard.
25)	SheerWeave Performance+ 2410 by Phifer: 500 denier fiberglass, vinyl coated and woven into a 2 x 2 basket weave with metalized coating on outward side. Fire rating: California U.S. Title 19 (small scale), NFPA 101 (Class A Rating), BS 5867 Part 2 Type B Performance, CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80, NFPA 701 TM1 (small scale), IBC Section 803.1.1 (Class A Rating), NFPA 701 TM2 (large scale). Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 3 percent open .019 inches thick. 14.1 oz/square yard.
26)	SheerWeave Performance+ 2390 by Phifer: 500 denier fiberglass, vinyl coated and woven into a 2 x 2 basket weave with metalized coating on outward side. Fire rating: California U.S. Title 19 (small scale), NFPA 101 (Class A Rating), BS 5867 Part 2 Type B Performance, CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80, NFPA 701 TM1 (small scale), IBC Section 803.1.1 (Class A Rating), NFPA 701 TM2 (large scale). Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 5 percent open. .017 inches thick. 11.8 oz/square yard.
b.	Ribbed Weave
1)	M Screen 1% by Mermet: PVC coated fiberglass in 1 by 2 ribbed weave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 1 percent open, .022 inches thick, 13.12 oz/square yard.
2)	M Screen 3% by Mermet: PVC coated fiberglass in 1 by 2 ribbed weave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 3 percent open, .022 inches thick, 12.27 oz/square yard.
3)	M Screen 5% by Mermet: PVC coated fiberglass in 1 by 2 ribbed weave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 5 percent open, .022 inches thick, 11.3 oz/square yard.
4)	M Screen Deco 5% by Mermet: PVC coated fiberglass in 1 by 2 ribbed weave. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 5 percent open, .020 inches thick, 11.3 oz/square yd.
5)	SheerWeave Series SW1000 SunScreen by Phifer. PVC coated fiberglass in a ribbed weave. Fire Classification: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large scale). Bacteria and Fungal Resistance: ASTM E 2180, ASTM G21, AATCC30 Part 3, ASTM D 3273, GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental: Certified to UL GREENGUARD and GREENGUARD Gold standards. Lead Free: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 25% Open.
6)	SheerWeave Series SW3000 by Phifer: Vinyl coated fiberglass and vinyl coated polyester woven into 62 by 20 mesh. Fire rating: NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), NFPA 701 TM2 (large scale). Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 13.46 oz/sq yd, .028 inches thick. 14 percent open.
7)	SilverScreen 4% by Verosol: 36 percent fiberglass and 64 percent vinyl with an ultra-fine layer of aluminum on the backside. Fire rating: NFP 92503 specification M1, NFPA 701, B5 5867 Part 2 Type B, AS 1530. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - Lead Free, Formaldehyde free. 5 percent Open, 0.020 inches thick, 11.7974 oz/square yard.
c.	Satin Weave
1)	T Screen with KOOLBLACK 1% by Mermet: PVC coated fiberglass woven mesh. Dark on one side, light on the other. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 1 percent open, .024 inches thick, 13.54 oz/square yard.
2)	T Screen with KOOLBLACK 3% by Mermet: PVC coated fiberglass woven mesh. Dark on one side, light on the other. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 3 percent open, .029 inches thick, 13.27 oz/square yard.
3)	T Screen with KOOLBLACK. 5 percent open factor by Mermet: PVC coated fiberglass woven mesh. Dark on one side, light on the other. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 5 percent open, .027 inches thick, 12.48 oz/ square yard.
4)	T Screen Deco 1% by Mermet: PVC coated fiberglass satin style. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 1 percent open, .028 inches thick, 13.76 oz/square yd.
5)	T Screen Deco 3% by Mermet: PVC coated fiberglass satin style. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 3 percent open, .028 inches thick, 12.98 oz/square yard.
6)	T Screen Deco 5% by Mermet: PVC coated fiberglass satin style. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 5 percent open, .028 inches thick, 11.89 oz/square yard.
d.	Twill Weave
1)	9803 3% by Mermet: PVC coated fiberglass woven mesh. Dark on one side, light on the other. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 3 percent open, .025 inches thick, 11.6 oz/square yard.
2)	SheerWeave Series SW2701 by Phifer: Duplex basketweave fabric-light exterior color combined with dark interior color for thermal comfort and view-through. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4. 162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental Certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 1 percent open. .027 inches thick. 14.6 oz/square yard.
3)	SheerWeave Series SW2703 by Phifer: Duplex basketweave fabric-light exterior color combined with dark interior color for thermal comfort and view-through. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4. 162-M80, CAN/ULC S-102. Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. 3 percent open. .028 inches thick. 14.0 oz/square yard.
4)	SheerWeave Series SW2705 by Phifer: Duplex basketweave fabric-light exterior color combined with dark interior color for thermal comfort and view-through. GREENGUARD Gold. Manufacturer to supply GREENGUARD Gold certificate. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4. 162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental Certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 5 percent open. .025 inches thick. 11.8 oz/square yard.
5)	SheerWeave Series SW2710 by Phifer: Duplex basketweave fabric-light exterior color combined with dark interior color for thermal comfort and view-through. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4. 162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental Certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 10 percent open. .023 inches thick. 10.4 oz/square yard.
6)	T Screen 1% by Mermet: PVC coated fiberglass woven mesh. White, charcoal, or pearl backing color. Fire rating: NFPA 701-15 TM1, California U.S. Title 19 CAN/ULC-S109-14 Small Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. 1 percent open, .028 inches thick, 13.83 oz/square yard.
2.	Fiberglass
a.	Mock Leno Weave
1)	GreenScreen Nature 5%: GreenScreen Nature is an inherently fire-retardant fabric constructed of 100 percent fiberglass yarn in a mock leno weave. Additional fire retardancy chemicals are not required. Recyclable, halogen- and PVC-free. Red List compliant. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109 Small and Large Scale. Microbial Resistance, ASTM E 2180 and ASTM G 21: Pass. UL GREENGUARD, GREENGUARD Gold. 5 percent open. Average Fabric Thickness: 0.010 inch (.024 mm). Average Fabric Weight: 5.10 ounces per square yard (174 grams per square meter).
b.	Ribbed Weave
1)	Vizela less than 1% by Mermet: 100 percent fiberglass with an EVA coating and PVC free. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E 2180, ASTM G 21. less than 1% open, .013 inches thick, 8.7 oz/square yard.
3.	PVC Coated Polyester
a.	Basketweave
1)	SunTex 90 by Phifer. Vinyl-coated polyester woven into a basketweave. For outdoor use. Fire Classification: NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), CFR 49V 571.302 (FMVSS 302), California Technical Bulletin 117, CAN/ULC S-109 (large scale) and ASTM E-662. Bacteria and Fungal Resistance: ASTM E 2180 and ASTM G21; includes Microban antimicrobial additives. Environmental: Certified to UL GREENGUARD and GREENGUARD Gold standards. Lead Free: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 10% open. Thickness: 0.039 inches. Weight: 17.2 oz/square yard.
2)	SunTex 90 Design by Phifer. Vinyl-coated polyester woven into a basketweave. For outdoor use. Fire Classification: NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), CFR 49V 571.302 (FMVSS 302), California Technical Bulletin 117, CAN/ULC S-109 (large scale) and ASTM E-662. Bacteria and Fungal Resistance: ASTM E 2180 and ASTM G 21; includes Microban antimicrobial additives. Environmental: Certified to UL GREENGUARD and GREENGUARD Gold standards. Lead Free: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 10% open. Thickness: 0.039 inches. Weight: 17.2 oz/square yard.
3)	SunTex 95 by Phifer. Vinyl-coated polyester woven into a basketweave. For outdoor use. Fire Classification: NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), CFR 49V 571.302 (FMVSS 302), California Technical Bulletin 117, CAN/ULC S-109 (large scale) and ASTM E-662. Bacteria and Fungal Resistance: ASTM E 2180 and ASTM G 21; includes Microban antimicrobial additives. Environmental: Certified to UL GREENGUARD and GREENGUARD Gold standards. Lead Free: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 5% open. Thickness: 0.029 inches. Weight: 15.4 oz/square yard.
4)	SunTex 97 by Phifer. Vinyl-coated polyester woven into a basketweave. For outdoor use. Fire Classification: NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), CFR 49V 571.302 (FMVSS 302), California Technical Bulletin 117, CAN/ULC S-109 (large scale) and ASTM E-662. Bacteria and Fungal Resistance: ASTM E 2180 and ASTM G 21; includes Microban antimicrobial additives. Environmental: Certified to UL GREENGUARD and GREENGUARD Gold standards. Lead Free: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 3% open. Thickness: 0.033 inches. Weight: 16.0 oz/square yard.
5)	SheerWeave Series PW3500 (4000) by Phifer: Vinyl coated polyester yarn woven into basketweave pattern. Uses DOW ECOLIBRIUM bio-based, phthalate-free plasticizer. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental Certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content, REACH (EC 1907/2006) compliant. 5 percent open, 19.2 oz/sq yd, .036 inches thick.
6)	SheerWeave Series PW4100 by Phifer: Vinyl coated polyester yarn woven into basketweave pattern. Uses DOW ECOLIBRIUM bio-based, phthalate-free plasticizer. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G 21, ASTM G 22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental Certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content, REACH (EC 1907/2006) compliant. 10 percent open, 17.5 oz/sq yd, .035 inches thick.
7)	SheerWeave Series PW4400 by Phifer: Vinyl coated polyester yarn woven into basketweave pattern. Uses DOW ECOLIBRIUM bio-based, phthalate-free plasticizer. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G21, ASTM G22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental Certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content, REACH (EC 1907/2006) compliant. 3 percent open, 20.7 oz/sq yd, .037 inches thick.
8)	SheerWeave Series PW4500 by Phifer: Vinyl coated polyester yarn woven into basketweave pattern. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale). Bacteria and fungal resistance: ASTM E 2180, ASTM G21, ASTM G22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to GREENGUARD and GREENGUARD UL Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 5 percent open, 14.4 oz/sq yd, .024 inches thick.
9)	SheerWeave Series PW4600 by Phifer: Vinyl coated polyester yarn woven into basketweave pattern. Fire rating: Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale). Bacteria and fungal resistance: ASTM E 2180, ASTM G21, ASTM G22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 3 percent open, 17.4 oz/sq yd, .030 inches thick.
10)	Soltis Harmony 88 by Ferrari. PVC-coated polyester with pre-tensioning process for dimensional stability. Flame Retardancy: B-s2,d0 / EN 13501-1, M1/NFP92-507, B1/DIN 4102-1, BS 7837, BS 5867, Schwerbrennbar Q1-Tr1/ONORM, A3800-1, CAN/ULC-S 109, M1/UNE 23727-90, Classe 1/EN 13773, CSFM T19, Method 1 and 2/ NFPA 701, Class A/ASTM E84, 1530.3/AS NZS, Group 1/AS NZS 3837, G1/GOST.30244.94. Environment: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Recyclable through TexyLoop. 8 percent open, .018 inches thick, 10.61 oz/square yard.
11)	Soltis Horizon 86 by Ferrari. PVC-coated polyester with pre-tensioning process for dimensional stability. Flame Retardancy: B-s2,d0 / EN 13501-1, M1/NFP92-507, B1/DIN 4102-1, BS 7837, BS 5867, Schwerbrennbar Q1-Tr1/ONORM, A3800-1, CAN/ULC-S 109, M1/UNE 23727-90, Classe 1/EN 13773, CSFM T19, Method 1 and 2/ NFPA 701, Class A/ASTM E84, 1530.3/AS NZS, Group 1/AS NZS 3837, G1/GOST.30244.94. Environment: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Recyclable through TexyLoop. 14 percent open, .018 inches thick, 11.2 oz/square yard.
12)	Soltis Master 99 by Serge Ferrari: PVC-coated polyester with silver backing on outside and pre-tensioning process for dimensional stability. Fire rating: Method 1/NFPA 701, CSFM T19, Class A/ ASTM E 84. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Recyclable through TexyLoop. 3 percent open, .0156 inches thick, 8.6 oz/ square yard.
13)	Soltis Perform 92 by Serge Ferrari: PVC-coated polyester with silver backing on outside and pre-tensioning process for dimensional stability. Fire rating: Method 1/NFPA 701, CSFM T19, Class A/ ASTM E84. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Recyclable through TexyLoop. 4 percent open, .018 inches thick, 12.4 oz/square yard.
b.	Decorative Weave
1)	SheerWeave Series SW5000 by Phifer: Polyester and vinyl coated polyester woven into a 42 by 20 mesh. Fire rating: California Technical Bulletin 117 Sect. E. Part 1/ /UBC (Class 1)/British Standard 5867. Varies depending on color. Bacteria and fungal resistance: ASTM E 2180, ASTM G21, ASTM G22, ASTM D3273, AATCC 30 Part 3, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 12.3 to14.5 oz/sq yd, .035 inches - .044 inches thick, depending on color. 5 to 10 percent open, depending on color.
c.	Plain Weave
1)	SheerWeave PW4800 by Phifer: Vinyl coated polyester with maximum UV blockage. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ ULC-S 109 (large and small scale), CAN/CGSB2-4.162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G21, ASTM G22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 1 percent open. 18.5 oz/sq yd, .036 inches thick.
d.	Twill Weave
1)	SheerWeave Series PW4550 by Phifer: Vinyl coated polyester yarn woven into basketweave pattern. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale). Bacteria and fungal Resistance. ASTM E 2180, ASTM G21, ASTM G22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 5 percent open, 12.5 oz/sq yd, .025 inches thick.
2)	SheerWeave Series PW4650 by Phifer: Vinyl coated polyester yarn woven into basketweave pattern. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale). Bacteria and fungal Resistance. ASTM E 2180, ASTM G21, ASTM G22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. 3 percent open, 13.3 oz/sq yd, .026 inches thick.
3)	SheerWeave PW4901 by Phifer: Vinyl coated polyester with maximum UV blockage. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ ULC-S 109 (large and small scale), CAN/CGSB2-4. 162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G21, ASTM G22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. UV protection: Seal of Approval by the Melanoma International Foundation (MIF) for effectiveness in preventing sun damage to the skin or eyes. 1 percent open. 15.85 oz/sq yd, .028 inches thick.
4)	SheerWeave PW4903 by Phifer: Vinyl coated polyester with maximum UV blockage. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), NFPA 101 (Class A Rating), IBC Section 803.1.1 (Class A Rating), BS 5867 Part 2 Type B Performance, NFPA 701 TM2 (large scale), CAN/ ULC-S 109 (large and small scale), CAN/CGSB2-4. 162-M80. Bacteria and fungal resistance: ASTM E 2180, ASTM G21, ASTM G22, AATCC30 Part 3, ASTM D 3273, UL GREENGUARD Mold and Bacteria Standard ASTM 6329; includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. UV protection: Seal of Approval by the Melanoma International Foundation (MIF) for effectiveness in preventing sun damage to the skin or eyes. 3 percent open. 14.9 oz/sq yd, .027 inches thick.
4.	Polyester
a.	Basketweave
1)	SheerWeave Series SW8000 by Phifer: PVC-free polyester. Fire rating: California U.S. Title 19 (small scale), BS 5867 2008 Part 2 Type B Performance, IBC Section 803.1.1 (Class A Rating), NFPA 701 TM1 (small scale), NFPA 701 TM2 (large scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4. 162-M80, B1 (DIN 4102-1), NFPA 101 (Class A Rating). Bacteria and fungal resistance: ASTM E 2180, ASTM G21. Environmental certification: Cradle to Cradle Certified Bronze and certified to ul GREENGUARD and GREENGUARD Golld standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, ANSI/WCMA A 100.1-2007 for lead content, US Consumer Product Safety Commission Section 101and REACH (EC 1907/2006) compliant. UV Protection: Seal of Approval by the Melanoma International Foundation (MIF) for effectiveness in preventing sun damage to the skin or eyes. 3% open. .019 inches thick. 7.35 oz/square yard.
b.	Decorative Weave
1)	SheerWeave Series SW7450 by Phifer: PVC-free polyester with acrylic coating. Fire rating: California Technical Bulletin 117, IBC Section 803.1.1 (Class A Rating), NFPA 101 (Class A Rating). Bacteria and Fungal Resistance: ASTM G21-96, AATCC 174-1998 Part II and III. Environmental Certification: Certified to GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe Use: RoHS/Directive 2002/95/EC, ANSI/WCMA A 100.1-2007 for lead content, US Consumer Product Safety Commission Section 101. UV Protection: Seal of Approval by the Melanoma International Foundation (MIF) for effectiveness in preventing sun damage to the skin or eyes. .026 inches thick, 6.54 oz/square yard.
c.	Fancy Weave
1)	Verona Daylight by Mermet. 100% PVC-free polyester. Fire Classifications: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Bacterial Resistance: ASTM E2180, ASTM G21. Environment: RoHS - Lead Free, certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. 1% open. .021 inches thick, 5.90 oz/square yard.
d.	Diamond Knit
1)	GreenScreen Evolve 3%: GreenScreen Evolve is a fire retardant PVC-free fabric is constructed of 100 percent polyester yarn, with up to 78% Repreve polyester. Repreve is recycled and recyclable, contains low VOC's, and made in the USA. Fire rating: NFPA 701-99 TM1, California U.S. Title 19, Cradle to Cradle Certified Silver, UL GREENGUARD, GREENGUARD Gold, PVC Free. 3 percent open. Average Fabric Thickness: 0.027 inch (.068 mm). Average Fabric Weight: 8.41 ounces per square yard. Microbial Resistance, ASTM E2180 and ASTM G21: Pass.
2)	GreenScreen Revive 1%. GreenScreen Revive is a fire retardant PVC-free fabric constructed of 100 percent polyester yarn, with a minimum of 89 percent Repreve polyester. Repreve is recycled and recyclable, contains low VOC's, and made in the USA. Fire rating: NFPA 701-99 TM1, California U.S. Title 19, Cradle to Cradle Certified Silver, UL GREENGUARD, GREENGUARD Gold. 1 percent open. Average Fabric Thickness: 0.019 inch (0.48 mm). Average Fabric Weight: 5.87 ounces per square yard.
3)	GreenScreen Revive 5%. GreenScreen Revive is a fire retardant PVC-free fabric is constructed of 100 percent polyester yarn, with a minimum of 89 percent Repreve polyester. Repreve is recycled and recyclable, contains low VOC's, and made in the USA. Fire rating: NFPA 701-99 TM1, California U.S. Title 19, Cradle to Cradle Certified Silver, UL GREENGUARD, GREENGUARD Gold, Green PVC Free. 5 percent open. Average Fabric Thickness: 0.017 inch (.043 mm). Average Fabric Weight: 5.01 ounces per square yard.
e.	Linen Pattern
1)	SheerWeave Series SW7650 by Phifer: PVC-free polyester. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), BS 5867 Part 2 Type B Performance, CAN/ULC-S 109 (large and small scale). Bacteria and fungal resistance: ASTM G21-96, AATCC 174-1998 Part II and III. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, ANSI/WCMA A 100.1-2007 for lead content, US Consumer Product Safety Commission Section 101. UV protection: Seal of Approval by the Melanoma International Foundation (MIF) for effectiveness in preventing sun damage to the skin or eyes. .014 inches thick, 6.2 oz/square yard.
5.	Thermoplastic Olefin
a.	Basketweave
1)	SheerWeave Infinity2 1%: sustainable window treatment fabric eco-friendly basketweave. Core yarn and coating are PVC-free, lead-free and 100 percent recyclable. Fire classification: ASTM E-84 (Class I), NFPA 701-2004 TM1 (small scale), NFPA 101 (Class A Rating) and CAN/ULC-S 109-03 Large, UL GREENGUARD, GREENGUARD Gold. 1 percent open. Average Fabric Thickness: .033 inch (.838 mm) Average Fabric Weight: 14.63 ounces per square yard.
2)	SheerWeave Infinity2 3%: sustainable window treatment fabric eco-friendly basketweave. Core yarn and coating are PVC-free, lead-free and 100 percent recyclable. Fire classification: ASTM E-84 (Class I), NFPA 701-2004 TM1 (small scale), NFPA 101 (Class A Rating) and CAN/ULC-S 109-03 Large, UL GREENGUARD, GREENGUARD Gold. 3 percent open. Average Fabric Thickness: .031 inch (.79 mm) Average Fabric Weight: 13.69 ounces per square yard.
3)	SheerWeave Infinity2 5%: sustainable window treatment fabric eco-friendly basketweave. Core yarn and coating are PVC-free, lead-free and 100 percent recyclable. Fire classification: ASTM E-84 (Class I), NFPA 701-2004 TM1 (small scale), NFPA 101 (Class A Rating) and CAN/ULC-S 109-03 Large, UL GREENGUARD, GREENGUARD Gold. 5 percent open. Average Fabric Thickness: .03 inch (.76 mm). Average Fabric Weight: 12.82 ounces per square yard.
B.	Room Darkening Fabrics
1.	Opaque
a.	PVC Coated Fiberglass
1)	SheerWeave Series SW7100 Blackout by Phifer: PVC-coated Fiberglass laminated with a 2-ply PVC film. Fire rating: NFPA 701 TM1 (small scale), NFPA 701 TM2 (large scale), BS 5867 Part 2 Type B Performance, CAN/ULC-S 109 (large and small scale), NFPA 101 (Class B Rating), IBC Section 803.1.1 (Class B Rating). Bacterial and fungal resistance: ASTM E 2180, ASTM G21, ASTM G22, AATCC30 Part 3, ASTM D 3273, GREENGUARD Mold and Bacterial Standard ASTM 6329; Style 2000 face includes Microban antimicrobial additives. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe Use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101, ANSI/WCMA A 100.1-2007 for lead content and REACH (EC 1907/2006) compliant. Opaque, .025 inches thick, 21.6 oz/square yard, opaque.
b.	Fiberglass
1)	Apagon Style III is a 3-ply opaque shade fabric consisting of vinyl, fiberglass, and a proprietary coating for maximum blackout. Thread Count: 59 threads per square inch. Fire rating: NFPA 701-2019 Test Method 1. Environmental Benefits: ASTM D3335 85a - Lead Testing. Bacterial and fungal resistance: ASTM Method G-21-15 - Resistance to Fungi. Opaque, .0131 inches thick, 12.8 oz/square yard.
2)	Flocke by Mermet: Opaque, PVC-free fiberglass textile with acrylic flocked backing. Antistatic treated. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E2180, ASTM G21. Draper shades made with this fabric are GreenSpec listed. Opaque, .020 inches thick, 15.93 oz/square yard.
3)	SunBloc Series SB9000: Close woven fiberglass base textile with sun-resistant vinyl film bonded to each side, opaque with minimum tensile strength of 190 pounds for warp and 180 pounds for fill. Fire rating: NFPA 701 1006-Test 1, California U.S. Title 19. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. REACH and RoHS compliant - Lead Free. Bacterial and fungal resistance: ASTM E2180, ASTM G21. Washable and stain resistant. Same color both sides. Opaque, .015 inches thick, 12 oz/square yard.
4)	SunBloc Series SB9100: Close woven fiberglass base textile with sun-resistant vinyl film bonded to each side, opaque with minimum tensile strength of 190 pounds for warp and 180 pounds for fill. Fire rating: NFPA 701 1006-Test 1, California U.S. Title 19. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. REACH and RoHS compliant - Lead Free. Bacterial and fungal resistance: ASTM E2180, ASTM G21. Washable and stain resistant. White exterior in all colors. Opaque, .013 inches thick, 12 oz/square yard.
c.	PVC Coated Polyester.
1)	Soltis Opaque B92 by Serge Ferrari. PVC-coated polyester with silver backing on outside and pre-tensioning process for dimensional stability. Fire rating: Method 1 and 2/NFPA 701, Class A / ASTM E84. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Recyclable through TexyLoop. 0 percent open, .0312 inches thick, 19.1 oz/square yard.
d.	Polyester
1)	SheerWeave Series SW7000 Blackout by Phifer: PVC-free polyester with acrylic foamed backing. Fire rating: California U.S. Title 19 (small scale), BS 5867 Part 2 Type B Performance, IBC Section 803.1.1 (Class A Rating), NFPA 101 (Class A Rating), NFPA 701 TM1 (small scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB2-4. 162-M80. Bacteria and fungal resistance: ASTM G21, AATCC 174-1998 Part II and III. E/nvironmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content. Draper shades made with this fabric are GreenSpec listed. Opaque, .030 inches thick, 13.92 oz/square yard.
2)	SheerWeave Series SW7400 by Phifer: PVC-free polyester with acrylic foamed backing. Fire rating: California U.S. Title 19 (small scale), CAN/ULC-S 109 (large and small scale), CAN/CGSB 2-4. 162-M80, NFPA 701 TM1 (small scale), NFPA 701 TM2 (large scale). Bacteria and Fungal Resistance: ASTM G21-96, AATCC 174-1998 Part II and III. Environmental Certification: Certified to UL GREENGUARD and GRENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe Use: RoHS/Directive 2002/95/EC, ANSI/WCMA A 100.1-2007 for lead content, US Consumer Product Safety Commission Section 101. UV Protection: Seal of Approval by the Melanoma International Foundation (MIF) for effectiveness in preventing sun damage to the skin or eyes. Opaque, .029 inches thick, 12.53 oz/square yard.
3)	SheerWeave Series SW7500 by Phifer: PVC-free polyester with an acrylic coating. Fire rating: California U.S. Title 19 (small scale), NFPA 101 (Class A Rating), NFPA 701 TM1 (small scale), BS 5867 Part 2 Type B Performance, CAN/ULC-S 109 (large and small scale), IBC Section 803.1.1 (Class A Rating), CAN/CGSB 2-4.162-M80. Bacterial and fungal resistance: ASTM E 2180 and ASTM G21. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, US Consumer Product Safety Commission Section 101 and ANSI/WCMA A 100.1-2007 for lead content. Opaque, .016 inches thick, 12.14 oz/square yard.
4)	SheerWeave Series SW7600 by Phifer: PVC-free polyester with an acrylic foamed backing. Fire rating: California U.S. Title 19 (small scale), NFPA 701 TM1 (small scale), BS 5867 Part 2 Type B Performance, CAN/ULC-S 109 (large and small scale). Bacterial and fungal resistance: ASTM G21-96, AATCC 174-1998 Part II and III. Environmental certification: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. Safe use: RoHS/Directive 2002/95/EC, ANSI/WCMA A 100.1-2007 for lead content, US Consumer Product Safety Commission Section 101. UV protection: Seal of approval by the Melanoma International Foundation (MIF) for effectiveness in preventing sun damage to the skin or eyes. Opaque, .020 inches thick, 11.8 oz/square yard.
5)	Verona Twilight by Mermet. 50 percent Polyester and 50 percent acrylic with foam backing. Duraguard fabric protector and Sanitized Antimicrobial Protection. Plain weave that is 100% PVC free. Fire rating: NFPA 701-10 TM1, California U.S. Title 19, CAN/ULC-S109-03 Small and Large Flame Test. Environmental Benefits: Certified to UL GREENGUARD and GREENGUARD Gold standards for low chemical emissions into indoor air during product usage. RoHS compliant - lead free. Bacterial and fungal resistance: ASTM E2180. 0% open, .024 inches thick, 11.65 oz/square yard.
C.	Color and pattern: __________, No. _____.
D.	Color and pattern: As indicated in Color Schedule on Drawings.
E.	Color and pattern: As selected by Architect from manufacturer's standard range.
F.	Custom Printed Graphics: As submitted to manufacturer in accordance with manufacturer's guidelines
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Coordinate requirements for blocking and structural supports to ensure adequate means for installation of window shades.
B.	Coordinate requirements for blocking, construction of shade pockets, and structural supports to ensure adequate means for installation of window shades.
C.	Coordinate installation of recessed shade pockets with construction of suspended acoustical panel ceilings specified in Section 09 51 23 - Acoustical Tile Ceilings.
D.	Coordinate installation of recessed shade pockets with construction of suspended gypsum board ceilings specified in Section 09 21 16.33 - Gypsum Board Area Separation Wall Assemblies.
E.	Coordinate requirements for power supply conduit, and wiring required for window shade motors and controls.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions.
B.	Install roller shades level, plumb, square, and true. Allow proper clearances for window operation hardware.
C.	Shade pockets:
1.	Install shade pockets prior to installation of suspended ceiling system. Attach to supporting structure with screws through top of pocket at 24 inches (610 mm) minimum centers.
2.	Install shade pockets in conjunction with installation of suspended ceiling system. Attach to supporting structure with screws through top of pocket at 24 inches (610 mm) minimum centers.
3.	Install corner pieces securely and in alignment with pockets. 
4.	Install pocket ends securely and in alignment with pockets. 
5.	After interior construction is essentially complete, install shade and operating mechanism in pocket.
D.	Install the following items to conceal roller and operating mechanism. Do not use exposed fasteners.
1.	Fascias.
2.	Closure panels.
3.	Endcaps.
E.	Install headbox, side channels, and sill channel with sealant specified in Section 07 90 00 - Joint Protection.
F.	Position shades level, plumb, and at proper height relative to adjacent construction. Secure with fasteners recommended by manufacturer.
3.4	TESTING AND DEMONSTRATION
A.	Test motorized window shades to verify that controls, limit switches, interface to other building systems, and other operating components are functional. Correct deficiencies.
B.	Test window shades to verify that operating mechanism, fabric retainer, and other operating components are functional. Correct deficiencies.
1.	Crank.
2.	Chain and clutch.
3.	Motorized operating mechanism.
C.	During daylight hours, lower shades and turn off interior lights. Verify that there are no light leaks at perimeter or within shade assembly. Correct deficiencies.
D.	Demonstrate operation of shades to Owner's designated representatives.
3.5	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.
3.6	SCHEDULES
A.	Manually Operated Shades: 
1.	Shade Type SM-1 Single Roller
a.	Mounting Type: 
2.	Shade Type SM-2 Dual Roller
a.	Mounting Type: 
B.	Motorized Shades:
1.	Shade Type MS-1 Single Roller
a.	Configuration/Mounting:
2.	Shade Type MS-2 Dual Roller
a.	Configuration/Mounting:

END OF SECTION