SECTION 11 67 33

CLIMBING WALL SYSTEMS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2019 -  2019 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Climbing wall system components of the following types:
1.	Climbing walls.
2.	Hand holds.
3.	Mat locking system and safety mats.
4.	Climbing wall accessories.
B.	Physical education equipment of the following types:
1.	Indoor jungle gym.
2.	Ninja course.
C.	Premium climbing wall systems.
1.2	RELATED SECTIONS
A.	Section 03 30 00 - Cast-in-Place Concrete.
B.	Section 05 50 00 - Metal Fabrications.
C.	Section 06 10 00 - Rough Carpentry.
D.	Section 09 21 16.33 - Gypsum Board Area Separation Wall Assemblies.
1.3	REFERENCES
A.	ASTM International (ASTM):
1.	ASTM E84 - Standard Test Method for Surface Burning Characteristics of Building Materials.
2.	ASTM F1292 - Standard Specification for Impact Attenuation of Surfacing Materials within the Use Zone of Playground Equipment.
3.	ASTM F2440 - Standard Specification for Indoor Wall/Feature Padding.
B.	Climbing Wall Association (CWA).
1.	CWA Standards for the Design and Engineering of Manufactured Climbing Structures.
C.	National Fire Protection Association (NFPA):
1.	NFPA 286 - Standard Methods of Fire Tests for Evaluation Contribution of Wall and Ceiling Interior Finish to Room Fire Growth.
1.4	DEFINITIONS
A.	Artificial Climbing Wall: A wall with indentations, overhand, roofs or other projections such as hand holds, or foot holds used for rock climbing.
B.	Surfacing: The patent-pending substrate with aggregate that provides durable and texture while allowing the wood or colored stain to show through to create visual appeal. 
C.	Route: Surface for climbing that is approximately four to five feet wide, extending vertically from the floor. 
D.	Anchor Point: The location on the climbing wall where anchors are placed that are used to belay climbers during their climb. 
E.	Top Rope Climbing Route: Climbing routes which have anchor points at the top of the wall that support the climber via rope that is held by a belayer on the floor below the climber. The anchor point is always located above the climber.
F.	Lead Climbing Route: Climbing routes which have anchor points throughout the wall that support the climber via rope that is held by a belayer on the floor below the climber. The anchor point may sometime be located below the climber until the climber ascends above that anchor point and connects to another anchor point. 
1.5	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Verification Samples: For each finish product specified, two samples, minimum size 6 inches (150 mm) square representing actual product, color, and patterns.
D.	Shop Drawings: Include details of materials, construction and finish. Include relationship with adjacent construction. 
1.6	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
D.	Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
1.	Intent of mock-up is to demonstrate quality of workmanship and visual appearance.
2.	If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
3.	Retain mock-up during construction as a standard for comparison with completed work. 
4.	Do not alter or remove mock-up until work is completed or removal is authorized.
1.7	PRE-INSTALLATION CONFERENCE
A.	Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
1.8	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.9	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.10	SEQUENCING
A.	Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
1.11	WARRANTY
A.	Manufacturer's Warranty: Provide manufacturer's standard limited warranty.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Everlast Climbing a PlayCore Company, which is located at:<BR />5522 Lakeland Ave. N.<BR />Minneapolis, MN 55429<BR />Toll Free Tel: 800-476-7366<BR />Tel: 651-665-9131<BR />Fax: 651-665-9130<BR />Email: request info (info@everlastclimbing.com);Web: https://everlastclimbing.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	CLIMBING WALLS
A.	Magnetic Wall: Basis of Design: Magna Wall; as manufactured by Everlast Climbing.
1.	Description: Magnetic surface.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 20 per panel.
f.	T-Nuts: 66 per panel for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Wall Height: 10 feet (3048 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) and 4 x 2 foot (1219 x 610 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, Green, and Blue.
2)	Quantity: 25 per section.
f.	T-Nuts: 82 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per section.
4.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Climbing the Walls Activity Guide, 250 pages.
e.	Magnets: Number, letter, and sentence-building magnets.
5.	Finish: Multi-colored texture paint.
B.	Textured Wall: Basis of Design: Standard Wall; as manufactured by Everlast Climbing.
1.	Description: Textured paint surface.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 20 per panel.
f.	T-Nuts: 66 per panel for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Wall Height: 10 feet (3048 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) and 4 x 2 foot (1219 x 610 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, Green, and Blue.
2)	Quantity: 25 per section.
f.	T-Nuts: 82 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per section.
4.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Climbing the Walls Activity Guide, 250 pages.
5.	Finish: Multi-color textured paint.
C.	Slate Look Wall: Basis of Design: River Rock Wall - Slate; as manufactured by Everlast Climbing.
1.	Description: Smooth surface.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 20 per panel.
f.	T-Nuts: 66 per panel for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Wall Height: 10 feet (3048 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) and 4 x 2 foot (1219 x 610 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, Green, and Blue.
2)	Quantity: 25 per section.
f.	T-Nuts: 82 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per section.
4.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Climbing the Walls Activity Guide, 250 pages.
5.	Finish: Slate.
D.	Granite Look Panels: Basis of Design: River Rock Wall - Granite; as manufactured by Everlast Climbing.
1.	Description: Smooth surface.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 20 per panel.
f.	T-Nuts: 66 per panel for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Wall Height: 10 feet (3048 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) and 4 x 2 foot (1219 x 610 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, Green, and Blue.
2)	Quantity: 25 per section.
f.	T-Nuts: 82 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per section.
4.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Climbing the Walls Activity Guide, 250 pages.
5.	Finish: Granite.
E.	Dry Erase Wall: Basis of Design: Discovery Dry-Erase Wall; as manufactured by Everlast Climbing.
1.	Description: White, dry-erase, magnetic surface.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 20 per panel.
f.	T-Nuts: 66 per panel for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Wall Height: 10 feet (3048 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) and 4 x 2 foot (1219 x 610 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, Green, and Blue.
2)	Quantity: 25 per section.
f.	T-Nuts: 82 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per section.
4.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Climbing the Walls Activity Guide, 250 pages.
e.	Magnets: Number, letter, and sentence-building magnets.
f.	Dry-erase markers.
F.	Adaptive Wall: Basis of Design: Adaptive Wall; as manufactured by Everlast Climbing.
1.	Description: White, dry-erase, magnet-accepting surface with adaptive hand and foot holds.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 20 per panel.
f.	Adaptive Holds: 4 hand holds and 2 ledge foot holds per panel.
g.	T-Nuts: 66 per panel for mounting hand holds.
h.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Activity Wall Activity guide.
e.	Magnets: Number, letter, and sentence-building magnets.
f.	Dry-erase markers.
G.	Birch Panels: Basis of Design: Baltic Birch Wall; as manufactured by Everlast Climbing.
1.	Description: Birch surface.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 20 per panel.
f.	T-Nuts: 66 per panel for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Wall Height: 10 feet (3048 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) and 4 x 2 foot (1219 x 610 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, Green, and Blue.
2)	Quantity: 25 per section.
f.	T-Nuts: 82 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per section.
4.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Climbing the Walls Activity Guide, 250 pages.
5.	Finish: Clear coated Birch.
H.	Color Wall: Basis of Design: Chroma Wall; as manufactured by Everlast Climbing.
1.	Description: Smooth, durable surface.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 20 per panel.
f.	T-Nuts: 66 per panel for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Wall Height: 10 feet (3048 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) and 4 x 2 foot (1219 x 610 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, Green, and Blue.
2)	Quantity: 25 per section.
f.	T-Nuts: 82 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per section.
4.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Climbing the Walls Activity Guide, 250 pages.
5.	Color: Blue.
6.	Color: Red.
7.	Color: Green.
I.	Relief Wall: Basis of Design: Relief-Feature Wall; as manufactured by Everlast Climbing.
1.	Description: Textured paint surface with rock-like relief features.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 20 per panel.
f.	T-Nuts: 66 per panel for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Wall Height: 10 feet (3048 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) and 4 x 2 foot (1219 x 610 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, Green, and Blue.
2)	Quantity: 25 per section.
f.	T-Nuts: 82 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per section.
4.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Climbing the Walls Activity Guide, 250 pages.
5.	Finish: Multi-color textured paint.
J.	Magnetic Relief Wall: Basis of Design: Magna Relief-Feature Wall; as manufactured by Everlast Climbing.
1.	Description: Magnet-accepting surface with rock-like relief features.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 20 per panel.
f.	T-Nuts: 66 per panel for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Wall Height: 10 feet (3048 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) and 4 x 2 foot (1219 x 610 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, Green, and Blue.
2)	Quantity: 25 per section.
f.	T-Nuts: 82 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per section.
4.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Climbing the Walls Activity Guide, 250 pages.
e.	Magnets: Number, letter, and sentence-building magnets.
5.	Finish: Multi-color textured paint.
K.	Sandstone Look Relief Wall: Basis of Design: Sandstone Relief-Feature Wall; as manufactured by Everlast Climbing.
1.	Description: Textured paint surface with Sandstone relief features.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Sandstone Style Hand Holds.
1)	Colors: Red, Orange, and Grey.
2)	Quantity: 20 per panel.
f.	T-Nuts: 66 per panel for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Wall Height: 10 feet (3048 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) and 4 x 2 foot (1219 x 610 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Sandstone Style Hand Holds.
1)	Colors: Red, Orange, and Grey.
2)	Quantity: 25 per section.
f.	T-Nuts: 82 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per section.
4.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Climbing the Walls Activity Guide, 250 pages.
5.	Color: Sandstone.
L.	Rock Wall: Basis of Design: Superior Rock Wall; as manufactured by Everlast Climbing.
1.	Description: Molded from rock for realistic look and feel.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 4 foot (1219 x 1219 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 20 per section.
f.	T-Nuts: 50 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Wall Height: 10 feet (3048 mm).
a.	Panels: 4 x 4 foot (1219 x 1219 mm) and 4 x 2 foot (1219 x 610 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 25 per section.
f.	T-Nuts: 70 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per section.
4.	Additional Components:
a.	Safety, care, and maintenance manual.
b.	Rules and guidelines sign.
c.	Climbing the Walls Activity Guide, 250 pages.
5.	Color: Dark gray.
M.	Blackboard Wall: Basis of Design: Discovery Blackboard Wall; as manufactured by Everlast Climbing.
1.	Description: Black, magnetic, chalkboard surface.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 20 per section.
f.	T-Nuts: 66 per section for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Climbing the Walls Activity Guide, 250 pages.
e.	Magnets: Number, letter, and sentence-building magnets.
f.	Chalk.
N.	Mural Wall: Basis of Design: Mural Wall; as manufactured by Everlast Climbing.
1.	Description: Illustrated mural wall.
2.	Wall Height: 8 feet (2438 mm).
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Length: 20 feet (6096 mm).
c.	Length: 40 feet (12192 mm).
d.	Length: _____.
e.	Hand Holds: Groperz Hand Holds.
1)	Colors: Coordinating with mural.
2)	Quantity: 20 per panel.
f.	T-Nuts: 20 per panel for mounting hand holds.
g.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Additional Components:
a.	Safety, care, and maintenance manual.
b.	Rules and guidelines sign.
c.	Climbing the Walls Activity Guide, 250 pages.
4.	Image: Mountain Scene.
5.	Image: Forest Scene.
6.	Image: Jungle Scene.
7.	Image: Outer Space Scene.
8.	Image: Ocean Scene.
9.	Image: Custom, to be provided by Architect.
10.	Image: Custom, as indicated on Drawings.
O.	Angled Panels: Basis of Design: Climb-Able Wall; as manufactured by Everlast Climbing.
1.	Description: Birch surface angled outward for easier climbing.
2.	Panel Size: 4 x 7.5 feet (1219 x 2286 mm).
3.	Hand Holds: WeeKidz Hand Holds.
a.	Colors: Red and Yellow.
b.	Quantity: 20 per panel.
4.	Cordless Mat Locking System and Safety Mat: 1 per panel.
5.	Additional Components:
a.	Safety, care, and maintenance manual.
b.	Rules and guidelines sign.
c.	Activity guide.
6.	Finish: Clear finish.
P.	Freestanding Wall: Basis of Design: 360 Magna Freestanding Wall; as manufactured by Everlast Climbing.
1.	Description: Freestanding, 4 sided wall with magnetic surface.
2.	Wall Size: 8 x 32 feet (2438 x 9754 mm) - 8 feet (2438 mm) per side.
a.	Panels: 4 x 8 foot (1219 x 2438 mm) panels.
b.	Hand Holds: Groperz Route-Setting Hand Holds.
1)	Colors: Red, Yellow, and Green.
2)	Quantity: 160.
c.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Activity guide.
4.	Color: Magna blue.
Q.	Overhang Wall: Basis of Design: Overhang; as manufactured by Everlast Climbing.
1.	Description: Baltic birch panels at 14 degrees from vertical.
2.	Panel Size: 4 x 7.5 feet (1219 x 2286 mm).
3.	Finish: Clear.
R.	Playground Wall: Basis of Design: Playground Wall; as manufactured by Everlast Climbing.
1.	Description: IPEMA certified waterproof outdoor climbing wall.
2.	Wall Size: 6 x 12 feet (1829 x 3658 mm).
a.	Panels: 4 x 6 foot (1219 x 1829 mm) panels.
b.	Hand Holds: UV Hand Holds.
1)	Colors: Red and Yellow.
2)	Quantity: 120.
c.	Steel Posts: 4.
d.	Required safety surfacing, not included.
3.	Color: Clear.
4.	Color: Gray.
S.	Top Rope Wall: Basis of Design: Top Rope Walls; as manufactured by Everlast Climbing.
1.	Construction: Panels are constructed of fire-treated plywood.
2.	Panel Type: Magna.
3.	Panel Type: Sculpted Magna.
4.	Panel Type: As indicated on Drawings.
5.	Panel Type: _____.
6.	Wall Size: As indicated on Drawings.
7.	Wall Size: _____.
8.	Hand Holds: Groperz Route-Setting Hand Holds.
a.	Colors: Red, Yellow, and Green.
b.	Colors: _____.
c.	Quantity: 20 per panel.
d.	Quantity: _____.
9.	T-Nuts: 66 per panel for mounting hand holds.
10.	T-Nuts: _____ per panel for mounting hand holds.
11.	Cordless Mat Locking System and Safety Mat: 1 premium 3 inch (76 mm) mats per 4 foot (1219 mm) horizontal section.
12.	Designed and installed to CWA standards.
13.	Additional Components:
a.	Relief Line: Red-Relief Line: A safety feature that reminds climbers to stay within a distance of three feet from the floor and acts as helpful tool for climbing wall supervisor when using as a Traverse Wall.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Activity guide.
e.	Outlet frames.
14.	Equipment Package:
a.	Fully Adjustable Harnesses: 3 per station.
b.	Semiautomatic Belay Devices: 1 per station.
c.	Locking Carabiners: 4 per station.
d.	Helmets: 2 per station.
e.	Dynamic Top Ropes: 1 per station.
f.	One-day top rope site management training.
T.	Pool Climbing Wall: Basis of Design: Kersplash Pool Climbing Wall; as manufactured by Everlast Climbing.
1.	Description: Waterproof panels on stainless steel structure.
2.	Structure Finish: Spectra Shield coating.
3.	Wall Width: 4 feet (1219 mm).
4.	Wall Width: 8 feet (2438 mm).
5.	Wall Width: 12 feet (3658 mm).
6.	Wall Width: 16 feet (4877 mm).
7.	Wall Height: 8 feet (2438 mm).
8.	Wall Height: 12 feet (3658 mm).
9.	Wall Height: 16 feet (4877 mm).
10.	Hand Holds: Groperz Hand Holds - Orange, Yellow, and Red.
11.	Additional Components:
a.	Top Guard Safety Panel.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
12.	Color: Clear.
13.	Color: Blue and Green.
U.	Beginner Climbing Wall: Basis of Design: Beginner WeeKidz Traverse Wall; as manufactured by Everlast Climbing.
1.	Wall Height: 6'-10" feet (2083 mm).
a.	Length: 20 feet (6096 mm).
b.	Length: _____.
c.	Panels: 4 foot x 6'-10" (1219 x 2083 mm) panels.
d.	Hand Holds:
1)	12 WeeKidz Hand Holds - Red and Yellow, per panel.
2)	5 Grab-bar style hand holds - Blue and Yellow, per panel.
3)	3 Ledge style foot holds - Blue, per panel.
e.	Cordless Mat Locking System and Safety Mat: 1 per panel.
2.	Additional Components:
a.	Safety, care, and maintenance manual.
b.	Rules and guidelines sign.
c.	Activity guide.
V.	Kids Climbing Wall: Basis of Design: WeeKidz Traverse Wall; as manufactured by Everlast Climbing.
1.	Description: Magna surface.
2.	Wall Height: 6'-10" feet (2083 mm).
a.	Length: 20 feet (6096 mm).
b.	Length: _____.
c.	Panels: 4 foot x 6'-10" (1219 x 2083 mm) panels.
d.	Hand Holds:
1)	100 WeeKidz Hand Holds - Red and Yellow.
2)	10 Groperz Critterz Hand Holds.
e.	Cordless Mat Locking System and Safety Mat: 1 per panel.
3.	Additional Components:
a.	Foam letter and number magnets.
b.	Safety, care, and maintenance manual.
c.	Rules and guidelines sign.
d.	Activity guide.
2.3	HAND HOLDS
A.	Challenge Course Hand Holds: Basis of Design: Ultimate Challenge Course; as manufactured by Everlast Climbing.
1.	Hook Holds: Holds designed for a ring to hook over.
a.	Hook Hold Quantity: 6.
b.	Hook Hold Quantity: _____.
c.	Ring Quantity: 2.
d.	Ring Quantity: _____.
e.	Color: Yellow.
2.	Loop Holds: Loop with a stationary ring attached.
a.	Loop Quantity: 6.
b.	Loop Quantity: _____.
c.	Ring Quantity: 6.
d.	Ring Quantity: _____.
e.	Color: Blue.
3.	Peg Holds: Holds designed for a peg to be inserted.
a.	Peg Hold Quantity: 12.
b.	Peg Hold Quantity: _____.
c.	Peg Quantity: 2.
d.	Peg Quantity: _____.
e.	Color: Red.
B.	Challenge Course Hand Holds: Basis of Design: Versa Challenge Course; as manufactured by Everlast Climbing.
1.	Hoop Holds: Specialized holds with clips for plastic hoops that can be positioned in any direction and angle.
a.	Quantity: 5.
b.	Quantity: 10.
c.	Quantity: _____.
2.	Hoops: Plastic hoops designed to clip to hoop holds.
a.	Quantity: 5.
b.	Quantity: 10.
c.	Quantity: _____.
3.	Includes hardware and activity guide.
C.	Beginner Hand Holds: Basis of Design: Beginner Route Setting Hand Holds; as manufactured by Everlast Climbing.
1.	Description: Large, easy to grab designs.
2.	Set A: Set of 10 hand holds.
3.	Set B: Set of 10 hand holds.
4.	Set C: Set of 10 hand holds.
5.	Set D: Set of 10 hand holds.
6.	Color: Green.
7.	Includes mounting hardware and Allen wrench.
D.	Intermediate Hand Holds: Basis of Design: Intermediate Route Setting Hand Holds; as manufactured by Everlast Climbing.
1.	Description: Variety of medium size designs.
2.	Set E: Set of 10 hand holds.
3.	Set F: Set of 10 hand holds.
4.	Set G: Set of 10 hand holds.
5.	Set H: Set of 10 hand holds.
6.	Color: Yellow.
7.	Includes mounting hardware and Allen wrench.
E.	Advanced Hand Holds: Basis of Design: Advanced Route Setting Hand Holds; as manufactured by Everlast Climbing.
1.	Description: Small to medium sizes and technical designs.
2.	Set I: Set of 10 hand holds.
3.	Set J: Set of 10 hand holds.
4.	Set K: Set of 10 hand holds.
5.	Set L: Set of 10 hand holds.
6.	Color: Red.
7.	Includes mounting hardware and Allen wrench.
F.	Rock Realistic Hand Holds: Basis of Design: Groperz Rock Realistic Hand Holds; as manufactured by Everlast Climbing.
1.	Description: Hand holds that look and feel like real rock.
2.	Level: Beginner to intermediate.
3.	Set X: Set of 10 hand holds.
4.	Set Y: Set of 10 hand holds.
5.	Set Z: Set of 10 hand holds.
6.	Color: Brown.
7.	Includes mounting hardware and Allen wrench.
G.	Alphabet Hand Holds: Basis of Design: Alphabet Hand Holds; as manufactured by Everlast Climbing.
1.	Description: Hand holds in the shape of letters A to Z.
2.	Attachment: Bolt on.
3.	Attachment: Screw on.
4.	Set of 26 hand holds.
5.	Color: Blue.
H.	Ball Holder Hand Holds: Basis of Design: Ball Holder Hand Hold; as manufactured by Everlast Climbing.
1.	Description: Designed to hold a ball during climbing wall activities and can be used as hand hold.
2.	Quantity: Single hand hold.
3.	Quantity: _____.
4.	Quantity: Set of 10 hand holds.
5.	Color: Blue.
I.	Animal Shaped Hand Holds: Basis of Design: Critterz Hand Holds; as manufactured by Everlast Climbing.
1.	Description: Hand holds in animal shapes.
2.	Quantity: Set of 13 hand holds.
3.	Color: Yellow.
J.	Character Hand Holds: Basis of Design: Groperz Character Holds; as manufactured by Everlast Climbing.
1.	Description: Each set spells out four character concepts in individual letters.
2.	Set 1: Caring - Responsibility - Honesty - Respect.
3.	Set 2: Courage - Diligence - Trust - Kindness.
4.	Colors: Red, Green, Blue, and Yellow.
5.	Includes mounting hardware
2.4	MAT LOCKING SYSTEM AND SAFETY MATS
A.	Cordless Mat Locking System: Hook and loop fastening system with security slider and lock.
1.	Two nylon-webbing loops attached to each mat.
2.	Security latch system attaches to wall.
3.	Two highly durable thermal plastic coated tabs attach to each mat and connect to base of the wall.
4.	Hook and loop fastening system with security slider and lock.
a.	Two nylon-webbing loops attached to each mat.
b.	Security latch system attaches to wall.
c.	Two highly durable thermal plastic-coated tabs attach to each mat and connect to base of the wall.
5.	Side Locks: Hook and loop flaps secure mats side-by-side. Locks each end of system to prevent climbing in between the mats and the closed climbing wall.
B.	Standard Mats: Basis of Design: Standard Mats; as manufactured by Everlast Climbing.
1.	Description: Polyethylene foam enclosed in an 18-ounce (0.51 kg) polyester-reinforced vinyl cover.
2.	Hook and loop fastening system with security slider and lock.
a.	Two nylon-webbing loops attached to each mat.
b.	Security latch system attaches to wall.
c.	Two highly durable thermal plastic-coated tabs attach to each mat and connect to base of the wall.
3.	Side Locks: Hook and loop flaps secure mats side-by-side. Locks each end of system to prevent climbing in between the mats and the closed climbing wall.
4.	Compliant with ASTM F2440 and ASTM F1292.
5.	Color: Red.
6.	Color: Royal Blue.
7.	Color: Custom color, to be selected by Architect.
8.	Color: _____.
9.	Thickness: 2 inches (51 mm).
10.	Thickness: 3 inches (76 mm).
C.	Fire Resistant Mats: Basis of Design: FR Mats; as manufactured by Everlast Climbing.
1.	Description: Polyethylene foam enclosed in an 18-ounce (0.51 kg) polyester-reinforced vinyl cover.
2.	Compliant with ASTM F2440 and ASTM F1292.
3.	Fire Resistance, ASTM E84: Class C.
4.	Hook and loop fastening system with security slider and lock.
a.	Two nylon-webbing loops attached to each mat.
b.	Security latch system attaches to wall.
c.	Two highly durable thermal plastic-coated tabs attach to each mat and connect to base of the wall.
5.	Side Locks: Hook and loop flaps secure mats side-by-side. Locks each end of system to prevent climbing in between the mats and the closed climbing wall.
6.	Color: Red.
7.	Color: Royal Blue.
8.	Color: Custom color, to be selected by Architect.
9.	Color: _____.
10.	Thickness: 2 inches (51 mm).
11.	Thickness: 3 inches (76 mm).
D.	Fire Retardant Mats: Basis of Design: Ultra FR Mats; as manufactured by Everlast Climbing.
1.	Description: Fire retardant foam enclosed in an 18-ounce (0.51 kg) polyester-reinforced vinyl cover.
2.	Compliant with ASTM F2440 and ASTM F1292.
3.	Fire Resistance: Compliant with NFPA 286.
4.	Hook and loop fastening system with security slider and lock.
a.	Two nylon-webbing loops attached to each mat.
b.	Security latch system attaches to wall.
c.	Two highly durable thermal plastic-coated tabs attach to each mat and connect to base of the wall.
5.	Side Locks: Hook and loop flaps secure mats side-by-side. Locks each end of system to prevent climbing in between the mats and the closed climbing wall.
6.	Color: Red.
7.	Color: Royal Blue.
8.	Color: Custom color, to be selected by Architect.
9.	Color: _____.
10.	Thickness: 2 inches (51 mm).
11.	Thickness: 3 inches (76 mm).
2.5	CLIMBING WALL ACCESSORIES
A.	Climbing Wall Challenge Course: Made of specially-designed hand holds and noodles to create an obstacle course on the climbing wall.
B.	Discovery Plates: Set of ten magnetic, dry-erase plates.
C.	Magna Flags: Red, yellow, and green activity flags that magnetically attach to bolt holes in hand holds.
D.	Outlet Frames: Surrounds outlets to make them aesthetic and functional parts of the climbing wall.
2.6	PHYSICAL EDUCATION EQUIPMENT
A.	Indoor Jungle Gym: Basis of Design: Safari Jungle Gym; as manufactured by Everlast Climbing.
1.	Safari Circle Steppers: Five hanging discs create a balance challenge.
2.	Safari Monkey Bars: Indoor monkey bars that stow up and out of the way when not in use.
3.	Safari Plank Walk: A low ropes course element with hanging plank and adjacent hanging ropes for balance and travel.
4.	Safari Swing Steppers: Five swinging steps.
5.	Safari Wild Web: Indoor cargo net climbing element.
6.	Mat-Locking System provides a cushioned landing surface for participants and helps to close and prevent access when the Safari Jungle Gym is not being used and supervised.
7.	Must be installed on concrete masonry wall.
B.	Ninja Course: Basis of Design: Hijinx Ninja Course; as manufactured by Everlast Climbing.
1.	Grades K-2 Hijinx Ninja Course:
a.	This beginner-level package helps develop balance, coordination and gross motor skills.
b.	Package includes 4 Slant Steps, 1 small Octagon, 1 medium Octagon, 3 Posts, 3 Balance Beams, 1 Crawl Tunnel, 6 Straight Poly Arrows, 6 Curved Poly Arrows and 10 Agility Rings.
2.	Grades 3-5 Hijinx Ninja Course:
a.	This package brings some additional challenge and excitement ideal for upper-elementary age children. 
b.	Package includes 4 Slant Steps, 1 medium Octagon, 3 Posts, 3 Balance Beams, 2 Trapezoids, 6 Straight Poly Arrows, 6 Curved Poly Arrows, 10 Agility Rings and 10 Step Hurdles.
3.	Grades 6-8 Hijinx Ninja Course:
a.	This package keeps middle schoolers engaged, challenged, and having fun. 
b.	Package includes 6 Slant Steps, 1 large Octagon, 1 Agility Ladder, 2 Posts, 1 River Log, 1 Trapezoid and 6 Step Hurdles.
4.	Grades 9-12 Hijinx Ninja Course:
a.	The most challenging course designed for high school students. 
b.	Package includes 4 Slant Steps, 3 Plyo Box Steppers, 1 Pro Agility Pole Set, 4 Plyo Hurdles, 1 River Log, 1 Trapezoid and 4 BOSU Balance Trainers.
5.	Flooring: Carpet-bonded foam.
C.	Safari Ninja Course: Basis of Design: Safari Ninja Circuit; as manufactured by Everlast Climbing.
1.	Small Safari Ninja Circuit:
a.	The Small Ninja Circuit Package is a great starter package. 
b.	The Small Ninja Circuit Package includes two Single Rings, one Triple Ring, one Double Ring and a 7 foot (2134 mm) Knotted Rope with Disc.
2.	Medium Safari Ninja Circuit:
a.	This package offers an exciting mix of objects to challenge kids of all ages.
b.	Includes two Single Rings, one Triple Ring, two 18 inch (457 mm) Knotted Ropes and one Ladder.
3.	Large Safari Ninja Circuit:
a.	The Large Ninja Circuit Package includes different objects that offer an exciting challenge.
b.	Includes four Single Rings, one Triple Ring, four 18 inch (457 mm) Knotted Ropes and one 7 foot (2134 mm) Knotted Rope with Disc.
2.7	PREMIUM CLIMBING WALL SYSTEMS
A.	Design and Performance Requirements:
1.	Compliant with CWA standards.
2.	Climbing wall shall be designed to suit the facility and meet the needs of the client as follows:
a.	Percentage of Less-than-Vertical to Vertical Surfaces: _____.
b.	Percentage of Minimally Overhung Surfaces: _____.
c.	Percentage of Moderately to Substantially Overhung Surfaces: _____.
B.	Description: Panelized, wood-based interior climbing wall system with texture and internal bolt-together truss assembly.
1.	Panels shall be compatible with modular, internal bolt-together truss assembly and shall allow for replacement of the climbing surface.
2.	All fasteners shall be behind the wall and not visible on climbing surface.
3.	Panel system must be able to contain multiple configurations such as overhangs, slabs, roofs and straight vertical sections.
4.	Steel support system shall be bolt-together, no on-site welding will be allowed.
C.	Panels: Basis of Design: Kumiki Bouldering Walls; as manufactured by Kumiki Climbing.
1.	Substrate: Baltic birch plywood panels.
2.	Veneer Species: Maple.
3.	Veneer Species: Walnut.
4.	Veneer Species: ______.
5.	Finish: Durable clear finish.
6.	Frame: Structural steel with Kumiki Climbing panel connectors.
7.	Height: As indicated on Drawings.
8.	Height: _____.
9.	Configuration: As indicated on Drawings.
10.	Finish: Clear.
D.	Climbing Wall Returns: Return to the facility walls and conceal the interior structure of the climbing wall and restrict access behind the climbing wall.
E.	Equipment:
1.	Lead Routes: 
a.	First anchor installed 10 feet (3048 mm) above ground level
b.	Subsequent anchors spaced approximately every 4 feet (1219 mm) vertically.
2.	Climbing Rope: Dynamic ropes, 1 per climbing route.
3.	Climbing Harnesses: 2 per climbing route.
4.	Belay Devices: Auto locking or manual tube belay device chosen during the pre-design discussions.
5.	Quick Draws: Fixe or equivalent, foreach lead anchor.
6.	Auto-Belay System: Trublue.
7.	Auto-locking carabiners.
F.	Flooring, Carpet Bonded: Basis of Design: Carpet-Bonded Foam Flooring; as manufactured by Kumiki Climbing.
1.	Description: Carpet-bonded foam with integral hook and loop connection.
2.	Layers:
a.	Bottom Layer: 2 inches (51 mm) closed-cell foam.
b.	Mid Layer: 8 inches (203 mm) open-cell foam.
c.	Top Layer: 1-3/8 inches (35 mm) carpet-bonded foam.
3.	Seams: Edges glued together for a uniform fall zone.
4.	Color: As selected by Architect from Manufacturer's full range.
5.	Color: As indicated on Drawings.
6.	Color: _____.
7.	Vapor Barrier: Manufacturer's standard.
8.	Vapor Barrier: As indicated on Drawings.
9.	Vapor Barrier: _____.
10.	Built-In Seating: As indicated on Drawings.
11.	Built-In Seating: ______.
12.	Edging: Hard curb.
13.	Edging: Soft curb.
14.	Edging: Ramp.
15.	Edging: Squared-off sides.
16.	Edging: ______.
G.	Flooring, Cordura: Basis of Design: Cordura Flooring; as manufactured by Kumiki Climbing.
1.	Description: Multi-layer foam with Cordura finish surface.
2.	Foam Layers:
a.	Bottom Layer: 2 inches (51 mm) closed-cell foam.
b.	Mid Layer: 6 inches (152 mm) open-cell foam.
c.	Top Layer: 6 inches (152 mm) open-cell foam.
3.	Seams: Edges glued together for a uniform fall zone.
4.	Color: As selected by Architect from Manufacturer's full range.
5.	Color: As indicated on Drawings.
6.	Color: _____.
7.	Vapor Barrier: Manufacturer's standard.
8.	Vapor Barrier: As indicated on Drawings.
9.	Vapor Barrier: _____.
10.	Built-In Seating: As indicated on Drawings.
11.	Built-In Seating: ______.
12.	Edging: Hard curb.
13.	Edging: Soft curb.
14.	Edging: Ramp.
15.	Edging: Squared-off sides.
16.	Edging: ______.
H.	Flooring, Vinyl Basis of Design: Vinyl Flooring; as manufactured by Kumiki Climbing.
1.	Description: Multi-layer foam with vinyl finish surface.
2.	Foam Layers:
a.	Bottom Layer: 2 inches (51 mm) closed-cell foam.
b.	Mid Layer: 6 inches (152 mm) open-cell foam.
c.	Top Layer: 6 inches (152 mm) open-cell foam.
3.	Seams: Edges glued together for a uniform fall zone.
4.	Color: As selected by Architect from Manufacturer's full range.
5.	Color: As indicated on Drawings.
6.	Color: _____.
7.	Vapor Barrier: Manufacturer's standard.
8.	Vapor Barrier: As indicated on Drawings.
9.	Vapor Barrier: _____.
10.	Built-In Seating: As indicated on Drawings.
11.	Built-In Seating: ______.
12.	Edging: Hard curb.
13.	Edging: Soft curb.
14.	Edging: Ramp.
15.	Edging: Squared-off sides.
16.	Edging: ______.
I.	Holds: Basis of Design: Kumiki Holds; as manufactured by Kumiki Climbing.
1.	Hold Set: Pies Small.
2.	Hold Set: Pies Medium.
3.	Hold Set: Pies Large.
4.	Hold Set: Flow Ledges.
5.	Hold Set: Flow Pinches.
6.	Hold Set: Flow Shadowless Screw Ons, Small Set.
7.	Hold Set: Flow Butter Flys Screw Ons.
8.	Hold Set: Flow Youth D Pinches.
9.	Hold Set: Flow Frequent Flyer Screw Ons.
10.	Hold Set: Flow Shadowless Screw Ons, Large Set.
11.	Hold Set: Puzzles, SM.
12.	Hold Set: Puzzles, MD.
13.	Hold Set: Puzzles, LG.
14.	Hold Set: Puzzles, XL.
J.	Handhold T-Nut Density: 4 handhold fasteners per every square foot of climbing wall surface area.
K.	Volumes: Basis of Design: Kumiki Volumes; as manufactured by Kumiki Climbing.
1.	Volume: Bowtie Small.
2.	Volume: Bowtie Medium.
3.	Volume: Bowtie Large.
4.	Volume: Diamond Small.
5.	Volume: Diamond Medium.
6.	Volume: Diamond Large.
7.	Volume: Lightning Bolt Small.
8.	Volume: Lightning Bolt Medium.
9.	Volume: Lightning Bolt Large.
10.	Volume: Stacked Triangle Small.
11.	Volume: Stacked Triangle Medium.
12.	Volume: Stacked Triangle Large.
13.	Volume: Stacked Triangle Set.
14.	Volume: Equal Triangle Medium.
15.	Volume: Equal Triangle Large.
16.	Volume: Rail Triangle Pointed.
17.	Volume: Rail Triangle.
18.	Volume: Tilted Triangle Pointed.
19.	Volume: Tilted Triangle Rail.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, approved submittals and in proper relationship with adjacent construction.
B.	Completed wall shall comply with specified tolerances.
3.4	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.
B.	Manufacturer's Services: Coordinate manufacturer's services in accordance with appropriate sections in Division 01.
3.5	TRAINING
A.	Provide full day training session for the facility operations staff, following the climbing wall installation. Training shall cover the following topics:
1.	Climbing wall maintenance and periodic inspections.
2.	Route-setting methods and management.
3.	Sample handhold installation and removal.
3.6	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturers recommendations. 
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION