SECTION 13 24 16

SAUNAS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2011 -  2015 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Precut sauna packages and wall and ceiling framing and insulation.
B.	Prefabricated modular saunas for interior installation.
C.	Prefabricated modular saunas for exterior application, with roof package.
D.	Sauna doors.
E.	Sauna heaters and accessories.
1.2	RELATED SECTIONS
A.	Section 03 30 00 - Cast-in-Place Concrete.
B.	Section 06 10 00 - Rough Carpentry.
C.	Section 07 21 26 - Blown Insulation.
D.	Section 09 30 00 - Tiling.
E.	Section 09 65 13 - Resilient Base and Accessories.
F.	Section 22 13 26 - Sanitary Waste Separators.
G.	Section 26 05 00 - Common Work Results for Electrical.
1.3	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	[ Product Data ]: Manufacturer's descriptive literature for saunas and components specified in this section.
C.	Shop Drawings: Plan and elevations of sauna design, indicating construction details. Include electrical rough-in and wiring requirements for heater/control, including pre-installation and final hookup.
D.	Samples: Two samples, minimum size 4 inch (102 mm) wide x 8 inch (203 mm) long, of specified materials for wood paneling.
E.	Installation Instructions: Manufacturer's printed installation instructions for sauna, benches, and accessories.
F.	Operation and Maintenance Data: Sauna enclosure, heater, and control/monitoring equipment.
G.	Warranty Documents: Issued and executed by manufacturer.
1.4	DELIVERY, STORAGE, AND HANDLING
A.	Store products of this section in manufacturer's unopened packaging until installation.
B.	Maintain dry, heated storage area for products of this section until installation of products.
1.5	WARRANTY
A.	Provide manufacturer's standard one year warranty on heaters, controls, room materials and workmanship when installed according to manufacturer's specifications and wiring information.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Finlandia Sauna Products, Inc., which is located at:<BR />14010-B  S.W. 72nd Ave.<BR />Portland, OR 97224-0088<BR />Toll Free Tel: 800-354-3342<BR />Tel: 503-684-8289<BR />Fax: 503-684-1120<BR />Email: request info (info@finlandiasauna.com);Web: https://www.finlandiasauna.com 
B.	Substitutions: Not permitted.
C.	Provide all saunas and accessories from a single manufacturer.
2.2	MATERIALS
A.	Sauna (FPC): Precut sauna material package and related framing and finishing as required to complete sauna installation and as indicated on Drawings. Wall paneling to be installed the horizontal direction to the stud frame.
1.	Size: __________________. 
2.	Size: As indicated on Drawings. To fit field dimensions inside of 2x4 or 2x6 wood framing or 1x2 wooden nailing strips.
3.	Wall and Ceiling Framing: Specified in Section 06 10 00 - Rough Carpentry.
4.	Wall and Ceiling Insulation: Specified in Section 07 21 26 - Blown Insulation.
5.	Interior Wall and Ceiling Finish: "A" export grade, clear, kiln-dried (8 percent - 11 percent moisture) 1x4, 11/16 inch (17.4 mm) thick material.
a.	Western Red Cedar (standard). 
b.	Western Hemlock (upgrade). 
c.	Alaskan Yellow Cedar (upgrade). 
d.	California Redwood (upgrade). 
6.	Assembled benches, clear, V.G., S4S, kiln-dried, 2x2, 1-1/2 inches x 1-1/2 inches (38 mm x 38 mm) tops with 3/8 inch (10 mm) spacing.
a.	Facing: 2x4, 1-1/2 inches x 3-1/2 inches (38 mm x 89 mm).
b.	Fastening: From bottom without exposed metal. 
7.	Pre-hung glass door 24 inches wide x 6 feet 8 inches high (610 mm x 2032 mm); interior casing provided to match sauna room wood species.
8.	Heater fence.
9.	Assembled headrest/backrest No. 079 for upper benches.
10.	Trim (1x1) for ceiling, corners, and base (1x2).
11.	Super Dek, sufficient quantity for walking area of sauna room.
12.	Finlandia heater.
13.	Peridotite stones.
14.	Control/contactor panel if required by heater.
15.	Wall-mounted, vapor-proof light, Progress P5511, satin finish cast aluminum, 100 watt bulb max.
16.	Two sets of vents for installation in upper and lower wall areas. R.O. 4 inches x 10 inches (102 mm by 252 mm).
a.	Metal vent set V10, register and grill. 
b.	Cedar vent set V5 (upgrade), register and grill. 
17.	Accessories including wooden thermometer No. 0301K, wooden bucket No. 102N with bucket liner, wooden dipper No. 106/40, and bathing sign.
18.	Type C building foil.
19.	Hot-dipped galvanized nails, 5d size (upon request only).
20.	Installation DVD.
B.	Sauna (FPF): Provide prefabricated modular sauna panels approx. 2 feet wide x 7 feet high (610 mm x 2134 mm) with concealed locking system for assembly, concealed electrical conduit, and finished exterior. Wall paneling runs vertical direction. Verify that size of space shall be larger than the exterior size of the prefabricated sauna and that job site ceiling height is at least 7 feet 3 inches (2210 mm) for proper assembly. Prefab saunas 8 feet x 8 feet size or larger require 7 feet 5 inches (2261 mm) ceiling height for proper assembly. 
1.	Size: _______________ .
2.	Size: 5-sided.
3.	Size: As indicated on Drawings.
4.	Wall and Ceiling Framing: 2x2 (38 x 38 mm) Oregon Douglas Fir.
5.	Wall and Ceiling Insulation: R-11 fiberglass batts.
6.	Wall and Ceiling Vapor Barrier: Type C building foil.
7.	Interior Wall and Ceiling Finish: "A" export grade, clear, kiln-dried (8 percent -11 percent moisture) 1x4, 11/16 inch (17.4 mm) thick material.
a.	Western Red Cedar (Standard). 
b.	Western Hemlock (upgrade). 
c.	Alaskan Yellow Cedar (upgrade). 
d.	California Redwood (upgrade). 
8.	Exterior Siding: 11/32 inch (8.7 mm) rough-sawn mahogany plywood.
9.	Exterior Paneling: 1/2 x 4 (12 x 102 mm) tongue-and-groove Western Red Cedar (upgrade).
10.	Assembled benches, clear, V.G., S4S, kiln-dried, 2x2, 1-1/2 inches x 1-1/2 inches (38 mm x 38 mm) tops with 3/8 inch (10 mm) spacing.
a.	Facing: 2x4, 1-1/2 inches x 3-1/2 inches (38 mm x 89 mm).
b.	Fastening: From bottom without exposed metal. 
11.	Pre-hung glass door 24 inches wide (610 mm); interior casing provided to match room wood species.
12.	Heater fence.
13.	Assembled headrest/backrest No. 079 for upper benches.
14.	Trim (1x1) for ceiling.
15.	Super Dek, sufficient quantity for walking area of sauna room.
16.	Finlandia heater.
17.	Peridotite stones.
18.	Control/contactor panel if required by heater.
19.	Wall-mounted, vapor-proof light, Progress P5511, satin finish cast aluminum, 100 watt bulb max.
20.	Vents: One lower vent slot cut neatly into 2x4 base. One upper vent for installation in precut space (usually front wall).
a.	Metal vent set V10, register and grill.
b.	Cedar vent set V5 (upgrade), register and grill. 
21.	Accessories including wooden thermometer No. 0301K, wooden bucket No. 102N with bucket liner, wooden dipper No. 106/40, and bathing sign.
22.	Outdoor Sauna: Includes roof package with cedar shingles, rafter sections, 1x4 pine nailers, facia, and metal flashings. Roof height is 8 feet 6 inches to 9 feet 8 inches (depending on room size) at peak after roof kit assembly.
23.	Assembly DVD.
C.	Flooring: "Super Dek" 12 inch x 12 inch x 1/2 inch (305 mm x 305 mm x 13 mm) flooring squares for walking areas over concrete, tile, or vinyl; removable, washable, sanitary, non-skid, synthetic injected molded plastic material.
1.	Color: Terra cotta.
2.	Color: Beige.
D.	Doors and Frames:
1.	Door Type: Prehung for FPC sauna room.
2.	Door Type: Prefabricated for FPF sauna room.
3.	Door Rails: Solid wood laminated on both faces with clear, vertical grain Douglas fir veneer.
4.	Jamb size: up to 5-1/4 inch (133 mm) wide, over 5-1/4 inch (133 mm) to 7-1/4 inch (184 mm) wide (oversize), Casing (1x2): to match room species, and Threshold (3/4 inch thick): Hemlock.
5.	Door Size: 24 inches inch wide x 6 feet 8 inches (610 x 2032 mm). Standard size.
6.	Door Size: 28 inches inch wide x 6 feet 8 inches (711 x 2032 mm).
7.	Door Size: 30 inches wide x 6 feet 8 inches (762 x 2032 mm).
8.	Door Size: 32 inches wide x 6 feet 8 inches (813 x 2032 mm).
9.	Door Size: 34 inches wide x 6 feet 8 inches (864 x 2032 mm).
10.	Door Size: 36 inches wide x 6 feet 8 inches (915 x 2032 mm).
11.	Door swing, as viewed from outside sauna, out swinging: Model FGD-L, hinged left side.
12.	Door swing, as viewed from outside sauna, out swinging: Model FGD-R, hinged right side.
13.	Glass: Hermetically-sealed double glass (insulated), tempered.
a.	Clear (standard).
b.	Etched with Negative Sauna image.
c.	Etched with Positive Sauna image.
d.	Etched with Negative Rustic Sauna image.
e.	Etched with Positive Rustic Sauna image. 
f.	Etched Obscure.
g.	Etched with Mt. Hood image.
h.	Etched with Multnomah Falls image.
i.	Etched with Sailboat image.
j.	Etched with Lighthouse image.
14.	Hinges: Three 4 inch x 4 inch (102 mm x 102 mm) butt hinges, chrome finish.
15.	Roller catch latch, chrome finish.
16.	Door Pulls: Two wood pulls each door.
E.	Sauna Heater: Finlandia FLB; wall mounted with built-in controls; for room size up to 425 cu ft (12 cu m); residential model only.
1.	Electrical Characteristics: 240 VAC single phase.
2.	Size: 16 inch (406 mm) wide, 11 inch (279 mm) deep, 24 inch (610 mm) high.
3.	Capacity: As recommended by manufacturer for room volume.
4.	Controls: Built-in, 60 minute timer, thermostat, 8-hour time delay.
5.	Front mounted controls.
6.	Side mounted controls (option).
7.	Construction: Three-wall pressed metal construction, stainless steel heating elements, 50 pounds (20 kg) stones, direct rock contact with heating elements, free air flow.
8.	Surfaces: Stainless steel interior and top, and baked enamel exterior.
9.	Surfaces: Stainless steel interior and top, and optional stainless steel exterior.
10.	UL tested and listed.
F.	Sauna Heater: Finlandia FIN; wall mounted with exterior wall mounted controls; for room size up to 425 cu ft (12 cu m).
1.	Electrical Characteristics: 240 VAC single phase.
2.	Electrical Characteristics: 208 VAC three phase.
3.	Size: 16 inches (406 mm) wide, 11 inches (279 mm) deep, 24 inches (610 mm) high.
4.	Capacity: As recommended by manufacturer for room volume.
5.	Controls:
a.	F-1T mechanical Wall Control with thermostat, 60-minute timer, light switch, and indicator light; for FIN heater up to 6kw, 240 VAC single phase power.
b.	F-2T mechanical Wall Control with thermostat, 60-minute timer, light switch, and indicator light; for heaters 8kw and greater or any FIN-3ph heater; proper contactor specified by manufacturer.
c.	F-2 mechanical control (commercial location only) with no 60-minute timer. Use with 24HTC timer clock for all day operation.
d.	Griffin CG-170-U1 (1ph) or CG-170-U3 (3ph) digital control with temperature, 60-minute timer, 12-hour delay timer, light switch, F/C readings; includes separate power unit..
6.	Construction: Three-wall pressed metal construction, stainless steel heating elements, large rock capacity, 50 pounds (20 kg) stones, direct rock contact with heating elements, free air flow.
7.	Surfaces: Stainless steel interior and top, and baked enamel exterior.
8.	Surfaces: Stainless steel interior and top, and optional stainless steel exterior.
9.	UL listed heater and ETL listed control.
G.	Sauna Heater: Club model; floor mounted with exterior wall mounted controls; for room size from 388 to 989 cu ft (10.9 to 28.0 cu m).
1.	Electrical Characteristics: 240 VAC single phase.
2.	Electrical Characteristics: 208 VAC three phase.
3.	Size: 19-7/8 inches (505 mm) wide, 17 inches (432 mm) deep, 27-1/2 inches (699 mm) high.
4.	Capacity: As recommended by manufacturer for room volume.
5.	Controls: 
a.	F-2T mechanical Wall Control with thermostat, 60-minute timer, light switch, and indicator light; for heaters 8kw and greater or any FIN-3ph heater; proper contactor specified by manufacturer.
b.	F-2 mechanical control (commercial location only) with no 60-minute timer. Use with 24HTC timer clock for all day operation.
c.	Griffin CG-170-U1 (1ph), CG-170-U3 (3ph), or CG-170-15-U3 (12.5kw & 15kw 3ph) digital control with temperature, 60-minute timer, 12-hour delay timer, light switch, F/C readings; includes separate power unit.
6.	Construction: Deluxe chrome, stainless steel interior and exterior; triple-wall pressed metal construction, stainless steel heating elements, 132 pounds (60 kg) stones, direct rock contact with heating elements, free air flow.
7.	ETL tested and listed.
H.	Sauna Heater: Finlandia Compact JM; wall mounted with built-in reversible controls and protective fence; for room volume from 42 to 138 cu ft (1.2 to 3.9 cu m), 21 pounds of stones; residential model only.
1.	Electrical Characteristics: 120 VAC, single phase.
2.	Electrical Characteristics: 240 VAC, single phase.
3.	Size: 9 inches (230 mm) wide, 12 inches (305 mm) deep, 25 inches (635 mm) high.
4.	Capacity: As recommended by manufacturer for room volume.
5.	Construction: Stainless steel interior and top, stainless steel exterior; three-wall pressed metal construction, stainless steel heating elements, 20 pounds (9 kg) stones, direct rock contact with heating elements, free air flow.
6.	UL tested and listed.
I.	Sauna Heater: Finlandia Topclass KV; wall mounted with built-in lighted control panel which is reversible; for room volume from 100 to 425 cu ft (2.8 to 12 cu m); residential model only.
1.	Electrical Characteristics: 240 VAC single phase.
2.	Size: 10 inches (254 mm) wide, 18 inches (457 mm) deep, 25 inches (635 mm) high.
3.	Capacity: As recommended by manufacturer for room volume.
4.	Controls: 60 minute timer and 8 hour time delay.
5.	Construction: Three-wall pressed metal construction, stainless steel heating elements, 50 pounds (20 kg) stones, direct rock contact with heating elements, free air flow.
6.	Surfaces: Stainless steel interior and top, stainless steel exterior.
7.	UL tested and listed.
2.3	ACCESSORIES
A.	Standard Accessories:
1.	102N; Wood bucket, 1 gallon (3.8 L) with plastic liner.
2.	106/40; Wood dipper, 16 inch (406 mm) long.
3.	079; Tapered headrest.
4.	0301K; Birch thermometer.
5.	PBS; Plexiglas bathing sign.
6.	P5511; Vapor-proof wall light.
7.	SD12; Interlocking Super Dek flooring, 12 inch (305 mm) square.
8.	DVD showing sauna room assembly.
B.	Optional Accessories:
1.	442F; Cedar towel hanger.
2.	5499; Chrome/glass thermometer/hygrometer, 7 inch (178 mm) diameter.
3.	5498; Chrome/glass thermometer/hygrometer, 5 inch (127 mm) diameter.
4.	5355; Chrome/glass thermometer, 4 inch (102 mm) diameter.
5.	4355; Chrome/glass hygrometer, 4 inch (102 mm) diameter.
6.	280K; Wood encased thermometer/hygrometer.
7.	210K; Sauna sand timer.
8.	490-128; Set of two brushes.
9.	101N; Wood bucket, 1.84 gallons (6.9 L).
10.	3465; Light copper bucket.
11.	3455; Light copper dipper.
12.	539; Stainless steel bucket with wood handle, 1 gallon (3.8 L)
13.	540; Stainless steel dipper with wood handle, 15-3/4 inches (400 mm).
14.	106/50; Wood dipper, 19 inch (483 mm) long.
15.	108N; Wood pail, 2 gallons (7.5 L).
16.	AR5, set of 5 aromas, 1.8 oz. ea. (Eucalyptus, Cherry, Citrus, Birch, and Fir).
17.	V5; Cedar vent set (register and grill) 
18.	SHADE; Curved and slatted birch light shade for P551 wall light.
19.	SAUNAHEART; Humidifier tube insert for FLB, FIN, KV, and CLUB heaters. 
20.	FLT; Finlandia cotton towel 36 inch x 63 inch (915 mm x 1600 mm).
21.	BENCH SKIRT; 5 slat wooden skirt to cover open space between upper and lower bench(es); made to fit sauna room.
22.	PERMANENT BACKREST; 3 slat backrest to attach to wall 10 inches (254 mm) above upper bench(es); made to fit sauna room.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Verify that utility services are of correct type and in correct locations.
B.	Verify that construction activities affecting work of this section are correct and complete.
C.	Examine conditions under which work of this section is to be performed.
1.	Submit written notification if such conditions are unacceptable.
2.	Transmit two copies of installer's report to Architect within 24 hours of receipt.
3.	Beginning work of this section before unacceptable conditions have been corrected is prohibited.
4.	Beginning construction activities of this section indicates installer's acceptance of conditions.
3.2	INSTALLATION
A.	Install saunas and accessories in accordance with shop drawings and manufacturer's printed installation instructions.
B.	Connection of heater, lighting, and control/monitoring equipment, to electrical service is specified in Section 26 05 00 - Common Work Results for Electrical.
3.3	CLEANING
A.	Clean soiled surfaces in accordance with manufacturer's instructions.
3.4	PROTECTION OF INSTALLED PRODUCTS
A.	Protect sauna and components from damage to finishes and operation until Substantial Completion.

END OF SECTION