SECTION 08 81 13

DECORATIVE GLASS GLAZING

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2019 -  2019 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Decorative Glass Types Including:
1.	Etched glass.
2.	Carved glass.
3.	Patterned glass.
4.	Fire molded kiln fired glass.
5.	Elements recycled glass.
6.	EcoLuxe recycled glass.
7.	Fire polished glass.
8.	Fused glass.
9.	Color coat back painted glass.
10.	Classic mirror glass.
11.	Antique mirror glass.
12.	Stained / leaded glass.
13.	Laminated glass.
1.2	RELATED SECTIONS
A.	Section  - .
B.	Section 08 11 13.13 - Standard Hollow Metal Doors and Frames.
C.	Section 08 41 13 - Aluminum-Framed Entrances and Storefronts.
D.	Section 08 44 16 - Glazed Bronze Curtain Walls.
E.	Section 08 50 00 - Windows.
F.	Section 08 83 00 - Mirrors.
G.	Section 10 11 39 - Visual Display Rails.
H.	Section 12 10 00 - Art.
I.	Section  - .
1.3	REFERENCES
A.	U.S. Consumer Product Safety Commission (CPSC):
1.	CPSC 16 CFR 1201 Safety Standard for Architectural Glazing Materials.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used and installation instructions.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Verification Samples: Two representative units of each type, pattern and color.
1.	Glass: Two 12 x 12 inch (305 by 305 mm) glass samples.
2.	Glass: Two _____ x _____ inch (_____ x _____ mm) glass samples.
D.	Shop Drawings: Include details of materials, construction and finish. Include relationship with adjacent construction.
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
D.	Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
1.	Intent of mock-up is to demonstrate quality of workmanship and visual appearance.
2.	If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
3.	Retain mock-up during construction as a standard for comparison with completed work.
4.	Do not alter or remove mock-up until work is completed or removal is authorized.
1.6	PRE-INSTALLATION CONFERENCE
A.	Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: GlassArt Design, which is located at:<BR />427 N. 10th Ave.<BR />Minneapolis, MN 55401<BR />Tel: 612-870 0247<BR />Fax: 612-870 0186<BR />Email: request info (sales@glassartdesign.com);Web: http://glassartdesign.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	PERFORMANCE REQUIREMENTS
A.	Provide safety glass tested and labeled to CPSC 16 CFR 1201 for locations subject to human impact as required by:
1.	Applicable Building Code.
2.	Authorities having jurisdiction.
2.3	DECORATIVE GLASS GLAZING
A.	Basis of Design: Etched Glassas manufactured and supplied by GlassArt Design.
1.	Glass Type: Clear float.
2.	Glass Type: Clear float matte/satin.
3.	Glass Type: Clear low iron
4.	Glass Type: Clear low-iron matte/satin.
5.	Glass Type: Tinted.
6.	Glass Type: Clear mirror.
7.	Glass Type: Antique Mirror.
8.	Glass Thickness (in/mm): ________.
9.	Glass Sheet Size (in/mm): ________.
10.	Pattern, One Surface: Morrocan.
11.	Pattern, One Surface: Mosaic.
12.	Pattern, One Surface: Damask.
13.	Pattern, One Surface: Venetian.
14.	Pattern, One Surface: Eden.
15.	Pattern, One Surface: Casa.
16.	Pattern, One Surface: Geo-fade.
17.	Pattern, Two Surface: Ribbons.
18.	Pattern, Two Surface: Aspen.
19.	Pattern, Two Surface: Burlap.
20.	Pattern, Two Surface: Mid-modern.
21.	Pattern, Two Surface: Pebble.
22.	Pattern, Two Surface: Trigometric.
23.	Pattern, Two Surface: Herringbone.
24.	Pattern, Two Surface: Strand.
25.	Pattern: As indicated on Drawings.
26.	Pattern: As provided by Architect.
27.	Pattern: As determined by the Architect from Manufacturer's selection.
28.	Pattern: _______.
29.	Glass Edges: Pencil polished.
30.	Glass Edges: Pencil ground.
31.	Glass Edges: Flat polished.
32.	Glass Edges: Flat ground.
33.	Glass Edges: Plateau.
34.	Glass Edges: Nibbled.
35.	Glass Edges: Broken.
36.	Glass Edges: Seamed
37.	Glass Edges: As determined by the Architect from Manufacturer's selection.
38.	Custom Options:
a.	Safety Glazing: Laminated.
b.	Safety Glazing: Tempered.
c.	Custom Bent: As detailed on the drawings.
d.	Notches: As detailed on the drawings.
e.	Shapes: As detailed on the drawings.
f.	Holes: As detailed on the drawings.
g.	Outlets: As detailed on the drawings.
h.	Applied Opaque Color Coating: ________.
i.	Applied Translucent Color Coating: ________.
j.	Marine-grade clear coating.
B.	Basis of Design: Carved Glass as manufactured by GlassArt Design.
1.	Glass Type: Clear float.
2.	Glass Type: Clear float matte/satin.
3.	Glass Type: Clear low-iron.
4.	Glass Type: Clear low iron matte/satin.
5.	Glass Type: Tinted.
6.	Glass Thickness (in/mm): ________.
7.	Glass Sheet Size (in/mm): ________.
8.	Pattern: Deep-Carved Dunes.
9.	Pattern: Deep-Carved Dunes 2.
10.	Pattern: Stage-Carved Dunes.
11.	Pattern: Granite.
12.	Pattern: Stucco.
13.	Pattern: Stucco 2.
14.	Pattern: Fresco.
15.	Pattern: Lunar.
16.	Pattern: Single Glue Chip.
17.	Pattern: Soft Chip.
18.	Pattern: Japanese Wave 3.
19.	Pattern: As indicated on Drawings.
20.	Pattern: As provided by the Architect.
21.	Pattern: As determined by the Architect from Manufacturer's selection
22.	Pattern: _______.
23.	Glass Edges: Seamed.
24.	Glass Edges: Pencil polished.
25.	Glass Edges: Pencil ground.
26.	Glass Edges: Flat polished.
27.	Glass Edges: Flat ground.
28.	Glass Edges: Plateau.
29.	Glass Edges: Nibbled.
30.	Glass Edges: Broken.
31.	Custom Options:
a.	Safety Glazing: Laminated.
b.	Safety Glazing: Tempered.
c.	Custom Bent: As detailed on the drawings.
d.	Notches: As detailed on the drawings.
e.	Shapes: As detailed on the drawings.
f.	Holes: As detailed on the drawings.
g.	Outlets: As detailed on the drawings.
h.	Applied Opaque Color Coating: ________.
i.	Applied Translucent Color Coating: ________.
j.	Apply marine-grade clear coating.
C.	Basis of Design: Patterned Glass as provided by GlassArt Design.
1.	Glass Thickness: 1/8 inch (3 mm).
2.	Glass Thickness: 5/32 inch (4 mm).
3.	Glass Thickness: 1/4 inch (6.5 mm).
4.	Glass Thickness: 3/8 (9.5 mm).
5.	Glass Thickness (in/mm): _______.
6.	Glass Sheet Size: As specified by pattern.
7.	Glass Color: Clear float.
8.	Pattern: 1/2 inch Cross Reeded. 
9.	Pattern: Double Gluechip. 
10.	Pattern: English Muffle. 
11.	Pattern: GNA clear. 
12.	Pattern: K-Seedy. 
13.	Pattern: Ligne. 
14.	Pattern: Pointe. 
15.	Pattern: Carre. 
16.	Pattern: Autumn. 
17.	Pattern: Rain glass.
18.	Pattern: Raye. 
19.	Pattern: Euro Rain. 
20.	Pattern: Single Gluechip. 
21.	Pattern: S-Seedy. 
22.	Pattern: Waterglass. 
23.	Pattern: Wide Reeded. 
24.	Pattern: Winterlake. Sheet Size: 
25.	Pattern: Lo-Iron Velour. Sheet Size: 
26.	Pattern: Wavevue. 
27.	Pattern: Chinchilla. 
28.	Pattern: Cottswald. 
29.	Pattern: Delta. 
30.	Pattern: Frosted Delta. 
31.	Pattern: Euro Granite. 
32.	Pattern: Master Lens. 
33.	Pattern: Faux Restoration. 
34.	Pattern: Narrow Reeded. 
35.	Pattern: Silvit. 
36.	Pattern: Sparkolite. 
37.	Pattern: Stippolyte. 
38.	Pattern: Sycamore. 
39.	Glass Edges: Seamed.
40.	Glass Edges: Flat ground.
41.	Custom Options:
a.	Safety Glazing: Tempered.
b.	Safety Glazing: Laminated.
c.	Custom Bent: As detailed on the drawings.
d.	Notches: As detailed on the drawings.
e.	Patterns: As detailed on the drawings.
f.	Holes: As detailed on the drawings.
g.	Outlets: As detailed on the drawings.
h.	Applied Opaque Color Coating: ________.
i.	Applied Translucent Color Coating: ________.
j.	Marine-grade clear coating.
D.	Basis of Design: Firemolded Kiln Fired Glass as manufactured by GlassArt Design:
1.	Glass Type: Clear float.
2.	Glass Type: Clear low-iron.
3.	Glass Type: Tinted Grey
4.	Glass Type: Tinted Bronze
5.	Glass Type: Tinted Graylite.
6.	Glass Type: Tinted Atlantica.
7.	Glass Type: Tinted Azuria.
8.	Glass Type: Tinted Blue Green.
9.	Glass Type: Tinted Evergreen.
10.	Glass Type: Tinted Pacifica.
11.	Glass Type: Tinted Solar Blue.
12.	Glass Type: Tinted Solexia.
13.	Glass Thickness (in/mm): ________.
14.	Glass Sheet Size (in/mm): ________.
15.	Pattern: Sandstone.
16.	Pattern: Delta.
17.	Pattern: Lagoon.
18.	Pattern: Bamboo.
19.	Pattern: Elephant.
20.	Pattern: Ripple.
21.	Pattern: Geo.
22.	Pattern: Adobe.
23.	Pattern: Canvas.
24.	Pattern: Agate.
25.	Pattern: Linen.
26.	Pattern: Shabori.
27.	Pattern: Pinstripes.
28.	Pattern: Sienna.
29.	Pattern: Mezella.
30.	Pattern: Nieve.
31.	Pattern: Vides.
32.	Pattern: Winterlake.
33.	Pattern: Ocean.
34.	Pattern: Crezca.
35.	Pattern: Sonris.
36.	Pattern: Cielo.
37.	Pattern: Bayou.
38.	Pattern: Lava.
39.	Pattern: Batik.
40.	Pattern: Terra.
41.	Pattern: Lantero.
42.	Pattern: Sirrus.
43.	Pattern: Casero.
44.	Pattern: Spirit.
45.	Pattern: Grassland.
46.	Pattern: Tempest.
47.	Pattern: River.
48.	Pattern: Savana.
49.	Pattern: Pantera.
50.	Pattern: Matrice.
51.	Pattern: Shoal.
52.	Pattern: Constellation.
53.	Pattern: Mars.
54.	Pattern: Fizz.
55.	Pattern: Cedar.
56.	Pattern: GlassArt-Antique
57.	Pattern: As indicated on Drawings.
58.	Pattern: As provided by Architect.
59.	Pattern: As determined by the Architect from Manufacturer's selection.
60.	Pattern: _______.
61.	Glass Edges: Fire polished.
62.	Glass Edges: Flat.
63.	Custom Options:
a.	Safety Glazing: Laminated.
b.	Safety Glazing: Tempered.
c.	Custom Bent: As detailed on the drawings.
d.	Combined Textures on One Panel: As detailed on the drawings.
e.	Applied Opaque Color Coating: ________.
f.	Applied Translucent Color Coating: ________.
g.	Etched: ________.
h.	Carved: ________.
i.	Marine-grade clear coating.
E.	Basis of Design: Elements Recycled Glass as manufactured by GlassArt Design.
1.	Glass Color: Ancient Gray.
2.	Glass Color: Black.
3.	Glass Color: Brown.
4.	Glass Color: Jade.
5.	Glass Color: White.
6.	Glass Thickness: 7/8 inch (22 mm).
7.	Glass Sheet Size (in/mm): ________.
8.	Glass Finish: Polished.
9.	Glass Edges: Flat Polished.
10.	Glass Edges: Flat Ground.
11.	Glass Edges: Mitered.
12.	Custom Options:
a.	Holes: As detailed on the Drawings.
b.	Sink Cutouts: As detailed on the Drawings.
c.	Sink Cutouts: With polishing.
d.	Sink Cutouts: Without polishing.
F.	Basis of Design: EcoLuxe Recycled Glass as manufactured by GlassArt Design.
1.	Applied Opaque Color Coating: ________.
2.	Applied Translucent Color Coating: ________.
3.	Glass Thickness (in/mm): ________.
4.	Glass Sheet Size (in/mm): ________.
5.	Glass Finish: Natural Fused, Epoxy coated
6.	Glass Finish: Flat, matte finish.
7.	Glass Finish: Flat epoxy coated. 
8.	Glass Edges: Flat Ground.
9.	Glass Edges: Hand Polished.
10.	Custom Options:
a.	Holes: As detailed on the Drawings.
b.	Sink Cutouts: As detailed on the Drawings.
c.	Outlet Cutouts: As detailed on the Drawings.
d.	Notches: As detailed on the Drawings.
e.	Shapes: As detailed on the Drawings.
f.	Holes / Cutouts / Notches: With polishing.
g.	Holes / Cutouts / Notches: Without polishing.
h.	Safety Glazing: Laminated.
i.	Safety Glazing: Safety Backing.
G.	Basis of Design: FirePolished Glass as manufactured by GlassArt Design.
1.	Glass Type: Clear float.
2.	Glass Type: Clear float matte/satin.
3.	Glass Type: Clear low-iron.
4.	Glass Type: Clear low iron matte/satin.
5.	Glass Type: Tinted Grey
6.	Glass Type: Tinted Bronze
7.	Glass Type: Tinted Graylite.
8.	Glass Type: Tinted Atlantica.
9.	Glass Type: Tinted Azuria.
10.	Glass Type: Tinted Blue Green.
11.	Glass Type: Tinted Evergreen.
12.	Glass Type: Tinted Pacifica.
13.	Glass Type: Tinted Solar Blue.
14.	Glass Type: Tinted Solexia.
15.	Delete glass thickness options not required.
16.	Glass Thickness: 1/4 inch (6.5 mm).
17.	Glass Thickness: 1/2 inch (12.7 mm).
18.	Glass Thickness: 3/4 inch (19.1 mm).
19.	Glass Thickness: 1 inch (25.4 mm).
20.	Glass Thickness (in/mm): _______.
21.	Glass Edges: Fire polished.
22.	Glass Edges: Flat polished.
23.	Glass Edges: Flat ground.
24.	Glass Edges: Nibbled.
25.	Glass Edges: Plateau edge.
26.	Custom Options:
a.	Safety Glazing: Laminated.
b.	Safety Glazing: Tempered.
c.	Custom Bent: As detailed on the drawings.
d.	Applied Opaque Color Coating: ________.
e.	Applied Translucent Color Coating: ________.
f.	Marine-grade clear coating.
H.	Basis of Design: Fused Glass as manufactured by GlassArt Design.
1.	Glass Type: Clear float.
2.	Glass Type: Clear low-iron.
3.	Glass Type: Tinted
4.	Glass Type: Custom Color: _______.
5.	Glass Thickness (in/mm): ________.
6.	Glass Sheet Size (in/mm): ________.
7.	Pattern: Custom pattern as indicated on Drawings.
8.	Pattern: Custom pattern to be provided by Architect.
9.	Glass Edges: Fire polished.
10.	Glass Edges: Flat polished.
11.	Glass Edges: Flat ground.
12.	Glass Edges: Nibbled.
13.	Custom Options:
a.	Applied Opaque Color Coating: ________.
b.	Applied Translucent Color Coating: ________.
c.	Marine-grade clear coating.
I.	Basis of Design: Colorcoat Back Painted Glass as manufactured by GlassArt Design.
1.	Glass Type: Clear float.
2.	Glass Type: Clear float matte/satin.
3.	Glass Type: Clear low iron
4.	Glass Type: Clear low-iron matte/satin.
5.	Glass Type: Tinted Bronze.
6.	Glass Type: Tinted Gray. 
7.	Glass Type: Tinted Graylite.
8.	Glass Type: Tinted Atlantica.
9.	Glass Type: Tinted Azuria.
10.	Glass Type: Tinted Blue Green.
11.	Glass Type: Tinted Evergreen.
12.	Glass Type: Tinted Pacifica.
13.	Glass Type: Tinted Solar Blue.
14.	Glass Type: Tinted Solexia.
15.	Glass Type: Firemolded Glass.
16.	Glass Type: Etched Glass.
17.	Glass Type: Pattern Glass.
18.	Glass Type: Clear mirror.
19.	Glass Type: Antique mirror.
20.	Glass Type: Carved.
21.	Glass Type: Fused.
22.	Glass Thickness (in/mm): ________.
23.	Glass Sheet Size (in/mm): ________.
24.	Pattern: Solid over entire surface.
25.	Pattern: Custom pattern as indicated on Drawings.
26.	Pattern: Custom pattern to be provided by Architect.
27.	Glass Edges: Seamed.
28.	Glass Edges: Pencil Polished.
29.	Glass Edges: Pencil Ground.
30.	Glass Edges: Flat Polished.
31.	Glass Edges: Flat Ground.
32.	Glass Edges: Plateau.
33.	Glass Edges: Nibbled.
34.	Glass Edges: Broken.
35.	Glass Edges: Beveled.
36.	Custom Options:
a.	Safety Gazing: Laminated.
b.	Safety Glazing: Tempered.
c.	Custom Bent: As detailed on the drawings.
d.	Notches: As detailed on the drawings.
e.	Shapes: As detailed on the drawings.
f.	Holes: As detailed on the drawings.
g.	Outlets: As detailed on the drawings.
h.	Etching Clearshield: As detailed on the drawings.
i.	Custom etched: As detailed on the drawings.
j.	LED Lighting.
k.	Opacity Customization
l.	Applied Opaque Color Coating: ________.
m.	Applied Translucent Color Coating: ________.
n.	Marine-grade clear coating.
J.	Basis of Design: Classic Mirror Glass as manufactured by GlassArt Design.
1.	Glass Color: Clear.
2.	Glass Color: Bronze.
3.	Glass Color: Gray.
4.	Glass Color: Specialty ________.
5.	Glass Thickness: 1/8 inch (3 mm).
6.	Glass Thickness: 1/4 inch (6.5 mm).
7.	Glass Sheet Size (in/mm): ________.
8.	Pattern: Solid over entire surface.
9.	Pattern: Custom pattern as indicated on Drawings.
10.	Pattern: Custom pattern to be provided by Architect.
11.	Glass Edges: Flat Polished.
12.	Glass Edges: Flat Ground.
13.	Glass Edges: Beveled.
14.	Glass Edges: Pencil Ground.
15.	Glass Edges: Pencil Polished.
16.	Custom Options:
a.	Safety Gazing: Laminated.
b.	Notches: As detailed on the drawings.
c.	Shapes: As detailed on the drawings.
d.	Holes: As detailed on the drawings.
e.	Outlets: As detailed on the drawings.
f.	Safety Mesh: Category 2.
g.	Custom Etched: As detailed on the drawings.
h.	Custom Carved Design: As detailed on the drawings.
i.	Custom Desilvering.
j.	Applied Opaque Color Coating: ________.
k.	Applied Translucent Color Coating: ________.
l.	Stained Custom Color: ________.
K.	Basis of Design: Antique Mirror Glass as manufactured by GlassArt Design.
1.	Glass Color: Clear.
2.	Glass Thickness: 1/8 inch (3 mm).
3.	Glass Thickness: 1/4 inch (6.5 mm).
4.	Glass Sheet Size (in/mm): ________.
5.	Pattern: Solid over entire surface.
6.	Pattern: Custom pattern as indicated on Drawings.
7.	Pattern: Custom pattern to be provided by Architect.
8.	Glass Edges: Flat Polished.
9.	Glass Edges: Flat Ground.
10.	Glass Edges: Beveled.
11.	Glass Finish: Dark Cloud.
12.	Glass Finish: Rainbow.
13.	Glass Finish: Sunset.
14.	Glass Finish: Snow Cloud.
15.	Glass Finish: Silver Patina.
16.	Glass Finish: Summer Cloud.
17.	Glass Finish: French.
18.	Additional patterns/finishes available upon request: ______.
19.	Custom Options:
a.	Safety Gazing: Laminated.
b.	Notches: As detailed on the drawings.
c.	Shapes: As detailed on the drawings.
d.	Holes: As detailed on the drawings.
e.	Outlets: As detailed on the drawings.
f.	Safety Mesh: Category 2.
g.	Etching Clearshield: As detailed on the drawings.
h.	Custom Etched: As detailed on the drawings.
i.	Custom Carved Design: As detailed on the drawings.
j.	Custom Desilvering.
k.	Applied Opaque Color Coating: ________.
l.	Applied Translucent Color Coating: ________.
L.	Basis of Design: Stained and Leaded Glass as manufactured by GlassArt Design.
1.	Glass Type: Custom colored.
2.	Glass Type: Patterned.
3.	Glass Type: Clear float.
4.	Glass Type: Clear float matte/satin.
5.	Glass Type: Clear low-iron.
6.	Glass Type: Clear low-iron matte/satin.
7.	Glass Type: Tinted.
8.	Glass Type: Clear mirror.
9.	Glass Type: Antique mirror.
10.	Glass Type: As shown on Architectural drawings.
11.	Glass Thickness: Nominal thickness 5/16 inch (8 mm).
12.	Profile: Round.
13.	Profile: Flat.
14.	Cames Edges: Lead.
15.	Cames Edges: Brass.
16.	Cames Edges: Zinc.
17.	Color and Pattern: As indicated on Drawings.
18.	Color and Pattern: As provided by Architect.
M.	Basis of Design: Laminated Glass as manufactured by GlassArt Design.
1.	Glass Type: Clear float.
2.	Glass Type: Clear float matte/satin.
3.	Glass Type: Clear low-iron.
4.	Glass Type: Clear low-iron matte/satin
5.	Glass Type: Tinted.
6.	Glass Type: Clear mirror.
7.	Glass Type: Antique mirror.
8.	Glass Edges: Seamed.
9.	Glass Edges: Flat polish.
10.	Glass Edges: Flat ground.
11.	Glass Thickness (in/mm): ________.
12.	Custom Options:
a.	Safety Gazing: Tempered.
b.	Patterns: As detailed on the drawings.
c.	Notches: As detailed on the drawings.
d.	Shapes: As detailed on the drawings.
e.	Holes: As detailed on the drawings.
f.	Applied Opaque Color Coating: ________.
g.	Applied Translucent Color Coating: ________.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions approved submittals and in proper relationship with adjacent construction.
3.4	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.
3.5	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturers recommendations.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION