SECTION 12 36 26

GLASS COUNTERTOPS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2024 -  2024 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Glass countertops Including:
1.	Elements recycled glass.
2.	Gemma glass countertops.
1.2	RELATED SECTIONS
A.	Section 12 10 00 - Art.
B.	Section.12 30 00 - Casework
C.	Section 12 35 00 - Specialty Casework.
D.	Section 12 40 00 - Furnishings and Accessories
1.3	REFERENCES
A.	U.S. Consumer Product Safety Commission (CPSC):
1.	CPSC 16 CFR 1201 Safety Standard for Architectural Glazing Materials.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used and installation instructions.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Verification Samples: Two representative units of each type, pattern, and color.
1.	Glass: Two 12 x 12 inch (305 by 305 mm) glass samples.
2.	Glass: Two _____ x _____ inch (_____ x _____ mm) glass samples.
D.	Shop Drawings: Include details of materials, construction, and finish. Include relationship with adjacent construction.
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
D.	Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
1.	Intent of mock-up is to demonstrate quality of workmanship and visual appearance.
2.	If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
3.	Retain mock-up during construction as standard for comparison with completed work.
4.	Do not alter or remove mock-up until work is completed or removal is authorized.
1.6	PRE-INSTALLATION CONFERENCE
A.	Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: GlassArt Design, which is located at:<BR />427 N. 10th Ave.<BR />Minneapolis, MN 55401<BR />Tel: 612-870 0247<BR />Fax: 612-870 0186<BR />Email: request info (sales@glassartdesign.com);Web: http://glassartdesign.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	PERFORMANCE REQUIREMENTS
A.	Provide safety glass tested and labeled to CPSC 16 CFR 1201 for locations subject to human impact as required by:
1.	Applicable Building Code.
2.	Authorities having jurisdiction.
2.3	GLASS COUNTER TOPS
A.	Basis of Design: Elements Recycled Glass as manufactured by GlassArt Design.
1.	Glass Color: Ancient Gray.
2.	Glass Color: Brown.
3.	Glass Color: Jade.
4.	Glass Color: White.
5.	Glass Thickness: 7/8 inch (22 mm).
6.	Glass Thickness: ___inches (___ mm).
7.	Glass Thickness: As detailed on the Drawings.
8.	Glass Sheet Size: ___inches (___ mm).
9.	Glass Sheet Size: As detailed on the Drawings.
10.	Glass Finish: Polished.
11.	Glass Edges: Flat Polished.
12.	Glass Edges: Flat Ground.
13.	Glass Edges: Mitered.
14.	Glass Edges: As detailed on the Drawings.
15.	Custom Options:
a.	Holes: As detailed on the Drawings.
b.	Sink Cutouts: As detailed on the Drawings.
c.	Sink Cutouts: With polishing.
d.	Sink Cutouts: Without polishing.
B.	Basis of Design: Gemma Glass Countertops as manufactured by GlassArt Design.
1.	Glass Color: Brown.
2.	Glass Color: Jade.
3.	Glass Color: White.
4.	Glass Color: White/Brown.
5.	Glass Color: White/Gray.
6.	Glass Color: Gray.
7.	Glass Color: Green/Brown.
8.	Glass Color: Black.
9.	Glass Color: Navy.
10.	Glass Color: Tortoise Shell.
11.	Glass Color: ________.
12.	Glass Thickness: 1 inch (25 mm).
13.	Glass Thickness: ___inches (___ mm).
14.	Glass Thickness: As detailed on the Drawings.
15.	Glass Sheet Size: ___inches (___ mm).
16.	Glass Sheet Size: As detailed on the Drawings.
17.	Glass Finish: Flat, matte finish.
18.	Glass Edges: Flat Ground.
19.	Glass Edges: Hand Polished.
20.	Custom Options:
a.	Holes: As detailed on the Drawings.
b.	Sink Cutouts: As detailed on the Drawings.
c.	Outlet Cutouts: As detailed on the Drawings.
d.	Notches: As detailed on the Drawings.
e.	Shapes: As detailed on the Drawings.
f.	Holes / Cutouts / Notches: With polishing.
g.	Holes / Cutouts / Notches: Without polishing.
h.	Safety Glazing: Laminated.
i.	Safety Glazing: Safety Backing.
C.	Basis of Design: Fused Glass as manufactured by GlassArt Design.
1.	Glass Type: Clear float.
2.	Glass Type: Clear low-iron.
3.	Glass Type: Tinted
4.	Glass Type: Custom Color: _______.
5.	Glass Thickness: ___ inches (___ mm).
6.	Glass Sheet Size: ___ inches (___ mm).
7.	Custom Pattern: As indicated on Drawings.
8.	Custom Pattern: To be provided by Architect.
9.	Glass Edges: Fire polished.
10.	Glass Edges: Flat polished.
11.	Glass Edges: Flat ground.
12.	Glass Edges: Nibbled.
13.	Custom Options:
a.	Applied Opaque Color Coating: ________.
b.	Applied Translucent Color Coating: ________.
c.	Marine-grade clear coating.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions approved submittals and in proper relationship with adjacent construction.
3.4	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.
3.5	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturers recommendations.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION