SECTION 08 36 13

SECTIONAL DOORS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2015 -  2024 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Sectional doors of the following types:
1.	Full view aluminum garage doors. (RA-360)
2.	Commercial aluminum garage doors. (CA-315/CA-320/CA-110)
3.	Insulated aluminum sectional doors.  (CHT-5800) (CHT-5200) (CHT-5700)
4.	Insulated steel sectional doors. (CHT-800) (CHT-2000) (CHT-700) (CHT-600)
5.	Commercial ribbed steel garage doors. (C2000) (C2400) (C2500)
6.	Steel garage stamped panel pan doors. (2400/2500)
7.	Overlay carriage house garage doors. (American Tradition 9000 Series)
1.2	RELATED SECTIONS
A.	Section 05 50 00 - Metal Fabrications.
B.	Section 08 71 00 - Door Hardware.
C.	Section 09 90 00 - Painting and Coating.
D.	Section 11 12 26.13 - Parking Fee Coin Collection Equipment.
E.	Section 26 05 00 - Common Work Results for Electrical.
1.3	REFERENCES
A.	ASTM International (ASTM):
1.	ASTM A 653/A 653M - Standard Specification for Steel Sheet, Zinc-Coated (Galvanized) or Zinc-Iron Alloy-Coated (Galvannealed) by the Hot-Dip Process.
2.	ASTM B209 - Standard Specification for Aluminum and Aluminum-Alloy Sheet and Plate.
B.	American Society of Heating, Refrigerating, and Air-Conditioning Engineers (ASHRAE)
1.	ASHRAE Standard 90.1
C.	American National Standards Institute/Door and Access Systems Manufacturers Association (ANSI/DASMA). 
1.	ANSI/DASMA 102 - Specifications for Sectional Doors. 
2.	ANSI/DASMA 105 - Thermal Performance and Verification Program.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings:
1.	Provide drawings indicating track details, head and jamb conditions, spring shafts, anchorage, accessories, finish colors, patterns and textures, operator mounts and other related information. 
2.	Indicate door designs, configurations, window designs and glass lite materials.
3.	Regulatory Requirements and Approvals: Provide shop drawings in compliance with local Authority Having Jurisdiction (AHJ).
D.	Verification Samples: Color chip representing color selected. 
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Minimum 5 years experience manufacturing similar products.
B.	Installer Qualifications: Minimum 2 years experience installing similar products.
1.6	PRE-INSTALLATION MEETINGS
A.	Convene minimum two weeks prior to starting work of this section.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Deliver and store products in manufacturer's unopened packaging bearing the brand name and manufacturer's identification until ready for installation.
B.	Handling: Handle materials to avoid damage.
1.8	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.9	SEQUENCING
A.	Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
1.10	WARRANTY
A.	Residential Warranty: Provide manufacturer's standard limited lifetime warranty.
B.	Commercial Warranty:  Provide manufacturer�s standard limited warranty.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Haas Door Co.; 320 Sycamore Street, Wauseon, OH 43567; ASD Tel: (419) 337-9900; Fax: (800) 874-4227; Email: specs@haasdoor.com; Web: http://www.haasdoor.com.
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00.
2.2	SECTIONAL DOORS
A.	Operation and Construction:
1.	Doors are built to meet or exceed standards established by ANSI/DASMA 102-2011.
2.	Operation: Manual operation.
a.	Chain hoist.
3.	Operation: Motor operated.
a.	Operator Type: Trolley operator.
b.	Operator Type: Jackshaft operator.
c.	Power Supply: 120 volts.
d.	Power Supply: 208/240 volts.
e.	Power Supply: 480 volts.
f.	Control Accessory: 24 volt 2-button station (open/close).
g.	Control Accessory: 24 volt 3-button station (open/close/stop).
h.	Control Accessory: 24 volt key switch.
4.	Track:
a.	Material: Hot-dipped galvanized steel (ASTM A-653).
b.	Configuration Type: Standard lift.
c.	Configuration Type: Low headroom.
d.	Configuration Type: Vertical lift.
e.	Configuration Type: High lift.
f.	Configuration Type: Follow roof pitch.
g.	Size: 2 inches (51 mm), track rollers consistent with track size, with hardened steel ball bearings.
h.	Size: 3 inches (76 mm), track rollers consistent with track size, with hardened steel ball bearings.
5.	Counterbalance System: Provided with aircraft-type, galvanized steel lifting cables with minimum safety factor of 6. Torsion Springs consisting of heavy-duty oil-tempered wire torsion springs on a continuous ball-bearing cross-header shaft.
a.	Spring Cycle Life: 10,000 cycles.
b.	Spring Cycle Life: 25,000 cycles.
c.	Spring Cycle Life: 50,000 cycles.
d.	Spring Cycle Life: 75,000 cycles.
e.	Spring Cycle Life: 100,000 cycles.
6.	Hardware:
a.	Hinges and Brackets: Hot-dipped galvanized steel, 14 gauge minimum. Double end hinges are supplied on doors 18 feet (5486 mm) and wider.
b.	Lock Device: Exterior key lock with five-pin tumbler cylinder, night latch and steel bar engaging track.
c.	Lock Device: Interior slide bar lock to be spring loaded, mounted on end stile and shall engage slot in track.
7.	Weatherstripping:
a.	Perimeter Seal: Flexible perimeter seal for jambs and header.
b.	Bottom Seal: Full length vinyl astragal retainer. Weather strip to be "U" shaped flexible extruded vinyl.
8.	Wind Loading: +____ /-____ psf Design Pressure.
a.	Wind Load Test Pressure: 1.5 times the Design Pressure.
B.	Full View Aluminum Garage Door - RA-360 Series as manufactured by Haas Door Co.
1.	Garage Door - General: 
a.	Application:  Residential. 
b.	Framing: Sections will be 1.75 inches (44.5 mm) thick full tubular aluminum framework with 0.125 inch (3.18 mm) wall thickness wherever hardware attaches. Vertical stiles and horizontal rails will be assembled using internal steel thru-bolts. Horizontal meeting rails will have tongue and groove joints. Bottom rails, top rails and end stiles are 6 inches (152 mm). Center stiles are 2 inches (51 mm). Meeting rails are 4 inches (102 mm).
1)	Doors are built to meet or exceed standards established by ANSI/DASMA 102.
c.	Panels: 
1)	Section height as indicated. 
2)	Glazing and solid panels as selected will be set in a continuous glazing sealant and held in place by inside vinyl snap-in glazing bead.
d.	End Stile:  6 inch (152 mm). 
e.	Bottom Rail:  6 inch (152 mm). 
f.	Top Rail:  6 inch (152 mm). 
g.	Insulation in Rails and Stiles:  Polystyrene. 
2.	Color: Clear Anodized.
3.	Color: Dark Bronze Anodized.
4.	Color: Black Anodized.
5.	Color: Polar White.
6.	Color: Almond.
7.	Color: Painted Black.
8.	Color: Painted Bronze.
9.	Color: Brown.
10.	Color: Charcoal.
11.	Color:  Espresso.
12.	Color:  Gray.
13.	Color:  Sandstone. 
14.	Color:  Sahara Tan.
15.	Powder Coated Woodgrain: National Oak.
16.	Powder Coated Woodgrain: European Cherry.
17.	Powder Coated Woodgrain: Coffee.
18.	Powder Coated Woodgrain: National Cherry.
19.	Powder Coated Woodgrain: Black Walnut.
20.	Powder Coated Woodgrain: Cherry with Flame.
21.	Powder Coated Woodgrain: Antique Cherry.
22.	Powder Coated Woodgrain: Knotty Pine.
23.	Powder Coated Woodgrain: Colony Maple.
24.	Powder Coated Woodgrain: Heritage Maple.
25.	Powder Coated Woodgrain: Spiced Walnut.
26.	Glazing Types: 
a.	Glass: 1/8 Inch (3 mm):
1)	Clear Tempered.
2)	Frosted Tempered.
3)	Bronze Tempered.
4)	Dark Gray Tempered.
5)	Light Gray Tempered.
6)	Obscure Pattern 62.
7)	Rain Tempered. 
8)	Clear Acrylic (Plexiglass).
9)	Clear Polycarbonate (Lexan).
b.	Glass: 3/16 Inch (4 mm):	 
1)	Arctic Tempered. 
2)	Reed Tempered. 
c.	Glass: 1/4 Inch (6 mm):
1)	Clear Tempered.
2)	Frosted Tempered.
3)	Bronze Tempered.
4)	Dark Gray Tempered.
5)	Light Gray Tempered.
6)	Clear Laminated.
7)	Reflective Bronze.
8)	Clear Acrylic (Plexiglass).
9)	Clear Polycarbonate (Lexan).
10)	Wire.
11)	Hurricane Impact Resistant Clear Polycarbonate.
12)	Hurricane Impact Resistant Bronze Polycarbonate.
13)	Hurricane Impact Resistant Dark Gray Polycarbonate.
14)	Hurricane Impact Resistant Pebble Polycarbonate.
15)	Hurricane Impact Resistant Frosted Polycarbonate. 
d.	Glass: 1/2 Inch (12 mm) Insulated:
1)	Clear Tempered.
2)	Frosted over Clear Tempered.
3)	Bronze over Clear Tempered.
4)	Bronze over Frosted Tempered.
5)	Dark Gray over Clear Tempered.
6)	Dark Gray over Frosted Tempered.
7)	Dark Gray over Dark Gray Tempered.
8)	Light Gray over Clear Tempered.
9)	Light Gray over Frosted Tempered. 
10)	Rain over Clear Tempered. 
11)	Rain over Frosted Tempered. 
12)	Low E - Standard Clear Tempered.
13)	Low E - Tinted Light Gray Tempered.
14)	Low E - Tinted Dark Gray Tempered. 
15)	Low E - Tinted Bronze Tempered. 
16)	SolarShield w/ Argon Gas Tempered.
17)	Obscure Pattern 62 over Clear Tempered.
18)	Obscure Pattern 62 over Frosted Tempered. 
19)	Translucent Mirror.
27.	Solid Panels: 
a.	Panel: 0.050 Inch (1.25 mm) smooth aluminum panel.
b.	Insulation in Panel: Laminated polystyrene.
C.	Commercial Aluminum Garage Doors - CA-320 Heavy Duty Frame as manufactured by Haas Door Co.
1.	Garage Door - General: 
a.	Application:  Commercial. 
b.	Framing: Sections will be 1.75 inches (44.5 mm) thick full tubular aluminum framework with 0.125 inch (3.18 mm) wall thickness wherever hardware attaches. Vertical stiles and horizontal rails will be assembled using internal steel thru-bolts. Horizontal meeting rails will have tongue and groove joints. Center stiles are 2 inches (51 mm). Meeting rails are 4 inches (102 mm).
1)	Doors are built to meet or exceed standards established by ANSI/DASMA 102.
c.	Panels: 
1)	Section height as indicated. 
2)	Glazing and solid panels as selected will be set in a continuous glazing sealant and held in place by inside vinyl snap-in glazing bead. 
d.	End Stile:
1)	4 inch (102 mm).
2)	6 inch (152 mm).
e.	Bottom Rail:
1)	4 inch (102 mm).
2)	6 inch (152 mm).
f.	Top Rail:
1)	4 inch (102 mm).
2)	6 inch (152 mm).
g.	Insulation in Rails and Stiles:  Polystyrene. 
2.	Color: Clear Anodized.
3.	Color: Dark Bronze Anodized.
4.	Color: Black Anodized.
5.	Color: Polar White.
6.	Color: Almond.
7.	Color: Painted Black.
8.	Color: Painted Bronze.
9.	Color: Brown.
10.	Color: Charcoal.
11.	Color:  Espresso.
12.	Color:  Gray.
13.	Color:  Sandstone. 
14.	Color:  Sahara Tan.
15.	Powder Coated Woodgrain: National Oak.
16.	Powder Coated Woodgrain: European Cherry.
17.	Powder Coated Woodgrain: Coffee.
18.	Powder Coated Woodgrain: National Cherry.
19.	Powder Coated Woodgrain: Black Walnut.
20.	Powder Coated Woodgrain: Cherry with Flame.
21.	Powder Coated Woodgrain: Antique Cherry.
22.	Powder Coated Woodgrain: Knotty Pine.
23.	Powder Coated Woodgrain: Colony Maple.
24.	Powder Coated Woodgrain: Heritage Maple.
25.	Powder Coated Woodgrain: Spiced Walnut.
26.	Glazing Types: 
a.	Glass: 1/8 Inch (3 mm):
1)	Clear Tempered.
2)	Frosted Tempered.
3)	Bronze Tempered.
4)	Dark Gray Tempered.
5)	Light Gray Tempered.
6)	Obscure Pattern 62.
7)	Rain Tempered. 
8)	Clear Acrylic (Plexiglass).
9)	Clear Polycarbonate (Lexan).
b.	Glass: 3/16 Inch (4 mm):	 
1)	Arctic Tempered. 
2)	Reed Tempered.  
c.	Glass: 1/4 Inch (6 mm):
1)	Clear Tempered.
2)	Frosted Tempered.
3)	Bronze Tempered.
4)	Dark Gray Tempered.
5)	Light Gray Tempered.
6)	Clear Laminated.
7)	Reflective Bronze.
8)	Clear Acrylic (Plexiglass).
9)	Clear Polycarbonate (Lexan).
10)	Wire.
11)	Hurricane Impact Resistant Clear Polycarbonate.
12)	Hurricane Impact Resistant Bronze Polycarbonate.
13)	Hurricane Impact Resistant Dark Gray Polycarbonate.
14)	Hurricane Impact Resistant Pebble Polycarbonate.
15)	Hurricane Impact Resistant Frosted Polycarbonate. 
d.	Glass: 1/2 Inch (12 mm) Insulated:
1)	Clear Tempered.
2)	Frosted over Clear Tempered.
3)	Bronze over Clear Tempered.
4)	Bronze over Frosted Tempered.
5)	Dark Gray over Clear Tempered.
6)	Dark Gray over Frosted Tempered.
7)	Dark Gray over Dark Gray Tempered.
8)	Light Gray over Clear Tempered.
9)	Light Gray over Frosted Tempered. 
10)	Rain over Clear Tempered. 
11)	Rain over Frosted Tempered.
12)	Low E - Standard Clear Tempered.
13)	Low E - Tinted Light Gray Tempered.
14)	Low E - Tinted Dark Gray Tempered. 
15)	Low E - Tinted Bronze Tempered. 
16)	SolarShield w/ Argon Gas Tempered.
17)	Obscure Pattern 62 over Clear Tempered.
18)	Obscure Pattern 62 over Frosted Tempered. 
19)	Translucent Mirror. 
27.	Solid Panels: 
a.	Panel: 0.040 Inch (1 mm) stucco embossed aluminum panel.
b.	Panel: 0.050 Inch (1.25 mm) smooth aluminum panel.
c.	Insulation in Panel: Laminated polystyrene. 
D.	Commercial Aluminum Garage Doors - CA-315 Heavy Duty Frame as manufactured by Haas Door Co.
1.	Garage Door - General: 
a.	Application:  Commercial. 
b.	Framing: Sections will be 1.75 inches (44.5 mm) thick full tubular aluminum framework with 0.125 inch (3.18 mm) wall thickness wherever hardware attaches. Vertical stiles and horizontal rails will be assembled using internal steel thru-bolts. Horizontal meeting rails will have tongue and groove joints. Center stiles are 1 inches (25 mm). Meeting rails are 4 inches (102 mm).
1)	Doors are built to meet or exceed standards established by ANSI/DASMA 102.
c.	Panels: 
1)	Section height as indicated. 
2)	Glazing and solid panels as selected will be set in a continuous glazing sealant and held in place by inside vinyl snap-in glazing bead.
d.	End Stile:
1)	4 inch (102 mm).
2)	6 inch (152 mm).
e.	Bottom Rail:
1)	4 inch (102 mm).
2)	6 inch (152 mm).
f.	Top Rail:
1)	4 inch (102 mm).
2)	6 inch (152 mm).
2.	Color: Clear Anodized.
3.	Color: Dark Bronze Anodized.
4.	Color: Black Anodized.
5.	Color: Polar White.
6.	Color: Almond.
7.	Color: Painted Black.
8.	Color: Painted Bronze.
9.	Color: Brown.
10.	Color: Charcoal.
11.	Color:  Espresso.
12.	Color:  Gray.
13.	Color:  Sandstone. 
14.	Color:  Sahara Tan.
15.	Glazing Types: 
a.	Glass: 1/8 Inch (3 mm):
1)	Clear Tempered.
2)	Frosted Tempered.
3)	Bronze Tempered.
4)	Dark Gray Tempered.
5)	Light Gray Tempered.
6)	Obscure Pattern 62.
7)	Rain Tempered. 
8)	Clear Acrylic (Plexiglass).
9)	Clear Polycarbonate (Lexan).
b.	Glass: 3/16 Inch (4 mm):	 
1)	Arctic Tempered. 
2)	Reed Tempered. 
c.	Glass: 1/4 Inch (6 mm):
1)	Clear Tempered.
2)	Frosted Tempered.
3)	Bronze Tempered.
4)	Dark Gray Tempered.
5)	Light Gray Tempered.
6)	Clear Laminated.
7)	Reflective Bronze. 
8)	Clear Acrylic (Plexiglass).
9)	Clear Polycarbonate (Lexan).
10)	Wire.
d.	Glass: 1/2 Inch (12 mm) Insulated:
1)	Clear Tempered.
2)	Frosted over Clear Tempered.
3)	Bronze over Clear Tempered.
4)	Bronze over Frosted Tempered.
5)	Dark Gray over Clear Tempered.
6)	Dark Gray over Frosted Tempered.
7)	Dark Gray over Dark Gray Tempered.
8)	Light Gray over Clear Tempered.
9)	Light Gray over Frosted Tempered. 
10)	Rain over Clear Tempered. 
11)	Rain over Frosted Tempered.
12)	Low E - Standard Clear Tempered.
13)	Low E - Tinted Light Gray Tempered.
14)	Low E - Tinted Dark Gray Tempered. 
15)	Low E - Tinted Bronze Tempered. 
16)	SolarShield w/ Argon Gas Tempered. 
17)	Obscure Pattern 62 over Clear Tempered.
18)	Obscure Pattern 62 over Frosted Tempered. 
19)	Translucent Mirror. 
16.	Solid Panels: 
a.	Panel: 0.040 Inch (1 mm) stucco embossed aluminum panel.
b.	Panel: 0.050 Inch (1.25 mm) smooth aluminum panel.
c.	Insulation in Panel: Laminated polystyrene. 
E.	Commercial Aluminum Garage Doors - CA-110 Narrow Line Frame as manufactured by Haas Door Co.
1.	Garage Door - General: 
a.	Application:  Commercial. 
b.	Framing: Sections will be 1.75 inches (44.5 mm) thick full tubular aluminum framework with 0.125 inch (3.18 mm) wall thickness wherever hardware attaches. Vertical stiles and horizontal rails will be assembled using internal steel thru-bolts. Horizontal meeting rails shall have rabbeted overlap joints. Center stiles are 1 inches (25 mm). Meeting rails are 2 inches (51 mm).
1)	Doors are built to meet or exceed standards established by ANSI/DASMA 102.
c.	Panels: 
1)	Section height as indicated. 
2)	Glazing and solid panels as selected will be set in a continuous glazing sealant and held in place by inside vinyl snap-in glazing bead.
d.	End Stile:
1)	3 inch (76 mm)
2)	4 inch (102 mm)
3)	6 inch (152 mm)
e.	Bottom Rail:
1)	3 inch (76 mm)
2)	4 inch (102 mm)
3)	6 inch (152 mm)
f.	Top Rail:
1)	3 inch (76 mm)
2)	4 inch (102 mm)
3)	6 inch (152 mm)
2.	Color: Clear Anodized.
3.	Color: Dark Bronze Anodized.
4.	Color: Black Anodized.
5.	Color: Polar White.
6.	Glazing Types: 
a.	Glass: 1/8 Inch (3 mm):
1)	Clear Tempered.
2)	Frosted Tempered.
3)	Bronze Tempered.
4)	Dark Gray Tempered.
5)	Light Gray Tempered.
6)	Obscure Pattern 62.
7)	Rain Tempered. 
8)	Clear Acrylic (Plexiglass).
9)	Clear Polycarbonate (Lexan).
b.	Glass: 3/16 Inch (4 mm):	 
1)	Arctic Tempered. 
2)	Arctic Reed. 
c.	Glass: 1/4 Inch (6 mm):
1)	Clear Tempered.
2)	Frosted Tempered.
3)	Bronze Tempered.
4)	Dark Gray Tempered.
5)	Light Gray Tempered.
6)	Clear Laminated.
7)	Reflective Bronze.
8)	Clear Acrylic (Plexiglass).
9)	Clear Polycarbonate (Lexan).
10)	Wire.
d.	Glass: 1/2 Inch (12 mm) Insulated:
1)	Clear Tempered.
2)	Frosted over Clear Tempered.
3)	Bronze over Clear Tempered.
4)	Bronze over Frosted Tempered.
5)	Dark Gray over Clear Tempered.
6)	Dark Gray over Frosted Tempered.
7)	Dark Gray over Dark Gray Tempered.
8)	Light Gray over Clear Tempered.
9)	Light Gray over Frosted Tempered. 
10)	Rain over Clear Tempered. 
11)	Rain over Frosted Tempered.
12)	Low E - Standard Clear Tempered.
13)	Low E - Tinted Light Gray Tempered.
14)	Low E - Tinted Dark Gray Tempered. 
15)	Low E -  Tinted Bronze Tempered. 
16)	SolarShield w/ Argon Gas Tempered. 
17)	Obscure Pattern 62 over Clear Tempered.
18)	Obscure Pattern 62 over Frosted Tempered. 
19)	Translucent Mirror. 
7.	Solid Panels: 
a.	Panel: 0.040 Inch (1 mm) stucco embossed aluminum panel.
b.	Panel: 0.050 Inch (1.25 mm) smooth aluminum panel.
c.	Insulation in Panel: Laminated polystyrene.
F.	Insulated Aluminum Sectional Door:  CHT-5800 Series as manufactured by Haas Door Co.
1.	Application:  Commercial. 
2.	Construction: 
a.	Sections: 3 inches (76 mm) thick roll formed inside and outside, tempered aluminum alloy, insulated with high density polyurethane foam. 
b.	Thermal Break: Full tongue-and-groove thermal break construction with rigid vinyl extrusions. 
c.	Material: Tempered aluminum alloy (ASTM B-209). 
1)	Gauge:  24 gauge stucco texture exterior and 24 gauge stucco texture interior. 
d.	Exterior Panel Design:  Flush. 
e.	Exterior Panel Design:  V-groove on 3 inch centers. 
f.	Exterior Panel Design:  Standard Raised Panel with shadow lines. 
g.	Exterior Panel Design:  Ranch Raised Panel with shadow lines. 
h.	Interior Design:  V-groove on 3 inch centers.
3.	Insulation:  Fully insulated section using high density environmentally compliant polyurethane foam, pressure injected to completely fill the section.  ANSI/DASMA 105 tested U-factor = 0.089.
a.	Fire Rated Foam:  Class II fire rated foam. 
4.	Performance: Doors to meet the ASHRAE Standard 90.1 specification for wind infiltration, specifically for sectional garage doors described in Addendum O. 
5.	Doors are built to meet or exceed standards established by ANSI/DASMA 102. 
6.	Steel End Stile: 16 ga. hot-dipped galvanized steel, installed over vinyl end cap to maintain the thermal break. 
7.	Intermediate Reinforcing: Nominal 18 gauge full vertical steel back-up plates, inserted prior to foaming, to provide proper position and reinforcing for attachment of various hardware.
8.	Exterior Finish Coat: Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.  
a.	Color: Polar White. 
9.	Interior Finish Coat: Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.  
a.	Color: Polar White. 
10.	Safety Device:  Cam type safety device.  
11.	Windows: 
a.	Window Design:  25 x 12 inches (635 x 305 mm) TL windows. 
b.	Window Design:  24 x 6 inches (610 x 152 mm) TL windows. 
c.	Glazing Type:
1)	Glass:  Insulated tempered. 
a)	Clear Tempered. 
b)	Frosted over Clear Tempered. 
c)	Obscure Pattern 62 over Clear Tempered. 
d)	Obscure Pattern 62 over Frosted Tempered. 
G.	Insulated Aluminum Sectional Door:  CHT-5200 Series as manufactured by Haas Door Co.
1.	Application:  Residential. 
2.	Application:  Commercial. 
3.	Construction: 
a.	Sections: 2 inches (50.8 mm) thick roll formed inside and outside, tempered aluminum alloy, insulated with high density polyurethane foam.
b.	Thermal Break: Full tongue-and-groove thermal break construction with rigid vinyl extrusions. 
c.	Material: Tempered aluminum alloy (ASTM B-209). 
1)	Gauge:  24 gauge stucco texture exterior and 24 gauge stucco texture interior. 
d.	Exterior Panel Design:  Flush. 
e.	Exterior Panel Design:  V-groove on 3 inch (76 mm) centers. 
f.	Exterior Panel Design:  Standard Raised Panel with shadow lines. 
g.	Exterior Panel Design:  Ranch Raised Panel with shadow lines. 
h.	Interior Design:  V-groove on 3 inch (76 mm) centers. 
4.	Insulation:  Fully insulated section using high density environmentally compliant polyurethane foam, pressure injected to completely fill the section. ANSI/DASMA TPVP105 tested U-Factor = 0.110.
a.	Fire Rated Foam:  Class II fire rated foam. 
5.	Performance: Doors shall meet the ASHRAE Standard 90.1 specification for wind infiltration, specifically for sectional garage doors described in Addendum O. 
6.	Doors are built to meet or exceed standards established by ANSI/DASMA 102. 
7.	End Stiles: 
a.	Vinyl End Stiles: Integral rigid vinyl to ensure consistent thermal break and provide protection to the foam along with sealing it from excessive air exposure.
b.	Steel End Stile: 16 ga. hot-dipped galvanized steel, installed over vinyl end cap to maintain the thermal break. 
8.	Intermediate Reinforcing: Nominal 18 gauge full vertical steel back-up plates, inserted prior to foaming, to provide proper position and reinforcing for attachment of various hardware. 
9.	Exterior Finish Coat: Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.  
a.	Color: Polar White. 
10.	Interior Finish Coat: Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.  
a.	Color: Polar White. 
11.	Safety Device:  Cam type safety device. 
12.	Windows: 
a.	Window Design: Carriage House Series Windows. 
b.	Window Design:  Ranch Series Windows. 
c.	Window Design:  Standard Series Windows. 
d.	Window Design: SlimLine Windows.  
e.	Window Design: Double SlimLine Windows. 
f.	Window Design:  25 x 12 inches (635 x 305 mm) TL windows. 
g.	Window Design:  24 x 6 inches (610 x 152 mm) TL windows. 
h.	Glazing Type: 1/2 Inch (16 mm) Insulated: 
1)	Clear Tempered. 
2)	Frosted over Clear Tempered. 
3)	Bronze over Clear Tempered. 
4)	Bronze over Frosted Tempered. 
5)	Dark Gray over Clear Tempered. 
6)	Dark Gray over Frosted Tempered. 
7)	Dark Gray over Dark Gray Tempered. 
8)	Light Gray over Frosted Tempered.
9)	Light Gray over Clear Tempered. 
10)	Rain over Clear Tempered. 
11)	Rain over Frosted Tempered. 
12)	Arctic over Clear Tempered. 
13)	Arctic over Frosted Tempered. 
14)	Reed over Clear Tempered. 
15)	Reed over Frosted Tempered. 
16)	Low E - Standard Clear Tempered. 
17)	Obscure Pattern 62 over Clear Tempered. 
18)	Obscure Pattern 62 over Frosted Tempered. 
19)	SolarShield Tempered. 
20)	Translucent Mirror.
i.	Glazing Type: 1/4 Inch (6 mm): 
1)	Hurricane Impact Resistant Clear Polycarbonate. 
2)	Hurricane Impact Resistant Bronze Polycarbonate. 
3)	Hurricane Impact Resistant Dark Gray Polycarbonate. 
4)	Hurricane Impact Resistant Pebble Polycarbonate. 
5)	Hurricane Impact Resistant Frosted Polycarbonate. 
13.	Full Vision Sections: 
a.	Framing: Sections will be 1.75 inches (44.5 mm) thick full tubular aluminum framework with 0.125 inch (3.18 mm) wall thickness wherever hardware attaches.  Vertical stiles and horizontal rails will be assembled using internal steel thru-bolts. 
b.	Insulation in Rails and Stiles:  Polystyrene. 
c.	Glazing Types: 
1)	Glass:  1/8 Inch (3 mm): 
a)	Clear Tempered. 
b)	Frosted Tempered. 
c)	Bronze Tempered. 
d)	Dark Gray Tempered. 
e)	Light Gray Tempered. 
f)	Obscure Pattern 62. 
g)	Rain Tempered. 
h)	Clear Acrylic (Plexiglass). 
i)	Clear Polycarbonate (Lexan). 
2)	Glass: 3/16 Inch (4 mm):	 
a)	Arctic Tempered. 
b)	Reed Tempered. 
3)	Glass:  1/4 Inch (6 mm): 
a)	Clear Tempered. 
b)	Frosted Tempered. 
c)	Bronze Tempered. 
d)	Dark Gray Tempered. 
e)	Light Gray Tempered. 
f)	Clear Laminated. 
g)	Reflective Bronze. 
h)	Clear Acrylic (Plexiglass). 
i)	Clear Polycarbonate (Lexan). 
j)	Wire. 
4)	Glass:  1/2 Inch (12 mm) Insulated: 
a)	Clear Tempered. 
b)	Frosted over Clear Tempered. 
c)	Bronze over Clear Tempered. 
d)	Bronze over Frosted Tempered. 
e)	Dark Gray over Clear Tempered. 
f)	Dark Gray over Frosted Tempered. 
g)	Dark Gray over Dark Gray Tempered. 
h)	Light Gray over Clear Tempered. 
i)	Light Gray over Frosted Tempered.  
j)	Rain over Clear Tempered. 
k)	Rain over Frosted Tempered.
l)	Low E - Standard Clear Tempered. 
m)	Low E - Tinted Light Gray Tempered.
n)	Low E - Tinted Dark Gray Tempered. 
o)	Low E - Tinted Bronze Tempered. 
p)	SolarShield w/ Argon Gas Tempered. 
q)	Obscure Pattern 62 over Clear Tempered. 
r)	Obscure Pattern 62 over Frosted Tempered. 
s)	Translucent Mirror. 
d.	Glazing:  Set in a continuous glazing sealant and held in place by inside vinyl snap-in glazing bead.
H.	Insulated Aluminum Sectional Door:  CHT-5700 Series as manufactured by Haas Door Co.
1.	Application:  Residential. 
2.	Application:  Commercial. 
3.	Construction:  
a.	Sections: 1-3/4 inches (44.5 mm) thick roll formed inside and outside, tempered aluminum alloy, insulated with high density polyurethane foam.
b.	Thermal Break: Full tongue-and-groove thermal break construction with rigid vinyl extrusions. 
c.	Material: Tempered aluminum alloy (ASTM B-209). 
1)	Gauge:  24 gauge stucco texture exterior and 24 gauge stucco texture interior. 
d.	Exterior Panel Design:  Flush. 
e.	Exterior Panel Design:  V-groove on 3 inch (76 mm) centers. 
f.	Exterior Panel Design:  Standard Raised Panel with shadow lines. 
g.	Exterior Panel Design:  Ranch Raised Panel with shadow lines. 
h.	Interior Design:  V-groove on 3 inch centers. 
4.	Insulation:  Fully insulated section using high density environmentally compliant polyurethane foam, pressure injected to completely fill the section. ANSI/DASMA TPVP105 tested U-Factor = 0.097. 
a.	Fire Rated Foam:  Class II fire rated foam. 
5.	Doors are built to meet or exceed standards established by ANSI/DASMA 102. 
6.	End Stiles: 
a.	Vinyl End Stiles: Integral rigid vinyl to ensure consistent thermal break and provide protection to the foam along with sealing it from excessive air exposure.
b.	Steel End Stile: 16 ga. hot-dipped galvanized steel, installed over vinyl end cap to maintain the thermal break. 
7.	Intermediate Reinforcing: Nominal 18 gauge full vertical steel back-up plates, inserted prior to foaming, to provide proper position and reinforcing for attachment of various hardware. 
8.	Exterior Finish Coat: Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.  
a.	Color: Polar White. 
9.	Interior Finish Coat: Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.  
a.	Color: Polar White. 
10.	Safety Device:  Cam type safety device. 
11.	Windows: 
a.	Window Design: Carriage House Series Windows. 
b.	Window Design:  Ranch Series Windows. 
c.	Window Design:  Standard Series Windows. 
d.	Window Design: SlimLine Windows.  
e.	Window Design: Double SlimLine Windows. 
f.	Window Design:  25 x 12 inches (635 x 305 mm) TL windows. 
g.	Window Design:  24 x 6 inches (610 x 152 mm) TL windows. 
h.	Glazing Types: 1/8 Inch (3 mm):  
1)	Clear Tempered.
2)	Frosted Tempered. 
3)	Bronze Tempered. 
4)	Dark Gray Tempered. 
5)	Clear Polycarbonate (Lexan). 
6)	Light Gray Tempered. 
7)	Obscure Pattern 62. 
8)	Rain Tempered. 
i.	Glass: 3/16 Inch (4 mm):	 
1)	Arctic Tempered. 
2)	Reed Tempered. 
j.	Glazing Types: 1/4 Inch (6 mm): 
1)	Hurricane Impact Resistant Clear Polycarbonate. 
2)	Hurricane Impact Resistant Bronze Polycarbonate. 
3)	Hurricane Impact Resistant Dark Gray Polycarbonate. 
4)	Hurricane Impact Resistant Pebble Polycarbonate. 
5)	Hurricane Impact Resistant Frosted Polycarbonate. 
k.	Glazing Types: 1/2 Inch (12 mm) Insulated: 
1)	Clear Tempered. 
2)	Frosted over Clear Tempered. 
3)	Bronze over Clear Tempered. 
4)	Bronze over Frosted Tempered. 
5)	Dark Gray over Clear Tempered. 
6)	Dark Gray over Frosted Tempered. 
7)	Dark Gray over Dark Gray Tempered. 
8)	Light Gray over Clear Tempered. 
9)	Light Gray over Frosted Tempered.  
10)	Rain over Clear Tempered. 
11)	Rain over Frosted Tempered. 
12)	Arctic over Clear Tempered. 
13)	Arctic over Frosted Tempered. 
14)	Reed over Clear Tempered. 
15)	Reed over Frosted Tempered. 
16)	Low E - Standard Clear Tempered. 
17)	Obscure Pattern 62 over Clear Tempered.
18)	Obscure Pattern 62 over Frosted Tempered. 
19)	SolarShield Tempered. 
20)	Translucent Mirror. 
12.	Full Vision Sections: 
a.	Framing: Sections will be 1.75 inches (44.5 mm) thick full tubular aluminum framework with 0.125 inch (3.18 mm) wall thickness wherever hardware attaches.  Vertical stiles and horizontal rails will be assembled using internal steel thru-bolts.
b.	Insulation in Rails and Stiles:  Polystyrene. 
c.	Glazing Types:  
1)	Glass: 1/8 Inch (3 mm):  
a)	Clear DSB/Annealed. 
b)	Clear Tempered. 
c)	Bronze Tempered. 
d)	Dark Gray Tempered. 
e)	Light Gray Tempered. 
f)	Obscure Pattern 62. 
g)	Rain Tempered. 
h)	Clear Acrylic (Plexiglass). 
i)	Clear Polycarbonate (Lexan). 
2)	Glass: 3/16 Inch (4 mm):	 
a)	Arctic Tempered. 
b)	Reed Tempered. 
3)	Glass: 1/4 Inch (6 mm): 
a)	Clear Tempered. 
b)	Frosted Tempered. 
c)	Bronze Tempered. 
d)	Dark Gray Tempered. 
e)	Light Gray Tempered. 
f)	Clear Laminated. 
g)	Reflective Bronze. 
h)	Clear Acrylic (Plexiglass). 
i)	Clear Polycarbonate (Lexan). 
j)	Wire. 
4)	Glass: 1/2 Inch (12 mm) Insulated: 
a)	Clear Tempered. 
b)	Frosted over Clear Tempered. 
c)	Bronze over Clear Tempered. 
d)	Bronze over Frosted Tempered. 
e)	Dark Gray over Clear Tempered. 
f)	Dark Gray over Frosted Tempered. 
g)	Dark Gray over Dark Gray Tempered. 
h)	Light Gray over Clear Tempered. 
i)	Light Gray over Frosted Tempered.  
j)	Rain over Clear Tempered. 
k)	Rain over Frosted Tempered.
l)	Low E - Standard Clear Tempered. 
m)	Low E - Tinted Light Gray Tempered. 
n)	Low E - Tinted Dark Gray Tempered.
o)	Low E - Tinted Bronze Tempered 
p)	SolarShield w/ Argon Gas Tempered. 
q)	Obscure Pattern 62 over Clear Tempered. 
r)	Obscure Pattern 62 over Frosted Tempered. 
s)	Translucent Mirror. 
d.	Glazing: Set in a continuous glazing sealant and held in place by inside vinyl snap-in glazing bead.
I.	Insulated Steel Sectional Door - CHT-800 Series as manufactured by Haas Door Co.
1.	Application:  Commercial. 
2.	Construction:
a.	Sections: 3 inches (76.2 mm) thick roll formed inside and outside, hot-dipped galvanized steel, insulated with high density polyurethane foam.
b.	Thermal Break: Full tongue-and-groove thermal break construction with rigid vinyl extrusions.
c.	Material: Hot-dipped galvanized steel (ASTM A-653).
1)	Gauge: 26 gauge woodgrain texture exterior and 26 gauge woodgrain texture interior.
2)	Gauge: 20 gauge smooth exterior and 26 gauge woodgrain interior.
3)	Gauge: 20 gauge smooth exterior and 20 gauge smooth interior.
d.	Exterior Panel Design:
1)	Exterior Panel Design: Flush.
2)	Exterior Panel Design: V-groove on 3 inch centers.
3)	Exterior Panel Design: Standard Raised Panel with shadow lines.
4)	Exterior Panel Design: Ranch Raised Panel with shadow lines.
e.	Interior Design: V-groove on 3 inch centers
3.	Insulation: Fully insulated section using high density environmentally compliant polyurethane foam, pressure injected to completely fill the section. ANSI/DASMA TPVP105 tested U-Factor = 0.089.
a.	Fire Rated Foam: Class II fire rated foam.
4.	Performance: Doors shall meet the ASHRAE Standard 90.1 specification for wind infiltration, specifically for sectional garage doors described in Addendum O.
5.	Doors are built to meet or exceed standards established by ANSI/DASMA 102. 
6.	Steel End Stile: 16 ga. hot-dipped galvanized steel, installed over vinyl end cap to maintain the thermal break.
7.	Intermediate Reinforcing:  Nominal 18 gauge full vertical steel back-up plates, inserted prior to foaming, to provide proper position and reinforcing for attachment of various hardware.
8.	Exterior Finish Coat: Solid colors. Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.
9.	Exterior Finish Coat: Traditional wood grain. 1 mil total dry film, 3-coat system, consisting of an enhanced polyester base coat plus an ink coat and polyester clear coat.
10.	Exterior Finish Color: Polar White.
11.	Exterior Finish Color: Almond.
12.	Exterior Finish Color: Bronze.
13.	Exterior Finish Color: Brown.
14.	Exterior Finish Color: Charcoal.
15.	Exterior Finish Color:  Espresso.
16.	Exterior Finish Color:  Gray.
17.	Exterior Finish Color:  Sandstone.
18.	Exterior Finish Color:  Sahara Tan.
19.	Exterior Finish Color: Trinar Beige. 
20.	Exterior Finish Color: Trinar Brown. 
21.	Exterior Finish Color:  Ash.
22.	Exterior Finish Color:  Mahogany.
23.	Exterior Finish Color:  English Oak.
24.	Exterior Finish Bi-Directional Color:  Ash.
25.	Exterior Finish Bi-Directional Color:  Mahogany.
26.	Exterior Finish Bi-Directional Color:  English Oak.
27.	Exterior Finish Color: American Walnut. 
28.	Exterior Finish Bi-Directional Color: American Walnut. 
29.	Exterior Finish Color:  Carbon Black. 
30.	Interior Finish Coat: Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish. 
a.	Color: Polar White.
31.	Safety Device: Cam type safety device. 
32.	Windows:
a.	Window Design:  25 x 12 inches (635 x 305 mm) TL windows.
b.	Window Design:  24 x 6 inches (610 x 152 mm) TL windows.
c.	Glazing Types:
1)	Glass: Insulated tempered.
a)	Clear Tempered.
b)	Frosted over Clear Tempered.
c)	Obscure Pattern 62 over Clear Tempered. 
d)	Obscure Pattern 62 over Frosted Tempered.
J.	Insulated Steel Sectional Door - CHT-2000 Series as manufactured by Haas Door Co.
1.	Application:  Residential. 
2.	Application:  Commercial. 
3.	Construction:
a.	Sections: 2 inches (50.8 mm) thick roll formed inside and outside, hot-dipped galvanized steel, insulated with high density polyurethane foam.
b.	Thermal Break: Full tongue-and-groove thermal break construction with rigid vinyl extrusions.
c.	Material: Hot-dipped galvanized steel (ASTM A-653).
1)	Gauge: 26 gauge woodgrain texture exterior and 26 gauge woodgrain texture interior.
2)	Gauge: 20 gauge smooth exterior and 26 gauge woodgrain interior.
3)	Gauge: 20 gauge smooth exterior and 20 gauge smooth interior.
d.	Exterior Panel Design:
1)	Exterior Panel Design: Flush.
2)	Exterior Panel Design: V-groove on 3 inch (76 mm) centers.
3)	Exterior Panel Design: Standard Raised Panel with shadow lines.
4)	Exterior Panel Design: Ranch Raised Panel with shadow lines.
5)	Exterior Panel Design: Short Ribbed Panel.
6)	Exterior Panel Design: Short Recessed Panel.
7)	Exterior Panel Design: Long Ribbed Panel.
8)	Exterior Panel Design: Long Recessed Panel.
e.	Interior Design: V-groove on 3 inch (76 mm) centers.
4.	Insulation:  Fully insulated section using high density environmentally compliant polyurethane foam, pressure injected to completely fill the section. ANSI/DASMA TPVP105 tested U-Factor = 0.094.
a.	Fire Rated Foam: Class II fire rated foam.
5.	Performance: Doors shall meet the ASHRAE Standard 90.1 specification for wind infiltration, specifically for sectional garage doors described in Addendum O.
6.	Doors are built to meet or exceed standards established by ANSI/DASMA 102. 
7.	End Stiles:
a.	Vinyl End Stiles: Integral rigid vinyl to ensure consistent thermal break and provide protection to the foam along with sealing it from excessive air exposure.
b.	Steel End Stile: 16 ga. hot-dipped galvanized steel, installed over vinyl end cap to maintain the thermal break.
8.	Intermediate Reinforcing: Nominal 18 gauge full vertical steel back-up plates, inserted prior to foaming, to provide proper position and reinforcing for attachment of various hardware.
9.	Exterior Finish Coat: Solid colors. Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.
10.	Exterior Finish Coat: Traditional wood grain. 1 mil total dry film, 3-coat system, consisting of an enhanced polyester base coat plus an ink coat and polyester clear coat.
11.	Exterior Finish Coat: Plank wood grain. White base coat plus ink and a polyester clear coat.
12.	Exterior Finish Color: Polar White.
13.	Exterior Finish Color: Almond.
14.	Exterior Finish Color: Bronze.
15.	Exterior Finish Color: Brown.
16.	Exterior Finish Color: Charcoal.
17.	Exterior Finish Color:  Espresso.
18.	Exterior Finish Color:  Gray.
19.	Exterior Finish Color:  Sandstone.
20.	Exterior Finish Color:  Sahara Tan.
21.	Exterior Finish Color: Trinar Beige. 
22.	Exterior Finish Color: Trinar Brown. 
23.	Exterior Finish Color:  Ash.
24.	Exterior Finish Color:  Mahogany.
25.	Exterior Finish Color:  English Oak. 
26.	Exterior Finish Color:  Graywood.
27.	Exterior Finish  Bi-Directional Color:  Ash.
28.	Exterior Finish Bi-Directional Color:  Mahogany.
29.	Exterior Finish Bi-Directional Color:  English Oak.
30.	Exterior Finish Color: English Oak Plank. 
31.	Exterior Finish Color: Cedar Plank. 
32.	Exterior Finish Color: American Walnut. 
33.	Exterior Finish Bi-Directional Color: American Walnut. 
34.	Exterior Finish Color: American Walnut Plank. 
35.	Exterior Finish Color: Carbon Black.
36.	Interior Finish Coat: Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish. 
a.	Color: Polar White.
37.	Provide the following assembly components:
a.	Cam safety device.
b.	Pass door.
38.	Windows:
a.	Window Design:
1)	Window Design: Carriage House Series Windows.
2)	Window Design: Ranch Series Windows.
3)	Window Design: Standard Series Windows.
4)	Window Design: SlimLine Windows. 
5)	Window Design: Double SlimLine Windows. 
6)	Window Design:  25 x 12 inches (635 x 305 mm) TL windows.
7)	Window Design:  24 x 6 inches (610 x 152 mm) TL windows.
b.	Glazing Types:
1)	Glass: 1/2 Inch (16 mm) Insulated:
a)	Clear Tempered.
b)	Frosted over Clear Tempered.
c)	Bronze over Clear Tempered.
d)	Bronze over Frosted Tempered.
e)	Dark Gray over Clear Tempered.
f)	Dark Gray over Frosted Tempered.
g)	Dark Gray over Dark Gray Tempered.
h)	Light Gray over Clear Tempered.
i)	Rain over Clear Tempered. 
j)	Rain over Frosted Tempered. 
k)	Arctic over Clear Tempered. 
l)	Arctic over Frosted Tempered. 
m)	Reed over Clear Tempered. 
n)	Reed over Frosted Tempered. 
o)	Low E - Standard Clear Tempered.
p)	Obscure Pattern 62 over Clear Tempered.
q)	Obscure Pattern 62 over Frosted Tempered. 
r)	SolarShield Tempered. 
s)	Translucent Mirror. 
2)	Glass: 1/4 Inch (6 mm):
a)	Hurricane Impact Resistant Clear Polycarbonate.
b)	Hurricane Impact Resistant Bronze Polycarbonate.
c)	Hurricane Impact Resistant Dark Gray Polycarbonate.
d)	Hurricane Impact Resistant Pebble Polycarbonate.
e)	Hurricane Impact Resistant Frosted Polycarbonate. 
39.	Full Vision Sections:
a.	Framing: Sections will be 1.75 inches (44.5 mm) thick full tubular aluminum framework with 0.125 inch (3.18 mm) wall thickness wherever hardware attaches. Vertical stiles and horizontal rails will be assembled using internal steel thru-bolts.
b.	Glazing Types: 
1)	Glass: 1/8 Inch (3 mm):
a)	Clear Tempered.
b)	Frosted Tempered.
c)	Bronze Tempered.
d)	Dark Gray Tempered.
e)	Light Gray Tempered.
f)	Obscure Pattern 62.
g)	Rain Tempered. 
h)	Clear Acrylic (Plexiglass).
i)	Clear Polycarbonate (Lexan).
2)	Glass: 3/16 Inch (4 mm):	 
a)	Arctic Tempered. 
b)	Reed Tempered. 
3)	Glass: 1/4 Inch (6 mm):
a)	Clear Tempered.
b)	Frosted Tempered.
c)	Bronze Tempered.
d)	Dark Gray Tempered.
e)	Light Gray Tempered.
f)	Clear Laminated.
g)	Reflective Bronze.
h)	Clear Acrylic (Plexiglass).
i)	Clear Polycarbonate (Lexan).
j)	Wire.
4)	Glass: 1/2 Inch (12 mm) Insulated:
a)	Clear Tempered.
b)	Frosted over Clear Tempered.
c)	Bronze over Clear Tempered.
d)	Bronze over Frosted Tempered.
e)	Dark Gray over Clear Tempered.
f)	Dark Gray over Frosted Tempered.
g)	Dark Gray over Dark Gray Tempered.
h)	Light Gray over Clear Tempered.
i)	Light Gray over Frosted Tempered. 
j)	Rain over Clear Tempered. 
k)	Rain over Frosted Tempered.
l)	Low E - Standard Clear Tempered.
m)	Low E - Tinted Light Gray Tempered.
n)	Low E - Tinted Dark Gray Tempered. 
o)	Low E - Tinted Bronze Tempered. 
p)	SolarShield w/ Argon Gas Tempered. 
q)	Obscure Pattern 62 over Clear Tempered.
r)	Obscure Pattern 62 over Frosted Tempered. 
s)	Translucent Mirror.
c.	Glazing: Set in a continuous glazing sealant and held in place by inside vinyl snap-in glazing bead.
K.	Insulated Steel Sectional Door - CHT-700 Series as manufactured by Haas Door Co.
1.	Application:  Residential. 
2.	Application:  Commercial. 
3.	Construction: 
a.	Sections: 1-3/4 inches (44.5 mm) thick roll formed inside and outside, hot-dipped galvanized steel, insulated with high density polyurethane foam.
b.	Thermal Break: Full tongue-and-groove thermal break construction with rigid vinyl extrusions.
c.	Material: Hot-dipped galvanized steel (ASTM A-653).
1)	Gauge: 26 gauge woodgrain texture exterior and 26 gauge woodgrain texture interior.
2)	Gauge: 20 gauge smooth exterior and 26 gauge woodgrain interior.
3)	Gauge: 20 gauge smooth exterior and 20 gauge smooth interior.
d.	Exterior Panel Design:
1)	Exterior Panel Design: Flush.
2)	Exterior Panel Design: V-groove on 3 inch (76 mm) centers.
3)	Exterior Panel Design: Standard Raised Panel with shadow lines.
4)	Exterior Panel Design: Ranch Raised Panel with shadow lines.
5)	Exterior Panel Design: Short Ribbed Panel.
6)	Exterior Panel Design: Short Recessed Panel.
7)	Exterior Panel Design: Long Ribbed Panel.
8)	Exterior Panel Design: Long Recessed Panel.
e.	Interior Design: V-groove on 3 inch centers.
4.	Insulation:  Fully insulated section using high density environmentally compliant polyurethane foam, pressure injected to completely fill the section. ANSI/DASMA TPVP105 tested U-Factor = 0.093.
a.	Fire Rated Foam: Class II fire rated foam.
5.	Doors are built to meet or exceed standards established by ANSI/DASMA 102. 
6.	End Stiles:
a.	Vinyl End Stiles: Integral rigid vinyl to ensure consistent thermal break and provide protection to the foam along with sealing it from excessive air exposure.
b.	Steel End Stile: 16 ga. hot-dipped galvanized steel, installed over vinyl end cap to maintain the thermal break.
7.	Intermediate Reinforcing: Nominal 18 gauge full vertical steel back-up plates, inserted prior to foaming, to provide proper position and reinforcing for attachment of various hardware.
8.	Exterior Finish Coat: Solid colors. Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.
9.	Exterior Finish Coat: Traditional wood grain. 1 mil total dry film, 3-coat system, consisting of an enhanced polyester base coat plus an ink coat and polyester clear coat.
10.	Exterior Finish Coat: Plank wood grain. White base coat plus ink and a polyester clear coat.
11.	Exterior Finish Color: Polar White.
12.	Exterior Finish Color: Almond.
13.	Exterior Finish Color: Bronze.
14.	Exterior Finish Color: Brown.
15.	Exterior Finish Color: Charcoal.
16.	Exterior Finish Color:  Espresso.
17.	Exterior Finish Color:  Gray.
18.	Exterior Finish Color:  Sandstone.
19.	Exterior Finish Color:  Sahara Tan.
20.	Exterior Finish Color: Trinar Beige. 
21.	Exterior Finish Color: Trinar Brown. 
22.	Exterior Finish Color:  Ash.
23.	Exterior Finish Color:  Mahogany.
24.	Exterior Finish Color:  English Oak. 
25.	Exterior Finish Color:  Graywood.
26.	Exterior Finish Bi-Directional Color:  Ash.
27.	Exterior Finish Bi-Directional Color:  Mahogany.
28.	Exterior Finish Bi-Directional Color:  English Oak.
29.	Exterior Finish Color: English Oak Plank. 
30.	Exterior Finish Color: Cedar Plank. 
31.	Exterior Finish Color: American Walnut. 
32.	Exterior Finish Bi-Directional Color: American Walnut. 
33.	Exterior Finish Color: American Walnut Plank. 
34.	Exterior Finish Color: Carbon Black.
35.	Interior Finish Coat: Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish. 
a.	Color: Polar White.
36.	Provide the following assembly components:
a.	Cam safety device.
b.	Pass door.
37.	Windows:
a.	Window Design:
1)	Window Design: Carriage House Series Windows.
2)	Window Design: Ranch Series Windows.
3)	Window Design: Standard Series Windows.
4)	Window Design: SlimLine Windows. 
5)	Window Design: Double SlimLine Windows. 
6)	Window Design:  25 x 12 inches (635 x 305 mm) TL windows.
7)	Window Design:  24 x 6 inches (610 x 152 mm) TL windows.
b.	Glazing Types:
1)	Glass: 1/8 Inch (3 mm): 
a)	Clear Tempered.
b)	Frosted Tempered.
c)	Bronze Tempered.
d)	Dark Gray Tempered.
e)	Clear Polycarbonate (Lexan). 
f)	Light Gray Tempered.
g)	Obscure Pattern 62.
h)	Rain Tempered. 
2)	Glass: 3/16 Inch (4 mm):	 
a)	Arctic Tempered. 
b)	Reed Tempered. 
3)	Glass: 1/4 Inch (6 mm):
a)	Hurricane Impact Resistant Clear Polycarbonate.
b)	Hurricane Impact Resistant Bronze Polycarbonate.
c)	Hurricane Impact Resistant Dark Gray Polycarbonate.
d)	Hurricane Impact Resistant Pebble Polycarbonate.
e)	Hurricane Impact Resistant Frosted Polycarbonate. 
4)	Glass: 1/2 Inch (12 mm) Insulated:
a)	Clear Tempered.
b)	Frosted over Clear Tempered.
c)	Bronze over Clear Tempered.
d)	Bronze over Frosted Tempered.
e)	Dark Gray over Clear Tempered.
f)	Dark Gray over Frosted Tempered.
g)	Dark Gray over Dark Gray Tempered.
h)	Light Gray over Clear Tempered.
i)	Light Gray over Frosted Tempered. 
j)	Rain over Clear Tempered. 
k)	Rain over Frosted Tempered. 
l)	Arctic over Clear Tempered. 
m)	Arctic over Frosted Tempered. 
n)	Reed over Clear Tempered. 
o)	Reed over Frosted Tempered. 
p)	Low E - Standard Clear Tempered.
q)	Obscure Pattern 62 over Clear Tempered.
r)	Obscure Pattern 62 over Frosted Tempered. 
s)	SolarShield Tempered. 
t)	Translucent Mirror. 
38.	Full Vision Sections:
a.	Framing: Sections will be 1.75 inches (44.5 mm) thick full tubular aluminum framework with 0.125 inch (3.18 mm) wall thickness wherever hardware attaches. Vertical stiles and horizontal rails will be assembled using internal steel thru-bolts.
b.	Glazing Types: 
1)	Glass: 1/8 Inch (3 mm): 
a)	Clear Tempered.
b)	Frosted Tempered.
c)	Bronze Tempered.
d)	Dark Gray Tempered.
e)	Light Gray Tempered.
f)	Obscure Pattern 62.
g)	Rain Tempered. 
h)	Clear Acrylic (Plexiglass).
i)	Clear Polycarbonate (Lexan).
2)	Glass: 3/16 Inch (4 mm):  	 
a)	Arctic Tempered. 
b)	Reed Tempered. 
3)	Glass: 1/4 Inch (6 mm):
a)	Clear Tempered.
b)	Frosted Tempered.
c)	Bronze Tempered.
d)	Dark Gray Tempered.
e)	Light Gray Tempered.
f)	Clear Laminated.
g)	Reflective Bronze.
h)	Clear Acrylic (Plexiglass).
i)	Clear Polycarbonate (Lexan).
j)	Wire.
4)	Glass: 1/2 Inch (12 mm) Insulated:
a)	Clear Tempered.
b)	Frosted over Clear Tempered.
c)	Bronze over Clear Tempered.
d)	Bronze over Frosted Tempered.
e)	Dark Gray over Clear Tempered.
f)	Dark Gray over Frosted Tempered.
g)	Dark Gray over Dark Gray Tempered.
h)	Light Gray over Clear Tempered.
i)	Light Gray over Frosted Tempered. 
j)	Rain over Clear Tempered. 
k)	Rain over Frosted Tempered.
l)	Low E - Standard Clear Tempered.
m)	Low E - Tinted Light Gray Tempered.
n)	Low E - Tinted Dark Gray Tempered. 
o)	Low E - Tinted Bronze Tempered. 
p)	SolarShield w/ Argon Gas Tempered. 
q)	Obscure Pattern 62 over Clear Tempered.
r)	Obscure Pattern 62 over Frosted Tempered. 
s)	Translucent Mirror.
c.	Glazing: Set in a continuous glazing sealant and held in place by inside vinyl snap-in glazing bead.
L.	Insulated Steel Sectional Door - CHT-600 Series as manufactured by Haas Door Co.
1.	Application:  Residential. 
2.	Application:  Commercial. 
3.	Construction: 
a.	Sections: 1-3/8 inches (34.9 mm) thick roll formed inside and outside, hot-dipped galvanized steel, insulated with high density polyurethane foam. 
b.	Thermal Break: Full tongue-and-groove thermal break construction with rigid vinyl extrusions.
c.	Material: Hot-dipped galvanized steel (ASTM A-653).
1)	Gauge: 26 gauge woodgrain texture exterior and 26 gauge woodgrain texture interior.
2)	Gauge: 20 gauge smooth exterior and 26 gauge woodgrain interior.
3)	Gauge: 20 gauge smooth exterior and 20 gauge smooth interior.
d.	Exterior Panel Design:
1)	Exterior Panel Design: Flush.
2)	Exterior Panel Design: V-groove on 3 inch centers.
3)	Exterior Panel Design: Standard Raised Panel with shadow lines.
4)	Exterior Panel Design: Ranch Raised Panel with shadow lines.
5)	Exterior Panel Design: Short Ribbed Panel.
6)	Exterior Panel Design: Short Recessed Panel.
7)	Exterior Panel Design: Long Ribbed Panel.
8)	Exterior Panel Design: Long Recessed Panel.
e.	Interior Design: V-groove on 3 inch centers.
4.	Insulation:  Fully insulated section using high density environmentally compliant polyurethane foam, pressure injected to completely fill the section. ANSI/DASMA TPVP105 tested U-Factor = 0.106.
a.	Fire Rated Foam: Class II fire rated foam.
5.	Doors are built to meet or exceed standards established by ANSI/DASMA 102. 
6.	End Stiles:
a.	Vinyl End Stiles: Integral rigid vinyl to ensure consistent thermal break and provide protection to the foam along with sealing it from excessive air exposure.
b.	Steel End Stile: 16 ga. hot-dipped galvanized steel, installed over vinyl end cap to maintain the thermal break.
7.	Intermediate Reinforcing: Nominal 18 gauge full vertical steel back-up plates, inserted prior to foaming, to provide proper position and reinforcing for attachment of various hardware.
8.	Exterior Finish Coat: Solid colors. Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.
9.	Exterior Finish Coat: Traditional wood grain. 1 mil total dry film, 3-coat system, consisting of an enhanced polyester base coat plus an ink coat and polyester clear coat.
10.	Exterior Finish Coat: Plank wood grain. White base coat plus ink and a polyester clear coat.  
11.	Exterior Finish Color: Polar White.
12.	Exterior Finish Color: Almond.
13.	Exterior Finish Color: Bronze.
14.	Exterior Finish Color: Brown.
15.	Exterior Finish Color: Charcoal.
16.	Exterior Finish Color:  Espresso.
17.	Exterior Finish Color:  Gray.
18.	Exterior Finish Color:  Sandstone.
19.	Exterior Finish Color:  Sahara Tan.
20.	Exterior Finish Color: Trinar Beige. 
21.	Exterior Finish Color: Trinar Brown. 
22.	Exterior Finish Color:  Ash.
23.	Exterior Finish Color:  Mahogany.
24.	Exterior Finish Color:  English Oak.
25.	Exterior Finish Color:  Graywood.
26.	Exterior Finish Bi-Directional Color:  Ash.
27.	Exterior Finish Bi-Directional Color:  Mahogany.
28.	Exterior Finish Bi-Directional Color:  English Oak.
29.	Exterior Finish Bi-Directional Color: English Oak Plank. 
30.	Exterior Finish Color: Cedar Plank. 
31.	Exterior Finish Color: American Walnut. 
32.	Exterior Finish Bi-Directional Color: American Walnut. 
33.	Exterior Finish Color: American Walnut Plank. 
34.	Exterior Finish Color: Carbon Black.
35.	Interior Finish Coat: Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish. 
a.	Color: Polar White.
36.	Provide the following assembly components:
a.	Cam Safety Device.
37.	Windows:
a.	Window Design:
1)	Window Design: Carriage House Series Windows.
2)	Window Design: Ranch Series Windows.
3)	Window Design: Standard Series Windows.
4)	Window Design: SlimLine Windows. 
5)	Window Design: Double SlimLine Windows. 
6)	Window Design:  25 x 12 inches (635 x 305 mm) TL windows.
7)	Window Design:  24 x 6 inches (610 x 152 mm) TL windows.
b.	Glazing Types:
1)	Glass: 1/8 Inch (3 mm):
a)	Clear Tempered.
b)	Frosted Tempered.
c)	Bronze Tempered.
d)	Dark Gray Tempered.
e)	Clear Polycarbonate (Lexan). 
f)	Light Gray Tempered.
g)	Obscure Pattern 62.
h)	Rain Tempered. 
2)	Glass: 3/16 Inch (4 mm):	 
a)	Arctic Tempered. 
b)	Reed Tempered. 
3)	Glass: 1/4 Inch (6 mm):
a)	Hurricane Impact Resistant Clear Polycarbonate.
b)	Hurricane Impact Resistant Bronze Polycarbonate.
c)	Hurricane Impact Resistant Dark Gray Polycarbonate.
d)	Hurricane Impact Resistant Pebble Polycarbonate.
e)	Hurricane Impact Resistant Frosted Polycarbonate. 
4)	Glass: 1/2 Inch (12 mm) Insulated:
a)	Clear Tempered.
b)	Frosted over Clear Tempered.
c)	Bronze over Clear Tempered.
d)	Bronze over Frosted Tempered.
e)	Dark Gray over Clear Tempered.
f)	Dark Gray over Frosted Tempered.
g)	Dark Gray over Dark Gray Tempered.
h)	Light Gray over Clear Tempered.
i)	Light Gray over Frosted Tempered. 
j)	Rain over Clear Tempered. 
k)	Rain over Frosted Tempered. 
l)	Arctic over Clear Tempered. 
m)	Arctic over Frosted Tempered. 
n)	Reed over Clear Tempered. 
o)	Reed over Frosted Tempered. 
p)	Low E - Standard Clear Tempered.
q)	Obscure Pattern 62 over Clear Tempered. 
r)	Obscure Pattern 62 over Frosted Tempered. 
s)	SolarShield Tempered.
t)	Translucent Mirror.
M.	Commercial Ribbed Steel Garage Door - C2000 series as manufactured by Haas Door Co.
1.	Application:  Commercial. 
2.	Construction: 
a.	Sections: 2 inches (50.8 mm) thick roll formed hot-dipped galvanized steel.
b.	Material: Hot-dipped galvanized steel (ASTM A-653).
1)	Gauge: 20 gauge smooth ribbed exterior.
2)	Gauge: 24 gauge smooth ribbed exterior.
3)	Gauge: 24 gauge nominal smooth ribbed exterior.
c.	Provide interior thermal insulation panels.
1)	Laminated matt back
2)	26 gauge smooth steel back
d.	Stiles: ' C'-shaped galvanized steel pre-punched for hinge and reinforcing strut attachment.
1)	18 gauge.
2)	16 gauge.
3.	Doors are built to meet or exceed standards established by ANSI/DASMA 102. 
4.	Exterior Finish Coat: Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.
a.	Color: Polar White.
b.	Color: Brown.
c.	Color: Sandstone.
d.	Color: Carbon Black. 
5.	Interior Finish Coat: Two-coat finish painting process consisting of a bake-on urethane primer and a baked polyester finish. 
a.	Color: Polar White.
6.	Provide the following assembly components:
a.	Cam Safety Device.
7.	Windows:
a.	Window Design:
1)	Window Design:  24 x 12 inches (610 x 305 mm) windows.
2)	Window Design: 24 x 6 inches (610 x 152 mm) windows.
b.	Glazing Types:
1)	Glass: 1/8 inch (3 mm)  tempered glass. (non-insulated sections)
a)	Clear Tempered. 
b)	Frosted Tempered.
2)	Glass: 1/2 Inch (13 mm)  insulated tempered. (insulated sections)
a)	Clear Tempered. 
b)	Frosted over Clear Tempered. 
8.	Full Vision Sections:
a.	Framing: Sections will be 1.75 inches (44.5 mm) thick full tubular aluminum framework with 0.125 inch (3.18 mm) wall thickness wherever hardware attaches.  Vertical stiles and horizontal rails will be assembled using internal steel thru-bolts.
b.	Glazing Types: 
1)	Glass: 1/8 Inch (3 mm):
a)	Clear Tempered.
b)	Frosted Tempered.
c)	Bronze Tempered.
d)	Dark Gray Tempered.
e)	Light Gray Tempered.
f)	Obscure Pattern 62.
g)	Rain Tempered. 
h)	Clear Acrylic (Plexiglass).
i)	Clear Polycarbonate (Lexan).
2)	Glass: 3/16 Inch (4 mm):	 
a)	Arctic Tempered. 
b)	Reed Tempered. 
3)	Glass: 1/4 Inch (6 mm):
a)	Clear Tempered.
b)	Frosted Tempered.
c)	Bronze Tempered.
d)	Dark Gray Tempered.
e)	Light Gray Tempered.
f)	Clear Laminated.
g)	Reflective Bronze.
h)	Clear Acrylic (Plexiglass).
i)	Clear Polycarbonate (Lexan).
j)	Wire.
k)	Hurricane Impact Resistant Clear Polycarbonate.
l)	Hurricane Impact Resistant Bronze Polycarbonate.
m)	Hurricane Impact Resistant Dark Gray Polycarbonate.
n)	Hurricane Impact Resistant Pebble Polycarbonate.
o)	Hurricane Impact Resistant Frosted Polycarbonate. 
4)	Glass: 1/2 Inch (12 mm) Insulated:
a)	Clear Tempered.
b)	Frosted over Clear Tempered.
c)	Bronze over Clear Tempered.
d)	Bronze over Frosted Tempered.
e)	Dark Gray over Clear Tempered.
f)	Dark Gray over Frosted Tempered.
g)	Dark Gray over Dark Gray Tempered.
h)	Light Gray over Clear Tempered.
i)	Light Gray over Frosted Tempered. 
j)	Rain over Clear Tempered. 
k)	Rain over Frosted Tempered.
l)	Low E - Standard Clear Tempered.
m)	Low E - Tinted Light Gray Tempered.
n)	Low E - Tinted Dark Gray Tempered. 
o)	Low E - Tinted Bronze Tempered.
p)	SolarShield w/ Argon Gas Tempered. 
q)	Obscure Pattern 62 over Clear Tempered.
r)	Obscure Pattern 62 over Frosted Tempered. 
s)	Translucent Mirror.
c.	Glazing: Set in a continuous glazing sealant and held in place by inside vinyl snap-in glazing bead.
N.	Steel Stamped Panel Pan Garage Door - 2400 and 2500 series as manufactured by Haas Door Co.
1.	Application:  Residential. 
2.	Application:  Commercial. 
3.	Construction: 
a.	Sections: 2 inches (50.8 mm) thick roll formed hot-dipped galvanized steel.
b.	Material: Hot-dipped galvanized steel (ASTM A-653).
1)	Gauge for 2400 Series:  24 gauge woodgrain texture exterior.
2)	Gauge for 2500 Series:  24 gauge nominal woodgrain texture exterior.
c.	Insulated Panels:  Provide interior thermal insulation panels to provide an ANSI/DASMA TPVP105 tested U-Factor of 0.231.
d.	Stiles: 'C'-shaped galvanized steel pre-punched for hinge and reinforcing strut attachment.
1)	20 gauge.
2)	18 gauge.
3)	16 gauge.
4.	Exterior Panel Design:
a.	Exterior Panel Design: Flush. 
b.	Exterior Panel Design: Standard Raised panel with shadow lines. 
c.	Exterior Panel Design: Ranch Raised Panel with shadow lines. 
d.	Exterior Panel Design: Short Ribbed Panel. 
e.	Exterior Panel Design: Short Recessed Panel. 
5.	Doors are built to meet or exceed standards established by ANSI/DASMA 102. 
6.	Exterior Finish Coat: Solid colors. Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.
7.	Exterior Finish Coat: Traditional wood grain. 1 mil total dry film, 3-coat system, consisting of an enhanced polyester base coat plus an ink coat and polyester clear coat.
8.	Exterior Finish Color: Polar White.
9.	Exterior Finish Color: Almond.
10.	Exterior Finish Color: Brown.
11.	Exterior Finish Color: Charcoal.
12.	Exterior Finish Color: Sandstone.
13.	Exterior Finish Color:  Sahara Tan. 
14.	Exterior Finish Color: Carbon Black. 
15.	Exterior Finish Color: Espresso. 
16.	Exterior Finish Premium Color:  English Oak. 
17.	Interior Finish Coat: Two-coat finish painting process consisting of a bake-on urethane primer and a baked polyester finish. 
a.	Color: Polar White.
18.	Provide the following assembly components:
a.	Cam Safety Device.
19.	Windows:
a.	Window Design:  
1)	Window Design: Carriage House Series Windows.
2)	Window Design: Ranch Series Windows.
3)	Window Design: Standard Series Windows.
b.	Glazing Type:
1)	Glass: 1/8 Inch (3 mm): 
a)	Clear Tempered.
b)	Frosted Tempered.
c)	Bronze Tempered.
d)	Dark Gray Tempered.
e)	Clear Polycarbonate (Lexan). 
f)	Light Gray Tempered.
g)	Obscure Pattern 62.
h)	Rain Tempered. 
2)	Glass: 3/16 Inch (4 mm):	 
a)	Arctic Tempered. 
b)	Reed Tempered. 
20.	Full Vision Sections:
a.	Framing: Sections will be 1.75 inches (44.5 mm) thick full tubular aluminum framework with 0.125 inch (3.18 mm) wall thickness wherever hardware attaches.  Vertical stiles and horizontal rails will be assembled using internal steel thru-bolts.
b.	Glazing Types: 
1)	Glass: 1/8 Inch (3 mm):
a)	Clear Tempered.
b)	Frosted Tempered.
c)	Bronze Tempered.
d)	Dark Gray Tempered.
e)	Light Gray Tempered.
f)	Obscure Pattern 62.
g)	Rain Tempered. 
h)	Clear Acrylic (Plexiglass).
i)	Clear Polycarbonate (Lexan).
2)	Glass: 3/16 Inch (4 mm):	 
a)	Arctic Tempered. 
b)	Reed Tempered. 
3)	Glass: 1/4 Inch (6 mm):
a)	Clear Tempered.
b)	Frosted Tempered.
c)	Bronze Tempered.
d)	Dark Gray Tempered.
e)	Light Gray Tempered.
f)	Clear Laminated.
g)	Reflective Bronze.
h)	Clear Acrylic (Plexiglass).
i)	Clear Polycarbonate (Lexan).
j)	Wire.
k)	Hurricane Impact Resistant Clear Polycarbonate.
l)	Hurricane Impact Resistant Bronze Polycarbonate.
m)	Hurricane Impact Resistant Dark Gray Polycarbonate.
n)	Hurricane Impact Resistant Pebble Polycarbonate.
o)	Hurricane Impact Resistant Frosted Polycarbonate. 
4)	Glass: 1/2 Inch (12 mm) Insulated:
a)	Clear Tempered.
b)	Frosted over Clear Tempered.
c)	Bronze over Clear Tempered.
d)	Bronze over Frosted Tempered.
e)	Dark Gray over Clear Tempered.
f)	Dark Gray over Frosted Tempered.
g)	Dark Gray over Dark Gray Tempered.
h)	Light Gray over Clear Tempered.
i)	Light Gray over Frosted Tempered. 
j)	Rain over Clear Tempered. 
k)	Rain over Frosted Tempered.
l)	Low E - Standard Clear Tempered.
m)	Low E - Tinted Light Gray Tempered.
n)	Low E - Tinted Dark Gray Tempered. 
o)	Low E - Tinted Bronze Tempered. 
p)	SolarShield w/ Argon Gas Tempered. 
q)	Obscure Pattern 62 over Clear Tempered.
r)	Obscure Pattern 62 over Frosted Tempered. 
s)	Translucent Mirror.
c.	Glazing: Set in a continuous glazing sealant and held in place by inside vinyl snap-in glazing bead.
O.	Overlay Carriage House Garage Door - American Tradition 9200 Series as manufactured by Haas Door Co.
1.	Application:  Residential. 
2.	Application:  Commercial. 
3.	Construction: 
a.	Sections: 2-5/8 inches (51 mm) thick roll formed inside and outside, hot-dipped galvanized steel, insulated with high density polyurethane foam.
b.	Overlay: 5/8 inch (15.9 mm) textured high density polyurethane boards glued and pinned to the section.
c.	Thermal Break: Full tongue-and-groove thermal break construction with rigid vinyl extrusions.
d.	Material: Hot-dipped galvanized steel (ASTM A-653).
1)	Gauge: 26 gauge woodgrain texture exterior and 26 gauge woodgrain texture interior.
4.	Insulation:  Fully insulated section using high density environmentally compliant polyurethane foam, pressure injected to completely fill the section. ANSI/DASMA TPVP105 tested U-Factor = 0.081.
a.	Fire Rated Foam: Class II fire rated foam.
5.	Performance: Doors shall meet the ASHRAE Standard 90.1 specification for wind infiltration, specifically for sectional garage doors described in Addendum O.
6.	Doors are built to meet or exceed standards established by ANSI/DASMA 102.
7.	End Stiles:
a.	Vinyl End Stiles: Integral rigid vinyl to ensure consistent thermal break and provide protection to the foam along with sealing it from excessive air exposure.
b.	Steel End Stile: 16 ga. hot-dipped galvanized steel, installed over vinyl end cap to maintain the thermal break.
8.	Intermediate Reinforcing: Nominal 18 gauge full vertical steel back-up plates, inserted prior to foaming, to provide proper position and reinforcing for attachment of various hardware.
9.	Exterior Finish Coat: Solid Colors. Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.
10.	Exterior Finish Coat: Traditional Wood Grain. 1 mil total dry film, 3-coat system, consisting of an enhanced polyester base coat plus an ink coat and polyester clear coat.
11.	Exterior Finish Base Color: Polar White.
12.	Exterior Finish Base Color: Almond.
13.	Exterior Finish Base Color: Bronze.
14.	Exterior Finish Base Color: Brown.
15.	Exterior Finish Base Color: Charcoal.
16.	Exterior Finish Base Color:  Espresso.
17.	Exterior Finish Base Color:  Gray.
18.	Exterior Finish Base Color:  Sandstone.
19.	Exterior Finish Base Color:  Sahara Tan.
20.	Exterior Finish Base Color: Trinar Beige. 
21.	Exterior Finish Base Color: Trinar Brown. 
22.	Exterior Finish Base Color: Graywood.
23.	Exterior Finish Base Color:  Ash.
24.	Exterior Finish Base Color:  Mahogany.
25.	Exterior Finish Base Color:  English Oak.
26.	Exterior Finish Base Color: American Walnut. 
27.	Exterior Finish Base Color: Carbon Black.
28.	Overlay Color: Polar White.
29.	Overlay Color: Almond.
30.	Overlay Color: Bronze.
31.	Overlay Color: Brown.
32.	Overlay Color: Charcoal.
33.	Overlay Color:  Espresso.
34.	Overlay Color:  Gray.
35.	Overlay Color:  Sandstone.
36.	Overlay Color:  Sahara Tan.
37.	Overlay Color: Trinar Beige. 
38.	Overlay Color: Trinar Brown. 
39.	Overlay Color:  Ash.
40.	Overlay Color:  Mahogany.
41.	Overlay Color:  English Oak.  
42.	Overlay Color:  Graywood.
43.	Overlay Color: American Walnut. 
44.	Overlay Color: Carbon Black.
45.	Interior Finish Coat: Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish. 
a.	Color: Polar White.
46.	Top Section Design:
a.	Top Section Design: Solid Rectangle top.
b.	Top Section Design: Solid Arch top.
c.	Top Section Design: Glazed Rectangle top.
d.	Top Section Design: Glazed Arch top.
47.	Glazed Top Design:
a.	Glazed Top Design: Plain Top. 
b.	Glazed Top Design: 3-Pane Top.
c.	Glazed Top Design: 4-Pane Top.
d.	Glazed Top Design: 6-Pane Top.
e.	Glazed Top Design: 8-Pane Top.
48.	Glazing Types:
a.	Glass: 1/4 Inch (6 mm):
1)	Hurricane Impact Resistant Clear Polycarbonate.
2)	Hurricane Impact Resistant Bronze Polycarbonate.
3)	Hurricane Impact Resistant Dark Gray Polycarbonate.
4)	Hurricane Impact Resistant Pebble Polycarbonate.
5)	Hurricane Impact Resistant Frosted Polycarbonate.
b.	Glass: 1/2 Inch (12 mm) Insulated:
1)	Clear Tempered.
2)	Frosted over Clear Tempered.
3)	Bronze over Clear Tempered.
4)	Bronze over Frosted Tempered.
5)	Dark Gray over Clear Tempered.
6)	Dark Gray over Frosted Tempered.
7)	Dark Gray over Dark Gray Tempered.
8)	Light Gray over Clear Tempered.
9)	Light Gray over Frosted Tempered. 
10)	Rain over Clear Tempered. 
11)	Rain over Frosted Tempered. 
12)	Arctic over Clear Tempered. 
13)	Arctic over Frosted Tempered. 
14)	Reed over Clear Tempered. 
15)	Reed over Frosted Tempered. 
16)	Low E - Standard Clear Tempered.
17)	Obscure Pattern 62 over Clear Tempered. 
18)	Obscure Pattern 62 over Frosted Tempered. 
19)	SolarShield Tempered.
20)	Translucent Mirror.
P.	Overlay Carriage House Garage Door - American Tradition 9600 Series as manufactured by Haas Door Co.
1.	Application:  Residential.  
2.	Application:  Commercial.  
3.	Construction:
a.	Sections:  2 inches (51 mm) thick roll formed inside and outside, hot-dipped galvanized steel, insulated with high density polyurethane foam. 
b.	Overlay:  5/8 inch (15.9 mm) textured high density polyurethane boards glued and pinned to the section. 
c.	Thermal Break:  Full tongue-and-groove thermal break construction with rigid vinyl extrusions. 
d.	Material:  Hot-dipped galvanized steel (ASTM A-653). 
1)	Gauge:  26 gauge woodgrain texture exterior and 26 gauge woodgrain texture interior.
4.	Insulation:  Fully insulated section using high density environmentally compliant polyurethane foam, pressure injected to completely fill the section. ANSI/DASMA TPVP105 tested U-Factor = 0.96.
a.	Fire Rated Foam:  Class II fire rated foam. 
5.	Doors are built to meet or exceed standards established by ANSI/DASMA 102.
6.	End Stiles: 
a.	Vinyl End Stiles:  Integral rigid vinyl to ensure consistent thermal break and provide protection to the foam along with sealing it from excessive air exposure. 
b.	Steel End Stile:  16 ga. hot-dipped galvanized steel, installed over vinyl end cap to maintain the thermal break. 
7.	Intermediate Reinforcing:  Nominal 18 gauge full vertical steel back-up plates, inserted prior to foaming, to provide proper position and reinforcing for attachment of various hardware. 
8.	Exterior Finish Coat: Solid Colors. Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.
9.	Exterior Finish Coat: Traditional Wood Grain. 1 mil total dry film, 3-coat system, consisting of an enhanced polyester base coat plus an ink coat and polyester clear coat.
10.	Exterior Finish Base Color:  Polar White. 
11.	Exterior Finish Base Color:  Almond. 
12.	Exterior Finish Base Color:  Bronze. 
13.	Exterior Finish Base Color:  Brown. 
14.	Exterior Finish Base Color:  Charcoal. 
15.	Exterior Finish Base Color:  Espresso.
16.	Exterior Finish Base Color:  Gray. 
17.	Exterior Finish Base Color:  Sandstone.  
18.	Exterior Finish Base Color:  Sahara Tan.
19.	Exterior Finish Base Color: Trinar Beige. 
20.	Exterior Finish Base Color: Trinar Brown. 
21.	Exterior Finish Base Color: Graywood.
22.	Exterior Finish Base Color:  Ash. 
23.	Exterior Finish Base Color:  Mahogany. 
24.	Exterior Finish Base Color:  English Oak.
25.	Exterior Finish Base Color: American Walnut. 
26.	Exterior Finish Base Color:  Carbon Black.
27.	Overlay Color:  Polar White. 
28.	Overlay Color:  Almond. 
29.	Overlay Color:  Bronze. 
30.	Overlay Color:  Brown. 
31.	Overlay Color:  Charcoal. 
32.	Overlay Color:  Espresso.
33.	Overlay Color:  Gray. 
34.	Overlay Color:  Sandstone. 
35.	Overlay Color:  Sahara Tan.
36.	Overlay Color: Trinar Beige. 
37.	Overlay Color: Trinar Brown. 
38.	Overlay Color: Ash. 
39.	Overlay Color:  Mahogany. 
40.	Overlay Color:  English Oak.  
41.	Overlay Color:  Graywood. 
42.	Overlay Color: American Walnut. 
43.	Overlay Color:  Carbon Black.
44.	Interior Finish Coat:  Two-coat finish 1.0 mil total thickness painting process consisting of a bake-on urethane primer and a baked polyester finish.  
a.	Color:  Polar White. 
45.	Top Section Design: 
a.	Top Section Design:  Solid Rectangle top. 
b.	Top Section Design:  Solid Arch top. 
c.	Top Section Design:  Glazed Rectangle top. 
d.	Top Section Design:  Glazed Arch top. 
46.	Glazed Top Design: 
a.	Glazed Top Design: Plain Top. 
b.	Glazed Top Design:  3-Pane Top. 
c.	Glazed Top Design:  4-Pane Top. 
d.	Glazed Top Design:  6-Pane Top. 
e.	Glazed Top Design:  8-Pane Top. 
47.	Glazing Types: 
a.	Glass:  1/8 Inch (3 mm): 
1)	Clear Tempered. 
2)	Frosted Tempered. 
3)	Bronze Tempered. 
4)	Dark Gray Tempered. 
5)	Clear Polycarbonate (Lexan). 
6)	Light Gray Tempered. 
7)	Obscure Pattern 62. 
8)	Rain Tempered. 
b.	Glass: 3/16 Inch (4 mm):	 
1)	Arctic Tempered. 
2)	Reed Tempered. 
c.	Glass:  1/4 Inch (6 mm): 
1)	Hurricane Impact Resistant Clear Polycarbonate. 
2)	Hurricane Impact Resistant Bronze Polycarbonate. 
3)	Hurricane Impact Resistant Dark Gray Polycarbonate. 
4)	Hurricane Impact Resistant Pebble Polycarbonate. 
5)	Hurricane Impact Resistant Frosted Polycarbonate. 
d.	Glass:  1/2 Inch (12 mm) Insulated: 
1)	Clear Tempered. 
2)	Frosted over Clear Tempered. 
3)	Bronze over Clear Tempered. 
4)	Bronze over Frosted Tempered. 
5)	Dark Gray over Clear Tempered. 
6)	Dark Gray over Frosted Tempered. 
7)	Dark Gray over Dark Gray Tempered. 
8)	Light Gray over Clear Tempered. 
9)	Light Gray over Frosted Tempered. 
10)	Rain over Clear Tempered. 
11)	Rain over Frosted Tempered. 
12)	Arctic over Clear Tempered. 
13)	Arctic over Frosted Tempered. 
14)	Reed over Clear Tempered. 
15)	Reed over Frosted Tempered. 
16)	Low E - Standard Clear Tempered. 
17)	Obscure Pattern 62 over Clear Tempered. 
18)	Obscure Pattern 62 over Frosted Tempered. 
19)	SolarShield Tempered.
20)	Translucent Mirror.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	General: Install door, track and operating equipment complete with all necessary accessories and hardware according to shop drawings, manufacturer's instructions.
B.	Lubricate bearings and sliding parts, and adjust doors for proper operation, balance, clearance and similar requirements.
3.4	PROTECTION
A.	Clean installed products in accordance with manufacturer's instructions prior to Owner's acceptance. Remove and legally dispose of construction debris from project site.
B.	Remove temporary coverings and protection of adjacent work areas. Repair or replace installed products damaged prior to or during installation.
C.	Lubricate bearings and sliding parts, assure weather tight fit around door perimeter and adjust doors for proper operation, balance, clearance and similar requirements. Protect installed products until completion of project.
D.	Touch-up, repair or replace damaged products before Substantial Completion.
3.5	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION