SECTION 05 73 00

CABLE RAILING SYSTEMS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2011 -  2025 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Stainless steel cable railing system.
B.	Pre-engineered railing system.
1.2	RELATED SECTIONS
A.	Section 03 30 00 - Cast-in-Place Concrete.
B.	Section 05 51 00 - Metal Stairs.
C.	Section 05 52 17 - Roof Fall Protection.
D.	Section 05 71 00 - Decorative Metal Stairs.
E.	Section 06 40 00 - Architectural Woodwork.
1.3	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
4.	Cleaning and maintenance instructions.
C.	Shop Drawings: Provide shop drawings indicating details of construction, installation and relationships to adjacent construction. Shop drawings shall be stamped by a professional engineer licensed in the jurisdiction of the project.
D.	Selection Samples: Submit two sets of samples showing available finishes and configurations.
E.	Verification Samples: For each product specified, two samples, representing actual finishes and configurations specified.
1.4	QUALITY ASSURANCE
A.	Single Source: To the greatest extent possible obtain components for railing systems from single manufacturer.
1.5	DELIVERY, STORAGE AND HANDLING
A.	Deliver, store and handle materials and products in strict compliance with manufacturer's instructions and recommendations and industry standards. Protect from damage.
B.	Store products in manufacturer's labeled packaging until ready for installation.
1.6	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
1.7	SEQUENCING AND SCHEDULING
A.	Conference: Convene a pre-installation conference to establish procedures to maintain optimum working conditions and to coordinate this work with related and adjacent work.
1.8	WARRANTY 
A.	Manufacturer's standard limited lifetime warranty for defects in materials.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Hayn Enterprises, LLC, which is located at:<BR />51 Inwood Rd.<BR />Rocky Hill, CT 06067<BR />Toll Free Tel: 800-346-4296<BR />Tel: 860-257-0680<BR />Fax: 860-257-0683<BR />Email: request info (sales@hayn.com);Web: https://hayn.com/lines | https://hayn.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	STAINLESS STEEL CABLE RAILING SYSTEMS
A.	Toggle Jaw Stainless Steel Cable Railing Systems: As manufactured by Hayn Enterprises, LLC.
1.	General: Cable, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
2.	Material: 316 stainless steel.
3.	Stainless Steel Cable: 1x19, Item no. ______.
4.	Stainless Steel Cable: 7x19, Item no. ______.
5.	Stainless Steel Cable: 7x7, Item no. ______.
6.	Stainless Steel Cable: Vinyl coated, 7x7, Item no. ______.
7.	Toggle Jaw Turnbuckles: Tubular style bodies.
a.	Jaw To Swage Style Turnbuckles: Item no. ______.
b.	Jaw To Hayn Grip Style Turnbuckles: Item no. ______.
c.	Jaw To Handy Crimp Style Turnbuckles: Item no. ______.
8.	Toggle Jaws:
a.	Swage Style Toggle Jaws: Item no. ______.
b.	Hayn Grip Style Toggle Jaws: Item no. ______
c.	Handy Crimp Style Toggle Jaws: Item no. ______.
9.	Inline Turnbuckles: Tubular style bodies.
a.	Swage To Swage Style Turnbuckles: Item no. ______.
b.	Hayn Grip to Hayn Grip Style Turnbuckles: Item no. ______.
c.	Handy Crimp To Handy Crimp Style Turnbuckles: Item no. ______.
10.	Weld-On Loops for Toggle Jaws: Item no. WL
11.	Eye Bolts: Welded, Item no. ______.
12.	Eye Lags: Welded, Item no. ______.
B.	Termination Stud Stainless Steel Cable Railing Systems: As manufactured by Hayn Enterprises, LLC.
1.	General: Cable, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
2.	Material: 316 stainless steel.
3.	Stainless Steel Cable: 1x19, Item no. ______.
4.	Stainless Steel Cable: 7x19, Item no. ______.
5.	Stainless Steel Cable: 7x7, Item no. ______.
6.	Stainless Steel Cable: Vinyl coated, 7x7, Item no. ______.
7.	Termination Stud Turnbuckles: Tubular style bodies.
a.	Swage Style Termination Stud Turnbuckles: Item no. ______.
b.	Hayn Grip Style Termination Stud Turnbuckles: Item no. ______.
c.	Handy Crimp Style Termination Stud Turnbuckles: Item no. ______.
8.	Termination Stud:
a.	Swage Style Termination Studs: Item no. ______.
b.	Hayn Grip Style Termination Studs: Item no._______
c.	Handy Crimp Style Termination Studs: Item no. ______.
9.	Inline Turnbuckles: Tubular style bodies.
a.	Swage To Swage Style Turnbuckles: Item no. ______.
b.	Hayn Grip to Hayn Grip Style Turnbuckles: Item no. ______.
c.	Handy Crimp To Handy Crimp Style Turnbuckles: Item no. ______.
10.	Bevel Washers: Item no. ______.
11.	Adjust-A-Ball Fittings: For use with termination studs, Item no. ______.
C.	Countersunk Termination Stud Stainless Steel Cable Railing Systems: As manufactured by Hayn Enterprises, LLC.
1.	General: Cable, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
2.	Material: 316 stainless steel.
3.	Stainless Steel Cable: 1x19, Item no. ______.
4.	Stainless Steel Cable: 7x19, Item no. ______.
5.	Stainless Steel Cable: 7x7, Item no. ______.
6.	Stainless Steel Cable: Vinyl coated, 7x7, Item no. ______.
7.	Countersunk Termination Stud Turnbuckles: Tubular style bodies.
a.	Swage Style Countersunk Termination Stud Turnbuckles: Item no. ______.
b.	Handy Crimp Style Countersunk Termination Stud Turnbuckles: Item no. ______.
8.	Countersunk Termination Studs:
a.	Swage Style Countersunk Termination Studs: Item no. ______.
1)	Handy Crimp Style Countersunk Termination Studs: Item no. ______.
9.	Countersunk Thread on Top Termination Studs: Item no. CTST14.
10.	Inline Turnbuckles: Tubular style bodies.
a.	Swage To Swage Style Turnbuckles: Item no. ______.
b.	Handy Crimp To Handy Crimp Style Turnbuckles: Item no. ______.
D.	Stud Tensioning Internal Adjuster Stainless Steel Cable Railing Systems: As manufactured by Hayn Enterprises, LLC.
1.	General: Cable, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
2.	Material: 316 stainless steel.
3.	Stainless Steel Cable: 1x19, Item no. ______.
4.	Stainless Steel Cable: 7x19, Item no. ______.
5.	Stainless Steel Cable: 7x7, Item no. ______.
6.	Stainless Steel Cable: Vinyl coated, 7x7, Item no. ______.
7.	Stud Tensioning Internal Adjusters: Assemblies.
a.	Swage Style Stud Tensioning Internal Adjuster Assemblies: Item no. ______.
b.	Hayn Grip Style Stud Tensioning Internal Adjuster Assemblies: Item no. ______.
c.	Handy Crimp Style Stud Tensioning Internal Adjuster Assemblies: Item no. ______.
8.	Stud Tensioning Internal Adjuster: Item no. ______.
9.	Stud Tensioning Internal Adjuster Studs:
a.	Swage Style Studs: Item no. ______.
b.	Hayn Grip Style Studs: Item no. ______.
c.	Handy Crimp Style Studs: Item no. ______.
10.	Bevel Washers: Item no. ______.
11.	Adjust-A-Ball Fittings: For use with termination studs, Item no. ______.
E.	Threaded Stud Stainless Steel Cable Railing Systems: As manufactured by Hayn Enterprises, LLC.
1.	General: Cable, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
2.	Material: 316 stainless steel.
3.	Stainless Steel Cable: 1x19, Item no. ______.
4.	Stainless Steel Cable: 7x19, Item no. ______.
5.	Stainless Steel Cable: 7x7, Item no. ______.
6.	Stainless Steel Cable: Vinyl coated, 7x7, Item no. ______.
7.	Threaded Studs:
a.	Lifeline Studs: Swage Style, Item no. ______.
b.	Lifeline Studs: Hayn Grip Style, Item no. ______.
c.	Lifeline Studs: Swage Style with wrench flats, Item no. ______.
d.	Lifeline Studs: Handy Crimp Style, Item no. ______.
8.	Inline Turnbuckles: Tubular style bodies.
a.	Swage To Swage Style Turnbuckles: Item no. ______.
b.	Hayn Grip to Hayn Grip Style Turnbuckles: Item no. ______.
c.	Handy Crimp To Handy Crimp Style Turnbuckles: Item no. ______.
9.	Bevel Washers: Item no. ______.
10.	Adjust-A-Ball Fittings: For use with threaded stud system, Item no. ______.
11.	Washers:
a.	Material: 18-8 stainless steel.
1)	Flat Washers: Item no. ______.
2)	Lock Washers: Item no. ______.
3)	Fender Washers: Item no. ______.
12.	Nuts:
a.	Material: 18-8 stainless steel.
1)	Hex Nuts: Item no. ______.
2)	Hex Acorn Cap Nuts: Item no. ______.
F.	Deck Toggle-Surface Mount Stainless Steel Cable Railing Systems: As manufactured by Hayn Enterprises, LLC.
1.	General: Cable, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
2.	Material: 316 stainless steel.
3.	Stainless Steel Cable: 1x19, Item no. ______.
4.	Stainless Steel Cable: 7x19, Item no. ______.
5.	Stainless Steel Cable: 7x7, Item no. ______.
6.	Stainless Steel Cable: Vinyl coated, 7x7, Item no. ______.
7.	Deck Toggle Turnbuckles: Tubular style bodies.
a.	Swage Style Deck Toggle Turnbuckles: Item no. ______.
b.	Hayn Grip Style Deck Toggle Turnbuckles: Item no. ______.
c.	Handy Crimp Style Deck Toggle Turnbuckles: Item no. ______.
8.	Deck Toggle Jaws:
a.	Swage Style Deck Toggle Jaws: Item no. ______.
b.	Hayn Grip Style Deck Toggle Jaws: Item no. ______.
c.	Handy Crimp Style Deck Toggle Jaws: Item no. ______.
9.	Inline Turnbuckles: Stainless tubular style bodies.
a.	Swage To Swage Style Turnbuckles: Item no. ______.
b.	Hayn Grip to Hayn Grip Style Turnbuckles: Item no. ______.
c.	Handy Crimp to Handy Crimp Style Turnbuckles: Item no. ______.
10.	Lag Screws: Hex Head Deck Toggle Hardware, Item no. ______.
G.	Threaded Termination Stud Stainless Steel Cable Railing Systems: As manufactured by Hayn Enterprises, LLC.
1.	General: Cable, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
2.	Material: 316 stainless steel.
3.	Stainless Steel Cable: 1x19, Item no. ______.
4.	Stainless Steel Cable: 7x19, Item no. ______.
5.	Stainless Steel Cable: 7x7, Item no. ______.
6.	Stainless Steel Cable: Vinyl coated, 7x7, Item no. ______.
7.	Threaded Termination Stud Turnbuckles: Tubular style bodies.
a.	Swage Style Threaded Termination Stud Turnbuckles: Item no. ______.
b.	Hayn Grip Style Threaded Termination Stud Turnbuckles: Item no._______
c.	Handy Crimp Style Threaded Termination Stud Turnbuckles: Item no. ______.
8.	Threaded Termination Studs:
a.	Swage Style Threaded Termination Studs: Item no. ______.
b.	Hayn Grip Style Threaded Termination Studs: Item no._________
c.	Handy Crimp Style Threaded Termination Studs: Item no. ______.
9.	Termination Stud Thread on Cap: Item no. TST14.
10.	Inline Turnbuckles: Stainless tubular style bodies.
a.	Swage To Swage Style Turnbuckles: Item no. ______.
b.	Hayn Grip to Hayn Grip Style Turnbuckles: Item no. ______.
c.	Handy Crimp to Handy Crimp Style Turnbuckles: Item no. ______.
11.	Bevel Washers: Item no. ______.
12.	Washers:
a.	Material: 18-8 stainless steel.
1)	Flat Washers: Item no. ______.
2)	Lock Washers: Item no. ______.
3)	Fender Washers: Item no. ______.
13.	Dome Nut Fittings: Item no. ______.
14.	Adjust-A-Ball Fittings: For use with threaded termination studs, Item no. ______.
15.	Ball End Fittings: Item no. ______.
16.	Nuts:
a.	Material: 18-8 stainless steel.
1)	Hex Nuts: Item no. ______.
2)	Hex Acorn Cap Nuts: Item no. ______.
H.	Lag System - Surface Mount Stainless Steel Cable Railing Systems: As manufactured by Hayn Enterprises, LLC.
1.	General: Cable, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
2.	Material: 316 stainless steel.
3.	Stainless Steel Cable: 1x19, Item no. ______.
4.	Stainless Steel Cable: 7x19, Item no. ______.
5.	Stainless Steel Cable: 7x7, Item no. ______.
6.	Stainless Steel Cable: Vinyl coated, 7x7, Item no. ______.
7.	Lag Stud Turnbuckles: Tubular style bodies.
a.	Swage Style Lag Stud Turnbuckles: Item no. ______.
b.	Hayn Grip Style Lag Stud Turnbuckles: Item no. ______.
c.	Handy Crimp Style Lag Stud Turnbuckles: Item no. ______.
8.	Lag Studs:
a.	Swage Style Lag Studs: Item no. ______.
b.	Hayn Grip Style Lag Studs: Item no. ______.
c.	Handy Crimp Style Lag Studs: Item no. ______.
9.	Inline Turnbuckles: Stainless tubular style bodies.
a.	Swage To Swage Style Turnbuckles: Item no. ______.
b.	Hayn Grip to Hayn Grip Style Turnbuckles: Item no._________
c.	Handy Crimp To Handy Crimp Style Turnbuckles: Item no. ______.
I.	Trellis Stainless Steel Cable Systems: As manufactured by Hayn Enterprises, LLC.
1.	General: Cable, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
2.	Material: 316 stainless steel.
3.	Stainless Steel Cable: 1x19, Item no. ______.
4.	Stainless Steel Cable: 7x19, Item no. ______.
5.	Stainless Steel Cable: 7x7, Item no. ______.
6.	Stainless Steel Cable: Vinyl coated, 7x7, Item no. ______.
7.	Trellis Posts:
a.	Trellis End Posts: Item no. ______.
b.	Trellis Post Assemblies, Single Stud: Item no. ______.
c.	Trellis Post Assemblies, Double Stud: Item no. ______.
d.	Trellis Post WIDE Support Base: Item no. ______.
e.	Mount Screws - Socket Head Cap Screw: Item no. ______.
f.	Drop In Concrete Anchors: Item no. DIA38.
8.	Threaded Studs:
a.	Lifeline Studs: Swage Style, Item no. ______.
b.	Lifeline Studs: Hayn Grip style, Item no. ______.
c.	Lifeline Studs: Swage Style with wrench flats, Item no. ______.
d.	Lifeline Studs: Handy Crimp Style, Item no. ______.
9.	Trellis Cross Clamps: Item no. ______.
J.	Architectural Adjuster Fork Systems: As manufactured by Hayn Enterprises, LLC.
1.	General: Cable, rod, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
2.	Material: 316 stainless steel.
3.	Stainless Steel Cable: 1x19, Item no. ______.
4.	Stainless Steel Cable: 7x19, Item no. ______.
5.	Stainless Steel Cable: 7x7, Item no. ______.
6.	Stainless Steel Cable: Vinyl coated, 7x7, Item no. ______.
7.	Stainless Steel Rod: 316 Grade, Diameter____________.
8.	Architectural Adjuster Forks: Item no. ______.
9.	Architectural Adjuster Fork Lock Nuts: Item no. ______.
10.	Architectural Adjuster Fork Double Headed Clevis Pin Assemblies: Item no. ______.
11.	Swage Studs - Rigging Style for use with Cable: Item no. ______. 
K.	Hayn Lines Hardware Accessories for Stainless Steel Cable Railing Systems: As manufactured by Hayn Enterprises, LLC.
1.	General: Cable, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
2.	Material: 316 stainless steel.
3.	Stainless Steel Cable: 1x19, Item no. ______.
4.	Stainless Steel Cable: 7x19, Item no. ______.
5.	Stainless Steel Cable: 7x7, Item no. ______.
6.	Stainless Steel Cable: Vinyl coated, 7x7, Item no. ______.
7.	Flush Mount Ball Sockets:
a.	Ball Sockets, Back Mount: No Slots, Item no. BCM6.
b.	Ball Sockets, Back Mount: With Slots, Item no. BCM6-C.
8.	Surface Mount Ball Sockets: Item no. ______.
9.	Forks, Swage Type: Item no. ______.
10.	Wire Rope Clips: Item no. ______.
11.	Thimbles: Item no. ______.
12.	Eye Bolts: Welded, Item no. ______.
13.	Eye Lag Bolts: Welded, Item no. ______.
14.	Lag Screws: Hex head deck toggle hardware, Item no. ______.
15.	Drop In Concrete Anchors: Item no. ______.
16.	Washers:
a.	Material: 18-8 stainless steel.
1)	Flat Washers: Item no. ______.
2)	Lock Washers: Item no. ______.
3)	Fender Washers: Item no. ______.
17.	Nuts:
a.	Material: 18-8 stainless steel.
1)	Hex Nuts: Item no. ______.
2)	Hex Acorn Cap Nuts: Item no. ______.
18.	Bushings:
a.	Material: Nylon
1)	Bushings: Nylon, split, black, Item no. ______.
2)	Bushings: Nylon, split, silver, Item no. ______.
3)	Bushings: Nylon, split, white, Item no. ______.
4)	Bushings: Nylon, split, 31 degree angle, black, Item no. ______.
5)	Bushings: Nylon, split, 31 degree angle, silver, Item no. ______.
6)	Bushings: Nylon, split, 31 degree angle, white, Item no. ______.
19.	Copper Oval Sleeves: Zinc plated, Item no. ______.
20.	Hayn Finishing Wipes: Lint free, Item no. WIPES-CASE.
L.	Hayn Swaging Equipment/Cable Cutting Tools/Dies: As distributed by Hayn Enterprises, LLC.
1.	Swaging Equipment/Cable Cutting Tools:
a.	Nicopress, Handy Crimp Tools: Item no. HCTOOL.
b.	Cable Cutters: Item no. ______.
c.	Top Reff Swagers/Dies: Item no. ______.
1)	Top Reff Swagers: Item no. K50E
2)	Top Reff Dies: Item no. ______.
3)	Top Reff Foot Switch: Item no. K50EFOOTSWITCH
2.	WireTeknik Roll Swagers/Dies/Power Packs:
a.	WireTeknik Roll Swagers: Item no. ______.
b.	Dies For WireTeknik Roll Swagers: Item no. ______.
1)	Hydraulic Power Pack:
2)	Swager Hand Pump: Item no. HYDHANDPUMP.
3)	Air/Hydraulic Power Packs: Item no. ZAP102.
4)	Drill Operated Power Packs: Item no. BDHPP.
2.3	PRE-ENGINEERED RAILING SYSTEMS
A.	Pre-Engineered Cable Railing Systems: System 2000 Series with stainless steel handrails as distributed by Hayn Enterprises, LLC.
1.	General: Cable, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
2.	Materials: 316 stainless steel, #3 brushed finish.
3.	Materials: 304 stainless steel, #3 brushed finish.
4.	Cable Infill: 1/8 inch (3 mm), 3/16 inch (5 mm), or 1/4 inch (6 mm) diameter. 
a.	Stainless Steel Cable: 1x19, Item no. ______.
1)	Stainless Steel Cable: 7x19, Item no. ______.
2)	Stainless Steel Cable: 7x7, Item no. ______.
3)	Stainless Steel Cable: Vinyl coated, 7x7, Item no. ______.
5.	Attachment: 4 inch x 4 inch (102 mm x 102 mm) surface mounted base plate.
6.	Attachment: Core drill. 
7.	Attachment: Fascia mount. 
8.	Attachment: As indicated on Drawings.
9.	Railing System: System 2000 Series, SP1-2000 Square Post / Cable Infill as distributed by Hayn Enterprises, LLC.
a.	Description: Stainless steel construction with 1-1/2 inch (38 mm) square tube posts on 48 inch (1219 mm) centers. 
b.	Railing Height: 36 inches (914 mm).
c.	Railing Height: 42 inches (1067 mm).
d.	Top Cap: 1-1/2 inch (38 mm) diameter tube.
10.	Railing System: System 2000 Series, FB1-2000 Flat Bar Post / Cable Infill as distributed by Hayn Enterprises, LLC.
a.	Description: Stainless steel construction with posts crafted from two 1/2 inch x 1-1/2 inch (13 mm x 38 mm) flat bars welded to one another by 1/2 inch (13 mm) diameter x 1-1/2 inch (38 mm) long tubes. Posts are on 48 inch (1219 mm) centers.
b.	Railing Height: 36 inches (914 mm).
c.	Railing Height: 42 inches (1067 mm).
d.	Top Cap: 1-1/2 inch (38 mm) diameter tube.
11.	Railing System: System 2000 Series, FB3-2000 as distributed by Hayn Enterprises, LLC.
a.	Description: All stainless steel construction, posts are crafted from two 1/2 inch x 1-1/2 inch (13 mm x 38 mm) flat bars welded to one another by a welded tab. Posts on 48 inches (1219 mm) centers.
b.	Railing Height: 36 inches (914 mm).
c.	Railing Height: 42 inches (1067 mm).
d.	Top Cap: 1-1/2 inch (38 mm) diameter tube.
12.	Railing System: System 2000 Series, VC1-2000 as distributed by Hayn Enterprises, LLC.
a.	Description: Stainless steel vertical cable railing system with vertical frame members crafted from 3/4 inch x 2 inch (19 mm x 51 mm) flat bar and horizontal members manufactured from 1-1/2 inch (38 mm) square tube. 
b.	Railing Height: 36 inches (914 mm).
c.	Railing Height: 42 inches (1067 mm).
d.	Top Cap: 2 inch (51 mm) diameter tube.
13.	Railing System: System 2000 Series, SPG1-2000 as distributed by Hayn Enterprises, LLC.
a.	Description: Designed for areas where falling objects are of concern. Crafted from stainless steel and glass; glass panel at bottom to prevent objects from falling to the level below used in conjunction with cabling. Glass paneling is 3/8" thick and typically 10" high. Glass options include clear, smoke, and frosted as well as safety film and graphic film layovers. 
b.	Glass Paneling: 3/8 inch (9.5 mm) thick, ___________ height.
c.	Glass Paneling: 3/8 inch (9.5 mm) thick, 10 inch (254 mm) height.
d.	Glass Type: Clear. 
e.	Glass Type: Smoke.
f.	Glass Type: Frosted. 
g.	Glass Feature: Safety film layovers. 
h.	Glass Feature: Graphic film layovers, as indicated on Drawings. 
i.	Railing Height: 36 inches (914 mm).
j.	Railing Height: 42 inches (1067 mm).
k.	Top Cap: 2 inch (51 mm) diameter tube.
14.	Railing System: System 2000 Series, SPG2-2000 as distributed by Hayn Enterprises, LLC.
a.	Description: Crafted from stainless steel and glass with 1-1/2 inch (38 mm) square tube posts on 48 inches (1219 mm) centers. 
b.	Glass Paneling: 3/8 inch (9.5 mm) thick.
c.	Glass Type: Clear. 
d.	Glass Type: Smoke.
e.	Glass Type: Frosted. 
f.	Glass Feature: Safety film layovers. 
g.	Glass Feature: Graphic film layovers, as indicated on Drawings. 
h.	Railing Height: 36 inches (914 mm).
i.	Railing Height: 42 inches (1067 mm).
j.	Top Cap: 1-1/2 inch (38 mm) diameter tube.
B.	Pre-Engineered Cable Railing Systems: System 2000 Series with aluminum handrails as distributed by Hayn Enterprises, LLC.
1.	Railing System: System 2000 Series, AP1-2000 Aluminum Handrail and Posts / Stainless Steel Cable Infill.
2.	General: Cable, hardware components and accessories as required for complete system installation in accordance with structural requirements and governing codes.
3.	Description: Aluminum powder coated frame and stainless steel cables for infill. 
4.	Powder Coating: ____________.
5.	Powder Coating: As indicated on Drawings.
6.	Vertical Posts: 2-3/8 inch (60 mm) square tube on 48 inch (1219 mm) centers. 
7.	Top Cap: 2 inch x 3-3/4 inch (51 mm x 95 mm) oval. 
8.	Railing Height: 36 inches (914 mm).
9.	Railing Height: 42 inches (1067 mm).
10.	Cable Infill: 1/8 inch (3 mm) diameter 1x19 strand cabling with swage stud adjusters at each end for cable tensioning. 
11.	Attachment: 5 inch x 5 inch (127 mm x 127 mm) surface mounted base plate.
12.	Attachment: Core drill. 
13.	Attachment: Fascia mount. 
14.	Attachment: As indicated on Drawings.
PART 3    EXECUTION
3.1	PREPARATION
A.	If preparation is the responsibility of another installer, notify Architect in writing of deviations from manufacturer's recommended installation tolerances and conditions.
B.	Do not proceed with installation until substrates have been properly prepared and deviations from manufacturer's recommended tolerances are corrected. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions. 
C.	Commencement of installation constitutes acceptance of conditions. 
3.2	INSTALLATION
A.	Install in accordance with manufacturer's written instructions and recommendations. Adjust for proper tension and appearance. Clean with Hayn Lint Free Finishing Wipes.
3.3	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION