SECTION 07 44 00

CEMENTITIOUS PANELS

(HZ5 or HZ10 Hardie Reveal Panels)

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2009 -  2023 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Cementitious express/reveal jointed panel with accessories. (James Hardie HZ5 or HZ10 Hardie Reveal Panels.)
1.2	RELATED SECTIONS
A.	Section 05 40 00 - Cold-Formed Metal Framing.
B.	Section 06 10 00 - Rough Carpentry.
C.	Section 06 10 00 - Rough Carpentry. 
D.	Section 07 21 19 - Foamed-In-Place Insulation.
1.3	REFERENCES
A.	ASTM International (ASTM):
1.	ASTM B136 - Standard Method for Measurement of Stain Resistance of Anodic Coatings on Aluminum.
2.	ASTM B244 - Standard Test Method for Measurement of Thickness of Anodic Coatings on Aluminum and of Other Nonconductive Coatings on Nonmagnetic Basis Metals with Eddy-Current Instruments.
3.	ASTM C834 - Standard Specification for Latex Sealants.
4.	ASTM C920 - Standard Specification for Elastomeric Joint Sealants.
5.	ASTM C1186 - Standard Specification for Flat Non-Asbestos Fiber-Cement Sheets.
6.	ASTM D523 - Standard Test Method for Specular Gloss.
7.	ASTM D1117 - Standard Guide for Evaluating Nonwoven Fabrics.
8.	ASTM D1308 - Standard Test Method for Effect of Household Chemicals on Clear and Pigmented Organic Finishes.
9.	ASTM D1730 - Standard Practices for Preparation of Aluminum and Aluminum-Alloy Surfaces for Painting.
10.	ASTM D2794 - Standard Test Method for Resistance of Organic Coatings to the Effects of Rapid Deformation (Impact).
11.	ASTM D3363 - Standard Test Method for Film Hardness by Pencil Test.
12.	ASTM D3359 - Standard Test Methods for Rating Adhesion by Tape Test.
13.	ASTM D4585 - Standard Practice for Testing Water Resistance of Coatings Using Controlled Condensation.
14.	ASTM E84 - Standard Test Method for Surface Burning Characteristics of Building Materials.
15.	ASTM E96 - Test Methods for Water Vapor Transmission of Materials.
16.	ASTM E119 - Standard Test Methods for Fire Tests of Building Construction and Materials.
17.	ASTM E136 - Standard Test Method for Behavior of Materials in a Vertical Tube Furnace at 750 degrees C.
18.	ASTM E330 - Standard Test Method for Structural Performance of Exterior Windows, Doors, Skylights and Curtain Walls by Uniform Static Air Pressure
B.	AATCC127 - Water Resistance: Hydrostatic Pressure Test.
C.	TAPPI - T460 - Air Resistance of Paper (Gurley Method).
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Installation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Manufacturer's best practice guide.
4.	Technical data sheet.
5.	Standard CAD drawings
C.	Shop Drawings: Provide detailed drawings of atypical non-standard applications of cladding junctions and penetrations which are outside the scope of the standard details and specifications provided by the manufacturer.
D.	Selection Samples: For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.
E.	Verification Samples: For each finish product specified, two samples, minimum size 4 by 6 inches (100 by 150 mm), representing actual product, color, and patterns.
1.5	QUALITY ASSURANCE
A.	Mock-Up: Provide a mock-up for evaluation of surface preparation techniques 
1.	Finish areas designated by Architect.
2.	Do not proceed with remaining work until workmanship, color, and sheen are approved by Architect.
3.	Refinish mock-up area as required to produce acceptable work.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging until ready for installation.
B.	Store siding flat on a smooth level surface. Protect edges and corners from chipping. Store sheets under cover and keep dry prior to installing.
C.	Store and dispose of solvent-based materials, and materials used with solvent-based materials, in accordance with requirements of local authorities having jurisdiction.
1.7	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
1.8	WARRANTY
A.	Manufacturer's Warranty: Provide Hardie HZ5 or HZ10 Reveal Panel Limited Product Warranty, with 30-year limited product warranty against manufacturing defects. 
1.	Application Warranty: Application limited warranty for 2 years.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Substitutions: Not permitted.
B.	Requests for approval of equal substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	CLADDING
A.	Cement Cladding Panels: Hardie Reveal Panel as manufactured by James Hardie Building Products, Inc. 7/16 inches (11 mm) thick, 3 feet 11.5 inches (1206 mm) wide by 7 feet 11.5 inches (2426 mm) long. Product shall be engineered for climate conditions.
1.	Manufacturer's Climate Zone Product: HZ5 for freezing wet climates with a green tint primer.
2.	Manufacturer's Climate Zone Product: HZ10 for hot humid and wet climates with a yellow tint primer.
3.	Refer to hardiezone.com to identify the specific zone of your project.
B.	Code Compliance Requirement for Siding Materials:
1.	Fiber-cement siding, complies with ASTM C 1186 Type A Grade II.
2.	Fiber-cement siding, complies with ASTM E 136 as a noncombustible material.
3.	Fiber-cement siding, complies with ASTM E 84 Flame Spread Index = 0, Smoke Developed Index = 5.
4.	Fiber-cement siding, complies with ASTM E 119 1 hour and 2 hour fire resistive assemblies listed with Warnock Hersey.
5.	Fiber-cement siding, tested to ASTM E330 for Transverse Loads.
6.	Intertek Warnock Hersey Product Listing.
7.	Manufacturer's Technical Data Sheet.
2.3	WEATHER BARRIER
A.	Weather Barrier: James Hardie HardieWrap and HardieWrap Flashing and Seam Tapes.
B.	Code Compliance Requirement for Weather Barrier:
1.	Thickness, 11 mil sheet.
2.	Breathability in accordance with ASTM E96.
3.	Tear strength in accordance with ASTM D1117.
4.	Water resistance in accordance with AATCC127.
5.	Air Penetration in accordance with TAPPI - T460.
6.	HardieWrap Weather Barrier ICC-ES Evaluation Report ESR-2258.
2.4	FURRING (STRAPPING)
A.	Rainscreen Cavity: Install Hardie Reveal Panels on a drained and vented rainscreen cavity, with a minimum 3/4 inch (19mm) air cavity. Selection of cavity vent materials shall be incorporated into the design to prevent insect and pest entry.
2.5	ACCESSORIES
A.	Trims: Reveal Trims manufactured by Custom Aluminum of Elgin, IL in the following profiles supplied by James Hardie. Aluminum alloy 6063-T5 with a minimum thickness of 0.050 inch. All reveal trims are 8 feet in length.
1.	Surround horizontal trim.
2.	Surround vertical trim.
3.	Surround horizontal end cut transition trim.
4.	Surround outside corner trim.
5.	Surround inside corner trim.
6.	Surround J channel trim.
7.	Surround drainage flashing.
8.	Recess horizontal trim.
9.	Recess vertical trim.
10.	Recess horizontal edge trim.
11.	Recess vertical F-trim.
12.	Recess outside corner trim.
13.	Recess drainage flashing.
B.	Finishes of Reveal Trims:
1.	Primed for field painting; coating tested to ASTM D3363, ASTM D3359, D2794, D4585, D523, and D1308.
2.	Clear anodized; conforming to ASTM B244 and ASTM B136. 
2.6	FASTENERS
A.	Fasteners: For attaching Hardie Reveal Panel direct to sheathing to a rain screen provide the following:
1.	Wood Framing, Exposed Screws: No. 10 by 0.472 inch (11.99 mm) head diameter by 1.5 inch (.38 mm) long.
2.	Wood Framing, Countersunk Screws: No. 8 by 0.390 inch (9.91 mm) head diameter by 1-5/8 inch (41 mm) long.
3.	Steel Framing, Exposed Screws: No. 10 by 0.472 inch (11.99 mm) head diameter by 1-1/4 inch (32 mm) long.
4.	Steel Framing, Countersunk Screws: No. 8 by 0.390 inch (9.91 mm) head diameter by 1-5/8 inch (41 mm) long.
5.	Fasteners shall be of high quality stainless steel to ensure resistance to corrosion. For field painting, fasteners shall be treated to accept paint adhesion.
a.	Alternatives must be approved by the architect. e.g. decorative screws, nails, bugle head screws, and similar items.
2.7	FINISHES
A.	Factory Primer: Provide factory applied universal primer.
1.	Primer: Factory applied sealer/primer by James Hardie. Apply flat sheen finishes to panels.
2.	Topcoat: Refer to Section 09 90 00 - Painting and Coating and Exterior Finish Schedule.
B.	Factory Finish for Trim: 
1.	Trim for Factory-Applied Coating and Field-Applied Finish: Chem Film.
2.	Trim for Factory-Applied Finish and No Field-Applied Finish: Clear anodized.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If framing preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
C.	Ensure that drainage plane in intact and all penetrations are sealed.
3.3	INSTALLATION
A.	Wood Framing: Nominal 2 inch by 4 inch (51 m by 102 mm) wood framing selected for minimal shrinkage and complying with local building codes, including the use of water-resistive barriers or vapor barriers where required. Minimum 1-1/2 inches (38 mm) face and straight, true, of uniform dimensions and properly aligned.
1.	Install water-resistive barriers and claddings to dry surfaces.
2.	Repair any punctures or tears in the water-resistive barrier prior to the installation of the siding.
3.	Protect siding from other trades.
B.	Metal Framing: Minimum 20 gauge (33 mm) 3-5/8 inch (92 mm) C-Stud 16 inches maximum metal framing complying with local building codes, including the use of water-resistive barriers and/or vapor barriers where required. Minimum 1-1/2 inches (38 mm) face and straight, true, of uniform dimensions and properly aligned.
1.	Install water-resistive barriers and claddings to dry surfaces.
2.	Repair any punctures or tears in the water-resistive barrier prior to the installation of the siding.
3.	Protect siding from other trades.
C.	Furring: Install furring on a minimum 3/4 inch (19 mm) rainscreen cavity, or in accordance with local building code for rainscreen requirements.
D.	Installation: Install materials in strict accordance with manufacturer's installation instructions.
1.	Fastening Method: Exposed.
2.	Fastening Method: Countersunk and filled.
3.	Place fasteners no closer than 3/4 inch (9.5 mm) from panel edges and 2 inches (51 mm) from panel corners.
4.	Use fasteners as specified in the James Hardie Tech Data sheet and in the Hardie Reveal Panel Installation Instruction.
5.	Install panel using 1/2 inch (13 mm) spacers at horizontal joints. Leave bottom edge of panel above all horizontal trims exposed, no caulking shall be placed at this overlap of Horizontal Reveal Trim. Factory primed edge shall always be used.
6.	Install a kickout flashing to deflect water away from the siding at the roof intersection.
7.	Install a self-adhering membrane on the wall before the subfascia and trim boards are nailed in place, and then install the kickout.
8.	Allow minimum vertical clearance between the bottom edge of siding and any other material in strict accordance with the manufacturer's installation instructions and as determined by James Hardie Zone.
9.	Maintain clearance between siding and adjacent finished grade.
10.	Specific framing and fastener requirements - refer to the applicable building code compliance reports.
3.4	FINISHING
A.	Finish factory primed siding with a minimum of one coat of high quality 100 percent acrylic exterior flat grade paint with flat finish within 180 days of installation. Follow paint manufacturer's written product recommendation and written application instructions.
B.	Field cut edges shall be coated during the installation process using an exterior grade primer/sealer that is compatible with the type of paint to used on project.
3.5	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION