SECTION 12 93 00

SITE FURNISHINGS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2014 -  2023 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Site furnishings of the following types:
1.	Benches.
2.	Picnic tables.
3.	Recycled plastic furniture.
4.	Outdoor grills and fire rings.
5.	Trash receptacles.
6.	Fiberglass pedal boats.
7.	Concrete site amenities.
8.	Strap steel furnishings.
9.	Drinking fountains and coolers.
10.	Garden furniture.
11.	Bike racks.
12.	Windsor series site furnishings.
13.	Planters.
14.	Snuffers.
15.	Crowd barriers.
16.	Shade solutions.
17.	Umbrellas.
18.	Outdoor sports equipment.
19.	Pet waste stations.
1.2	RELATED SECTIONS
A.	Section 31 20 00 - Earth Moving.
B.	Section 32 90 00 - Planting.
C.	Section 03 30 00 - Cast-in-Place Concrete
1.3	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Detail drawings.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Installation methods.
C.	Shop Drawings: Indicate materials, dimensions, tolerances, welding, fasteners, hardware, mounting, finish, and accessories. Include manufacturer's installation instructions.
1.4	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Minimum five years experience in producing site furnishings of the type specified.
1.5	DELIVERY, STORAGE, AND HANDLING
A.	Deliver and store products in manufacturer's unopened packaging bearing the brand name and manufacturer's identification until ready for installation.
B.	Handle materials to avoid damage. 
1.6	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.7	WARRANTY
A.	Manufacturer's Warranty: Provide manufacturer's standard warranty against defects in materials and workmanship.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Kay Park Recreation Corp., which is located at:<BR />1301 Pine St.<BR />Janesville, IA 50647<BR />Toll Free Tel: 800-553-2476<BR />Tel: 319-987-2313<BR />Fax: 319-987-2900<BR />Email: request info (sales@kaypark.com);Web: https://kaypark.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	SITE FURNISHINGS
A.	Benches:
1.	Perforated Series Benches:
a.	PSPB4TPP, Perforated Steel Bench with Back, 4 feet, Portable.
b.	PSPB6TPP, Perforated Steel Bench with Back, 6 feet, Portable.
c.	PSPB8TPP, Perforated Steel Bench with Back, 8 feet, Portable.
d.	PSPB10TPP, Perforated Steel Bench with Back, 10 feet, Portable.
e.	PSPB15TPP, Perforated Steel Bench with Back, 12 feet, Portable.
f.	PSPB4TPSM, Perforated Steel Bench with Back, 4 feet, Surface Mount.
g.	PSPB6TPSM, Perforated Steel Bench with Back, 6 feet, Surface Mount.
h.	PSPB8TPSM, Perforated Steel Bench with Back, 8 feet, Surface Mount.
i.	PSPB10TPSM, Perforated Steel Bench with Back, 10 feet, Surface Mount.
j.	PSPB15TPSM, Perforated Steel Bench with Back, 15 feet, Surface Mount.
k.	PSPB4TPIG, Perforated Steel Bench with Back, 4 feet, In-Ground Mount.
l.	PSPB6TPIG, Perforated Steel Bench with Back, 6 feet, In-Ground Mount.
m.	PSPB8TPIG, Perforated Steel Bench with Back, 8 feet, In-Ground Mount.
n.	PSPB10TPIG, Perforated Steel Bench with Back, 10 feet, In-Ground Mount.
o.	PSPB15TPIG, Perforated Steel Bench with Back, 15 feet, In-Ground Mount.
p.	SIPSPB4TPP, Special Identity Bench with Back, 4 feet, Portable. 
q.	SIPSPB6TPP, Special Identity Bench with Back, 6 feet, Portable.
r.	SIPSPB8TPP, Special Identity Bench with Back, 8 feet, Portable.
s.	SIPSPB10TPP, Special Identity Bench with Back, 10 feet, Portable.
t.	SIPSPB15TPP, Special Identity Bench with Back, 15 feet, Portable.
u.	SIPSPB4TPSM, Special Identity Bench with Back, 4 feet, Surface Mount.
v.	SIPSPB6TPSM, Special Identity Bench with Back, 6 feet, Surface Mount.
w.	SIPSPB8TPSM, Special Identity Bench with Back, 8 feet, Surface Mount. 
x.	SIPSPB10TPSM, Special Identity Bench with Back, 10 feet, Surface Mount.
y.	SIPSPB15TPSM, Special Identity Bench with Back, 15 feet, Surface Mount.
z.	SIPSPB4TPIG, Special Identity Bench with Back, 4 feet, In-Ground Mount.
aa.	SIPSPB6TPIG, Special Identity Bench with Back, 6 feet, In-Ground Mount.
ab.	SIPSPB8TPIG, Special Identity Bench with Back, 8 feet, In-Ground Mount.
ac.	SIPSPB10TPIG, Special Identity Bench with Back, 10 feet, In-Ground Mount.
ad.	SIPSPB15TPIG, Special Identity Bench with Back, 15 feet, In-Ground Mount.
ae.	PSBB4TPP, Perforated Backless Bench, 4 feet, Portable.
af.	PSBB6TPP, Perforated Backless Bench, 6 feet, Portable.
ag.	PSBB8TPP, Perforated Backless Bench, 8 feet, Portable.
ah.	PSBB10TPP, Perforated Backless Bench, 10 feet, Portable.
ai.	PSBB15TPP, Perforated Backless Bench, 15 feet, Portable.
aj.	PSBB4TPSM, Perforated Backless Bench, 4 feet, Surface Mount.
ak.	PSBB6TPSM, Perforated Backless Bench, 6 feet, Surface Mount.
al.	PSBB8TPSM, Perforated Backless Bench, 8 feet, Surface Mount.
am.	PSBB10TPSM, Perforated Backless Bench, 10 feet, Surface Mount.
an.	PSBB15TPSM, Perforated Backless Bench, 15 feet, Surface Mount.
ao.	PSBB4TPIG, Perforated Backless Bench, 4 feet, In-Ground Mount.
ap.	PSBB6TPIG, Perforated Backless Bench, 6 feet, In-Ground Mount.
aq.	PSBB8TPIG, Perforated Backless Bench, 8 feet, In-Ground Mount. 
ar.	PSBB10TPIG, Perforated Backless Bench, 10 feet, In-Ground Mount.
as.	PSBB15TPIG, Perforated Backless Bench, 15 feet, In-Ground Mount.
2.	Roll Formed Perforated Benches:
a.	SIPSRB6TP, Special Identity Roll Formed Bench with Back, 6 feet, Portable or Surface Mount..
b.	SIPSRB8TP, Special Identity Roll Formed Bench with Back, 8 feet, Portable or Surface Mount.
c.	PSRB6TP, Roll Formed Bench with Back, 6 feet, Portable or Surface Mount.
d.	PSRB8TP, Roll Formed Bench with Back, 8 feet, Portable or Surface Mount.
e.	PSURB6TP, U-Leg Bench with Back 6 feet, Portable or Surface Mount.
f.	PSURB8TP, U-Leg Bench with Back., 8 feet, Portable or Surface Mount.
g.	PSURBB6TP, U-Leg Bench w/o Back., 6 feet, Portable or Surface Mount.
h.	PSURBB8TP, U-Leg Bench w/o Back, 8 feet, Portable or Surface Mount.
3.	Renaissance Park Benches:
a.	RBS48, 48 inch, Cast Aluminum, Powder Coated.
b.	RBP60, 60 inch, Cast Aluminum, Powder Coated.
c.	RBLF80, 80 inch, Cast Aluminum, Powder Coated.
4.	Backless Renaissance Park Benches:
a.	RBBS48, 48 inch, Cast Aluminum, Powder Coated, White Oak.
b.	RBBP60, 60 inch, Cast Aluminum, Powder Coated, White Oak.
c.	RBBLF80, 80 inch, Cast Aluminum, Powder Coated, White Oak
5.	Victorian Park Benches:
a.	VBS48, 48 inch, Cast Aluminum, Powder Coated, White Oak.
b.	VBP60, 60 inch, Cast Aluminum, Powder Coated, White Oak.
c.	VBLF80, 80 inch, Cast Aluminum, Powder Coated, White Oak.
6.	Woodland Park Benches:
a.	WBS48, 48 inch, Cast Aluminum, Powder Coated, White Oak.
b.	WBP60, 60 inch, Cast Aluminum, Powder Coated, White Oak.
c.	WBLF80, 80 inch, Cast Aluminum, Powder Coated, White Oak.
7.	Contour Park Benches:
a.	CB2, Coated Black, Surface Mount.
b.	CB2IG, Coated Black, In Ground.
c.	6CB2SYP, 6 feet, Coated Black, SYP Pine, 2 x 4 inch, In-Ground Mount.
d.	8CB2SYP, 8 feet, Coated Black, SYP Pine, 2 x 4 inch, In-Ground Mount.
e.	4CB3RP, 4 feet, Coated Black, Recycled Plastic, 3 x 4 inch, In-Ground Mount.
f.	6CB3RP, 6 feet, Coated Black, Recycled Plastic, 3 x 4 inch, In-Ground Mount.
g.	6CB4RP, 6 feet, Coated Black, Recycled Plastic, 4 x 4 inch, In-Ground Mount.
h.	8CB4RP, 8 feet, Coated Black, Recycled Plastic, 4 x 4 inch, In-Ground Mount.
i.	ARCB, Coated Black.
8.	Flat Park Benches:
a.	FB2, Coated Black Powder, In-Ground Mount.
b.	6FB2SYP, 6 feet, Coated Black Powder, SYP Pine, 2 x 4 inch, In-Ground Mount.
c.	8FB2SYP, 8 feet, Coated Black Powder, SYP Pine, 2 x 4 inch, In-Ground Mount.
d.	4FB3RP, 4 feet, Coated Black Powder, Recycled Plastic, 3 x 4 inch, In-Ground Mount.
e.	6FB3RP, 6 feet, Coated Black Powder, Recycled Plastic, 3 x 4 inch, In-Ground Mount.
f.	6FB4RP, 6 feet, Coated Black Powder, Recycled Plastic, 4 x 4 inch, In-Ground Mount.
g.	8FB4RP, 8 feet, Coated Black Powder, Recycled Plastic, 4 x 4 inch, In-Ground Mount.
9.	Plastisol Coated Curved Rod Bench:
a.	CRB48VP, Curved Rod. Legs: Black Powder Coated. Seat and Back: PVC Coated.
b.	CRB72VP, Curved Rod, Legs: Black Powder Coated. Seat and Back: PVC Coated
10.	Portable Benches without Back:
a.	2PGL2-6,6 feet, 2 3/8 inch O.D. Tube, 2 x 10 or 2 x 4 inch, Frame Only.
b.	2PGL2-8, 8 feet, 2 3/8 inch O.D. Tube, 2 x 10 or 2 x 4 inch, Frame Only.
c.	2PGL3-15, 15 feet, 2 3/8 inch O.D. Tube, 2 x 10 or 2 x 4 inch, Frame Only.
d.	62PGL-P, 6 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, L-3 Treated Pine.
e.	82PGL-P, 8 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, L-3 Treated Pine.
f.	152PGL-P, 15 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, L-3 Treated Pine.
g.	62PGL-A, 6 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Aluminum.
h.	82PGL-A, 8 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Aluminum.
i.	152PGL-A, 15 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Aluminum.
j.	62PGL-F, 6 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Fiberglass.
k.	82PGL-F, 8 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Fiberglass.
l.	152PGL-F, 15 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Fiberglass.
m.	62PGL-VP, 6 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Vinyl Plastisol.
n.	82PGL-VP, 8 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Vinyl Plastisol.
o.	152PGL-VP, 15 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Vinyl Plastisol.
p.	62PGL-RRP, 6 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Recycled Plastic.
q.	82PGL-RRP, 8 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Recycled Plastic. 
11.	Portable Benches with Back:
a.	2PG2-6, 6 feet, 2 3/8 inch O.D. Tube.
b.	2PG2-8, 8 feet, 2 3/8 inch O.D. Tube.
c.	62PG-P, 6 feet, 2 3/8 inch O.D. Tube, SYP Pine, 2 x 10 inch.
d.	82PG-P,8 feet, 3/8 inch O.D. Tube, SYP Pine, 2 x 10 inch.
e.	152PG-P, 15 feet, 2 3/8 inch O.D. Tube, SYP Pine, 2 x 10 inch.
f.	62PGA, 6 feet, 2 3/8 inch O.D. Tube, Aluminum, 2 x 10 inch.
g.	82PG-A,8 feet, 2 3/8 inch O.D. Tube, Aluminum, 2 x 10 inch.
h.	152PG-A, 15 feet, 2 3/8 inch O.D. Tube, Aluminum, 2 x 10 inch.
i.	62PG-F, 6 feet, 2 3/8 inch O.D. Tube, Fiberglass, 2 x 10 inch.
j.	82PG-F, 8 feet, 2 3/8 inch O.D. Tube, Fiberglass, 2 x 10 inch.
k.	152PG-F, 15 feet, 2 3/8 inch O.D. Tube, Fiberglass, 2 x 10 inch.
l.	62PG-VP, 6 feet, 2 3/8 inch O.D. Tube, Vinyl Plastisol, 2 x 10 inch.
m.	82PG-VP, 8 feet, 2 3/8 inch O.D. Tube, Vinyl Plastisol, 2 x 10 inch.
n.	152PG-VP, 15 feet, 2 3/8 inch O.D. Tube, Vinyl Plastisol, 2 x 10 inch.
o.	62PG-RRP, 6 feet, 2 3/8 inch O.D. Tube, Recycled Plastic, 2 x 10 inch.
p.	82PG-RRP, 8 feet, 2 3/8 inch O.D. Tube, Recycled Plastic, 2 x 10 inch.
q.	2PG3-15, 15 feet, 2 3/8 inch O.D. Tube.
r.	62PG-AS,6 feet, 2 3/8 inch O.D. Tube, Aluminum, 2 x 4 inch.
s.	82PG-AS, 8 feet, 2 3/8 inch O.D. Tube, Aluminum, 2 x 4 inch.
t.	62PG-PS, 6 feet, 2 3/8 inch O.D. Tube, L-3 Treated Pine, 2 x 4 inch.
u.	82PG-PS,8 feet,2 3/8 inch O.D. Tube, L-3 Treated Pine, 2 x 4 inch.
v.	62PG-RPS, 6 feet, 2 3/8 inch O.D. Tube, Recycled Plastic, 2 x 4 inch.
w.	82PG-RPS, 8 feet, 2 3/8 inch O.D. Tube, Recycled Plastic, 2 x 4 inch.
12.	Stationary Benches with Back:
a.	2SG2-6,6 feet, 2 3/8 inch O.D. Tube.
b.	2SG2-8, 8 feet, 2 3/8 inch O.D. Tube.
c.	2SG3-15, 15 feet, 2 3/8 inch O.D. Tube.
d.	62SG-P, 6 feet, 2 3/8 inch O.D. Tube, L-3 Treated Pine, 2 x 10 inch.
e.	82SG-P, 8 feet, 2 3/8 inch O.D. Tube, L-3 Treated Pine, 2 x 10 inch.
f.	152SG-P, 15 feet, 2 3/8 inch O.D. Tube, L-3 Treated Pine, 2 x 10 inch.
g.	62SG-A, 6 feet, 2 3/8 inch O.D. Tube, Aluminum, 2 x 10 inch.
h.	82SG-A, 8 feet, 2 3/8 inch O.D. Tube, Aluminum, 2 x 10 inch.
i.	152SG-A, 15 feet, 2 3/8 inch O.D. Tube, Aluminum, 2 x 10 inch.
j.	62SG-F, 6 feet, 2 3/8 inch O.D. Tube, Fiberglass, 2 x 10 inch.
k.	82SG-F, 8 feet, 2 3/8 inch O.D. Tube, Fiberglass, 2 x 10 inch.
l.	152SG-F, 15 feet, 2 3/8 inch O.D. Tube, Fiberglass, 2 x 10 inch.
m.	62SG-VP, 6 feet, 2 3/8 inch O.D. Tube, Vinyl Plastisol,2 x 10 inch.
n.	82SG-VP, 8 feet, 2 3/8 inch O.D. Tube, Vinyl Plastisol, 2 x 10 inch.
o.	152SG-VP, 15 feet, 2 3/8 inch O.D. Tube, Vinyl Plastisol, 2 x 10 inch.
p.	62SG-RRP, 6 feet, 2 3/8 inch O.D. Tube, Recycled Plastic, 2 x 10 inch.
q.	82SG-RRP, 8 feet, 2 3/8 inch O.D. Tube, Recycled Plastic, 2 x 10 inch,
r.	62SG-RPS, 6 feet, 2 3/8 inch O.D. Tube, Recycled Plastic, 2 x 4 inch.
s.	82SG-RPS, 8 feet, 2 3/8 inch O.D. Tube, Recycled Plastic, 2 x 4 inch.
t.	62SG-PS, 6 feet, 2 3/8 inch O.D. Tube, L-3 Treated Pine, 2 x 4 inch.
u.	82SG-PS, 8 feet, 2 3/8 inch O.D. Tube, L-3 Treated Pine,2 x 4 inch.
v.	62SG-AS, 6 feet, 2 3/8 inch O.D. Tube, Aluminum, 2 x 4 inch.
w.	82SG-AS, 8 feet, 2 3/8 inch O.D. Tube, Aluminum, 2 x 4 inch.
13.	Stationary Benches without Back:
a.	2SGL2-6, 6 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch.
b.	2SGL2-8, 8 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch.
c.	2SGL3-15, 15 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch.
d.	62SGL-P, 6 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, L-3 Treated Pine.
e.	82SGL-P, 8 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, L-3 Treated Pine.
f.	152SGL-P, 15 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, L-3 Treated Pine.
g.	62SGL-A, 6 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Aluminum.
h.	82SGL-A, 8 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Aluminum.
i.	152SGL-A, 15 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Aluminum.
j.	62SGL-F, 6 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Fiberglass.
k.	82SGL-F, 8 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Fiberglass.
l.	152SGL-F, 15 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Fiberglass.
m.	62SGL-VP, 6 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Vinyl Plastisol.
n.	82SGL-VP, 8 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Vinyl Plastisol.
o.	152SGL-VP, 15 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Vinyl Plastisol.
p.	62SGL-RRP, 6 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Recycled Plastic.
q.	82SGL-RRP, 8 feet, 2 3/8 inch O.D. Tube, 2 x 10 inch, Recycled Plastic.
14.	Double Shelf-Back Players Bench:
a.	15DSBPBA, Double Shelf-Back Players Bench, 15 feet.
b.	21DSBPBA, Double Shelf-Back Players Bench, 21 feet.
15.	Windsor Select Benches:
a.	WS6LCBRP, Windsor Select Bench with Back, 6 feet, Recycled Plastic.
b.	WS6FCBRP, Windsor Select Bench Backless, 6 feet, Recycled Plastic.
16.	Plastisol-Coated Benches:
a.	CWB6VPP, 6 feet Classic Portable Bench with Back, 6 feet.
b.	CWB8VPP, 8 feet Classic Portable Bench with Back, 8 feet.
c.	CWB6VPSM, 6 feet Classic Surface Mount Bench with Back, 6 feet.
d.	CWB8VPSM, 8 feet Classic Surface Mount Bench with Back, 8 feet.
e.	CWB6VPIG, 6 feet Classic In-Ground Bench with Back, 6 feet.
f.	CWB8VPIG, 8 feet Classic in-Ground Bench with Back, 8 feet.
g.	CF6VPP, 6 feet Classic Flat Portable Bench, 6 feet.
h.	CF8VPP, 8 feet Classic Flat Portable Bench, 8 feet.
i.	CF6VPIG, 6 feet Classic Flat In-Ground Bench, 6 feet.
j.	CF8VPIG, 8 feet Classic Flat In-Ground Bench, 8 feet.
k.	CF6VPWM, 6 feet Classic Flat Wall Mount Bench, 6 feet.
l.	CF8VPWM, 8 feet Classic Flat Wall Mount Bench, 8 feet.
m.	CHB72VP, Concrete Bench with Thermoplastic Coated Seat, 8 feet.
n.	CSB72VP, Concrete Bench with Thermoplastic Coated Seats, 8 feet.
o.	CSF6VPP, 6 feet Classic Supreme Flat Portable Bench, 6 feet.
p.	CSF8VPP, 8 feet Classic Supreme Flat Portable Bench, 8 feet. 
q.	CSF6VPSM, 6 feet Classic Supreme Flat Surface Mount Bench, 6 feet.
r.	CSF8VPSM, 8 feet Classic Supreme Flat Surface Mount Bench, 8 feet.
s.	CSF6VPIG, 6 feet Classic Supreme Flat In-Ground Bench, 6 feet.
t.	CSF8VPIG, 8 feet Classic Supreme Flat In-Ground Bench, 8 feet.
u.	DBB6PVP, 6 feet Plastisol-Coated Double Back Bench, 6 feet.
v.	DBB8PVP, 8 feet Plastisol-Coated Double Back Bench, 8 feet.
17.	Plastisol-Coated Laser Cut Benches:
a.	LCB48VP, Laser Cut, Legs: Black Powder Coated. Seat and Back: PVC Coated.
b.	LCB72VP, Laser Cut, Legs: Black Powder Coated. Seat and Back: PVC Coated.
18.	Triple Bench Chairs:
a.	WCCV3SBIG, Concave with Back, In-Ground.
b.	WCCV3SBSM, Concave with Back, Surface Mount.
c.	WCCV3SBBIG, Concave Backless, In-Ground.
d.	WCCV3SBBSM, Concave Backless, Surface Mount.
e.	WCVX3SBIG, Convex with back, In-Ground.
f.	WCVX3SBSM, Convex with back, Surface Mount.
g.	WCVX3SBBIG, Convex Backless, In-Ground.
h.	WCVX3SBBSM, Convex Backless, Surface Mount.
i.	WINL3SBIG, In-Line with back, In-Ground.
j.	WINL3SBSM, In-Line with back, Surface Mount.
k.	WINL3SBBIG, In-line Backless, In-Ground.
l.	WINL3SBBSM, In-line Backless, Surface Mount.
m.	TBCARMS, Optional Armrests.
19.	Iron Valley Benches:
a.	IVB48PC, 48 inch Long Bench with Back, Ductile Iron and Steel, Powder coating, 48 inch.
b.	IVB60PC, 60 inch Long Bench with Back, Ductile Iron and Steel, Powder coating, 60 inch.
c.	IVB72PC, 72 inch Long Bench with Back, Ductile Iron and Steel, Powder coating, 72 inch.
d.	IVB96PC, 96 inch Long Bench with Back, Ductile Iron and Steel, Powder coating, 96 inch.
e.	IVBB48PC, 48 inch Backless Bench, Ductile Iron and Steel, Powder coating, 48 inch.
f.	IVBB60PC, 60 inch Backless Bench, Ductile Iron and Steel, Powder coating, 60 inch.
g.	IVBB72PC, 72 inch Backless Bench, Ductile Iron and Steel, Powder coating, 72 inch.
h.	IVBB96PC, 96 inch Backless Bench, Ductile Iron and Steel, Powder coating, 96 inch.
20.	Strap Steel Benches:
a.	SSABB48, 48 inch L Backless Bench, 3/4 inch solid steel.
b.	SSABB72, 72 inch L Backless Bench, 3/4 inch solid steel.
c.	SSAPB48, 48 inch L Park Bench with Back, 3/4 inch solid steel.
d.	SSAPB72, 72 inch L Park Bench with Back, 3/4 inch solid steel.
e.	SSCB48, 48 inch L Contour Bench with Back, 3/4 inch solid steel.
f.	SSCB72, 72 inch L Contour Bench with Back.
21.	Concrete Benches:
a.	CCB72CL, 72 inch, 18 inch.
b.	CMB84R8, 4 inch, 19 inch.
c.	CMB90C, 90 inch, 18 inch.
d.	CFB84C, 84 inch, 17 inch.
e.	CHB72VP, 72 inch, 17 inch..
f.	CSB72VP, 72 inch, 17 inch..
g.	CTB58C, 58 inch, 18 1/2 inch.
h.	CTB72C, 72 inch, 18 1/2 inch.
i.	CTB84C, 84 inch, 18 1/2 inch.
j.	CPB58C, 58 inch, 33 inch.
k.	CPB72C, 72 inch, 33 inch.
l.	CPB84C, 84 inch, 33 inch.
m.	CPB84R, 84 inch, 33 inch.
n.	CSB84R, 84 inch, 33 inch.
o.	CKIB84C, 84 inch, 37 inch.
p.	CPB72M, 72 inch, 33 inch.
q.	CPB96M, 96 inch, 33 inch.
r.	CPB60X, 60 inch, 34 inch.
s.	HLB4, 48 inch, 18 inch.
t.	HLB6, 72 inch, 18 inch.
u.	HLB8, 96 inch, 18 inch.
22.	Recycled Plastic Benches:
a.	JPSB42, Backless Bench -2 Legs, 4 feet, Black recycled plastic.
b.	JPSB63, Backless Bench -3 Legs, 6 feet, Black recycled plastic.
c.	JPSB83, Backless Bench -3 Legs, 8 feet, Black recycled plastic.
d.	JPAB4, Bench with Back, 4 feet, Cast Aluminum, Green, Black.
e.	JPAB5, Bench with Back, 5 feet, Cast Aluminum, Green, Black.
f.	JPAB6, Bench with Back, 6 feet, Cast Aluminum, Green, Black.
g.	JPCB4, Bench with back -2 Legs, 4 feet, Black recycled plastic.
h.	JPCB6, Bench with back -3 Legs, 6 feet, Black recycled plastic.
i.	JPCB8, Bench with back -3 Legs, 8 feet, Black recycled plastic.
j.	JPCB42, Bench with back -2 Legs, 4 feet, Black recycled plastic.
k.	JPCB63, Bench with back -3 Legs, 6 feet, Black recycled plastic.
l.	JPCB83, Bench with back -3 Legs, 8 feet, Black recycled plastic.
m.	RCB48B, Bench with Back - 2 Legs, 4 feet, Black recycled plastic.
n.	RCB60B, Bench with Back - 3 Legs, 5 feet, Black recycled plastic.
o.	RCB72B, Bench with Back, 6 feet, Black recycled plastic.
p.	RMB48NB, Backless Bench - 2 Legs, 4 feet, Black recycled plastic.
q.	RMB60NB, Backless Bench - 3 Legs, 5 feet, Black recycled plastic.
r.	RMB72NB, Backless Bench - 3 Legs, 6 feet, Black recycled plastic.
s.	4CB3RP, 4 feet Frame with Recycled Plastic 3 x 4 Contour Park Bench, 4 feet, 3/8 x 4 inch Rolled steel, Coated Black.
t.	6CB3RP, 6 feet, 3/8 x 4 inch Rolled steel, Coated Black.
u.	6CB4RP, 6 feet, 3/8 x 4 inch Rolled steel, Coated Black.
v.	8CB4RP, 8 feet, 3/8 x 4 inch Rolled steel, Coated Black.
w.	62PG-RPS, 6 feet Recycled Plastic, 2 x 4 inch Slats, 6 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
x.	62PG-RRP, 6 feet Recycled Plastic, 2 x 10 inch Plank, 6 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
y.	82PG-RPS, 8 feet Recycled Plastic, 2 x 4 inch Slats, 8 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
z.	82PG-RRP, 8 feet Recycled Plastic, 2 x 10 inch Plank, 8 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
aa.	62PGL-RRP, 6 feet Recycled Plastic, 2 x 10 inch Plank for Portable Bench without Back, 6 feet, 2 3/8 inch O.D. Tube, Black Powder Coating Standard: Galvanized.
ab.	82PGL-RRP, 8 feet Recycled Plastic, 2 x 10 inch Plank for Portable Bench without Back, 8 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
ac.	152SG-A, 15 feet Aluminum, 2 x 10 inch Plank for Stationary Bench with Back, 15 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
ad.	62SG-RPS, 6 feet Recycled Plastic, 2 x 4 inch Slats for Stationary Bench with Back, 6 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
ae.	62SG-RRP, 6 feet Recycled Plastic, 2 x 10 inch Plank for Stationary Bench with Back, 6 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
af.	82SG-RPS, 8 feet Recycled Plastic, 2 x 4 inch Slats for Stationary Bench with Back, 8 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
ag.	82SG-RRP, 8 feet Recycled Plastic, 2 x 10 inch Plank for Stationary Bench with Back, 8 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
ah.	62SGL-RRP, 6 feet Recycled Plastic, 2 x 10 inch Plank for Stationary Bench without Back, 6 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
ai.	82SGL-RRP, 8 feet Recycled Plastic, 2 x 10 inch Plank for Stationary Bench without Back, 8 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
aj.	WS6FCBRP, Windsor Select Bench Backless, 6 feet, Steel, Coated Black Powder.
ak.	WS6LCBRP, Windsor Select Bench with Back, 6 feet, Steel, Coated Black Powder.
B.	Picnic Tables:
1.	J2 Series Welded Frame Tables:
a.	J2G-6 6 feet, 2 3/8, Frame Only.
b.	J2G-8, 8 feet, 2 3/8, Frame Only.
c.	J2G-12, 12 feet, 2 3/8, Frame Only.
d.	6J2GW, 6 feet, 2 3/8, L3 Treated Wood.
e.	8J2GW, 8 feet, 2 3/8, L3 Treated Wood.
f.	12J2GW, 12 feet, 2 3/8, L3 Treated Wood.
g.	6J2GF, 6 feet, 2 3/8, Fiberglass.
h.	8J2GF, 8 feet, 2 3/8, Fiberglass.
i.	6J2GA, 6 feet, 2 3/8, Aluminum.
j.	8J2GA, 8 feet, 2 3/8, Aluminum.
k.	12J2GA, 12 feet, 2 3/8, Aluminum.
l.	6J2GVP, 6 feet, 2 3/8, Vinyl Plastisol (PVC.)
m.	8J2GVP, 8 feet, 2 3/8, Vinyl Plastisol (PVC).
n.	6J2GRRP, 6 feet, 2 3/8, Recycled Plastic.
o.	8J2GRRP, 8 feet, 2 3/8, Recycled Plastic.
2.	CJ Series Welded Frame Tables:
a.	CJG-6, 6 feet, 1 5/8, 40 Pipe, Frame Only.
b.	CJG-8, 8 feet, 1 5/8, 40 Pipe, Frame Only.
c.	CJG-12, 12 feet, 1 5/8, 40 Pipe, Frame Only.
d.	6CJGW, 6 feet, 1 5/8, 40 Pipe, L3 Treated Wood.
e.	8CJGW, 8 feet, 1 5/8, 40 Pipe, L3 Treated Wood.
f.	12CJGW, 12 feet, 1 5/8, 40 Pipe, L3 Treated Wood.
g.	6CJGVP, 6 feet, 1 5/8, 40 Pipe, Vinyl Plastisol (PVC).
h.	8CJGVP, 8 feet, 1 5/8, 40 Pipe, Vinyl Plastisol (PVC).
i.	6CJGF, 6 feet, 1 5/8, 40 Pipe, Fiberglass.
j.	8CJGF, 8 feet, 1 5/8, 40 Pipe, Fiberglass.
k.	6CJGA, 6 feet, 1 5/8, 40 Pipe, Aluminum.
l.	8CJGA, 8 feet, 1 5/8, 40 Pipe, Aluminum.
m.	12CJGA, 12 feet, 1 5/8, 40 Pipe, Aluminum.
n.	6CJGRRP, 6 feet, 1 5/8, 40 Pipe, Recycled Plastic.
o.	8CJGRRP, 8 feet, 1 5/8, 40 Pipe, Recycled Plastic.
3.	2BG Series Bolted Frame Tables:
a.	682BG, 8 feet, 6 feet, 2 3/8, Galvanized, Frame Only.
b.	682BC, 8 feet, 6 feet, 2 3/8, Black powder coated, Frame Only.
c.	62BGW, 6 feet, 2 3/8, Galvanized, L3 Treated Wood.
d.	62BCW, 6 feet, 2 3/8, Black powder coated, L3 Treated Wood.
e.	82BGW, 8 feet, 2 3/8, Galvanized, L3 Treated Wood.
f.	82BCW, 8 feet, 2 3/8, Black powder coated, L3 Treated Wood.
g.	62BGF, 6 feet, 2 3/8, Galvanized, Fiberglass.
h.	62BCF, 6 feet, 2 3/8, Black powder coated, Fiberglass.
i.	82BGF, 8 feet, 2 3/8, Galvanized, Fiberglass.
j.	82BCF, 8 feet, 2 3/8, Black powder coated, Fiberglass.
k.	62BGA, 6 feet, 2 3/8, Galvanized, Aluminum.
l.	62BCA, 6 feet, 2 3/8, Black powder coated, Aluminum.
m.	82BGA, 8 feet, 2 3/8, Galvanized, Aluminum.
n.	82BCA, 8 feet, 2 3/8, Black powder coated, Aluminum.
o.	62BGVP, 6 feet, 2 3/8, Galvanized, Vinyl Plastisol (PVC).
p.	62BCVP, 6 feet, 2 3/8, Black powder coated, Vinyl Plastisol (PVC).
q.	82BGVP, 8 feet, 2 3/8, Galvanized, Vinyl Plastisol (PVC).
r.	82BCVP, 8 feet, 2 3/8, Black powder coated, Vinyl Plastisol (PVC).
s.	62BGRRP, 6 feet, 2 3/8, Galvanized, Recycled Plastic.
t.	62BCRRP, 6 feet, 2 3/8, Black powder coated, Recycled Plastic.
u.	82BGRRP, 8 feet, 2 3/8, Galvanized, Recycled Plastic.
v.	82BCRRP, 8 feet, 2 3/8, Black powder coated, Recycled Plastic.
4.	BG Series Bolted Frame Tables:
a.	68BG, 8 feet, 6 feet, 1 5/8, Galvanized, Frame Only.
b.	68BC, 8 feet, 6 feet, 1 5/8, Black powder coated, Frame Only.
c.	6BGW, 6 feet, 1 5/8, Galvanized, L3 Treated Wood.
d.	6BCW, 6 feet, 1 5/8, Black powder coated, L3 Treated Wood.
e.	8BGW, 8 feet, 1 5/8, Galvanized, L3 Treated Wood,
f.	8BCW, 8 feet, 1 5/8, Black powder coated, L3 Treated Wood,
g.	6BGVP, 6 feet, 1 5/8, Galvanized, Vinyl Plastisol (PVC)
h.	6BCVP, 6 feet, 1 5/8, Black powder coated, Vinyl Plastisol (PVC)
i.	8BGVP, 8 feet, 1 5/8, Galvanized, Vinyl Plastisol (PVC).
j.	8BCVP, 8 feet, 1 5/8, Black powder coated, Vinyl Plastisol (PVC).
k.	6BGF, 6 feet, 1 5/8, Galvanized, Fiberglass,
l.	6BCF, 6 feet, 1 5/8, Black powder coated, Fiberglass,
m.	8BGF, 8 feet, 1 5/8, Galvanized, Fiberglass.
n.	8BCF, 8 feet, 1 5/8, Black powder coated, Fiberglass.
o.	6BGA, 6 feet, 1 5/8, Galvanized, Aluminum.
p.	6BCA, 6 feet, 1 5/8, Black powder coated, Aluminum.
q.	8BGA, 8 feet, 1 5/8, Galvanized, Aluminum.
r.	8BCA, 8 feet, 1 5/8, Black powder coated, Aluminum.
s.	6BGRRP, 6 feet, 1 5/8, Galvanized, Recycled Plastic.
t.	6BCRRP, 6 feet, 1 5/8, Black powder coated, Recycled Plastic.
u.	8BGRRP, 8 feet, 1 5/8, Galvanized, Recycled Plastic.
v.	8BCRRP, 8 feet, 1 5/8, Black powder coated, Recycled Plastic.
5.	J2GWC Series Welded Frame Tables:
a.	6J2G-SWC, 6 feet, Side, 1, Frame Only.
b.	6J2GW-SWC, 6 feet, Side, 1, L3 Treated Wood.
c.	6J2GA-SWC, 6 feet, Side, 1, Aluminum.
d.	6J2GF-SWC, 6 feet, Side, 1, Fiberglass.
e.	6J2GVP-SWC, 6 feet, Side, 1, Vinyl Plastisol (PVC).
f.	6J2GRRP-SWC, 6 feet, Side, 1, Recycled Plastic.
g.	8J2G-SWC, 8 feet, Side, 1, Frame Only.
h.	8J2GW-SWC, 8 feet, Side, 1, L3 Treated Wood.
i.	8J2GA-SWC, 8 feet, Side, 1, Aluminum.
j.	8J2GF-SWC, 8 feet, Side, 1, Fiberglass.
k.	8J2GVP-SWC, 8 feet, Side, 1, Vinyl Plastisol (PVC).
l.	8J2GRRP-SWC, 8 feet, Side, 1, Recycled Plastic.
m.	12J2GSWC, 12 feet, Side, 2, Frame Only.
n.	12J2GW-SWC, 12 feet, Side, 2, L3 Treated Wood.
o.	12J2GA-SWC, 12 feet, Side, 2, Aluminum.
p.	12J2GRRP-SWC, 12 feet, Side, 2, Recycled Plastic.
q.	8J2G-EWC, 8 feet, End, 1, Frame Only.
r.	8J2GW-EWC, 8 feet, End, 1, L3 Treated Wood.
s.	8J2GA-EWC, 8 feet, End, 1, Aluminum.
t.	8J2GF-EWC, 8 feet, End, 1, Fiberglass.
u.	8J2GVP-EWC, 8 feet, End, 1, Vinyl Plastisol (PVC).
v.	8J2GRRP-EWC, 8 feet, End, 1, Recycled Plastic.
w.	8J2G-SEWC, 8 feet, End, Side, 2, Frame Only.
x.	8J2GW-SEWC, 8 feet, End, Side, 2, L3 Treated Wood.
y.	8J2GA-SEWC, 8 feet, End, Side, 2, Aluminum.
z.	8J2GF-SEWC, 8 feet, End, Side, 2, Fiberglass.
aa.	8J2GVP-SEWC, 8 feet, End, Side, 2, Vinyl Plastisol (PVC).
ab.	8J2GRRP-SEWC, 8 feet, End, Side, 2, Recycled Plastic.
6.	6SPT Series Single Post Tables:
a.	6SPTG, Frame Only, Hot Dip Galvanized, Surface Mount, In-Ground.
b.	6SPTC, Frame Only, Black powder coated, Surface Mount, In-Ground.
c.	6SPTGW, Wood, Hot Dip Galvanized, Surface Mount, In-Ground.
d.	6SPTCW, Wood, Black powder coated, Surface Mount, In-Ground.
e.	6SPTGA, Aluminum, Hot Dip Galvanized, Surface Mount, In-Ground.
f.	6SPTCA, Aluminum, Black powder coated (, Surface Mount, In-Ground.
g.	6SPTGF, Fiberglass, Hot Dip Galvanized, Surface Mount, In-Ground.
h.	6SPTCF, Fiberglass, Black powder coated, Surface Mount, In-Ground.
i.	6SPTGVP, Vinyl Plastisol (PVC), 378 lbs, Hot Dip Galvanized, Surface Mount, In-Ground.
j.	6SPTCVP, Vinyl Plastisol (PVC), 378 lbs, Black powder coated, Surface Mount, In-Ground.
k.	6SPTGRRP, Recycled Plastic, Hot Dip Galvanized,.
l.	6SPTCRRP, Recycled Plastic, Black powder coated.
7.	4SPT Series Single Post Tables:
a.	4SPTG, Frame Only, Hot Dip Galvanized, Surface Mount, In-Ground.
b.	4SPTC, Frame Only, Black powder coated, Surface Mount, In-Ground.
c.	4SPTGW, L3 Treated Wood, 48 x 48 inch, Hot Dip Galvanized, Surface Mount, In-Ground.
d.	4SPTCW, L3 Treated Wood, 48 x 48 inch, Black powder coated, Surface Mount, In-Ground.
e.	4SPTGA, Aluminum, 48 x 48 inch, Hot Dip Galvanized, Surface Mount, In-Ground.
f.	4SPTCA, Aluminum, 48 x 48 inch, Black powder coated, Surface Mount, In-Ground.
g.	4SPTGF, Fiberglass, 48 x 48 inch, Hot Dip Galvanized, Surface Mount, In-Ground.
h.	4SPTCF, Fiberglass, 48 x 48 inch, Black powder coated, Surface Mount, In-Ground.
i.	4SPTGVP, Vinyl Plastisol (PVC), 46 x 46 inch, Hot Dip Galvanized, Surface Mount, In-Ground. 
j.	4SPTCVP, Vinyl Plastisol (PVC), 46 x 46 inch, Black powder coated, Surface Mount, In-Ground. 
k.	4SPTGRP, Recycled Plastic, 48 x 48 inch, Hot Dip Galvanized, Surface Mount, In-Ground.
l.	4SPTCRP, Recycled Plastic, 48 x 48 inch, Black powder coated, Surface Mount, In-Ground.
m.	BackrestW, L3 Treated Wood.
n.	BackrestA, Aluminum.
o.	BackrestF, Fiberglass.
p.	BackrestVP, Vinyl Plastisol (PVC).
q.	BackrestRP, Recycled Plastic.
8.	Child Size Tables:
a.	4CSVPT, 4 feet Plastisol Coated Child Size Table.
b.	6CSVPT, 6 feet Plastisol Coated Child Size Table.
c.	8CSVPT, 6 feet Plastisol Coated Child Size Table.
d.	LTFCT42, 42 inch Child Size, Almond Colored, Folding Picnic Table.
e.	JPAFCS4, 4 feet Child Size Recycled Plastic Table.
f.	CSRTRCF, Round Fiberglass Child Size Table Black Frame.
g.	CSRTRCVP, Round Plastisol Child Size Table Black Frame.
h.	CS4SJCVP, Square Plastisol Child Size Table Black Frame.
9.	Oval Plastisol Coated Tables:
a.	6OVPT, 6 feet Vinyl Plastisol (PVC) Table.
10.	Double Pedestal Coated Tables:
a.	6DPTVP, 6 feet, Vinyl Plastisol (PVC).
b.	8DPTVP, 8 feet, Vinyl Plastisol (PVC).
c.	8HDPTVP, Vinyl Plastisol (PVC).
11.	Round Portable Tables:
a.	RTRCVP, 48 inch, 390 lbs, Vinyl Plastisol (PVC).
b.	RTRGVP, 48 inch, 390 lbs, Vinyl Plastisol (PVC).
c.	RTRCF, 48 inch, 205 lbs, Fiberglass.
d.	RTRGF, 48 inch, 205 lbs, Fiberglass.
12.	Round Single Post Tables:
a.	RSPTGVP, Galvanized after Fabrication, 48 inch, Vinyl Plastisol (PVC), Surface Mount, In-Ground
b.	RSPTCVP, Powder Coating, 48 inch, Vinyl Plastisol (PVC), Surface Mount, In-Ground.
c.	RSPTGF, Galvanized after Fabrication, 48 inch, Fiberglass, Surface Mount, In-Ground.
d.	RSPTCF, Powder Coating, 48 inch, Fiberglass, Surface Mount, In-Ground.
13.	Round Fiberglass Portable Tables:
a.	RTRCF, 1 5/8, Black Coated, 48 inch, Fiberglass.
b.	RTRGF, 1 5/8, Galvanized, 48 inch, Fiberglass.
14.	Square Portable Tables:
a.	4SJC, Standard: Black coated, Galvanized, Frame Only, 48 x 48 inch.
b.	4SJCW, Standard: Black coated, Galvanized, Wood, 48 x 48 inch.
c.	4SJCA, Standard: Black coated, Galvanized, Aluminum, 48 x 48 inch.
d.	4SJCF, Standard: Black coated, Galvanized, Fiberglass, 48 x 48 inch.
e.	4SJCVP, Standard: Black coated, Galvanized, Vinyl Plastisol (PVC), 46 x 46 inch.
f.	4SJCRP, Standard: Black coated, Galvanized, Recycled Plastic, 48 x 48 inch.
g.	BackrestW, Black Powder Coating, Hot Dip Galvanized, L3 Treated Wood.
h.	BackrestA, Black Powder Coating, Hot Dip Galvanized, Aluminum.
i.	BackrestF, Black Powder Coating, Hot Dip Galvanized, Fiberglass.
j.	BackrestVP, Black Powder Coating, Hot Dip Galvanized, Vinyl Plastisol (PVC).
k.	BackrestRP, Black Powder Coating, Hot Dip Galvanized, Recycled Plastic.
15.	Windsor Tables:
a.	WS6JCRP, Windsor 6 feet Picnic Tables, 6 feet, 1 5/8 inch, Free Standing.
b.	WS4JCRP, Windsor 4 feet Square Tables, 4 feet, 1 5/8 inch, Free Standing.
c.	WS6SPTCRP-SM, Windsor Single Post Table, 6 feet, 3 1/2 inch, Surface Mount.
d.	WS6SPTCRP-IG, Windsor Single Post Table, 6 feet, 3 1/2 inch, Inground Mount.
16.	Recycled Plastic Tables:
a.	JPPT63, 6 feet Table-3 Legs, 6 feet, Black recycled plastic.
b.	JPPT83, 8 feet Table-3 Legs, 8 feet, Black recycled plastic.
c.	JPPT83ADA, 8 feet Table-3 Legs, 8 feet, Black recycled plastic.
d.	RPT722S, 6 feet Table with 2 Seats, 6 feet, Black recycled plastic.
e.	RPT721S, 6 feet Table with 1 Seat, 6 feet, Black recycled plastic.
f.	JPHT, Hexagon Table, Black recycled plastic.
g.	JPHTADA, Hexagon Table ADA, Black recycled plastic.
h.	JPAFCS4, 4 feet Child Size Recycled Plastic Table, 4 feet, Black recycled plastic.
i.	JPAF6ADA, 6 feet "A" Frame, ADA Accessible Recycled Plastic Table, 6 feet, Black recycled plastic.
j.	JPAF6, 6 feet "A" Frame Recycled Plastic Table, 6 feet, Black recycled plastic.
17.	Concrete Tables:
a.	CTR4S, Round Top 4 Seat, 68 inch, 30 inch, 68 inch. 
b.	CTR3H, Round Top 3 Seat for Wheelchair Access.
c.	UMBRKT, Optional- Umbrella Bracket for Round Concrete Table.
d.	CTO4S, Octagon Top 4 Seat, 66 inch, 29 inch, 66 inch.
e.	CTS4S, Square Top 4 Seat, 66 inch, 29 inch, 66 inch.
f.	CTS2S, Square Top 2 Seats, 30 inch, 29 inch, 66 inch.
g.	UMBKT, Optional- Umbrella Bracket for Square or Octagon Tables.
h.	CTR6MTP, Rectangle Mesh Top, 72 inch, 29 inch, 66 inch.
i.	CTR8MTP, Rectangle Mesh Top, 96 inch, 29 inch, 66 inch.
j.	CTRJ60C, Rectangle Top, 60 inch, 29 inch, 58 inch.
k.	CTRJ84C, Rectangle Top, 84 inch, 29 inch, 58 inch.
l.	CTRJ84H, Handicap Rectangle Top, 84 inch, 29 inch, 58 inch.
m.	CTRJ84R, Redwood Rectangle Top, 84 inch, 29 inch, 58 inch.
n.	CTOV72, Oval Top, 72 inch, 30 inch, 60 inch.
o.	CTOV84, Oval Top, 84 inch, 30 inch, 60 inch.
p.	CTOV84H, Oval Top for Wheelchair Access, 84 inch, 30 inch, 60 inch.
q.	CMT84C, Concrete Monster Table, 84 inch, 29 inch, 62 inch. 
r.	CMT84H, Concrete Monster Table with Handicap Benches, 84 inch, 29 inch, 62 inch.
s.	CTRT84C, Rectangular Top, 84 inch, 30 inch, 62 inch.
t.	CTRT96C, Rectangular Top, 96 inch, 30 inch, 62 inch.
u.	GBI, Game Board Insert.
18.	Perforated Series Tables:
a.	PSPT6TP, Portable Perforated Table, 6 feet.
b.	PSPT8TP, Portable Perforated Table, 8 feet,.
c.	PSPT8TPADA, Portable Perforated ADA Table, 8 feet.
d.	PSPT10TP, Portable Perforated Table, 10 feet.
e.	PSPT12TP, Portable Perforated Table, 12 feet.
f.	REPST6TP, Portable Rolled Edge Table, 6 feet.
g.	REPST8TP, Portable Rolled Edge Table, 8 feet.
h.	REPST10TP, Portable Rolled Edge Table, 10 feet.
i.	PSST4TP, Portable Square Table, 4 feet.
j.	PSST3TP, Portable Square Table 3 Seat.
k.	PSRT4TP, Portable Round Table, 4 feet.
l.	PSRT3TP, Portable Round Table 3 Seat, 4 feet.
m.	PSPT3630, Round Patio Table, 3 feet
n.	PSPT3640, Round Cafe Table, 3 feet.
o.	PSPC36, 36 inch Patio Chair, 3 feet.
p.	PSPC46, 46 inch Patio Chair, 4 feet.
19.	Iron Valley Tables:
a.	IVPTSP3, 36 inch Sq. Table only, Ductile Iron and Steel, Powder coating, 36 inch.
b.	IVPTCB2, 24 inch Chair with Back, Ductile Iron and Steel, Powder coating.
c.	IVPTC2, 24 inch Chair without Back, Ductile Iron and Steel, Powder coating.
d.	IVMPT6, 6 feet Multipost Table w/ Benches, Ductile Iron and Steel, Powder coating, 72 inch.
e.	IVMPT8, 8 feet Multipost Table w/ Benches, Ductile Iron and Steel, Powder coating, 96 inch.
20.	Strap Steel Tables:
a.	SSHSST, One Piece Square Table with Four Seats, 3/4 inch sold steel, Standard Free-Standing, Surface Mount..
21.	Lifetime Folding Tables:
a.	LTFPT72, 6 feet Putty Colored, Folding Picnic Table.
b.	LTFCT42, 42 inch Child Size, Almond Colored, Folding Picnic Table.
c.	LTFRT, 44 inch Round Folding Picnic Table, Almond Color.
C.	Recycled Plastic Furniture:
1.	Recycled Plastic Message Centers:
a.	JPMCL1P, Large Message Center, Recycled plastic, 1 Side w/ Posts, 
b.	JPMCL1W, Large Message Center, Recycled plastic, 1 Side Wall Mount.
c.	JPMCL2P, Large Message Center, Recycled plastic, 2 Side w/ Posts.
d.	JPMCM1P, Medium Message Center, Recycled plastic, 1 Side w/ Posts.
e.	JPMCM1W, Medium Message Center, Recycled plastic, 1 Side Wall Mount.
f.	JPMCM2P, Medium Message Center, Recycled plastic, 2 Side w/ Posts.
g.	JPMCS1P, Small Message Center, Recycled plastic, 1 Side w/ Post.
h.	JPMCS1W, Small Message Center, Recycled plastic, 1 Side Wall Mount.
2.	Recycled Plastic Tables:
a.	JPPT63, 6 feet Table-3 Legs, 6 feet, Black recycled plastic.
b.	JPPT83, 8 feet Table-3 Legs, 8 feet, Black recycled plastic.
c.	JPPT83ADA, 8 feet Table-3 Legs, 8 feet, Black recycled plastic.
d.	RPT722S, 6 feet Table with 2 Seats, 6 feet, Black recycled plastic.
e.	RPT721S, 6 feet Table with 1 Seat, 6 feet, Black recycled plastic. 
f.	JPHT, Hexagon Table, Black recycled plastic.
g.	JPHTADA, Hexagon Table ADA, Black recycled plastic.
h.	JPAFCS4, 4 feet Child Size Recycled Plastic Table, 4 feet, Black recycled plastic.
i.	JPAF6ADA, 6 feet "A" Frame, ADA Accessible Recycled Plastic Table, 6 feet, Black recycled plastic.
j.	JPAF6, 6 feet "A" Frame Recycled Plastic Table, 6 feet, Black recycled plastic
3.	Recycled Plastic Receptacles:
a.	JPSLR32, 32 Gal. Square Receptacles, Black recycled plastic, Free Standing.
b.	JPRLR32, 32 Gal. Round Receptacles, Black recycled plastic, Free Standing.
c.	JPRLR55, 55 Gal. Round Receptacle, Black recycled plastic, Free Standing.
d.	JPTLR20, 20 Gal. Round Traditional Receptacle, Cast Aluminum, Free Standing.
e.	JPTLR32, 32 Gal. Round Traditional Receptacle, Cast Aluminum, Free Standing.
f.	JP32LINER, 32 Gallon Plastic Liner.
g.	JP55LINER, 55 Gallon Plastic Liner.
4.	Recycled Plastic Benches:
a.	JPSB42, Backless Bench -2 Legs, 4 feet, Black recycled plastic.
b.	JPSB63, Backless Bench -3 Legs, 6 feet, Black recycled plastic.
c.	JPSB83, Backless Bench -3 Legs, 8 feet, Black recycled plastic. 
d.	JPAB4, Bench with Back, 4 feet, Cast Aluminum, Green, Black.
e.	JPAB5, Bench with Back, 5 feet, Cast Aluminum, Green, Black.
f.	JPAB6, Bench with Back, 6 feet, Cast Aluminum, Green, Black.
g.	JPCB4, Bench with back -2 Legs, 4 feet, Black recycled plastic.
h.	JPCB6, Bench with back -3 Legs, 6 feet, Black recycled plastic.
i.	JPCB8, Bench with back -3 Legs, 8 feet, Black recycled plastic.
j.	JPCB42, Bench with back -2 Legs, 4 feet, Black recycled plastic.
k.	JPCB63, Bench with back -3 Legs, 6 feet, Black recycled plastic.
l.	JPCB83, Bench with back -3 Legs, 8 feet, Black recycled plastic.
m.	RCB48B, Bench with Back - 2 Legs, 4 feet, Black recycled plastic,.
n.	RCB60B, Bench with Back - 3 Legs, 5 feet, Black recycled plastic.
o.	RCB72B, Bench with Back, 6 feet, Black recycled plastic.
p.	RMB48NB, Backless Bench - 2 Legs, 4 feet, Black recycled plastic.
q.	RMB60NB, Backless Bench - 3 Legs, 5 feet, Black recycled plastic.
r.	RMB72NB, Backless Bench - 3 Legs, 6 feet, Black recycled plastic.
s.	4CB3RP, 4 feet Frame with Recycled Plastic 3 x 4 Contour Park Bench, 4 feet, 3/8 x 4 inch Rolled steel, Coated Black.
t.	6CB3RP, 6 feet, 3/8 x 4 inch Rolled steel, Coated Black.
u.	6CB4RP, 6 feet, 3/8 x 4 inch Rolled steel, Coated Black.
v.	8CB4RP, 8 feet, 3/8 x 4 inch Rolled steel, Coated Black.
w.	62PG-RPS, 6 feet Recycled Plastic, 2 x 4 inch Slats, 6 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
x.	62PG-RRP, 6 feet Recycled Plastic, 2 x 10 inch Plank, 6 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized
y.	82PG-RPS, 8 feet Recycled Plastic, 2 x 4 inch Slats, 8 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
z.	82PG-RRP, 8 feet Recycled Plastic, 2 x 10 inch Plank, 8 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
aa.	62PGL-RRP, 6 feet Recycled Plastic, 2 x 10 inch Plank for Portable Bench without Back, 6 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
ab.	82PGL-RRP, 8 feet Recycled Plastic, 2 x 10 inch Plank for Portable Bench without Back, 8 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
ac.	152SG-A, 15 feet Aluminum, 2 x 10 inch Plank for Stationary Bench with Back, 15 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
ad.	62SG-RPS, 6 feet Recycled Plastic, 2 x 4 inch Slats for Stationary Bench with Back, 6 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
ae.	62SG-RRP, 6 feet Recycled Plastic, 2 x 10 inch Plank for Stationary Bench with Back, 6 feet, 2 3/8 inch O.D. Tube,Black Powder Coating, Standard: Galvanized.
af.	82SG-RPS, 8 feet Recycled Plastic, 2 x 4 inch Slats for Stationary Bench with Back, 8 feet, 2 3/8 inch O.D. Tube, Black Powder Coating Standard: Galvanized.
ag.	82SG-RRP, 8 feet Recycled Plastic, 2 x 10 inch Plank for Stationary Bench with Back, 8 feet, 2 3/8 inch O.D. Tube, Black Powder Coating Standard: Galvanized.
ah.	62SGL-RRP, 6 feet Recycled Plastic, 2 x 10 inch Plank for Stationary Bench without Back, 6 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
ai.	82SGL-RRP, 8 feet Recycled Plastic, 2 x 10 inch Plank for Stationary Bench without Back, 8 feet, 2 3/8 inch O.D. Tube, Black Powder Coating, Standard: Galvanized.
aj.	WS6FCBRP, Windsor Select Bench Backless, 6 feet, Steel, Coated Black Powder.
ak.	WS6LCBRP, Windsor Select Bench with Back, 6 feet, Steel, Coated Black Powder.
5.	Landscape Timbers:
a.	JPLT8, 8 feet Railroad Tie.
6.	Car Stops:
a.	JPCS8, 6 feet 3 inch Car Stop.
7.	ECO-Series Recycled Plastic Products:
a.	PR4CMB, Curved Mesa Bench, Brown RP, Gray RP.
D.	Outdoor Grills and Fire Rings:
1.	Group Grills:
a.	SPD450, Group Grill w/ 1 Side Shelf, Surface Mount, 1368 sq. inch, SPDUT (12 x 36 Utility Shelf).
b.	SPD450IG, Group Grill w/ 1 Side Shelf, In Ground Mount, 1368 sq. inch.
c.	SPDUT, Additional 12 inch x 36 inch Shelf for SPD450 Group Grill, 432 sq. inch.
d.	SB3628U, Group Grill- Surface Mount, Quick Ship item, 1008 sq. inch.
e.	SB3628UIG, Group Grill- In Ground Mount, Quick Ship item, 1008 sq. inch.
f.	XB16, Group Grill, Two Pedestal, In Ground Mounting, 860 sq. inch.
g.	XB16SM, Group Grill, Two Pedestal, Surface Mount, 860 sq. inch.
2.	Covered Grills:
a.	ECG1929, Covered Grill- 19.5 x 29.25 x 16.5 inch 320 sq. inch ECPCB (Portable Caster Base), ECSUS (Utility Shelf).
b.	ECG1941, Covered Grill- 19.5 x 41.5 x 16.5 inch 500 sq. inch ECPCB (Portable Caster Base), ECSUS (Utility Shelf).
c.	ECSUS, Optional Side Utility Shelf for Covered Grill.
d.	ECPCB, Optional Portable Castor Base for Covered Grill. 
3.	MB16 Pedestal Grills:
a.	MB16, 2 3/8 Inc, 280 sq. inch, In-Ground, Surface Mount, UT (Painted Shelf).
b.	MB1635, 3 1/2 inch, 280 sq. inch, In-Ground, Surface Mount, UT (Painted Shelf).
c.	MB14, 2 3/8 inch, 280 sq. inch, In-Ground, Surface Mount, UT (Painted Shelf)
d.	MB1435, 3 1/2 inch, 280 sq. inch, In-Ground, Surface Mount .
e.	UT, 160 sq. inch.
4.	SB16 Pedestal Grills:
a.	SB16, Painted Black w/ Galv. Pedestal, 2 3/8 inch, 300 sq. inch, In-Ground, Surface Mount, UT (Painted Shelf).
b.	SB16G, All Galvanized, 2 3/8 inch, 300 sq. inch, In-Ground, Surface Mount, UTG (Galvanized Shelf).
c.	SB1635, Painted Black w/ Galv. Pedestal, 3 1/2 inch, 300 sq. inch, In-Ground, Surface Mount, UT (Painted Shelf).
d.	SB1635G, All Galvanized, 3 1/2 inch, 300 sq. inch, In-Ground Surface Mount, UTG (Galvanized Shelf)
e.	UT, Painted Black, 160 sq. inch.
f.	UTG, Galvanized,160 sq. inch.
5.	SF16 Pedestal Grills:
a.	SF16, Painted Black w/ Galv. Pedestal, 2 3/8 inch, 300 sq. inch, In-Ground, Surface Mount, UT (Painted Shelf.)
b.	SF16G, All Galvanized, 2 3/8 inch, 300 sq. inch, In-Ground, Surface Mount, UTG (Galvanized Shelf)
c.	SF1635, Painted Black w/ Galv. Pedestal, 3 1/2 inch, 300 sq. inch, In-Ground, Surface Mount, UT (Painted Shelf)
d.	SF1635G, All Galvanized, 3 1/2 inch, 300 sq. inch, In-Ground, Surface Mount, UTG (Galvanized Shelf).
e.	UT, Painted Black, 160 sq. inch.
f.	UTG, Galvanized, 160 sq. inch.
6.	Fire Rings:
a.	FR730TB, FR730 Fire Ring with Tilt Back Staples.
b.	FR730SAS, FR730 Fire Ring with Spade Anchors.
c.	FR930TB, FR930 Fire Ring with Tilt Back Staples.
d.	FR930SAS, FR930 Fire Ring with Spade Anchors.
e.	FR1130TB, FR1130 Fire Ring with Tilt Back Staples.
f.	FR1130SAS, FR1130 Fire Ring with Spade Anchors.
g.	FR1830WCSAS, ADA Accessible Fire Ring.
h.	AFG80TB, AFG80 Fire Ring with Tilt Back Staples.
i.	AFG80SAS, AFG80 Fire Ring with Spade Anchors.
j.	AFG80WCSAS, ADA Accessible Fire Ring.
7.	Hot Ash Receptacle:
a.	CHAR2235, Hot Ash Receptacle, 24 inch Sq. x 35 inch High inch.
E.	Trash Receptacles:
1.	132LR Series Litter Receptacles:
a.	132LR, Frame only, 32 Gal.
b.	132LRSYP, Southern Yellow Pine, 32 Gal.
c.	132LRRPS, Recycled Plastic, 32 Gal.
d.	CG32, galvanized lid and liner.
e.	CP32, plastic liner.
f.	DLG55, Galvanized Dome Lid.
g.	DLTH32, 22 3/4 inch I.D. fits 122LRVP, 132LRVP, 32 gal. Wood, Recycled Plastic and Windsor Series receptacles. Comes in gray only.
h.	PCVL, Convex plastic lid for W3032LRRP Windsor, 132LRSYP & 132LRRPS litter receptacles only. Comes in Black only.
i.	PCCL, Concave plastic lid for W3032LRRP Windsor, 132LRSYP & 132LRRPS litter receptacles only. Comes in Gray only.
2.	SLR Series Litter Receptacles:
a.	SLR, Frame Only for SLR Series Litter Receptacle (no slats), 20 Gal., In-Ground Mount, Surface Mount.
b.	SLR24, SLR Series Litter Receptacle with Mahogany Stained Pine Slats, In-Ground Mount, Surface Mount.
c.	CP20, 20 Gal. Plastic Can.
d.	DLP20, Painted Steel Dome Lid.
e.	DLMP22, Plastic Dome Lid - Brown Only.
3.	CPW Wood Canpost Litter Receptacles:
a.	CPW-S, Single Side Wood Holder, In-Ground Mount.
b.	CPW-D, Double Side Wood Holder, In-Ground Mount.
c.	CPH-D, Double Side Hardware Only, In-Ground Mount.
d.	CPRP-S, Single Side Recycled Plastic Holder, In-Ground Mount.
e.	CPRP-D, Double Side Recycled Plastic Holder.
f.	CG32, 2 Gal. Galvanized Can.
g.	CG20, 20 Gal. Galvanized Can.
h.	DLG30, Galvanized Dome Lid.
4.	CAP Galvanized Canpost Litter Receptacles:
a.	CG32, 2 Gal. Galvanized Can.
b.	CG20, 20 Gal. Galvanized Can.
c.	DLG30, Galvanized Dome Lid.
d.	CAP-S, Single Side Galvanized Post, In-Ground Mount.
e.	CAP-D, Double Side Galvanized Post, In-Ground Mount.
5.	Windsor Series Litter Receptacles:
a.	WS3032LRRP, Windsor Series Litter Receptacle.
b.	3032LRIG, In-Ground Post for Windsor Series Receptacle.
c.	PCVL, Convex Plastic Lid 12 inch Opening.
d.	PCCL, Concave Plastic Lid, 8 inch Opening.
e.	CP32, 32 Gal. Plastic Can.
f.	DLTH32, Plastic Top Hat Lid
6.	Lids and Liners:
a.	CG32, 32 Gal. Galvanized Can.
b.	CG20, 20 Gal. Galvanized Can.
c.	PCCL, Concave Plastic Lid, 8 inch Opening.
d.	PCVL, Convex Plastic Lid 12 inch Opening.
e.	CP32, 32 Gal. Plastic Can.
f.	CP20, 20 Gal. Plastic Can.
g.	DLP20, Painted Steel Dome Lid.
h.	PLH32-55, Plastic Hood Lid.
i.	DLG30, Galvanized Dome Lid.
j.	DLG55, Galvanized Dome Lid..
k.	DLTH32, Plastic Top Hat Lid.
l.	DLMP32-55, Plastic Dome Lid, Plastic Dome Lid.
m.	DLMP22, Plastic Dome Lid - Brown Only.
n.	FLS8-32, Steel Lid with 8 inch Hole for 32 Gal. Receptacle.
o.	FLS8-55, Steel Lid with 8 inch Hole for 55 Gal. Receptacle.
p.	FLS16-32, Steel Lid with 16 inch Hole for 32 Gal. Receptacle.
q.	FLS16-55, Steel Lid with 16 inch Hole for 55 Gal. Receptacle
7.	Round Plastisol Litter Receptacles:
a.	122LRVP, Round Plastisol Free Standing Receptacle.
b.	122LRVPSM, Round Plastisol Surface Mount Receptacle.
c.	122LRVPIG, Round Plastisol In-Ground Mount Receptacle.
d.	132LRVP, Round Plastisol Free Standing Receptacle.
e.	132LRVPSM, Round Plastisol Surface Mount Receptacle.
f.	132LRVPIG, , Round Plastisol In-Ground Mount Receptacle.
g.	155LRVP, Round Plastisol Free Standing Receptacle.
h.	155LRVPSM, Round Plastisol Surface Mount Receptacle.
i.	155LRVPIG, Round Plastisol In-Ground Mount Receptacle.
j.	CP32, 32 Gal. Plastic Can.
k.	CP20, 20 Gal. Plastic Can.
l.	PLH32-55, Plastic Hood Lid.
m.	DLTH32, Plastic Top Hat Lid.
n.	DLMP32-55, Plastic Dome Lid.
8.	Square Litter Receptacles:
a.	S32LRVPC, Expanded Metal Square Litter Receptacle with Arch Cover.
b.	S32LRVPCSM, Expanded Metal Square Litter Receptacle with Arch Cover.
c.	S32LRWR, Welded Rod Square Litter Receptacle with Arch Cover.
d.	S32LRWRSM, Welded Rod Square Litter Receptacle with Arch Cover.
e.	S32LRLC, Laser Cut Square Litter Receptacle with Arch Cover. Gal.
f.	S32LRLCSM, Laser Cut Square Litter Receptacle with Arch Cover.
9.	Perforated Series Litter Receptacles:
a.	PS32LR, Perforated Receptacle.
b.	SI32LR, Personalized Receptacle.
c.	PSLRSM, Surface Mount Kit.
d.	PSLRIG, In-Ground Mount Kit.
e.	PSLR32L, Plastic Liner with Rope Handles.
f.	PSLRABT, Ash Bonnet Top for Receptacle.
g.	PSLRCXT, Convex Top for Receptacle.
h.	PSLRCVT, Concave Top for Receptacle.
10.	52 gal. Steel Mesh Trash Baskets:
a.	DLG55, Galvanized Dome Lid.
b.	DLMP32-55, Plastic Dome Lid.
c.	SMTB52, Galvanized Steel Mesh Trash Basket.
d.	SMTB52C, Powder Coated Steel Mesh Trash Basket.
e.	SMTB52HD, Heavy Duty Galvanized Steel Mesh Trash Basket.
f.	SMTB52HDC, Heavy Duty Powder Coated Steel Mesh Trash Basket.
11.	Outdoor Stone Panel Receptacles:
a.	SPR12WUMB, Brown w/ Black Top, 14x32 inch.
b.	SPR-36HT-DG, Dark Green, 29 Gal., 22 x 40 inch.
c.	SPR-36HT-LG, Light Gray, 29 Gal., 22 x 40 inch.
d.	SPR-36HT-MB, Medium Brown, 29 Gal., 22 x 40 inch.
e.	SPR-38HT-DG, Dark Green, 38 Gal., 26 x 40 inch.
f.	SPR-38HT-LG, Light Gray, 38 Gal., 26 x 40 inch.
g.	SPR-38HT-MB, Medium Brown, 38 Gal., 26 x 40 inch.
h.	SPR-48HT-DG, Dark Green, 48 Gal., 26 x 40 inch.
i.	SPR-48HT-LG, Light Gray, 48 Gal., 26 x 40 inch.
j.	SPR-48HT-MB, Medium Brown, 48 Gal., 26 x 40 inch.
k.	SPR-18AT-DG, Dark Green, 18 Gal., 18 x 32 inch.
l.	SPR-18AT-LG, Light Gray, 18 Gal., 18 x 32 inch.
m.	SPR-18AT-MB, Medium Brown, 18 Gal., 18 x 32 inch.
n.	SPR-12AT-DG, Dark Green, 12 Gal., 14 x 32 inch.
o.	SPR-12AT-LG, Light Gray, 12 Gal., 14 x 32 inch.
p.	SPR-12AT-MB, Medium Brown, 12 Gal., 14 x 32 inch.
q.	SPR-02AT-DG, Dark Green, 2 Gal., 10 x 24 inch.
r.	SPR-02AT-LG, Light Gray, 2 Gal., 10 x 24 inch.
s.	SPR-02AT-MB, Medium Brown, 2 Gal., 10 x 24 inch.
t.	SPR-00AT-DG, Dark Green, 10 x 24 inch.
u.	SPR-00AT-LG, Light Gray, 10 x 24 inch.
v.	SPR-00AT-MB, Medium Brown, 10 x 24 inch.
w.	SPR-12FT-DG, Dark Green, 12 Gal., 14 x 32 inch.
x.	SPR-12FT-LG, Light Gray, 12 Gal., 14 x 32 inch.
y.	SPR-12FT-MB, Medium Brown, 12 Gal., 14 x 32 inch.
12.	Indoor-Outdoor Receptacles:
a.	MRLR35, 20 x 20x 39 inch, 35 Gal.
b.	MRLR50, 24 x 24 x 49 inch, 50 Gal.
13.	Hot Ash Receptacle:
a.	CHAR2235, Concrete Hot Ash Receptacle, 24 inch Sq. x 35 inch High inch.
14.	Stone Panel and Metal Receptacles:
a.	LRSP322748, 32 gal. capacity, hinged lid, powder coated black frame with stone panels, standard. Available in custom colors.
15.	Recycled Plastic Receptacles:
a.	JPSLR32, 32 Gal. Square Receptacles, Black recycled plastic, Free Standing.
b.	JPRLR32, 32 Gal. Round Receptacles, Black recycled plastic, Free Standing.
c.	JPRLR55, 55 Gal. Round Receptacle, Black recycled plastic, Free Standing.
d.	JPTLR20, 20 Gal. Round Traditional Receptacle, Cast Aluminum, Free Standing.
e.	JPTLR32, 32 Gal. Round Traditional Receptacle, Cast Aluminum, Free Standing.
f.	JP32LINER, 32 Gallon Plastic Liner.
g.	JP55LINER, 55 Gallon Plastic Liner.
16.	Iron Valley Trash Receptacles:
a.	IVILRPC, 45 Gal. Receptacle 23 x 50 inch, Ductile Iron and Steel, Powder coating.
b.	IVAT, Ashtray Top and Rain Cover, Ductile Iron and Steel, Powder coating.
17.	Strap Steel Trash Receptacles:
a.	SSASLR32, 32 Gallon Litter Receptacle, 3/4 inch solid steel.
b.	SSVSLR32, 32 Gal. "V" Style Litter Receptacle, 3/4 inch solid steel.
c.	SSHRLRCS, 32 Gal. Round Litter Receptacle with Snuffer Top, 3/4 inch solid steel.
18.	Concrete Trash Containers:
a.	CTCR30AR, CTCR30AR Concrete Trash Container, 26 inch, 33 inch.
b.	CTCR30PL, CTCR30PL - 30 Gal. Liner.
c.	CTCR30AP, CTCR30AP Concrete Trash Container, 24 inch, 33 inch.
d.	CTCR30MD, CTCR30MD Concrete Trash Container, 24 inch, 43 inch.
e.	CTCR30PH, CTCR30PH Concrete Trash Container, 26 1/4 inch, 44 inch.
f.	CTCR30AK, CTCR30AK Concrete Trash Container, 30 inch, 36 inch.
g.	CTCR22FP, CTCR22FP Concrete Trash Container, 21 inch, 33 inch.
h.	CTCR20PL, CTCR20PL- 20 Gal. Liner.
i.	CTCR30FP, CTCR30FP Concrete Trash Container, 31 inch, 33 inch.
j.	CHAR2235, Hot Ash Receptacle, 35 inch.
k.	CTCS22FP, Popular Square Trash Container- 22 gal. Unit.
l.	CTC20PL, Popular Square Trash Container- 20 gal. Liner.
m.	CTCS30FP, Unit Popular Square Trash Container- 30 gal. Unit.
n.	CTC30PL, Popular Square Trash Container- 30 gal. Liner.
o.	CTCS22PB, Square Receptacle- 22 gal. Unit.
p.	CTCS40PB, Square Receptacle- 40 gal. Unit.
q.	CTC36PL, Square Receptacle- 36 gal. Liner.
r.	CTCS30FT, Large Capacity Receptacle- 45 gal. Unit.
s.	CTC45PL, Large Capacity Receptacle- 45 gal. Liner.
t.	WTTF, Concrete 3 Station Recycling Center.
19.	Tuffcan:
a.	TC42LR, complete with dome and lid, 42 gal. liner. Neutral brown. 28 inch h x 42 inch dia. 
F.	Fiberglass Pedal Boats:
1.	Pedal Cruisers:
a.	PCII GLITTER, 2 Person Glitter Finish Pedal Cruiser.
b.	PCIV GLITTER, 4 Person Glitter Finish Pedal Cruiser.
c.	PCI, 2 Person Pedal Cruiser.
d.	PCIV, 4 Person Pedal Cruiser. 
e.	PCIVCOVER, Weather Cover for PCIV Boat Light Gray, Pedal Cruiser Cover.
f.	CANOPY, White Pedal Cruiser Canopy, Pedal Cruiser Canopy.
G.	Concrete Site Amenities:
1.	Concrete Tables:
a.	CTR4S, Round Top 4 Seat, 68 inch, 30 inch, 68 inch.
b.	CTR3H, Round Top 3 Seat for Wheelchair Access.
c.	UMBRKT, Optional- Umbrella Bracket for Round Concrete Table.
d.	CTO4S, Octagon Top 4 Seat, 66 inch, 29 inch, 66 inch.
e.	CTS4S, Square Top 4 Seat, 66 inch, 29 inch, 66 inch
f.	CTS2S, Square Top 2 Seats, 30 inch, 29 inch, 66 inch.
g.	UMBKT, Optional- Umbrella Bracket for Square or Octagon Tables.
h.	CTR6MTP, Rectangle Mesh Top, 72 inch, 29 inch, 66 inch.
i.	CTR8MTP, Rectangle Mesh Top, 96 inch, 29 inch, 66 inch.
j.	CTRJ60C, Rectangle Top, 60 inch, 29 inch, 58 inch.
k.	CTRJ84C, Rectangle Top, 84 inch, 29 inch, 58 inch.
l.	CTRJ84H, Handicap Rectangle Top, 84 inch, 29 inch, 58 inch.
m.	CTRJ84R, Redwood Rectangle Top, 84 inch, 29 inch, 58 inch.
n.	CTOV72, Oval Top, 72 inch, 30 inch, 60 inch.
o.	CTOV84, Oval Top, 84 inch, 30 inch.
p.	CTOV84H, Oval Top for Wheelchair Access, 84 inch, 30 inch, 60 inch.
q.	CMT84C, Concrete Monster Table, 84 inch, 29 inch, 62 inch.
r.	CMT84H, Concrete Monster Table with Handicap Benches, 84 inch, 29 inch, 62 inch.
s.	CTRT84C, Rectangular Top, 84 inch, 30 inch, 62 inch.
t.	CTRT96C, Rectangular Top, 96 inch, 30 inch, 62 inch.
u.	GBI, Game Board Insert.
2.	Concrete Basketball Goal:
a.	WTBS, Concrete Basketball Goal System.
3.	Concrete Drinking Fountains:
a.	CHFFBS, Handicap Accessible Drinking Fountain- Standard., Chrome Bowl.
b.	CHFFBC, Handicap Accessible Drinking Fountain- Standard.
c.	CHFFBCT, Handicap Accessible Drinking Fountain- Tamper Guard.
d.	CHFFBSF, Handicap Accessible Drinking Fountain- Freeze Proof.
e.	CHFFBSTF, Handicap Accessible Drinking Fountain- Tamper Guard and Freeze Proof.
f.	CDFPBC, Vertical Upright Cylindrical Drinking Fountain- Push Button Bubbler.
g.	CDF1BC, Vertical Upright Cylindrical Drinking Fountain- 1 Side Button.
h.	CDF1BCF, Vertical Upright Cylindrical Drinking Fountain- Push Button and Freeze Proof Valve.
i.	CDFFBS, Vertical Upright Cylindrical Drinking Fountain- Front Push Button.
j.	CDFOCS, Optional Concrete Child Step for Vertical Upright Cylindrical Drinking Fountain.
k.	CWFS, Wall Mounted Chrome Bowl Drinking Fountain.
l.	CWFC, Wall Mounted Concrete Bowl Drinking Fountain.
m.	CDHF2BS, Dual-Height Concrete Drinking Fountain.
n.	CDFOSF, Optional Side Faucet for any Concrete Drinking Fountain.
4.	Concrete Planters:
a.	CPR2417, Ever Popular Round Planters, 24 inch dia., 17 inch height.
b.	CPR2424, Ever Popular Round Planters, 24 inch dia., 24 inch height.
c.	CPR2433, Ever Popular Round Planters, 24 inch, 33 inch.
d.	CPR3017, Ever Popular Round Planters, 30 inch, 17 inch.
e.	CPR3030, Ever Popular Round Planters, 30 inch, 30 inch.
f.	CPR3624, Ever Popular Round Planters, 36 inch, 24 inch.
g.	CPR3630, Ever Popular Round Planters, 36 inch, 30 inch.
h.	CPR4817, Ever Popular Round Planters, 48 inch, 17 inch.
i.	CPR4824, Ever Popular Round Planters, 48 inch, 24 inch.
j.	CPR6036, Ever Popular Round Planters, 60 inch, 36 inch.
k.	CPAR3622, Aspen Round Planters, 36 inch, 22 inch.
l.	CPAR4836, Aspen Round Planters, 48 inch, 36 inch.
m.	CPAR6036, Aspen Round Planters, 60 inch, 36 inch.
n.	CPAR3630, Aspen Round Planters, 36 inch, 30 inch.
o.	CTCA-30AP, Aspen Trash Receptacle, 31 inch, 38 inch.
p.	CSA-2319, Aspen Ash Urn- Snuffer, 19 inch, 23 inch.
q.	CPRR2424, Brighton Planters- 24 inch Dia., 24 inch, 24 inch.
r.	CPRR4224, Brighton Planters- 42 inch - 24 inch Dia., 42 inch, 24 inch.
s.	CPS1818, Rectangular and Square Planters, 18 inch.
t.	CPS2428, Rectangular and Square Planters, 28 inch.
u.	CPS3630, Rectangular and Square Planters, 30 inch.
v.	CPS4230, Rectangular and Square Planters, 30 inch.
w.	CP183320, Rectangular and Square Planters, 20 inch.
x.	CP184820, Rectangular and Square Planters, 20 inch.
y.	CP186020, Rectangular and Square Planters, 20 inch.
z.	CP187220, Rectangular and Square Planters, 20 inch.
aa.	CP244830, Rectangular and Square Planters, 30 inch.
ab.	CPAS2418, Square and Rectangular Aspen Planters, 18 inch.
ac.	CPAS2436, Square and Rectangular Aspen Planters, 18 inch .
ad.	CPAS2448, Square and Rectangular Aspen Planters, 30 inch.
ae.	CPAS3648, Square and Rectangular Aspen Planters, 36 inch. 
af.	CPAS4848, Square and Rectangular Aspen Planters, 36 inch,.
ag.	CPAS3660, Square and Rectangular Aspen Planters, 36 inch.
ah.	CPAS3672, Square and Rectangular Aspen Planters, 36 inch.
ai.	CPAS1660, Square and Rectangular Aspen Planters, 18 inch.
aj.	CPAS2472, Square and Rectangular Aspen Planters, 18 inch.
ak.	CPSW2424, Southwest Look Dish style Planters, 24 inch, 24 inch.
al.	CPSW3017, Southwest Look Dish style Planters, 30 inch, 17 inch.
am.	CPSW4817, Southwest Look Dish style Planters, 48 inch, 17 inch.
an.	CTCRS30A, Matching Trash Receptacle, 24 inch, 33 inch.
5.	Concrete Snuffers:
a.	CSR-1130, High Round Snuffer- 11 inch Dia x 30 inch, 11 inch, 30 inch.
b.	CSK-1524, High Round Snuffer- 15 inch Dia x 24 inch, 15 inch, 24 inch.
c.	CSR-1324, High Round Snuffer- 13 inch Dia x 24 inch, 13 inch, 24 inch.
d.	CSR-1224, High Round Snuffer- 12 inch Dia x 24 inch, 12 inch, 24 inch.
e.	CSR-1124, High Round Snuffer- 11 inch Dia x 24 inch, 11 inch, 24 inch.
f.	CSR-1117, High Round Snuffer- 11 inch Dia x 17 inch, 11 inch, 17 inch.
g.	CSA-2319, High Round Snuffer- 19 inch Dia x 23 inch, 19 inch, 23 inch.
h.	CSS-1632, High Square Snuffer- 16 inch Dia x 32 inch, 16 inch, 32 inch.
i.	CSS-1424, High Square Snuffer- 14 inch Dia x 24 inch, 14 inch, 24 inch.
j.	CSS-1230, High Square Snuffer- 12 inch Dia x 30 inch, 12 inch, 30 inch.
k.	CSS-1521, High Square Snuffer- 15 inch Dia x 21 inch, 15 inch, 21 inch,.
l.	CSV-1524, High Square Snuffer- 15 inch Dia x 24 inch, 15 inch, 24 inch.
m.	CSS-1824, High Square Snuffer- 18 inch Dia x 24 inch, 18 inch, 24 inch.
n.	CSS-1224, High Square Snuffer- 12 inch Dia x 24 inch, 12 inch, 24 inch,.
o.	CSTD-1440, Snuffer/Trash Combination Unit- 14 x 21 x 22 inch, 14 inch, 40 inch.
p.	CSTR-1230, Snuffer/Trash Combination Unit- 12 inch Dia x 30 inch, 12 inch, 30 inch.
q.	CSTR-1332, Snuffer/Trash Combination Unit- 13 inch Dia x 32 inch, 13 inch.
r.	CSOSK, Stainless Steel Skimmer, 5 inch.
6.	Concrete Bollards:
a.	CBRD, 12 inch dia., 54 inch ht.
b.	CBS16, 16 Sq. inch, 28 inch.
c.	CBRP, 20 inch, 40 inch.
d.	CBS24, 24 Sq. inch, 40 inch.
e.	CBRT10, 10 inch, 34 inch.
f.	CBPB, 12 inch, 35 inch.
g.	CBS12, 12 Sq. inch, 35 inch.
h.	CBSL, 12 Sq. inch, 42 inch.
i.	CBRL, 12 inch, 54 inch.
j.	CBR18, 18 inch, 35 inch.
k.	CBR12, 12 inch, 34 inch.
l.	CBH, 6x12 inch, 48 inch.
m.	CBRT12, 12 inch, 30 inch.
n.	CBRF, 12 inch, 30 inch.
7.	Concrete Benches:
a.	CCB72CL, 72 inch, 18 inch.
b.	CMB84R, 84 inch, 19 inch.
c.	CMB90C, 90 inch, 18 inch.
d.	CFB84C, 84 inch, 17 inch.
e.	CHB72VP, 72 inch, 17 inch.
f.	CSB72VP, 72 inch, 17 inch.
g.	CTB58C, 58 inch, 18 1/2 inch.
h.	CTB72C, 72 inch, 18 1/2 inch.
i.	CTB84C, 84 inch, 18 1/2 inch.
j.	CPB58C, 58 inch, 33 inch.
k.	CPB72C, 72 inch, 33 inch.
l.	CPB84C, 84 inch, 33 inch.
m.	CPB84R, 84 inch, 33 inch.
n.	CSB84R, 84 inch, 33 inch.
o.	CKIB84C, 84 inch, 37 inch.
p.	CPB72M, 72 inch, 33 inch.
q.	CPB96M, 96 inch, 33 inch.
r.	CPB60X, 60 inch, 34 inch.
s.	HLB4, 48 inch, 18 inch.
t.	HLB6, 72 inch, 18 inch.
u.	HLB8, 96 inch, 18 inch.
8.	Precast Stone Furnishings:
a.	SFRPTH, ADA Precast Stone Round Table, 30 inch, 66 inch, 66 inch.
b.	SFRPT, Precast Stone Round Table, 30 inch, 66 inch, 66 inch.
c.	SFSPTH, ADA Precast Stone Square Table, 30 inch, 65 inch, 65 inch.
d.	SFSPT, Precast Stone Square Table, 30 inch, 65 inch.
e.	SFPB72, Precast Stone Bench w/Back, 72 inch.
H.	Strap Steel Furnishings:
1.	Iron Valley Benches:
a.	IVB48PC, 48 inch Long Bench with Back, Ductile Iron and Steel, Powder coating, 48 inch.
b.	IVB60PC, 60 inch Long Bench with Back, Ductile Iron and Steel, Powder coating, 60 inch.
c.	IVB72PC, 72 inch Long Bench with Back, Ductile Iron and Steel, Powder coating, 72 inch.
d.	IVB96PC, 96 inch Long Bench with Back, Ductile Iron and Steel, Powder coating, 96 inch.
e.	IVBB48PC, 48 inch Backless Bench, Ductile Iron and Steel, Powder coating, 48 inch.
f.	IVBB60PC, 60 inch Backless Bench, Ductile Iron and Steel, Powder coating, 60 inch.
g.	IVBB72PC, 72 inch Backless Bench, Ductile Iron and Steel, Powder coating, 72 inch.
h.	IVBB96PC, 96 inch Backless Bench, Ductile Iron and Steel, Powder coating, 96 inch.
2.	Iron Valley Tables:
a.	IVPTSP3, 36 inch Sq. Table only, Ductile Iron and Steel, Powder coating, 36 inch, length.
b.	IVPTCB2, 24 inch Chair with Back, Ductile Iron and Steel, Powder coating.
c.	IVPTC2, 24 inch Chair without Back, Ductile Iron and Steel, Powder coating.
d.	IVMPT6, 6 feet Multipost Table w/ Benches, Ductile Iron and Steel, Powder coating, 72 inch, length.
e.	IVMPT8, 8 feet Multipost Table w/ Benches, Ductile Iron and Steel, Powder coating, 96 inch, length.
3.	Iron Valley Trash Receptacles:
a.	IVILRPC, 45 Gal. Receptacle 23 x 50 inch, Ductile Iron and Steel, Powder coating.
b.	IVAT, Ashtray Top and Rain Cover, Ductile Iron and Steel, Powder coating.
4.	Strap Steel Tables:
a.	SSHSST, One Pc., Square Table with Four Seats, 3/4 inch solid steel, free-standing or surface mount, several color options.
5.	Strap Steel Benches:
a.	SSABB48, . 48 inch L Backless Bench, 3/4 inch solid steel.
b.	SSABB72, . 72 inch L Backless Bench, 3/4 inch solid steel.
c.	SSAPB48, .48 inch L Park Bench with Back, 3/4 inch solid steel.
d.	SSAPB72, 72 inch L Park Bench with Back, 3/4 inch solid steel.
e.	SSCB48, 48 inch L Contour Bench with Back, 3/4 inch solid steel.
f.	SSCB72, 72 inch L Contour Bench with Back, 3/4 inch solid steel.
6.	Strap Steel Trash Receptacles:
a.	SSASLR32, 32 Gallon Litter Receptacle, 3/4 inch solid steel.
b.	SSVSLR32, 32 Gal. "V" Style Litter Receptacle, 3/4 inch solid steel.
c.	SSHRLRCS, 32 Gal. Round Litter Receptacle with Snuffer Top, 3/4 inch solid steel.
7.	Strap Steel Planters:
a.	SSAP3624, 36 inch sq. x 24 inch H Planter with Liner and Drain Holes, 3/4 inch solid steel, free standing or surface mount, several color options.
I.	Drinking Fountains and Coolers:
1.	Wall Mount Fountains:
a.	KP53SWF, Outdoor Use Wall Mounted Fountain, 20 inch, 8 inch.
b.	KP53SWFFP, Outdoor Use Wall Mounted Fountain Freezeproof, 20 inch, 8 inch.
c.	CWFS, Outdoor Use Wall Mounted Fountain, 14 inch, 9 inch.
d.	CWFC, Outdoor Use Wall Mounted Fountain, 14 inch, 9 inch.
2.	Water Coolers:
a.	CWC, Outdoor Use Floor Model Concrete Electric Cooler, 16 1/2 inch width x 32 inch height.
3.	Steel Drinking Fountains:
a.	KP59THF, Standard Triple Height Fountain.
b.	KP59THFFP, Freezeproof Triple Height Fountain.
c.	KP47SHF, Standard Wheelchair Accessible Fountain.
d.	KP47SHFFP, Freezeproof Wheelchair Accessible Fountain.
e.	KP57SDF, Standard Dual-Height Drinking Fountain.
f.	KP57SDFFP, Freezeproof Dual-Height Drinking Fountain.
g.	KP25SPF, Standard Cylindrical Pedestal Fountain.
h.	KP25SPFFP, Freezeproof Cylindrical Pedestal Fountain.
i.	KP44SEF, Standard Economical Fountain.
j.	KP62BFS, Standard Outdoor Shower and Footwash.
k.	KP53SWPF, Standard Cylinder with Pet Fountain.
4.	Concrete Drinking Fountains:
a.	CHFFBS, Handicap Accessible Drinking Fountain- Standard.
b.	CHFFBC, Handicap Accessible Drinking Fountain- Standard.
c.	CHFFBCT, Handicap Accessible Drinking Fountain- Tamper Guard.
d.	CHFFBSF, Handicap Accessible Drinking Fountain- Freeze Proof,.
e.	CHFFBSTF, Handicap Accessible Drinking Fountain- Tamper Guard and Freeze Proof.
f.	CDFPBC, Vertical Upright Cylindrical Drinking Fountain- Push Button Bubbler.
g.	CDF1BC, Vertical Upright Cylindrical Drinking Fountain- 1 Side Button.
h.	CDF1BCF, Vertical Upright Cylindrical Drinking Fountain- Push Button and Freeze Proof Valve.
i.	CDFFBS, Vertical Upright Cylindrical Drinking Fountain- Front Push Button.
j.	CDFOCS, Optional Concrete Child Step for Vertical Upright Cylindrical Drinking Fountain.
k.	CWFS, Wall Mounted Chrome Bowl Drinking Fountain.
l.	CWFC, Wall Mounted Concrete Bowl Drinking Fountain.
m.	CDHF2BS, Dual-Height Concrete Drinking Fountain.
n.	CDFOSF, Optional Side Faucet for any Concrete Drinking Fountain.
J.	Garden Furniture:
1.	"Shorea" Timeless Garden Series Furniture:
a.	TG2C, One Chair, for Dinning Table, 2 feet Arm Chair, 23 inch, 26 inch, 35 inch.
b.	TG4B, 4 feet Bench with Back, 48 inch, 26 inch, 35 inch.
c.	TG5B, 5 feet Bench with Back, 60 inch, 26 inch, 35 inch.
d.	TG5BB,5 feet Backless Bench, 60 inch, 21 inch, 17 inch.
e.	TG36CT,Cocktail Table, 36 inch, 20 inch, 17 inch.
f.	TG18ET, End Table, 18 inch, 18 inch, 17 inch.
g.	TG42DT, 42 inch Dining Table, 42 inch, 42 inch, 29 inch.
h.	TG2C, One Chair, for Dinning Table.
i.	TG22LR, Litter Receptacle, 22 inch, 22 inch, 33 inch.
j.	TG15P, 15 inch Planter, 15 inch, 15 inch, 15 inch.
k.	TG19P, 19 inch Planter, 19 inch, 19 inch, 17 inch.
K.	Bike Racks:
1.	Bike Racks Loop Style:
a.	611GIG, 15 inch length, 3 Spaces, 1 5/8 inch Pipe O.D.
b.	613GIG, 39 inch, 5, 1 5/8 inch.
c.	615GIG, 64 inch, 7, 1 5/8 inch.
d.	617GIG, 88 inch, 9, 1 5/8 inch.
e.	619GIG, 113 inch, 11, 1 5/8 inch.
f.	611CIG, 15 inch, 3, 1 5/8 inch.
g.	613CIG, 39 inch, 5, 1 5/8 inch.
h.	615CIG, 64 inch, 7, 1 5/8 inch.
i.	617CIG, 88 inch, 9, 1 5/8 inch.
j.	619CIG, 113 inch, 11, 1 5/8 inch.
k.	611GSM, 15 inch, 3, 1 5/8 inch.
l.	613GSM, 39 inch, 5, 1 5/8 inch.
m.	615GSM, 64 inch, 7, 1 5/8 inch.
n.	617GSM, 88 inch, 9, 1 5/8 inch.
o.	619GSM, 113 inch, 11, 1 5/8 inch.
p.	611CSM, 15 inch, 3, 1 5/8 inch.
q.	613CSM, 39 inch, 5, 1 5/8 inch.
r.	615CSM, 64 inch, 7, 1 5/8 inch.
s.	617CSM, 88 inch, 9, 1 5/8 inch.
t.	619CSM, 113 inch, 11, 1 5/8 inch.
u.	621GIG, 15 inch, 3, 2 3/8 inch.
v.	623GIG, 39 inch, 5, 2 3/8 inch.
w.	625GIG, 64 inch, 7, 2 3/8 inch.
x.	627GIG, 88 inch, 9, 2 3/8 inch.
y.	629GIG, 113 inch, 11, 2 3/8 inch.
z.	6211GIG, 143 inch, 13, 2 3/8 inch.
aa.	621CIG, 15 inch, 3, 2 3/8 inch.
ab.	623CIG, 39 inch, 5, 2 3/8 inch.
ac.	625CIG, 64 inch, 7, 2 3/8 inch.
ad.	627CIG, 88 inch, 9, 2 3/8 inch.
ae.	629CIG, 113 inch, 11, 2 3/8 inch.
af.	6211CIG, 143 inch, 13, 2 3/8 inch.
ag.	621GSM, 15 inch, 3, 2 3/8 inch.
ah.	623GSM, 39 inch, 5, 2 3/8 inch.
ai.	625GSM, 64 inch, 7, 2 3/8 inch.
aj.	627GSM, 88 inch, 9, 2 3/8 inch.
ak.	629GSM, 113 inch, 11, 2 3/8 inch.
al.	6211GSM, 143 inch, 13, 2 3/8 inch.
am.	621CSM, 15 inch, 3, 2 3/8 inch.
an.	623CSM, 39 inch, 5, 2 3/8 inch.
ao.	625CSM, 64 inch, 7, 2 3/8 inch.
ap.	627CSM, 88 inch, 9, 2 3/8 inch.
aq.	629CSM, 113 inch, 11, 2 3/8 inch,.
ar.	6211CSM, 143 inch, 13, 2 3/8 inch.
2.	Bike Racks Circle Style:
a.	3051, 5 feet, 4, 2 3/8 inch.
b.	3052, 5 feet, 8, 2 3/8 inch.
c.	3101, 10 feet, 7, 2 3/8 inch.
d.	3102, 10 feet, 14, 2 3/8 inch.
3.	Bike Racks Low Profile:
a.	4052, 5 feet length, 6 spaces, 1 5/8 inch Pipe O.D., 1 1/16 inch Tube O.D., 4100 Mounting Kit Free Standing.
b.	4102, 10 feet, 12, 1 5/8 inch, 1 1/16 inch, 4100 Mounting Kit, Free Standing.
c.	4100, Anchor set, Galvanized.
4.	"J" Style Bike Rack Series 1:
a.	1052, 5 feet, 8, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
b.	1052C, 5 feet, 8, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
c.	1082, 8 feet, 14, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
d.	1082C, 8 feet, 14, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
e.	1102, 10 feet, 18, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
f.	1102C, 10 feet, 18, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
g.	1162, 16 feet, 28, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
h.	1162C, 16 feet, 28, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
i.	1202, 20 feet, 36, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
j.	1202C, 20 feet, 36, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
5.	"H" Style Bike Rack Series 2:
a.	2052, 5 feet, 8, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
b.	2052C, 5 feet, 8, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
c.	2082, 8 feet, 14, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
d.	2082C, 8 feet, 14, 1 5/8 inch, 1 inch, Standing 1100 Anchor Kit.
e.	2102, 10 feet, 18, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
f.	2102C, 10 feet, 18, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
g.	2162, 16 feet, 28, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
h.	2162C, 16 feet, 28, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
i.	2202, 20 feet, 36, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
j.	2202C, 20 feet, 36, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
k.	1100, Anchor set.
6.	"A" Style Bike Rack Series 5:
a.	5052, 5 feet, 8 Spaces, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
b.	5052C, 5 feet, 8, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
c.	5082, 8 feet, 14, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
d.	5082C, 8 feet, 14, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
e.	5102, 10 feet, 18, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
f.	5102C, 10 feet, 18, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
g.	5162, 16 feet, 28, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
h.	5162C, 16 feet, 28, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
i.	5202, 20 feet, 36, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
j.	5202C, 20 feet, 36, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
k.	1100, Anchor set.
7.	"W" Style Bike Rack Series:
a.	7052, 5 feet, 8, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
b.	7052C, 5 feet, 8, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
c.	7082, 8 feet, 14, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
d.	7082C, 8 feet, 14, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
e.	7102, 10 feet, 18, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
f.	7102C, 10 feet, 18, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
g.	7162, 16 feet, 28, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
h.	7162C, 16 feet, 28, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
i.	7202, 20 feet, 36, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
j.	7202C, 20 feet, 36, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit
8.	"S" Style Bike Rack Series 8:
a.	8052, 5 feet, 8, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
b.	8052C, 5 feet, 8, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
c.	8082, 8 feet, 14, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
d.	8082C, 8 feet, 14, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
e.	8102, 10 feet, 18, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
f.	8102C, 10 feet, 18, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
g.	8162, 16 feet, 28, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
h.	8162C, 16 feet, 28, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
i.	8202, 20 feet, 36, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
j.	8202C, 20 feet, 36, 1 5/8 inch, 1 inch, Free Standing 1100 Anchor Kit.
k.	1100, Anchor set.
9.	Skateboard Racks:
a.	MSR4G, Single Sided Galvanized Skateboard Rack, Surface Mount, 30 inch, 12 inch, 10 inch.
b.	MSR4C, Single Sided Powder Coated Skateboard Rack, Surface Mount, 30 inch, 12 inch, 10 inch.
c.	MSR8G, Double Sided Galvanized Skateboard Rack, Surface Mount, 30 inch, 20 inch, 10 inch.
d.	MSR8C, Double Sided Powder Coated Skateboard Rack, Surface Mount, 30 inch, 20 inch.
10.	Bollard Style Bike Rack:
a.	CPBB2CSM, Surface Mount.
b.	CPBB2CIG, Inground.
11.	Horseshoe Style Bike Rack:
a.	MHS2GSM, Hot Dip Galvanized.
b.	MHS2CSM, Powder Coated.
12.	Triangle Style Bike Rack:
a.	TRBR7C, 50 inch L, 7 Spaces.
13.	Heritage Steel Bike Rack:
a.	SSABR6, 72 inch L, 10 Spaces.
L.	Windsor Series Site Furnishings:
1.	Windsor Tables:
a.	WS6JCRP, Windsor 6 feet Picnic Tables, 6 feet, 1 5/8 inch, Free Standing.
b.	WS4JCRP, Windsor 4 feet Square Tables, 4 feet, 1 5/8 inch, Free Standing.
c.	WS6SPTCRP-SM, Windsor Single Post Table, 6 feet, 3 1/2 inch, Surface Mount.
d.	WS6SPTCRP-IG, Windsor Single Post Table, 6 feet, 3 1/2 inch, Inground Mount.
2.	Windsor Select Benches:
a.	WS6LCBRP, Windsor Select Bench with Back, 6 feet, Recycled Plastic.
b.	WS6FCBRP, Windsor Select Bench Backless, 6 feet, Recycled Plastic.
3.	Windsor Series Litter Receptacles:
a.	WS3032LRRP, Windsor Series Litter Receptacle.
b.	3032LRIG, In-Ground Post for Windsor Series Receptacle.
c.	PCVL, Convex Plastic Lid 12 inch Opening.
d.	PCCL, Concave Plastic Lid, 8 inch Opening.
e.	CP32, 32 Gal. Plastic Can.
4.	DLTH32, Plastic Top Hat Lid. Windsor Select Planters:
a.	WSRP2630RP, Recycled Plastic, Round.
b.	WSRP2624RP, Recycled Plastic, Round.
c.	WSRP2618RP, Recycled Plastic, Round.
d.	WSSP2630RP, Recycled Plastic, Square.
e.	WSSP2624RP, Recycled Plastic, Square.
f.	WSSP2618RP, Recycled Plastic, Square.
M.	Planters:
1.	Strap Steel Planters:
a.	SSAP3624, 36 inch sq. x 24 inch H Planter with Liner and Drain Holes.
2.	Concrete Planters:
a.	CPR2417, Ever Popular Round Planters, 24 inch, 17 inch.
b.	CPR2424, Ever Popular Round Planters, 24 inch, 24 inch.
c.	CPR2433, Ever Popular Round Planters, 24 inch, 33 inch.
d.	CPR3017, Ever Popular Round Planters, 30 inch, 17 inch.
e.	CPR3030, Ever Popular Round Planters, 30 inch, 30 inch.
f.	CPR3624, Ever Popular Round Planters, 36 inch, 24 inch.
g.	CPR3630, Ever Popular Round Planters, 36 inch, 30 inch.
h.	CPR4817, Ever Popular Round Planters, 48 inch, 17 inch.
i.	CPR4824, Ever Popular Round Planters, 48 inch, 24 inch.
j.	CPR6036, Ever Popular Round Planters, 60 inch.
k.	CPAR3622, Aspen Round Planters, 36 inch, 22 inch.
l.	CPAR4836, Aspen Round Planters, 48 inch, 36 inch. Aspen Round Planters, 60 inch, 36 inch.
m.	CPAR3630, Aspen Round Planters, 36 inch, 30 inch.
n.	CTCA-30AP, Aspen Trash Receptacle, 31 inch, 38 inch.
o.	CSA-2319, Aspen Ash Urn- Snuffer, 19 inch, 23 inch.
p.	CPRR2424, Brighton Planters- 24 inch Dia., 24 inch, 24 inch.
q.	CPRR4224, Brighton Planters- 42 inch - 24 inch Dia., 42 inch, 24 inch.
r.	CPS1818, Rectangular and Square Planters, .18 inch.
s.	CPS2428, Rectangular and Square Planters, 28 inch.
t.	CPS3630, Rectangular and Square Planters, 30 inch.
u.	CPS4230, Rectangular and Square Planters, 30 inch.
v.	CP183320, Rectangular and Square Planters, 20 inch.
w.	CP184820, Rectangular and Square Planters, 20 inch.
x.	CP186020, Rectangular and Square Planters, 20 inch.
y.	CP187220, Rectangular and Square Planters, 20 inch.
z.	CP244830, Rectangular and Square Planters, 30 inch.
aa.	CPAS2418, Square and Rectangular Aspen Planters, 18 inch.
ab.	CPAS2436, Square and Rectangular Aspen Planters, 18 inch.
ac.	CPAS2448, Square and Rectangular Aspen Planters, 30 inch.
ad.	CPAS3648, Square and Rectangular Aspen Planters, 36 inch.
ae.	CPAS4848, Square and Rectangular Aspen Planters, 36 inch.
af.	CPAS3660, Square and Rectangular Aspen Planters, 36 inch.
ag.	CPAS3672, Square and Rectangular Aspen Planters, 36 inch.
ah.	CPAS1660, Square and Rectangular Aspen Planters,18 inch.
ai.	CPAS2472, Square and Rectangular Aspen Planters, 18 inch.
aj.	CPSW2424, Southwest Look Dish style Planters, 24 inch, 24 inch.
ak.	CPSW3017, Southwest Look Dish style Planters, 30 inch, 17 inch.
al.	CPSW4817, Southwest Look Dish style Planters, 48 inch, 17 inch.
am.	CTCRS30A, Matching Trash Receptacle, 24 inch
3.	Windsor Select Planters:
a.	WSRP2630RP, Recycled Plastic, Round.
b.	WSRP2624RP, Recycled Plastic, Round.
c.	WSRP2618RP, Recycled Plastic, Round.
d.	WSSP2630RP, Recycled Plastic, Square.
e.	WSP2624RP, Recycled Plastic, Square.
f.	WSSP2618RP, Recycled Plastic, Square.
N.	Snuffers:
1.	Plastisol Snuffer:
a.	SVP1224, Plastisol Litter Receptacle, 3/4 inch No. 9 expanded metal with heavy PVC coating, UV and mildew resistant.
2.	Snuffer and Trash Units:
a.	STTW314, Smoker's Tidy Wall Tube, Wall Model.
b.	STTF436, Smoker's Tidy Floor Tube, Floor Model.
c.	SOCS, Wall Mount "Smoke Out".
d.	ASU, "Aladdin" Smoker's Unit.
e.	BCCR, "Butt Can".
f.	SSCR, "Safe Smoker".
g.	SBCR, Smoker's Butler.
h.	DSSCR, Safe Smoker.
3.	Concrete Snuffers:
a.	CSR-1130, High Round Snuffer- 11 inch Dia x 30 inch, 11 inch, 30 inch.
b.	CSK-1524, High Round Snuffer- 15 inch Dia x 24 inch, 15 inch, 24 inch.
c.	CSR-1324, High Round Snuffer- 13 inch Dia x 24 inch, 13 inch, 24 inch.
d.	CSR-1224, High Round Snuffer- 12 inch Dia x 24 inch, 12 inch, 24 inch.
e.	CSR-1124, High Round Snuffer- 11 inch Dia x 24 inch, 11 inch, 24 inch.
f.	CSR-1117, High Round Snuffer- 11 inch Dia x 17 inch, 11 inch, 17 inch.
g.	CSA-2319, High Round Snuffer- 19 inch Dia x 23 inch, 19 inch, 23 inch.
h.	CSS-1632, High Square Snuffer- 16 inch Dia x 32 inch, 16 inch, 32 inch.
i.	CSS-1424, High Square Snuffer- 14 inch Dia x 24 inch, 14 inch, 24 inch.
j.	CSS-1230, High Square Snuffer- 12 inch Dia x 30 inch, 12 inch, 30 inch.
k.	CSS-1521, High Square Snuffer- 15 inch Dia x 21 inch, 15 inch, 21 inch.
l.	CSV-1524, High Square Snuffer- 15 inch Dia x 24 inch, 15 inch, 24 inch.
m.	CSS-1824, High Square Snuffer- 18 inch Dia x 24 inch, 18 inch, 24 inch.
n.	CSS-1224, High Square Snuffer- 12 inch Dia x 24 inch, 12 inch, 24 inch.
o.	CSTD-1440, Snuffer/Trash Combination Unit- 14 x 21 x 22 inch, 14 inch, 40 inch.
p.	CSTR-1230, Snuffer/Trash Combination Unit- 12 inch Dia x 30 inch, 12 inch, 30 inch.
q.	CSTR-1332, Snuffer/Trash Combination Unit- 13 inch Dia x 32 inch, 13 inch, 32 inch.
r.	CSOSK, Stainless Steel Skimmer, 5 inch.
O.	Crowd Barriers:
1.	Crowd Barriers:
a.	WALL4296, Crowd Barrier.
b.	WALLGATE, Barricade Gate.
c.	SF142120, 42 inch x 120 inch Sport Barricade.
P.	Shade Solutions:
1.	Dugout Shades:
a.	DS1012G, 10 inch, 12 inch, 8 inch.
b.	DS1016G, 10 inch, 16 inch, 8 inch.
c.	DS1018G, 10 inch, 18 inch, 8 inch.
d.	DS1020G, 10 inch, 20 inch, 8 inch.
2.	Table/Bench Shades:
a.	WT1422SS, 168 inch, 264 inch, 138 inch.
b.	WT918RTSS, 108 inch, 216 inch, 138 inch.
3.	Millennium Canopy:
a.	WT1010MC, Millennium Canopy, 10 x 10 feet.
b.	WT1515MC, Millennium Canopy, 15 x 15 feet.
c.	WT2020MC, Millennium Canopy, 20 x 20 feet.
4.	Party Canopy:
a.	WT2020PC, Party Canopy, 20 x 20 feet.
b.	WT2030PC, Party Canopy, 20 x 30 feet.
c.	WT2040PC, Party Canopy, 20 x 40 feet.
5.	Perma-Brella:
a.	WT12PB, Perma-Brella, 12 feet.
b.	WT14PB, Perma-Brella, 14 feet.
c.	WT20PB, Perma-Brella, 20 feet.
6.	Festive Quick-Loc Canopy:
a.	WT1414FC, Festive Quick-Loc Canopy, 14 x 14 feet.
b.	WT2020FC, Festive Quick-Loc Canopy, 20 x 20 feet.
c.	WT2030FC, Festive Quick-Loc Canopy, 20 x 30 feet.
d.	WT2040FC, Festive Quick-Loc Canopy, 20 x 40 feet.
7.	Bleacher Sunshades:
a.	BS1810, Covers a 3 Row 15 feet Bleacher, 18 feet, 10 feet, 8 feet.
b.	Surface Mount.
c.	BS2410, Covers a 3 Row 21 feet Bleacher, 24 feet, 10 feet, 8 feet.
d.	BS3010, Covers a 3 Row 27 feet Bleacher, 30 feet, 10 feet, 8 feet.
e.	BS1812, Covers a 5 Row 15 feet Bleacher, 18 feet, 12 feet, 9 feet.
f.	BS2412, Covers a 5 Row 21 feet Bleacher, 24 feet, 12 feet, 9 feet.
g.	BS3012, Covers a 5 Row 27 feet Bleacher, 30 feet, 12 feet, 9 feet.
h.	BS2218, Covers a 10 Row 15 feet Bleacher, 18 feet, 22 feet, 12 feet.
i.	BS2422, Covers a 10 Row 21 feet Bleacher, 24 feet, 22 feet, 12 feet.
j.	BS3022, Covers a 10 Row 27 feet Bleacher, 30 feet, 22 feet, 12 feet.
Q.	Umbrellas:
1.	Vinyl Umbrellas:
a.	UV, 3-ply vinyl with nylon scrim reinforcing between layers. 7 1/2 feet diameter. Available in several colors.
2.	Fiberglass Umbrellas:
a.	UF, tough and weather resistant, 7 1/2 feet diameter.
3.	Wind-Resistant Umbrellas:
a.	UVFL7-TC, Garden Valance, 7 1/2 feet.
b.	UHM7OC, 6 Rib Hexagon Patio, 7 1/2 feet.
c.	UHM9OC, 8 Rib Octagon Patio, 9 feet.
d.	UOM7MC, 8 Rib Octagon Market - Crank, 7 1/2 feet.
e.	UOM7MU, 8 Rib Octagon Market - Push Up, 7 1/2 feet.
f.	UOM9MC, 8 Rib Octagon Market - Crank, 9 feet.
g.	UOM9MP, 8 Rib Octagon Market - Pulley & Pin, 9 feet.
h.	UOM11MP, 8 Rib Octagon Market - Pulley & Pin, 11 feet.
i.	ULP7MU, 8 Rib Ultra Heavy Duty, 7 1/2 feet.
j.	ULP9MU, 8 Rib Ultra Heavy Duty, 9 feet.
k.	ULP11MP, 8 Rib Ultra Heavy Duty, 11 feet.
4.	Umbrella Bases:
a.	UBCW, Concrete Umbrella Base, 19 inch dia x 14 inch high.
b.	UBCC, Concrete Umbrella Base, 19 inch dia x 14 inch high.
c.	UBCB, Concrete Umbrella Base, 19 inch dia x 14 inch high.
d.	UBSL, Steel Umbrella Base, 24 inch sq x 12 1/2 inch high.
e.	UBSLW, Steel Umbrella Base with Wheels, 24 inch sq x 12 1/2 inch high.
5.	Ubrace:
a.	Ubrace, Umbrella Anchor, stainless steel.
R.	Outdoor Sports Equipment:
1.	Basketball Goal Systems:
a.	WTBS, Concrete Basketball Goal System.
b.	AC44G, 4 1/2 inch OD Post Basketball Goal System.
c.	AC66GF, 6 5/8 inch OD Post Basketball Goal System w/Fan Backboard.
d.	AC66GR, 6 5/8 inch OD Post Basketball Goal System w/Rectangle Backboard.
2.	Sport Fence:
a.	SF142120, 42 inch x 120 inch Sport Barricade.
S.	Pet Waste Stations:
1.	"Dogipot" Brand:
a.	KDP1005, Dog Valet, Green.
b.	KDP1006, Dog Valet, Sand.
c.	KDP1002, Aluminum, Bag Dispenser Only.
d.	KDP1003, Pet Station, Complete.
e.	KDP1010, Poly Pet Station complete.
f.	KDP1007, Poly, Bag Dispenser Only.
g.	KDP140210, Case of 10, 200 count Rolls, 2000 total Litter Bags.
h.	KDP140220, Case of 20, 200 count Rolls, 4000 total Litter Bags.
i.	KDP140230, Case of 30, 200 count Rolls, 6000 total Litter Bags.
j.	KDP1404, 50 Heavy-Duty Oxo-Biodegradable Trash Liner Bags.
2.	"Mutt Mitt" Brand:
a.	MMKITG, Mutt Mitt Kit - Green (Receptacle not Included).
b.	MMKITY, Mutt Mitt Kit - Yellow (Receptacle not Included).
c.	MMKITW, Mutt Mitt Kit - White (Receptacle not Included).
d.	MM22GALG, 22 Gallon Green Receptacle w/o Lid.
e.	MM22GALK, 22 Gallon Black Receptacle w/o Lid.
f.	MM10GALG, 10 Gallon Green Receptacle w/o Lid.
g.	MM10GALK, 10 Gallon Black Receptacle w/o Lid.
h.	MMDISPG, Dispenser Only - Green.
i.	MMDISPW, Dispenser Only - White.
j.	MMDISPY, Dispenser Only - Yellow.
k.	MMREFILLS, 2 Ply 1.0 mill 800 ct. Bag Refill.
l.	MMSINGLES, 1 Ply .75 mill 2000 ct. Bag Refill.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	INSTALLATION
A.	Install site furnishings in accordance with manufacturer's installation instructions and in proper relationship with adjacent construction. Adjust until satisfactory results are achieved.
B.	Install site furnishings level, plumb, square, accurately aligned, correctly located per drawings, and without warp. Use hardware and fasteners acceptable to manufacturer.
3.3	CLEANING AND PROTECTION
A.	Clean in accordance with manufacturer's recommendations.
B.	Protect installed products until completion of project.
C.	Touch-up, repair or replace damaged products and finishes in accordance with manufacturer's instructions before Substantial Completion.

END OF SECTION