SECTION 06 05 23

WOOD, PLASTIC, COMPOSITE, AND STEEL CONSTRUCTION FASTENERS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2023 -  2023 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Fasteners: Self tappers.
B.	Fasteners: Self drillers.
1.2	RELATED SECTIONS
A.	Section 06 05 00 - Common Work Results for Wood, Plastics, and Composites.
B.	Section 06 05 05 - Selective Demolition for Wood, Plastics, and Composites.
C.	Section 06 08 00 - Commissioning of Wood, Plastics, and Composites.
D.	Section 06 10 00 - Rough Carpentry.
E.	Section 06 15 00 - Wood Decking.
F.	Section 06 60 00 - Plastic Fabrications.
G.	Section 06 80 00 - Composite Fabrications.
H.	Section 07 72 50 - Roofing Fasteners.
1.3	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Verification Samples: Two representative units of each type, size, pattern, and color.
D.	Shop Drawings: Include details of materials, construction, and finish. Include relationship with adjacent construction.
1.4	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
D.	Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
1.	Intent of mock-up is to demonstrate quality of workmanship and visual appearance.
2.	If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
3.	Retain mock-up during construction as a standard for comparison with completed work. 
4.	Do not alter or remove mock-up until work is completed or removal is authorized.
1.5	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.6	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.7	WARRANTY
A.	Manufacturer's standard limited warranty unless indicated otherwise.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Lakeside Construction Fasteners, which is located at:<BR />6476 Hwy. 135 N.<BR />Paragould, AR 72450<BR />Toll Free Tel: 800-537-4160<BR />Tel: 870-586-0703<BR />Fax: 870-586-0643<BR />Email: request info (sales@lakeside-fasteners.com);Web: https://lakeside-fasteners.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	FASTENERS: SELF TAPPERS
A.	Fastener T17 Fastlok: A deep major thread design helps bond metal panels together to resist panel separation when utilizing it as a stitch fastener.
1.	T17 cut point for quick panel penetration.
2.	Fastener Dia.: No. 12.
3.	Head Size: 1/4 inch (6 mm).
4.	Head Size: 5/16 inch (8 mm).
5.	Threads: 14 per inch (14 per 25 mm). Engineered thread design to lock panels in-place.
6.	Material: C1022.
7.	Washer, Positive Seal: EPDM.
8.	Finish: Coating System. L3 Dura Protec.
9.	Finish: Painted. Color: ________.
10.	Finish: Powder Coated. Color: ________.
11.	Length: 3/4 inch (19 mm).
12.	Length: 1 inch (25 mm).
13.	Length: 1/2 inch (13 mm).
14.	Pullout Test Values:
a.	Plywood 1/2 inch (13 mm). 400 lbs (181.44 kg).
b.	Plywood 5/8 inch (16 mm). 600 lbs (272.16 kg).
c.	Plywood 3/4 inch (19 mm). 700 lbs (317 51 kg).
d.	OSB: 7/16 inch (11 mm). 315 lbs (142.88 kg).
e.	Southern Pine: 1 inch (25 mm). 1060 lbs (480.81 kg).
f.	Southern Pine: 1-1/2 inch (38 mm). 1500 lbs (680.39 kg).
B.	Fastener T17 WOOD-X System: Wood fasteners for post frame and residential applications. For all types of decking substrate materials including hard woods. High-low threads along with the sharp cut point allows the fastener to quickly penetrate the metal panel for easier fastener installation.
1.	Miami Dade County Approved.
2.	H-LOW threads for Speed of Installation.
3.	T17 point for High Performance.
4.	Engineered head flute resists High Torque Environments.
5.	Innovative L3 Dura Protec coating to prevent Red Rust.
6.	EPDM washer for a Positive Seal.
7.	Fastener Dia.: No. 10.
8.	Head Size: 1/4 inch (6 mm).
9.	Threads: 14. Reinforced Flute under fastener head H-Low Threads
a.	Reinforced Flute: Located under the head of the fastener.
1)	Engineered and reinforced for high torque environments.
2)	Can be used with battery operated screw guns and Impact Screw Guns.
10.	Material: C1022.
11.	Washer, Positive Seal: EPDM.
12.	Finish: Coating System. L3 Dura Protec.
13.	Finish: Painted. Color: ________.
14.	Finish: Powder Coated. Color: ________.
15.	Length: 1-1/2 inch (38 mm).
16.	Length: 2 inch (51 mm).
17.	Length: 2-1/2 inch (64 mm).
18.	Length: 3 inch (76 mm) (76 mm).
19.	Length: 4 inch (102 mm).
20.	Pullout Test Values:
a.	Plywood 1/2 inch (13 mm). 425 lbs (192.78 kg).
b.	Plywood 5/8 inch (16 mm). 600 lbs (272.16 kg).
c.	Plywood 3/4 inch (19 mm). 725 lbs (328.85 kg).
d.	OSB: 7/16 inch (11 mm). 325 lbs (147.42 kg).
e.	Southern Pine: 1 inch (25 mm). 735 lbs (333.39 kg).
f.	Southern Pine: 1-1/2 inch (38 mm). 1205 lbs (546.58 kg).
C.	Fastener 304 Wood-X Stainless with Washer.
D.	Fastener 410 Wood-X Stainless with Washer.
1.	Miami Dade County Listed.
2.	Fastener Dia.: No. 10.
3.	Head Size: 1/4 inch (6 mm).
4.	Length: 2 inches (51 mm mm).
5.	Length: 2-1/2 inches (64 mm).
E.	Fastener 410 Wood-X Stainless without Washer.
1.	Miami Dade County Listed.
2.	Fastener Dia.: No. 10.
3.	Head Size: 1/4 inch (6 mm).
4.	Length: 2 inches (51 mm mm).
5.	Length: 2-1/2 inches (64 mm).
F.	Fastener COR10 Wood-X: No. 10 x 1 to 3 inches (25 to 76 mm) long, Engineered to secure corten metal panels into hardwood decking substrates. Offers a sealed protective barrier, and pre-weathered for exact corten metal panel color match.
1.	H-LOW threads for Speed of Installation.
2.	T17 Cut point for High Performance.
3.	Engineered head flute resists High Torque Environments.
4.	EPDM positive seal washer.
5.	Finish: Pre-weathered for exact corten metal panel color match.
6.	Finish: Painted. Color: ________.
G.	Fastener T17 MasterGrip: For high wind environments. A deep major thread design allows the fastener to be embedded in all wood substrates for maximum pull-out. Will secure the metal panel to the wood structure to help prevent panel pullover and shear in the most extreme high wind conditions.
1.	T17 cut point for quick Panel Penetration.
2.	Engineered head design for High Shear Environments.
3.	Innovative L3 Dura Protec coating to Prevent Red Rust.
4.	Fastener Dia.: No. 14.
5.	Head Size: 5/16 inch (8 mm).
6.	Threads: 10. Special major thread design for High Pull-out.
7.	Material: C1022.
8.	Washer, Positive Seal: EPDM.
9.	Finish: Coating System. L3 Dura Protec.
10.	Finish: Painted. Color: ________.
11.	Finish: Powder Coated. Color: ________.
12.	Length: 1 inch (25 mm).
13.	Length: 1-1/2 inch (38 mm).
14.	Length: 2 inch (51 mm).
15.	Length: 2-1/2 inch (64 mm).
16.	Length: 3 inch (76 mm).
17.	Length: 4 inch (102 mm).
18.	Pullout Test Values:
a.	Plywood 1/2 inch (13 mm). 425 lbs (192.78 kg).
b.	Plywood 5/8 inch (16 mm). 700 lbs (317 51 kg).
c.	Plywood 3/4 inch (19 mm). 900 lbs (408.23 kg).
d.	OSB: 7/16 inch (11 mm). 350 lbs (138 kg).
e.	Southern Pine: 1 inch (25 mm). 825 lbs (374.2 kg).
f.	Southern Pine: 1-1/2 inch (38 mm). 1200 lbs (544.31 kg).
H.	Fastener T17 MasterGrip XL.
1.	Dia.: No. 14 or No. 1/4 inch (6 mm).
2.	Head Size: 3/8 inch (10 mm).
3.	Length: 2 inch (51 mm).
4.	Length: 2-1/2 inch (64 mm).
5.	Length: 3 inch (76 mm).
6.	Length: 4 inch (102 mm).
7.	Washer: 3/4 inches (19 mm) Flat Bond.
8.	Washer: 1 inch (25 mm) Flat Bond.
9.	Washer: 1 inch (25 mm) Multi-Seal.
I.	Fastener 410 MasterGrip Stainless.
J.	Fastener SC Steel Guard: Concealed weather-tite EPDM washer. Engineered and designed for high torque applications.
1.	Fastener Dia.: No. 10.
2.	Head Size: 1/4 inch (6 mm). Fastener Head will not Red Rust.
3.	Threads: 14 per inch. H-Low Threads.
4.	Material: C1022.
5.	Washer, Positive Seal: Tubular EPDM.
6.	Finish: Coating System. L3 Dura Protec.
7.	Finish: Painted. Color: ________.
8.	Finish: Powder Coated. Color: ________.
9.	Length: 1-1/2 inch (38 mm).
10.	Length: 2 inch (51 mm).
11.	Length: 2-1/2 inch (64 mm).
12.	Length: 3 inch (76 mm).
13.	Length: 4 inch (102 mm).
14.	Pullout Test Values:
a.	Plywood 1/2 inch (13 mm). 450 lbs (204.12 kg).
b.	Plywood 5/8 inch (16 mm). 600 lbs (272.16 kg).
c.	Plywood 3/4 inch (19 mm). 750 lbs (340.19 kg).
d.	OSB: 7/16 inch (11 mm). 350 lbs (138 kg).
e.	Southern Pine: 1 inch (25 mm). 805 lbs (365.14 kg).
f.	Southern Pine: 1-1/2 inch (38 mm). 1250 lbs (567 kg).
K.	Fastener Pro Cliplok XL.
L.	Fastener Pro Cliplok: 
1.	Head Type: Pancake Wood Screws.
a.	Threads: 12 per inch.
b.	Threads Self Drilling: 16 per inch.
c.	Reinforced Flute Cut Point: Type-17, Self-Driller No. 3.
d.	Length: 1 inch (25 mm).
e.	Length: 1-1/2 inch (38 mm).
f.	Length: 2 inch (51 mm).
g.	Material C1022.
h.	Material: Stainless steel.
i.	Drive: No. 2 Phillip Combo Drive.
j.	Drive: No. 2 Square Drive,
2.	Head Type: Wafers/X-treme Lo Wood Screws:
a.	Threads: 12 per inch.
b.	Threads Self Drilling: 16 per in.
c.	Pierce Point, Self-Driller No. 3.
d.	Length: 1 inch (25 mm).
e.	Length: 1-1/2 inch (38 mm).
f.	Length: 2 inch (51 mm).
g.	Material C1022.
h.	Material: Stainless steel.
i.	Drive: No. 2 Phillip Combo Drive.
j.	Drive: No. 2 Square Drive,
3.	Head Type: Button Truss/Lath:
a.	Threads: 14 threads per inch. 
b.	H-Low Threads 
c.	Cut Point: Type-17
d.	Length: 1 inch (25 mm).
e.	Length: 1-1/2 inch (38 mm).
f.	Length: 2 inch (51 mm).
g.	Material C1022.
h.	Material: Stainless steel.
i.	Drive: No. 2 Phillip Combo Drive.
4.	Pullout Test Values: Self Tapping:
a.	Plywood 1/2 inch (13 mm). 425 lbs (192.78 kg).
b.	Plywood 5/8 inch (16 mm). 600 lbs (272.16 kg).
c.	Plywood 3/4 inch (19 mm). 725 lbs (328.85 kg).
d.	OSB: 7/16 inch (11 mm). 325 lbs (147.42 kg).
e.	Southern Pine: 1 inch (25 mm). 735 lbs (333.39 kg).
f.	Southern Pine: 1-1/2 inch (38 mm). 1205 lbs (546.58 kg).
5.	Pullout Test Values: Self Drilling:
a.	12 ga: 1679 lbs (761.58 kg).
b.	14 ga: 1107 lbs (502.13 kg).
c.	16 ga: 932 lbs (422.75 kg).
6.	Finish: Painted. Color: ________.
7.	Finish: Powder Coated. Color: ________.
M.	Fastener 8Z-Stitch: A full line of wood fasteners for post frame, gutter, HVAC, and residential applications. Designed for all types of stitching applications from metal panels to gutter strapping. Coarse threads with the sharp cut point allows the fasteners to quickly penetrate metal for easier fastener installation.
1.	True 1/4 HWH for Positive Drive Engagement.
2.	Thread under head of fastener for Maximum Stitching Power.
3.	Fastener Dia.: No. 8.
4.	Head Size: 1/4 inch (6 mm).
5.	Threads: 10 per inch. Stitch thread.
6.	Innovation: Engineered True 1/4 HWH.
7.	Cut Point: Type-17.
8.	Material: C1022.
9.	Length: 1/2 inch (13 mm).
a.	Finish: Coating System. L3 Dura Protec.
b.	Finish: Painted. Color: ________.
10.	Length: 3/4 inch (19 mm).
a.	Finish: Coating System. L3 Dura Protec.
b.	Finish: Painted. Color: ________.
11.	Pullout Test Values:
a.	Plywood 1/4 inch (6 mm). 200 lbs (90.72 kg).
b.	Plywood 1/2 inch (13 mm). 250 lbs (113.40 kg).
c.	Plywood 3/4 inch (19 mm). 350 lbs (138 kg).
d.	OSB: 1/4 inch (6 mm). 300 lbs (136.08 kg).
e.	Steel Plate: 14 ga. 500 lbs (26.80 kg).
f.	Steel Plate: 20 ga. 450 lbs (204.12 kg).
N.	Fastener Zmax: Alloy head fasteners are engineered and developed for high corrosion applications. A larger outer head diameter to prevent wind uplift and suitable in high snow load regions. Ideal for coastal environments, preventing Red Rust on fastener heads once installed into metal building systems. 
1.	T17 cut point for quick Panel Penetration.
2.	Fastener Dia.: No. 10.
3.	Head Size: 5/16 inch (8 mm). Will not red rust.
4.	Threads: 14 per inch. Special major thread design for High Pull-out.
5.	HWH: ZAMAK forged alloy head.
6.	Material: C1022.
7.	Washer, Positive Seal: Tubular EPDM.
8.	Finish: Coating System. L3 Dura Protec.
9.	Finish: Painted. Color: ________.
10.	Finish: Powder Coated. Color: ________.
11.	Length: 1 inch (25 mm).
12.	Length: 1-1/2 inch (38 mm).
13.	Length: 2 inch (51 mm).
14.	Length: 2-1/2 inch (64 mm).
15.	Length: 3 inch (76 mm).
16.	Pullout Test Values:
a.	Plywood 1/2 inch (13 mm). 450 lbs (204.12 kg).
b.	Plywood 5/8 inch (16 mm). 600 lbs (272.16 kg).
c.	Plywood 3/4 inch (19 mm). 750 lbs (340.19 kg).
d.	OSB: 7/16 inch (11 mm). 350 lbs (138 kg).
e.	Southern Pine: 1 inch (25 mm). 805 lbs (365.14 kg).
f.	Southern Pine: 1-1/2 inch (38 mm). 1250 lbs (567 kg).
2.3	FASTENERS: SELF DRILLERS
A.	Fastener SD Pro-Tek Self-Drilling. For metal-to-metal building applications. A larger head diameter limits wind uplift, and the concealed EPDM tubular washer system allows for a weather-tite seal. The engineered flat surface area on the fastener provides positive nutsetter engagement, preventing wobble during fastener install. Deep root cut threads give maximum holding power when installed into metal building panels.
1.	Fastener Dia: No. 12.
2.	Head Size: 5/16 inch (8 mm).
3.	Threads: 14 per inch.
4.	Innovation: Self Driller Point and Cut Threads.
5.	SD Point: SD1 and SD3.
6.	HWH: Low Profile Head.
7.	Material: C1022.
8.	Washer: EPDM Tubular. Available without washer upon request.
9.	Coating System: L3 Dura Protec.
10.	Length: 3/4 inch (19 mm). Stitch.
11.	Length: 7/8 inch (22 mm). Lap.
12.	Length: 1 inch (25 mm). Stitch.
13.	Length: 1-1/4 inch (32 mm). Lap.
14.	Length: 1-1/2 inch (38 mm). Stitch.
15.	Length: 2 inch (51 mm). Lap.
16.	Finish: Wet paint.
17.	Finish: Powder coat.
18.	Fastener: Pro-Tek 12-14:
a.	Pull-Out Test Values: 
1)	12 ga: 1679 lbs (761.58 kg).
2)	14 ga: 1107 lbs (502.13 kg).
3)	16 ga: 932 lbs (422.75 kg).
b.	Fastener System Values:
1)	Torsional: 115 inch lbs (13 Nm).
2)	Shear: 2235 lbs (103.78 kg).
3)	Tensile: 3300 lbs (1496.85 kg).
19.	Fastener: Pro-Tek 1/4-14:
a.	Pull-Out Test Values: 
1)	12 ga.: 1269 lbs (575.61 kg).
2)	14 ga.: 1050 lbs (476.27 kg).
3)	16 ga.: 683 lbs (309.80 kg).
b.	Fastener System Values:
1)	Torsional: 160 inch lbs (18.08 Nm).
2)	Shear: 2755 lbs (1249.65 kg).
3)	Tensile: 3915 lbs (1775.81 kg).
B.	Fastener SD3 Steel-X. A full line of innovative self-drilling fasteners for steel frame and industrial applications for all types of metal decking substrate material. A self-drill point allows fasteners to quickly penetrate metal panels for easier fastener installation and no metal curls.
1.	Penetrates 10 Ga., 12 Ga. and 14 Ga. Steel.
2.	Innovative L3 Dura Protec Coating prevents Red Rust.
3.	EPDM Flat Bonded Washer Promoting a Weather-Tite Seal.
4.	Hardened Tap Threads Reduces Torque.
5.	Innovative HEX Head Design prevents wobble with LCF Quick Drill Technologies. 
6.	Fastener Dia.: No. 12.
7.	Head Size: 5/16 inch (8 mm).
8.	Threads: 14 per inch.
9.	Innovation: Penetrates 10 Ga., 12 Ga. and 14 Ga. Steel.
10.	Cut Point: True Self Driller No. 3.
11.	Material: C1022.
12.	Washer: EPDM, Flat Bonded.
13.	Length: 3/4 inch (19 mm). Stitch.
14.	Length: 1 inch (25 mm). Stitch.
15.	Length: 1-1/4 inch (32 mm). Stitch.
16.	Length: 1-1/2 inch (38 mm). Stitch.
17.	Length: 2 inch (51 mm). Stitch.
18.	Length: 2-1/2 inch (64 mm). Stitch.
19.	Length: 3 inch (76 mm). Stitch.
20.	Finish: Coating System. L3 Dura Protec.
21.	Finish: Wet paint.
22.	Finish: Powder coat.
23.	Color: ________.
24.	Pull-Out Test Values:
a.	12 ga.: 2020 lbs (916.26 kg).
b.	14 ga.: 1300 lbs (589.67 kg).
c.	16 ga.: 1000 lbs (453.59 kg).
d.	20 ga,: 525 lbs (238.14 kg).
25.	Fastener System Values:
a.	Torsional: 152 inch lbs (17.17 Nm).
b.	Shear: 2150 lbs (975.22 kg).
c.	Tensile: 3105 lbs (1408.40 kg).
C.	Fastener 410 Steel-X Stainless Self Drillers.
1.	Length: 1 inch (25 mm). With Washer.
2.	Length: 1-1/2 inch (38 mm). With Washer.
D.	Fastener Pro Cliplok:
1.	Type: Self-Drilling Fasteners:
a.	Pull Out Values:
1)	12 ga: 1679 lbs (761.58 kg).
2)	14 ga: 1107 lbs (502.13 kg).
3)	16 ga: 932 lbs (422.75 kg).
4)	Torsional: 115 in lbs.
5)	Shear: 2235 lbs (103.78 kg).
6)	Tensile: 3300 lbs (1496.85 kg).
b.	Head Type: Pancake Self-Driller.
1)	Threads: 12 per inch.
2)	SD3: 16 per inch.
3)	Flute: Reinforced.
4)	Cut Point: Type-17 / Self-Driller No. 3.
5)	Drive: No. 2 Phillips Combo.
6)	Drive: No. 2 Square.
7)	Material: C1022.
8)	Material: Stainless steel.
9)	Length: 1 inch (25 mm).
10)	Length: 1-1/2 inch (38 mm).
11)	Length: 2 inch (51 mm).
c.	Head Type: Wafers/X-treme Lp Self-Driller.
1)	Threads: 12 per inch.
2)	SD3: 16 per inch.
3)	Flute: Reinforced.
4)	Cut Point: Pierce Point / Self-Driller No. 3.
5)	Drive: No. 2 Phillips Combo.
6)	Drive: No. 2 Square.
7)	Material: C1022.
8)	Material: Stainless steel.
9)	Length: 1 inch (25 mm).
10)	Length: 1-1/2 inch (38 mm).
11)	Length: 2 inch (51 mm).
2.	Type: Self-Tapping Fasteners.
a.	Pull Out Values:
1)	Plywood, 1/2 inch (13 mm): 425 lbs (192.78 kg).
2)	Plywood, 5/8 inch (16 mm): 600 lbs (272.16 kg).
3)	Plywood, 3/4 inch (19 mm): 725 lbs (328.85 kg).
4)	OSB, 7/16 inch (11 mm): 325 lbs (147.42 kg).
5)	Southern Pine, 1 inch (25 mm): 735 lbs (333.39 kg).
6)	Southern Pine, 1-1/2 inch (38 mm): 1205 lbs (546.58 kg).
7)	Torsional: 70 in lbs (7.91 Nm).
8)	Shear: 1900 lbs (408.23 kg) (861.82 kg).
9)	Tensile: 2300 lbs (1045.26 kg).
b.	Head Type: Pancake Self-Tappers.
1)	Threads: 12 per inch.
2)	SD3: 16 per inch.
3)	Flute: Reinforced.
4)	Cut Point: Type-17 / Self-Driller No. 3.
5)	Drive: No. 2 Phillips Combo.
6)	Drive: No. 2 Square.
7)	Material: C1022.
8)	Material: Stainless steel.
9)	Length: 1 inch (25 mm).
10)	Length: 1-1/2 inch (38 mm).
11)	Length: 2 inch (51 mm).
c.	Head Type: Wafers/X-treme LP Self-Tappers.
1)	Threads: 12 per inch.
2)	SD3: 16 per inch.
3)	Flute: Reinforced.
4)	Cut Point: Pierce Point / Self-Driller No. 3.
5)	Drive: No. 2 Phillips Combo.
6)	Drive: No. 2 Square.
7)	Material: C1022.
8)	Material: Stainless steel.
9)	Length: 1 inch (25 mm).
10)	Length: 1-1/2 inch (38 mm).
11)	Length: 2 inch (51 mm).
d.	Head Type: Button Truss/Lath
1)	Threads: 14 threads per inch.
2)	H-Low Threads.
3)	Cut Point: Type-17.
4)	Drive: No. 2 Phillips.
5)	Material: C1022.
6)	Material: Stainless steel.
7)	Length: 1 inch (25 mm).
8)	Length: 1-1/2 inch (38 mm).
9)	Length: 2 inch (51 mm).
E.	Hurricane Fastener Solutions: For High Wind Uplift Resistance. 3/4 and 1 inch (19 and 25 mm) Oversized Washers For WeatherTite Seal. Secure Tarps or Synthetic Overlays During Roof Repairs. ZMAX Long-Life Heads For Coastal Applications. Longer Length Fasteners Engineered For Retrofit Roofing Systems.
1.	Color: Caribbean Aqua - AQ76.
2.	Color: Caribbean Red - RD76.
3.	Color: Caribbean White - WH02.
4.	Color: Caribbean Green - GN76.
5.	Fastener ZMAX:
a.	Fastener Dia.: No. 10.
b.	Head Size: 5/16 inch (8 mm).
c.	Length: 1 inch (25 mm).
d.	Length: 1-1/2 inch (38 mm).
e.	Length: 2 inch (51 mm).
f.	Length: 2-1/2 inch (64 mm).
g.	Length: 3 inch (76 mm).
h.	Washer Dia.: 7/16 inches (11 mm).
6.	Fastener T17 MasterGrip:
a.	Fastener Dia.: No. 14.
b.	Head Size: 5/16 inch (8 mm).
c.	Length: 1 inch (25 mm).
d.	Length: 1-1/2 inch (38 mm).
e.	Length: 2 inch (51 mm).
f.	Length: 2-1/2 inch (64 mm).
g.	Length: 3 inch (76 mm).
h.	Length: 4 inch (102 mm).
i.	Washer Dia.: 5/8 inch (16 mm) Standard.
7.	Fastener T17 MasterGrip XL:
a.	Fastener Dia.: No. 14.
b.	Head Size: 3/8 inch (10 mm).
c.	Length: 1-1/2 inch (38 mm).
d.	Length: 2 inch (51 mm).
e.	Length: 2-1/2 inch (64 mm).
f.	Length: 3 inch (76 mm).
g.	Length: 4 inch (102 mm).
h.	Washer Dia.: 3/4 inch (19 mm).
i.	Washer Dia.: 1 inch (25 mm).
8.	Fastener Secure-Tek:
a.	Fastener Dia.: 1/4 inch (6 mm).
b.	Head Size: 3/8 inch (10 mm).
c.	Length: 7/8 inch (22 mm) LAP.
d.	Length: 1 inch (25 mm).
e.	Length: 1-1/4 inch (32 mm).
f.	Length: 1-1/2 inch (38 mm).
g.	Washer Dia.: 5/8 inch (16 mm Standard.
9.	Fastener Secure-Tek XL:
a.	Fastener Dia.: 1/4 inch (6 mm).
b.	Head Size: 3/8 inch (10 mm).
c.	Length: 7/8 inch (22 mm) LAP.
d.	Length: 2 inch (51 mm).
e.	Length: 2-1/2 inch (64 mm).
f.	Washer Dia.: 3/4 inch (19 mm) Standard.
g.	Washer Dia.: 1 inch (25 mm) Standard.
2.4	FASTENER PAINT COLOR SELECTION GUIDE
A.	Color Selections and RAL Numbers:
1.	Color: Arctic/Brilliant (AB01).
2.	Color: Ash Grey 25 (AG06).
3.	Color: Barn Red (RD03).
4.	Color: Black (BK02).
5.	Color: Bone White S03 (BW05).
6.	Color: Bright Red (BR02).
7.	Color: Bright White (BW02).
8.	Color: Brown 01 (BN01).
9.	Color: Brown 02 (BN02).
10.	Color: Burgundy 01 (BU01).
11.	Color: Burgundy 02 (BU02).
12.	Color: Burnished Slate 49 (BS06).
13.	Color: Charcoal 17 (CH06).
14.	Color: Charcoal S01 (CH05).
15.	Color: Colonial Red S10 (CR05).
16.	Color: Colony (CO01).
17.	Color: Copper Metallic (CM01).
18.	Color: Crimson (CS01).
19.	Color: Dark Bronze S04 (DZ05).
20.	Color: Emerald Green (EG02).
21.	Color: Fern (FR01).
22.	Color: Forest (FT01).
23.	Color: Gallery (GB01).
24.	Color: Gray (GR01).
25.	Color: Hawaiian Blue 70 (HB06).
26.	Color: Hunter (HG01).
27.	Color: Ivory (IW01).
28.	Color: Light Stone 01 (LS01).
29.	Color: Light Stone 03 (LS03).
30.	Color: Mocha Tan 22 (MT06).
31.	Color: Ocean (OC01).
32.	Color: Ocean Blue 35 (OB06).
33.	Color: Prairie Wheat (PW02).
34.	Color: Rustic (RU01).
35.	Color: Slate Gray S19 (SL05).
36.	Color: Surrey Beige S21 (BE05).
37.	Color: Tan (TN03).
38.	Color: Taupe (TP01).
39.	Color: White 39 (WH06).
40.	Color: White (WH02).
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
3.4	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.
B.	Manufacturer's Services: Coordinate manufacturer's services in accordance with appropriate sections in Division 01.
3.5	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturers recommendations. 
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION