SECTION 08 32 13

ALUMINUM FRAMED INTERIOR SLIDING DOOR SYSTEMS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2024 -  2024 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Aluminum framed interior sliding door systems. (Universal) (Magic 2) (120 Series) (130 Series)
1.2	RELATED SECTIONS
A.	Section 08 71 00 - Door Hardware.
B.	Section 10 22 00 - Demountable Partitions - Glazed and Solid.
1.3	SUBMITTALS
A.	Submit under provisions of Section 01 30 00.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Verification Samples: Two representative units of each type, size, pattern, and color.
D.	Shop Drawings: Include details of materials, construction, and finish. Include relationship with adjacent construction.
1.4	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum of five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
D.	Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
1.	The intent of mock-up is to demonstrate quality of workmanship and visual appearance.
2.	If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
3.	Retain mock-up during construction as a standard for comparison with completed work.
4.	Do not alter or remove mock-up until work is completed or removal is authorized.
1.5	PRE-INSTALLATION CONFERENCE
A.	Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.7	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.8	WARRANTY
A.	Manufacturer's standard limited warranty unless indicated otherwise.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Linear Interior Systems Inc., which is located at:<BR />1 Saramia Crescent<BR />Concord, ON, Canada  L4K 3S6<BR />Tel: 905-265-0055<BR />Fax: 905-265-0035<BR />Email: request info (info@linearinteriorsystems.com);Web: https://www.linearinteriorsystems.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with the provisions of Section. 01 60 00.
2.2	ALUMINUM FRAMED INTERIOR SLIDING DOOR SYSTEMS
A.	URL Link to Brochure: Universal Interior Sliding Door System : https://www.dropbox.com/scl/fo/7ve6yiqmmmo8zah6o8qy1/h?rlkey=74u4vfj0vap62m72xd87nclqy&dl=0
B.	Basis of Design: Universal Interior Sliding Door System as manufactured by Linear Interior Systems Inc. Non-load bearing. A Terno Scorrevoli frame, designed for doors in glass, timber, and aluminum. Clean lines, reduced encumbrances, high resistance.
1.	Operation: Manual.
2.	Configuration: Single track.
3.	Configuration: Double track.
4.	Rolling Style: Top rollers, bottom guide.
a.	Single Undermount: Model 0427.7.3.
1)	Track Width: 1-3/4 inches (45 mm).
2)	Track Height: 1-3/4 inches (44 mm).
3)	Vertical Door Adjustment: 0 to 1/4 inches (0 to 6 mm).
b.	Single Wall Mount: Model 0427.5.3.
1)	Track Width: 2-1/4 inches (57 mm).
2)	Track Height: 1-5/8 inches (42 mm).
3)	Vertical Door Adjustment: 0 to 1/4 inches (0 to 6 mm).
c.	Double Undermount: Model 0427.8.3.
1)	Track Width: 3-3/4 inches (95 mm).
2)	Track Height: 1-3/4 inches (44 mm).
3)	Vertical Door Adjustment: 0 to 1/4 inches (0 to 6 mm).
d.	Double Undermount Recessed: Model 0427.8.3.
1)	Track Width: 3-3/4 inches (95 mm).
2)	Track Height: 1-3/4 inches (44 mm).
3)	Vertical Door Adjustment: 0 to 1/4 inches (0 to 6 mm).
5.	Aluminum Track and Framing Material: 6061-T6 extruded profiles.
6.	Aluminum Track and Door Frame Finish: Anodized Silver.
7.	Aluminum Track and Door Frame Finish: Brushed Anodized Silver.
8.	Aluminum Track and Door Frame Finish: Brushed Anodized Dark Brown.
9.	Aluminum Track and Door Frame Finish: Brushed Anodized Black.
10.	Aluminum Track and Door Frame Finish: Brushed Anodized Nickel.
11.	Rollers: Basic rollers; system type A. Stainless steel with precision bearings.
a.	Door Weight: 110 lbs (50 kg).
b.	Door Weight: 176 lbs (80 kg).
c.	Door Weight: 264 lbs (120 kg).
12.	Rollers: Fluid rollers system type B. Stainless steel with precision bearings.
a.	Door Weight: 110 lbs (50 kg).
b.	Door Weight: 176 lbs (80 kg).
c.	Door Weight: 264 lbs (120 kg).
d.	Door Weight: 353 lbs (160 kg).
e.	Door Panel (WxH): ___ inches (___ mm).
13.	Door Frame Thickness: 1-3/4 (45 mm).
14.	Weight: 176 lbs (80 kg) maximum.
15.	Glass Thickness: 3/16 to 5/16 inches (5 to 8.5 mm). 
16.	Glass Finish: Transparent.
17.	Glass Finish: Frosted.
18.	Glass Finish: Transparent Bronze.
19.	Glass Finish: Transparent Grey.
20.	Glass Finish: Frosted Super White.
21.	Glass Finish: Reeded Glass.
22.	Options:
a.	Damper Stops.
b.	Fluid dampers.
c.	Handle kit.
d.	Load bearing mullion kit.
e.	Adjustable Closing jamb kit.
C.	Basis of Design: Magic 2 Frame Sliding Door System as manufactured by Linear Interior Systems Inc. Non-load bearing invisible sliding door system.
1.	Rolling Style: Bottom and top rollers, with bottom guide.
2.	Operation: Manual.
a.	Opening Direction: Left.
b.	Opening Direction: Right.
3.	Configuration: Single track.
4.	Width: ___ inches (___ mm).
5.	Weight: 176 lbs (80 kg) maximum.
6.	External aluminum track cover. Aligns with door minimizing the gap. Between door and frame.
7.	Aluminum Track Material: 6061-T6 extruded profiles.
8.	Aluminum Track Finish: Brushed Anodized Silver.
9.	Aluminum Track Finish: Brushed Anodized Dark Brown.
10.	Aluminum Track Finish: Brushed Anodized Black.
11.	Aluminum Track Finish: Brushed Anodized Nickel.
D.	URL Link to Brochure: Basic Rollers and Fluid Rollers : https://www.dropbox.com/scl/fo/7ve6yiqmmmo8zah6o8qy1/h?rlkey=74u4vfj0vap62m72xd87nclqy&dl=0
1.	Rollers: Basic rollers; system type A. Stainless steel with precision bearings.
a.	Door Weight: 110 lbs (50 kg).
b.	Door Weight: 176 lbs (80 kg).
c.	Door Weight: 264 lbs (120 kg).
2.	Rollers: Fluid rollers system type B. Stainless steel with precision bearings.
a.	Door Weight: 110 lbs (50 kg).
b.	Door Weight: 176 lbs (80 kg).
c.	Door Weight: 264 lbs (120 kg).
d.	Door Weight: 353 lbs (160 kg).
3.	Glass Thickness: 3/16 to 5/16 inches (5 to 8.5 mm).
4.	Glass Finish: Transparent.
5.	Glass Finish: Frosted.
6.	Glass Finish: Transparent Bronze.
7.	Glass Finish: Transparent Grey.
8.	Glass Finish: Frosted Super White.
9.	Glass Finish: Reeded Glass.
10.	Glazing Gasket: Bi-extruded.
11.	Options:
a.	Damper Stops.
b.	Fluid dampers.
c.	Handle kit.
d.	Load bearing mullion kit.
e.	Closing jamb kit.
E.	Basis of Design: 120 Series Top Rolling Sliding Glass Doors With Aluminum Frame.
1.	Operation: Manual.
2.	Configuration: Sliding door panel. And fixed door panel.
3.	Rolling Style: Top rollers, bottom guide.
a.	Single Undermount: Model 1280.
1)	Track Width: 2-3/16 inches (56 mm).
2)	Track Height: 2-3/4 inches (70 mm).
3)	Vertical Door Adjustment: 1/4 to 1/2 inches (7 to 13 mm).
b.	Double Undermount: 1285.
1)	Track Width: 3-3/4 inches (95 mm).
2)	Track Height: 2-15/16 (75 mm). 
3)	Vertical Door Adjustment: 1/4 to 1/2 inches (7 to 13 mm).
c.	Wall Mount: Model 1259.
1)	Track Width: 2-3/8 inches (61 mm).
2)	Track Height: 2-1/16 inches (53 mm).
3)	Cover: 2-3/4 inches (70 mm).
4)	Vertical Door Adjustment: 1/4 to 1/2 inches (7 to 13 mm).
d.	Wall Mount: Model 1270.
1)	Track Width: 1-9/16 inches (65 mm).
2)	Track Height: 1-5/16 inches (34 mm).
3)	Cover: 3-15/16 inches (100 mm).
4)	Vertical Door Adjustment: 1/4 to 1/2 inches (7 to 13 mm).
4.	Aluminum Track Material: 6061-T6 extruded profiles.
5.	Aluminum Track Door Frame Finish: Brushed Anodized Silver.
6.	Aluminum Track Door Frame Finish: Painted Black.
7.	Aluminum Track Door Frame Finish: Graphite.
8.	Aluminum Track Door Frame Finish: Metal Grey.
9.	Aluminum Track Door Frame Finish: White RAL 9002.
10.	Aluminum Track Door Frame Finish: White.
11.	Rollers: Basic rollers; system type A. Stainless steel with precision bearings.
a.	Door Weight: 110 lbs (50 kg).
b.	Door Weight: 176 lbs (80 kg).
c.	Door Weight: 264 lbs (120 kg).
12.	Rollers: Fluid rollers system type B. Stainless steel with precision bearings.
a.	Door Weight: 110 lbs (50 kg).
b.	Door Weight: 176 lbs (80 kg).
c.	Door Weight: 264 lbs (120 kg).
d.	Door Weight: 353 lbs (160 kg).
13.	Door Panel (WxH): ___ inches (___ mm).
14.	Door Frame Thickness: 1-3/4 inches (45 mm).
15.	Weight: (80 kg) maximum.
16.	Glass Thickness: 3/16 to 5/16 inches (5 to 8.5 mm). Monolithic mullions.
17.	Stile Profile Width: 1 inch (25 mm).
18.	Stile Profile Width with Gasket: 1-3/16 inch (30 mm).
19.	Handle: Short.
20.	Handle: Long.
21.	Glass Finish: Transparent.
22.	Glass Finish: Frosted.
23.	Glass Finish: Transparent Bronze.
24.	Glass Finish: Transparent Grey.
25.	Glass Finish: Frosted Super White.
26.	Glass Finish: Reeded Glass.
27.	Glazing Gasket: Bi-extruded.
28.	Options:
a.	Damper Stops.
b.	Fluid dampers.
c.	Handle kit.
d.	Load bearing mullion kit.
e.	Closing jamb kit.
F.	Basis of Design: 130 Series Bottom Rolling Sliding Glass Doors With Aluminum Frame as manufactured by Linear Interior Systems Inc.
1.	Operation: Manual.
2.	Configuration: Sliding door panel.
3.	Configuration: Double sliding door panel.
4.	Configuration: Triple sliding door panel.
5.	Rolling Style: Bottom rollers.
a.	Single Undermount: Model 250.
1)	Track Width: 1-5/8 inches (41 mm).
2)	Track Height: 2-3/16 inches (55 mm).
b.	Double Undermount: 260.
1)	Track Width: 3-1/8 inches (79 mm). 
2)	Track Height: 2-3/16 inches (55 mm).
c.	Triple Undermount: 270.
1)	Track Width: 3-1/8 inches (79 mm).
2)	Track Height: 2-3/16 inches (55 mm).
d.	Wall Mount, Single : Model 1642.
1)	Track Width: 4-3/4 inches (120 mm).
2)	Track Height: 2-3/16 inches (55 mm).
6.	Aluminum Track Material: 6061-T6 extruded profiles.
7.	Aluminum Track Door Frame Finish: Anodized Silver.
8.	Aluminum Track Door Frame Finish: Painted Black.
9.	Aluminum Track Door Frame Finish: Graphite.
10.	Aluminum Track Door Frame Finish: Metal Grey.
11.	Aluminum Track Door Frame Finish: White RAL 9002.
12.	Aluminum Track Door Frame Finish: White.
13.	Rollers: Basic rollers; system type A. Stainless steel with precision bearings.
a.	Door Weight: 110 lbs (50 kg).
b.	Door Weight: 176 lbs (80 kg).
c.	Door Weight: 264 lbs (120 kg).
14.	Rollers: Fluid rollers system type B. Stainless steel with precision bearings.
a.	Door Weight: 110 lbs (50 kg).
b.	Door Weight: 176 lbs (80 kg).
c.	Door Weight: 264 lbs (120 kg).
d.	Door Weight: 353 lbs (160 kg).
e.	Material: Stainless steel with stainless steel precision bearings.
15.	Door Panel (WxH): ___ inches (___ mm).
16.	Door Frame Thickness: 1 inch (26 mm).
17.	Weight: 176 lbs (80 kg) maximum.
18.	Glass Thickness: 3/16 to 5/16 inches (5 to 8.5 mm). Monolithic.
19.	Mullions.
20.	Stile Profile Width: 1 inch (25 mm).
21.	Stile Profile Width with Gasket: 1-3/16 inch (30.16 mm).
22.	Handle: Short.
23.	Handle: Long.
24.	Glass Finish: Transparent.
25.	Glass Finish: Frosted.
26.	Glass Finish: Transparent Bronze.
27.	Glass Finish: Transparent Grey.
28.	Glass Finish: Frosted Super White.
29.	Glass Finish: Reeded Glass.
30.	Glazing Gasket: Bi-extruded.
31.	Options:
a.	Damper Stops.
b.	Fluid dampers.
c.	Handle kit.
d.	Load bearing mullion kit.
e.	Closing jamb kit.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until the substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
3.4	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.
B.	Manufacturer's Services: Coordinate manufacturer's services in accordance with appropriate sections in Division 01.
3.5	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturers recommendations. 
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION