SECTION 10 30 00

MANUFACTURED FIREPLACES

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2019 -  2019 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Manufactured Fireplaces of the following types:
1.	Wood burning fireboxes.
2.	Gas B-vent system.
3.	Linear gas B-vent fireboxes.
4.	Vent free fireboxes.
B.	Pizza ovens.
1.2	RELATED SECTIONS
A.	Section 03 30 00 - Cast-in-Place Concrete.
B.	Section 04 20 00 - Unit Masonry.
C.	Section 05 50 00 - Metal Fabrications.
D.	Section 06 10 00 - Rough Carpentry.
E.	Section 21 20 00 - Fire-Extinguishing Systems.
1.3	REFERENCES
A.	American National Standards Institute (ANSI):
1.	ANSI Z21.11.2 - Gas-Fired Room Heaters, Volume II, Unvented Room Heaters.
2.	ANSI Z21.50 - Vented Decorative Gas Appliances.
B.	National Fire Protection Association (NFPA):
1.	NFPA 54 - National Fuel Gas Code.
2.	NFPA 211 - Standard for Chimneys, Fireplaces, Vents, and Solid Fuel-Burning Appliances.
C.	Underwriters Laboratories (UL):
1.	UL 103 - Standard for Factory-Built Chimneys for Residential Type and Building Heating Appliances.
2.	UL 127 - Standard for Factory-Built Fireplaces.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Verification Samples: Two representative units of each type, size, pattern and color.
D.	Shop Drawings: Include details of materials, construction and finish. Include relationship with adjacent construction. 
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
D.	Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
1.	Intent of mock-up is to demonstrate quality of workmanship and visual appearance.
2.	If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
3.	Retain mock-up during construction as a standard for comparison with completed work. 
4.	Do not alter or remove mock-up until work is completed or removal is authorized.
1.6	PRE-INSTALLATION CONFERENCE
A.	Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.8	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.9	WARRANTY
A.	Manufacturer's Limited LifetimeWarranty: Provide manufacturer's standard limited warranty.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Masonry Fireplace Industries, Inc., which is located at:<BR />P. O. Box 4338<BR />Riverside, CA 92514<BR />Toll Free Tel: 800-345-7078 <BR />Tel: 714-542-5397<BR />Fax: 951-588-8046<BR />Email: request info (bharris@mason-lite.com);Web: https://www.mason-lite.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	WOOD BURNING FIREBOXES
A.	Performance Requirements:
1.	Standards Compliance: UL 127 and UL 103.
2.	Heat resistant fire tested up to 1700 degrees F (927 degrees C).
B.	Basis of Design: Mason-Lite Firebox; as manufactured and supplied by Mason-Lite by MFI, Masonry Fireplace Industries, LLC.
1.	Description: Modular concrete fire box with lightweight design.
2.	Application: Indoor use.
3.	Application: Outdoor use.
4.	Model MFP33:
a.	Configuration: Single sided.
b.	Opening Size: 33 x 22-1/2 inches (838 x 572 mm).
c.	Flue Size: 12 inches (305 mm).
5.	Model MFP39:
a.	Configuration: Single sided.
b.	Opening Size: 39 x 30-1/2 inches (991 x 775 mm).
c.	Flue Size: 12 inches (305 mm).
6.	Model MFP44:
a.	Configuration: Single sided.
b.	Opening Size: 44 x 30-1/2 inches (1118 x 775 mm).
c.	Flue Size: 12 inches (305 mm).
7.	Model MFP49:
a.	Configuration: Single sided.
b.	Opening Size: 49 x 30-1/2 inches (1245 x 775 mm).
c.	Flue Size: 14 inches (356 mm).
8.	Model MFP63:
a.	Configuration: Single sided.
b.	Opening Size: 63 x 30-1/2 inches (1600 x 775 mm).
c.	Flue Size: 16 inches (406 mm).
9.	Model MFP75:
a.	Configuration: Single sided.
b.	Opening Size: 75 x 30-1/2 inches (1905 x 775 mm).
c.	Flue Size: 16 inches (406 mm).
10.	Model MFPST43:
a.	Configuration: See through, double sided.
b.	Opening Size: 43 x 24-3/4 inches (1092 x 629 mm).
c.	Flue Size: 16 inches (406 mm).
11.	Base: Metal base.
12.	Base: Concrete block.
13.	Base: _____.
14.	Liner: Firebrick, full running bond.
15.	Liner: Firebrick, split herringbone.
16.	Liner: Split running bond.
17.	Liner: _____.
2.3	GAS B-VENT SYSTEM
A.	Performance Requirements:
1.	Standards Compliance: ANSI Z21.50.
B.	Basis of Design: Mason-Lite Gas B-Vent System; as manufactured and supplied by Mason-Lite by MFI, Masonry Fireplace Industries, LLC.
1.	Description: Gas burning fireplace system utilizing B-Vent.
2.	Application: Indoor use.
3.	Application: Outdoor use.
4.	Model MGFP39:
a.	Configuration: Single sided.
b.	Opening Size: 39 x 32-7/8 inches (991 x 835 mm).
c.	Fuel: Natural gas, 65,000 BTU.
d.	Fuel: Propane.
e.	B-Vent: 10 inches (254 mm).
5.	Model MGFP44:
a.	Configuration: Single sided.
b.	Opening Size: 44 x 32-7/8 inches (1118 x 835 mm).
c.	Fuel: Natural gas, 65,000 BTU.
d.	Fuel: Propane.
e.	B-Vent: 10 inches (254 mm).
6.	Model MGFP49:
a.	Configuration: Single sided.
b.	Opening Size: 49 x 32-7/8 inches (1245 x 835 mm).
c.	Fuel: Natural gas, 80,000 BTU.
d.	Fuel: Propane.
e.	B-Vent: 10 inches (254 mm).
7.	Model MGFPST43:
a.	Configuration: See through, double sided.
b.	Opening Size: 43 x 24-3/4 inches (1092 x 629 mm).
c.	Fuel: Natural gas.
d.	Fuel: Propane.
e.	B-Vent: 12 inches (305 mm).
8.	Gas Logs: R.H. Peterson Real-Fyre realistic gas logs.
9.	Remote: Handheld remote for turning gas on or off.
10.	Ignition: Electronic with battery back-up.
11.	Shut-Off: Safety shut-off for fail safe operation.
12.	Base: Metal base.
13.	Base: Concrete block.
14.	Base: _____.
15.	Liner: Firebrick, full running bond.
16.	Liner: Firebrick, split herringbone.
17.	Liner: Split running bond.
18.	Liner: _____.
2.4	LINEAR GAS B-VENT FIREPLACES
A.	Performance Requirements:
1.	Standards Compliance: ANSI Z21.50 and NFPA 211.
B.	Basis of Design: Mason-Lite Gas B-Vent System; as manufactured and supplied by Mason-Lite by MFI, Masonry Fireplace Industries, LLC. Tested and Listed by Radco Laboratories.
1.	Description: Gas burning fireplace system utilizing B-Vent.
2.	Application: Indoor use.
3.	Application: Outdoor use.
4.	Model LMFP48:
a.	Configuration: Single sided.
b.	Opening Size: 48 x 22-1/2 inches (1219 x 572 mm).
c.	Flue: 12 inches (305 mm).
5.	Model LMFP48-NT:
a.	Configuration: Single sided, no trough.
b.	Opening Size: 48 x 22-1/2 inches (1219 x 572 mm).
c.	Flue: 12 inches (305 mm).
6.	Model LMFP60:
a.	Configuration: Single sided.
b.	Opening Size: 60 x 22.53 inches (1524 x 572 mm).
c.	Flue: 12 inches (305 mm).
7.	Model LMFP60-NT:
a.	Configuration: Single sided, no trough.
b.	Opening Size: 60 x 22-1/2 inches (1524 x 572 mm).
c.	Flue: 12 inches (305 mm).
8.	Model LMFP72:
a.	Configuration: Single sided.
b.	Opening Size: 72 x 22-1/2 inches (1829 x 572 mm).
c.	Flue: 12 inches (305 mm).
9.	Model LMFP72-NT:
a.	Configuration: Single sided, no trough.
b.	Opening Size: 72 x 22-1/2 inches (1829 x 572 mm).
c.	Flue: 12 inches (305 mm).
10.	Model LMFP84:
a.	Configuration: Single sided.
b.	Opening Size: 84 x 22-1/2 inches (2134 x 572 mm).
c.	Flue: 12 inches (305 mm).
11.	Model LMFP84-NT:
a.	Configuration: Single sided, no trough.
b.	Opening Size: 84 x 22-1/2 inches (2134 x 572 mm).
c.	Flue: 12 inches (305 mm).
12.	Model LMFP96:
a.	Configuration: Single sided.
b.	Opening Size: 96 x 22-1/2 inches (2438 x 572 mm).
c.	Flue: Two, 12 inches (305 mm) each.
13.	Model LMFP96-NT:
a.	Configuration: Single sided, no trough.
b.	Opening Size: 96 x 22-1/2 inches (2438 x 572 mm).
c.	Flue: Two, 12 inches (305 mm) each.
14.	Model LMFP108:
a.	Configuration: Single sided.
b.	Opening Size: 108 x 22-1/2 inches (2743 x 572 mm).
c.	Flue: Two, 12 inches (305 mm) each.
15.	Model LMFP108-NT:
a.	Configuration: Single sided, no trough.
b.	Opening Size: 108 x 22-1/2 inches (2743 x 572 mm).
c.	Flue: Two, 12 inches (305 mm) each.
16.	Model LMFP120:
a.	Configuration: Single sided.
b.	Opening Size: 120 x 22-1/2 inches (3048 x 572 mm).
c.	Flue: Two, 12 inches (305 mm) each.
17.	Model LMFP120-NT:
a.	Configuration: Single sided, no trough.
b.	Opening Size: 120 x 22-1/2 inches (3048 x 572 mm).
c.	Flue: Two, 12 inches (305 mm) each.
18.	Fuel: Natural gas.
19.	Fuel: Propane.
20.	Burner: Alpine Linear Burner.
21.	Burner: _____.
22.	Liner: Firebrick, full running bond.
23.	Liner: Firebrick, split herringbone.
24.	Liner: _____.
2.5	VENT FREE FIREBOXES
A.	Performance Requirements:
1.	Standards Compliance: ANSI Z21.11.2.
B.	Basis of Design: Mason-Lite Vent Free Firebox; as manufactured and supplied by Mason-Lite by MFI, Masonry Fireplace Industries, LLC.
1.	Description: Modular concrete fire box with lightweight design.
2.	Application: Indoor use.
3.	Application: Outdoor use.
4.	Model MFP39VF:
a.	Configuration: Single sided.
b.	Opening Size: 39 x 30-1/2 inches (991 x 775 mm).
5.	Model MFP44 VF:
a.	Configuration: Single sided.
b.	Opening Size: 44 x 30-1/2 inches (1118 x 775 mm).
6.	Model MFP49 VF:
a.	Configuration: Single sided.
b.	Opening Size: 49 x 30-1/2 inches (1245 x 775 mm).
7.	Model MFPST43VF:
a.	Configuration: See through, double sided.
b.	Opening Size: 43 x 30-1/2 inches (1092 x 775 mm).
8.	Fuel: Natural gas.
9.	Fuel: Propane.
10.	Burner: To be selected by Architect.
11.	Burner: _____.
12.	Liner: Firebrick, full running bond.
13.	Liner: Firebrick, split herringbone.
14.	Liner: Split running bond.
15.	Liner: _____.
2.6	PIZZA OVENS
A.	Basis of Design: Toscana Wood Fired Pizza Oven; as manufactured and supplied by Mason-Lite by MFI, Masonry Fireplace Industries, LLC.
1.	Application: Outdoor use.
2.	Table Top Model:
a.	Overall Size: 48 x 28 x 42.125 inches (1219 x 711 x 1070 mm).
b.	Opening Size: Arched 18 x 10 inches (457 x 254 mm).
c.	Base: _____.
d.	Base: As indicated on Drawings.
3.	Model with Wood Storage:
a.	Overall Size: 48 x 28 x 75 inches (1219 x 711 x 1905 mm).
b.	Opening Size: Arched 18 x 10 inches (457 x 254 mm).
4.	Finish: Stucco.
5.	Finish: Rock.
6.	Finish: Tile.
7.	Finish: Brick.
8.	Finish: _____.
9.	Door: Powder coated steel.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
C.	Verify proper fuel source is available.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, approved submittals, and in proper relationship with adjacent construction.
B.	Use manufacturer's guidelines for minimum clearances to combustibles, walls, and finishes.
C.	Set fireplace units plumb, level, and rigid.
D.	Anchor all components firmly in position.
E.	Connect to fuel system in accordance with NFPA 54.
3.4	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate field inspection in accordance with appropriate sections in Division 01.
B.	Test for proper operation, control and safety devices.
3.5	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturer's recommendations. 
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION