SECTION 09 54 00

RECESSED SHADE POCKETS FOR ROLLER SHADES

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2018 -  2018 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Ceiling-recessed pockets for the following types of roller shades:
1.	Manual shades.
2.	Motorized shades.
3.	Motorized shades with wire raceway.
4.	Double shades.
1.2	RELATED SECTIONS
A.	Section 09 51 23 - Acoustical Tile Ceilings.
B.	Section 09 28 13 - Cementitious Backing Boards.
C.	Section 12 23 00 - Interior Shutters* .
D.	Section 12 25 13 - Motorized Drapery Rods.
E.	Division 16 - Electrical.
1.3	REFERENCES
A.	ETL/UL 235: Standard for Door, Drapery, Gate, Louver, and Window Operators and Systems.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used.
C.	Shop Drawings: Plans, elevations, sections, product details, installation details, operational clearances, wiring diagrams and relationship to adjacent work.
D.	Warranty: Provide manufacturer's warranty documents as specified in this Section.
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Obtain roller shades system through one source from a single manufacturer with a minimum of ten years experience with roller shades.
B.	Installer Qualifications: Installer trained and certified by the manufacturer.
C.	Mock-Up: Provide a mock-up of one ceiling pocket assembly for evaluation of mounting, appearance and accessories.
1.	Locate mock-up where designated by Architect.
2.	Do not proceed with remaining work until, mock-up is accepted by Architect.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Deliver units in factory-labeled packages, marked with manufacturer and product name.
1.7	PROJECT CONDITIONS
A.	Environmental Limitations: Install units after finish work including painting is complete and ambient temperature and humidity conditions are maintained at the levels indicated for Project when occupied for its intended use.
1.8	WARRANTY
A.	Warranty: Provide manufacturer's standard limited 5 year warranty.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Mecho, which is located at:<BR />42-03  35th St.<BR />Long Island City, NY 11101<BR />Tel: 718-729-2020<BR />Fax: 718-729-2941<BR />Email: request info (marketing@mechoshade.com);Web: http://www.mechoshade.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	SHADE POCKETS
A.	Roller Shade Pocket: ElectroPocket and Non-ElectroPocket from Macho. For recessed mounting in acoustical tile, or drywall ceilings as indicated on the Drawings. For manual and motorized shades.
1.	Provide either extruded aluminum and or formed steel shade pocket with extruded aluminum trim for all exposed components, sized to accommodate roller shades, with exposed extruded aluminum closure, tile support and removable closure panel to provide access to shades. The max roll diameter shall provide a minimum of clearance of 1/4 inch (6 mm) from the top and 2 sides of the pocket and 1/2 inch (13 mm) clear from the inside of the accessible pocket closure. 
a.	Provide "Vented Pocket" such that there will be a minimum 12 sq inch (7742 sq mm) of return air per lineal foot allowing the solar gain to flow above the ceiling line into the plenum or over the roller shades into the interior space.
2.	Provide ETL/UL 235 Approved extruded aluminum KD ElectroPocket, in 10 ft. (3048 mm) lengths assembled on job site, with an integrated wiring raceway and mounting clips for: 
a.	Line Voltage disconnect connectors.
b.	Wireless receivers.
c.	Low Voltage splitters.
d.	Daisy chain non-plenum wiring raceway and integrated pocket assembly.
3.	Model: ElectroPocket 4155 with tile support.
a.	Dimensions: (W x H): 5-3/4 x 6-1/4 inch (146 x 159 mm).
b.	Maximum Roll Up Diameter: 4-1/4 inch (108 mm).
4.	Model: ElectroPocket Model 4156 without tile support.
a.	Dimensions: (W x H): 5-3/4 x 6-1/4 inch (146 x 159 mm).
b.	Maximum Roll Up Diameter: 4-1/4 inch (108 mm).
5.	Model: ElectroPocket Model 4165 with tile support.
a.	Dimensions (W x H): 6-5/8 x 6-1/4 inch (168 x 159 mm).
b.	Maximum Roll Up Diameter: 4-5/8 inch (117.5 mm)
6.	Model: ElectroPocket Model 4166 without tile support.
a.	Dimensions (W x H): 6-5/8 x 6-1/4 inch (168 x 159 mm).
b.	Maximum Roll Up Diameter: 4-5/8 inch (117.5 mm).
7.	Model: Non-ElectroPocket 4157 with tile support.
a.	Dimensions: (W x H): 5-3/4 x 6-1/4 inch (146 x 159 mm).
b.	Maximum Roll Up Diameter: 4-5/8 inch (117.5 mm).
8.	Model: Non-ElectroPocket without tile support.
a.	Dimensions (W x H): 5-3/4 x 6-1/4 inch (146 x 159 mm).
b.	Maximum Roll Up Diameter: 4-5/8 inch (117.5 mm).
9.	Model: Non-ElectroPocket with tile support.
a.	Dimensions (W x H): 6-5/8 x 6-1/4 inch (168 x 159 mm).
b.	Maximum Roll Up Diameter: 5-1/8 inch (130 mm).
10.	Model: Non-ElectroPocket 4168 without tile support.
a.	Dimensions (W x H): 6-5/8 x 6-1/4 inch (168 x 159 mm).
b.	Maximum Roll Up Diameter: 5-1/8 inch (130 mm).
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
C.	Confirm that blocking for roller shades is installed plumb, level, and in accordance with industry standard tolerances. The horizontal surface of the shade pocket shall not be out-of-level more than 1/16 inch (1.6 mm) over 20 linear feet (6 m).
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install ceiling-recessed pockets in accordance with manufacturer's recommendations, approved submittals, and in proper relationship with adjacent construction.
3.4	CLEANING AND PROTECTION
A.	Clean surfaces after installation, according to manufacturer's written instructions. Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION