SECTION 14 20 00

ELEVATORS AND DUMBWAITERS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2016 -  2020 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Residential Elevators.
1.	Glass home elevator
2.	Birdcage home elevator.
3.	Green home elevator.
4.	Hydraulic home elevator
5.	Elite home elevator.
B.	Commercial Elevators: Limited-use, limited access (LULA).
C.	Wheelchair lifts.
D.	Dumbwaiters:
1.	Residential.
2.	Commercial.
1.2	RELATED SECTIONS
A.	Section 03 30 00 - Cast-in-Place Concrete.
B.	Section 06 10 00 - Rough Carpentry.
C.	Section 08 11 00 - Metal Doors and Frames.
D.	Section 09 21 16.33 - Gypsum Board Area Separation Wall Assemblies.
E.	Section 09 60 00 - Flooring.
F.	Section 28 44 00 - Refrigerant Detection and Alarm.
G.	Division 16 Sections for electrical service for elevators to and including disconnect and fused switches at machine room.
H.	Division 16 Sections for standby power source, transfer switch, and connection from auxiliary contacts in transfer switch to controller.
I.	Division 16 Section for voice and data communication cabling for telephone service to elevators.
1.3	REFERENCES
A.	American Society of Mechanical Engineers (ASME) A17.1 - Safety Code for Elevators and Escalators.
B.	American Society of Mechanical Engineers (ASME) A18.1 - Safety Standard for Platform and Stairway Chair Lifts.
C.	CSA B44.1 - Safety Code for Elevators and Escalators.
D.	ANSI/NFPA 70 - National Electric Code.
E.	CAN/CSA C22.1 - Canadian Electrical Code.
F.	ICC/ANSI A117.1 - Accessible and Usable Buildings and Facilities.
G.	ANSI/NFPA 80 - Fire Doors and Windows.
H.	ANSI/UL 10B - Fire Tests of Door Assemblies.
I.	BADAAG - Americans with Disabilities Act Accessibility Guidelines.
J.	ISO 9001: 2000 - Quality Management Systems - Requirements.
K.	Model and Local Building Codes.
1.4	REQUIREMENTS OF REGULATORY AGENCIES
A.	Supply equipment in compliance with applicable jurisdictional authorities.
B.	File permits and execute inspections as required by jurisdictional authorities.
1.5	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Submit manufacturer/installer's product data, including:
1.	Descriptive brochures and product features.
2.	Power Information: Voltage, phase, and current electrical requirements.
C.	Shop Drawings: Submit manufacturer/installer's shop drawings, including plans, elevations, sections, and details, indicating location of equipment, loads, dimensions, and finish.
D.	Operation and Maintenance Manual: Submit manufacturer/installer's operation and maintenance manual; including operation, maintenance, adjustment, and cleaning instructions; and electrical wiring diagrams.
E.	Warranty: Submit documentation associated with manufacturer/installer's standard warranty.
1.6	QUALITY ASSURANCE
A.	Installer must have minimum 2-year experience installing similar products.
B.	Installer must be licensed according to jurisdictional authority.
C.	Installer must have sufficient liability insurance.
D.	Installer must be acceptable to the manufacturer. 
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Deliver and store products in manufacturer's unopened packaging until installation.
B.	Handle materials with proper equipment to avoid damage.
1.8	PRE-INSTALLATION MEETINGS
A.	Convene pre-installation meeting before start of installation of elevators.
B.	Require attendance of parties directly affecting work of this section, including Contractor, Architect, and elevator manufacturer/installer.
C.	Review examination, installation, field quality control, adjusting, cleaning, protection, and coordination with other work.
1.9	PROJECT CONDITIONS
A.	Hoistway complete and finished according to drawings.
B.	Temporary platforms at each landing with OSHA complian barricades.
C.	Coordinate availability of permanent power prior to installation start.
D.	Coordinate availability of secure, clean, dry storage area prior to delivery.
1.10	WARRANTY
A.	Residential Elevators: Manufacturer/installer shall guarantee materials and workmanship of equipment installed under these specifications according to manufacturer's published warranty policy.
1.	Warranty for Mechanical Components: 10 year.
2.	Warranty for Electrical Components: 3 year.
3.	Warranty for Labor: 1 year.
B.	Commercial Elevators: Manufacturer/installer shall guarantee materials and workmanship of equipment installed under these specifications according to manufacturer's published warranty policy.
1.	Warranty for Mechanical Components: 3 year.
2.	Warranty for Electrical Components: 3 year.
3.	Warranty for Labor: 1 year.
C.	Wheelchair Lifts: Manufacturer/installer shall guarantee materials and workmanship of equipment installed under these specifications according to manufacturer's published warranty policy.
1.	Warranty for Mechanical Components: 3 year.
2.	Warranty for Electrical Components: 3 year.
3.	Warranty for Labor: 1 year.
D.	Dumbwaiters: Manufacturer/installer shall guarantee materials and workmanship of equipment installed under these specifications according to manufacturer's published warranty policy.
1.	Warranty for Mechanical Components: 3 year.
2.	Warranty for Electrical Components: 3 year.
3.	Warranty for Labor: 1 year.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Nationwide Lifts, which is located at:<BR />6181 Thompson Rd.<BR />Syracuse, NY 13206<BR />Toll Free Tel: 888-323-8755<BR />Email: request info (info@nwlifts.com);Web: https://www.elevators.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	GLASS HOME ELEVATOR - ARTISAN ELEVATOR
A.	Installation by manufacturer authorized installer.
B.	Compliance with ASME A17.1 Section 5.3; Residential Elevators.
C.	Specifications:
1.	Number of Levels: 1 stop.
2.	Number of Levels: 2 stops.
3.	Number of Levels: 3 stops.
4.	Number of Levels: 4 stops.
5.	Number of Levels: 5 stops.
6.	Number of Levels: 6 stops.
7.	Vertical Travel (inch/mm): ______.
8.	Vertical Travel: As determined by the Architect.
9.	Vertical Travel: As detailed on the Drawings.
10.	Pit Depth: 0 inches; minimum.
11.	Pit Depth: 4 inches (102 mm)
12.	Pit Depth (inch/mm): ______.
13.	Pit Depth: As determined by the Architect.
14.	Pit Depth: As detailed on the Drawings.
15.	Overhead: ______.
16.	Overhead: As determined by the Architect.
17.	Overhead: As detailed on the Drawings.
18.	Enclosure Shape: Rectangular.
19.	Enclosure Shape: Square.
20.	Enclosure Shape: __________.
21.	Cab Height: 78 inches (1981 mm).
a.	Requires overhead of 96 inches (2438 mm) or greater.
22.	Cab Height: 84 inches (2134 mm).
a.	Requires overhead of 102 inches(2591 mm) or greater.
23.	Cab Height: 96 inches (2438 mm).
a.	Requires overhead of 114 inches (2896 mm) or greater.
24.	Cab Size (WxD): 28 x 26 inches (711 x 660 mm).
a.	Enclosure Footprint (WxD): 36 x 36 inches (914 x 914 mm).
25.	Cab Size (WxD): 40 x 38 inches (1016 x 965 mm).
a.	Enclosure Footprint (WxD): 48 x 48 inches (1219 x 1219 mm).
26.	Cab Size (WxD): 28 x 36 inches (711 x 914 mm). 
a.	Enclosure Footprint (WxD): 36 x 46 inches (914 x 1168 mm).
27.	Cab Size (WxD): 28 x 42 inches (711 x 1067 mm).
a.	Enclosure Footprint (WxD): 36 x 52 inches (914 x 1321 mm).
28.	Cab Size (WxD): 28 x 48 inches (711 x 1219 mm).
a.	Enclosure Footprint (WxD): 36 x 58 inches (914 x 1473 mm).
29.	Cab Size (WxD): 36 x 48 inches (914 x 1219 mm). 
a.	Enclosure Footprint (WxD): 44 x 58 inches (1118 x 1473 mm).
30.	Cab Size (WxD): 36 x 54 inches (914 x 1372 mm).
a.	Enclosure Footprint (WxD): 44 x 64 inches (1118 x 1626 mm).
31.	Cab Size (WxD): 36 x 60 inches (914 x 1524 mm).
a.	Enclosure Footprint (WxD): 44 x 70 inches (1118 x 1778 mm).
32.	Cab Size (WxD): 40 x 48 inches (1016 x 1219 mm).
a.	Enclosure Footprint (WxD): 48 x 58 inches (1219 x 1473 mm).
33.	Cab Size (WxD): 40 x 54 inches (1016 x 1372 mm).
a.	Enclosure Footprint (WxD): 48 x 64 inches (914 x 1626 mm).
34.	Cab Size (WxD): 44 x 48 inches (1118 x 1219 mm).
a.	Enclosure Footprint (WxD): 52 x 58 inches (1321 x 1473 mm).
35.	Cab Size (WxD): 40 x 60 inches (1016 x 1524 mm).
a.	Enclosure Footprint (WxD): 48 x 70 inch (1219 x 1778 mm).
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
36.	Cab Size (WxD): 44 x 54 inch (1118 x 1372 mm).
a.	Approx. Enclosure Footprint (WxD): 52 x 64 (1321 x 1626 mm).
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
37.	Cab Size (WxD): 48 x 48 inch (1219 x 1219 mm)
a.	Approx. Enclosure Footprint (WxD): 56 x 58 inch (1422 x 1473 mm)
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
38.	Cab Size (WxD): ____ x ____ inch (____ x ____ mm).
a.	Enclosure Footprint (WxD): ____ x ____ inch (____ x ____ mm).
39.	Cab Configuration: Enter/exit same side.
40.	Cab Configuration: Enter/exit opposite sides
41.	Load Capacity: 950 lbs (430.9 kg).
42.	Load Capacity: 1000 lbs (453.6 kg).
43.	Load Capacity: 1400 lbs (635 kg). Requires variance.
44.	Rated Speed: 40 ft per min (203 mm per sec).
45.	Power Supply: 230 V, 1 PH, 60 Hz, 30 A.
46.	Lighting Supply: 115 V, 60 Hz, 15 A.
47.	Communication: Functional phone line.
48.	Drive System: Winding drum with variable frequency drive.
49.	Machine Room: Not Required 
50.	Controller (WxHxD): 24 x 24 x 8 inch (610 x 610 x 203 mm). Must be hung on wall near elevator.
51.	Control System: PLC with error log and troubleshooting indicators.
52.	Temperature Range: 14 to 104 degrees F (Minus 10 to 40 degrees C).
53.	Cab Lighting: Automatic LED.
54.	Cab Phone: Hands-free, recessed in wall.
55.	Safety Features:
a.	Cab emergency stop switch.
b.	Cab gate switch.
c.	Pit stop switch 
d.	Car top stop switch.
e.	Battery backup lowering
f.	Battery backup lighting.
g.	Upper and lower final limit switches. 
h.	Safety brakes.
i.	Slack cable switch.
j.	Auxiliary safety circuit for service.
56.	Cab Panels: Clear Acrylic
57.	Cab Panels: Laminated Glass
58.	Enclosure Panels: Clear Acrylic
59.	Enclosure Panels: Laminated Glass
60.	Frame Powder Coat Color: Fine Texture Black.
61.	Frame Powder Coat Color: Fine Texture White.
62.	Frame Powder Coat Color: Gun Metal.
63.	Frame Powder Coat Color: Bronze.
64.	Frame Powder Coat Color: Copper Vein.
65.	Frame Powder Coat Color: Blue-Grey.
66.	Frame Powder Coat Color: Anthracite Metallic.
67.	Frame Powder Coat Color: Greco.
68.	Frame Powder Coat Color: Taupe.
69.	Frame Powder Coat Color: Hartford Green.
70.	Frame Powder Coat Color: Deore (Gold).
71.	Frame Powder Coat Color: _____________.
72.	Frame Powder Coat Color: As determined by Architect.
2.3	BIRDCAGE HOME ELEVATOR - ARTISAN BIRDCAGE ELEVATOR
A.	Installation by manufacturer authorized installer.
B.	Compliance with ASME A17.1 Section 5.3; Residential Elevators.
C.	Specifications:
1.	Number of Levels: 1 stop.
2.	Number of Levels: 2 stops.
3.	Number of Levels: 3 stops.
4.	Number of Levels: 4 stops.
5.	Number of Levels: 5 stops.
6.	Number of Levels: 6 stops.
7.	Vertical Travel (inch/mm): ______.
8.	Vertical Travel: As determined by the Architect.
9.	Vertical Travel: As detailed on the Drawings.
10.	Pit Depth: 0 inches; minimum.
11.	Pit Depth: 4 inches (102 mm)
12.	Pit Depth (inch/mm): ______.
13.	Pit Depth: As determined by the Architect.
14.	Pit Depth: As detailed on the Drawings.
15.	Overhead: ______.
16.	Overhead: As determined by the Architect.
17.	Overhead: As detailed on the Drawings.
18.	Enclosure Shape: Round.
19.	Enclosure Shape: Rectangular.
20.	Enclosure Shape: Square.
21.	Enclosure Shape: __________.
22.	Cab Height: 78 inches (1981 mm).
a.	Requires overhead of 96 inches (2438 mm) or greater.
23.	Cab Height: 84 inches (2134 mm).
a.	Requires overhead of 102 inches(2591 mm) or greater.
24.	Cab Height: 96 inches (2438 mm).
a.	Requires overhead of 114 inches (2896 mm) or greater.
25.	Cab Size: 38 inch (965 mm) diameter.
a.	Approx. Enclosure Footprint (WxD): 48 inches (1219 mm) diameter.
26.	Cab Size: 48 inch (1219 mm) diameter.
a.	Approx. Enclosure Footprint (WxD): 58 inches (1473 mm) diameter.
27.	Cab Size (WxD): 28 x 26 inches (711 x 660 mm).
a.	Enclosure Footprint (WxD): 36 x 36 inches (914 x 914 mm).
28.	Cab Size (WxD): 40 x 38 inches (1016 x 965 mm).
a.	Enclosure Footprint (WxD): 48 x 48 inches (1219 x 1219 mm).
29.	Cab Size (WxD): 28 x 36 inches (711 x 914 mm). 
a.	Enclosure Footprint (WxD): 36 x 46 inches (914 x 1168 mm).
30.	Cab Size (WxD): 28 x 42 inches (711 x 1067 mm).
a.	Enclosure Footprint (WxD): 36 x 52 inches (914 x 1321 mm).
31.	Cab Size (WxD): 28 x 48 inches (711 x 1219 mm).
a.	Enclosure Footprint (WxD): 36 x 58 inches (914 x 1473 mm).
32.	Cab Size (WxD): 36 x 48 inches (914 x 1219 mm). 
a.	Enclosure Footprint (WxD): 44 x 58 inches (1118 x 1473 mm).
33.	Cab Size (WxD): 36 x 54 inches (914 x 1372 mm).
a.	Enclosure Footprint (WxD): 44 x 64 inches (1118 x 1626 mm).
34.	Cab Size (WxD): 36 x 60 inches (914 x 1524 mm).
a.	Enclosure Footprint (WxD): 44 x 70 inches (1118 x 1778 mm).
35.	Cab Size (WxD): 40 x 48 inches (1016 x 1219 mm).
a.	Enclosure Footprint (WxD): 48 x 58 inches (1219 x 1473 mm).
36.	Cab Size (WxD): 40 x 54 inches (1016 x 1372 mm).
a.	Enclosure Footprint (WxD): 48 x 64 inches (914 x 1626 mm).
37.	Cab Size (WxD): 44 x 48 inches (1118 x 1219 mm).
a.	Enclosure Footprint (WxD): 52 x 58 inches (1321 x 1473 mm).
38.	Cab Size (WxD): 40 x 60 inches (1016 x 1524 mm).
a.	Enclosure Footprint (WxD): 48 x 70 inch (1219 x 1778 mm).
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
39.	Cab Size (WxD): 44 x 54 inch (1118 x 1372 mm).
a.	Approx. Enclosure Footprint (WxD): 52 x 64 (1321 x 1626 mm).
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
40.	Cab Size (WxD): 48 x 48 inch (1219 x 1219 mm)
a.	Approx. Enclosure Footprint (WxD): 56 x 58 inch (1422 x 1473 mm)
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
41.	Cab Size (WxD): ____ x ____ inch (____ x ____ mm).
a.	Enclosure Footprint (WxD): ____ x ____ inch (____ x ____ mm).
42.	Cab Configuration: Enter/exit same side.
43.	Cab Configuration: Enter/exit opposite sides
44.	Load Capacity: 950 lbs (430.9 kg).
45.	Load Capacity: 1000 lbs (453.6 kg).
46.	Load Capacity: 1400 lbs (635 kg). Requires variance.
47.	Rated Speed: 40 ft per min (203 mm per sec).
48.	Power Supply: 230 V, 1 PH, 60 Hz, 30 A.
49.	Lighting Supply: 115 V, 60 Hz, 15 A.
50.	Communication: Functional phone line.
51.	Drive System: Winding drum with variable frequency drive.
52.	Machine Room: Not Required 
53.	Controller (WxHxD): 24 x 24 x 8 inch (610 x 610 x 203 mm). Must be hung on wall near elevator.
54.	Control System: PLC with error log and troubleshooting indicators.
55.	Temperature Range: 14 to 104 degrees F (Minus 10 to 40 degrees C).
56.	Cab Lighting: Automatic LED.
57.	Cab Phone: Hands-free, recessed in wall.
58.	Safety Features:
a.	Cab emergency stop switch.
b.	Cab gate switch.
c.	Pit stop switch 
d.	Car top stop switch.
e.	Battery backup lowering. 
f.	Battery backup lighting.
g.	Upper and lower final limit switches. 
h.	Safety brakes.
i.	Slack cable switch. 
j.	Auxiliary safety circuit for service.
59.	Cab Panels: Clear Acrylic
60.	Cab Panels: Laminated Glass
61.	Cab Panels: As determined by the Architect
62.	Cab Panels: ________
63.	Enclosure Panels: Clear Acrylic
64.	Enclosure Panels: Laminated Glass
65.	Enclosure Panels: As determined by the Architect.
66.	Enclosure Panels: ________.
67.	Frame Powder Coat Color: Fine Texture Black.
68.	Frame Powder Coat Color: Fine Texture White.
69.	Frame Powder Coat Color: Gun Metal.
70.	Frame Powder Coat Color: Bronze.
71.	Frame Powder Coat Color: Copper Vein.
72.	Frame Powder Coat Color: Blue-Grey.
73.	Frame Powder Coat Color: Anthracite Metallic.
74.	Frame Powder Coat Color: Greco.
75.	Frame Powder Coat Color: Taupe.
76.	Frame Powder Coat Color: Hartford Green.
77.	Frame Powder Coat Color: Deore (Gold).
78.	Frame Powder Coat Color: _____________.
79.	Frame Powder Coat Color: As determined by Architect.
2.4	GREEN HOME ELEVATOR - FREEDOM GREEN 
A.	Installation by manufacturer authorized installer.
B.	Compliance with ASME A17.1 Section 5.3; Residential Elevators.
C.	Specifications:
1.	Number of Levels: 1 stop.
2.	Number of Levels: 2 stops.
3.	Number of Levels: 3 stops.
4.	Number of Levels: 4 stops.
5.	Number of Levels: 5 stops.
6.	Number of Levels: 6 stops.
7.	Vertical Travel (ft/mm) ______. 
8.	Pit Depth: 0 inches; minimum.
9.	Pit Depth: 8 inches (203 mm)
10.	Pit Depth:  14 inches (356 mm)
11.	Pit Depth (inch/mm): ______.
12.	Pit Depth: As determined by the Architect.
13.	Pit Depth: As detailed on the Drawings.
14.	Overhead: ______.
15.	Overhead: As determined by the Architect.
16.	Overhead: As detailed on the Drawings.
17.	Cab Height: 78 inches (1981 mm).
a.	Requires overhead of 96 inches (2438 mm) or greater.
18.	Cab Height: 84 inches (2134 mm).
a.	Requires overhead of 102 inches(2591 mm) or greater.
19.	Cab Height: 96 inches (2438 mm).
a.	Requires overhead of 114 inches (2896 mm) or greater.
20.	Cab Size (WxD): 28 x 26 inches (711 x 660 mm).
a.	Enclosure Footprint (WxD): 36 x 36 inches (914 x 914 mm).
21.	Cab Size (WxD): 40 x 38 inches (1016 x 965 mm).
a.	Enclosure Footprint (WxD): 48 x 48 inches (1219 x 1219 mm).
22.	Cab Size (WxD): 28 x 36 inches (711 x 914 mm). 
a.	Enclosure Footprint (WxD): 36 x 46 inches (914 x 1168 mm).
23.	Cab Size (WxD): 28 x 42 inches (711 x 1067 mm).
a.	Enclosure Footprint (WxD): 36 x 52 inches (914 x 1321 mm).
24.	Cab Size (WxD): 28 x 48 inches (711 x 1219 mm).
a.	Enclosure Footprint (WxD): 36 x 58 inches (914 x 1473 mm).
25.	Cab Size (WxD): 36 x 48 inches (914 x 1219 mm). 
a.	Enclosure Footprint (WxD): 44 x 58 inches (1118 x 1473 mm).
26.	Cab Size (WxD): 36 x 54 inches (914 x 1372 mm).
a.	Enclosure Footprint (WxD): 44 x 64 inches (1118 x 1626 mm).
27.	Cab Size (WxD): 36 x 60 inches (914 x 1524 mm).
a.	Enclosure Footprint (WxD): 44 x 70 inches (1118 x 1778 mm).
28.	Cab Size (WxD): 40 x 48 inches (1016 x 1219 mm).
a.	Enclosure Footprint (WxD): 48 x 58 inches (1219 x 1473 mm).
29.	Cab Size (WxD): 40 x 54 inches (1016 x 1372 mm).
a.	Enclosure Footprint (WxD): 48 x 64 inches (914 x 1626 mm).
30.	Cab Size (WxD): 44 x 48 inches (1118 x 1219 mm).
a.	Enclosure Footprint (WxD): 52 x 58 inches (1321 x 1473 mm).
31.	Cab Size (WxD): 40 x 60 inches (1016 x 1524 mm).
a.	Enclosure Footprint (WxD): 48 x 70 inch (1219 x 1778 mm).
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
32.	Cab Size (WxD): 44 x 54 inch (1118 x 1372 mm).
a.	Approx. Enclosure Footprint (WxD): 52 x 64 (1321 x 1626 mm).
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
33.	Cab Size (WxD): 48 x 48 inch (1219 x 1219 mm)
a.	Approx. Enclosure Footprint (WxD): 56 x 58 inch (1422 x 1473 mm)
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
34.	Cab Size (WxD): ____ x ____ inch (____ x ____ mm).
a.	Enclosure Footprint (WxD): ____ x ____ inch (____ x ____ mm).
35.	Cab Configuration: Enter/exit same side.
36.	Cab Configuration: Enter/exit opposite sides
37.	Cab Configuration: Enter/exit 90 degrees
38.	Load Capacity: 950 lbs (430.9 kg).
39.	Load Capacity: 1000 lbs (453.6 kg).
40.	Load Capacity: 1400 lbs (635 kg). Requires variance.
41.	Rated Speed: 40 ft per min (203 mm per sec).
42.	Power Supply: 230 V, 1 PH, 60 Hz, 30 A.
43.	Lighting Supply: 115 V, 60 Hz, 15 A.
44.	Communication: Functional phone line.
45.	Drive System: Winding drum with variable frequency drive.
46.	Machine Room: Not Required 
47.	Controller (WxHxD): 24 x 24 x 8 inch (610 x 610 x 203 mm). Must be hung on wall near elevator.
48.	Control System: PLC with error log and troubleshooting indicators.
49.	Temperature Range: 14 to 104 degrees F (Minus 10 to 40 degrees C).
50.	Cab Lighting: Automatic LED.
51.	Cab Phone: Hands-free, recessed in wall.
52.	Safety Features:
a.	Cab emergency stop switch.
b.	Cab gate switch.
c.	Pit stop switch.
d.	Car top stop switch.
e.	Battery backup lowering.
f.	Battery backup lighting.
g.	Upper and lower final limit switches.
h.	Safety brakes.
i.	Slack cable switch.
j.	Auxiliary safety circuit for service.
53.	Hall Station / COP Finish: Stainless steel.
54.	Hall Station / COP Finish: Brass.
55.	Hall Station / COP Finish: Bronze.
56.	Cab Panel: Melamine. Gray.
57.	Cab Panel: Melamine. Oak.
58.	Cab Panel: Melamine. Maple.
59.	Cab Panel: Melamine. Cherry.
60.	Cab Panel: Unfinished Hardwood Veneer. Oak.
61.	Cab Panel: Unfinished Hardwood Veneer. Maple.
62.	Cab Panel: Unfinished Hardwood Veneer. Cherry.
63.	Cab Panel: Unfinished Hardwood Veneer. Mahogany.
64.	Cab Panel: Stainless steel.
65.	Cab Panel: Glass.
66.	Cab Panel: As determined by the Architect.
67.	Cab Panel: ________.
68.	Cab Gate: Center-parting dual bi-fold gate, automatic.
a.	Material: Glass.
b.	Material: Stainless.
c.	Material: Painted steel.
69.	Cab Gate: Accordion gate, manual.
a.	Material: Vinyl.
b.	Material: Aluminum.
c.	Material: Acrylic.
d.	Material: Wood veneer.
70.	Cab Gate: Accordion, automatic. 
a.	Material: Vinyl.
b.	Material: Aluminum.
c.	Material: Acrylic.
d.	Material: Wood veneer.
71.	Cab Gate: 2-speed sliding gate
a.	Material: Stainless steel.
b.	Material: Primed steel.
c.	Material: Glass.
72.	Cab Gate: 3-speed sliding gate.
a.	Material: Stainless steel.
b.	Material: Primed steel.
c.	Material: Glass.
73.	Landing Doors: Swing doors by others. EMI interlocks provided with elevator.
74.	Landing Doors: 2-speed sliding door.
a.	Material: Stainless steel.
b.	Material: Primed steel.
c.	Material: Glass.
75.	Landing Doors: 3-speed sliding door.
a.	Material: Stainless steel.
b.	Material: Primed steel.
c.	Material: Glass.
76.	Landing Doors: Fire-rated 2-speed sliding doors.
a.	Material: Stainless steel.
b.	Material: Primed steel.
2.5	HYDRAULIC HOME ELEVATOR - FREEDOM HYDRO 
A.	Installation by manufacturer authorized installer.
B.	Compliance with ASME A17.1 Section 5.3; Residential Elevators.
C.	Specifications:
1.	Number of Levels: 1 stop.
2.	Number of Levels: 2 stops.
3.	Number of Levels: 3 stops.
4.	Number of Levels: 4 stops.
5.	Number of Levels: 5 stops.
6.	Number of Levels: 6 stops.
7.	Vertical Travel (inch/mm): ______.
8.	Vertical Travel: As determined by the Architect. 
9.	Vertical Travel: As detailed on the Drawings.
10.	Pit Depth:. 8 inches (203 mm)
11.	Pit Depth: 14 inches (356 mm)
12.	Overhead: ______.
13.	Overhead: As determined by the Architect.
14.	Overhead: As detailed on the Drawings.
15.	Cab Height: 78 inches (1981 mm).
a.	Requires overhead of 96 inches (2438 mm) or greater.
16.	Cab Height: 84 inches (2134 mm).
a.	Requires overhead of 102 inches(2591 mm) or greater.
17.	Cab Height: 96 inches (2438 mm).
a.	Requires overhead of 114 inches (2896 mm) or greater.
18.	Cab Size (WxD): 36 x 48 inches (914 x 1219 mm). 
a.	Enclosure Footprint (WxD): 44 x 58 inches (1118 x 1473 mm).
19.	Cab Size (WxD): 36 x 54 inches (914 x 1372 mm).
a.	Enclosure Footprint (WxD): 44 x 64 inches (1118 x 1626 mm).
20.	Cab Size (WxD): 36 x 60 inches (914 x 1524 mm).
a.	Enclosure Footprint (WxD): 44 x 70 inches (1118 x 1778 mm).
21.	Cab Size (WxD): 40 x 48 inches (1016 x 1219 mm).
a.	Enclosure Footprint (WxD): 48 x 58 inches (1219 x 1473 mm).
22.	Cab Size (WxD): 40 x 54 inches (1016 x 1372 mm).
a.	Enclosure Footprint (WxD): 48 x 64 inches (914 x 1626 mm).
23.	Cab Size (WxD): 44 x 48 inches (1118 x 1219 mm).
a.	Enclosure Footprint (WxD): 52 x 58 inches (1321 x 1473 mm).
24.	Cab Size (WxD): 40 x 60 inches (1016 x 1524 mm).
a.	Enclosure Footprint (WxD): 48 x 70 inch (1219 x 1778 mm).
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
25.	Cab Size (WxD): 44 x 54 inch (1118 x 1372 mm).
a.	Approx. Enclosure Footprint (WxD): 52 x 64 (1321 x 1626 mm).
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
26.	Cab Size (WxD): 48 x 48 inch (1219 x 1219 mm)
a.	Approx. Enclosure Footprint (WxD): 56 x 58 inch (1422 x 1473 mm)
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
27.	Cab Size (WxD): ____ x ____ inch (____ x ____ mm).
a.	Enclosure Footprint (WxD): ____ x ____ inch (____ x ____ mm).
28.	Cab Configuration: Enter/exit same side.
29.	Cab Configuration: Enter/exit opposite sides.
30.	Cab Configuration: Enter/exit 90 degrees.
31.	Load Capacity: 950 lbs (430.9 kg).
32.	Load Capacity: 1000 lbs (453.6 kg).
33.	Load Capacity: 1400 lbs (635 kg). Requires variance.
34.	Rated Speed: 40 ft per min (203 mm per sec).
35.	Power Supply: 230 V, 1 PH, 60 Hz, 30 A.
36.	Lighting Supply: 115 V, 60 Hz, 15 A.
37.	Communication: Functional phone line.
38.	Drive System: Winding drum with variable frequency drive.
39.	Machine Room: Not Required 
40.	Controller (WxHxD): 24 x 24 x 8 inch (610 x 610 x 203 mm). Must be hung on wall near elevator.
41.	Control System: PLC with error log and troubleshooting indicators.
42.	Temperature Range: 14 to 104 degrees F (Minus 10 to 40 degrees C).
43.	Cab Lighting: Automatic LED.
44.	Cab Phone: Hands-free, recessed in wall.
45.	Safety Features:
a.	Cab emergency stop switch.
b.	Cab gate switch.
c.	Pit stop switch 
d.	Car top stop switch.
e.	Battery backup lowering
f.	Battery backup lighting.
g.	Upper and lower final limit switches. 
h.	Safety brakes.
i.	Slack cable switch.
j.	Auxiliary safety circuit for service.
46.	Hall Station / COP Finish: Stainless steel.
47.	Hall Station / COP Finish: Brass.
48.	Hall Station / COP Finish: Bronze.
49.	Cab Panel: Melamine. Gray.
50.	Cab Panel: Melamine. Oak.
51.	Cab Panel: Melamine. Maple.
52.	Cab Panel: Melamine. Cherry.
53.	Cab Panel: Unfinished Hardwood Veneer. Oak.
54.	Cab Panel: Unfinished Hardwood Veneer. Maple.
55.	Cab Panel: Unfinished Hardwood Veneer. Cherry.
56.	Cab Panel: Unfinished Hardwood Veneer. Mahogany.
57.	Cab Panel: Stainless Steel.
58.	Cab Panel: Glass.
59.	Cab Panel: As determined by the Architect.
60.	Cab Panel: ________.
61.	Cab Gate: Center-parting dual bi-fold gate, automatic.
a.	Material: Glass.
b.	Material: Stainless.
c.	Material: Painted steel.
62.	Cab Gate: Accordion gate, manual.
a.	Material: Vinyl.
b.	Material: Aluminum.
c.	Material: Acrylic.
d.	Material: Wood veneer.
63.	Cab Gate: Accordion, automatic. 
a.	Material: Vinyl.
b.	Material: Aluminum.
c.	Material: Acrylic.
d.	Material: Wood veneer.
64.	Cab Gate: 2-speed sliding gate
a.	Material: Stainless steel.
b.	Material: Primed steel.
c.	Material: Glass.
65.	Cab Gate: 3-speed sliding gate.
a.	Material: Stainless steel.
b.	Material: Primed steel.
c.	Material: Glass.
66.	Landing Doors: Swing doors by others. EMI interlocks provided with elevator.
67.	Landing Doors: 2-speed sliding door.
a.	Material: Stainless steel.
b.	Material: Primed steel.
c.	Material: Glass.
68.	Landing Doors: 3-speed sliding door.
a.	Material: Stainless steel.
b.	Material: Primed steel.
c.	Material: Glass.
69.	Landing Doors: Fire-rated 2-speed sliding doors.
a.	Material: Stainless steel.
b.	Material: Primed steel.
2.6	ELITE HOME ELEVATOR - FREEDOM ELITE 
A.	Installation by manufacturer authorized installer.
B.	Compliance with ASME A17.1 Section 5.3; Residential Elevators.
C.	Specifications:
1.	Number of Levels: 1 stop.
2.	Number of Levels: 2 stops.
3.	Number of Levels: 3 stops.
4.	Number of Levels: 4 stops.
5.	Number of Levels: 5 stops.
6.	Number of Levels: 6 stops.
7.	Vertical Travel (ft/mm) ______. 
8.	Vertical Travel: As determined by the Architect. 
9.	Vertical Travel: As detailed on the Drawings.
10.	Pit Depth: 0 inches. Minimum.
11.	Pit Depth: 14 inch (356 mm) 
12.	Pit Depth (inch/mm): ______.
13.	Overhead: ______.
14.	Overhead: As determined by the Architect.
15.	Overhead: As detailed on the Drawings.
16.	Cab Height: 84 inches (2134 mm).
a.	Requires overhead of 108 inches (2743 mm) or greater.
17.	Cab Height: 96 inches (2438 mm).
a.	Requires overhead of 120 inches (3048 mm) or greater.
18.	Cab Size (WxD): 40 x 48 inches (1016 x 1219 mm).
a.	Enclosure Footprint (WxD): 48 x 58 inches (1219 x 1473 mm).
19.	Cab Size (WxD): 40 x 54 inches (1016 x 1372 mm).
a.	Enclosure Footprint (WxD): 48 x 64 inches (914 x 1626 mm).
20.	Cab Size (WxD): 44 x 48 inches (1118 x 1219 mm).
a.	Enclosure Footprint (WxD): 52 x 58 inches (1321 x 1473 mm).
21.	Cab Size (WxD): 40 x 60 inches (1016 x 1524 mm).
a.	Enclosure Footprint (WxD): 48 x 70 inch (1219 x 1778 mm).
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
22.	Cab Size (WxD): 44 x 54 inch (1118 x 1372 mm).
a.	Approx. Enclosure Footprint (WxD): 52 x 64 (1321 x 1626 mm).
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
23.	Cab Size (WxD): 48 x 48 inch (1219 x 1219 mm)
a.	Approx. Enclosure Footprint (WxD): 56 x 58 inch (1422 x 1473 mm)
b.	Requires 1400 lbs (635 kg) capacity.
c.	Requires variance.
24.	Cab Size (WxD): ____ x ____ inch (____ x ____ mm).
a.	Enclosure Footprint (WxD): ____ x ____ inch (____ x ____ mm).
25.	Cab Configuration: Enter/exit same side.
26.	Cab Configuration: Enter/exit opposite sides.
27.	Cab Configuration: Enter/exit 90 degrees.
28.	Load Capacity: 950 lbs (430.9 kg).
29.	Load Capacity: 1000 lbs (453.6 kg).
30.	Load Capacity: 1400 lbs (635 kg). Requires variance.
31.	Rated Speed: 40 ft per min (203 mm per sec).
32.	Power Supply: 230 V, 1 PH, 60 Hz, 30 A.
33.	Lighting Supply: 115 V, 60 Hz, 15 A.
34.	Communication: Functional phone line.
35.	Drive System: Winding drum with variable frequency drive.
36.	Machine Room: Not Required 
37.	Controller (WxHxD): 24 x 24 x 8 inch (610 x 610 x 203 mm). Must be hung on wall near elevator.
38.	Control System: PLC with error log and troubleshooting indicators.
39.	Temperature Range: 14 to 104 degrees F (Minus 10 to 40 degrees C).
40.	Cab Lighting: Automatic LED.
41.	Cab Phone: Hands-free, recessed in wall.
42.	Safety Features:
a.	Cab emergency stop switch.
b.	Cab gate switch.
c.	Pit stop switch 
d.	Car top stop switch.
e.	Battery backup lowering. 
f.	Battery backup lighting.
g.	Upper and lower final limit switches. 
h.	Safety brakes.
i.	Slack cable switch. 
j.	Auxiliary safety circuit for service.
43.	Hall Station / COP Finish: Stainless steel.
44.	Hall Station / COP Finish: Brass.
45.	Hall Station / COP Finish: Bronze.
46.	Cab Panel: Melamine. Gray.
47.	Cab Panel: Melamine. Oak.
48.	Cab Panel: Melamine. Maple.
49.	Cab Panel: Melamine. Cherry.
50.	Cab Panel: Unfinished Hardwood Veneer. Oak.
51.	Cab Panel: Unfinished Hardwood Veneer. Maple.
52.	Cab Panel: Unfinished Hardwood Veneer. Cherry.
53.	Cab Panel: Unfinished Hardwood Veneer. Mahogany.
54.	Cab Panel: Stainless steel.
55.	Cab Panel: Glass.
56.	Cab Panel: As determined by the Architect.
57.	Cab Panel: ________.
58.	Cab Gate: Center-parting dual bi-fold gate, automatic.
a.	Material: Glass.
b.	Material: Stainless.
c.	Material: Painted steel.
59.	Cab Gate: Accordion gate, manual.
a.	Material: Vinyl.
b.	Material: Aluminum.
c.	Material: Acrylic.
d.	Material: Wood veneer.
60.	Cab Gate: Accordion, automatic. 
a.	Material: Vinyl.
b.	Material: Aluminum.
c.	Material: Acrylic.
d.	Material: Wood veneer.
61.	Cab Gate: 2-speed sliding gate
a.	Material: Stainless steel.
b.	Material: Primed steel.
c.	Material: Glass.
62.	Cab Gate: 3-speed sliding gate.
a.	Material: Stainless steel.
b.	Material: Primed steel.
c.	Material: Glass.
63.	Landing Doors: Swing doors by others. EMI interlocks provided with elevator.
64.	Landing Doors: 2-speed sliding door.
a.	Material: Stainless steel.
b.	Material: Primed steel.
c.	Material:  Glass.
65.	Landing Doors: 3-speed sliding door.
a.	Material: Stainless steel.
b.	Material: Primed steel.
c.	Material: Glass.
66.	Landing Doors: Fire-rated 2-speed sliding doors.
a.	Material: Stainless steel.
b.	Material: Primed steel.
2.7	COMMERCIAL ELEVATOR - LULA - LIMITED-USE, LIMITED-ACCESS ELEVATORS
A.	Installation by manufacturer authorized installer.
B.	Compliance with ASME A17.1 Section 5.2; LULA Elevators.
C.	Specifications:
1.	Number of Levels: 1 stop.
2.	Number of Levels: 2 stops.
3.	Number of Levels: 3 stops.
4.	Number of Levels: 4 stops.
5.	Vertical Travel (ft/mm): ______. 
6.	Vertical Travel: As determined by the Architect. 
7.	Vertical Travel: As detailed on the Drawings.
8.	Pit Depth: 14 inch (356 mm) minimum.
9.	Overhead: 108 inches (2743 mm).
10.	Overhead: 134 inch (3404 mm).
11.	Overhead: ______.
12.	Overhead: As determined by the Architect.
13.	Travel Speed: 30 ft per min (152 mm per sec).
14.	Drive System:
a.	Roped Hydraulic; hole-less.
b.	Submersible pump unit.
15.	Safety Features:
a.	Overspeed valve.
b.	Safety brake system.
c.	Emergency alarm and stop switch.
d.	Final limit switches.
e.	Gate switch.
f.	Landing door interlocks.
16.	Elevator Power Requirements: 208 V, 3 Phase, 30 A service to fused, lockable disconnect with auxiliary contact.
17.	Elevator Power Requirements: 240 V, 1 Phase, 40 A service to fused, lockable disconnect with auxiliary contact.
18.	Lighting Power Requirements: 120 V, 20 A service to a fused, lockable disconnect (for lighting circuit).
19.	Communication Requirements: Dedicated phone line. 
20.	Controls:
a.	Fully automatic push button in cab and at landings.
b.	Automatic car lighting.
c.	Position indicator in cab.
d.	Microprocessor based controller.
21.	Capacity: 1400 lbs. (635 kg).
22.	Cab Size (WxD): 48 x 54 inches (1219 x 1372 mm).
23.	Cab Size (WxD): 42 x 60 inches (1067 x 1524 mm).
24.	Cab Configuration: Enter/exit same side.
25.	Cab Configuration: Enter/exit opposite sides; front and rear. 
26.	Cab Fixtures Finish: Stainless Steel.
27.	Cab Fixtures Finish: Oil Rubbed Bronze.
28.	Cab Fixtures Finish: Brass.
29.	Cab Gates: Sliding 2-speed gate.
30.	Cab Gate Finish: Primed for paint.
31.	Cab Gate Finish: Powder Coated Black.
32.	Cab Gate Finish: Powder Coated White.
33.	Cab Gate Finish: Stainless Steel.
34.	Landing Doors: Sliding 2-speed doors.
35.	Landing Door Finish: Primed for paint.
36.	Landing Door Finish: Stainless Steel.
37.	Cab Wall Finish: Powder Coat White.
38.	Cab Wall Finish: Powder Coat Black.
39.	Cab Wall Finish: Stainless Steel.
40.	Cab Wall Finish: Powder Coat White with Raised Laminate Panels; Oak.
41.	Cab Wall Finish: Powder Coat White with Raised Laminate Panels; Stone.
42.	Cab Wall Finish: Powder Coat White with Raised Laminate Panels; Mahogany.
43.	Cab Wall Finish: Powder Coat White with Raised Laminate Panels; Fog.
44.	Cab Wall Finish: Powder Coat Black with Raised Laminate Panels; Oak.
45.	Cab Wall Finish: Powder Coat Black with Raised Laminate Panels; Stone.
46.	Cab Walls Finish: Powder Coat Black with Raised Laminate Panels; Mahogany.
47.	Cab Wall Finish: Powder Coat Black with Raised Laminate Panels; Fog.
48.	Cab Wall Finish: Stainless Steel with Raised Laminate Panels; Walnut.
49.	Cab Wall Finish: Stainless Steel with Raised Laminate Panels; Gray.
50.	Cab Ceiling: Powder Coat White.
51.	Cab Ceiling: Powder Coat Black.
52.	Cab Ceiling: Stainless Steel.
2.8	WHEELCHAIR LIFT - ARTISAN WHEELCHAIR LIFT WITH GLASS ENCLOSURE
A.	Installation by manufacturer authorized installer.
B.	Compliance with ASME A18.1
C.	Specifications:
1.	Number of Levels: 1 stop.
2.	Number of Levels: 2 stops.
3.	Number of Levels: 3 stops.
4.	Vertical Travel (inch/mm): ______.
5.	Vertical Travel: As determined by the Architect.
6.	Vertical Travel: As detailed on the Drawings.
7.	Pit Depth: 0 inches; minimum.
8.	Pit Depth: 3 inches (76 mm).
9.	Pit Depth (inch/mm): ______.
10.	Overhead: ______.
11.	Overhead: As determined by the Architect.
12.	Overhead: As detailed on the Drawings.
13.	Enclosure Shape: Rectangular.
14.	Enclosure Shape: Square.
15.	Enclosure Shape: ________.
16.	Cab Height: 78 inches (1981 mm).
a.	Requires overhead of 96 inches (2438 mm) or greater.
17.	Cab Height: 84 inches (2164 mm).
a.	Requires overhead of 102 inches (2591 mm) or greater.
18.	Cab Height: 96 inches (2438 mm).
a.	Requires overhead of 114 inches (2896 mm) or greater.
19.	Cab Size (WxD): 36 x 48 inches (914 x 1219 mm). 
a.	Enclosure Footprint (WxD): 44 x 58 inches (1118 x 1473 mm).
20.	Cab Size (WxD): 36 x 54 inches (914 x 1372 mm).
a.	Enclosure Footprint (WxD): 44 x 64 inches (1118 x 1626 mm).
21.	Cab Size (WxD): 36 x 60 inches (914 x 1524 mm).
a.	Enclosure Footprint (WxD): 44 x 70 inches (1118 x 1778 mm).
22.	Cab Size (WxD): 40 x 48 inches (1016 x 1219 mm).
a.	Enclosure Footprint (WxD): 48 x 58 inches (1219 x 1473 mm).
23.	Cab Size (WxD): 40 x 54 inches (1016 x 1372 mm).
a.	Enclosure Footprint (WxD): 48 x 64 inches (914 x 1626 mm).
24.	Cab Size (WxD): 44 x 48 inches (1118 x 1219 mm).
a.	Enclosure Footprint (WxD): 52 x 58 inches (1321 x 1473 mm).
25.	Cab Size (WxD): 40 x 60 inches (1016 x 1524 mm).
a.	Enclosure Footprint (WxD): 48 x 70 inch (1219 x 1778 mm).
26.	Cab Size (WxD): 44 x 54 inch (1118 x 1372 mm).
a.	Approx. Enclosure Footprint (WxD): 52 x 64 (1321 x 1626 mm).
b.	Capacity: 1400 lbs (635 kg).
27.	Cab Size (WxD): 48 x 48 inch (1219 x 1219 mm)
a.	Approx. Enclosure Footprint (WxD): 56 x 58 inch (1422 x 1473 mm)
b.	Capacity: 1400 lbs (635 kg).
28.	Cab Size (WxD): ____ x ____ inch (____ x ____ mm).
a.	Enclosure Footprint (WxD): ____ x ____ inch (____ x ____ mm).
29.	Cab Configuration: Enter/exit same side.
30.	Cab Configuration: Enter/exit opposite sides
31.	Load Capacity: 750 lbs (340 kg).
32.	Load Capacity:  1400 lbs (635 kg). 
33.	Rated Speed: 30 fpm (152 mm per sec).
34.	Power Supply: 230 V, 1 PH, 60 Hz, 30 A.
35.	Lighting Supply: 115 V, 60 Hz, 15 A.
36.	Communication: Functional phone line.
37.	Drive System: Winding drum with variable frequency drive.
38.	Machine Room: Not Required 
39.	Controller (WxHxD): 24 x 24 x 8 inch (610 x 610 x 203 mm). Must be hung on wall near elevator.
40.	Control System: PLC with error log and troubleshooting indicators.
41.	Operation: Continuous pressure.
42.	Temperature Range: 14 to 104 degrees F (Minus 10 to 40 degrees C).
43.	Cab Lighting: Automatic LED.
44.	Cab Phone: Hands-free, recessed in wall.
45.	Landing Doors: Manual swing.
46.	Landing Doors: Automatic swing.
47.	Safety Features:
a.	Cab emergency stop switch.
b.	Cab gate switch.
c.	Pit stop switch 
d.	Car top stop switch.
e.	Battery backup lowering. 
f.	Battery backup lighting.
g.	Upper and lower final limit switches. 
h.	Safety brakes.
i.	Slack cable switch. 
j.	Auxiliary safety circuit for service.
48.	Cab Panels: Clear Acrylic.
49.	Cab Panels: Laminated Glass.
50.	Enclosure Panels: Clear Acrylic.
51.	Enclosure Panels: Laminated Glass.
52.	Frame Powder Coat Color: Fine Texture Black.
53.	Frame Powder Coat Color: Fine Texture White.
54.	Frame Powder Coat Color: Gun Metal.
55.	Frame Powder Coat Color: Bronze.
56.	Frame Powder Coat Color: Copper Vein.
57.	Frame Powder Coat Color: Blue-Grey.
58.	Frame Powder Coat Color: Anthracite Metallic.
59.	Frame Powder Coat Color: Greco.
60.	Frame Powder Coat Color: Taupe.
61.	Frame Powder Coat Color: Hartford Green.
62.	Frame Powder Coat Color: Deore (Gold).
63.	Frame Powder Coat Color: _____________.
64.	Frame Powder Coat Color: As determined by Architect.
2.9	RESIDENTIAL DUMBWAITER - JEEVES ECONOLIFT
A.	Installation by manufacturer authorized installer.
B.	Compliance with ASME A17.1 Section 7.2; Electric Dumbwaiters.
C.	Specifications:
1.	Number of Levels: 1 stop.
2.	Number of Levels: 2 stops.
3.	Number of Levels: 3 stops.
4.	Vertical Travel (inch/mm): ______.
5.	Vertical Travel: As determined by the Architect. 
6.	Vertical Travel: As detailed on the Drawings.
7.	Travel Speed: 30 ft per min (152 mm per sec).
8.	Door Configuration: Same side.
9.	Doors Configuration: Front and back.
10.	Car Size (WxDxH): 20 x 20 x 30 inches (508 x 208 x 762 mm).
a.	Capacity: 100 lbs (45.4 kg).
11.	Car Size (WxDxH): 24 x 24 x 30 inches (610 x 610 x 762 mm).
a.	Capacity: 150 lbs (68 kg).
12.	Power: 115 V, 15 A circuit in a lockable fused disconnect.
13.	Drive System: Winding drum.
14.	Car Construction: Birch plywood with roll-up gate.
15.	Landing Doors: Primed steel.
16.	Landing Doors: Stainless steel.
17.	Landing Doors: Wood.
18.	Landing Controls: Wall mounted push button station.
19.	Machine Location: Bottom of hoistway.
20.	Machine Location: Top of hoistway.
21.	Safety Features:
a.	Safety brake system.
b.	Final limit switches.
c.	Gate switch.
d.	Landing door interlocks.
2.10	COMMERCIAL DUMBWAITER - JEEVES PRO DUMBWAITER
A.	Installation by manufacturer authorized installer.
B.	Compliance with ASME A17.1 Section 7.2; Electric Dumbwaiters.
C.	Specifications:
1.	Number of Levels: 1 stop.
2.	Number of Levels: 2 stops.
3.	Number of Levels: 3 stops.
4.	Number of Levels: 4 stops.
5.	Number of Levels: 5 stops.
6.	Number of Levels: 6 stops.
7.	Vertical Travel (ft/mm) ______. 
8.	Vertical Travel: As determined by the Architect. 
9.	Vertical Travel: As detailed on the Drawings.
10.	Travel Speed: 30 ft per min (152 mm per sec).
11.	Door Configuration: Same side.
12.	Doors Configuration: Front and back.
13.	Loading Height: Counter loading.
14.	Loading Height: Floor loading.
15.	Car Size (WxDxH): 24 x 24 x 24 inches (610 x 610 x 610 mm).
a.	Capacity: 125 lbs (56.7 kg).
b.	Power:  115 V, 20 A to a lockable fused disconnect. 
16.	Car Size (WxDxH): 28 x 28 x 28 inches (711 x 711 x 711 mm).
a.	Capacity: 250 lbs (113.4 kg).
b.	Power:  115 V, 20 A to a lockable fused disconnect. 
17.	Car Size (WxDxH): 20 x 30 x 36 inches (508 x 762 x 914 mm).
a.	Capacity: 250 lbs (113.4 kg).
b.	Power:  115 V, 20 A to a lockable fused disconnect.
18.	Car Size (WxDxH): 36 x 36 x 48 inches (914 x 914 x 1219 mm).
a.	Capacity: 500 lbs (226.8 kg).
b.	Power: 230 V, 20 A to a lockable fused disconnect.
19.	Drive System: Winding drum.
20.	Car Construction: Powder coated steel.
21.	Car Construction: Stainless steel.
22.	Car Gate: Bi-parting.
23.	Car Gate: Slide-up.
24.	Landing Doors: Bi-parting, Primed steel.
25.	Landing Doors: Bi-parting, Stainless steel.
26.	Landing Doors: Swing, Primed steel.
27.	Landing Doors: Swing, Stainless steel.
28.	Landing Doors: Roll-up, Primed steel.
29.	Landing Doors: Roll-up, Stainless steel.
30.	Landing Controls: Wall mounted push button station.
31.	Machine Location: Bottom of hoistway. 
32.	Machine Location: Top of hoistway.
33.	Safety Features:
a.	Safety brake system.
b.	Final limit switches.
c.	Gate switch.
d.	Landing door interlocks.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until site has been properly prepared.
B.	Hoistway shall be constructed in accordance with applicable safety code and must comply with State and Local codes.
C.	Hoistway shall be plumb and square within tolerance of manufacturer's requirements.
D.	Hoistway shall provide attachment and support of equipment inside hoistway.
E.	If site preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions. 
B.	Hoistway doors shall comply with local fire and building code for fire rated openings. 
3.4	FIELD QUALITY CONTROL
A.	Perform tests of elevator as required by governing codes.
3.5	ADJUSTING
A.	Adjust elevators for proper operation in accordance with manufacturer/installer's instructions.
B.	Adjust elevators for smooth acceleration and deceleration of car so not to cause passenger discomfort.
C.	Adjust doors to prevent opening of doors at landing on corridor side, unless car is at rest at that landing, or is in leveling zone and stopping at that landing.
D.	Adjust automatic floor leveling feature at each floor to within 1/4 inch (6 mm) of landing.
E.	Repair minor damages to finish in accordance with manufacturer/installer's instructions and as approved by Architect.
F.	Remove and replace damaged components that cannot be successfully repaired as determined by Architect.
3.6	CLEANING AND PROTECTION
A.	Clean in accordance with manufacturer's recommendations. Clean elevators promptly after installation in accordance with manufacturer/installer's instructions. Do not use cleaning materials or methods that could damage finish.
B.	Protect installed elevators from damage during construction in accordance with the negotiated temporary use agreement between Owner and manufacturer's installer. Protect installed products until completion of project.
C.	Touch-up, repair or replace damaged products and finishes in accordance with manufacturer's instructions before Substantial Completion.

END OF SECTION