SECTION 08 32 16

VINYL PATIO DOORS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2018 -  2023 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Vinyl Patio Doors of the following types:
1.	Brighton Series.
2.	Hampton Series.
3.	Windsor Series.
4.	Victorian Series.
5.	Kent Series.
6.	Newcastle Series.
7.	Essex Series.
B.	Vinyl-Clad Patio Doors of the following types:
1.	Buckingham 1000 Series.
2.	Buckingham ECO Series.
1.2	RELATED SECTIONS
A.	Section 06 10 00 - Rough Carpentry.
B.	Section 08 32 13 - Sliding Aluminum-Framed Glass Doors.
C.	Section 08 35 13.13 - Accordion Folding Doors.
1.3	REFERENCES
A.	AAMA/WDMA/CSA 101/I.S.2/A440 - NAFS - North American Fenestration Standard/Specification for windows, doors and skylights.
B.	Standards Council of Canada:
1.	CAN/CGSB-82.1-M89 - Sliding Doors.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data:
1.	Manufacturer's data sheets on each product to be used.
2.	Preparation instructions and recommendations.
3.	Storage and handling requirements and recommendations.
4.	Typical installation methods.
C.	Selection Samples: For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.
D.	Verification Samples: For each finish product specified, two samples, minimum size 6 inches (150 mm) square representing actual product, color, and patterns.
E.	Shop Drawings: Include elevations of each opening and details of materials, construction and finish. Include relationship with adjacent construction. 
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
D.	Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
1.	Intent of mock-up is to demonstrate quality of workmanship and visual appearance.
2.	If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
3.	Retain mock-up during construction as a standard for comparison with completed work. 
4.	Do not alter or remove mock-up until work is completed or removal is authorized.
1.6	PRE-INSTALLATION CONFERENCE
A.	Convene a conference approximately two weeks before scheduled commencement of the Work. Attendees shall include Architect, Contractor and trades involved. Agenda shall include schedule, responsibilities, critical path items and approvals.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Store and handle in strict compliance with manufacturer's written instructions and recommendations.
B.	Protect from damage due to weather, excessive temperature, and construction operations.
1.8	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.9	SEQUENCING
A.	Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
1.10	WARRANTY
A.	Manufacturer's Warranty: Provide manufacturer's standard limited warranty.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Novatech Group, which is located at:<BR />160 Murano, https://www.groupenovatechgroup.com<BR />Sainte-Julie, QC, Canada J3E 0C6<BR />Tel: 450-922-6106<BR />Fax: 450-922-9633<BR />Email: request info (marketing@groupenovatech.com);Web: https://www.novatechgroup.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	VINYL PATIO DOORS
A.	Basis of Design: Brighton Knock Down Patio Door; as manufactured by Sunview Patio Doors Ltd.
1.	Performance and Design Requirements
a.	AAMA/WDMA/CSA 101/1.S.2/A440: Meets NAFS/Class R-PG30.
2.	Frame: 4-7/8 inch (124 mm) vinyl frame.
3.	Sash reinforced with steel to withstand higher wind loads.
4.	Double perimeter seal.
5.	Configuration: 
a.	Door/Panel: OX-Slide Left.
b.	Door/Panel: XO-Slide Right.
c.	Door/Panel: OXO-Slide Right to Left.
d.	Door/Panel: OZO-Slide Left to Right.
e.	Door/Panel: OOX-Slide Left.
f.	Door/Panel: XOO-Slide Right.
g.	Door/Panel: OXXO-Slide Right and Slide Left from Centre.
h.	Transom: As indicated on Drawings.
i.	Transom: _____.
j.	Sidelight: As indicated on Drawings.
k.	Sidelight: _____.
6.	Insulating Glass: One-inch (25 mm), argon-filled, Low-E coated, tempered, sealed, insulating glass.
7.	Decorative Internal Grills: Flat, two-tone.
8.	Decorative Internal Grills: Flat, white.
9.	Decorative Internal Grills: Georgian, two-tone.
10.	Decorative Internal Grills: Georgian, white.
11.	Decorative Internal Grills: Pencil, white.
12.	Decorative Internal Grills: Pencil, brass.
13.	Decorative Internal Grills: Pencil, pewter.
14.	Decorative Internal Grills: Square, white.
15.	Decorative Internal Grills: Square, brass.
16.	Decorative Internal Grills: Square, pewter.
17.	Weather Stripping: Full perimeter double fin-seal weather stripping.
18.	Hardware:
a.	Elite handle, white finish.
b.	Elite handle, black finish.
c.	Euro handle, white finish.
d.	Euro handle, black finish.
e.	Euro handle, brass finish.
f.	Euro handle, black nickel finish.
g.	Euro handle, satin nickel finish.
h.	Euro handle, bright chrome finish.
i.	Two position kick locks.
j.	Multi-point locks.
k.	Rollers: Adjustable tandem nylon ball bearing rollers.
19.	Finish: To be selected by Architect.
20.	Finish: As indicated on Drawings.
21.	Finish: _____.
B.	Basis of Design: Hampton Patio Door Series; as manufactured by Sunview Patio Doors Ltd.
1.	Performance and Design Requirements
a.	AAMA/WDMA/CSA 101/1.S.2/A440: Meets NAFS/Class R-PG35.
b.	Compliant with CAN/CGSB-82.1-M89.
2.	Frame: 4-7/8 inch (124 mm) vinyl frame.
3.	Sash reinforced with steel to withstand higher wind loads.
4.	Double perimeter seal.
5.	Configuration: 
a.	Door/Panel: OX-Slide Left.
b.	Door/Panel: XO-Slide Right.
c.	Door/Panel: OXO-Slide Right to Left.
d.	Door/Panel: OZO-Slide Left to Right.
e.	Door/Panel: OOX-Slide Left.
f.	Door/Panel: XOO-Slide Right.
g.	Door/Panel: OXXO-Slide Right and Slide Left from Centre.
h.	Transom: As indicated on Drawings.
i.	Transom: _____.
j.	Sidelight: As indicated on Drawings.
k.	Sidelight: _____.
6.	Insulating Glass: One-inch (25 mm), Low-E coated, tempered, sealed, insulating glass.
7.	Decorative Internal Grills: Flat, white.
8.	Decorative Internal Grills: Georgian, white.
9.	Decorative Internal Grills: Georgian, brass.
10.	Decorative Internal Grills: Georgian, pewter.
11.	Decorative Internal Grills: Pencil, white.
12.	Decorative Internal Grills: Pencil, brass.
13.	Decorative Internal Grills: Pencil, pewter.
14.	Weather Stripping: Full perimeter double fin-seal weather stripping.
15.	Hardware:
a.	Standard handle, white finish.
b.	Standard handle, black finish.
c.	Upgrade handle, brass finish.
d.	Upgrade handle, nickel finish.
e.	Upgrade handle, satin chrome finish.
f.	Upgrade handle, bright chrome finish.
g.	Two position kick locks.
h.	Multi-point locks.
i.	Rollers: Adjustable tandem nylon ball bearing rollers.
16.	Finish: To be selected by Architect.
17.	Finish: As indicated on Drawings.
18.	Finish: _____.
C.	Basis of Design: Windsor Patio Door Series; as manufactured by Sunview Patio Doors Ltd.
1.	Performance and Design Requirements
a.	AAMA/WDMA/CSA 101/1.S.2/A440: Meets NAFS/Class R-PG40.
b.	AAMA/WDMA/CSA 101/1.S.2/A440: Meets NAFS/Class R-PG50.
2.	Frame: 4-7/8 inch (124 mm) vinyl frame.
3.	Sash reinforced with steel to withstand higher wind loads.
4.	Double perimeter seal.
5.	Configuration: 
a.	Door/Panel: OX-Slide Left.
b.	Door/Panel: XO-Slide Right.
c.	Door/Panel: OXO-Slide Right to Left.
d.	Door/Panel: OZO-Slide Left to Right.
e.	Door/Panel: OOX-Slide Left.
f.	Door/Panel: XOO-Slide Right.
g.	Door/Panel: OXXO-Slide Right and Slide Left from Centre.
h.	Transom: As indicated on Drawings.
i.	Transom: _____.
j.	Sidelight: As indicated on Drawings.
k.	Sidelight: _____.
6.	Insulating Glass: One-inch (25 mm), Low-E coated, tempered, sealed, insulating glass.
7.	Decorative Internal Grills: Flat, white.
8.	Decorative Internal Grills: Georgian, white.
9.	Decorative Internal Grills: Georgian, brass.
10.	Decorative Internal Grills: Georgian, pewter.
11.	Decorative Internal Grills: Pencil, white.
12.	Decorative Internal Grills: Pencil, brass.
13.	Decorative Internal Grills: Pencil, pewter.
14.	Weather Stripping: Full perimeter double fin-seal weather stripping.
15.	Hardware:
a.	Standard handle, white finish.
b.	Standard handle, black finish.
c.	Upgrade handle, brass finish.
d.	Upgrade handle, nickel finish.
e.	Upgrade handle, satin chrome finish.
f.	Upgrade handle, bright chrome finish.
g.	Two position kick locks.
h.	Multi-point locks.
i.	Rollers: Adjustable tandem nylon ball bearing rollers.
16.	Finish: To be selected by Architect.
17.	Finish: As indicated on Drawings.
18.	Finish: _____.
D.	Basis of Design: Victorian Patio Door Series; as manufactured by Sunview Patio Doors Ltd.
1.	Performance and Design Requirements
a.	AAMA/WDMA/CSA 101/1.S.2/A440: Meets NAFS/Class LC-PG55.
2.	Frame: 
a.	Depth: 5-7/8 inch (149 mm).
b.	Three weather seals.
c.	Anodized screen track and stainless steel roller track.
d.	Sill slopes 8 degrees for optimal drainage.
3.	Sash:
a.	Reinforced with steel to withstand high wind loads.
b.	Double perimeter seal for superior air-tightness.
c.	Adjustable nylon tandem ball-bearing rollers.
4.	Configuration: 
a.	Door/Panel: OX-Slide Left.
b.	Door/Panel: XO-Slide Right.
c.	Door/Panel: OXO-Slide Right to Left.
d.	Door/Panel: OZO-Slide Left to Right.
e.	Door/Panel: OOX-Slide Left.
f.	Door/Panel: XOO-Slide Right.
g.	Door/Panel: OXXO-Slide Right and Slide Left from Centre.
h.	Transom: As indicated on Drawings.
i.	Transom: _____.
j.	Sidelight: As indicated on Drawings.
k.	Sidelight: _____.
5.	Insulating Glass: One-inch (25 mm), Low-E coated, tempered, sealed, insulating glass.
6.	Hardware:
a.	Elite handle, white finish.
b.	Elite handle, black finish.
c.	Elite handle, ivory finish.
d.	Elite handle, sandalwood finish.
e.	Two position kick locks.
f.	Guardian locks.
g.	Folding security bars.
7.	Accessories and Options:
a.	Frame Extension: 1-1/4 inch (32 mm).
b.	Frame Extension: 2 inch (51 mm).
c.	Frame Extension: 3-3/8 inch (86 mm).
d.	Brick mold.
e.	Sill extensions.
f.	Internal mini-blinds.
g.	V-Groove Glass: Colonial.
h.	V-Groove Glass: Prairie.
i.	Decorative Internal Grills: Flat, two-tone.
j.	Decorative Internal Grills: Flat, white.
k.	Decorative Internal Grills: Flat, brass.
l.	Decorative Internal Grills: Flat, pewter.
m.	Decorative Internal Grills: Georgian, white.
n.	Decorative Internal Grills: Pencil, white.
o.	Decorative Internal Grills: Pencil, brass.
p.	Decorative Internal Grills: Pencil, pewter.
8.	Finish: To be selected by Architect.
9.	Finish: As indicated on Drawings.
10.	Finish: _____.
E.	Basis of Design: Kent Patio Door Series; as manufactured by Sunview Patio Doors Ltd.
1.	Performance and Design Requirements
a.	AAMA/WDMA/CSA 101/1.S.2/A440: Meets NAFS/Class LC-PG55.
2.	Frame: 
a.	Victorian all-vinyl frame.
b.	Buckingham wood frame with vinyl cladding.
c.	Buckingham eco frame with vinyl cladding.
d.	Depth: 5-7/8 inch (149 mm).
e.	Three weather seals.
f.	Anodized screen track and stainless steel roller track.
g.	Sill slopes 8 degrees for optimal drainage.
3.	Sash:
a.	Reinforced with steel to withstand high wind loads.
b.	Double perimeter seal for superior air-tightness.
c.	Adjustable nylon tandem ball-bearing rollers.
4.	Configuration: 
a.	Door/Panel: OX-Slide Left.
b.	Door/Panel: XO-Slide Right.
c.	Door/Panel: OXO-Slide Right to Left.
d.	Door/Panel: OZO-Slide Left to Right.
e.	Door/Panel: OOX-Slide Left.
f.	Door/Panel: XOO-Slide Right.
g.	Door/Panel: OXXO-Slide Right and Slide Left from Centre.
h.	Transom: As indicated on Drawings.
i.	Transom: _____.
j.	Sidelight: As indicated on Drawings.
k.	Sidelight: _____.
5.	Insulating Glass: One-inch (25 mm), Low-E coated, tempered, sealed, insulating glass.
6.	Insulating Glass: 1-3/8 inch (35 mm), Low-E coated, argon filled, tempered, sealed, triple glazed, insulating glass.
7.	Hardware:
a.	Elite handle, white finish.
b.	Elite handle, black finish.
c.	Elite handle, sandalwood finish.
d.	Euro handle, white finish.
e.	Euro handle, black finish.
f.	Euro handle, brass finish.
g.	Euro handle, black nickel finish.
h.	Euro handle, satin nickel finish.
i.	Euro handle, bright chrome finish.
j.	Multi-point keylock.
k.	Two position kick locks.
l.	Guardian locks.
m.	Folding security bars.
8.	Accessories and Options:
a.	Frame Extension: 1-1/4 inch (32 mm).
b.	Frame Extension: 2 inch (51 mm).
c.	Frame Extension: 3-3/8 inch (86 mm).
d.	Brick Mold: 1-1/4 inch (32 mm).
e.	Brick Mold: 1-7/8 inch (48 mm).
f.	Drywall Return: 3/4 inch (19 mm).
g.	Sill Extension: 1-1/4 inch (32 mm).
h.	Sill Plate: 4-1/2 inch (114 mm).
i.	Decorative Internal Grills: Flat, two-tone.
j.	Decorative Internal Grills: Flat, white.
k.	Decorative Internal Grills: Flat, brass.
l.	Decorative Internal Grills: Flat, pewter.
m.	Decorative Internal Grills: Georgian, white.
n.	Decorative Internal Grills: Pencil, white.
o.	Decorative Internal Grills: Pencil, brass.
p.	Decorative Internal Grills: Pencil, pewter.
9.	Finish: To be selected by Architect.
10.	Finish: As indicated on Drawings.
11.	Finish: _____.
F.	Basis of Design: Newcastle Patio Door Series; as manufactured by Sunview Patio Doors Ltd.
1.	Performance and Design Requirements
a.	AAMA/WDMA/CSA 101/1.S.2/A440: Meets NAFS/Class R-PG50.
2.	Elegant heavy-duty screen.
3.	Pocket covers on interior, exterior jambs, and sill.
4.	Frame: 
a.	Depth: 4-7/8 inch (124 mm).
b.	Depth: 6-1/8 inch (156 mm).
c.	Depth: 6-7/8 inch (175 mm).
d.	Three weather seals.
e.	Anodized screen track and stainless steel roller track.
f.	Sill slopes 8 degrees for optimal drainage.
5.	Sash:
a.	Reinforced with steel to withstand high wind loads.
b.	Double perimeter seal for superior air-tightness.
c.	Adjustable nylon tandem ball-bearing rollers.
6.	Configuration: 
a.	Door/Panel: OX-Slide Left.
b.	Door/Panel: XO-Slide Right.
c.	Door/Panel: OXO-Slide Right to Left.
d.	Door/Panel: OZO-Slide Left to Right.
e.	Door/Panel: OOX-Slide Left.
f.	Door/Panel: XOO-Slide Right.
g.	Door/Panel: OXXO-Slide Right and Slide Left from Centre.
h.	Transom: As indicated on Drawings.
i.	Transom: _____.
j.	Sidelight: As indicated on Drawings.
k.	Sidelight: _____.
7.	Insulating Glass: One-inch (25 mm), Low-E coated, tempered, sealed, insulating glass.
8.	Hardware:
a.	Handle Finish: Satin nickel.
b.	Handle Finish: Polished brass
c.	Handle Finish: Oil bronze.
d.	Multi-point keylock.
e.	Two position kick locks.
f.	Guardian locks.
9.	Accessories and Options:
a.	Brick mold.
b.	Sill Plate: 4-1/2 inch (114 mm).
c.	Stainless steel hardware kit.
d.	Internal mini-blinds.
e.	Decorative Internal Grills: Flat, two-tone.
f.	Decorative Internal Grills: Flat, white.
g.	Decorative Internal Grills: Flat, brass.
h.	Decorative Internal Grills: Flat, pewter.
i.	Decorative Internal Grills: Georgian, white.
j.	Decorative Internal Grills: Pencil, white.
k.	Decorative Internal Grills: Pencil, brass.
l.	Decorative Internal Grills: Pencil, pewter.
m.	Decorative Glass: Venice, wrought iron.
n.	Decorative Glass: Spectrum, decorative bevels.
o.	Retractable screen.
10.	Finish: To be selected by Architect.
11.	Finish: As indicated on Drawings.
12.	Finish: _____.
G.	Basis of Design: Essex Swing Patio Door Series; as manufactured by Sunview Patio Doors Ltd.
1.	Performance and Design Requirements
a.	AAMA/WDMA/CSA 101/1.S.2/A440: Meets NAFS/Class R-PG35.
2.	Frame Depth: 4-7/8 inch (124 mm).
3.	Sash:
a.	Reinforced with steel to withstand high wind loads.
b.	Double perimeter seal for superior air-tightness.
c.	Adjustable nylon tandem ball-bearing rollers.
4.	Configuration: 
a.	Door/Panel: One panel, in-swing.
b.	Door/Panel: One panel, out-swing.
c.	Door/Panel: Two panel, in-swing.
d.	Door/Panel: Two panel, out-swing.
e.	Transom: As indicated on Drawings.
f.	Transom: _____.
g.	Sidelight: As indicated on Drawings.
h.	Sidelight: _____.
5.	Insulating Glass: One-inch (25 mm), Low-E coated, tempered, sealed, insulating glass.
6.	Hardware:
a.	Handle Finish: Brushed nickel.
b.	Handle Finish: Bright brass
c.	Handle Finish: Oil bronze.
d.	Sentry adjustable hinges.
e.	Multi-point keylock.
7.	Accessories and Options:
a.	Frame Extension: 1-1/4 inch (32 mm).
b.	Brick mold.
c.	Sill Plate: 4-1/2 inch (114 mm).
d.	Internal mini-blinds.
e.	Decorative Internal Grills: Flat, two-tone.
f.	Decorative Internal Grills: Flat, white.
g.	Decorative Internal Grills: Georgian, two-tone.
h.	Decorative Internal Grills: Georgian, white.
i.	Decorative Internal Grills: Pencil, white.
j.	Decorative Internal Grills: Pencil, brass.
k.	Decorative Internal Grills: Pencil, pewter.
l.	Decorative Internal Grills: Square, white.
m.	Decorative Internal Grills: Square, brass.
n.	Decorative Internal Grills: Square, pewter.
o.	Decorative Glass: Venice, wrought iron.
p.	Decorative Glass: Spectrum, decorative bevels.
q.	Retractable screen.
8.	Finish: To be selected by Architect.
9.	Finish: As indicated on Drawings.
10.	Finish: _____.
2.3	VINYL-CLAD PATIO DOORS
A.	Basis of Design: Buckingham Series 1000 Vinyl-Clad Patio Door; as manufactured by Sunview Patio Doors Ltd.
1.	Performance and Design Requirements
a.	AAMA/WDMA/CSA 101/1.S.2/A440: Meets NAFS/Class LC-PG55.
2.	Frame: 
a.	Depth: 5-7/8 inch (149 mm).
b.	Wood buck frame is economical, durable, and easy to install.
c.	Three weather seals.
d.	Anodized screen track and stainless steel roller track.
e.	Sill slopes 8 degrees for optimal drainage.
f.	All vinyl sill.
3.	Sash:
a.	Reinforced with steel to withstand high wind loads.
b.	Double perimeter seal for superior air-tightness.
c.	Adjustable nylon tandem ball-bearing rollers.
4.	Configuration: 
a.	Door/Panel: OX-Slide Left.
b.	Door/Panel: XO-Slide Right.
c.	Door/Panel: OXO-Slide Right to Left.
d.	Door/Panel: OZO-Slide Left to Right.
e.	Door/Panel: OOX-Slide Left.
f.	Door/Panel: XOO-Slide Right.
g.	Door/Panel: OXXO-Slide Right and Slide Left from Centre.
h.	Transom: As indicated on Drawings.
i.	Transom: _____.
j.	Sidelight: As indicated on Drawings.
k.	Sidelight: _____.
5.	Insulating Glass: One-inch (25 mm), Low-E coated, tempered, sealed, insulating glass.
6.	Hardware:
a.	Elite handle, white finish.
b.	Elite handle, black finish.
c.	Elite handle, ivory finish.
d.	Elite handle, sandalwood finish.
e.	Optional Handle:
1)	Single-point keylock.
2)	Heavy duty multi-point keylock.
3)	Finish: White.
4)	Finish: Black.
5)	Finish: Brass.
6)	Finish: Black Nickel.
7)	Finish: Satin Nickel.
8)	Finish: Bright Chrome.
f.	Two position kick locks.
g.	Guardian locks.
h.	Folding security bars.
7.	Accessories and Options:
a.	Frame Extension: 1-1/4 inch (32 mm).
b.	Frame Extension: 2 inch (51 mm).
c.	Frame Extension: 3-3/8 inch (86 mm).
d.	Sill Plate: 4-1/2 inch (114 mm).
e.	Brick mold.
f.	Sill extensions.
g.	Internal mini-blinds.
h.	V-Groove Glass: Colonial.
i.	V-Groove Glass: Prairie.
j.	Decorative Internal Grills: Flat, two-tone.
k.	Decorative Internal Grills: Flat, white.
l.	Decorative Internal Grills: Flat, brass.
m.	Decorative Internal Grills: Flat, pewter.
n.	Decorative Internal Grills: Georgian, white.
o.	Decorative Internal Grills: Pencil, white.
p.	Decorative Internal Grills: Pencil, brass.
q.	Decorative Internal Grills: Pencil, pewter.
8.	Exterior Finish: To be selected by Architect.
9.	Exterior Finish: As indicated on Drawings.
10.	Exterior Finish: _____.
11.	Interior Finish: Same as exterior.
12.	Interior Finish: Natural oak woodgrain look.
13.	Interior Finish: Cherry woodgrain look.
B.	Basis of Design: Buckingham Eco - Series 1000 Patio Door; as manufactured by Sunview Patio Doors Ltd.
1.	Performance and Design Requirements
a.	AAMA/WDMA/CSA 101/1.S.2/A440: Meets NAFS/Class LC-PG55.
2.	Frame: 
a.	Depth: 5-7/8 inch (149 mm).
b.	Core: Rice hull combined with polyolefin.
c.	Three weather seals.
d.	Anodized screen track and stainless steel roller track.
e.	Sill slopes 8 degrees for optimal drainage.
f.	Enhanced fire resistance.
g.	Improved strength.
h.	Improved thermal resistance.
3.	Sash:
a.	Reinforced with steel to withstand high wind loads.
b.	Double perimeter seal for superior air-tightness.
c.	Adjustable nylon tandem ball-bearing rollers.
4.	Configuration: 
a.	Door/Panel: OX-Slide Left.
b.	Door/Panel: XO-Slide Right.
c.	Door/Panel: OXO-Slide Right to Left.
d.	Door/Panel: OZO-Slide Left to Right.
e.	Door/Panel: OOX-Slide Left.
f.	Door/Panel: XOO-Slide Right.
g.	Door/Panel: OXXO-Slide Right and Slide Left from Centre.
h.	Transom: As indicated on Drawings.
i.	Transom: _____.
j.	Sidelight: As indicated on Drawings.
k.	Sidelight: _____.
5.	Insulating Glass: One-inch (25 mm), Low-E coated, tempered, sealed, insulating glass.
6.	Hardware:
a.	Elite handle, white finish.
b.	Elite handle, black finish.
c.	Elite handle, ivory finish.
d.	Elite handle, sandalwood finish.
e.	Euro Style Handle:
1)	Single-point keylock.
2)	Heavy duty multi-point keylock.
3)	Finish: White.
4)	Finish: Black.
5)	Finish: Brass.
6)	Finish: Black Nickel.
7)	Finish: Satin Nickel.
8)	Finish: Bright Chrome.
f.	Two position kick locks.
g.	Guardian locks.
h.	Folding security bars.
7.	Accessories and Options:
a.	Frame Extension: 1-1/4 inch (32 mm).
b.	Frame Extension: 2 inch (51 mm).
c.	Frame Extension: 3-3/8 inch (86 mm).
d.	Sill Plate: 4-1/2 inch (114 mm).
e.	Brick mold.
f.	Sill extensions.
g.	Stainless steel hardware kit.
h.	Internal mini-blinds.
i.	V-Groove Glass: Colonial.
j.	V-Groove Glass: Prairie.
k.	Decorative Internal Grills: Flat, two-tone.
l.	Decorative Internal Grills: Flat, white.
m.	Decorative Internal Grills: Flat, brass.
n.	Decorative Internal Grills: Flat, pewter.
o.	Decorative Internal Grills: Georgian, white.
p.	Decorative Internal Grills: Pencil, white.
q.	Decorative Internal Grills: Pencil, brass.
r.	Decorative Internal Grills: Pencil, pewter.
8.	Exterior Finish: To be selected by Architect.
9.	Exterior Finish: As indicated on Drawings.
10.	Exterior Finish: _____.
11.	Interior Finish: Same as exterior.
12.	Interior Finish: Natural oak woodgrain look.
13.	Interior Finish: Cherry woodgrain look.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly constructed and prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect in writing of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, approved submittals and in proper relationship with adjacent construction.
3.4	CLEANING AND PROTECTION
A.	Clean products in accordance with the manufacturers recommendations. 
B.	Protect installed products until completion of project.
C.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION