SECTION 08 11 66

RETRACTABLE SCREENS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2016 -  2025 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Retractable door screens; manually operated, side-coiling, insect screens.
B.	Retractable window screens; manually operated, roll-up, insect and shade screens.
C.	Retractable vertically acting screens for large openings.
D.	Retractable horizontally acting screens for large openings.
1.2	RELATED SECTIONS
A.	Section 08 11 13.13 - Standard Hollow Metal Doors and Frames.
B.	Section 08 11 73 - Sliding Metal Fire Doors.
C.	Section 08 43 29 - Sliding Storefronts.
D.	Section 08 52 13 - Metal-Clad Wood Windows.
E.	Section  - .
F.	Section 08 52 13.10 - Aluminum-Clad Wood Windows*.
G.	Section 08 53 13 - Vinyl Windows.
H.	Section 08 44 16 - Glazed Bronze Curtain Walls.
1.3	REFERENCES
A.	American Architectural Manufacturers Association (AAMA):
1.	AAMA 2604 - Voluntary Specification, Performance Requirements and Test Procedures for Pigmented Organic Coatings on Aluminum Extrusions and Panels.
B.	ASTM International (ASTM):
1.	ASTM B 221 - Standard Specification for Aluminum and Aluminum-Alloy Extruded Bars, Rods, Wire, Profiles, and Tubes.
2.	ASTM B 429 - Standard Specification for Aluminum-Alloy Extruded Structural Pipe and Tube.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Verification Samples: For each finish product specified, two samples, representing actual product, color, and patterns.
D.	Sustainable Design Certifications: Submit manufacturer's documentation of sustainable design certification for product proposed for use.
E.	Installer Qualification: Submit documentation that installer is authorized by the manufacturer.
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Minimum 5 year experience manufacturing similar products.
B.	Installer Qualifications: Must be a manufacturer authorized installer.
C.	Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
1.	Finish areas designated by Architect.
2.	Install one complete, operable unit including accessories, then test operation and make adjustments required for proper operation.
3.	Do not proceed with remaining work until workmanship is approved by Architect.
4.	Rebuild mock-up area as required to produce acceptable work.
1.6	PRE-INSTALLATION MEETINGS
A.	Convene minimum two weeks prior to starting work of this section.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Deliver and store products in manufacturer's unopened packaging bearing the brand name and manufacturer's identification until ready for installation.
B.	Store packaged units in a horizontal position, evenly supported, and without top loading.
C.	Handling: Handle materials to avoid damage.
1.8	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.9	SEQUENCING
A.	Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
B.	Coordinate with Phantom Representative regarding installation schedule for recessed components.
1.10	WARRANTY
A.	Provide manufacturer's limited lifetime material warranty on aluminum components, plastics and coatings.
1.	2 Year Warranty on labor from the date of original installation.
2.	7 Year Warranty on Electric Motors and Manually Operated Gears.
3.	7 Year Warranty on Electronic Components.
4.	Registration: All products must be registered with Phantom Screens warranty registration system on www.phantomscreens.com by Owner or Authorized Phantom Distributor.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Phantom Screens, which is located at:<BR />30451 Simpson Rd.<BR />Abbotsford, BC, Canada V2T 6C7<BR />Tel: 604-855-3654<BR />Fax: 604-855-7834<BR />Email: request info (phantom@phantomscreens.com);Web: https://www.phantomscreens.com/ 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	RETRACTABLE SCREENS FOR DOORS
A.	Model: Phantom Door Screen with Latching Handle, manually operated, side-coiling, latching handle, retractable door screens.
1.	Single Unit Maximum Application Sizes (WxH): 48 x 100 inches (1219 x 2540 mm); or (WxH): 36 x 120 inches (914 x 3048 mm).
2.	Double Unit Maximum Application Sizes (WxH): 96 x 100 inches (2438 x 2540 mm); or (WxH): 72 x 120 inches (1829 x 3048 mm).
B.	Model: Phantom Door Screen with Magnet Fastener, manually operated, side-coiling, magnet fastener, retractable door screens.
1.	Single Unit Maximum Application Sizes (WxH): 48 x 100 inches (1219 x 2540 mm); or (WxH): 36 x 120 inches (914 x 3048 mm).
2.	Double Unit Maximum Application Sizes (WxH): 96 x 100 inches (2438 x 2540 mm); or (WxH): 72 x 120 inches (1829 x 3048 mm).
C.	Finish: Semi-gloss, weather resistant powder coat: Tiger Drylac Polyester Base, AAMA 2604.
1.	Color: Classic White.
2.	Color: Calico Linen.
3.	Color: Slivered Almond.
4.	Color: Sandal Wood.
5.	Color: Driftwood Beige.
6.	Color: Hartford Green.
7.	Color: Rideau Brown.
8.	Color: Coastal Grey.
9.	Color: Mineral Bronze.
10.	Color: Phantom Black.
11.	Color: ______.
12.	Color: As selected by Architect.
13.	Color: Custom coated as selected by Architect.
D.	Screen Mesh:
1.	18/14, PVC coated fiberglass mesh, up to 44 percent solar blockage.
a.	Color: Charcoal.
2.	20/20, PVC coated fiberglass mesh, up to 57 percent solar blockage.
a.	Color: Charcoal.
3.	SheerWeave 2360, PVC coated fiberglass mesh, up to 90 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Chestnut.
c.	Color: Pearl Gray.
d.	Color: Beige.
e.	Color: Oyster.
4.	SheerWeave 2390, PVC coated fiberglass mesh, up to 95 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Chestnut.
c.	Color: Beige.
d.	Color: Oyster.
5.	E-Screen 7510, PVC coated fiberglass mesh, up to 90 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Gray.
c.	Color: Charcoal/Cocoa.
6.	E-Screen 7505, PVC coated fiberglass mesh, up to 95 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Gray.
c.	Color: Charcoal/Cocoa.
E.	Materials:
1.	Extruded Shapes: Alloy 6063-T5.
2.	Extruded Tubes: Alloy 6063-T5.
3.	Latch Rod: Alloy 6063-T5.
F.	Components:
1.	Slide Bar, housing and track system, and sill adaptors: Extruded aluminum.
2.	Screen Retracting Mechanism: Constant tension Class B spring in lubricated and enclosed unit.
3.	Roller Assembly: Extruded aluminum.
4.	Door Latch Mechanism: Nylon gear assembly, aluminum rods, chrome plated zinc handle levers.
5.	Door Latch Mechanism: Ceramic magnet and corrosion resistant plated steel strike plate.
6.	Housing End Caps, Slide Bar End Caps, Track Catches and Door Handle: UV protected, nylon (or Triax for custom color).
a.	Integrally colored to match standard housing color.
b.	Alkyd industrial enamel painted to match custom colored housings.
7.	Label: Provide label with serial number and date of manufacture on each screen unit.
8.	Other miscellaneous items typically provided by manufacturer as required to complete installation.
G.	Accessories:
1.	Speed reducer / roll control insert to slow retraction speed.
2.	Swing restrictor to prevent open doors from slamming back on screen when in the closed position.
3.	Pin lock.
4.	Alarm chime; mount on doors to announce opening and closing of the screen.
5.	Threshold Adaptors: Configuration as shown on Drawings. Mill finish.
6.	Threshold Adaptors: Configuration as shown on Drawings. Black anodized finish.
7.	Threshold Adaptors: Configuration as shown on Drawings. Brass anodized finish.
8.	Threshold Adaptors: Configuration as shown on Drawings. Bronze anodized finish.
9.	Threshold Adaptors: Configuration as shown on Drawings. Finish as selected by Architect.
2.3	RETRACTABLE SCREENS FOR WINDOWS
A.	Model: Phantom Window Screen, manually operated, roll-up, retractable window screens.
1.	Maximum Application Size (WxH): 84 x 90 inches (2134 x 2286 mm).
B.	Model: Phantom Wood Window Screen, manually operated, roll-up, retractable window screens.
1.	Maximum Application Size (WxH): 72 x 78 inches (1829 x 1981 mm).
C.	Finish: Semi-gloss weather resistant powder coat: Akzo Nobel Polyester Base, AAMA 2604.
1.	Color of Window Screen Housing: Classic White.
2.	Color of Window Screen Housing: Slivered Almond.
3.	Color of Window Screen Housing: Sandal Wood.
4.	Color of Window Screen Housing: Driftwood Beige.
5.	Color of Window Screen Housing: Hartford Green.
6.	Color of Window Screen Housing: Rideau Brown.
7.	Color of Window Screen Housing: Coastal Grey.
8.	Color of Window Screen Housing: Phantom Black.
9.	Color of Window Screen Housing: ______.
10.	Color of Window Screen Housing: As selected by Architect.
11.	Color of Window Screen Housing: Custom coated as selected by Architect.
D.	Finish: Wood veneering for window screen housing only.
1.	Pine.
2.	Douglas Fir.
3.	Alder.
4.	Mahogany.
5.	Walnut.
6.	Cherry.
7.	Red Oak.
8.	Veneer Color: ______.
9.	Veneer Color: As selected by Architect.
10.	Veneer Color: Custom coated as selected by Architect.
E.	Screen Mesh:
1.	18/14, PVC coated fiberglass mesh, up to 44 percent solar blockage.
a.	Color: Charcoal.
2.	20/20, PVC coated fiberglass mesh, up to 57 percent solar blockage.
a.	Color: Charcoal.
3.	BetterVue, PVC coated fiberglass mesh, up to 33 percent solar blockage.
a.	Color: Black.
4.	SheerWeave 2360, PVC coated fiberglass mesh, up to 90 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Chestnut.
c.	Color: Pearl Gray.
d.	Color: Beige.
e.	Color: Oyster.
5.	Opaque, PVC coated fiberglass, up to 100 percent solar blockage.
a.	Color: Black.
b.	Color: Pewter.
c.	Color: Suede.
6.	E-Screen 7510, PVC coated fiberglass mesh, up to 90 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Gray.
c.	Color: Charcoal/Cocoa.
7.	E-Screen 7505, PVC coated fiberglass mesh, up to 95 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Gray.
c.	Color: Charcoal/Cocoa.
8.	E-Screen 7501, PVC coated fiberglass mesh, up to 99 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Gray.
c.	Color: Charcoal/Cocoa.
F.	Materials:
1.	Extruded Shapes: Alloy 6063-T5.
2.	Extruded Tubes: Alloy 6063-T5.
3.	Laser-cut Wood Shapes for Phantom Wood Window Screen Line Only: As specified to match wood veneers.
4.	Sealants: As specified in the appropriate Division 07 section for joint sealants.
G.	Components:
1.	Housing, and Track System: Extruded aluminum.
a.	Finish: Powder coated.
b.	Finish: Custom coated.
c.	Finish: Wood veneer.
2.	Slide Bar: Extruded aluminum.
3.	Slide Bar: Solid wood.
4.	Screen Retracting Mechanism: Constant tension class B spring in lubricated and sealed unit.
5.	Roller Assembly: Extruded aluminum.
6.	Track End Cap, Latching Mechanism, Slide Bar End Caps, Housing End Caps, and Accessory Handle: UV protected; nylon, Triax for custom colors.
a.	Integrally colored to match standard housing color.
b.	Alkyd industrial enamel painted to match custom colored housings.
7.	Label: Provide label with serial number and date of manufacture on each screen unit.
8.	Other miscellaneous items typically provided by manufacturer as required to complete installation.
H.	Accessories:
1.	Speed reducer/roll control insert to slow retraction speed.
2.	Telescoping hook to pull and retract high mounted screens: 9 inches (229 mm) to 36 inches (914 mm) chrome handle with black vinyl tip.
3.	Fob and chord to pull and retract high mounted screens.
2.4	RETRACTABLE VERTICALLY ACTING SCREENS FOR LARGE OPENINGS
A.	Model: Phantom Motorized Screen I; 4 inches (102 mm) housing / 2.5 inches (64 mm) tube.
1.	Maximum Application Size (WxH): 120 x 96 inches (3048 x 2438 mm).
B.	Model: Phantom Motorized Screen II; 5-1/2 inches (134 mm) housing / 4 inches (102 mm) tube.
1.	Maximum Application Sizes (WxH): 240 x 132 inches (6096 x 3353 mm); or (WxH): 480 x 132 inches (12192 x 3353 mm) with carriers.
C.	Model: Phantom Motorized Screen III; 7-1/8 inches (181 mm) housing / 5 inches (127 mm) tube.
1.	Maximum Application Size (WxH): 300 x 192 inches (7620 x 4877 mm).
D.	Model: Phantom Manual Overhead Screen IV; 5-1/2 inches (134 mm) housing only / 4 inches (102 mm) tube.
1.	Maximum Application Size (WxH): 216 x 132 inches (5486 x 3353 mm).
2.	Gear system with removable long handle crank.
a.	Gear Ratio: 11:1.
b.	Crank and gear shaft located at the right side of the operable unit.
c.	Crank Length: 59 inches (1499 mm).
d.	Crank Length: 78.75 inches (2000 mm).
E.	Finish: Semi-gloss weather resistant powder coat: Akzo Nobel Polyester Base, AAMA 2604.
1.	Color: Classic White.
2.	Color: Slivered Almond.
3.	Color: Sandal Wood.
4.	Color: Driftwood Beige.
5.	Color: Hartford Green.
6.	Color: Rideau Brown.
7.	Color: Coastal Grey.
8.	Color: Mineral Bronze.
9.	Color: Phantom Black.
10.	Color: ______.
11.	Color: As selected by Architect.
12.	Color: Custom coated as selected by Architect.
F.	Mesh Type:
1.	18/14, PVC coated fiberglass mesh, up to 44 percent solar blockage.
a.	Color: Charcoal.
2.	20/20, PVC coated fiberglass mesh, up to 57 percent solar blockage.
a.	Color: Charcoal.
3.	Tuff Screen (Petscreen Lite), PVC coated polyester, up to 55 percent solar blockage.
a.	Color: Black.
4.	Tuff Screen No-See-Um, PVC coated polyester, up to 58 percent solar blockage.
a.	Color: Black.
5.	Nano 50, PVC coated polyester, up to 50 percent solar blockage.
a.	Color: Black.
6.	Nano 55, PVC coated polyester, up to 55 percent solar blockage.
a.	Color: Black.
7.	Crystal Clear 20/20, PVC, up to 90 percent UV-only, no shade properties, blockage.
a.	Color: Clear.
b.	Border Material: Precontraint 502 Satin, Perimeter fabric for vinyl only, PVC coated polyester, up to 100 percent solar blockage.
c.	Border Material Color: Black.
d.	Border Material Color: Brown.
e.	Border Material Color: Sand.
f.	Border Material Color: White.
g.	Border Material Color: Concrete.
8.	SheerWeave1000, PVC coated fiberglass mesh, up to 75 percent solar blockage.
a.	Color: White.
b.	Color: Antique White.
9.	Suntex 80, PVC coated polyester, up to 80 percent solar blockage.
a.	Color: Black.
b.	Color: Gray.
c.	Color: Brown.
d.	Color: Stucco.
10.	SheerWeave 2360, PVC coated fiberglass mesh, up to 90 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Chestnut.
c.	Color: Pearl Gray.
d.	Color: Beige.
e.	Color: Oyster.
11.	SheerWeave 2390, PVC coated fiberglass mesh, up to 95 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Chestnut.
c.	Color: Beige.
d.	Color: Oyster.
12.	SheerWeave 2500, PVC coated fiberglass mesh, up to 99 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Chestnut.
c.	Color: Beige.
d.	Color: Oyster.
13.	Opaque, PVC coated fiberglass, up to 100 percent solar blockage.
a.	Color: Black.
b.	Color: Pewter.
c.	Color: Suede.
14.	E-Screen 7510, PVC coated fiberglass mesh, up to 90 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Gray.
c.	Color: Charcoal/Cocoa.
15.	E-Screen 7505, PVC coated fiberglass mesh, up to 95 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Gray.
c.	Color: Charcoal/Cocoa.
16.	E-Screen 7501, PVC coated fiberglass mesh, up to 99 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Gray.
c.	Color: Charcoal/Cocoa.
G.	Materials:
1.	Extruded Shapes: Alloy 6063-T5; except the 4 inch (102 mm) motorized housing 1.5 inch (37 mm) octagonal insert, slidebar and u-channel is composed of alloy 6063-T5.
2.	Extruded Tubes: Alloy 6063-T5.
H.	Components:
1.	Housing Back, Top, and Cover: Surface mounted, extruded aluminum. End caps are cast aluminum, ADC12 Aluminum Alloy.
a.	Fabricate surface mounted housings and covers to be the same size.
2.	Angle Mounting Bracket: Recessed, extruded aluminum.
3.	Motor: Somfy, Inc., Maestria RTS 525A2 OR 535A2 tubular type, 120v AC, 60 Hz, with 12.3 feet (3.75 m) grounded plug-in power cord; model as recommended by screen manufacturer based on screen size.
4.	Motor: Somfy Inc., Sonesse RTS 510S2 tubular type, 120v AC, 60 Hz, with 6.5 feet (2 m) grounded plug-in power cord; model as recommended by screen manufacturer based on screen size.
5.	Motor: Somfy Inc., LT50 RS485 star head motor, 120v AC, 60 Hz with 9.8 feet (3 m) grounded plug-in power cord, model as recommended by screen manufacturer based on screens size; used for integration with building automation systems.
6.	Motor: Somfy, Inc., RTS Motor LS404S2 or LS409R2 tubular type, 120v AC, 60 Hz, with 23 feet (7 m) grounded plug-in power cord; model as recommended by screen manufacturer based on screen size.
7.	Manual Gear: Simu, Inc., 11: 1 Manual gear, single stop, with oval eye and shaft for operation via manual cranking wand. Model as recommended by screen manufacturer.
8.	Roller Assembly: Extruded aluminum, outside diameter as specified by manufacturer based on screen size.
9.	Sidetrack and Cover: Surface mounted, extruded aluminum.
10.	Sidetrack and Roller/Tube: Recessed, extruded aluminum.
11.	Slide Bar: Extruded aluminum.
I.	Bottom Seal: 3 inches (76 mm) black or grey vinyl.
J.	Bottom Seal: 4 inches (102 mm) black or grey vinyl.
K.	Bottom Seal: 6 inches (152 mm) black or grey vinyl.
L.	Bottom Seal: 0.75 inches (19 mm) brush pile, black.
M.	Bottom Seal: 1.5 inches (38 mm) black brush pile.
N.	Zipper: No. 3, acetal teeth, polyester webbing, white, black, or grey color coordinated to suit screen mesh.
O.	Zipper: No. 8, acetal teeth, polyester webbing, white or black color coordinated to suit screen mesh.
P.	Control System.
1.	Programmable handheld single channel remote.
a.	Weather Exposure: Standard.
b.	Weather Exposure: All weather.
c.	Number of units: ______.
d.	Number of units as scheduled.
e.	Number of units as shown on schematic drawing.
2.	Programmable handheld five channel remote.
a.	Weather Exposure: Standard.
b.	Weather Exposure: All weather.
c.	Number of units: ______.
d.	Number of units as scheduled.
e.	Number of units as shown on schematic drawing.
3.	Programmable battery operated, recessed wall mount single channel control.
a.	Color: White.
b.	Color: Black.
c.	Number of units: ______.
d.	Number of units as scheduled.
e.	Number of units as shown on schematic drawing.
4.	Programmable battery operated, recessed wall mount five channel control.
a.	Color: White.
b.	Color: Black.
c.	Number of units: ______.
d.	Number of units as scheduled.
e.	Number of units as shown on schematic drawing.
5.	Programmable 16 channel remote:
a.	Number of units: ______.
b.	Number of units as scheduled.
c.	Number of units as shown on schematic drawing.
6.	Smoove Origin programmable battery operated surface mounted single channel control; high tech styling.
a.	Number of units: ______.
b.	Number of units as scheduled.
c.	Number of units as shown on schematic drawing.
7.	Smoove Origin programmable battery operated surface mounted four channel control; high tech styling.
a.	Number of units: ______.
b.	Number of units as scheduled.
c.	Number of units as shown on schematic drawing.
8.	Tahoma Switch Wifi to radio transmission interface, for smart phone and tablet control:
a.	Number of units: ______.
b.	Number of units as scheduled.
c.	Number of units as shown on schematic drawing.
9.	Programmable 16 channel universal radio transmission interface, for control integration into a building automation system:
a.	Number of units: ______.
b.	Number of units as scheduled.
c.	Number of units as shown on schematic drawing.
10.	Building Automation System:
a.	Control systems required:
1)	______.
b.	Refer to the appropriate specifications in Division 26 for more detailed information concerning building automation systems.
Q.	Accessories:
1.	Sun and wind sensor.
2.	Sun and rain sensor.
3.	Timer.
2.5	RETRACTABLE HORIZONTALLY ACTING SCREENS FOR LARGE OPENINGS
A.	Model: Phantom Manual Screen.
1.	Operation: Manual, horizontal.
2.	Single Unit Maximum Application Sizes (WxH): 180 x 144 inches (4572 x 3658 mm).
3.	Double Unit Maximum Application Sizes (WxH): 360 x 144 inches (9144 x 3658 mm).
B.	Finish: Semi-gloss weather resistant powder coat: Akzo Nobel Polyester Base, AAMA 2604.
1.	Color: Classic White.
2.	Color: Calico Linen.
3.	Color: Slivered Almond.
4.	Color: Sandal Wood.
5.	Color: Driftwood Beige.
6.	Color: Hartford Green.
7.	Color: Rideau Brown.
8.	Color: Coastal Grey.
9.	Color: Mineral Bronze.
10.	Color: Phantom Black.
11.	Color: ______.
12.	Color: As selected by Architect.
13.	Color: Custom coated as selected by Architect.
C.	Finish: Silver Anodized, AAMA A31.
D.	Mesh Type:
1.	18/14, PVC coated fiberglass mesh, up to 44 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Silver Gray.
2.	20/20, PVC coated fiberglass mesh, up to 57 percent solar blockage.
a.	Color: Charcoal.
3.	Tuff Screen (Petscreen Lite), PVC coated polyester, up to 55 percent solar blockage.
a.	Color: Black.
4.	Tuff Screen No-See-Um, PVC coated polyester, up to 58 percent solar blockage.
a.	Color: Black.
5.	Nano 50, PVC coated polyester, up to 50 percent solar blockage percent.
a.	Color: Black.
6.	SheerWeave 2360, PVC coated fiberglass mesh, up to 90 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Chestnut.
c.	Color: Pearl Gray.
d.	Color: Beige.
e.	Color: Oyster.
7.	SheerWeave 2390, PVC coated fiberglass mesh, up to 95 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Chestnut.
c.	Color: Beige.
d.	Color: Oyster.
8.	E-Screen 7510, PVC coated fiberglass mesh, up to 90 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Gray.
c.	Color: Charcoal/Cocoa.
9.	E-Screen 7505, PVC coated fiberglass mesh, up to 95 percent solar blockage.
a.	Color: Charcoal.
b.	Color: Charcoal/Gray.
c.	Color: Charcoal/Cocoa.
E.	Materials:
1.	Extruded Shapes and Tubes: Alloy 6063-T5.
2.	Mesh Port Extrusion: PVC.
3.	Top Track Aluminum Insert: 6061 T6, 11G sheet slits.
4.	Latch Rod: 6063-T5 extruded.
F.	Components:
1.	Slide Bar, housing, roller, slidebar tracks (standard top track, standard bottom track, recessed bottom track), sill adaptors: Extruded aluminum. Mesh track PVC; top mesh track uses aluminum insert, slit sheet.
2.	Screen Retracting Mechanism: Constant tension Class B spring in lubricated and enclosed unit.
3.	Zipper: No 2, Coil zipper, black, weldable.
4.	Door Latch Mechanism: Nylon gear assembly, aluminum rods, chrome plated zinc handle levers.
5.	Housing End Caps: End caps are cast ADC12 Aluminum Alloy.
6.	Slide Bar End Caps, Track Catches and Door Handle: UV protected, nylon (or Triax for custom color).
a.	Integrally colored to match standard housing color.
b.	Alkyd industrial enamel painted to match custom colored housings.
G.	Accessories:
1.	Housing cup for recessing, black nylon.
2.	Bottom recessed track catches and track joiner to stop slidebar from over extending on a double unit, black nylon.
3.	U-Channel, extruded aluminum.
4.	Swing restrictor to prevent open doors from slamming back on screen when in the closed position.
5.	Threshold Adaptors: Configuration as shown on Drawings. Mill finish.
6.	Threshold Adaptors: Configuration as shown on Drawings. Black anodized finish.
7.	Threshold Adaptors: Configuration as shown on Drawings. Brass anodized finish.
8.	Threshold Adaptors: Configuration as shown on Drawings. Bronze anodized finish.
9.	Threshold Adaptors: Configuration as shown on Drawings. Finish as selected by Architect.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates upon which screen components will be installed have been properly prepared.
1.	Verify that screen opening complies with manufacturer's requirements for being square, plumb, and level.
B.	Notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install screens per manufacturer's instructions and requirements to provide performance as designed and maintain warranties offered.
1.	Ensure mounting surface is prepared per manufacturer's instructions and requirements to provide performance as designed and maintain warranties offered.
2.	Install sealant in joints between metal screen members and adjacent construction.
B.	Demonstrate operation to Owner's Representative.
3.4	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION