SECTION 09 22 36

PLASTIC ACCESSORIES FOR GYPSUM BOARD AND PLASTER

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2007 -  2017 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Lathing, furring and finishing components for gypsum board, plaster, and stucco.
1.2	RELATED SECTIONS
A.	Section 04 70 00 - Manufactured Masonry.
B.	Section 07 95 00 - Expansion Control.
C.	Section 06 10 00 - Rough Carpentry.
D.	Section 09 26 00 - Veneer Plastering.
E.	Section 09 29 00 - Gypsum Board. 
1.3	REFERENCES
A.	ASTM International (ASTM):
1.	ASTM C1047 - Standard Specification for Accessories for Gypsum Wallboard and Gypsum Veneer Base. 
2.	ASTM C 1063 - Standard Specification for Installation of Lathing and Furring to Receive Interior and Exterior Portland Cement-Based Plaster. 
3.	ASTM C 1764 - Standard Test Methods for Non-Metallic Plaster Bases (Lath) Used with Portland Cement-Based Plaster in Vertical Wall Applications. 
4.	ASTM C 1780 - Standard Practice for Installation Methods for Adhered Manufactured Stone Masonry Veneer. 
5.	ASTM C 1787 - Standard Specification for Non-Metallic Plaster Bases (Lath) Used with Portland Cement-Based Plaster in Vertical Wall Applications. 
6.	ASTM C 1788 - Standard Specification for Non-Metallic Plaster Bases. 
7.	ASTM D 256 - Standard Test Methods for Determining the Izod Pendulum Impact Resistance of Plastics. 
8.	ASTM D579 - Standard Specification for Greige Woven Glass Fabrics.
9.	ASTM D638 - Standard Test Method for Tensile Properties of Plastics. 
10.	ASTM D648 - Standard Test Method for Deflection Temperature of Plastics Under Flexural Load in the Edgewise Position. 
11.	ASTM D696 - Standard Test Method for Coefficient of Linear Thermal Expansion of Plastics Between -30C and 30C with a Vitreous Silica Dilatometer. 
12.	ASTM D790 - Standard Test Methods for Flexural Properties of Unreinforced and Reinforced Plastics and Electrical Insulating Materials. 
13.	ASTM D1784 - Standard Specification for Rigid Poly (Vinyl Chloride) (PVC) Compounds and Chlorinated Poly (Vinyl Chloride) (CPVC) Compounds. 
14.	ASTM D3678 - Standard Specification for Rigid Poly (Vinyl Chloride (PVC) Interior- Profile Extrusions. 
15.	ASTM D4216 - Standard Specification for Rigid Poly (Vinyl Chloride) (PVC) and Related PVC and Chlorinated Poly (Vinyl Chloride) (CPVC) Building Products Compounds. 
16.	ASTM E84 - Standard Test Method for Surface Burning Characteristics of Building Materials. 
B.	IAPMO UER 0284 - ULTRA-LATH PLUS is recognized by IAPMO Uniform Evaluation Services report #0284 as code compliant to the 2009 and 2012 IBC and IRC.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings: Submit manufacturer's approved shop drawings detailing the size and type of each product specified. Coordinate locations of components with the Finish Schedules listed in the Contract Drawings.
D.	Selection Samples: For each finish product specified, two samples representing manufacturer's full range of available colors and styles.
E.	Verification Samples: For each finish product specified, two samples representing actual product, color, and style.
F.	Sustainable Design Submittals:  For projects seeking USGBC certification, submit the manufacturer's information documenting product contribution to the following LEED credits: 
1.	Recycled content. 
2.	Regional materials.
1.5	QUALITY ASSURANCE
A.	Manufacturer's products are evaluated, certified and listed by independent third party testing organization Intertek Testing Services NA Ltd./Warnock Hersey who conduct comprehensive review of manufacturer's facility and processes, including receipt and qualification of raw materials, manufacturing, packaging and shipping of finished product. The Warnock Hersey evaluation process is on-going.
B.	Manufacturer Qualifications: All primary products specified in this section will be supplied by a single manufacturer with a minimum of ten (10) years experience.
C.	Installer Qualifications: All products listed in this section are to be installed by a single installer with a minimum of five (5) years demonstrated experience in installing products of the same type and scope as specified.
D.	Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
1.	Finish areas designated by Architect.
2.	Do not proceed with remaining work until workmanship, color, and sheen are approved by Architect.
3.	Refinish mock-up area as required to produce acceptable work.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging until ready for installation.
B.	Store and dispose of hazardous materials, and materials contaminated by hazardous materials, in accordance with requirements of local authorities having jurisdiction.
1.7	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
1.8	WARRANTY
A.	At project closeout, provide to Owner or Owners Representative an executed copy of the manufacturer's standard limited warranty against manufacturing defect, outlining its terms, conditions, and exclusions from coverage.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Plastic Components, Inc., which is located at:<BR />9051 N.W. 97th Ter.<BR />Miami, FL 33178<BR />Toll Free Tel: 800-327-7077<BR />Tel: 305-885-0561<BR />Fax: 305-887-2452<BR />Email: request info (Pc_sales@plasticomponents.com);Web: http://www.plasticomponents.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	MATERIALS
A.	Polyvinyl Chloride (PVC):
1.	Tensile Strength - ASTM D 638 (psi):
a.	Plaster accessories at 0 F (-18C): 8100.
b.	Plaster accessories at 72 F (22C): 5900.
c.	Gypsum accessories at 72 F (22C): 6,200. 
2.	Tensile Modulus - ASTM D 638 (psi):
a.	Plaster accessories at 0 F (-18C): 425,000.
b.	Plaster accessories at 72 F (22C): 360,000.
c.	Gypsum accessories at 72 F (22C): 390,000. 
3.	Flexural Strength - ASTM D 790 (psi):
a.	Plaster accessories at 0 F (-18C): 16,500.
b.	Plaster accessories at 72 F (22C): 11,200.
c.	Gypsum accessories at 72 F (22C): 11,000. 
4.	Flexural Modulus - ASTM D 790 (psi):
a.	Plaster accessories at 0 F (-18C): 497,000.
b.	Plaster accessories at 72 F (22C): 415,000.
c.	Gypsum accessories at 72 F (22C): 35,000.
5.	IZOD Impact - ASTM D 256 (ft-lbs/in):
a.	Plaster accessories at 0 F (-18C): 1.1.
b.	Plaster accessories at 72 F (22C): 3.4.
c.	Gypsum accessories at 72 F (22C): 9.0. 
6.	Heat Distortion Temperature for Plaster and Gypsum - ASTM D648 (psi): 
a.	Heat Distortion Temperature at 254 F (123 C) 264 psi (1.82 MPa): 160 F (71C). 
7.	Coefficient of Linear Thermal Expansion - ASTM D696 (psi): 
a.	Plaster Coefficient of Linear Thermal Expansion (in/in F x 10E5): 3.45. 
b.	Gypsum Coefficient of Linear Thermal Expansion 105 in/in F (105 cm/cm C): 6.6.  
8.	Fire Tunnel Test for Plaster and Gypsum Accessories - ASTM E84:
a.	Flame Spread: 18.
b.	Fuel Contribution: ND.
c.	Smoke Density @ 35 Mils: 250.
d.	Fire Rating: Class A.
9.	Reaction to Stucco or Plaster: None.
10.	Reaction to Joint Cements: None.
2.3	GYPSUM BOARD TRIMS 
A.	RADii Trim Systems: 
1.	Description:  Finish for suspended ceiling terminating at a curved wall or surface. 
2.	Compliance:  ASTM C1047 and ASTM D3678. 
3.	Inside radius: 15 inch (381 mm), Outside radius 15 inch (381 mm), Size 9/16 inch (14 mm). 
4.	Inside radius: 24 inch (609 mm), Outside radius 24 inch (609 mm), Size 15/16 inch (24 mm). 
5.	Inside radius: 30 inch (762 mm), Outside radius 30 inch (762 mm), Size 3/8 inch (10 mm) Reveal. 
6.	Inside radius: 54 inch (1371 mm), Outside radius 36 inch (762 mm), Size 3/4 inch (19 mm) Reveal. 
7.	Inside radius: 30 inch (762 mm), Outside radius 30 inch (762 mm), Size 1/4 inch (6 mm) Reveal. 
B.	U Channels: 
1.	Description:  U-shaped edge trim to protect edges of gypsum board against moisture. 
2.	Compliance:  ASTM C1047 and ASTM D3678. 
3.	1/2 inch (13 mm) with 3/8 inch (10 mm) flange. 
4.	5/8 inch (16 mm) with 3/8 inch (10 mm) flange. 
5.	3/4 inch (19 mm) with 3/8 inch (10 mm) flange. 
C.	ULTRA-CORNERS: 
1.	Description:  Ultra-thin profile for use in cathedral ceilings or walls where off angle corners meet. Attach with adhesive or drywall mud. 
2.	Compliance:  ASTM C1047 and ASTM D3678. 
3.	Dimensions: 1/16 inch (2 mm) flexible profile can be angled to any degree. 
D.	Trim Moldings: 
1.	Compliance:  ASTM C1047 and ASTM D3678. 
2.	Inside Corners: 
a.	Description:  Used in lamination of vinyl wall coverings to form a finished inside corner. 
b.	Dimensions: 1/2 inch (13 mm) with 1/2 inch (13 mm) fold and 1 inch (25 mm) flange. 
3.	"F" Molding: 
a.	Description:  Outside corner for use in drywall or acoustical applications, can be laminated for vinyl wall covering applications. 
b.	Dimensions: 1 inch (25 mm) by 1 inch (25 mm) by 1-3/8 inch (35 mm). 
c.	Dimensions: 1 inch (25 mm) by 1/2 inch (13 mm) by 1-1/2 inch (38 mm). 
4.	"T" Molding: 
a.	Description:  Used to finish two adjoining surfaces. 
b.	Dimensions: 1/2 inch (13 mm) by 1/2 inch (13 mm). 
5.	"H" Molding: 
a.	Description:  May be laminated with vinyl wall covering of for connecting pre-finished panels. 
b.	Dimensions: 1/2 inch (13 mm) board thickness. 
c.	Dimensions: 5/8 inch (16 mm) board thickness. 
E.	Wall Angles: 
1.	Description:  Acoustical ceiling wall angle shadow molding. 
2.	Compliance:  ASTM C1047 and ASTM D3678. 
3.	Dimensions: 3/4 inch (19 mm) by 1/2 inch (13 mm) by 3/4 inch (19 mm). 
F.	Universal Flexible PVC Strips: 
1.	Description:  May be laminated with vinyl wall covering and used in either an inside or outside corner. 
2.	Compliance:  ASTM C1047 and ASTM D3678. 
3.	Dimensions: 2 inch (50 mm) wide by 10 feet (3 m) long. 
G.	Corner Caps: 
1.	Compliance:  ASTM C1047, ASTM D3678, and ASTM D4216. 
2.	2-Way Inside Corner Cap: 
a.	Description:  For joining two bullnose corners at 90 degree angles. 
b.	Dimensions: Manufacturer's standard. 
3.	2-Way Splayed Inside Corner Cap: 
a.	Description:  Two way splayed inside corner cap that forms a 135 degree corner. 
b.	Dimensions: Manufacturer's standard. 
4.	3-Way Outside Corner Cap: 
a.	Description:  Three way outside corner cap for joining three bullnose corners at 90 degree angles. 
b.	Dimensions: Manufacturer's standard. 
5.	3-Way Splayed Outside Corner Cap: 
a.	Description:  Three way splayed outside corner cap that forms a 135 degree corner. 
b.	Dimensions: Manufacturer's standard. 
6.	3-Way Inside Corner Cap: 
a.	Description:  Three way inside corner cap for joining three bullnose corners at 90 degree angles. 
b.	Dimensions: Manufacturer's standard.
H.	Control Joints: 
1.	Compliance:  ASTM C1047, ASTM D3678, and ASTM D4216. 
2.	Drywall Control Joint: 
a.	Description:  Surface mounted control joint with removable tape for use in wall or ceiling applications.  Designed to relived stress in large areas, removable tape protects the v-groove during installation, with built-in 1/16 inch (2 mm) stop to ensure proper finish thickness. 
b.	Dimensions: 2-1/4 inch (57 mm) wide, with groove 1/4 inch (6 mm) wide and 1/2 inch (13 mm) deep. 
3.	Sheathing Slip Joint: 
a.	Description:  Two-piece slip joint for sheathing products where unusual movement is anticipated.  Part must be installed before drywall is firmly attached, may be installed in horizontal or vertical applications. 
b.	Dimensions: Opens from 1-1/4 inch (32 mm) to 1-3/4 inch (44 mm), for use with 1/2 inch (13 mm) board thickness. 
c.	Dimensions: Opens from 1-1/4 inch (32 mm) to 1-3/4 inch (44 mm), for use with 5/8 inch (16 mm) board thickness. 
4.	Control Joint: 
a.	Description:  Flexible control joint for use in wall and ceiling designs to control movement. Has removable tape to protect v-groove during installation, with built-in 1/16 inch (2 mm) stops to ensure proper drywall thickness.  Flanges are placed on top of two separated boards with v-groove between boards. 
b.	Dimensions: Inverted 1/2 inch (13 mm) expansion joint, 1/16 inch (2 mm) finish top with removable tape. 
I.	Reveals: 
1.	Compliance:  ASTM C1047, ASTM D3678, and ASTM D4216. 
2.	Aesthetic Drywall Reveals: 
a.	Description:  Perforated flanges are placed on separated sheets of board with a "U" channel placed in a separate channel, with built-in stops to ensure proper thickness of base and finish.   Designed for use with 1/2 inch (13 mm) or 5/8 inch (16 mm) board thickness. 
b.	Dimensions:  Reveal width 1/2 inch (13 mm), Reveal depth 1/2 inch (13 mm), 1 inch (25 mm) flange. 
c.	Dimensions:  Reveal width 1 inch (25 mm), Reveal depth 1/2 inch (13 mm), 1 inch (25 mm) flange. 
d.	Dimensions:  Reveal width 3/4 inch (19 mm), Reveal depth 1/2 inch (13 mm), 1 inch (25 mm) flange. 
e.	Dimensions:  Reveal width 3/8 inch (10 mm), Reveal depth 1/2 inch (13 mm), 1 inch (25 mm) flange. 
f.	Dimensions:  Reveal width 5/8 inch (16 mm), Reveal depth 1/2 inch (13 mm), 1 inch (25 mm) flange. 
g.	Dimensions:  Reveal width 1-1/2 inch (38 mm), Reveal depth 1/2 inch (13 mm), 1 inch (25 mm) flange with large and small holes. 
h.	Dimensions:  Reveal width 2 inch (51 mm), Reveal depth 1/2 inch (13 mm), 1 inch (25 mm) flange. 
i.	Dimensions:  Reveal width 3 inch (76 mm), with no holes in the flange. 
j.	Dimensions:  Reveal width 4 inch (102 mm), with no holes in the flange. 
3.	Aesthetic Drywall Reveal Intersections: 
a.	Description:  Factory thermal welded, surface mounted intersections eliminate costly and time consuming field cut intersections. 
b.	Dimensions:  1/2 inch (13 mm) by 1/2 inch (13 mm). 
c.	Dimensions:  1 inch (25 mm) by 1/2 inch (13 mm). 
d.	Dimensions:  3/4 inch (19 mm) by 1/2 inch (13 mm). 
e.	Dimensions:  3/8 inch (10 mm) by 1/2 inch (13 mm). 
f.	Dimensions:  5/8 inch (16 mm) by 1/2 inch (13 mm). 
g.	Dimensions:  1-1/2 inch (38 mm) by 1/2 inch (13 mm). 
h.	Dimensions:  2 inch (51 mm) by 1/2 inch (13 mm). 
i.	Dimensions:  3 inch (76 mm) by 1/2 inch (13 mm). 
j.	Dimensions:  4 inch (102 mm) by 1/2 inch (13 mm).
J.	Corner Beads: 
1.	Compliance:  ASTM C1047, ASTM D3678, and ASTM D4216. 
2.	Corner Bead: 
a.	Description:  To be used on outside corner, tapered legs are perforated and striated for better adhesion, eliminating the need to tape the flange. 
b.	Dimensions: 1-1/4 by 1-1/4 inch (32 by 32 mm). 
c.	Dimensions: 1-5/8 by 1-5/8 inch (41 by 41 mm). 
3.	Arch Corner Bead: 
a.	Description:  To be used where a curve or arch is formed, pre-slotted flange allows for perfect arches, tapered flanges are perforated and striated for better adhesion, eliminating the need to tape the flange. 
b.	Dimensions: 1-1/4 by 1-1/4 inch (32 by 32 mm). 
4.	Inside Corner Bead: 
a.	Description:  Eliminates the need to tape inside corners to provide sharp 90 degree corners. 
b.	Dimensions: 1-1/4 by 1-1/4 inch (32 by 32 mm). 
5.	Splayed Corner Bead: 
a.	Description:  To be used in conditions where two 45 degree walls intersect forming a 120 to 135 degree angle. 
b.	Dimensions: Manufacturers standard. 
K.	Bullnose Trims: 
1.	Compliance:  ASTM C1047, ASTM D3678, and ASTM D4216. 
2.	Half Round Bullnose: 
a.	Description:  Used for terminations when a window or door casing trim is eliminated.  Can also be used where extra layers of drywall are used for decorative purposes.  Trim is installed after installation of gypsum board. 
b.	Dimensions: 3/4 inch (19 mm) half round bullnose. 
3.	Bullnose Corner Bead: 
a.	Description:  Used where smooth rounded corners are required, shallow shoulder eliminates heavy build-up of topping. 
b.	Dimensions: 5/8 inch (16 mm) flange, 3/4 inch (19 mm) radius. 
c.	Dimensions: 1 inch (25 mm) flange, 3/4 inch (19 mm) radius. 
d.	Dimensions: 1 inch (25 mm) offset flange, 3/4 inch (19 mm) radius. 
4.	Bullnose Arch with One Slotted Leg: 
a.	Description:  Used for faster installation of difficult arches. 
b.	Dimensions: 5/8 inch (16 mm) flange, 1 leg slotted. 
c.	Dimensions: 1 inch (25 mm) flange, 1 leg slotted. 
d.	Dimensions: 1 inch (25 mm) offset flange, 1 leg slotted. 
5.	Bullnose Inside Corner Bead: 
a.	Description:  For use when an inside corner is specified, serves as complimentary trim when an outside bullnose corner bead is being used. 
b.	Dimensions: Manufacturer's standard. 
6.	Splayed Bullnose Corner Bead: 
a.	Description:  To be used in conditions where two 45 degree walls intersect forming a 120 to 135 degree angle. 
b.	Dimensions: Manufacturer's standard. 
7.	Bullnose Base Adapter: 
a.	Description:  Transforms a bullnose corner bead to a 90 degree base molding. 
b.	Dimensions: 1-5/8 inch (41 mm) by 1-5/8 inch (41 mm) by 6-5/8 inch (168 mm) high, can be field cut for narrower bases. 
L.	Trim Tab: 
1.	Compliance:  ASTM C1047, ASTM D3678, and ASTM D4216. 
2.	Definition: To be used where a wall joins a suspended ceiling, window, or door frame.  Tear away tab eliminates the need for costly masking to provide a clean detail. 
3.	Dimensions: 1-1/16 (27 mm) perforated flange for 1/2 inch (13 mm) board thickness. 
4.	Dimensions: 1-1/16 (27 mm) perforated flange for 5/8 inch (16 mm) board thickness. 
M.	Shadow Mold: 
1.	Compliance:  ASTM C1047, ASTM D3678, and ASTM D4216. 
2.	Definition: Provides a reveal or relief detail around windows, doors, and wall to ceiling junctions.  Can be used in either vertical or horizontal applications. 
3.	Dimensions: 1/2 inch (13 mm) by 1/2 inch (13 mm) or more. 
4.	Dimensions: 3/4 inch (19 mm) by 1/2 inch (13 mm) or more. 
5.	Dimensions: 1 inch (25 mm) by 1/2 inch (13 mm) or more. 
N.	"J" Beads: 
1.	Compliance:  ASTM C1047, ASTM D3678, and ASTM D4216. 
2.	"J" Bead: 
a.	Description:  Edge trim for capping vertical or horizontal edges of raw gypsum board with tapered face return.  Protects moisture from weeping into board. 
b.	Dimensions: 1/4 inch (6 mm) with 1/2 inch (13 mm) front return and 1 inch (25 mm) back flange. 
c.	Dimensions: 3/8 inch (10 mm) with 1/2 inch (13 mm) front return and 1 inch (25 mm) back flange. 
d.	Dimensions: 1/2 inch (13 mm) with 1/2 inch (13 mm) front return and 1 inch (25 mm) back flange. 
e.	Dimensions: 5/8 inch (16 mm) with 1/2 inch (13 mm) front return and 1 inch (25 mm) back flange. 
f.	Dimensions: 3/4 inch (19 mm) with 1/2 inch (13 mm) front return and 1 inch (25 mm) back flange. 
3.	Fillable "J" Bead: 
a.	Description:  Used to encase raw edges of drywall, preventing moisture from migrating into board.  Wide perforated flange allows topping to key to board, eliminating the need to tape the flange. 
b.	Dimensions: 1/2 inch (13 mm) board thickness, with 1-1/16 (27 mm) perforated flange. 
c.	Dimensions: 5/8 inch (16 mm) board thickness, with 1-1/16 (27 mm) perforated flange. 
d.	Dimensions: 7/8 inch (22 mm) board thickness, with 1-1/16 (27 mm) perforated flange. 
O.	"L" Beads: 
1.	Compliance:  ASTM C1047, ASTM D3678, and ASTM D4216. 
2.	Fillable "L" Bead: 
a.	Description:  Used to create a clean detail at any point of termination of gypsum board into windows and doors.  Wide flange allows for positioning of trim to cover uneven edges.  Perforated flange allows topping to key to gypsum board, eliminating the need to tape the flange. 
b.	Dimensions: 1/2 inch (13 mm) board thickness with 1-1/16 (27 mm) perforated flange. 
c.	Dimensions: 5/8 inch (16 mm) board thickness with 1-1/16 (27 mm) perforated flange. 
3.	Reverse "L" Bead: 
a.	Description:  Fillable mudding flange and extra wide return flange eliminate the need to tape where vertical and horizontal planes meet.  Perfect product for remodeling. 
b.	Dimensions: 1-1/4 inch 32 mm)  with 1 inch (25 mm) flange. 
2.4	LATH (PLASTIC)
A.	Ultra-Lath Plus:
1.	Type: 1/4 inch (6 mm) self-furred.
2.	Compliance: ASTM C 1764, ASTM C 1780, ASTM C 1787 and ASTM C 1788, IAPMO UER 0284.
3.	Sheet Dimensions: 27 inches x 96 inches (686mm x 2438mm).
4.	Roll Dimensions: 27 inches x 75 feet (686mm x 22.9 m).
B.	Paper-Backed Ultra-Lath Plus:
1.	Type: 1/4 inch (6 mm) self-furred.
2.	Compliance: ASTM C 1764, ASTM C 1780, ASTM C 1787 and ASTM C 1788, IAPMO UER 0284.
3.	Sheet Dimensions: 27 inches x 96 inches (686mm x 2438mm).
C.	Strip-Lath Plus:
1.	Type: 1/4 inch (6 mm) self-furred.
2.	Compliance: ASTM C 1764, ASTM C 1780, ASTM C 1787 and ASTM C 1788, IAPMO UER 0284
3.	Roll Dimensions: 3 inches wide x 96 inches (76 mm x 2438 mm).
4.	Roll Dimensions: 4 inches wide x 96 inches (102 mm x 2438 mm).
5.	Roll Dimensions: 6 inches wide x 96 inches (152 mm x 2438 mm).
6.	Roll Dimensions: 8 inches wide x 96 inches (203 mm x 2438 mm).
D.	Ultra-Lath:
1.	Type: 1/8 inch (3 mm) self-furred.
2.	Compliance:  TCNA RH123-14 and F185-14.
3.	Sheet Dimensions: 27 inches x 96 inches (686mm x 2438mm).
4.	Roll Dimensions: 27 inches x 100 feet (686mm x 30.48 m).
E.	Paper-Backed Ultra-Lath:
1.	Type:  1/8 inch (3 mm) self-furred.
2.	Compliance: ICC-ES Number: 94182.
3.	Sheet Dimensions: 27 inches x 96 inches (686mm x 2438mm).
4.	Roll Dimensions: 27 inches x 100 feet (686mm x 30.48 m).
F.	Strip-Lath:
1.	Type: 1/8 inch (3 mm) self-furred.
2.	Roll Dimensions: 3 inches wide x 96 inches (76mm x 2438mm).
3.	Roll Dimensions: 4 inches wide x 96 inches (102mm x 2438mm).
4.	Roll Dimensions: 6 inches wide x 96 inches (152mm x 2438mm).
5.	Roll Dimensions: 8 inches wide x 96 inches (203mm x 2438mm).
2.5	CASING BEADS
A.	Corner Bead:
1.	Model: 1A - 2.5 inches by 2.5 inches (64mm x 64mm) 90 Degree Flange.
2.	Model: 1B - 1.5 inches by 1.5 inches (38mm x 38mm) 90 Degree Flange.
3.	Model: 2 - 2.75 inches by 2.75 inches (70mm x 70mm) 90 Degree Flange.
4.	Model: 3 - 2.5 inches by 1.5 inches (64mm x 38mm) 90 Degree Flange.
5.	Model: 1A4 - 4 inches by 4 inches (102mm x 102mm) 90 Degree Flange.
6.	Model: 1A135 - 2.5 inches by 2.5 inches (64mm x 64mm) Angled Flange.
7.	Model: BN1A - 2.5 inches by 2.5 inches (64mm x 64mm) Bullnose Flange.
B.	Standard Flange Casing Bead:
1.	Model: 1025 - 1/4 inch (6mm) depth x 1 3/4 inch (44mm) tall vertical leg.
2.	Model: 1038 - 3/8 inch (9.5mm) depth x 1 3/4 inch (44mm) tall vertical leg.
3.	Model: 1050 - 1/2 inch (13mm) depth x 1 3/4 inch (44mm) tall vertical leg.
4.	Model: 1058 - 5/8 inch (16mm) depth x 1 3/4 inch (44mm) tall vertical leg.
5.	Model: 1075 - 3/4 inch (19mm) depth x 1 3/4 inch (44mm) tall vertical leg.
6.	Model: 1078 - 7/8 inch (22mm) depth x 1 3/4 inch (44mm) tall vertical leg.
7.	WP - Casing bead to include weep holes.
C.	Narrow Flange Casing Bead:
1.	Model: 1038X - 3/8 inch (9.5mm) depth x 1-1/4 inch (32mm) tall vertical leg.
2.	Model: 1050X - 1/2 inch (13mm) depth x 1-1/4 inch (32mm) tall vertical leg.
3.	Model: 1075X - 3/4 inch (19mm) depth x 1-1/4 inch (32mm) tall vertical leg.
4.	Model: 1078X - 7/8 inch (22mm) depth x 1-1/4 inch (32mm) tall vertical leg.
5.	WP - Casing bead to include weep holes.
D.	"T" Bar Casing Bead:
1.	Model: 1100 - 1 inch (25mm) depth x 1 3/4 inch (44mm) tall vertical leg.
2.	Model: 1125 - 1-1/4 inch (32mm) depth x 1 3/4 inch (44mm) tall vertical leg.
3.	Model: 1150 - 1 -1/2 inch (38mm) depth x 1 3/4 inch (44mm) tall vertical leg.
4.	Model: 1200 - 2 inch (51mm) depth x 1 3/4 inch (44mm) tall vertical leg.
E.	Old Style Casing Bead:
1.	Model: 1100-O - 1 inch (25mm) depth x 1 3/4 inch (44mm) tall vertical leg.
2.	Model: 1125-O - 1-1/4 inch (32mm) depth x 1 3/4 inch (44mm) tall vertical leg.
3.	Model: 1150-O - 1-1/2 inch (38mm) depth x 1 3/4 inch (44mm) tall vertical leg.
4.	Model: 1200-O - 2 inch (51mm) depth x 1 3/4 inch (44mm) tall vertical leg.
5.	WP - Casing bead to include weep holes.
F.	Arched Casing Bead:
1.	Model: 1025A - 1/4 inch (6mm) depth x 1 3/4 inch (44mm) tall vertical leg.
2.	Model: 1038A - 3/8 inch (9.5mm) depth x 1 3/4 inch (44mm) tall vertical leg.
3.	Model: 1050A - 1/2 inch (13mm) depth x 1 3/4 inch (44mm) tall vertical leg.
4.	Model: 1058A - 5/8 inch (16mm) depth x 1 3/4 inch (44mm) tall vertical leg.
5.	Model: 1075A - 3/4 inch (19mm) depth x 1 3/4 inch (44mm) tall vertical leg.
6.	Model: 1078A - 7/8 inch (22mm) depth x 1 3/4 inch (44mm) tall vertical leg.
7.	Model: 1100-0-A - 1 inch (25mm) depth x 1 3/4 inch (44mm) tall vertical leg.
8.	Model: 1125-0-A - 1 -1/4 inch (32mm) depth x 1 3/4 inch (44mm) tall vertical leg.
9.	Model: 1150-0-A - 1 -1/2 inch (38mm) depth x 1 3/4 inch (44mm) tall vertical leg.
G.	Unpunched 3.5 Inch Wide Flange Casing Bead:
1.	Model: 3538 - 3/8 inch (9.5mm) depth x 3 1/2 inch (89mm) tall vertical leg.
2.	Model: 3550 - 1/2 inch (13mm) depth x 3 1/2 inch (89mm) tall vertical leg.
3.	Model: 3558 - 5/8 inch (16mm) depth x 3 1/2 inch (89mm) tall vertical leg.
4.	Model: 3575 - 3/4 inch (19mm) depth x 3 1/2 inch (89mm) tall vertical leg.
5.	Model: 3578 - 7/8 inch (22mm) depth x 3 1/2 inch (89mm) tall vertical leg.
6.	WP - Casing bead to include weep holes.
H.	Medium Flange Casing Bead:
1.	Model: WF1050 - 1/2 inch (13mm) depth x 2 1/4 inch (57mm) tall vertical leg.
2.	Model: WF1058 - 5/8 inch (16mm) depth x 2 1/4 inch (57mm) tall vertical leg.
3.	Model: WF1075 - 3/4 inch (19mm) depth x 2 1/4 inch (57mm) tall vertical leg.
4.	Model: WF1078 - 7/8 inch (22mm) depth x 2 1/4 inch (57mm) tall vertical leg.
5.	WP - Casing bead to include weep holes.
I.	Lap Siding Step Bead:
1.	Model: SSB 75-50 - 1/2 inch (13mm) depth stepped up to a 3/4 inch (19mm) intermediate width x 2 inch (51mm) tall vertical leg.
2.	Model: SSB 75-58 - 5/8 inch (16mm) depth stepped up to a 3/4 inch (19mm) intermediate width x 2 inch (51mm) tall vertical leg.
3.	Model: SSB 78-58 - 5/8 inch (16mm) depth stepped up to a 7/8 inch (22mm) intermediate width x 2 inch (51mm) tall vertical leg.
4.	Model: SSB 100-50 - 1/2 inch (13mm) depth stepped up to a 1 inch (25mm) intermediate width x 2 inch (51mm) tall vertical leg. 
5.	Model: SSB 100-58 - 5/8 inch (16mm) depth stepped up to a 1 inch (25mm) intermediate width x 2 inch (51mm) tall vertical leg. 
6.	Model: SSB 125-58- 5/8 inch (16mm) depth stepped up to a 1-1/4 inch (31mm) intermediate width x 2 inch (51mm) tall vertical leg.
J.	Channel Casing Bead: 
1.	Model: 1150250CCB - 1-1/2 inch (38mm) depth x 2-1/2 inch (64mm) channel width.
2.	Model: 1200100CCB - 2 inch (51mm) depth x 1 inch (25mm) channel width.
3.	Model: 1200150CCB - 2 inch (51mm) depth x 1-1/2 inch (38mm) channel width.
4.	Model: 1200200CCB - 2 inch (51mm) depth x 2 inch (51mm) channel width.
2.6	CONTROL JOINTS
A.	"M" Control Joint: 
1.	Model: 2025 - 1/4 inch (6mm) depth / 1/4 inch (6mm) opening width / 3/4 inch (19mm) finish width.
2.	Model: 2138XS - 3/8 inch (9.5mm) depth / 1/4 inch (6mm) opening width / 3/4 inch (19mm) finish width.
3.	Model: 2150X - 1/2 inch (13mm) depth / 1/4 inch (6mm) opening width / 3/4 inch (19mm) finish width.
4.	Model: 2158X - 5/8 inch (16mm) depth / 1/4 inch (6mm) opening width / 3/4 inch (19mm) finish width.
5.	Model: 2175X - 3/4 inch (19mm) depth / 1/4 inch (6mm) opening width / 3/4 inch (19mm) finish width.
6.	Model: 2178X - 7/8 inch (22mm) depth / 1/4 inch (6mm) opening width / 3/4 inch (19mm) finish width.
7.	Model: 2100X - 1 inch (25mm) depth / 1/4 inch (6mm) opening width / 3/4 inch (19mm) finish width.
B.	"V" Control Joint:
1.	Model: 2038 - 3/8 inch (9.5mm) depth / 3/8 inch (9.5mm) opening width / 4-1/8 inch (105mm) overall width.
2.	Model: 2050 - 1/2 inch (13mm) depth / 3/8 inch (9.5mm) opening width / 4 -1/8 inch (105mm) overall width.
3.	Model: 2058 - 5/8 inch (16mm) depth / 3/8 inch (9.5mm) opening width / 4 -1/8 inch (105mm) overall width.
4.	Model: 2075 - 3/4 inch (19mm) depth / 3/8 inch (9.5mm) opening width / 4-1/8 inch (105mm) overall width.
5.	Model: 2078 - 7/8 inch (22mm) depth / 3/8 inch (9.5mm) opening width / 4 -1/8 inch (105mm) overall width.
6.	Model: 2100 - 1 inch (25mm) depth / 3/8 inch (9.5mm) opening width / 4-1/8 inch (105mm) overall width.
C.	Floor Line Control Bead w/Drip Edge: 
1.	Model: 2078-50 - 1/2 inch (13mm) depth x 3 1/2 inch (89mm) tall vertical leg.
2.	Model: 2078-58 - 5/8 inch (16mm) depth x 3 1/2 inch (89mm) tall vertical leg.
3.	Model: 2078-78 - 7/8 inch (22mm) depth x 3 1/2 inch (89mm) tall vertical leg.
4.	Model: 2078-78UP - 7/8 inch (22mm) depth x 3 1/2 inch (89mm) tall vertical leg, completely unpunched.
2.7	SCREEDS
A.	Bridge Screed / Reveal: 
1.	Model: 520-38 - 3/8 inch (9.5mm) depth / 2 inch (51mm) leg length with 7/8 inch (21mm) opening / 3/4 to 1-1/4 inch (19-32mm) movement.
2.	Model: 520-50 - 1/2 inch (13mm) depth / 2 inch (51mm) leg length with 7/8 inch (21mm) opening / 3/4 to 1 -1/4 inch (19-32mm) movement.
3.	Model: 520-58 - 5/8 inch (16mm) depth / 2 inch (51mm) leg length with 7/8 inch (21mm) opening / 3/4 to 1-1/4 inch (19-32mm) movement.
4.	Model: 520-75 - 3/4 inch (19mm) depth / 2 inch (51mm) leg length with 7/8 inch (21mm) opening / 3/4 to 1-1/4 inch (19-32mm) movement.
5.	Model: 520-78 - 7/8 inch (22mm) depth / 2 inch (51mm) leg length with 7/8 inch (21mm) opening / 3/4 to 1 -/4 inch (19-32mm) movement.
B.	Drip Screed:
1.	Model: 540-25 - 1/4 inch (6mm) depth / 2 inch (51mm) leg lengths / 1/4 inch (6mm) channel.
2.	Model: 540-38 - 3/8 inch (9.5mm) depth / 2 inch (51mm) leg lengths / 1/2 inch (13mm) channel.
3.	Model: 540-50 - 1/2 inch (13mm) depth / 2 inch (51mm) leg lengths / 1/2 inch (13mm) channel.
4.	Model: 540-58 - 5/8 inch (16mm) depth / 2 inch (51mm) leg lengths / 1/2 inch (13mm) channel.
5.	Model: 540-75 - 3/4 inch (19mm) depth / 2 inch (51mm) leg lengths / 1/2 inch (13mm) channel.
6.	Model: 540-78 - 7/8 inch (22mm) depth / 2 inch (51mm) leg lengths / 1/2 inch (13mm) channel.
C.	Foundation Sill Screeds: 
1.	Model: 631-50 - 1/2 inch (13mm) depth / 2 1/2 inch (64mm) leg length / FHA.
2.	Model: 631-58 - 5/8 inch (16mm) depth / 2 1/2 inch (64mm) leg length / FHA.
3.	Model: 631-75 - 3/4 inch (19mm) depth / 2 1/2 inch (64mm) leg length / FHA.
4.	Model: 631-78 - 7/8 inch (22mm) depth / 2 1/2 inch (64mm) leg length / FHA.
5.	Model: 632-38 - 3/8 inch (9.5mm) depth / 3 1/2 inch (89mm) leg length / FHA.
6.	Model: 632-50 - 1/2 inch (13mm) depth / 3 1/2 inch (89mm) leg length / FHA.
7.	Model: 632-58 - 5/8 inch (16mm) depth / 3 1/2 inch (89mm) leg length / FHA.
8.	Model: 632-75 - 3/4 inch (19mm) depth / 3 1/2 inch (89mm) leg length / FHA.
9.	Model: 632-78 - 7/8 inch (22mm) depth / 3 1/2 inch (89mm) leg length / FHA.
10.	Model: 632-100 - 1 inch (25mm) depth / 3 1/2 inch (89mm) leg length / FHA.
11.	Model: 632-78EL - 7/8 inch (22mm) depth, 1/2 inch (13 mm) extended leg/ 3 1/2 inch (89mm) leg length / FHA.
2.8	SLIP JOINTS
A.	Slip Joint/Expansion Joint:
1.	Model: 2079 - 3/8 inch (9.5mm) depth / 2 inch (51mm) leg length / 0 to 1/2 inch (13mm) movement.
2.	Model: 501-38 - 3/8 inch (9.5mm) depth / 2 inch (51mm) leg length / 5/8 to 1 1/8 inch (15-29mm) movement.
3.	Model: 500-38 - 3/8 inch (9.5mm) depth / 1-1/2 inch (38mm) leg length / 1 1/4 to 1 5/8 inch (32-41mm) movement.
4.	Model: 2080 - 1/2 inch (13mm) depth / 2 inch (51mm) leg length / 0 to 1/2 inch (13mm) movement.
5.	Model: 501-50 - 1/2 inch (13mm) depth / 1 inch (25mm) leg length / 3/4 to 1 1/8 inch (19-29mm) movement.
6.	Model: 500-50 - 1/2 inch (13mm) depth / 1-1/2 inch (38mm) leg length / 1 1/4 to 1 5/8 inch (32-41mm) movement.
7.	Model: 2083 - 5/8 inch (16mm) depth / 2 inch (51mm) leg length / 0 to 1/2 inch (13mm) movement.
8.	Model: 501-58 - 5/8 inch (16mm) depth / 1 inch (25mm) leg length / 3/4 to 1 1/8 inch (19-29mm) movement.
9.	Model: 500-58 - 5/8 inch (16mm) depth / 1-1/2 inch (38mm) leg length / 1 1/4 to 1 5/8 inch (32-41mm) movement.
10.	Model: 2081 - 3/4 inch (19mm) depth / 2 inch (51mm) leg length / 0 to 1/2 inch (13mm) movement.
11.	Model: 501-75 - 3/4 inch (19mm) depth / 1 inch (25mm) leg length / 3/4 to 1 1/8 inch (19-29mm) movement.
12.	Model: 500-75 - 3/4 inch (19mm) depth / 1-1/2 inch (38mm) leg length / 1 1/4 to 1 5/8 inch (32-41mm) movement.
13.	Model: 2082 - 7/8 inch (22mm) depth / 2 inch (51mm) leg length / 0 to 1/2 inch (13mm) movement.
14.	Model: 501-78 - 7/8 inch (22mm) depth / 1 inch (25mm) leg length / 3/4 to 1 1/8 inch (19-29mm) movement.
15.	Model: 500-78 - 7/8 inch (22mm) depth / 1-1/2 inch (38mm) leg length / 1 1/4 to 1 5/8 inch (32-41mm) movement.
B.	Inside/Outside Corner Slip Joint/Expansion Joint: 
1.	Model: 511-38 - 3/8 inch (9.5mm) depth / 2 inch (51mm) leg length with 3/4 to 1 inch (19-25mm) inside corner exposure / 3/4 to 1 inch (19-25mm) movement.
2.	Model: 511-50 - 1/2 inch (13mm) depth / 2 inch (51mm) leg length with 3/4 to 1 inch (19-25mm) inside corner exposure / 3/4 to 1 inch (19-25mm) movement.
3.	Model: 511-58 - 5/8 inch (16mm) depth / 2 inch (51mm) leg length with 3/4 to 1 inch (19-25mm) inside corner exposure / 3/4 to 1 inch (19-25mm) movement.
4.	Model: 511-75 - 3/4 inch (19mm) depth / 2 inch (51mm) leg length with 3/4 to 1 inch (19-25mm) inside corner exposure / 3/4 to 1 inch (19-25mm) movement.
5.	Model: 511-78 - 7/8 inch (22mm) depth / 2 inch (51mm) leg length with 3/4 to 1 inch (19-25mm) inside corner exposure / 3/4 to 1 inch (19-25mm) movement.
2.9	ULTRA-TRAC REVEAL SYSTEM
A.	ULTRA-TRAC System Plaster Reveal:
1.	Model 707-25: 1/2 inch width x 1/4 inch depth (13mm x 6mm).
2.	Model 707-38: 1/2 inch width x 3/8 inch depth (13mm x 9.5mm).
3.	Model 707-50: 1/2 inch width x 1/2 inch depth (13mm x 13mm).
4.	Model 707-58: 1/2 inch width x 5/8 inch depth (13mm x 16mm).
5.	Model 707-75: 1/2 inch width x 3/4 inch depth (13mm x 19mm).
6.	Model 707-78: 1/2 inch width x 7/8 inch depth (13mm x 22mm).
7.	Model 708-25: 3/4 inch width x 1/4 inch depth (19mm x 6mm).
8.	Model 708-38: 3/4 inch width x 3/8 inch depth (19mm x 9.5mm).
9.	Model 708-50: 3/4 inch width x 1/2 inch depth (19mm x 13mm).
10.	Model 708-58: 3/4 inch width x 5/8 inch depth (19mm x 16mm).
11.	Model 708-75: 3/4 inch width x 3/4 inch depth (19mm x 19mm).
12.	Model 708-78: 3/4 inch width x 7/8 inch depth (19mm x 22mm).
13.	Model 709-25: 1 inch width x 1/4 inch depth (25mm x 6mm).
14.	Model 709-38: 1 inch width x 3/8 inch depth (25mm x 9.5mm).
15.	Model 709-50: 1 inch width x 1/2 inch depth (25mm x 13mm).
16.	Model 709-58: 1 inch width x 5/8 inch depth (25mm x 16mm).
17.	Model 709-75: 1 inch width x 3/4 inch depth (25mm x 19mm).
18.	Model 709-78: 1 inch width x 7/8 inch depth (25mm x 22mm).
19.	Model 710-25: 1-1/2 inch width x 1/4 inch depth (38mm x 6mm).
20.	Model 710-38: 1 -1/2 inch width x 3/8 inch depth (38mm x 9.5mm).
21.	Model 710-50: 1-1/2 inch width x 1/2 inch depth (38mm x 13mm).
22.	Model 710-58: 1-1/2 inch width x 5/8 inch depth (38mm x 16mm).
23.	Model 710-75: 1-1/2 inch width x 3/4 inch depth (38mm x 19mm).
24.	Model 710-78: 1 inch width x 7/8 inch depth (25mm x 22mm).
25.	Model 711-25: 2 inch width x 1/4 inch depth (51mm x 6mm).
26.	Model 711-38: 2 inch width x 3/8 inch depth (51mm x 9.5mm).
27.	Model 711-50: 2 inch width x 1/2 inch depth (51mm x 13mm).
28.	Model 711-58: 2 inch width x 5/8 inch depth (51mm x 16mm).
29.	Model 711-75: 2 inch width x 3/4 inch depth (51mm x 19mm).
30.	Model 712-50: 2-1/2 inch width x 1/2 inch depth (64mm x 13mm).
31.	Model 712-58: 2 -1/2 inch width x 5/8 inch depth (64mm x 16mm).
32.	Model 712-75: 2-1/2 inch width x 3/4 inch depth (64mm x 19mm).
33.	Model 713-50: 3 inch width x 1/2 inch depth (76mm x 13mm).
34.	Model 713-58: 3 inch width x 5/8 inch depth (76mm x 16mm).
35.	Model 713-75: 3 inch width x 3/4 inch depth (76mm x 19mm).
36.	Model 714-50: 4 inch width x 1/2 inch depth (102mm x 13mm).
37.	Model 714-58: 4 inch width x 5/8 inch depth (102mm x 16mm).
38.	Model 714-75: 4 inch width x 3/4 inch depth (102mm x 19mm).
39.	Model 714-78: 4 inch width x 7/8 inch depth (102mm x 22mm).
B.	"F" Plaster Reveal:
1.	Model F707-25: 1/2 inch width x 1/4 inch depth (13mm x 6mm).
2.	Model F707-38: 1/2 inch width x 3/8 inch depth (13mm x 9.5mm).
3.	Model F707-50: 1/2 inch width x 1/2 inch depth (13mm x 13mm).
4.	Model F707-58: 1/2 inch width x 5/8 inch depth (13mm x 16mm).
5.	Model F707-75: 1/2 inch width x 3/4 inch depth (13mm x 19mm).
6.	Model F707-78: 1/2 inch width x 7/8 inch depth (13mm x 22mm).
7.	Model F708-25: 3/4 inch width x 1/4 inch depth (19mm x 6mm).
8.	Model F708-38: 3/4 inch width x 3/8 inch depth (19mm x 9.5mm).
9.	Model F708-50: 3/4 inch width x 1/2 inch depth (19mm x 13mm).
10.	Model F708-58: 3/4 inch width x 5/8 inch depth (19mm x 16mm).
11.	Model F708-75: 3/4 inch width x 3/4 inch depth (19mm x 19mm)
12.	Model F708-78: 3/4 inch width x 7/8 inch depth (19mm x 22mm).
13.	Model F709-25: 1 inch width x 1/4 inch depth (25mm x 6mm).
14.	Model F709-38: 1 inch width x 3/8 inch depth (25mm x 9.5mm).
15.	Model F709-50: 1 inch width x 1/2 inch depth (25mm x 13mm).
16.	Model F709-58: 1 inch width x 5/8 inch depth (25mm x 15mm).
17.	Model F709-75: 1 inch width x 3/4 inch depth (25mm x 19mm)
18.	Model F709-78: 1 inch width x 7/8 inch depth (25mm x 22mm).
19.	Model F710-25: 1-1/2 inch width x 1/4 inch depth (38mm x 6mm).
20.	Model F710-38: 1-1/2 inch width x 3/8 inch depth (38mm x 9.5mm).
21.	Model F710-50: 1-1/2 inch width x 1/2 inch depth (38mm x 13mm).
22.	Model F710-58: 1-1/2 inch width x 5/8 inch depth (38mm x 16mm).
23.	Model F710-75: 1-1/2 inch width x 3/4 inch depth (38mm x 19mm).
24.	Model F710-78: 1-1/2 inch width x 7/8 inch depth (38mm x 22mm).
25.	Model F711-25: 2 inch width x 1/4 inch depth (51mm x 6mm).
26.	Model F711-38: 2 inch width x 3/8 inch depth (51mm x 9.5mm).
27.	Model F711-50: 2 inch width x 1/2 inch depth (51mm x 13mm).
28.	Model F711-58: 2 inch width x 5/8 inch depth (51mm x 16mm).
29.	Model F711-75: 2 inch width x 3/4 inch depth (51mm x 19mm).
30.	Model F712-50: 2-1/2 inch width x 1/2 inch depth (64mm x 13mm).
31.	Model F712-58: 2-1/2 inch width x 5/8 inch depth (64mm x 15mm).
32.	Model F712-75: 2-1/2 inch width x 3/4 inch depth (64mm x 19mm).
33.	Model F713-50: 3 inch width x 1/2 inch depth (76mm x 13mm).
34.	Model F713-58: 3 inch width x 5/8 inch depth (76mm x 16mm).
35.	Model F713-75: 3 inch width x 3/4 inch depth (76mm x 19mm).
36.	Model F714-50: 4 inch width x 1/2 inch depth (102mm x 13mm).
37.	Model F714-58: 4 inch width x 5/8 inch depth (102mm x 16mm).
38.	Model F714-75: 4 inch width x 3/4 inch depth (102mm x 19mm).
39.	Model F714-78: 4 inch width x 7/8 inch depth (102mm x 22mm).
2.10	ULTRA-TRAC INTERSECTIONS 
A.	90 Degree Angle Intersection:
1.	Reveal: 3/4 inch (19mm). Depth to match specified components.
2.	Reveal: 1 inch (25mm). Depth to match specified components.
3.	Reveal: 1-1/2 inches (38mm). Depth to match specified components.
4.	Reveal: 2 inches (51mm). Depth to match specified components.
5.	Reveal: 2-1/2 inches (64mm). Depth to match specified components.
6.	Reveal: 3 inches (76mm). Depth to match specified components.
B.	Cross Intersection:
1.	Reveal: 3/4 inch (19mm). Depth to match specified components.
2.	Reveal: 1 inch (25mm). Depth to match specified components.
3.	Reveal: 1-1/2 inches (38mm). Depth to match specified components.
4.	Reveal: 2 inches (51mm). Depth to match specified components.
5.	Reveal: 2-1/2 inches (64mm). Depth to match specified components.
6.	Reveal: 3 inches (76mm). Depth to match specified components.
C.	End Stop for Intersection:
1.	Reveal: 3/4 inch (19mm). Depth to match specified components.
2.	Reveal: 1 inch (25mm). Depth to match specified components.
3.	Reveal: 1-1/2 inches (38mm). Depth to match specified components.
4.	Reveal: 2 inches (51mm). Depth to match specified components.
5.	Reveal: 2-1/2 inches (64mm). Depth to match specified components.
6.	Reveal: 3 inches (76mm). Depth to match specified components.
D.	Inside Corners:
1.	Reveal: 3/4 inch (19mm). Depth to match specified components.
2.	Reveal: 1 inch (25mm). Depth to match specified components.
3.	Reveal: 1-1/2 inches (38mm). Depth to match specified components.
4.	Reveal: 2 inches (51mm). Depth to match specified components.
5.	Reveal: 2-1/2 inches (64mm). Depth to match specified components.
6.	Reveal: 3 inches (76mm). Depth to match specified components.
E.	Outside Corners:
1.	Reveal: 3/4 inch (19mm). Depth to match specified components.
2.	Reveal: 1 inch (25mm). Depth to match specified components.
3.	Reveal: 1-1/2 inches (38mm). Depth to match specified components.
4.	Reveal: 2 inches (51mm). Depth to match specified components.
5.	Reveal: 2-1/2 inches (64mm). Depth to match specified components.
6.	Reveal: 3 inches (76mm). Depth to match specified components. 
F.	T Intersection:
1.	Reveal: 3/4 inch (19mm). Depth to match specified components.
2.	Reveal: 1 inch (25mm). Depth to match specified components.
3.	Reveal: 1-1/2 inches (38mm). Depth to match specified components.
4.	Reveal: 2 inches (51mm). Depth to match specified components.
5.	Reveal: 2-1/2 inches (64mm). Depth to match specified components.
6.	Reveal: 3 inches (76mm). Depth to match specified components.
2.11	SOFFIT VENTS
A.	Continuous Soffit Vent:
1.	Model 300:
a.	Depth: 3/8 inch (9.5mm).
b.	Opening: 2-5/8 inches (67mm).
c.	NFVA: 15 sq inches per lineal foot (9,678 sqmm).
2.	Model 301:
a.	Depth: 3/8 inch (9.5mm).
b.	Opening: 1-3/4 inches (44mm).
c.	NFVA: 7 sq inches per lineal foot (4,516 sqmm).
3.	Model 3300:
a.	Depth: 3/8 inch (9.5mm).
b.	Opening: 3 inches (76mm).
c.	NFVA: 15 sq inches per lineal foot (9,678 sqmm). 
4.	Model 4300:
a.	Depth: 3/8 inch (9.5mm).
b.	Opening: 4 inches (102mm).
c.	NFVA: 16 sq inches per lineal foot (10,323 sqmm).
5.	Model 6300:
a.	Depth: 3/8 inch (9.5mm).
b.	Opening: 6 inches (152mm).
c.	NFVA: 20 sq inches per lineal foot (12,904 sqmm).
6.	Model 549: 
a.	Depth: 1/2 inch (13mm).
b.	Depth: 5/8 inch (16mm).
c.	Depth: 3/4 inch (19mm).
d.	Depth: 7/8 inch (22mm).
e.	Opening: 2-3/8 inches (60mm).
f.	NFVA: 15 sq inches per lineal foot (9,678 sqmm).
7.	Model 3549:
a.	Depth: 1/2 inch (13mm).
b.	Depth: 5/8 inch (16mm).
c.	Depth: 3/4 inch (19mm).
d.	Depth: 7/8 inch (22mm).
e.	Opening: 3 inches (76mm).
f.	NFVA: 15 sq inches per lineal foot (9,678 sqmm).
8.	Model 4549:
a.	Depth: 1/2 inch (13mm).
b.	Depth: 5/8 inch (16mm).
c.	Depth: 3/4 inch (19mm).
d.	Depth: 7/8 inch (22mm).
e.	Opening: 4 inches (102mm).
f.	NFVA: 16 sq inches per lineal foot (10,323 sqmm).
9.	Model 6549:
a.	Depth: 1/2 inch (13mm).
b.	Depth: 3/4 inch (19mm).
c.	Opening: 4 inches (102mm).
d.	NFVA: 18 sq inches per lineal foot (11,614 sqmm).
B.	Three Piece Continuous Soffit Vent with 90 Degree Leg:
1.	Model 551-50:
a.	Depth: 1/2 inch (13mm).
b.	Vertical Leg: 1-1/4 inch (32mm).
c.	Opening: 2-5/8 inch (67mm).
d.	Opening: 1-3/4 inches (44mm).
e.	Opening: 3 inches (76mm).
f.	Opening: 4 inches (102mm).
g.	Opening: 6 inches (152mm).
2.	Model 551-58:
a.	Depth: 5/8 inch (16mm).
b.	Vertical Leg: 1-1/4 inch (32mm).
c.	Opening: 2-5/8 inch (67mm).
d.	Opening: 1-3/4 inches (44mm).
e.	Opening: 3 inches (76mm).
f.	Opening: 4 inches (102mm).
g.	Opening: 6 inches (152mm).
3.	Model 551-75:
a.	Depth: 3/4 inch (19mm).
b.	Vertical Leg: 1 1/4 inch (32mm).
c.	Opening: 2-5/8 inch (67mm).
d.	Opening: 1-3/4 inches (44mm).
e.	Opening: 3 inches (76mm).
f.	Opening: 4 inches (102mm).
g.	Opening: 6 inches (152mm).
4.	Model 551-78:
a.	Depth: 7/8 inch (22mm).
b.	Vertical Leg: 1-1/4 inch (32mm).
c.	Opening: 2-5/8 inch (67mm).
d.	Opening: 1-3/4 inches (44mm).
e.	Opening: 3 inches (76mm).
f.	Opening: 4 inches (102mm).
g.	Opening: 6 inches (152mm).
C.	Two-Piece Continuous Soffit Vent:
1.	Model F549 WF551:
a.	Depth: 1/2 inch (13mm).
b.	Depth: 5/8 inch (16mm).
c.	Depth: 3/4 inch (19mm).
d.	Depth: 7/8 inch (22mm).
e.	Opening: 2-3/8 inches (60mm).
f.	NFVA: 15 sq inches per lineal foot (9,678 sqmm).
2.	Model F3549 WF551:
a.	Depth: 1/2 inch (13mm).
b.	Depth: 5/8 inch (16mm).
c.	Depth: 3/4 inch (19mm).
d.	Depth: 7/8 inch (22mm).
e.	Opening: 3 inches (76mm).
f.	NFVA: 15 sq inches per lineal foot (9,678 sqmm).
3.	Model F4549 WF551:
a.	Depth: 1/2 inch (13mm).
b.	Depth: 5/8 inch (16mm).
c.	Depth: 3/4 inch (19mm).
d.	Depth: 7/8 inch (22mm).
e.	Opening: 4 inches (102mm).
f.	NFVA: 16 sq inches per lineal foot (10,323 sqmm).
D.	Three-Piece Continuous Soffit Vent:
1.	Model 550:
a.	Depth: 3/8 inch (9.5mm).
b.	Depth: 1/2 inch (13mm).
c.	Depth: 5/8 inch (16mm).
d.	Depth: 3/4 inch (19mm).
e.	Depth: 7/8 inch (22mm).
f.	Opening: 2-5/8 inches (67mm).
g.	Opening: 1-3/4 inches (44mm).
h.	NFVA: Up to 15 sq inches per lineal foot (9,678 sqmm).
2.	Model 4550:
a.	Depth: 3/8 inch (9.5mm).
b.	Depth: 1/2 inch (13mm).
c.	Depth: 5/8 inch (16mm).
d.	Depth: 3/4 inch (19mm).
e.	Depth: 7/8 inch (22mm).
f.	Opening: 4 inches (102mm).
g.	Opening: 3 inches (76mm).
h.	NFVA: Up to 16 sq inches per lineal foot (10,323 sqmm).
3.	Model 6550:
a.	Depth: 3/8 inch (9.5mm).
b.	Depth: 1/2 inch (13mm).
c.	Depth: 5/8 inch (16mm).
d.	Depth: 3/4 inch (19mm).
e.	Depth: 7/8 inch (22mm).
f.	Opening: 6 inches (152mm).
g.	NFVA: 20 sq inches per lineal foot (12,904 sqmm).
2.12	MESH CORNER BEADS 
A.	Mesh Corner Beads: 
1.	Compliance:  ASTM D579, EIMA 1501.01. 
2.	Model:  2209MESH PVC corner bead and alkali-resistant fiberglass mesh, fire and alkaline-resistant mesh. 
3.	Dimensions:  7/8 inch (22 mm) flange with mesh attached to both legs; 3 inches (76 mm) on one leg and 5 inches (127 mm) on the other leg.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION - TRIMS
A.	Install trim and accessories in accordance with manufacturer's instructions.
B.	All butt joints, intersections and ends shall be caulked at the time of installation using an elastomeric sealant, such as Plastic Components' Ultra-Tech tm (PC-ULTW).
3.4	INSTALLATION - PLASTIC LATH
A.	Install lath in accordance with manufacturer's instructions.
B.	Apply lath with ribbed surface facing the substrate.
C.	Attach lath with fasteners approved by the manufacturer every 6 inches (152mm) on center into framing members. Where cementitious materials are present, space fastener rows 16 inches (406mm) apart.
3.5	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION